3GPP TSG-RAN WG2 #113bis-e R2-210xxxx

Electronic meeting, 12th April – 20th April 2021

Agenda Item: 6.1.4.1.3

Source: Ericsson

Title: Summary of [AT113bis-e][021][NR16] Sys Info Inter Node and Misc

Document for: Discussion, Decision

# 1 Introduction

This document is to handle the following email discussion:

* [AT113bis-e][021][NR16] Sys Info Inter Node and Misc (Ericsson)

 Scope: Treat R2-2102714, R2-2103582, R2-2103661, R2-2103929, R2-2104205, R2-2103851, R2-2103645, R2-2103936,

 Phase 1, determine agreeable parts, Phase 2, for agreeable parts Work on CRs.

 Intended outcome: Report and Agreed-in-principle CRs

 Deadline: Schedule A

Regarding the deadlines, I would like to set the following 2 deadlines:

1) First deadline on **Wednesday April 14 1000 UTC** to settle scope what is agreeable.

2) Second deadline on **Monday April 19 1800 UTC** to agree the CRs (where applicable) and final check.

# 2 Contact information

|  |  |
| --- | --- |
| Company (Name) | Email |
|  |  |
|  |  |
|  |  |

# 3 Discussion

## 3.1 Corrections to UE action upon SIB1 reception

[R2-2102714](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2102714.zip) Corrections to UE action upon SIB1 reception Samsung Electronics Co., Ltd CR Rel-16 38.331 16.4.0 2475 - F NR\_pos-Core, 5G\_V2X\_NRSL-Core

*Reason for change:*

If the UE needs to acquire a SIB, it checks si-BroadcastStatus in SIB1. According to current procedure, if UE has already acquired SIB1 in current modifictaion period, UE does not reacquire SIB1 for checking si-BroadcastStatus .

A) If the si-BroadcastStatus is set to broadcasting in the SIB1 acquired in current modification period, **there is no need to reacquire SIB1** as the value of the si-BroadcastStatus is valid until the end of the BCCH modification period when set to broadcasting.

B) If the si-BroadcastStatus is set to notbroadcasting in the SIB1 acquired in current modification period, SIB1 **needs to be reacquired**. si-BroadcastStatus can be changed from notbroadcasting to broadcasting during the modification period.

**Question 1**: Do company agree with the changes proposed in CR [R2-2102714](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2102714.zip)?

|  |  |  |
| --- | --- | --- |
| Company  | Agree (y/n) | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.2 Discussion on leap second and DST for R16 accurate time

[R2-2103582](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103582.zip) Discussion on leap second and DST for R16 accurate time ZTE Corporation, Sanechips discussion Rel-16 NR\_IIOT-Core

[R2-2104506](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2104506.zip)  Discussion on leap second and DST for R16 accurate time   ZTE Corporation, Sanechips, CMCC, China Southern Power Grid Co., Ltd Rel-16 NR\_IIOT-Core

*Observation 1: It can be seen that the leap seconds are not considered in the calculation of R16 accurate time based on referenceTimeInfo IE.*

*Observation 2a: If the referenceTimeInfo indicates the GPS time (Alt1), it’s no need for UE to correct the referenceTimeInfo when leap second occurs.*

*Observation 2b: When the time is from remote TSN GM clock (Alt2) or Local on-site TSN GM clock, leap second may exist in the TSN GM clock. The gNB may need to further notify this leap second information to UE for UE to correct the local time but this is infeasible based on the current referenceTimeInfo IE definition.*

*Observation 3a: Based on the leap second process mechanism from R15 (would be in R16 if Proposal 1 is agreed), if leap second occurs, there will be one second time difference between UE and gNB in the time duration between the occurrence of leap second and the subsequent reference time information provision. This would further cause negative impacts on deterministic delay, e.g., to the R16 TSN system.*

*Observation 3b: If DST/DSTE switch occurs, there will be one or two hours time difference between UE and gNB in the time duration between the occurrence of DST/DSTE switch and the subsequent reference time information provision.*

*Proposal 1: The R16 referenceTimeInfo IE definition of accurate reference timing delivery needs to take leapSeconds into account in order to correct the local time when leap second occurs.*

*Proposal 2a: To provide leap second prediction indication via referenceTimeInfo IE to UE in order that UE and gNB can apply the time with leap second synchronously.*

*Proposal 2b: To provide DST prediction indication via referenceTimeInfo IE to UE in order that UE and gNB can apply the time with DST/DSTE synchronously.*

**Question 2**: According to the analysis provided in [R2-2104506](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2104506.zip), do companies agree on the proposals regarding the issue regarding the leap second and DST for the R16 accurate time?

|  |  |  |
| --- | --- | --- |
| Company  | Proposal x:Agree (y/n) | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.3 Correction on failure type for SCG failure

### 3.3.1 Correction on failureType in FailureReportSCG-EUTRA and scgFailureInfoEUTRA

[R2-2103929](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103929.zip) Correction on failureType in FailureReportSCG-EUTRA and scgFailureInfoEUTRA Huawei, HiSilicon CR Rel-16 38.331 16.4.1 2540 - F NR\_newRAT-Core, NR\_unlic-Core

*Reason for change:*

In RAN2#113-e meeting, it has agreed to remove the *bh-RLF-r16* from *failureTypeEUTRA* within *scgFailureInfoEUTRA-r16*. The reason is that BH RLF cannot be detected in EUTRAN leg since EUTRAN leg cannot support the functionality of backhauling. Some other similar issues still exist in the current NR RRC spec.

The IE *FailureReportSCG-EUTRA* is used to report information about E-UTRA SCG failures detected by the UE. In the RRC spec, it is specified as:

|  |
| --- |
| The UE shall set the contents of the *SCGFailureInformationEUTRA* message as follows:1> include *failureType* within *failureReportSCG-EUTRA* and set it to indicate the SCG failure in accordance with TS 36.331 [10] clause 5.6.13.4; |

According to clause 5.6.13.4 of TS 36.331, failureType can be set as t313-Expiry, randomAccessProblem, rlc-MaxNumRetx, scg-ChangeFailure; however failureType cannot be set as scg-lbtFailure, beamFailureRecoveryFailure, or t312-Expiry. The text is excerpted as follows:

|  |
| --- |
| 5.6.13.4 Failure type determination in NE-DCThe UE shall:1> if SCG failure is due to T313 expiry:2> consider the *failureType* to be *t313-Expiry*;1> else if SCG failure is due to indication from SCG MAC that a random access problem was detected:2> consider the *failureType* to be *randomAccessProblem*;1> else if SCG failure is due to indication from SCG RLC that the maximum number of retransmissions was reached:2> consider the *failureType* to be *rlc-MaxNumRetx*;1> else if SCG failure is due to SCG change failure:2> consider the *failureType* to be *scg-ChangeFailure*; |

For a LTE eNB, the SpCell cannot be configured on the shared spectrum, thus *failureType* with *scg-lbtFailure* will never be reported in IE *failureReportedSCG-EUTRA*. Beam related operation is not supported for LTE and T312 will not be configured for LTE SCG, therefore *failureType* will never be set as *beamFailureRecoveryFailure* or *t312-Expiry* in IE *failureReportSCG-EUTRA*.

Similarly, for *failureTypeEUTRA* in the IE *scgFailureInfoEUTRA* of *CG-ConfigInfo* message, the values *scg-lbtFailure*, *beamFailureRecoveryFailure*, and *t312-Expiry* are of no use and can be removed. The consenquence is that *failureTypeEUTRA* in the IE *scgFailureInfoEUTRA* will only contain spare values. Considering *measResultSCG-EUTRA* within the same IE will never be reported either, we can dummify *scgFailureInfoEUTRA* from the *CG-ConfigInfo* message.

**Question 3**: Do company agree with the changes proposed in CR [R2-2103929](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103929.zip)?

|  |  |  |
| --- | --- | --- |
| Company  | Agree (y/n) | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

### 3.3.2 Correction to scgFailureInfoEUTRA and FailureReportSCG-EUTRA

[R2-2103936](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103936.zip) Correction to scgFailureInfoEUTRA and FailureReportSCG-EUTRA Ericsson CR Rel-16 38.331 16.4.1 2541 - F NR\_newRAT-Core

*Reason for change:*

The scgFailureInfoEUTRA IE within the CG-ConfigInfo-v1610-IEs and the FailureReportSCG-EUTRA IE within the SCGFailureInformationEUTRA include certain failure types which are not applicable to EUTRA. In particular, the scg-lbtFailure-r16, and beamFailureRecoveryFailure-r16 are not applicable to LTE, since in LTE specification there is no LBT failure handling procedure, and no beam failure recovery procedure.

**Question 4**: Do company agree with the changes proposed in CR [R2-2103936](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103936.zip)?

|  |  |  |
| --- | --- | --- |
| Company  | Agree (y/n) | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.4 Introduction of TDD Configuration Inter-node RRC Message

[R2-2104205](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2104205.zip) Introduction of TDD Configuration Inter-node RRC Message CATT draftCR Rel-16 38.331 16.4.1 F NR\_SON\_MDT-Core Late

*Reason for change:*

RAN3 has agreed to add the *TDD-UL-DL-ConfigurationCommon* in the Served Cell Information NR in 38.423 as following:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| >*TDD* |  |  |  |  |  |  |
| >>**TDD Info** |  | *1* |  |  | – |  |
| >>>Frequency Info | M |  | NR Frequency Info9.2.2.19 |  | – |  |
| >>>Transmission Bandwidth | M |  | NR Transmission Bandwidth9.2.2.20 |  | – |  |
| >>>Intended TDD DL-UL Configuration NR | O |  | 9.2.2.40 |  | YES | ignore |
| >>>TDD UL-DL Configuration Common NR  | O |  | OCTET STRING | The *tdd-UL-DL-ConfigurationCommon* as defined in TS 38.331 [10] | YES | ignore |

As the 38.423 specified, the TDD-UL-DL-ConfigurationCommon should be defined in 38.331, however in current 38.331, the definition of TDD-UL-DL-ConfigurationCommon for the inter-node message is missing.

**Question 5**: Do company agree with the changes proposed in CR [R2-2104205](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2104205.zip)?

|  |  |  |
| --- | --- | --- |
| Company  | Agree (y/n) | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.5 Correction on UTRA Capabilty forwarding in HO preparation

[R2-2103851](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103851.zip) Correction on UTRA Capabilty forwarding in HO preparation Apple CR Rel-16 36.331 16.4.0 4626 - F SRVCC\_NR\_to\_UMTS-Core

*Reason for change:*

For UTRA-FDD case, the UE UTRA capability must be known a-priori to the target RNC to build the HO to UTRA command. This also makes sense in the light of the UE RAT Container list in NR including the UTRA-FDD as one of the RATs which can be queried by the source NR RAT. Hence, there is no need to exclude this UTRA capability forwarding.

For NR to EUTRA case, the UTRA capability should be allowed to be forwarded to the target RAT in HO preparation and can be ignored by target eNB if received in case the target eNB would obtain UTRA capabilities from the UE for SRVCC.

Also, we need to align this with the agreement made in RAN2#113 for 38.331 CR ([R2-2102046](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2102046.zip)) regarding the UTRA capabilities in EUTRA-to-NR HO case.

**Question 6**: Do company agree with the changes proposed in CR [R2-2103851](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103851.zip)?

|  |  |  |
| --- | --- | --- |
| Company  | Agree (y/n) | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.6 Miscellaneous non-controversial corrections Set IX

[R2-2103645](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103645.zip) Miscellaneous non-controversial corrections Set IX Ericsson CR Rel-16 38.331 16.4.1 2519 - F NR\_newRAT-Core, TEI16

*This CR contains miscellaneous non-controversial correction for 38.331. It may also be used to merge editorial correction agreed in CRs submitted within this or other agenda items.*

**Question 7**: Do company agree with the changes proposed in CR [R2-2103645](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103645.zip)?

|  |  |  |
| --- | --- | --- |
| Company  | Agree (y/n) | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

Based on the discussion in the previous sections we propose the following:

# References