3GPP TSG-RAN WG2 Meeting #114 Electronic R2-210xxxx

Elbonia, 19 – 27 May 2021

**Agenda item: 5.4**

**Source: Qualcomm (Rapporteur)**

**Title: Offline 006 on Rel-15 Connection Control III**

**WID/SID: NR\_newRAT-Core**

**Document for: Discussion and Decision**

# 1 Introduction

This document reflects the content and outcome of the following email discussion:

* [AT114-e][006][NR15] Connection Control III (Qualcomm)

Scope: Treat R2-2106188, R2-2106189, R2-2106267, R2-2106270, R2-2105323, R2-2105324, R2-2105767, R2-2105950, R2-2105951, R2-2106182, R2-2106183, R2-2106178, R2-2106179, R2-2106077, R2-2106079

Phase 1, determine agreeable parts, Phase 2, for agreeable parts Work on CRs.

Intended outcome: Report and Agreed CRs.

Deadline: Schedule A

# 2 Contact Points

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| QCOM (Rapporteur) | Mouaffac Ambriss | [mambriss@qti.qualcomm.com](mailto:mambriss@qti.qualcomm.com) |
| MediaTek | Felix Tsai | Chun-Fan.tsai@mediatek.com |
| ZTE | Liu Yu | liu.yu3@zte.com.cn |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Discussion Phase 1

## 3.1 BWP

The CRs related to this topic are:

[R2-2106188](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106188.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106188.zip) Clarification on releasing of BWP Huawei, HiSilicon CR Rel-15 38.331 15.13.0 2678 - F NR\_newRAT-Core

[R2-2106189](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106189.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106189.zip) Clarification on releasing of BWP Huawei, HiSilicon CR Rel-16 38.331 16.4.0 2679 - A NR\_newRAT-Core

The CR clarifies by adding a note that “When releasing a BWP, the network should ensure that the active BWP is in place after the UE applies the RRC reconfiguration message, e.g. by including *firstActiveDownlinkBWP-Id/firstActiveUplinkBWP-Id* in the same RRC message”.

**Question 1**: do you agree with the addition of the note in order to clarify the expected network behaviour.

|  |  |  |
| --- | --- | --- |
| Answers to Question 1 | | |
| Company | Yes/No | Comments |
| QCOM | Yes | We’re fine with the note |
| MediaTek | No | It is unclear what does “in place” means in the NOTE and we don’t know why “e.g.” is used instead of “i.e.”.  We suggest to capture a NOTE same as previous agreement. i.e.  “If the network releases the active BWP using RRC reconfiguration message, it includes the *firstActiveDownlinkBWP-Id*/ *firstActiveUplinkBWP-Id* in the RRC Reconfiguration message” |
| ZTE | No | Firstly, We think the NOTE does not accurately capture the agreement ’if the network releases the active BWP using RRC reconfiguration message, it includes the firstActiveDownlinkBWP-Id/ firstActiveUplinkBWP-Id in the RRC Reconfiguration message’, same view as MediaTek.  Secondly, we think there is no need to capture anything in spec, also this is majority views in the last e-meeting. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 1**: TBD.

**Proposal 1**: TBD.

## 3.2 L1 Parameters

The CRs related to this topic are:

[R2-2106267](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106267.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106267.zip) Clarification of recurrence in RateMatchPattern Qualcomm Incorporated CR Rel-15 38.331 15.13.0 2687 - F NR\_newRAT-Core

[R2-2106270](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106270.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106270.zip) Clarification of recurrence in RateMatchPattern Qualcomm Incorporated CR Rel-16 38.331 16.4.1 2688 - A NR\_newRAT-Core

[R2-2105323](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2105323.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2105323.zip) Correction on CrossCarrierSchedulingConfig Introduced by Two PUCCH Group CATT CR Rel-15 38.331 15.13.0 2614 - F NR\_newRAT-Core

[R2-2105324](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2105324.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2105324.zip) Correction on CrossCarrierSchedulingConfig Introduced by Two PUCCH Group CATT CR Rel-16 38.331 16.4.1 2615 - A NR\_newRAT-Core

### 3.2.2 Clarification of recurrence in RateMatchPattern

In the field description of *periodicityAndPattern* of the IE *RateMatchPattern*, it is stated that the default value for the periodicity is 14 symbols. However, this is not in line with the referenced 38.214 specification where different values of *symbolsInResourceBlock*, i.e. 1 or 2 slots are captured separately. In addition, the slot length is 14 symbols only for NCP is 12 symbols for ECP. Therefore, it will be better just to refer to 38.214 where the pattern is described clearly in more detail.

**Question 2**: Do you agree with the proposed change, by removing the text regarding how the pattern repeats itself when *periodicityAndPattern* is not configured

|  |  |  |
| --- | --- | --- |
| Answers to Question 2 | | |
| Company | Yes/No | Comments |
| QCOM | Yes | Proponent aligning the 38.331 with the 38.214. |
| MediaTek | Yes |  |
| ZTE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 2**: TBD.

**Proposal 2**: TBD.

### 3.2.3 Correction on CrossCarrierSchedulingConfig

The CR captures the network restriction (based on 38.213 spec) that is not allowed to configure cross carrier scheduling cross different PUCCH groups.

**Question 3**: Do you agree with addition of this restriction into the 38.331 spec.

|  |  |  |
| --- | --- | --- |
| Answers to Question 3 | | |
| Company | Yes/No | Comments |
| QCOM | Yes | The change is aligned with our understanding of the spec. |
| MediaTek | Yes |  |
| ZTE | Yes | The CRs are fine to us. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 3**: TBD.

**Proposal 3**: TBD.

## 3.3 Processing Time

The CRs related to this topic are:

[R2-2105767](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2105767.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2105767.zip) RRC processing time for Scell modification Ericsson, Nokia, Nokia Shanghai Bell discussion Rel-15 NR\_newRAT-Core

[R2-2105950](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2105950.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2105950.zip) Correction for RRC Resume latency requirements Huawei, HiSilicon CR Rel-15 38.331 15.13.0 2656 - F NR\_newRAT-Core

[R2-2105951](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2105951.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2105951.zip) Correction for RRC Resume latency requirements Huawei, HiSilicon CR Rel-16 38.331 16.4.1 2657 - A NR\_newRAT-Core

### 3.3.1 RRC processing time for SCell modification

In the last RAN2#113-bis-e meeting, it was discussed on whether the RRC processing delay requirement for the SCell modification should be changed from 10ms to 16ms. However, no consensus has been reached and the discussion has been postponed.

This discussion paper shared the following observations:

[Observation 1 As in LTE, the processing delay requirement for the SCell modification is considered as the same of a simple](#_Toc71294077) *[RRCReconfiguration](#_Toc71294077)* [message (i.e., 10ms).](#_Toc71294077)

[Observation 2 Changing the RRC processing delay for the SCell modification from 10ms to 16ms is a NBC change.](#_Toc71294078)

[Observation 3 RAN4 does not define any specific UE requirement for the SCell modification procedure.](#_Toc71294079)

[Observation 4 The RRC segmentation was introduced in Rel-16 to address the case (among the others) of a large RRC reconfiguration message.](#_Toc71294080)

[Observation 5 Changing the RRC processing delay for the SCell modification from 10ms to 16ms only in Rel-16 it will result in different implementations and this is not desirable.](#_Toc71294081)

Therefore the discussion paper proposes:

[P 1 RAN2 confirms that the RRC processing delay for the SCell modification is 10ms.](#_Toc71294082)

**Question 4**: do you agree with the observations made? if not, please provide your comment accordingly.

|  |  |  |
| --- | --- | --- |
| Answers to Question 4 | | |
| Company | Yes/No | Comments on the observations |
| QCOM | Neutral | We don’t have a strong opinion, but we would like to make a few points:   * Not sure why we need match the NR performance to LTE, when in many places we defined different behaviour for LTE and NR * When claiming that the change of the processing delay from 10 ms to 16 ms is an NBC, it seems a bit over-stretched claim, as sending UL grant when no UL data is available yet, won’t break the system (may be inefficient) and UE can still SR to request UL grant a at later point. |
| MediaTek | Partial | We think observation 2 on NBC is not so correct. But in general we don’t have too strong opinion. |
| ZTE | Partial | We think changing the delay from 10ms to 16ms can’t cause NBC issue, but if there is no issue found in field, we suggest not to change spec. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 5**: do you agree with the P1? And if not, please provide your comment accordingly.

|  |  |  |
| --- | --- | --- |
| Answers to Question 5 | | |
| Company | Yes/No | Comments on the P1 |
| QCOM | Neutral | Will go with majority |
| MediaTek | Yes | But no need to have any agreement or SPEC change. There is no proposal to change the processing time in this meeting. |
| ZTE | Yes | There is no need to change spec. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 4**: TBD.

**Proposal 4**: TBD.

### 3.3.2 Correction for RRC Resume latency requirements

RAN2 have agreed to reuse LTE approach to reduce RRC resumption processing delay requirement in RAN2 #105. In addition, RAN2 also agrees that PDCP/RLC entity corresponding to SRB2/DRB(s) shall be re-established after RRC reestablishment or resumption, just like LTE. in NR an explicit indication is needed to establish the RLC/PDCP (unlike the LTE where entities are implicitly established) by introducing the flag in RB config and RLC bearer config.

Subsequently, there is a need to explicitly adding in the notes that the reestablishPDCP and reestablishRLC flags will be included during Resume procedure and this will not impact the 6 ms delay requirements for the for a UE supporting reduced CP latency.

**Question 6**: do you agree with the proposed changed ? And if not, please provide your comment accordingly.

|  |  |  |
| --- | --- | --- |
| Answers to Question 6 | | |
| Company | Yes/No | Comments |
| QCOM | Yes | Aligned with our understanding |
| MediaTek | Yes |  |
| ZTE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 5**: TBD.

**Proposal 5**: TBD

## 3.4 Deprioritisation

The CRs related to this topic are:

[R2-2106182](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106182.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106182.zip) Clarification on the frequency deprioritisation Huawei, HiSilicon, China Unicom CR Rel-15 38.331 15.13.0 2674 - F NR\_newRAT-Core

Chair: Same issue as IPA R2-2106300/6308 but a different change. If agreeable determine if separate CRs.

[R2-2106183](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106183.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106183.zip) Clarification on the frequency deprioritisation Huawei, HiSilicon, China Unicom CR Rel-16 38.331 16.4.1 2675 - A NR\_newRAT-Core

Adding a note in the 38.331 spec to clarify that when a frequency is configured with both absolute priority and deprioritisation, deprioritisation will override absolute priority. In addition the note specifying these points:

1. The deprioritisation will not be deleted when the UE enters RRC connected state
2. The deprioritisation will not be deleted when the UE enters another RAT

**Question 7**: do you agree with the change?

|  |  |  |
| --- | --- | --- |
| Answers to Question 7 | | |
| Company | Yes/No | Comments |
| QCOM | Yes but | We agree with the intention of the change, as similar topic was discussed in the previous meeting.  If CR was agreed, we would like to have a slight modification to the note:  *NOTE: The UE* *stores the deprioritisation request irrespective of any cell reselection absolute priority assignments (by dedicated or common signalling) and regardless of the serving cell if it is NR or other RATs unless specified otherwise.*  in addition, I would like to know what is the intention behind this clause? |
| MediaTek | Yes | And we think original wording is okay as it aligned with LTE wording. The yellow highlighted part is not used for now but there is no harm to keep it. |
| ZTE | Yes | This modification is aligned with LTE spec. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 8**: if you agree with the CR, is there a need for a separate CR, given a similar CR that carries the same intention was “in principle agreed” during the last meeting (R2-2106300/6308)?

|  |  |  |
| --- | --- | --- |
| Answers to Question 8 | | |
| Company | Yes/No | Comments |
| QCOM | Neutral | Will go with the majority |
| MediaTek | No | We prefer to just have single CR to address same issue. |
| ZTE | Neutral | Will go with the majority. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 6**: TBD.

**Proposal 6**: TBD.

## 3.5 Other

The CRs related to this topic are:

[R2-2106178](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106178.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106178.zip) OverheatingIndicationProhibitTimer for SCG in (NG)EN-DC Qualcomm Incorporated CR Rel-15 38.331 15.13.0 2672 - F NR\_newRAT-Core

[R2-2106179](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106179.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106179.zip) OverheatingIndicationProhibitTimer for SCG in (NG)EN-DC Qualcomm Incorporated CR Rel-16 38.331 16.4.1 2673 - A NR\_newRAT-Core

This CR clarifies that the prohibit timer (in the 38.331 spec) can’t be used to configure the NR SCG in (NG)EN-DC, and for the (NG)EN-DC case, the prohibit timer for overheating is only configured by the MN eNB. Therefore a clarification was added to the “overheatingIndicationProhibitTimer” field description that this timer is not used in (NG)EN-DC.

**Question 9**: Do you agree with the proposed changed? Please provide comment if needed.

|  |  |  |
| --- | --- | --- |
| Answers to Question 9 | | |
| Company | Yes/No | Comments |
| QCOM | Yes | Proponent  As per the current 38.331 spec, nothing prevents the network from configuring this overheating prohibit timer for the NR NCG while UE is in (NG)EN-DC.  **This CR is aligned with the previous effort to clarify the overheating parameters (e.g. reducedCCsDL/ reducedCCsUL) and their usage with EN-DC vs NR-DC** |
| MediaTek | No | This is related to the overheating of SCG feature introduced in TEI-16. So, R15 change is not necessary.The IE *OtherConfig* is not included in SN (NR) RRC message at all in R15.  In R16, for SCG, IE *OtherConfig* could be used for some configuration, but the field *overheatingAssistanceConfig* should not be present. This is captured in the following description.  ***otherConfig***  Contains configuration related to other configurations. When configured for the SCG, only fields *drx-PreferenceConfig, maxBW-PreferenceConfig, maxCC-PreferenceConfig, maxMIMO-LayerPreferenceConfig*, *minSchedulingOffsetPreferenceConfig, btNameList, wlanNameList, sensorNameList* and *obtainCommonLocation* can be included. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 7**: TBD.

**Proposal 7**: TBD.

## 3.6 L2 Parameter

The CRs related to this topic are:

[R2-2106077](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106077.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106077.zip) Correction on flow remapping to an added DRB Sequans Communications CR Rel-15 38.331 15.13.0 2666 - F NR\_newRAT-Core

[R2-2106079](file:///D:\\Documents\\3GPP\\tsg_ran\\WG2\\TSGR2_114-e\\Docs\\R2-2106079.zip" \o "D:Documents3GPPtsg_ranWG2TSGR2_114-eDocsR2-2106079.zip) Correction on flow remapping to an added DRB Sequans Communications CR Rel-16 38.331 16.4.1 2667 - A NR\_newRAT-Core

The CR clarifies that since a QFI value can be included at most once across configured instances of *SDAP-Config* with the same value of *pdu-Session,* the network cannot perform direct remapping to an added DRB, unless the old DRB is released. Therefore the CR add the removal of the QFI from the old DRB in case of flow remapping to a newly added DRB.

**Question 10**: do you agree with the CR? Please provide comment if needed.

|  |  |  |
| --- | --- | --- |
| Answers to Question 10 | | |
| Company | Yes/No | Comments |
| QCOM | Neutral | We don’t think the CR is needed, but we will go with the majority. |
| MediaTek | Yes | Not sure why the change is missing in DRB Add part but anyway it seems aligned with the original intention. |
| ZTE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 8**: TBD.

**Proposal 8**: TBD.

# 4 Discussion Phase 2

TBD.

# 5 Conclusion

TBD.