**3GPP TSG-RAN WG2 Meeting #115-e R2-210xxxx**

**Online, Aug 16th – 27th, 2021**

**Agenda Item: 6.1.4.3**

**Source: Huawei, HiSilicon**

**Title: Summary of [AT115-e][028][NR16] UE capabilities I**

**Document for: Discussion and decision**

# Introduction

This document summarizes the following offline discussion.

* [AT115-e][028][NR16] UE capabilities I (Huawei)

Scope: Determine agreeable parts and agree CRs, Treat R2-2108480, R2-2107342, R2-2108641, R2-2108468, R2-2108585, R2-2108586, R2-2108651, R2-2106952, R2-2108618, R2-2108619, R2-2108735, R2-2108736

Intended outcome: Report, Agreed CRs.

Deadline: Schedule 1

# Contact from companies

|  |  |
| --- | --- |
| Company | Email |
| Huawei, HiSilicon | Yiru Kuang, kuangyiru@huawei.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Discussion

## Part 1: Intended to determine agreeable parts

### **Misc Corrections**

[R2-2108480](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108480.zip) Miscellaneous corrections to UE capability descriptions Lenovo, Motorola Mobility CR Rel-16 38.306 16.5.0 0626 - F NR\_unlic-Core, TEI16

The proposed changes in above CR include:

1. offsetSRS-CB-PUSCH-PDCCH-MonitorAnyOccWithGap-fr1-r16: The description of the conditional support of pdcch-MonitoringAnyOccasions with value withDCI-Gap (FG 3-5a) has been added.

2. searchSpaceSetGroupSwitchingwWithDCI-r16: The capability name has been replaced by searchSpaceSwitchWithDCI-r16.

3. extendedSearchSpaceSwitchWithDCI-r16: It has been clarified that UE indicating support of this feature shall indicate support of searchSpaceSwitchWithDCI-r16.

4. Number of editorial issues have been fixed (missing suffices, misalignment of parameter names with TS 38.331 etc.).

**Q1 Do companies agree with the intention of the CR above?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments** |
| Huawei, HiSilicon | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### **DAPS**

[R2-2107342](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2107342.zip) Correction on the capability field DiffSCS-DAPS Huawei, HiSilicon discussion Rel-16 NR\_Mob\_enh-Core

[R2-2108641](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108641.zip) Correction on the capability field DiffSCS-DAPS Huawei, HiSilicon CR Rel-16 38.306 16.5.0 0636 - F NR\_Mob\_enh-Core

The proposal in above discussion paper is listed below. The above CR includes the corresponding change.

Proposal 1: for the two capability fields, i.e. intraFreqDiffSCS-DAPS-r16 and interFreqDiffSCS-DAPS-r16, add clarification that “In this release the UE shall not report this UE capability”.

**Q2 Do companies agree with the intention of Proposal 1 and CR above?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments** |
| Huawei, HiSilicon | Yes | Proponent. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### **eMIMO**

[R2-2108468](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108468.zip) Correction to ul-FullPwrMode capability Sequans Communications CR Rel-16 38.306 16.5.0 0625 - F NR\_eMIMO-Core

The proposed change in above CR includes: removing the misleading reference “fullpower as specified in clause 6.1.1.1 of TS.38.214 [12]” for *ul-FullPwrMode-r16*.

**Q3 Do companies agree with the intention of the CR above?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments** |
| Huawei, HiSilicon | Yes | Editorial change. Minor change, can be merged to e.g. Misc Corrections in [1]. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### **IIOT**

[R2-2108585](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108585.zip) Correction on PDCCH Blind Detection in CA Huawei, HiSilicon CR Rel-16 38.331 16.5.0 2781 - F NR\_IIOT-Core

[R2-2108586](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108586.zip) Correction on PDCCH Blind Detection in CA Huawei, HiSilicon CR Rel-16 38.306 16.5.0 0634 - F NR\_IIOT-Core

The proposed changes in above CRs include: To allow UE to report more than one combinations of pdcch-BlindDetectionCA1-r16 capability and pdcch-BlindDetectionCA2-r16 capability, add a list of elements of SEQUENCE type except for *pdcch-BlindDetectionCA-Mixed-r16* IE and *pdcch-BlindDetectionCA-Mixed-NonAlignedSpan-r16* IE.

**Q4 Do companies agree with the intention of the CRs above?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments** |
| Huawei, HiSilicon | Yes | Proponent. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### **UL Skipping**

[R2-2108651](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108651.zip) FR1FR2 differentiation for enhanced UL grant skipping capabilities Qualcomm Incorporated, Nokia, Nokia Shanghai Bell discussion Rel-16 TEI16

The proposal in above discussion paper is listed below. The above CR includes the corresponding change.

Proposal 1: RAN2 to discuss and decide on an approach to modify the current specification to allow FR differentiation

Proposal 2: RAN2 to introduce a new capability IE to allow frequency range differentiation. 2 options are proposed:

• Option-A: new capability is defined per nr-bands, to allow full flexibility for the UE to indicate the supported duplex mode and frequency range combination.

• Option-B: new TDD only capability with frequency range differentiation. Both, current and new IE may be used by the UE to convey its capability to the network.

Proposal 3: to have one of the proposed changes in section 4 &5 or 6&7 agreed.

**Q5 Do companies agree to modify the current specification to allow FR differentiation for *enhancedSkipUplinkTxConfigured-r16* and *enhancedSkipUplinkTxDynamic-r16*? If yes, which option above do companies prefer?**

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Yes or No** | **Option-A or B?** | **Comments** |
| Huawei, HiSilicon | No | Option-A if CR is agreed to pursue | In RAN2#113 meeting, this issue has been discussed in offline 019 and the conclusion is no need of FR1/FR2 differentiation, we don’t see strong motivation to revert the previous conclusion.  If majority of companies prefer to introduce this now, we would prefer Option-A which is more aligned with our Rel-16 principle for FRx/xDD capability design. |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

### **UL TX Switching**

[R2-2106952](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2106952.zip) LS on UL MIMO coherence for Tx switching between two carriers (R4-2107765; contact: China Telecom) RAN4 LS in Rel-16 NR\_RF\_FR1-Core To:RAN2, RAN1

[R2-2108618](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108618.zip) Adding UE capability of UL MIMO coherence for UL Tx switching Huawei, HiSilicon, China Telecom, Apple CR Rel-16 38.306 16.5.0 0635 - F NR\_RF\_FR1-Core

[R2-2108619](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108619.zip) Adding UE capability of UL MIMO coherence for UL Tx switching Huawei, HiSilicon, China Telecom, Apple CR Rel-16 38.331 16.5.0 2786 - F NR\_RF\_FR1-Core

[R2-2108735](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108735.zip) Introducing UL MIMO coherence capability for Tx switching ZTE Corporation, Sanechips CR Rel-16 38.306 16.5.0 0638 - F NR\_RF\_FR1-Core

[R2-2108736](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2108_R2_115-e/Docs/R2-2108736.zip) Introducing UL MIMO coherence capability for Tx switching ZTE Corporation, Sanechips CR Rel-16 38.331 16.5.0 2796 - F NR\_RF\_FR1-Core

The intention of CRs in [9][10] and [11][12] is the same, i.e. adding new per-BC capability *uplinkTxSwitching-PUSCH-TransCoherence-r16* based on LS R2-2106952. The main difference between CRs in [9][10] and [11][12] is the value of *uplinkTxSwitching-PUSCH-TransCoherence-r16*.

**Q6-1 Do companies agree with the intention of the CRs above, i.e. adding a new per-BC UE capability *uplinkTxSwitching-PUSCH-TransCoherence-r16*?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments** |
| Huawei, HiSilicon | Yes | Proponent of CRs [9][10]. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Option 1: The value set is: ENUMERATED {nonCoherent, partialCoherent, fullCoherent}

Option 2: The value set is: ENUMERATED {nonCoherent, coherent}

**Q6-2 if the answer for Q6-1 is yes, which option above do companies prefer?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option1 or 2?** | **Comments** |
| Huawei, HiSilicon | Option1 | The basic idea of option1 is to copy the value set of existing MIMO capability pusch-TransCoherence without change, in order to make sure the RAN1 spec related to the handling of pusch-TransCoherence can also applied to this new UE capability without any change. Regarding ‘fullCoherent’ in option1 v.s. ‘coherent’ in option2, the thing to be clarified is in RAN4 CR R4-2109582 the value of ‘coherent’ is used, but after checking with RAN4 colleague it actually meant ‘fullcoherent’, and RAN4 CR can be updated based on RAN2 agreed value set. Regarding ‘partialCoherent’, although we notified the value of partialCoherent will not be used for 2Tx UE, considering future-proof and spec maintenance we copied it here. But no strong view, we can follow majority views on whether to include partialCoherent or not. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusions

*To be added…*

# References

1. R2-2108480 Miscellaneous corrections to UE capability descriptions Lenovo, Motorola Mobility CR Rel-16 38.306 16.5.0 0626 - F NR\_unlic-Core, TEI16
2. R2-2107342 Correction on the capability field DiffSCS-DAPS Huawei, HiSilicon discussion Rel-16 NR\_Mob\_enh-Core
3. R2-2108641 Correction on the capability field DiffSCS-DAPS Huawei, HiSilicon CR Rel-16 38.306 16.5.0 0636 - F NR\_Mob\_enh-Core
4. R2-2108468 Correction to ul-FullPwrMode capability Sequans Communications CR Rel-16 38.306 16.5.0 0625 - F NR\_eMIMO-Core
5. R2-2108585 Correction on PDCCH Blind Detection in CA Huawei, HiSilicon CR Rel-16 38.331 16.5.0 2781 - F NR\_IIOT-Core
6. R2-2108586 Correction on PDCCH Blind Detection in CA Huawei, HiSilicon CR Rel-16 38.306 16.5.0 0634 - F NR\_IIOT-Core
7. R2-2108651 FR1FR2 differentiation for enhanced UL grant skipping capabilities Qualcomm Incorporated, Nokia, Nokia Shanghai Bell discussion Rel-16 TEI16
8. R2-2106952 LS on UL MIMO coherence for Tx switching between two carriers (R4-2107765; contact: China Telecom) RAN4 LS in Rel-16 NR\_RF\_FR1-Core To:RAN2, RAN1
9. R2-2108618 Adding UE capability of UL MIMO coherence for UL Tx switching Huawei, HiSilicon, China Telecom, Apple CR Rel-16 38.306 16.5.0 0635 - F NR\_RF\_FR1-Core
10. R2-2108619 Adding UE capability of UL MIMO coherence for UL Tx switching Huawei, HiSilicon, China Telecom, Apple CR Rel-16 38.331 16.5.0 2786 - F NR\_RF\_FR1-Core
11. R2-2108735 Introducing UL MIMO coherence capability for Tx switching ZTE Corporation, Sanechips CR Rel-16 38.306 16.5.0 0638 - F NR\_RF\_FR1-Core
12. R2-2108736 Introducing UL MIMO coherence capability for Tx switching ZTE Corporation, Sanechips CR Rel-16 38.331 16.5.0 2796 - F NR\_RF\_FR1-Core