3GPP TSG-RAN WG2 Meeting #115-e Tdoc R2- 210XXXX

Electronic Meeting, Aug 16th - 27th, 2021

Agenda Item: 9.2.4.1

Source: Ericsson

Title: Summary of AI 9.2.4.1 “TA and Mobility related” (Ericsson) - Ph2

Document for: Discussion, Decision

# 1 Introduction

In RAN#86, a SI was approved to determine and evaluate the minimum necessary specification updates to introduce NB-IoT/eMTC support for non-terrestrial networks (NTN), The description for the SI was updated in RAN#90 [1] and it was agreed to use the existing work on NR NTN captured in TR 38.821 [2] as a baseline. In RAN#92-e, a follow up WI was approved to specify NB-IoT/eMTC support for Non-Terrestrial Networks.

In R2-2109003, we summarized the contributions, submitted to the AI 9.2.4.1, on tracking area update and mobility mechanisms for NB-IoT and LTE-M devices in NTN. That document has been treated during the online session and a set of agreements have been made.

This document is to continue the discussion based on what has been agreed during the online session and rapporteur’s suggestions per topic on which proposals to continue the discussion with as given below:

**Idle mode mobility**

**Proposal 3**         Discuss whether satellite assistance information, e.g., ephemeris, for neighbour cell(s) is provided to UE.

**Proposal 7**          Discuss whether cell selection procedure is used instead of cell reselection procedure when a UE is configured with an eDRX cycle.

**Tracking area update**

**Proposal 16**       Discuss whether system information modification notification procedure is used to inform TAC updates and, if not, discuss the alternative mechanisms.

**Connected mode mobility**

**Proposal 23**       Discuss whether value range for parameter t304 needs to be extended. The values to be specified, if necessary, are FFS.

**Proposal 19**       Discuss whether RAN2 should check with RAN4 on the RRM impacts for supporting CHO and related measurements for LTE-M.

**Proposal 27**       Discuss whether UE specific timers and constants for RLF and RRC connection re-establishment procedure require any changes.

# 2 Discussion

### 2.1 Idle mode mobility

In RAN2#113-e, the following agreement was made: “The NTN ephemeris is divided into serving cell’s ephemeris and neighbour’s ephemeris. FFS how would they differ regarding e.g., the required accuracy or signalling impact.” Proposal 3, above, was briefly discussed, via emails, during Ph1, but some companies commented that it is not clear what such information, i.e., satellite assistance information, would be beneficial for at this point. Rapporteur thinks the intention is to have a similar agreement as in NR NTN and satellite assistance information for neighbour cells, in-line with what is to be provided for the serving cell, can be used for example to decide when to perform measurement on neighbour cells. Satellite assistance information for a neighbour cell can be subject of a discussion on whether it would be beneficial for estimating discontinuous coverage, but rapporteur thinks this is not within the context of this offline discussion. With the question below rapporteur would like to check if a reformulated version of **Proposal 3** above reflecting the intention better is acceptable to companies.

**Question 1: Do you think RAN2 should assume that satellite assistance information for neighbour cell(s) is provided to UE for cell selection/reselection?**

**Please note the following agreement for the serving cell “RAN2 assumes that satellite assistance information, e.g., for cell selection reselection, for serving cell is provided to UE” and that discontinuous coverage is not within the context of this discussion.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| MediaTek | No | Given the limited TU budget for this WI in R-17, we don’t think such optimizations are essential in the first release. We can consider it in Rel-18. |
| Lenovo | No | For continuous coverage we see no urgent necessity to introduce new mechanism for idle mode mobility. |
| Qualcomm | Maybe | Unless UE is provided information that which neighbor cells are out-going (no need to search) and which are good to search, neighbor satellite information can be useful. |
| Huawei, HiSilicon | No | This would be an optimisation and not critical for Rel-17 |
| CATT | No | It is unnecessary to introduce this mechanism in Rel-17. |
| OPPO | Yes | Similar to NR NTN, the timing information on when a cell is going to stop serving the area as well as the timing information on when a cell is going to start serving the area are needed to assist cell reselection in IoT NTN for earth fixed scenario and can be used to decide when to perform measurement on neighbor cells. |
| Xiaomi | No | We can discuss it later when the ephemeris data is decided. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 2: Do you think cell selection procedure should be used instead of cell reselection procedure when a UE is configured with an eDRX cycle?**

**If yes, please indicate whether the statement above should apply to any eDRX cycle or eDRX cycles with lengths above certain values.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| MediaTek | Yes | The eDRX cycle length does not matter, as the UE will know from the serving cell ephemeris whether it is going to be served by the same cell, when it wakes up. Based on this information the UE can decide whether to perform cell selection or not. |
| Lenovo | Yes with comments | If ephemeris is provided, UE can predict which cell will be serving when it wakes up. Cell selection can be used to replace reselection or not depending on the result.  So it could be “cell selection procedure **can** be used instead of cell reselection procedure…”. |
| Question | No | This is not clear what would be impact of this in specification. |
| Huawei, HiSilicon | No | We are also not clear what would be the impact on the specification. In general, already today, the UE performs cell selection when it wakes up and its serving cell is no longer there. |
| CATT | Yes | If UE is configured with eDRX cycle, the UE may already move into a new cell’s coverage when it wakes up, hence it had better perform cell selection instead of cell reselection. |
| OPPO | No | It is not clear what the spec impact is. |
| Xiaomi | No | UE can decide to perform cell selection or cell reselection based on UE implementation. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.2 Tracking area update

In RAN2#114-e, the following agreement was made for NR-NTN: “Change in TAC in SIB1 triggers SI update notification procedure as legacy behaviour. It is FFS whether broadcasting TAC update time can also be considered” In Ph1, rapporteur stated that one company [13] proposed using the legacy system information update notification mechanism to inform about the TAC update whereas three companies, [7] [8] [17], proposed not to use that procedure due to its impact on UE power consumption.

**Question 3: Do you think system information modification notification procedure should be used to inform TAC updates?**

**Please state the rationale for your reply regardless of whether you replied yes/no considering the arguments provided in the references given above.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| MediaTek | No | This is not essential and should be avoided as there is a chance of higher power consumption. If the UE changes its tracking area, it will anyway issue a TAU on cell reselection. |
| Lenovo | No | TAU mechanism is sufficient for now. |
| Qualcomm | No | Paging resource cannot be used for this purpose in LTE. |
| Huawei, HiSilicon | No | We do not think it can work in NB-IoT considering the large BCCH modification period (minimum 40.96 s). We also agree with Mediatek that TAU will solve any problem. |
| CATT | No | It can based on the legacy TAU mechanism. |
| OPPO | Yes | We can reuse the conclusion in NR NTN. It is not clear to us why above companies stated that the legacy TAU procedure is sufficient to handle this. We understand that for triggering TAU, UE needs to know the TAC broadcasted by the NW has been updated. Then how can UE initiate TAU if NW does not notify the TAC change to the UEs? |
| Xiaomi | Yes, but | If other companies think the system information notification procedure is not suitable，we can go along with the majority. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In [8] and [17] alternative mechanisms have been proposed to inform TAC updates.

**Question 4: If RAN2 agrees that system information modification notification procedure should NOT be used to inform TAC updates; do you think time information about TAC updates should be broadcast?**

**Please consider the mechanism proposed in [8] on a high level when you reply. Note that the details may be discussed separately, if needed, depending on the support.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| MediaTek | No | We think such optimizations can be done in later releases, after a working solution is made. If the UE changes its tracking area, it will anyway issue a TAU on cell reselection. |
| Lenovo | No | TAU mechanism is sufficient for now. |
| Qualcomm | Yes | This is agreement:   * When the network stops broadcasting a TAC, the UE needs to know it. FFS how this is done.   There should be some mechanism other than paging for UE to know when network stops this (doing nothing is not agreement).  eMTC and NB-IoT UEs support H-SFN, UTC time information is not the talk of this question. |
| Huawei, HiSilicon | No | TAU is sufficient |
| CATT | No | Same view as Lenovo. |
| OPPO | No | Same as NR-NTN, this can be handled by SI modification procedure. |
| Xiaomi | No | Maybe the existing TAU is sufficient. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 5: If RAN2 agrees that system information modification notification procedure should NOT be used to inform TAC updates; do you think that UE should ignore the notification if it is for TAC update and the UE is “stationary”?**

**Please consider the mechanism proposed in [17] on a high level when you reply. Note that the details may be discussed separately, if needed, depending on the support.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| MediaTek | Yes | Stationary UEs can ignore the notifications and if the UE changes its tracking area, it will anyway issue a TAU on cell reselection. |
| Lenovo | Yes |  |
| Qualcomm | No (question not clear) | If there is no SI modification notification, then how does UE know it is for TAC update? Existing notification does not indication TAC update and we have not introduced any new one. |
| Huawei, HiSilicon | No (do not understand the question) | We assume the question is in the case RAN2 agrees that SI update notification procedure is used to inform TAC change, otherwise it does not make sense  First we do not think SI notification procedure should be used as per Q4. Then, we think it may not be possible for the UE to know that the paging is for SI update (e.g. in case there is a message paging and thus direct information indication cannot be used) |
| CATT | See comment | We are confused that “If system information modification notification procedure should not be used to inform TAC update”, why there is “notification for TAC update”? How to understand it? |
| OPPO | No (question not clear) | If there is no SI modification notification, which notification should UE ignore? |
| Xiaomi | Yes | It UE is stationary, it should assume the TAC broadcasted by network would not be changed. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.3 Connected mode mobility

In [18], it was discussed whether value range for parameter *t304* needs to be extended. In Rel-13 an extended value, i.e., *ms10000-v1310* was introduced for UEs that support CE with the intention to cover cases where the UE is in enhanced coverage. Now that adaptation for NTN is specified, new values for this timer can be considered to compensate for propagation delay due to satellites

**Question 6: Do you think that value range for parameter *t304* needs to be extended to compensate for propagation delay due to satellites?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| MediaTek | Yes | The value range can be increased to accommodate the NTN RTT for eMTC. |
| Lenovo | No | We think the current value range is sufficient to cover UE-eNB RTT. |
| Qualcomm | No | 10s seems sufficient. If it means other smaller values with different granularities, then please clarify. |
| CATT | No | 1000ms is sufficient. |
| OPPO | No | 10s is sufficient. |
| Xiaomi | No | The maximum value of T304 is 10000ms, which is sufficient and much larger than the RTT between UE and gNB. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In [10], it is proposed that RAN2 should check with RAN4 on the RRM impacts for supporting CHO and related measurements for LTE-M.

**Question 7: Do you think RAN2 should check with RAN4 on the RRM impacts for supporting CHO and related measurements for LTE-M?**

**Please state the rationale for your reply regardless of whether you replied yes/no considering the arguments provided in the reference given above.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| MediaTek | Yes | We think RAN4 should be involved for considering RRM impacts of supporting CHO. |
| Lenovo | Yes | RAN4 can be informed if necessary. |
| Qualcomm | Yes | RAN4 should also add LTE-M devices in the CHO section. |
| Huawei, HiSilicon | Yes | RAN4 should not only check the impact and feasibility but introduce the corresponding requirements for CE-Mode A and CE-ModeB if both modes are supported. |
| CATT | Yes |  |
| OPPO | Yes |  |
| Xiaomi | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

During the online session, some companies indicated that more time is needed to check whether procedural update is required to support RLF and RRC connection re-establishment procedures in IoT NTN. Since there was no time to bring it up online, the rapporteur would like to check whether UE specific timers and constants for RLF and RRC connection re-establishment procedure require any changes, i.e., value range or behaviour, in IoT NTN.

**Question 8: Do you think that UE specific timers and constants for RLF and RRC connection re-establishment procedures require extended value range and/or new behaviour in IoT NTN?**

**Please state the rationale for your reply regardless of whether you replied yes/no and, if yes, provide the names of the timers and constants that you think which may require change.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| MediaTek | - | We think such UE specific timers need to be identified first, before considering their extension. |
| Lenovo | Yes | The triggering and recovery of RLF may bring additional delay and power consumption in NTN due to LEO movement or link switch. For NB-IoT mobility a more straightforward way is to use the conditional concept as CHO for NR NTN, i.e. conditional RRC re-establishment.  This can be implemented by introducing a timer or indicating a time so that UE can initiate RRC reestablishment to target cell at a given time, instead of triggering RLF and attempting recovery. |
| Qualcomm | Maybe | Extension of timers can be done if identified necessary. Agree with MediaTek. |
| Huawei, HiSilcon | probably no | This should be discussed in a per timer basis and separately for NB-IoT and eMTC as the value ranges may be different.  In general, in NB-IoT, the timers can already be very large and likely to be sufficient.  We may need to check RRC Connection Re-establishment in discontinuous coverage, but this is probably not critical for Rel-17 |
| CATT | See comments | Agree with MediaTek, the timers should be identified first. |
| OPPO | - | Agree with MediaTek. |
| Xiaomi | Maybe | Agree with MediaTek, we should identify the UE specific timers and constants first.  If it is necessary, extended value range and/or new behavior can be considered. For different UE specific timers and constants, we need to discuss the issue separately. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Summary

TBD

# 3 Conclusion

This document is to continue the discussion based on what has been agreed during the online session and rapporteur’s suggestions per topic on which proposals to continue the discussion with. Based on the discussion in the section above the following proposals are made:

[Proposal 1 ???.](#_Toc80614972)

# References

1. [1] R2-2108328 Mobility enhancement for IoT-NTN NEC Telecom MODUS Ltd.
2. [2] R2-2107083 Discussion on CP impact for IoT over NTN OPPO
3. [3] R2-2107084 Discussion on idle mode procedures for IoT over NTN OPPO
4. [4] R2-2107321 Discussion on connected mode UE of IoT NTN CATT
5. [5] R2-2107322 Discussion on IDLE mode UE of IoT NTN CATT
6. [6] R2-2107371 Discussion on the issue of mobility for IoT over NTN Spreadtrum Communications
7. [7] R2-2107426 TA and mobility for IOT NTN Huawei, HiSilicon
8. [8] R2-2107562 TAC update procedure Qualcomm Incorporated
9. [9] R2-2107767 Mobility issues of IoT NTN ZTE Corporation, Sanechips
10. [10] R2-2107813 Analysis on mobility aspects for IoT-NTN Nokia, Nokia Shanghai Bell
11. [11] R2-2107916 Considerations on NB-IoT mobility for IoT NTN Lenovo, Motorola Mobility
12. [12] R2-2108018 Discussion on connected mode mobility for IoT NTN Xiaomi
13. [13] R2-2108172 Discussion on TA and idle mode mobility enhancement Xiaomi
14. [14] R2-2108338 On Cell Re-selection in IoT-NTN MediaTek Inc.
15. [15] R2-2108339 On Improving Tracking Area Updates in IoT NTN MediaTek Inc.
16. [16] R2-2108546 Enhanced RRC re-establishment for mobility in IoT-NTN CMCC
17. [17] R2-2108548 Discussion on TA Update for IoT-NTN CMCC
18. [18] R2-2108757 Mobility for NB-IoT and LTE-M in NTN Ericsson