3GPP TSG-RAN WG2 Meeting #115 Electronic R2-210xxxx

Online Meeting, August 16th – 27th 2021

**Agenda item: 8.11.1**

**Source: CATT**

**Title: [AT115-e][612][POS] Reply LS to SA2 on scheduled location time (CATT)**

**WID/SID: NR\_pos\_enh-Core**

**Document for: Discussion and Agreement**

# 1 Introduction

This document is to kick off the following email discussion:

* [AT115-e][612][POS] Reply LS to SA2 on scheduled location time (CATT)

Scope: Reply to the SA2 LS on scheduled location time, indicating RAN2 view on the latency benefit (to the extent agreement is possible) and understanding of RAN2 spec impact.

Intended outcome: Approvable LS in R2-2108943

Deadline: Tuesday 2021-08-24 0800 UTC

This email discussion continues to discuss the possible content for the Reply LS.

# 2 Contact Information

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
| ZTE | pan.yu24@zte.com.cn |
| Ericsson | Ritesh.shreevastav@ericsson.com |
| Xiaomi | lixiaolong1@xiaomi.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 References

1. R2-2107680 "Summary of agenda 8.11.2 Latency enhancements" Intel Corporation discussion Rel-17 NR\_pos\_enh
2. R2-2106968 Response LS on Scheduling Location in Advance to reduce Latency (S2-2105122; contact: CATT) SA2 LS in Rel-17 5G\_eLCS\_ph2 To:RAN2 Cc:RAN1, RAN3

# 4 Discussion

## 4.1 Benefit analysis

According to the Summary of agenda 8.11.2 [1] and RAN2 on-line discussion, most companies believe that the benefit of scheduled location time in terms of reducing LCS latency is mainly reflected in the preparation phase of the positioning procedure, i.e. The LMF can complete the capabilities and assistance Data transmission in advance before initiating the corresponding location measurement procedure. Some companies do not see the latency benefit in general. They think this is for a specialised use case where the preparation phase can be handled earlier, and they see more of a benefit in reliability/accuracy of the location estimate.

**Question 1: Do you agree that the benefit of scheduled location time in terms of reducing LCS latency is mainly reflected in the preparation phase of the positioning procedure？ Please share your comments here.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/ No | Comments |
| Qualcomm | Yes, with comments | With the scheduled location time, the effective response time or latency equals the duration of the location execution phase and excludes the duration of the location preparation phase which can be performed ahead of the scheduled location time. This can be used to reduce latency, as already described in the SA2 CR (S2-2102047).  But there are of course other benefits inherent to the user case/application (i.e., enabling a client to request a UE location for a specified time). |
| ZTE | Yes | The scheduled location time is to let LMF know the deadline of triggering positioning request/sending assistance data. |
| Ericsson | Yes, but | For preparation phase it can help to reduce the latency if client does not know what is the typical TTTF. If a client can learn how long does it takes for NW to provide TTFF then client can request ahead of that time; in this scenario the time T is not critical in terms of latency.  But yes, in terms of improving accuracy/reliability it is good to have. |
| Xiaomi | Yes | The LMF can trigger positioning preparation phase in advance when LMF has the scheduled location time. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In the execution phase of the positioning procedure, there are two views to be considered:

* Option 1: LMF can initiate the corresponding location measurement procedure at or close to the scheduled location time;
* Option 2: LMF can send the Scheduled Location Time to NG-RAN and UE in order to trigger measurements at or close to the scheduled location time;

According to the Summary of agenda 8.11.2 [1] and RAN2 on-line discussion, both of the two options can meet SA2's requirement that the LMF must obtain a current location of the UE at or close to the scheduled location time. However, the difference between the two options lies in whether the location information of the UE can be accurately reflected. So most companies think the scheduled location time does not provide more benefits in the reduction of the LCS latency during execution phase of the positioning procedure.

**Question 2: Do you agree that the scheduled location time does not provide more benefits in the reduction of the LCS latency during execution phase of the positioning procedure？ Please share your comments here.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/ No | Comments |
| Qualcomm | Yes, with comment | With the scheduled locaton time, the latency the client observes is the delay between the time of fix and when it is available to the client. With the scheduled location time the time of fix should be (ideally) T (as requested by the client), and the latency comprise the location measurement time and signalling delay to the client. Since there is no change to e.g., architecture and signalling involved, the signalling latency of the location execution phase does not change. |
| ZTE | Yes |  |
| Ericsson | Yes |  |
| Xiaomi | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary:**

## 4.2 Specification impact

With regard to the impact of specification, based on the Summary of agenda 8.11.2 [1], there are two options:

* Option A: The scheduled location time does not need to be indicated to the UE or NG-RAN, since the LMF can implicitly trigger the positioning procedures at or close to it. Therefore, it is transparent to UE/NG-RAN stage-3 positioning procedures.
* Option B: Latency reduction can be accomplished by sending the scheduled location time T to the UEs and TRPs in order to trigger measurements at or close to it. Therefore, LPP and/or Napa signaling needs to be updated to indicate this information.

It is mainly related to the discussion of the previous chapter, if the above Q2 can be confirmed by most companies, it can be assumed that from the specification impact point of view, the scheduled location time T is transparent to UE/NG-RAN stage-3 positioning procedures.

**Question 3: Do you agree that the scheduled location time T is transparent to UE/NG-RAN stage-3 positioning procedures？Please share your comments here.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/ No | Comments |
| Qualcomm | No | Without providing the Scheduled Location Time T to the UE and TRPs, the LMF cannot reliably determine the UE location at the scheduled location time, and therefore, the location estimate returned to an LCS Client for a scheduled location time cannot be treated by the LCS Client as a reliable estimate of the location of the UE at the scheduled location time.  With the current LPP specification, the time when the UE should obtain the measurements/location estimate cannot be controlled by an LMF. The available LPP Response Time defines the time when to send a measurement report (at the latest), but not the time when the location measurements should be obtained/valid. The measurements/location estimate may be valid anywhere within the response time, which for some positioning methods could be relatively large.  Providing the scheduled location time (with uncertainty/measurement window) to the UE/TRPs would allow an LMF to more reliably control/trigger the UE and TRP measurements at or close to the scheduled location time. |
| ZTE | Yes | Only LMF knows the scheduled location time is enough. LMF knows the deadline(scheduled location time) for preparation phase, then LMF will schedule the request and AD transfer before the deadline. UE/NG-RAN node will perform measurements subsequently without the guidance of scheduled location time. |
| Ericsson | Yes | Agree with ZTE. The global time T can be transparent to UE/NG-RAN. The measurement window can still be defined in local time instances (SFN, Slot Number) by the LMF. |
| Xiaomi | Yes | The LMF can trigger The LPP location information request and/or NRPPa measurement request at or near to the scheduled location time T and then the UE and/or gNB can perform positioning measurement at or near the scheduled location time. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 4.3 Discussion about draft Reply LS

Based on the previous discussion, we draft the following contents of the Reply LS：

**1. Overall Description:**

RAN2 would like to thank SA2 for the LS on scheduled location time.

RAN2 thinks that this is for a specialised use case where the preparation phase can be handled earlier, but the scheduled location time does not provide more benefits in the reduction of the LCS latency during execution phase.

In addition, from the specification impact point of view, the LMF can implicitly trigger the positioning procedures at or close to the time point. Therefore, it is transparent to UE / NG-RAN stage-3 positioning procedures.

**2. Actions:**

**To SA2:**

RAN2 respectfully requests SA2 to take the above information into account.

**3. Date of Next RAN2 Meetings:**

TSG-RAN2 Meeting #116e 01 - 11 Nov 2021 Electronic Meeting

TSG-RAN2 Meeting #116bis-e 17 - 26 Jan 2022 Electronic Meeting

**Question 4: Do you agree with the above contents？Please share your comments in the table.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/ No | Comments |
| Qualcomm | No | The original question from SA2 in R2-2102665 was:  "SA2 would like to ask RAN1 and RAN2 whether support can be provided for a scheduled location time as part of Rel-17 and as defined in the attached CR to TS 23.273."  This question hasn't been answered yet. Instead, RAN2 sent several questions for clarification at RAN2#113bis-e.  The response LS to RAN2's questions in R2-2106968 included a further question for RAN2:  **Question A:** in order to get a clear view from RAN WG, SA2 sincerely ask RAN2 to investigate whether Scheduled Location Time could help the reduction of the LCS latency.  Therefore, RAN2 should (at least) answer this question (and not speculate or comment on e.g., user case, etc. )  For Question A, we suggest the following response (see also our input to this meeting (R2-2108376)):  "A scheduled location time T allows the latency for obtaining and reporting the location of a target device to be reduced by the duration of the location preparation phase which allows substantial reduction of latency. With the RAN2 assumptions summarized in TR 38.857, the latency reduction can be:  DL+UL NR positioning methods: Latency reduction of more than 62 %  UL-only NR positioning methods: Latency reduction of more than 78 %  DL-only NR positioning methods: Latency reduction of more than 50 %".  If there are concerns with the actual numbers (although, they are all based on TR 38.857), we would also be O.K. with a single sentence:  "A scheduled location time T allows the latency for obtaining and reporting the location of a target device to be reduced by the duration of the location preparation phase which allows substantial reduction of latency." |
| ZTE | Yes | Agree with the LS content |
| Ericsson | Yes |  |
| Xiaomi | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 5 Conclusion

TBD