**3GPP TSG-RAN WG2 Meeting #115e R2-21XXXX**

**E-Meeting, 9th - 27th Aug 2021**

**Source: Xiaomi**

**Title:****Report of [Offline-616]**

**Agenda Item:** **8.7.2.1**

**Document for:** **Discussion and Decision**

# Introduction

This contribution is to discuss following offline discussion.

* [AT115-e][616][Relay] Proposals from control plane summary (Xiaomi)

Scope: Briefly discuss P1/P4/P5 and P8/P9/P10 of R2-2108824 and attempt to reach consensus. Also confirm if P18 is agreeable.

Intended outcome: Report to comeback session, in R2-2108948

Deadline: Tuesday 2021-08-24 2000 UTC

# Discussion

## 2.1 Uu RLC configuration for remote UE’s SRB0/1

Regarding Uu RLC configuration for remote UE’s SRB0 message, companies’ views are observed as following,

Option 1, Fixed/specified [1], [6], [33], [36]

Option 2, Default [7], [9], [13]

Option 3, NW configured [4], [7], [9], [13], [15], [20], [26]

Proponents of option 1 prefer the same principle as PC-5 RLC configuration should be reused for Uu. Proponents of option 3 believes the NW is able to provide Uu RLC configuration since relay UE shall enter CONNECTED to relay remote UE’s SRB0 message. Meanwhile, [7], [9] and [13] also supports default configuration in case NW doesn’t provide dedicated configuration. There is no clear majority view. P1 in [39] propose RAN2 to discuss following question,

**Question 1: which Uu RLC configuration is used for remote UE’s SRB0 message.**

**Option 1, Fixed/specified.**

**Option 2, Default,**

**Option 3, NW configured.**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comments |
| Apple | Option 1 | We think it is simple for relay UE implementation to just use fixed/specified option for SRB0 in both PC5 and Uu hop. |
| Qualcomm | Option 2 and Option 3 | Option 1 doesn’t make sense. Fixed/specified configuration is used for SRB0 delivery, but relay is CONNECTED state. As a principle in Uu, CONNECTED UE with security generally can’t use SRB0.  For Option 2 and Option 3, we actually see below 3 different solutions:   * **Alt-1:** Specify a default Uu RLC channel in spec, which can be reconfigured to a dedicated RLC channel by gNB later * **Alt-2:** gNB configures **one Uu RLC channel shared by all remote UEs for SRB0 delivery** after the relay UE enters CONNECTED state with its L2 Relay capability indicated/authorized * **Alt-3:** gNB configures **different Uu RLC channels for different remote UEs for SRB0 delivery**, which requires CONNECTED relay to send SUI first   We think Alt-3 should be precluded because it has extra latency of 2 RRC messages (for SUI and responded RRC Reconfiguration message with dedicated Uu RLC channel config).  For Alt-1 and Alt-2, we think there is not much difference. Both of them need to reserve a fixed LCID for SRB0. The only difference is that the fixed LCID is specified in spec in Alt-1 while the fixed LCID is configured by gNB after relay authorization in Alt-2. We think RAN2 can pick either one based on majority. |
|  |  |  |
|  |  |  |

Regarding Uu RLC configuration for remote UE’s SRB1 message, companies’ views are observed as following,

Option 1, Fixed/specified [33]

Option 2, Default [1], [6], [7], [9], [13], [36]

Option 3, NW configured [4], [7], [9], [13], [15], [20], [26], [36]

Only one company prefers fixed/specified configuration. 6 companies prefer to use default configuration. 8 companies prefer to use NW configured configuration. RAN2 had agreed Uu RLC configuration for remote UE’s SRB1 message such as RRCResume and RRCReestablishment message could be (re-)configured by NW via dedicated signalling. It’s still FFS whether default configuration is supported. P4 in [39] propose RAN2 to discuss following question,

**Question 2: Do you agree default Uu RLC configuration for remote UE’s SRB1 message is supported.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Apple | Yes | It can be overridden by network configuration |
| Qualcomm | Yes | Because relay is in CONNECTED state, we prefer the same handling as SRB0 in Question 1, i.e. pick either one below Alt-1 or Alt-2:   * **Alt-1:** Specify a default Uu RLC channel, which can be reconfigured to a dedicated RLC channel by gNB later   **Alt-2:** gNB configures a **Uu RLC channel shared by all remote UEs for SRB0 delivery** after the relay UE enters CONNECTED state with its L2 Relay capability indicated/authorized |
|  |  |  |

[7] further discuss which RLC configuration is used for RRCReconfigurationComplete in path switch to indirect path. P5 in [39] propose RAN2 to discuss following question,

**Question 3: Do you agree dedicated signalling is used for the PC5 RLC and Uu RLC configuration of remote UE SRB1 for RRCReconfigurationComplete in path switch to indirect path.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Apple | Yes | This can be part of RRCReconfiguration message to the remote UE. |
| Qualcomm | See comments | If target relay is in CONNECTED state, we think both RRC reconfiguration message towards remote UE (i.e. step 3) and reconfiguration message towards relay (i.e. step 2) can include remote UE dedicated PC5 RLC and Uu RLC configuration for delivery of remote UE’s *RRCReconfigurationComplete* message. So, it is “Yes”  If target relay is in IDLE/INACTIVE state, this question needs further study whether default/specified PC5/Uu RLC need to be used. Please note that gNB can’t configure dedicated RLC for IDLE/INACTIVE relay UE (i.e. there is no step 2). |
|  |  |  |
|  |  |  |

## 2.3 Sharing of ID/DRX information for paging forward

In RAN2 114 meeting, it’s agreed that When Relay UE in RRC IDLE/RRC INACTVE and Remote UE in RRC IDLE/RRC INACTIVE, the Relay UE monitors paging occasions of its PC5-RRC connected Remote UE(s). However, it’s FFS how relay UE obtain remote UE’s paging occasions. Many companies support remote UE provides UE ID, i.e. 5G-S-TMSI/I-RNTI to relay UE. Relay UE could decode paging message to derive the UE ID and forward the paging message accordingly. P8/P9 in [39] propose RAN2 to discuss following question,

**Question 4: Do you agree IDLE/INACTIVE remote UE provides 5G-S-TMSI/I-RNTI to IDLE/INACTIVE relay UE.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Apple | Yes | As SA3 has confirmed there is no security concern on exposing the 5G-S-TMSI/I-RNTI, it is OK to share those with relay UE. |
| Qualcomm | Yes | It is straight forward to follow SA3 reply LS:  **A**: SA3 made an assumption that the relay UE is a trusted entity. Under this assumption, exposing the 5G-S-TMSI/I-RNTI of the remote UE to relay UE is acceptable.  In addition, please note that SA3 didn’t mention any condition of this trust assumption. Thus, RAN2 can assume relay is always trusted. We prefer to add “**full**” before “**5G-S-TMSI/I-RNTI”,** to make the proposal more clearly |
|  |  |  |
|  |  |  |

**Question 5: Do you agree IDLE/INACTIVE Relay UE decodes received paging message to derive the 5G-S-TSMI/I-RNTI and forward the paging message accordingly.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Apple | Yes |  |
| Qualcomm | Yes | As replied in Q4, please note that SA3 didn’t mention any condition of this trust assumption. Thus, RAN2 can assume relay is always trusted, and full UE-ID can be shared between remote UE and relay.  Therefore, we think there is no security concern for relay to decode paging message of remote UE. Then, relay UE can know which specific remote UE to receive the paging. As consequence, unicast PC5-RRC transmission for paging forwarding is sufficient. |
|  |  |  |
|  |  |  |

Relay UE shall be aware of remote UE’s PO to perform monitoring. [2], [8], [12], [27] propose to provide remote UE’s DRX cycle to relay UE. [21] propose to provide remote UE’s PO to relay UE. [30] believes the PO of remote UE is configured via SIB. However, according to 38.304 specification, the PO is calculated in MAC and the essential parameters, e.g. DRX cycle, may come from SIB or upper layer. It’s unclear how SIB could configure remote UE’s PO. P10 in [39] propose RAN2 to discuss following question,

**Question 6: Do you agree IDLE/INACTIVE remote UE provide its Uu DRX cycle T to IDLE/INACTIVE relay UE.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Apple | Yes |  |
| Qualcomm | Yes (see comments) | We are not sure what T means. All the following understandings can work:   * IDLE UE   + Alt-1: T=min (default cycle, cycle in NAS)   + Alt-2: T=cycle in NAS. * INACTIVE UE   + Alt-1: T=min (RAN paging cycle, cycle in NAS)   + Alt-2: T= RAN paging cycle and cycle in NAS   The difference b/w IDLE and INACTIVE is that default cycle is common to relay and remote UE, so no need for remote to share with relay.  We don’t have strong opinion for above understanding. Suggest to make it clear in agreement. |
|  |  |  |
|  |  |  |

## 2.4 Connection establishment for relay and remote UE

If both remote UE and relay UE are not in CONNECTED, both UEs need to enter CONNECTED for service transmission. [9] assumes remote UE and relay UE performs connection establishment/resume independently. [33] propose to discuss combined relay UE and remote UE’s RRC connection establishment/assumption. Rapporteur understands second option may require additional impact in RAN1, since current msg3 is not enough for two RRC messages. Furthermore, in TR, it’s agreed if the Relay UE had not started in RRC\_CONNECTED, it would need to do its own connection establishment upon reception of a message on the default L2 configuration on PC5. P10 in [39] propose RAN2 to discuss following question,

**Question 7: Do you agree, as baseline, Remote UE and relay UE performs connection establishment/resume independently, i.e. relay UE shall enter CONNECTED to be able to forward remote UE’s initial RRC messages.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Apple | Yes |  |
| Qualcomm | Yes | We prefer to complete baseline procedure first. |
|  |  |  |
|  |  |  |

# Report

Following proposals are made,

# Reference

[1] R2-2106989 Control Plane Procedures of L2 Relay CATT

[2] R2-2107039 Discussion on Control Plane Aspects for L2 Relay OPPO

[3] R2-2107044 Stage 2 level procedure for Connection Establishment MediaTek Inc.

[4] R2-2107103 Further discussion on RRC connection management of L2 U2N relay Qualcomm Incorporated

[5] R2-2107104 Further discussion on paging and SIB forwarding in L2 U2N relay Qualcomm Incorporated

[6] R2-2107176 Remaining issues on RRC connection management Samsung Electronics GmbH

[7] R2-2107231 Discussion on RRC connection management for L2 sidelink relay Huawei, HiSilicon

[8] R2-2107232 SI forwarding and paging for L2 sidelink relay Huawei, HiSilicon discussion

[9] R2-2107273 Connection Establishment Procedure for L2 UE to NW Relays InterDigital

[10] R2-2107274 Paging Procedures for L2 UE to NW Relays InterDigital discussion

[11] R2-2107275 SI Forwarding for L2 UE to NW Relays InterDigital discussion

[12] R2-2107304 Discussion on paging forwarding for a remote UE SHARP Corporation discussion

[13] R2-2107306 Remaining issues of L2 Relay connection management Intel Corporation

[14] R2-2107367 Discussion on control plane procedures for L2 U2N relay Spreadtrum Communications

[15] R2-2107541 Configuration of Uu Interface for Sidelink Relay Futurewei

[16] R2-2107622 Remaining issues on SIB forwarding for IDLE/INACTIVE remote UE Apple

[17] R2-2107623 Unified Access Control on Relay UE Apple

[18] R2-2107625 RNA Update via L2 UE-to-NW relay Apple

[19] R2-2107709 Paging delivery via L2 Relay in RRC\_CONNECTED Samsung

[20] R2-2107757 Way forward for L2 U2N Remote UE SRB0 SRB1 configuration vivo

[21] R2-2107966 Discussion on SI and paging delivery Xiaomi communications

[22] R2-2107967 Discussion on connection control Xiaomi communications

[23] R2-2108007 SI acquisition, CN Registration and RNAU Lenovo Mobile Com. Technology

[24] R2-2108008 Monitoring Paging by a U2N Relay Lenovo Mobile Com. Technology

[25] R2-2108060 L2 relay control plane procedures Sony discussion

[26] R2-2108145 Consideration on the connection management of SL relay ZTE, Sanechips

[27] R2-2108146 Consideration on the system information acquisition and paging in SL relay ZTE, Sanechips

[28] R2-2108153 SIB Delivery & Paging for Remote UE LG Electronics Inc

[29] R2-2108154 Connection Establishment LG Electronics Inc

[30] R2-2108192 Discussion on paging and SIB handling for L2 sidelink relay Ericsson

[31] R2-2108195 Discussion on RRC connection management procedures for L2 SL relay Ericsson

[32] R2-2108414 Discussion on SI and paging forwarding

[33] R2-2108458 Discussion on RRC connection establishment of remote UE in L2 U2N relay Nokia, Nokia Shanghai Bell

[34] R2-2108462 Support of idle mode mobility for remote-UE in SL UE-to-Nwk relay Nokia, Nokia Shanghai Bell

[35] R2-2108510 Control plane procedure CMCC

[36] R2-2108250 Sidelink Relay Uu RLC for Remote UE and Adaptation Layer Design Beijing Xiaomi Mobile Software

[37] R2-2108156 Relay reselection when Relay UE performs HO LG Electronics Inc

[38] R2-2108144 Further discussion on Relay selection ZTE, Sanechips

[39] R2-2108824 Summary of AI 8.7.2.1 Xiaomi Technology