3GPP RAN WG2 Meeting #116e R2-2111354

eMeeting November 1st – 12th, 2021

Agenda Item: 8.10.2.2

Source: InterDigital (offline rapporteur)

Title: [DRAFT] Summary of [AT116-e][101][NTN] Other MAC aspects: Phase 2

Document for: Discussion, Decision

# Introduction

This document is a intended to continue discussion on the following aspects:

* [AT116-e][101][NTN] Other MAC aspects (InterDigital)

Updated scope: Continue the discussion on remaining aspects of timers, HARQ, and LCP including CG/SPS aspects, based on the outcome of the discussion in R2-2111339

Updated intended outcome: Summary of the offline discussion with e.g.:

* List of proposals for agreement (if any)
* List of proposals that require online discussions
* List of proposals that should not be pursued (if any)

The following deadline for company feedback has been provided:

* Initial deadline (for companies' feedback): **Monday 2021-11-08 1600 UTC**
* Initial deadline (for rapporteur's summary in R2-2111354): Monday 2021-11-08 2000 UTC

Please also note the following chair guidance:

* Proposals marked "for agreement" in R2-2111354 not challenged until **Tuesday 2021-11-09 0800 UTC** will be declared as agreed via email by the session chair (for the rest the discussion will continue in the CB session in Week2).

Companies are encouraged to review Phase 1 discussion summary in [R2-2111339](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Inbox/R2-2111339.zip) for relevant background.

# Discussion

## P7

In Phase 1 discussion, possible LCH to HARQ process mappings were discussed and considered all possible configurations of LCH and HARQ. The following agreement was made based on outcome of Phase 1:

* *If uplinkHARQ-DRX-LCP-Mode-r17 is configured, a HARQ process may be mapped to either ‘HARQ mode A’ or ‘HARQ mode B’.*

Based on this agreement, if *uplinkHARQ-DRX-LCP-Mode-r17* is configured then all HARQ processes will either be HARQ mode A or HARQ mode B. If *uplinkHARQ-DRX-LCP-Mode-r17* is not configured, then no HARQ process is configured with a HARQ mode.

For the case *uplinkHARQ-DRX-LCP-Mode-r17* is not configured, an existing agreement from RAN2#115e covers the mapping behaviour:

* *If HARQ process has not been configured with an UL HARQ retransmission state, new LCH mapping rule has no effect (i.e. UE applies legacy behaviour).*

Therefore, the original proposal 7 can be simplified to describe behaviour when *uplinkHARQ-DRX-LCP-Mode-r17* is configured (i.e. all HARQ processes are either Mode A or B). Based on comments received, Rapporteur suggests the following behaviour:

If*uplinkHARQ-DRX-LCP-Mode-r17*is configured,the following LCH to HARQ process mapping rules are supported:

1. LCHismapped only to a HARQ process configured with HARQ mode A;
2. LCHismapped only to a HARQ process configured with HARQ mode B;
3. If an LCH is not configured with a mapping rule, it may be mapped to any HARQ process (HARQ mode A or B)."

Combing existing agreed behaviour with this proposal would result in the following mapping restriction:



**Question 1: Do you agree to the following proposal?:**

**“*If uplinkHARQ-DRX-LCP-Mode-r17 is configured, the following LCH to HARQ process mapping rules are supported:***

1. ***LCH is mapped only to a HARQ process configured with HARQ mode A;***
2. ***LCH is mapped only to a HARQ process configured with HARQ mode B;***
3. ***If an LCH is not configured with a mapping rule, it may be mapped to any HARQ process (HARQ mode A or B)."***

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## P10/P11/P13

The HARQ-processes ID of both CG and SPS are calculated from parameters of radio resource allocation in time domain, e.g. configured periodicity, start off in time domain, configured HARQ process number. This is different from dynamic scheduling, where there is no relationship between HARQ ID and radio resource allocation in time domain.

As noted in Phase 1, this may result in the HARQ processes used by an SPS configuration to have different HARQ feedback behaviour, or HARQ processes used by a CG configuration to have different a UL HARQ mode. There seems to be a general understanding that this is not desired behaviour.

In Phase 1 input, two main options were discussed to address this issue: Configure HARQ behaviour per CG/SPS configuration, or leave it to network implementation. From Phase 1 company feedback, a majority agreed that network configuration would be sufficient in both cases.

**Question 2: Do you agree to the following proposal?:**

**“*It is up to network implementation to ensure downlinkHARQ-FeedbackDisabled, if configured, has the same value for each HARQ process used in an SPS configuration (i.e. no specification impact)."***

**If ‘Disagree’, please provide technical justification why the above would not work and additional specified behaviour is required.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 3: Do you agree to the following proposal?:**

**“*It is up to network implementation to ensure uplinkHARQ-DRX-LCP-Mode-r17, if configured, has the same value for each HARQ process used in a configured grant configuration (i.e. no specification impact)."***

**If ‘Disagree’, please provide technical justification why the above would not work and additional specified behaviour is required.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## P16

In Phase 1 it was discussed whether to link the HARQ mode configuration with CG timer configuration (i.e. require the CGT setting / CGT not configured to match the HARQ mode uplinkHARQ-DRX-LCP-Mode-r17 of each HARQ process that belongs to the CG-config). For example:

* For the configured grant for which the *configuredGrantTimer* is configured, the HARQ retransmission state is considered to be “mode A”.
* For the configured grant for which the *configuredGrantTimer* is NOT configured, the HARQ retransmission state is considered to be “mode B”.

Justification for this is that for configured grant associated with HARQ state B, HARQ RTT timer is not used because retransmission is not expected. Then it is not clear why *configuredGrantTimer* needs to be used for this. It should be clarified that the network should not configure this timer for such CG configuration, otherwise it will block any new transmission in any CG associated with the same HARQ process. Considering the possible RTT in NTN, this could lead to large delay.

Rapporteur understanding is that the above is valid reasoning and that this would indeed be the intended behaviour. However, the question is whether this association needs to be specified or may be left to network implementation. Based on large majority from in Phase 1 responding an association is not needed, it is suggested that this be left to proper network configuration.

**Question 4: Do you agree that if *uplinkHARQ-DRX-LCP-Mode-r17*****is configured, proper setting/ configuration of the *configuredGrantTimer*  is left to network implementation?**

**If ‘Disagree’, please provide technical justification why the above would not work and additional specified behaviour is required.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Other proposals

### SR-Prohibit Timer

So far in RAN2#116e, the following has been agreed regarding extension of the *sr-ProhibitTimer* in NTN:

* *The extended values for sr-ProhibitTimer in NTN can include values less than UE-gNB RTT (as in legacy). FFS on the actual values and how this is extended*
* *Introduce a new sr-ProhibitTimerExt-r17 IE. Values FFS*

Taking the above agreements into consideration, companies are invited to propose a candidate set of additional values for the new *sr-ProhibitTimerExt-r17* IE.

**Question 5: What are possible values to be included in the *sr-ProhibitTimerExt-r17* IE ?**

|  |  |
| --- | --- |
| **Company** | **Possible values**  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### RRC details

In Phase 1 discussion the following was agreed with consensus:

* *uplinkHARQ-DRX-Mode shall be included in PUSCH-ServingCellConfig.*

Several companies also suggested revised placement for parameter *downlinkHARQ-FeedbackDisabled*. In light of the above agreement, Rapporteur thinks this proposal may be confirmed prior to session to save online time.

**Question 6: Do you agree to the following proposal?:**

**“*downlinkHARQ-FeedbackDisabled shall be included in PDSCH-ServingCellConfig."***

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Topics requiring further discussion

In Phase 1 discussion several topics had nearly split opinion, and resulting proposals were put under the ‘Requires further discussion’ section. To save online time, Rapporteur suggests that these topics be addressed via contribution to next meeting with the current set of proposals as baseline. If companies agree, then this may be captured in Chair notes as guidance for RAN2#116bis-e.

**Question 7: Do you agree the following proposals are be taken as baseline for further discussion (e.g. in contributions to RAN2#116bise)?**

* ***RAN2 to down-select between the following options to support blind retransmission for HARQ process(es) configured with HARQ state B: 1) Rely on UE being in DRX Active Time via other means (e.g. Inactivity Timer); or 2) Start drx-RetransmissionTimerUL at the end of PUSCH transmission;***
* ***RAN2 to down-select between the following options to support blind retransmission for HARQ process(es) configured with disabled HARQ feedback: 1) Rely on UE being in DRX Active Time via other means (e.g. Inactivity Timer); or 2) Start drx-RetransmissionTimerDL in the first symbol after the end of the reception of the last PDSCH or slot-aggregated PDSCH plus X (X = T\_proc,1);***
* ***For RACH in RRC\_CONNECTED mode, it is FFS whether UE ignores HARQ process configuration (e.g. configured HARQ mode) for the case of a PUSCH transmission scheduled by RAR.***
* ***RAN2 to down-select between the following options to extend configuredGrantTimer: 1) Introducing value(s) of configuredGrantTimer larger than 64; 2) Value of the configuredGrantTimer is extended by UE-gNB-RTT;***

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Summary

<To be generated pending company feedback>

# Conclusion

In this contribution the following proposals are suggested based on contributions submitted to RAN2#116e AI 8.10.2.2:

<To be generated pending company feedback>

# References

1. [R2-2109499](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109499.zip) Discussion on HARQ related aspects in NTN – OPPO
2. [R2-2109552](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109552.zip) Co-existence issue of BSR over CG and BSR over 2-step RA – CATT
3. [R2-2109631](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109631.zip) Remaining issue on disabling uplink HARQ retransmission – MediaTek Inc.
4. [R2-2109632](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109632.zip) Round trip delay offset for configured grant timers – MediaTek Inc.
5. [R2-2109661](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109661.zip) Further consideration on LCP and HARQ – Huawei, HiSilicon
6. [R2-2109968](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109968.zip) HARQ process for SPS and CG – Qualcomm
7. [R2-2110017](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110017.zip) Remaining issues related to HARQ retransmission state – Xiaomi
8. [R2-2110045](file:///C%3A%5CUsers%5Cwattsdy%5COneDrive%20-%20InterDigital%20Communications%2C%20Inc%5C3GPP%5CRAN2%5C116e%5CTdoc%20review%5CTdocs%5CR2-2110045.zip) NTN HARQ Management – Apple
9. [R2-2110126](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110126.zip) Discussion on HARQ and LCP remaining issues – Spreadtrum Communications
10. [R2-2110308](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110308.zip) Remaining UP issues for NR NTN – Lenovo, Motorola Mobility
11. [R2-2110354](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110354.zip) CG enhancements in NTN – Sony
12. [R2-2110704](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110704.zip) Discussion on UL scheduling, DRX and other MAC aspects – Nokia, Nokia Shanghai Bell
13. [R2-2110734](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110734.zip) Remaining issues on HARQ aspects – ZTE Corporation, Sanechips
14. [R2-2110859](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110859.zip) Remaining MAC open issues in NTN – InterDigital
15. [R2-2110926](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110926.zip) Updating SR-Prohibit Timer – MediaTek Inc.
16. [R2-2110951](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110951.zip) On configured scheduling, DRX, LCP, HARQ and SR/BSR in NTNs – Ericsson
17. [R2-2111044](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2111044.zip) Remaining Issue on LCP Restrictions and CG Impact in NTN – CMCC
18. [R2-2111139](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2111139.zip) Discussion on other MAC aspects – LG Electronics Inc.
19. [R2-2111151](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2111151.zip) Retransmission timer for HARQ state B – ITL
20. [R2-2111154](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2111154.zip) HARQ State A/B for CG aspects – ITL