**3GPP T****SG-RAN WG2 Meeting #117**   **R2-2203760**

**E-Meeting, Feb 21st – Mar 3rd, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **draft** | **rev** | **-** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | UE capability for NR and MR-DC measurement gap enhancements |
|  |  |
| ***Source to WG:*** | Intel Corporation |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_MG\_enh-Core |  | ***Date:*** | 2022-02-21 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Introduction of pre-configured, concurrent and NCSG measurement gap |
|  |  |
| ***Summary of change:*** | * Adding UE capability for support of pre-configured measurement gap with network-controlled activation and deactivation mechanism (RAN4 feature list 19-3-1)
* Pre-configured measurement gap with UE autonomous activation and deactivation mechanism (RAN4 feature list 19-3-2)
* Adding UE capability for support of concurrent measurement gap (RAN4 feature list 19-2)
* Adding UE capability for support of NCSG measurement (RAN4 feature list 19-1)
* Adding UE capability for support of NCSG measurement reporting for E-UTRA target band
 |
|  |  |
| ***Consequences if not approved:*** | Pre-configured, concurrent and NCSG measurement gap are not introduced. |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS/TR 38.306 CR XXX |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

START OF FIRST CHANGE

### 6.3.3 UE capability information elements

**<< OMMITED>>**

– *MeasAndMobParameters*

The IE *MeasAndMobParameters* is used to convey UE capabilities related to measurements for radio resource management (RRM), radio link monitoring (RLM) and mobility (e.g. handover).

***MeasAndMobParameters* information element**

-- ASN1START

-- TAG-MEASANDMOBPARAMETERS-START

MeasAndMobParameters ::= SEQUENCE {

 measAndMobParametersCommon MeasAndMobParametersCommon OPTIONAL,

 measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL,

 measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

MeasAndMobParametersCommon ::= SEQUENCE {

 supportedGapPattern BIT STRING (SIZE (22)) OPTIONAL,

 ssb-RLM ENUMERATED {supported} OPTIONAL,

 ssb-AndCSI-RS-RLM ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 eventB-MeasAndReport ENUMERATED {supported} OPTIONAL,

 handoverFDD-TDD ENUMERATED {supported} OPTIONAL,

 eutra-CGI-Reporting ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting ENUMERATED {supported} OPTIONAL

 ]],

 [[

 independentGapConfig ENUMERATED {supported} OPTIONAL,

 periodicEUTRA-MeasAndReport ENUMERATED {supported} OPTIONAL,

 handoverFR1-FR2 ENUMERATED {supported} OPTIONAL,

 maxNumberCSI-RS-RRM-RS-SINR ENUMERATED {n4, n8, n16, n32, n64, n96} OPTIONAL

 ]],

 [[

 nr-CGI-Reporting-ENDC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 eutra-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

 eutra-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 reportAddNeighMeasForPeriodic-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverParametersCommon-r16 SEQUENCE {

 condHandoverFDD-TDD-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverFR1-FR2-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 nr-NeedForGap-Reporting-r16 ENUMERATED {supported} OPTIONAL,

 supportedGapPattern-NRonly-r16 BIT STRING (SIZE (10)) OPTIONAL,

 supportedGapPattern-NRonly-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 maxNumberCLI-RSSI-r16 ENUMERATED {n8, n16, n32, n64} OPTIONAL,

 maxNumberCLI-SRS-RSRP-r16 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

 maxNumberPerSlotCLI-SRS-RSRP-r16 ENUMERATED {n2, n4, n8} OPTIONAL,

 mfbi-IAB-r16 ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NPN-r16 ENUMERATED {supported} OPTIONAL,

 idleInactiveEUTRA-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

 idleInactive-ValidityArea-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

 pcellT312-r16 ENUMERATED {supported} OPTIONAL,

 supportedGapPattern-r16 BIT STRING (SIZE (2)) OPTIONAL

 ]],

 [[

 -- R4 19-2 Concurrent measurement gaps

 concurrentMeasGap-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-1 Network controlled small gap (NCSG)

 ncsg-MeasGap-r17 ENUMERATED {supported} OPTIONAL,

 ncsg-MeasGapEUTRAN-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-3-2 pre-configured measurement gap

 preconfiguredUE-AutonomousMeasGap-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-3-1 pre-configured measurement gap

 preconfiguredNW-ControlledMeasGap-r17 ENUMERATED {supported} OPTIONAL
]]

}

MeasAndMobParametersXDD-Diff ::= SEQUENCE {

 intraAndInterF-MeasAndReport ENUMERATED {supported} OPTIONAL,

 eventA-MeasAndReport ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 handoverInterF ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 sftd-MeasNR-Neigh ENUMERATED {supported} OPTIONAL,

 sftd-MeasNR-Neigh-DRX ENUMERATED {supported} OPTIONAL

 ]],

 [[

 dummy ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersFRX-Diff ::= SEQUENCE {

 ss-SINR-Meas ENUMERATED {supported} OPTIONAL,

 csi-RSRP-AndRSRQ-MeasWithSSB ENUMERATED {supported} OPTIONAL,

 csi-RSRP-AndRSRQ-MeasWithoutSSB ENUMERATED {supported} OPTIONAL,

 csi-SINR-Meas ENUMERATED {supported} OPTIONAL,

 csi-RS-RLM ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 handoverInterF ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxNumberResource-CSI-RS-RLM ENUMERATED {n2, n4, n6, n8} OPTIONAL

 ]],

 [[

 simultaneousRxDataSSB-DiffNumerology ENUMERATED {supported} OPTIONAL

 ]],

 [[

 nr-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-ENDC-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 cli-RSSI-Meas-r16 ENUMERATED {supported} OPTIONAL,

 cli-SRS-RSRP-Meas-r16 ENUMERATED {supported} OPTIONAL,

 interFrequencyMeas-NoGap-r16 ENUMERATED {supported} OPTIONAL,

 simultaneousRxDataSSB-DiffNumerology-Inter-r16 ENUMERATED {supported} OPTIONAL,

 idleInactiveNR-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

 -- R4 6-2: Support of beam level Early Measurement Reporting

 idleInactiveNR-MeasBeamReport-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 increasedNumberofCSIRSPerMO-r16 ENUMERATED {supported} OPTIONAL

 ]]

}

-- TAG-MEASANDMOBPARAMETERS-STOP

-- ASN1STOP

**<< OMMITED>>**

END OF CHANGE

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Features** | **Index** | **Feature group** | **Components** | **Prerequisite feature groups** | **Field name in TS 38.331 [2]** | **Parent IE in TS 38.331 [2]** | **Need of FDD/TDD differentiation** | **Need of FR1/FR2 differentiation** | **Note** | **Mandatory/Optional** |
| x. NR\_MG\_enh | 1-1 | Network controlled small gap (NCSG) | UE capability for support of NCSG measurement reporting for E-UTRA target band |  | *ncsg-MeasGapEUTRAN-r17* | *MeasAndMobParametersCommon* | No | No |  | Optional with capability signalling |