**3GPP T****SG-RAN WG2 Meeting #117-e R2-220wxyz**

**Online Meeting, 21st February– 3rd March 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.306** | **CR** | **Draft** | **rev** | **-** | **Current version:** | **16.7.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft 38.306 CR for MBS UE capabilities | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | MediaTek Inc. | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_MBS-Core | | | | |  | ***Date:*** | | | 2022-03-02 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Introduction of R17 MBS feature. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | UE capabilities for R17 MBS feature are defined. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No UE capabilities for R17 MBS feature are defined. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.2.2, 4.2.4, 4.2.6, 8 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS38.331 CR TBD | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*First change*

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

BAP Backhaul Adaptation Protocol

BC Band Combination

BT Bluetooth

DAPS Dual Active Protocol Stack

DL Downlink

EHC Ethernet Header Compression

FS Feature Set

FSPC Feature Set Per Component-carrier

IAB-MT Integrated Access Backhaul Mobile Termination

MAC Medium Access Control

MCG Master Cell Group

MBS Multicast/Broadcast Service

MN Master Node

MRB MBS Radio Bearer

MR-DC Multi-RAT Dual Connectivity

PDCP Packet Data Convergence Protocol

RLC Radio Link Control

RTT Round Trip Time

SCG Secondary Cell Group

SDAP Service Data Adaptation Protocol

SN Secondary Node

UL Uplink

WLAN Wireless Local Area Network

*Next change*

### 4.2.2 General parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Definitions for parameters | Per | M | FDD-TDD DIFF | **FR1-FR2**  DIFF |
| ***accessStratumRelease***  Indicates the access stratum release the UE supports as specified in TS 38.331 [9]. | UE | Yes | No | No |
| ***delayBudgetReporting***  Indicates whether the UE supports delay budget reporting as specified in TS 38.331 [9]. | UE | No | No | No |
| ***dl-DedicatedMessageSegmentation-r16***  Indicates whether the UE supports reception of segmented DL RRC messages. | UE | No | No | No |
| ***drx-Preference-r16***  Indicates whether the UE supports providing its preference of a cell group on DRX parameters for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***inactiveState***  Indicates whether the UE supports RRC\_INACTIVE as specified in TS 38.331 [9]. | UE | Yes | No | No |
| ***inDeviceCoexInd-r16***  Indicates whether the UE supports IDC (In-Device Coexistence) assistance information as specified in TS 38.331 [9]. | UE | No | No | No |
| ***maxBW-Preference-r16***  Indicates whether the UE supports providing its preference of a cell group on the maximum aggregated bandwidth for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | Yes |
| ***maxCC-Preference-r16***  Indicates whether the UE supports providing its preference of a cell group on the maximum number of secondary component carriers for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***maxMIMO-LayerPreference-r16***  Indicates whether the UE supports providing its preference of a cell group on the maximum number of MIMO layers for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | Yes |
| ***maxMRB-Add-r17***  Indicates the additional maximum number of MRBs that the UE supports for MBS multicast reception as specified in TS 38.331[9]. | UE | No | No | No |
| ***mcgRLF-RecoveryViaSCG-r16***  Indicates whether the UE supports recovery from MCG RLF via split SRB1 (if supported) and via SRB3 (if supported) as specified in TS 38.331[9]. | UE | No | No | No |
| ***minSchedulingOffsetPreference-r16***  Indicates whether the UE supports providing its preference on the minimum scheduling offset for cross-slot scheduling of the cell group for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***mpsPriorityIndication-r16***  Indicates whether the UE supports *mpsPriorityIndication* on RRC release with redirect as defined in TS 38.331 [9]. | UE | No | No | No |
| ***onDemandSIB-Connected-r16***  Indicates whether the UE supports the on-demand request procedure of SIB(s) or posSIB(s) while in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***overheatingInd***  Indicates whether the UE supports overheating assistance information. | UE | No | No | No |
| ***partialFR2-FallbackRX-Req***  Indicates whether the UE meets only a partial set of the UE minimum receiver requirements for the eligible FR2 fallback band combinations as defined in Clause 4.2 of TS 38.101-2 [3] and Clause 4.2 of TS 38.101-3 [4]. If not indicated, the UE shall meet all the UE minimum receiver requirements for all the FR2 fallback combinations in TS 38.101-2 [3] and TS 38.101-3 [4]. The UE shall support configuration of any of the FR2 fallback band combinations regardless of the presence or the absence of this field. | UE | No | No | No |
| ***redirectAtResumeByNAS-r16***  Indicates whether the UE supports reception of *redirectedCarrierInfo* in an *RRCRelease* message in response to an *RRCResumeRequest* or *RRCResumeRequest1* which is triggered by the NAS layer, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***reducedCP-Latency***  Indicates whether the UE supports reduced control plane latency as defined in TS 38.331 [9] | UE | No | No | No |
| ***referenceTimeProvision-r16***  Indicates whether the UE supports provision of referenceTimeInfo in *DLInformationTransfer* message and in SIB9 and reference time information preference indication via assistance information, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***releasePreference-r16***  Indicates whether the UE supports providing its preference assistance information to transition out of RRC\_CONNECTED for power saving, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***resumeWithStoredMCG-SCells-r16***  Indicates whether the UE supports not deleting the stored MCG SCell configuration when initiating the resume procedure. | UE | No | No | No |
| ***resumeWithStoredSCG-r16***  Indicates whether the UE supports not deleting the stored SCG configuration when initiating resume. The UE which indicates support for *resumeWithStoredSCG-r16* shall also indicate support for *resumeWithSCG-Config-r16*. | UE | No | No | No |
| ***resumeWithSCG-Config-r16***  Indicates whether the UE supports (re-)configuration of an SCG during the resume procedure. | UE | No | No | No |
| ***splitSRB-WithOneUL-Path***  Indicates whether the UE supports UL transmission via MCG path and DL reception via either MCG path or SCG path, as specified for the split SRB in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). | UE | No | No | No |
| ***splitDRB-withUL-Both-MCG-SCG***  Indicates whether the UE supports UL transmission via both MCG path and SCG path for the split DRB as specified in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). | UE | Yes | No | No |
| ***srb3***  Indicates whether the UE supports direct SRB between the SN and the UE as specified in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). This field is not applied to NE-DC. | UE | Yes | No | No |

*Next change*

### 4.2.4 PDCP Parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Definitions for parameters | Per | M | FDD-TDD DIFF |
| ***continueEHC-Context-r16***  Indicates that the UE supports EHC context continuation operation where the UE keeps the established EHC context(s) upon PDCP re-establishment, as specified in TS 38.323 [16]. | UE | No | No |
| ***continueROHC-Context***  Defines whether the UE supports ROHC context continuation operation where the UE does not reset the current ROHC context upon PDCP re-establishment, as specified in TS 38.323 [16]. | UE | No | No |
| ***ehc-r16***  Indicates that the UE supports Ethernet header compression and decompression using EHC protocol, as specified in TS 38.323 [16]. The UE indicating this capability and indicating support for at least one ROHC profile, shall support simultaneous configuration of EHC and ROHC on different DRBs. | UE | No | No |
| ***extendedDiscardTimer-r16***  Indicates whether the UE supports the additional values of PDCP discard timer. The supported additional values are 0.5ms, 1ms, 2ms, 4ms, 6ms and 8ms, as specified in TS 38.331 [9]. | UE | No | No |
| ***jointEHC-ROHC-Config-r16***  Indicates whether the UE supports simultaneous configuration of EHC and ROHC protocols for the same DRB. | UE | No | No |
| ***maxNumberROHC-ContextSessions***  Defines the maximum number of ROHC header compression context sessions supported by the UE across all DRBs and multicast MRBs, excluding context sessions that leave all headers uncompressed. | UE | No | No |
| ***maxNumberEHC-Contexts-r16***  Defines the maximum number of Ethernet header compression contexts supported by the UE across all DRBs and multicast MRBs and across UE's EHC compressor and EHC decompressor. The indicated number defines the number of contexts in addition to CID = "all zeros" as specified in TS 38.323 [16]. | UE | No | No |
| ***outOfOrderDelivery***  Indicates whether UE supports out of order delivery of data to upper layers by PDCP. | UE | No | No |
| ***pdcp-DuplicationMCG-OrSCG-DRB***  Indicates whether the UE supports CA-based PDCP duplication over MCG or SCG DRB as specified in TS 38.323 [16]. | UE | No | No |
| ***pdcp-DuplicationMoreThanTwoRLC-r16***  Defines whether the UE supports PDCP duplication with more than two RLC entities as specified in TS 38.323 [16]. The UE supporting this feature supports secondary RLC entity(ies) activation and deactivation based on duplication RLC Activation/Deactivation MAC CE as specified in TS 38.321 [8]. A UE supporting this feature shall also support *pdcp-DuplicationMCG-OrSCG-DRB*, *pdcp-DuplicationSplitDRB*, *pdcp-DuplicationSplitSRB* and *pdcp-DuplicationSRB*. | UE | No | No |
| ***pdcp-DuplicationSplitDRB***  Indicates whether the UE supports PDCP duplication over split DRB as specified in TS 38.323 [16]. | UE | No | No |
| ***pdcp-DuplicationSplitSRB***  Indicates whether the UE supports PDCP duplication over split SRB1/2 as specified in TS 38.323 [16]. | UE | No | No |
| ***pdcp-DuplicationSRB***  Indicates whether the UE supports CA-based PDCP duplication over SRB1/2 and/or, if (NG)EN-DC is supported, SRB3 as specified in TS 38.323 [16]. | UE | No | No |
| ***shortSN***  Indicates whether the UE supports 12 bit length of PDCP sequence number. | UE | Yes | No |
| ***supportedROHC-Profiles***  Defines which ROHC profiles from the list below are supported by the UE:  - 0x0000 ROHC No compression (RFC 5795)  - 0x0001 ROHC RTP/UDP/IP (RFC 3095, RFC 4815)  - 0x0002 ROHC UDP/IP (RFC 3095, RFC 4815)  - 0x0003 ROHC ESP/IP (RFC 3095, RFC 4815)  - 0x0004 ROHC IP (RFC 3843, RFC 4815)  - 0x0006 ROHC TCP/IP (RFC 6846)  - 0x0101 ROHC RTP/UDP/IP (RFC 5225)  - 0x0102 ROHC UDP/IP (RFC 5225)  - 0x0103 ROHC ESP/IP (RFC 5225)  - 0x0104 ROHC IP (RFC 5225)  A UE that supports one or more of the listed ROHC profiles shall support ROHC profile 0x0000 ROHC uncompressed (RFC 5795).  An IMS voice capable UE shall indicate support of ROHC profiles 0x0000, 0x0001, 0x0002 and be able to compress and decompress headers of PDCP SDUs at a PDCP SDU rate corresponding to supported IMS voice codecs. | UE | No | No |
| ***uplinkOnlyROHC-Profiles***  Indicates the ROHC profile(s) that are supported in uplink-only ROHC operation by the UE.  - 0x0006 ROHC TCP (RFC 6846)  A UE that supports uplink-only ROHC profile(s) shall support ROHC profile 0x0000 ROHC uncompressed (RFC 5795). | UE | No | No |

*Next change*

### 4.2.6 MAC parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Definitions for parameters | Per | M | FDD-TDD DIFF | FR1-FR2 DIFF |
| ***autonomousTransmission-r16***  Indicates whether the UE supports autonomous transmission of the MAC PDU generated for a deprioritized configured uplink grant as specified in TS 38.321 [8]. A UE supporting this feature shall also support *lch-priorityBasedPrioritization-r16*. | UE | No | No | No |
| ***directMCG-SCellActivation-r16***  Indicates whether the UE supports direct NR MCG SCell activation, as specified in TS 38.321 [8], upon SCell addition, upon reconfiguration with sync of the MCG, as specified in TS 38.331 [9]. | UE | No | No | Yes |
| ***directMCG-SCellActivationResume-r16***  Indicates whether the UE supports direct NR MCG SCell activation, as specified in TS 38.321 [8], upon reception of an *RRCResume* message, as specified in TS 38.331 [9]. | UE | No | No | Yes |
| ***directSCG-SCellActivation-r16***  Indicates whether the UE supports direct NR SCG SCell activation, as specified in TS 38.321 [8], upon SCell addition and upon reconfiguration with sync of the SCG, both performed via an *RRCReconfiguration* message received via SRB3 or contained in an *RRC(Connection)Reconfiguration* message received via SRB1, as specified in TS 38.331 [9] and TS 36.331 [17].  A UE indicating support of *directSCG-SCellActivation-r16* shall indicate support of EN-DC or support of NGEN-DC as specified in TS 36.331 [17] or support of NR-DC as specified in TS 38.331 [9]. | UE | No | No | Yes |
| ***directSCG-SCellActivationResume-r16***  Indicates whether the UE supports direct NR SCG SCell activation, as specified in TS 38.321 [8]:  - upon reception of an *RRCReconfiguration* included in an *RRCConnectionResume* message, as specified in TS 38.331 [9] and TS 36.331 [17], if the UE indicates support of EN-DC or NGEN-DC, and support of *resumeWithSCG-Config-r16* as specified in TS 36.331 [17],  - upon reception of an *RRCReconfiguration* included in an *RRCResume* message, as specified in TS 38.331 [9], if the UE indicates support of NR-DC and of *resumeWithSCG-Config-r16* as specified in TS 38.331 [9].  A UE indicating support of *directSCG-SCellActivationResume-r16* shall indicate support of EN-DC or NGEN-DC and support of *resumeWithSCG-Config-r16* as specified in TS 36.331 [17] or indicate support of NR-DC and of *resumeWithSCG-Config-r16* as specified in TS 38.331 [9]. | UE | No | No | Yes |
| ***drx-Adaptation-r16***  Indicates whether the UE supports DRX adaptation comprised of the following functional components:  - Configured *ps-Offset* for the detection of DCI format 2\_6 with CRC scrambling by *ps*-RNTI and reported *MinTimeGap* before the start of *drx-onDurationTimer* of Long DRX  - Indication of UE whether or not to start *drx-onDurationTimer* for the next Long DRX cycle by detection of DCI format 2\_6  - Configured UE wakeup or not when DCI format 2\_6 is not detected at all monitoring occasions outside Active Time  - Configured periodic CSI report apart from L1-RSRP (*ps-TransmitOtherPeriodicCSI*) when impacted by DCI format 2\_6 that *drx-onDurationTimer* does not start for the next Long DRX cycle  - Configured periodic L1-RSRP report (*ps-TransmitPeriodicL1-RSRP*) when impacted by DCI format 2\_6 that *drx-onDurationTimer* does not start for the next Long DRX cycle  The capability signalling includes the minimum time gap between the end of the slot of last DCI format 2\_6 monitoring occasion and the beginning of the slot where the UE would start the *drx-onDurationTimer* of Long DRX for each SCS. The value *sl1* indicates 1 slot. The value *sl2* indicates 2 slots, and so on. Support of this feature is reported for licensed and unlicensed bands, respectively. When this field is reported, either of *sharedSpectrumChAccess-r16* or *non-SharedSpectrumChAccess-r16* shall be reported, at least. | UE | No | No | Yes |
| ***enhancedSkipUplinkTxConfigured-r16***  Indicates whether the UE supports skipping UL transmission for a configured uplink grant only if no data is available for transmission and no UCI is multiplexed on the corresponding PUSCH of the uplink grant as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***enhancedSkipUplinkTxDynamic-r16***  Indicates whether the UE supports skipping UL transmission for an uplink grant addressed to a C-RNTI only if no data is available for transmission and no UCI is multiplexed on the corresponding PUSCH of the uplink grant as specified in TS 38.321 [8]. | UE | No | Yes | No |
| *maxNumberRNTIs-MBS-r17*  Indicates the maximum number of simultaneous reception of PDCCH scrambled with G-RNTIs/G-CS-RNTIs for MBS multicast. | UE | No | No | No |
| ***lch-PriorityBasedPrioritization-r16***  Indicates whether the UE supports prioritization between overlapping grants and between scheduling request and overlapping grants based on LCH priority as specified in TS 38.321 [8]. | UE | No | No | No |
| ***lch-ToConfiguredGrantMapping-r16***  Indicates whether the UE supports restricting data transmission from a given LCH to a configured (sub-) set of configured grant configurations (see *allowedCG-List-r16* in *LogicalChannelConfig* in TS 38.331 [9]) as specified in TS 38.321 [8]. | UE | No | No | No |
| ***lch-ToGrantPriorityRestriction-r16***  Indicates whether the UE supports restricting data transmission from a given LCH to a configured (sub-) set of dynamic grant priority levels (see *allowedPHY-PriorityIndex-r16* in *LogicalChannelConfig* in TS 38.331 [9]) as specified in TS 38.321 [8]. | UE | No | No | No |
| ***lch-ToSCellRestriction***  Indicates whether the UE supports restricting data transmission from a given LCH to a configured (sub-) set of serving cells (see *allowedServingCells* in *LogicalChannelConfig*). A UE supporting *pdcp-DuplicationMCG-OrSCG-DRB* or *pdcp-DuplicationSRB* (see *PDCP-Config*) shall also support *lch-ToSCellRestriction*. | UE | No | No | No |
| ***lcp-Restriction***  Indicates whether UE supports the selection of logical channels for each UL grant based on RRC configured restriction using RRC parameters *allowedSCS-List*, *maxPUSCH-Duration*, and *configuredGrantType1Allowed* as specified in TS 38.321 [8]. | UE | No | No | No |
| ***logicalChannelSR-DelayTimer***  Indicates whether the UE supports the *logicalChannelSR-DelayTimer* as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***longDRX-Cycle***  Indicates whether UE supports long DRX cycle as specified in TS 38.321 [8]. | UE | Yes | Yes | No |
| ***multipleConfiguredGrants***  Indicates whether UE supports more than one configured grant configurations (including both Type 1 and Type 2) in a cell group. For each cell, the UE supports at most one configured grant per BWP and the maximum number of configured grant configurations per cell group is 2. If absent, for each configured cell group, the UE only supports one configured grant configuration on one serving cell. | UE | No | Yes | No |
| ***multipleSR-Configurations***  Indicates whether the UE supports 8 SR configurations per PUCCH cell group as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***recommendedBitRate***  Indicates whether the UE supports the bit rate recommendation message from the gNB to the UE as specified in TS 38.321 [8]. | UE | No | No | No |
| ***recommendedBitRateMultiplier-r16***  Indicates whether the UE supports the bit rate multiplier for recommended bit rate MAC CE as specified in TS 38.321 [8], clause 6.1.3.20. This field is only applicable if the UE supports recommendedBitRate. | UE | No | No | No |
| ***recommendedBitRateQuery***  Indicates whether the UE supports the bit rate recommendation query message from the UE to the gNB as specified in TS 38.321 [8]. This field is only applicable if the UE supports *recommendedBitRate*. | UE | No | No | No |
| ***secondaryDRX-Group-r16***  Indicates whether UE supports secondary DRX group as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***shortDRX-Cycle***  Indicates whether UE supports short DRX cycle as specified in TS 38.321 [8]. | UE | Yes | Yes | No |
| ***singlePHR-P-r16***  Indicates whether UE supports the P bit in single PHR MAC CE as specified in TS 38.321 [8]. | UE | No | No | No |
| ***skipUplinkTxDynamic***  Indicates whether the UE supports skipping of UL transmission for an uplink grant indicated on PDCCH if no data is available for transmission as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***spCell-BFR-CBRA-r16***  Indicates whether the UE supports sending BFR MAC CE for SpCell BFR as specified in TS 38.321 [8]. | UE | No | No | No |
| ***srs-ResourceId-Ext-r16***  Indicates whether the UE supports the extended 6-bit (Positioning) SRS resource ID in SP Positioning SRS Activation/Deactivation MAC CE, as specified in TS 38.321 [8]. | UE | No | No | No |
| ***tdd-MPE-P-MPR-Reporting-r16***  Indicates whether the UE supports P-MPR reporting for Maximum Permissible Exposure, as specified in TS38.321 [8]. | UE | No | TDD only | FR2 only |
| *ul-LBT-FailureDetectionRecovery-r16*  Indicates whether the UE supports consistent uplink LBT detection and recovery, as specified in TS 38.321 [8], for cells operating with shared spectrum channel access.  This field applies to all serving cells with which the UE is configured with shared spectrum channel access. | UE | No | No | No |

*Next change*

# 8 UE Capability Constraints

The following table lists constraints indicating the UE capabilities that the UE shall support.

| Parameter | Description | Value |
| --- | --- | --- |
| #DRBs | The number of DRBs that a UE shall support. | 16 per UE.  NOTE 1  NOTE 3  NOTE 4 |
| #minCellperMeasObjectNR | The minimum number of neighbour cells (excluding black list cells) that a UE shall be able to store associated with a MeasObjectNR. | 32  NOTE 2 |
| #minBlackCellRangesperMeasObjectNR | The minimum number of blacklist cell PCI ranges that a UE shall be able to store associated with a MeasObjectNR. | 8 |
| #minBlackCellperMeasObjectEUTRA | The minimum number of blacklist cells that a UE shall be able to store associated with a MeasObjectEUTRA. | 32 |
| #minCellperMeasObjectEUTRA | The minimum number of neighbour cells that a UE shall be able to store associated with a MeasObjectEUTRA. | 32  NOTE 2 |
| #minCellTotal | The minimum number of neighbour cells (excluding black list cells) that UE shall be able to store in total from all measurement objects configured. | 256 with counting CSI-RS and SSB as 2. |
| #maxDeprioritisationFreq | The UE shall be able to store a depriotisation request for up to 8 frequencies (applicable when receiving another frequency specific deprioritisation request via *RRCRelease* before T325 expiry). | 8 |
| #minCellperMeasObjectUTRA-FDD | The minimum number of neighbour cells that a UE shall be able to store associated with a MeasObjectUTRA-FDD. | 32 |
| NOTE 1: For one MAC entity, the maximum number of DRBs configured with PDCP duplication and with RLC entity(ies) associated with this MAC entity is 8.  NOTE 2: In case of CGI reporting, the limit regarding the cells configured includes the cell for which the UE is requested to report CGI i.e. the amount of neighbour cells that can be included is at most (# minCellperMeasObjectRAT - 1), where RAT represents NR and EUTRA.  NOTE 3: This requirement is applicable in NR SA, NR-DC and NE-DC.  NOTE 4: The maximum number is defined for the total number of multicast MRBs and DRBs, and the total number of DRBs for split-MRB is considered as two. | | |

*End of change*

# Annex

According to the following agreements made in RAN2#116-e, a draft subsection of RAN2 determined UE capabilities in TR 38.822 is included.

* [026] Separate UE capabilities for MBS multicast and broadcast is used.
* [026] Define a UE capability for the number of simultaneous G-RNTIs / G-CS-RNTIs reception for multicast. UE shall inform network of this capability.
* [026] A mandatory UE capability for split-bearer configurations of multicast is adopted without capability signalling.
* [026] Reuse the current defined max RB (i.e. 16 RB per UE). Additional note shall be added to TS 38.306 to clarify the max RB is a total number for MRBs and DRBs, and the total number of RBs for split-MRB is considered as two.
* [026] An optional UE capability of *maxMRB-Add* for additional MRBs support is adopted for multicast.
* [026] A set of mandatory MBS broadcast capabilities is adopted:

  PDCP short SN;

  RLC UM with short SN

  RLC UM with long SN

  DRX with long DRX cycle

* [026] No separate UE capability is needed for the maximum number of RoHC/EHC contexts for multicast MRBs. The limitation are across all DRB/ multicast MRBs configured with RoHC/EHC for a UE.
* [026] MBS DRX with long DRX cycle is mandatory for multicast capable UEs.

5.2.x NR\_MBS-Core

**Table 5.2.x-1: Layer-2 and Layer-3 feature list for NR\_MBS-Core**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Features** | **Index** | **Feature group** | **Components** | **Prerequisite feature groups** | **Field name in TS 38.331 [2]** | **Parent IE in TS 38.331 [2]** | **Need of FDD/TDD differentiation** | **Need of FR1/FR2 differentiation** | **Note** | **Mandatory/Optional** |
| x | x-1 | Additional maximum number of MRBs | Indicates the additional maximum number of MRB that the UE supports for MBS multicast reception. | [RAN1 FG 33-2] | *maxMRB-Add-r17* | *UE-NRMBS-Capability-v17x0* | No | No |  | Optional with capability signalling |
| x-2 | Number of simultaneous G-RNTIs / G-CS-RNTIs | Indicates the number of simultaneous G-RNTIs / G-CS-RNTIs reception for MBS multicast that a UE shall support. | [FFS] | *maxNumberRNTIs-MBS-r17* | *MAC-ParametersCommon* | No | No |  | Optional with capability signalling |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |