**3GPP T****SG-RAN WG2 Meeting #117-e R2-220wxyz**

**Online Meeting, 21st February– 3rd March 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.331** | **CR** | **Draft** | **rev** |  | **Current version:** | **0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft 331 CR for MBS UE capabilities | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | MediaTek Inc. | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_MBS-Core | | | | |  | ***Date:*** | | | 2022-03-02 |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | | 17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Introduction of R17 MBS feature. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | UE capabilities for R17 MBS feature. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No UE capabilities for R17 MBS feature are defined. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.3.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS38.306 CR TBD | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

# 6 Protocol data units, formats and parameters (ASN.1)

*First change*

### 6.3.3 UE capability information elements

**< *unmodified Subclauses removed*>**

#### – *MAC-Parameters*

The IE *MAC-Parameters* is used to convey capabilities related to MAC.

*MAC-Parameters* information element

-- ASN1START

-- TAG-MAC-PARAMETERS-START

MAC-Parameters ::= SEQUENCE {

mac-ParametersCommon MAC-ParametersCommon OPTIONAL,

mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL

}

MAC-Parameters-v1610 ::= SEQUENCE {

mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

MAC-ParametersCommon ::= SEQUENCE {

lcp-Restriction ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

lch-ToSCellRestriction ENUMERATED {supported} OPTIONAL,

...,

[[

recommendedBitRate ENUMERATED {supported} OPTIONAL,

recommendedBitRateQuery ENUMERATED {supported} OPTIONAL

]],

[[

recommendedBitRateMultiplier-r16 ENUMERATED {supported} OPTIONAL,

preEmptiveBSR-r16 ENUMERATED {supported} OPTIONAL,

autonomousTransmission-r16 ENUMERATED {supported} OPTIONAL,

lch-PriorityBasedPrioritization-r16 ENUMERATED {supported} OPTIONAL,

lch-ToConfiguredGrantMapping-r16 ENUMERATED {supported} OPTIONAL,

lch-ToGrantPriorityRestriction-r16 ENUMERATED {supported} OPTIONAL,

singlePHR-P-r16 ENUMERATED {supported} OPTIONAL,

ul-LBT-FailureDetectionRecovery-r16 ENUMERATED {supported} OPTIONAL,

-- R4 8-1: MPE

tdd-MPE-P-MPR-Reporting-r16 ENUMERATED {supported} OPTIONAL,

lcid-ExtensionIAB-r16 ENUMERATED {supported} OPTIONAL

]],

[[

spCell-BFR-CBRA-r16 ENUMERATED {supported} OPTIONAL

]],

[[

srs-ResourceId-Ext-r16 ENUMERATED {supported} OPTIONAL

]],

[[

maxNumberRNTIs-MBS-r17 INTEGER (1..FFS) OPTIONAL

]]

}

MAC-ParametersFRX-Diff-r16 ::= SEQUENCE {

directMCG-SCellActivation-r16 ENUMERATED {supported} OPTIONAL,

directMCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

directSCG-SCellActivation-r16 ENUMERATED {supported} OPTIONAL,

directSCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

-- R1 19-1: DRX Adaptation

drx-Adaptation-r16 SEQUENCE {

non-SharedSpectrumChAccess-r16 MinTimeGap-r16 OPTIONAL,

sharedSpectrumChAccess-r16 MinTimeGap-r16 OPTIONAL

} OPTIONAL,

...

}

MAC-ParametersXDD-Diff ::= SEQUENCE {

skipUplinkTxDynamic ENUMERATED {supported} OPTIONAL,

logicalChannelSR-DelayTimer ENUMERATED {supported} OPTIONAL,

longDRX-Cycle ENUMERATED {supported} OPTIONAL,

shortDRX-Cycle ENUMERATED {supported} OPTIONAL,

multipleSR-Configurations ENUMERATED {supported} OPTIONAL,

multipleConfiguredGrants ENUMERATED {supported} OPTIONAL,

...,

[[

secondaryDRX-Group-r16 ENUMERATED {supported} OPTIONAL

]],

[[

enhancedSkipUplinkTxDynamic-r16 ENUMERATED {supported} OPTIONAL,

enhancedSkipUplinkTxConfigured-r16 ENUMERATED {supported} OPTIONAL

]]

}

MinTimeGap-r16 ::= SEQUENCE {

scs-15kHz-r16 ENUMERATED {sl1, sl3} OPTIONAL,

scs-30kHz-r16 ENUMERATED {sl1, sl6} OPTIONAL,

scs-60kHz-r16 ENUMERATED {sl1, sl12} OPTIONAL,

scs-120kHz-r16 ENUMERATED {sl2, sl24} OPTIONAL

}

-- TAG-MAC-PARAMETERS-STOP

-- ASN1STOP

**< *unmodified Subclauses removed*>**

#### – *UE-NR-Capability*

The IE *UE-NR-Capability* is used to convey the NR UE Radio Access Capability Parameters, see TS 38.306 [26].

*UE-NR-Capability* information element

-- ASN1START

-- TAG-UE-NR-CAPABILITY-START

UE-NR-Capability ::= SEQUENCE {

accessStratumRelease AccessStratumRelease,

pdcp-Parameters PDCP-Parameters,

rlc-Parameters RLC-Parameters OPTIONAL,

mac-Parameters MAC-Parameters OPTIONAL,

phy-Parameters Phy-Parameters,

rf-Parameters RF-Parameters,

measAndMobParameters MeasAndMobParameters OPTIONAL,

fdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

tdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

fr1-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

featureSets FeatureSets OPTIONAL,

featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

lateNonCriticalExtension OCTET STRING (CONTAINING UE-NR-Capability-v15c0) OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1530 OPTIONAL

}

-- Regular non-critical extensions:

UE-NR-Capability-v1530 ::= SEQUENCE {

fdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

tdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

interRAT-Parameters InterRAT-Parameters OPTIONAL,

inactiveState ENUMERATED {supported} OPTIONAL,

delayBudgetReporting ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1540 OPTIONAL

}

UE-NR-Capability-v1540 ::= SEQUENCE {

sdap-Parameters SDAP-Parameters OPTIONAL,

overheatingInd ENUMERATED {supported} OPTIONAL,

ims-Parameters IMS-Parameters OPTIONAL,

fr1-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

fr2-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

fr1-fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1550 OPTIONAL

}

UE-NR-Capability-v1550 ::= SEQUENCE {

reducedCP-Latency ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1560 OPTIONAL

}

UE-NR-Capability-v1560 ::= SEQUENCE {

nrdc-Parameters NRDC-Parameters OPTIONAL,

receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1570 OPTIONAL

}

UE-NR-Capability-v1570 ::= SEQUENCE {

nrdc-Parameters-v1570 NRDC-Parameters-v1570 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1610 OPTIONAL

}

-- Late non-critical extensions:

UE-NR-Capability-v15c0 ::= SEQUENCE {

nrdc-Parameters-v15c0 NRDC-Parameters-v15c0 OPTIONAL,

partialFR2-FallbackRX-Req ENUMERATED {true} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v15g0 OPTIONAL

}

UE-NR-Capability-v15g0 ::= SEQUENCE {

rf-Parameters-v15g0 RF-Parameters-v15g0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical extensions:

UE-NR-Capability-v1610 ::= SEQUENCE {

inDeviceCoexInd-r16 ENUMERATED {supported} OPTIONAL,

dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

nrdc-Parameters-v1610 NRDC-Parameters-v1610 OPTIONAL,

powSav-Parameters-r16 PowSav-Parameters-r16 OPTIONAL,

fr1-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

fr2-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

bh-RLF-Indication-r16 ENUMERATED {supported} OPTIONAL,

directSN-AdditionFirstRRC-IAB-r16 ENUMERATED {supported} OPTIONAL,

bap-Parameters-r16 BAP-Parameters-r16 OPTIONAL,

referenceTimeProvision-r16 ENUMERATED {supported} OPTIONAL,

sidelinkParameters-r16 SidelinkParameters-r16 OPTIONAL,

highSpeedParameters-r16 HighSpeedParameters-r16 OPTIONAL,

mac-Parameters-v1610 MAC-Parameters-v1610 OPTIONAL,

mcgRLF-RecoveryViaSCG-r16 ENUMERATED {supported} OPTIONAL,

resumeWithStoredMCG-SCells-r16 ENUMERATED {supported} OPTIONAL,

resumeWithStoredSCG-r16 ENUMERATED {supported} OPTIONAL,

resumeWithSCG-Config-r16 ENUMERATED {supported} OPTIONAL,

ue-BasedPerfMeas-Parameters-r16 UE-BasedPerfMeas-Parameters-r16 OPTIONAL,

son-Parameters-r16 SON-Parameters-r16 OPTIONAL,

onDemandSIB-Connected-r16 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1640 OPTIONAL

}

UE-NR-Capability-v1640 ::= SEQUENCE {

redirectAtResumeByNAS-r16 ENUMERATED {supported} OPTIONAL,

phy-ParametersSharedSpectrumChAccess-r16 Phy-ParametersSharedSpectrumChAccess-r16 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1650 OPTIONAL

}

UE-NR-Capability-v1650 ::= SEQUENCE {

mpsPriorityIndication-r16 ENUMERATED {supported} OPTIONAL,

highSpeedParameters-v1650 HighSpeedParameters-v1650 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v17x0 OPTIONAL

}

UE-NR-Capability-v17x0 ::= SEQUENCE {

mbs-Parameters-v17x0 MBS-Parameters-v17x0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode ::= SEQUENCE {

phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL,

measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff

}

UE-NR-CapabilityAddFRX-Mode ::= SEQUENCE {

phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1540 ::= SEQUENCE {

ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1610 ::= SEQUENCE {

powSav-ParametersFRX-Diff-r16 PowSav-ParametersFRX-Diff-r16 OPTIONAL,

mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

BAP-Parameters-r16 ::= SEQUENCE {

flowControlBH-RLC-ChannelBased-r16 ENUMERATED {supported} OPTIONAL,

flowControlRouting-ID-Based-r16 ENUMERATED {supported} OPTIONAL

}

MBS-Parameters-v17x0 ::= SEQUENCE {

maxMRB-Add-r17 INTEGER (1..16) OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-UE-NR-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| *UE-NR-Capability* field descriptions |
| ***featureSetCombinations***  A list of *FeatureSetCombination:s* for *supportedBandCombinationList* in *UE-NR-Capability*. The *FeatureSetDownlink:s* and *FeatureSetUplink:s* referred to from these *FeatureSetCombination:s* are defined in the *featureSets* list in *UE-NR-Capability*. |

|  |
| --- |
| *UE-NR-Capability-v1540 field descriptions* |
| ***fr1-fr2-Add-UE-NR-Capabilities***  This instance of *UE-NR-CapabilityAddFRX-Mode* does not include any other fields than *csi-RS-IM-ReceptionForFeedback*/ *csi-RS-ProcFrameworkForSRS*/ *csi-ReportFramework*. |

*End of change*