**3GPP TSG- Meeting # *R2-220xxxx***

**,**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **xxxx** | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of sidelink relay capability |
|  |  |
| ***Source to WG:*** | Qualcomm Incorporated |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_SL\_Relay-Core |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Introduction of R17 features on sidelink relay.<To be added after R2#117 agreement>. |
|  |  |
| ***Summary of change:*** | UE capabilities for sidelink relay are defined.<To be added after R2#117 agreement>. |
|  |  |
| ***Consequences if not approved:*** | No UE capabilities for sidelink relay are defined. |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS/TR 38.306 CR xxxx  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*Start Change*

6.3.3 UE capability information elements

<Text Removed>

– *SidelinkParameters*

The IE *SidelinkParameters* is used to convey capabilities related to NR and V2X sidelink communications.

***SidelinkParameters* information element**

-- ASN1START

-- TAG-SIDELINKPARAMETERS-START

SidelinkParameters-r16 ::= SEQUENCE {

 sidelinkParametersNR-r16 SidelinkParametersNR-r16 OPTIONAL,

 sidelinkParametersEUTRA-r16 SidelinkParametersEUTRA-r16 OPTIONAL

}

SidelinkParameters-v17xy ::= SEQUENCE {

 sidelinkParametersNR-v17xy SidelinkParametersNR-v17xy OPTIONAL

}

SidelinkParametersNR-r16 ::= SEQUENCE {

 rlc-ParametersSidelink-r16 RLC-ParametersSidelink-r16 OPTIONAL,

 mac-ParametersSidelink-r16 MAC-ParametersSidelink-r16 OPTIONAL,

 fdd-Add-UE-Sidelink-Capabilities-r16 UE-SidelinkCapabilityAddXDD-Mode-r16 OPTIONAL,

 tdd-Add-UE-Sidelink-Capabilities-r16 UE-SidelinkCapabilityAddXDD-Mode-r16 OPTIONAL,

 supportedBandListSidelink-r16 SEQUENCE (SIZE (1..maxBands)) OF BandSidelink-r16 OPTIONAL,

 ...

}

SidelinkParametersNR-v17xy ::= SEQUENCE {

relay-Parameters-r17 Relay-Parameters-r17 OPTIONAL,

 discovery-Parameters-r17 Discovery-Parameters-r17 OPTIONAL,

 ...

}

SidelinkParametersEUTRA-r16 ::= SEQUENCE {

 sl-ParametersEUTRA1-r16 OCTET STRING OPTIONAL,

 sl-ParametersEUTRA2-r16 OCTET STRING OPTIONAL,

 sl-ParametersEUTRA3-r16 OCTET STRING OPTIONAL,

 supportedBandListSidelinkEUTRA-r16 SEQUENCE (SIZE (1..maxBandsEUTRA)) OF BandSidelinkEUTRA-r16 OPTIONAL,

 ...

}

RLC-ParametersSidelink-r16 ::= SEQUENCE {

 am-WithLongSN-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

 um-WithLongSN-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

 ...

}

MAC-ParametersSidelink-r16 ::= SEQUENCE {

 mac-ParametersSidelinkCommon-r16 MAC-ParametersSidelinkCommon-r16 OPTIONAL,

 mac-ParametersSidelinkXDD-Diff-r16 MAC-ParametersSidelinkXDD-Diff-r16 OPTIONAL,

 ...

}

UE-SidelinkCapabilityAddXDD-Mode-r16 ::= SEQUENCE {

 mac-ParametersSidelinkXDD-Diff-r16 MAC-ParametersSidelinkXDD-Diff-r16 OPTIONAL

}

MAC-ParametersSidelinkCommon-r16 ::= SEQUENCE {

 lcp-RestrictionSidelink-r16 ENUMERATED {supported} OPTIONAL,

 multipleConfiguredGrantsSidelink-r16 ENUMERATED {supported} OPTIONAL,

 ...

}

MAC-ParametersSidelinkXDD-Diff-r16 ::= SEQUENCE {

 multipleSR-ConfigurationsSidelink-r16 ENUMERATED {supported} OPTIONAL,

 logicalChannelSR-DelayTimerSidelink-r16 ENUMERATED {supported} OPTIONAL,

 ...

}

BandSidelinkEUTRA-r16 ::= SEQUENCE {

 freqBandSidelinkEUTRA-r16 FreqBandIndicatorEUTRA,

 -- R1 15-7: Transmitting LTE sidelink mode 3 scheduled by NR Uu

 gnb-ScheduledMode3SidelinkEUTRA-r16 SEQUENCE {

 gnb-ScheduledMode3DelaySidelinkEUTRA-r16 ENUMERATED {ms0, ms0dot25, ms0dot5, ms0dot625, ms0dot75, ms1,

 ms1dot25, ms1dot5, ms1dot75, ms2, ms2dot5, ms3, ms4,

 ms5, ms6, ms8, ms10, ms20}

 } OPTIONAL,

 -- R1 15-9: Transmitting LTE sidelink mode 4 configured by NR Uu

 gnb-ScheduledMode4SidelinkEUTRA-r16 ENUMERATED {supported} OPTIONAL

}

BandSidelink-r16 ::= SEQUENCE {

 freqBandSidelink-r16 FreqBandIndicatorNR,

 --15-1

 sl-Reception-r16 SEQUENCE {

 harq-RxProcessSidelink-r16 ENUMERATED {n16, n24, n32, n48, n64},

 pscch-RxSidelink-r16 ENUMERATED {value1, value2},

 scs-CP-PatternRxSidelink-r16 CHOICE {

 fr1-r16 SEQUENCE {

 scs-15kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2-r16 SEQUENCE {

 scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-120kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

 }

 } OPTIONAL,

 extendedCP-RxSidelink-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 --15-2

 sl-TransmissionMode1-r16 SEQUENCE {

 harq-TxProcessModeOneSidelink-r16 ENUMERATED {n8, n16},

 scs-CP-PatternTxSidelinkModeOne-r16 CHOICE {

 fr1-r16 SEQUENCE {

 scs-15kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2-r16 SEQUENCE {

 scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-120kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

 }

 },

 extendedCP-TxSidelink-r16 ENUMERATED {supported} OPTIONAL,

 harq-ReportOnPUCCH-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 --15-4

 sync-Sidelink-r16 SEQUENCE {

 gNB-Sync-r16 ENUMERATED {supported} OPTIONAL,

 gNB-GNSS-UE-SyncWithPriorityOnGNB-ENB-r16 ENUMERATED {supported} OPTIONAL,

 gNB-GNSS-UE-SyncWithPriorityOnGNSS-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 --15-10

 sl-Tx-256QAM-r16 ENUMERATED {supported} OPTIONAL,

 --15-11

 psfch-FormatZeroSidelink-r16 SEQUENCE {

 psfch-RxNumber ENUMERATED {n5, n15, n25, n32, n35, n45, n50, n64},

 psfch-TxNumber ENUMERATED {n4, n8, n16}

 } OPTIONAL,

 --15-12

 lowSE-64QAM-MCS-TableSidelink-r16 ENUMERATED {supported} OPTIONAL,

 --15-15

 enb-sync-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 --15-3

 sl-TransmissionMode2-r16 SEQUENCE {

 harq-TxProcessModeTwoSidelink-r16 ENUMERATED {n8, n16},

 scs-CP-PatternTxSidelinkModeTwo-r16 ENUMERATED {supported} OPTIONAL,

 dl-openLoopPC-Sidelink-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 --15-5

 congestionControlSidelink-r16 SEQUENCE {

 cbr-ReportSidelink-r16 ENUMERATED {supported} OPTIONAL,

 cbr-CR-TimeLimitSidelink-r16 ENUMERATED {time1, time2}

 } OPTIONAL,

 --15-22

 fewerSymbolSlotSidelink-r16 ENUMERATED {supported} OPTIONAL,

 --15-23

 sl-openLoopPC-RSRP-ReportSidelink-r16 ENUMERATED {supported} OPTIONAL,

 --13-1

 sl-Rx-256QAM-r16 ENUMERATED {supported} OPTIONAL

 ]]

}

Discovery-Parameters-r17 ::= SEQUENCE {

 relay-discovery-r17 ENUMERATED {supported} OPTIONAL,

 non-relay-discovery-r17 ENUMERATED {supported} OPTIONAL,

 ...

}

Realy-Parameters-r17 ::= SEQUENCE {

 relayUE-Operation-L2-r17 ENUMERATED {supported} OPTIONAL,

 remoteUE-Operation-L2-r17 ENUMERATED {supported} OPTIONAL,

 ...

}

-- TAG-SIDELINKPARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| ***SidelinkParametersEUTRA* field descriptions** |
| ***sl-ParametersEUTRA1, sl-ParametersEUTRA2, sl-ParametersEUTRA3***This field includes IE of *SL-Parameters-v1430* (where *v2x-eNB-Scheduled-r14* and *V2X-SupportedBandCombination-r14* shall not be included), *SL-Parameters-v1530* (where *V2X-SupportedBandCombination-r1530* shall not be included) and *SL-Parameters-v1540* respectively defined in 36.331 [10]. It is used for reporting the per-UE capability for V2X sidelink communication. |

<Text Removed>

– *UE-NR-Capability*

The IE *UE-NR-Capability* is used to convey the NR UE Radio Access Capability Parameters, see TS 38.306 [26].

***UE-NR-Capability* information element**

-- ASN1START

-- TAG-UE-NR-CAPABILITY-START

UE-NR-Capability ::= SEQUENCE {

 accessStratumRelease AccessStratumRelease,

 pdcp-Parameters PDCP-Parameters,

 rlc-Parameters RLC-Parameters OPTIONAL,

 mac-Parameters MAC-Parameters OPTIONAL,

 phy-Parameters Phy-Parameters,

 rf-Parameters RF-Parameters,

 measAndMobParameters MeasAndMobParameters OPTIONAL,

 fdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

 tdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

 fr1-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 featureSets FeatureSets OPTIONAL,

 featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

 lateNonCriticalExtension OCTET STRING (CONTAINING UE-NR-Capability-v15c0) OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1530 OPTIONAL

}

-- Regular non-critical extensions:

UE-NR-Capability-v1530 ::= SEQUENCE {

 fdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 tdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 interRAT-Parameters InterRAT-Parameters OPTIONAL,

 inactiveState ENUMERATED {supported} OPTIONAL,

 delayBudgetReporting ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1540 OPTIONAL

}

UE-NR-Capability-v1540 ::= SEQUENCE {

 sdap-Parameters SDAP-Parameters OPTIONAL,

 overheatingInd ENUMERATED {supported} OPTIONAL,

 ims-Parameters IMS-Parameters OPTIONAL,

 fr1-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

 fr2-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

 fr1-fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1550 OPTIONAL

}

UE-NR-Capability-v1550 ::= SEQUENCE {

 reducedCP-Latency ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1560 OPTIONAL

}

UE-NR-Capability-v1560 ::= SEQUENCE {

 nrdc-Parameters NRDC-Parameters OPTIONAL,

 receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1570 OPTIONAL

}

UE-NR-Capability-v1570 ::= SEQUENCE {

 nrdc-Parameters-v1570 NRDC-Parameters-v1570 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1610 OPTIONAL

}

-- Late non-critical extensions:

UE-NR-Capability-v15c0 ::= SEQUENCE {

 nrdc-Parameters-v15c0 NRDC-Parameters-v15c0 OPTIONAL,

 partialFR2-FallbackRX-Req ENUMERATED {true} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v15g0 OPTIONAL

}

UE-NR-Capability-v15g0 ::= SEQUENCE {

 rf-Parameters-v15g0 RF-Parameters-v15g0 OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical extensions:

UE-NR-Capability-v1610 ::= SEQUENCE {

 inDeviceCoexInd-r16 ENUMERATED {supported} OPTIONAL,

 dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

 nrdc-Parameters-v1610 NRDC-Parameters-v1610 OPTIONAL,

 powSav-Parameters-r16 PowSav-Parameters-r16 OPTIONAL,

 fr1-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

 fr2-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

 bh-RLF-Indication-r16 ENUMERATED {supported} OPTIONAL,

 directSN-AdditionFirstRRC-IAB-r16 ENUMERATED {supported} OPTIONAL,

 bap-Parameters-r16 BAP-Parameters-r16 OPTIONAL,

 referenceTimeProvision-r16 ENUMERATED {supported} OPTIONAL,

 sidelinkParameters-r16 SidelinkParameters-r16 OPTIONAL,

 highSpeedParameters-r16 HighSpeedParameters-r16 OPTIONAL,

 mac-Parameters-v1610 MAC-Parameters-v1610 OPTIONAL,

 mcgRLF-RecoveryViaSCG-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithStoredMCG-SCells-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithStoredSCG-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithSCG-Config-r16 ENUMERATED {supported} OPTIONAL,

 ue-BasedPerfMeas-Parameters-r16 UE-BasedPerfMeas-Parameters-r16 OPTIONAL,

 son-Parameters-r16 SON-Parameters-r16 OPTIONAL,

 onDemandSIB-Connected-r16 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1640 OPTIONAL

}

UE-NR-Capability-v1640 ::= SEQUENCE {

 redirectAtResumeByNAS-r16 ENUMERATED {supported} OPTIONAL,

 phy-ParametersSharedSpectrumChAccess-r16 Phy-ParametersSharedSpectrumChAccess-r16 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1650 OPTIONAL

}

UE-NR-Capability-v1650 ::= SEQUENCE {

 mpsPriorityIndication-r16 ENUMERATED {supported} OPTIONAL,

 highSpeedParameters-v1650 HighSpeedParameters-v1650 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v17xy OPTIONAL

}

UE-NR-Capability-v17xy ::= SEQUENCE {

 sidelinkParameters-v17xy SidelinkParameters-v17xy OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode ::= SEQUENCE {

 phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

 mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL,

 measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

 eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff

}

UE-NR-CapabilityAddFRX-Mode ::= SEQUENCE {

 phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

 measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1540 ::= SEQUENCE {

 ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1610 ::= SEQUENCE {

 powSav-ParametersFRX-Diff-r16 PowSav-ParametersFRX-Diff-r16 OPTIONAL,

 mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

BAP-Parameters-r16 ::= SEQUENCE {

 flowControlBH-RLC-ChannelBased-r16 ENUMERATED {supported} OPTIONAL,

 flowControlRouting-ID-Based-r16 ENUMERATED {supported} OPTIONAL

}

-- TAG-UE-NR-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| ***UE-NR-Capability* field descriptions** |
| ***featureSetCombinations***A list of *FeatureSetCombination:s* for *supportedBandCombinationList* in *UE-NR-Capability*. The *FeatureSetDownlink:s* and *FeatureSetUplink:s* referred to from these *FeatureSetCombination:s* are defined in the *featureSets* list in *UE-NR-Capability*. |

|  |
| --- |
| ***UE-NR-Capability-v1540 field descriptions*** |
| ***fr1-fr2-Add-UE-NR-Capabilities***This instance of *UE-NR-CapabilityAddFRX-Mode* does not include any other fields than *csi-RS-IM-ReceptionForFeedback*/ *csi-RS-ProcFrameworkForSRS*/ *csi-ReportFramework*. |

*End of Change*