3GPP TSG-RAN WG2 Meeting #118-e R2-220xxxx

Electronic, 9th May – 20th May 2022

**Agenda Item: 6.10.1.1**

**Source: CMCC**

**Title:** **Report of [AT118][0XX][NTN] reply LSs to CT1 (CMCC)**

**Document for: Discussion**

# Introduction

This document aims for gathering and summarizing companies’ views for the following offline discussion:

* [AT118-e][114][NTN] Reply LSs to CT1 (CMCC)

 Initial scope: Discuss whether some minimal update to 38.304 is needed related to the CT1 LS on list of PLMNs not allowed to operate at the present UE location and the need/content of a reply LS for CT1 LS about NR satellite RAT type in UE NAS

 Initial intended outcome: Agreeable TP for a 38.304 CR on list of PLMNs not allowed to operate at the present UE location and reply LS to CT1 on NR satellite RAT type in UE NAS

 Deadline (for companies' feedback): Tuesday 2022-05-16 12:00 UTC

 Deadline (for rapporteur's summary in R2-2206206): Tuesday 2022-05-17 08:00 UTC

**Note1:** All the proposals listed in the summary will be categorized into two types:

* **Type1:** proposal for agreement, e.g. reach consensus by the majority.
* **Type2:** proposal needs further discussion.

Contact table

|  |  |
| --- | --- |
| **Company** | **Contact details (name, e-mail)** |
| CMCC | chaili@chinamobile.com |
| Apple | pnuggehalli@apple.com |
| Lenovo | xumin13@lenovo.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Discussion

In last meeting, CT1 had sent LS to RAN2 on LS introducing the list of PLMNs not allowed to operate at the present UE location as below:

|  |
| --- |
| CT1 is working on the support of PLMN selection for satellite NG-RAN access technology, and has introduced a list of "PLMNs not allowed to operate at the present UE location". In this list for each entry there could be information related to whether or not the PLMN is allowed within a certain area.**To RAN2** **ACTION:** CT1 kindly asks to RAN2 to take above information into account for their future work on this work item. |

Per the agreed CRs in CT1, the UE shall store a list of "PLMNs not allowed to operate at the present UE location" as follows:

- *the PLMN identity of the PLMN which sent a message including 5GMM cause value #78 "PLMN not allowed to operate at the present UE location" via satellite NG-RAN access technology;*

*- the geographical location, if known by the UE, where 5GMM cause value #78 was received on satellite NG-RAN access technology;*

*- the distance to the current UE location;*

*- a timer which is started upon the UE receiving an integrity protected reject message with cause value #78 "PLMNs not allowed to operate at the present UE location" from a satellite NG-RAN cell.*

Therefore, the UE’s behaviours are as follows:

* In NTN, when a UE receives an reject message with cause value #78 "PLMNs not allowed to operate at the present UE location" from a NTN cell, the UE maintains a list of "PLMNs not allowed to operate at the present UE location" in which it stores the PLMN ID of the rejecting PLMN, and the current geographical location and a timer.
* And the List can be removed when the timer associated to the entry expires or the UE successfully registers to the PLMN stored in the entry.



Hence, in our understanding, since NOT ALL the coverage of the PLMN is forbidden, only the **partial coverage** which fulfils the conditions as depicted in 1) is not allowed to the UE, the information should be transmitted to the AS to facilitate the cell selection and re-selection. That is, during cell selection, the UE should take the list into account as **the list of “Forbidden TAs”**.

**Q1: which part is impacted by the new introduced list of "PLMNs not allowed to operate at the present UE location"?**

***A: Functional division between AS and NAS in RRC\_IDLE state and RRC\_INACTIVE state***

***B: Defintion of suitable cell***

***C: Cell selection/re-selection, e.g., description on Cells with cell reservations, access restrictions or unsuitable for normal camping***

***D: None***

|  |  |  |
| --- | --- | --- |
| **Company** | **Which part do you prefer** | **comments** |
| CMCC | A,B,C | From our understanding, since NOT ALL the coverage of the PLMN is forbidden, only the **partial coverage** which fulfils the conditions as depicted in 1) is not allowed to the UE, the information should be transmitted to the AS to facilitate the cell selection and re-selection. That is, during cell selection, the UE should take the list into account as **the list of “Forbidden TAs”.** |
| Apple | A or D | It seems cleaner from the spec point of view to let NAS deal with all aspects related to PLMN selection including located based aspects.  |
| Lenovo | A at least, B and C optional | At least we need to indicate in 4.2 of 38.304, that it is NAS to maintain a list of “PLMNs not allowed to operate at the present UE location”. The list may need to be provided to AS if impacts are identified.For B and C, we see some regulation requirements of forbidding UE access to a certain PLMN at certain locations, e.g. country border area. In our understanding it is about in what granularity do we need to meet the requirements. If the NTN cell coverage can align with borders or the regulation needs to be strictly complied, then B and C are reasonable to implement at cell level. Besides, as Rel-18 is considering UE location verification in NR NTN e.g. to fulfil the requirements defined in 22.926, implementation at verified location level is also an option. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2: If any part you prefer to update, please provide your text description.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Which part do you prefer** | **comments** |
| CMCC | A,B,C | As the TP part shown in [4]  |
| Apple | A | Can reuse the part of the provided TP impacting A |
| Lenoco | A at least, B and C can be accepted | As we replied to Q1, B and C is a possible option of implementing “PLMNs not allowed to operate at the present UE location”. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Besides, in the last meeting, RAN2 received an LS from CT1 describing the NR satellite RAT type in UE NAS[1]:

|  |
| --- |
| *CT1 is discussing extending NAS supervision timers at NR satellite access based on information on RAN delay provided in a Reply LS (C1-220079 / R2-2111612) and there have been discussions in CT1 to consider whether the NAS solution should take NR satellite RAT type into account for possible differentiation of the applied NAS timer extension.**CT1 understands that NR satellite RAT type (LEO/MEO/GEO/OTHERSAT) is provided to the AMF from the gNB via NGAP, but is not aware of any corresponding indication available to the NAS at the UE.**CT1 would therefore like to know:** *Is indication of the NR satellite RAT type available, or planned to be made available, to the NAS at the UE?*
* *If such indication is available, or will be available, can it be trusted that the UE value corresponds to the value provided to the AMF?*

*CT1 would like to make clear that there currently is no common agreement to differentiate extended NAS timers based on NR satellite RAT type even if NR satellite RAT type is available, or will be available, to the NAS at the UE.* |

For Question 1, in our understanding, UE can know the NW type implicitly through the satellite assistance information in *SIB19*, e.g. Ephemeris data, common TA parameters, koffset, validity duration for UL sync information and epoch time. However, such information is only available in AS layer. So far it seems RAN2 has not specified any solution on how to enable the NAS to be notified about this information yet.

**Q3: Do you agreed that so far RAN2 has not specified any solution on how to enable the NAS to be notified about this information yet.**

**.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **comments** |
| CMCC | agree | Currently, such information is only available in AS layer. |
| Apple | agree |  |
| Lenovo | Agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

From the LS, it seems that the information of NR satellite RAT type is possible to facilitate the differentiation of the applied NAS timer extension.

**Q4: If you agree Q3, do you agree that such indication of the NR satellite RAT type is helpful for NAS and support to forward the NR satellite RAT type from AS to the NAS at the UE side?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **comments** |
| CMCC | agree | From the LS, it seems that the information of NR satellite RAT type is possible to facilitate the differentiation of the applied NAS timer extension. And maybe there are other benefits, anyway, the identification of the benefit is CT1/SA2’s scope. Hence, we support to forward the NR satellite RAT type to the NAS at the UE. |
| Apple | Disagree | It is for CT1 to decide whether this information is needed in NAS or not.  |
| Lenovo | Agree | We are OK to ask in LS if NR satellite RAT type is needed at NAS. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

For Question 2 in the LS, since the AS layer in UE side indentify the NR satellite RAT type (LEO/MEO/GEO/OTHERSAT) implicitly through the satellite assistance information in *SIB19* broadcasted by gN*B*, e.g. Ephemeris data, common TA parameters, koffset, validity duration for UL sync information and epoch time. In principle, it will be align with the value gNB provided to the AMF. However, whether there are some uncertain error during type deriving depends on the UE implemention.

**Q5: Do you agree that since the AS layer in UE side derive the NR satellite RAT type (LEO/MEO/GEO/OTHERSAT) implicitly through the satellite assistance information in *SIB19* broadcasted by gN*B*. In principle, it will be align with the value gNB provided to the AMF. However, whether there are some uncertain error during type deriving depends on the UE implemention.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **comments** |
| CMCC | agree |  |
| Apple | Disagree | We expect all UEs will use the information broadcast in SIB19 to reach the same determination abour satellite NR type |
| Lenovo | Agree with comments | We think the UE-derived result shall align with the value gNB provided to the AMF. Therefore the last sentence may not be necessary. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q6: Do you agree that a reply LS is needed for the LS (C1-222098)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **comments** |
| CMCC | agree | The reply is needed for at least for the the NAS solution of differentiation of the applied NAS timer extension. |
| Apple | Agree | We should simply inform CT1 that satellite type information is available at the AS layer |
| Lenovo | Agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q7: If you agree to send a reply LS to CT1, which point would you like to mentioned in the LS?**

|  |  |
| --- | --- |
| **Company** | **comments** |
| CMCC | 1: For Question 1, the information of NR satellite RAT type is only available in AS layer. Per that the information is possible to facilitate the differentiation of the applied NAS timer extension indicated in the LS from CT1, RAN2 is planning to support forwarding the NR satellite RAT type to the NAS at the UE.2: For Question 2, since the AS layer in UE side derive the NR satellite RAT type (LEO/MEO/GEO/OTHERSAT) implicitly through the satellite assistance information in SIB19 broadcasted by gNB. In principle, it will be align with the value gNB provided to the AMF. However, whether there are some uncertain error during the type deriving depends on the UE implemention. |
| Apple | 1. We should inform CT1 that satellite type information is available at the AS layer. Whether CT1 decides to use the information or not should have no impact on our specs. 2. We should say RAN2 expects that the satellite type provided by UE should align with the type provided by the gNB to the AMF. |
| Lenovo | 1. Availability of satellite type information at AS, which could be helpful for NAS. 2. UE-derived RAT type aligns with the value provided to the AMF by gNB. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Summary

# References

1. [R2-2204450](file:///C%3A%5C%5CData%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2204450_C1-222096.doc%22%20%5Co%20%22C%3AData3GPPExtractsR2-2204450_C1-222096.doc) LS on introducing the list of PLMNs not allowed to operate at the present UE location (C1-222096; contact: CMCC) CT1 LS in Rel-17 5GSAT\_ARCH-CT To:RAN2
2. 23122\_CR0741r7\_(Rel-17)\_C1-221824-was-C1-221056\_23122\_cause78\_forbidn\_geo\_area\_05
3. 24501\_CR3975r1\_(Rel-17)\_C1-221744-was-C1-221073\_24501\_cond\_78\_list\_06

1. [R2-2205158](file:///C%3A%5C%5CData%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2205158%20Impact%20on%20Cell%20selection%20re-selection%20by%20the%20new%20PLMN%20list%20from%20CT1.docx%22%20%5Co%20%22C%3AData3GPPExtractsR2-2205158%20Impact%20on%20Cell%20selection%20re-selection%20by%20the%20new%20PLMN%20list%20from%20CT1.docx) Impact on Cell selection/re-selection by the new PLMN list from CT1 CMCC discussion Rel-17 NR\_NTN\_solutions-Core
2. [R2-2205159](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2205159%20draft%20Reply%20LS%20on%20introducing%20the%20list%20of%20PLMNs%20not%20allowed%20to%20operate%20at%20the%20present%20UE%20location.docx) draft Reply LS on introducing the list of PLMNs not allowed to operate at the present UE location CMCC LS out Rel-17 NR\_NTN\_solutions-Core To:CT1
3. R2-2204070 NR satellite RAT type in UE NAS (C1-222098; contact: Ericsson) CT1 LS in Rel-17 To:RAN2 Cc:RAN3, SA2
4. [R2-2205027](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2205027%20Discussion%20on%20CT1%20LS%20about%20NR%20satellite%20RAT%20type%20in%20UE%20NAS.docx) Discussion on CT1 LS about NR satellite RAT type in UE NAS CMCC discussion Rel-17 NR\_NTN\_solutions-Core
5. [R2-2205028](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2205028%20%5BDRAFT%5D%20Reply%20LS%20to%20CT1%20on%20NR%20satellite%20RAT%20type%20in%20UE%20NAS.docx) [DRAFT] Reply LS on NR satellite RAT type in UE NAS CMCC LS out Rel-17 NR\_NTN\_solutions-Core To:CT1 Cc:RAN3, SA2