3GPP TSG-RAN WG2 Meeting #119 Electronic R2-220xxxx

Elbonia, 17 – 26 August 2022

**Agenda item: 5.1.2**

**Source: Nokia (Rapporteur)**

**Title:** **[****309][R15/16 UP] CRs on UP (Nokia)**

**Document for: Discussion and Decision**

# 1 Introduction

This document is the report of the following email discussion:

* [AT119-e][309][R15/16 UP] CRs on UP (Nokia)

UP open issues and agreeable CRs capturing agreed corrections

Deadline: Monday Aug 22nd, 1000, UTC

[R2-2207896](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2207896.zip) Clarification on BFD while SCell is deactivated Nokia, Nokia Shanghai Bell CR Rel-16 38.321 16.9.0 1347 - F NR\_eMIMO-Core

[R2-2207897](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2207897.zip) Clarification on BFD while SCell is deactivated Nokia, Nokia Shanghai Bell CR Rel-17 38.321 17.1.0 1348 - A NR\_eMIMO-Core

[R2-2207898](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2207898.zip) Clarification on the matching TB size for 2-step RA Nokia, Nokia Shanghai Bell CR Rel-16 38.321 16.9.0 1349 - F NR\_2step\_RACH-Core

[R2-2207899](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2207899.zip) Clarification on the matching TB size for 2-step RA Nokia, Nokia Shanghai Bell CR Rel-17 38.321 17.1.0 1350 - A NR\_2step\_RACH-Core

[R2-2208024](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208024.zip) Clarification on configuredGrantTimer and cg-RetransmissionTimer Nokia, Nokia Shanghai Bell CR Rel-16 38.321 16.9.0 1362 - F TEI16, NR\_unlic-Core

[R2-2208025](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208025.zip) Clarification on configuredGrantTimer and cg-RetransmissionTimer Nokia, Nokia Shanghai Bell CR Rel-17 38.321 17.1.0 1363 - A TEI16, NR\_unlic-Core, NR\_SmallData\_INACTIVE-Core

[R2-2208254](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208254.zip) Correction on RA Resource Selection in Rel-15 vivo CR Rel-15 38.321 15.13.0 1373 - F NR\_newRAT-Core

[R2-2208261](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208261.zip) Correction on RA Resource Selection in Rel-16 vivo CR Rel-16 38.321 16.9.0 1375 - F NR\_newRAT-Core, NR\_2step\_RACH-Core

[R2-2208263](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208263.zip) Correction on RA Resource Selection in Rel-17 vivo CR Rel-17 38.321 17.1.0 1376 - A NR\_newRAT-Core, NR\_2step\_RACH-Core

# 2 Contact Points

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Nokia (Rapporteur) | SunYoung LEE | sunyoung.lee@nokia.com |
| Samsung | Sangkyu Baek | sangkyu.baek@samsung.com |
| Qualcomm | Linhai He | linhaihe@qti.qualcomm.com |
| LGE | Gyeong-Cheol LEE | gyeongcheol.lee@lge.com |
| Huawei, HiSilicon | Chong Lou | louchong@huawei.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Discussion

## 3.1 BFD while SCell is deactivated

[R2-2207896](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2207896.zip) Clarification on BFD while SCell is deactivated Nokia, Nokia Shanghai Bell CR Rel-16 38.321 16.9.0 1347 - F NR\_eMIMO-Core

[R2-2207897](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2207897.zip) Clarification on BFD while SCell is deactivated Nokia, Nokia Shanghai Bell CR Rel-17 38.321 17.1.0 1348 - A NR\_eMIMO-Core

It is proposed to clarify that BFD is performed only while the SCell is activated so that UE does not unnecessarily perform BFD/BFR and send BFR MAC CE while the SCell is deactivated.

**Question 1**: Do companies agree with the issue? If yes, are the proposed changes fine?

|  |
| --- |
| Answers to Question 1 |
| Company | Agree with the issue? (Yes/No) | If yes, are the proposed changes fine or are there any suggestion for improvement? If no, why? |
| Samsung | No | The source of confusion is that PHY may send beam failure instance indication. This is what RAN1 spec should capture. MAC spec only captures only beam failure recovery for which the current MAC spec is clear.  |
| Qualcomm | No | There is no issue, because it is already specified in the RAN4 spec that UE is not required to perform BFD measurements for a deactivated SCell. See clause 8.5.1 in TS 38.133. |
| LG | No | In MAC specification, “Beam failure is detected by counting beam failure instance indication from the lower layers to the MAC entity.” Thus, if beam failure instance indication is not received from PHY, the MAC entity will not detect beam failure. If any clarification is needed, it should be specified in RAN1 specification. |
| Huawei, HiSilicon | No | Agree with above comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 1**: TBD.

**Proposal 1**: TBD.

## 3.2 Matching TB size for 2-step RA

[R2-2207898](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2207898.zip) Clarification on the matching TB size for 2-step RA Nokia, Nokia Shanghai Bell CR Rel-16 38.321 16.9.0 1349 - F NR\_2step\_RACH-Core

[R2-2207899](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2207899.zip) Clarification on the matching TB size for 2-step RA Nokia, Nokia Shanghai Bell CR Rel-17 38.321 17.1.0 1350 - A NR\_2step\_RACH-Core

It is proposed to replace 'corresponds to' by 'matches with' because the intention is to check whether the TB size of two TBs are of the same or not.

**Question 2**: Do companies agree with the issue? If yes, are the proposed changes fine?

|  |
| --- |
| Answers to Question 2 |
| Company | Yes/No | If yes, are the proposed changes fine or are there any suggestion for improvement? If no, why? |
| Samsung | Yes/No | Not essential, but ok to clarify. No strong view |
| Qualcomm | Neutral | If majority of companies want to change the wording, maybe it can be included in the next rapporteur’s CR. |
| LG | Yes |  |
| Huawei, HiSilicon | No | Not essential, we don’t see any room for misunderstanding on the current wording.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 2**: TBD.

**Proposal 2**: TBD.

## 3.3 configuredGrantTimer and cg-RetransmissionTimer

[R2-2208024](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208024.zip) Clarification on configuredGrantTimer and cg-RetransmissionTimer Nokia, Nokia Shanghai Bell CR Rel-16 38.321 16.9.0 1362 - F TEI16, NR\_unlic-Core

[R2-2208025](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208025.zip) Clarification on configuredGrantTimer and cg-RetransmissionTimer Nokia, Nokia Shanghai Bell CR Rel-17 38.321 17.1.0 1363 - A TEI16, NR\_unlic-Core, NR\_SmallData\_INACTIVE-Core

It is explained that the current spec is not clear whether the MAC checks whether the *configuredGrantTimer*/*cg-RetransmissionTimer* is running at the time of PUSCH transmission or at the time when the MAC processes the UL grant. It is proposed to clearly specify that the MAC checks whether the timer is running at the time of corresponding PUSCH transmission, i.e., regardless of when the UE starts processing of the UL grant.

**Question 3**: Do companies agree with the issue? If yes, are the proposed changes fine?

|  |
| --- |
| Answers to Question 3 |
| Company | Yes/No | If yes, are the proposed changes fine or are there any suggestion for improvement? If no, why? |
| Samsung | No | Even in Rel-15, UE checks if *configuredGrantTimer* is running immediately before the MAC delivers configuration grant information to the HARQ entity. This is not a Rel-16 specific issue. There is no other way to interpret the current text even if the proposed changes are correct. In our view, the proposed changes are not essential so not needed. |
| Qualcomm | See comment | We agree that the current spec text is a bit vague and there is room for potential misunderstanding. But we doubt there would be a UE implementation which uses the state of timer at the time of UL grant processing instead of at start of PUSCH Tx when checking the condition. For R16, since in theory the proposed change is an NBC (if we are not mistaken), make no change to the spec. For R17, we are fine with adopting the proposed change to eliminate the potential ambiguity. |
| LGE | No | The *configuredGrantTimer* is configured as a number of periodicity. When the *configuredGrantTimer* is set to N, the correct UE behaviour is that new transmission using the CG should be blocked by this running *configuredGrantTimer* only for N\*periodicity. However, if the MAC determines whether *configuredGrantTimer* is running at the time when the MAC processes the UL grant, this would block new transmission for (N+1)\*periodicity and this is different from the original intention. Thus, we think that if the MAC specification is correctly implemented, this already should be based on at the time of PUSCH transmission without this clarification.  |
| Huawei, HiSilicon | No | It is obvious that the UE check the CG timer for each CG occasion from the spec, but the time point to check is total up to UE implementation. We tend to believe there is no ambiguity for sensible UE implementation in the field.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 3**: TBD.

**Proposal 3**: TBD.

## 3.4 RA Resource Selection

[R2-2208254](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208254.zip) Correction on RA Resource Selection in Rel-15 vivo CR Rel-15 38.321 15.13.0 1373 - F NR\_newRAT-Core

[R2-2208261](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208261.zip) Correction on RA Resource Selection in Rel-16 vivo CR Rel-16 38.321 16.9.0 1375 - F NR\_newRAT-Core, NR\_2step\_RACH-Core

[R2-2208263](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208263.zip) Correction on RA Resource Selection in Rel-17 vivo CR Rel-17 38.321 17.1.0 1376 - A NR\_newRAT-Core, NR\_2step\_RACH-Core

It is explained that, during RA procedure, the MAC does not deliver the selected SSB/CSI-RS to the PHY, which results in degraded performance of UL transmission. It is proposed to clarify that the MAC indicates the selected SSB/CSI-RS to the PHY.

**Question 4**: Do companies agree with the issue? If yes, are the proposed changes fine?

|  |
| --- |
| Answers to Question 4 |
| Company | Yes/No | If yes, are the proposed changes fine or are there any suggestion for improvement? If no, why? |
| Samsung | No | It is already assumed that this information is already sent to PHY layer. MAC does not capture all relevant cross-layer interaction. No room for misunderstanding. |
| Qualcomm | No | Same view as Samsung. It is not needed, as there is no room for misunderstanding. |
| LGE | No | In section 5.1.3, when the MAC instructs the selected PRACH occasion to the PHY as shown below yellow highlight, we think that the MAC already deliver the selected SSB/CSI-RS information to the PHY because the PRACH occasion is associated with the selected SSB or CSI-RS. 1> instruct the physical layer to transmit the Random Access Preamble using the selected PRACH occasion, corresponding RA-RNTI (if available), PREAMBLE\_INDEX, and PREAMBLE\_RECEIVED\_TARGET\_POWER. |
| Huawei, HiSilicon | No | Agree with above comments.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 4**: TBD.

**Proposal 4**: TBD.

# 4 Conclusion

TBD.