**3GPP TSG-RAN2 Meeting #119e *R2-2208822***

**Electronic, 17th – 29th August, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.331** | **CR** | 3321 | **rev** | **1** | **Current version:** | 17.1.0 |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction for SRS-PeriodicityAndOffset | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | RAN2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_pos-Core | | | | |  | ***Date:*** | | | 2022-08-17 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | RAN1#99 has agreed that the periodicities of the SRS for positioning support the union of periodicities (and associated slot offsets) supported for NR SRS Rel-15 and the NR DL-PRS Rel-16:  Agreement:  The union of periodicities (and associated slot offsets) supported for NR SRS Rel-15 and the NR DL-PRS Rel-16 is supported for SRS for positioning in Rel-16.  And RAN1#99 has agreed the following periodicity values are supported depending on SCS for NR DL-PRS Rel-16:  Agreement:  The following periodicity values of DL PRS resource allocation are supported depending on SCS   * {4, 5, 8, 10, 16, 20, 32, 40, 64, 80, 160, 320, 640, 1280, 2560, 5120, 10240} slots, µ = 0, 1, 2, 3 for SCS 15, 30, 60 and 120kHz respectively   However, the relationship between SCS and the periodicity is not mentioned in the current description in 38.331. And the periodicity for pos-SRS with 128, 256, 512, and 20480 slots is missing in the current RRC spec. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clarify that the periodicity values of SRS for positioning are supported depending on SCS, and add the value *sl128, sl256, sl512,* and *sl20480* in the *SRS-PeriodicityAndOffset-r16,* and add the capability *srs-ExtendedPeriodictyAndOffset-v16xy* in the UE capability information elements to ensure backward compatibility. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The periodicity of SRS for positioning is not aligned with the RAN1 agreement.  **Impact analysis**  **Impacted functionality:**  UL-TDOA positioning, and UL-AOA positioning  **Inter-operability:**  There is no inter-operability issue on dependence on the periodicity and SCS.  For the missing periodicity, if the UE is implemented according to the CR while the network is not, there is no inter-operability issue.  If the network is implemented according to the CR while the UE is not, the UE may not be able to correctly transmit SRS resource for positioning. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.3.2, 6.3.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 38.306 CR0781 | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Ver0 in RAN2#119e: R2-2207874  Ver1 in RAN2#119e: R2-2208822 | | | | | | | | |

=========================================================CHANGE BEGINS=======================================================

### 6.3.2 Radio resource control information elements

– *SRS-Config*

The IE *SRS-Config* is used to configure sounding reference signal transmissions. The configuration defines a list of SRS-Resources, a list of SRS-PosResources, a list of SRS-PosResourceSets and a list of SRS-ResourceSets. Each resource set defines a set of SRS-Resources or SRS-PosResources. The network triggers the transmission of the set of SRS-Resources or SRS-PosResources using a configured aperiodicSRS-ResourceTrigger (L1 DCI). The network does not configure SRS specific power control parameters, *alpha, p0* or *pathlossReferenceRS* if *unifiedTCI-StateType* is configured for the serving cell.

***SRS-Config* information element**

-- ASN1START

-- TAG-SRS-CONFIG-START

SRS-Config ::= SEQUENCE {

srs-ResourceSetToReleaseList SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSetId OPTIONAL, -- Need N

srs-ResourceSetToAddModList SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSet OPTIONAL, -- Need N

srs-ResourceToReleaseList SEQUENCE (SIZE(1..maxNrofSRS-Resources)) OF SRS-ResourceId OPTIONAL, -- Need N

srs-ResourceToAddModList SEQUENCE (SIZE(1..maxNrofSRS-Resources)) OF SRS-Resource OPTIONAL, -- Need N

tpc-Accumulation ENUMERATED {disabled} OPTIONAL, -- Need S

...,

[[

srs-RequestDCI-1-2-r16 INTEGER (1..2) OPTIONAL, -- Need S

srs-RequestDCI-0-2-r16 INTEGER (1..2) OPTIONAL, -- Need S

srs-ResourceSetToAddModListDCI-0-2-r16 SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSet OPTIONAL, -- Need N

srs-ResourceSetToReleaseListDCI-0-2-r16 SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSetId OPTIONAL, -- Need N

srs-PosResourceSetToReleaseList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSetId-r16

OPTIONAL, -- Need N

srs-PosResourceSetToAddModList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSet-r16 OPTIONAL,-- Need N

srs-PosResourceToReleaseList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResourceId-r16 OPTIONAL,-- Need N

srs-PosResourceToAddModList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResource-r16 OPTIONAL -- Need N

]]

}

SRS-ResourceSet ::= SEQUENCE {

srs-ResourceSetId SRS-ResourceSetId,

srs-ResourceIdList SEQUENCE (SIZE(1..maxNrofSRS-ResourcesPerSet)) OF SRS-ResourceId OPTIONAL, -- Cond Setup

resourceType CHOICE {

aperiodic SEQUENCE {

aperiodicSRS-ResourceTrigger INTEGER (1..maxNrofSRS-TriggerStates-1),

csi-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

slotOffset INTEGER (1..32) OPTIONAL, -- Need S

...,

[[

aperiodicSRS-ResourceTriggerList SEQUENCE (SIZE(1..maxNrofSRS-TriggerStates-2))

OF INTEGER (1..maxNrofSRS-TriggerStates-1) OPTIONAL -- Need M

]]

},

semi-persistent SEQUENCE {

associatedCSI-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

...

},

periodic SEQUENCE {

associatedCSI-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

...

}

},

usage ENUMERATED {beamManagement, codebook, nonCodebook, antennaSwitching},

alpha Alpha OPTIONAL, -- Need S

p0 INTEGER (-202..24) OPTIONAL, -- Cond Setup

pathlossReferenceRS PathlossReferenceRS-Config OPTIONAL, -- Need M

srs-PowerControlAdjustmentStates ENUMERATED { sameAsFci2, separateClosedLoop} OPTIONAL, -- Need S

...,

[[

pathlossReferenceRSList-r16 SetupRelease { PathlossReferenceRSList-r16} OPTIONAL -- Need M

]],

[[

usagePDC-r17 ENUMERATED {true} OPTIONAL, -- Need R

availableSlotOffsetList-r17 SEQUENCE (SIZE(1..4)) OF AvailableSlotOffset-r17 OPTIONAL, -- Need R

followUnifiedTCIstateSRS-r17 ENUMERATED {enabled} OPTIONAL -- Need R

]]

}

AvailableSlotOffset-r17 ::= INTEGER (0..7)

PathlossReferenceRS-Config ::= CHOICE {

ssb-Index SSB-Index,

csi-RS-Index NZP-CSI-RS-ResourceId

}

PathlossReferenceRSList-r16 ::= SEQUENCE (SIZE (1..maxNrofSRS-PathlossReferenceRS-r16)) OF PathlossReferenceRS-r16

PathlossReferenceRS-r16 ::= SEQUENCE {

srs-PathlossReferenceRS-Id-r16 SRS-PathlossReferenceRS-Id-r16,

pathlossReferenceRS-r16 PathlossReferenceRS-Config

}

SRS-PathlossReferenceRS-Id-r16 ::= INTEGER (0..maxNrofSRS-PathlossReferenceRS-1-r16)

SRS-PosResourceSet-r16 ::= SEQUENCE {

srs-PosResourceSetId-r16 SRS-PosResourceSetId-r16,

srs-PosResourceIdList-r16 SEQUENCE (SIZE(1..maxNrofSRS-ResourcesPerSet)) OF SRS-PosResourceId-r16

OPTIONAL, -- Cond Setup

resourceType-r16 CHOICE {

aperiodic-r16 SEQUENCE {

aperiodicSRS-ResourceTriggerList-r16 SEQUENCE (SIZE(1..maxNrofSRS-TriggerStates-1))

OF INTEGER (1..maxNrofSRS-TriggerStates-1) OPTIONAL, -- Need M

...

},

semi-persistent-r16 SEQUENCE {

...

},

periodic-r16 SEQUENCE {

...

}

},

alpha-r16 Alpha OPTIONAL, -- Need S

p0-r16 INTEGER (-202..24) OPTIONAL, -- Cond Setup

pathlossReferenceRS-Pos-r16 CHOICE {

ssb-IndexServing-r16 SSB-Index,

ssb-Ncell-r16 SSB-InfoNcell-r16,

dl-PRS-r16 DL-PRS-Info-r16

} OPTIONAL, -- Need M

...

}

SRS-ResourceSetId ::= INTEGER (0..maxNrofSRS-ResourceSets-1)

SRS-PosResourceSetId-r16 ::= INTEGER (0..maxNrofSRS-PosResourceSets-1-r16)

SRS-Resource ::= SEQUENCE {

srs-ResourceId SRS-ResourceId,

nrofSRS-Ports ENUMERATED {port1, ports2, ports4},

ptrs-PortIndex ENUMERATED {n0, n1 } OPTIONAL, -- Need R

transmissionComb CHOICE {

n2 SEQUENCE {

combOffset-n2 INTEGER (0..1),

cyclicShift-n2 INTEGER (0..7)

},

n4 SEQUENCE {

combOffset-n4 INTEGER (0..3),

cyclicShift-n4 INTEGER (0..11)

}

},

resourceMapping SEQUENCE {

startPosition INTEGER (0..5),

nrofSymbols ENUMERATED {n1, n2, n4},

repetitionFactor ENUMERATED {n1, n2, n4}

},

freqDomainPosition INTEGER (0..67),

freqDomainShift INTEGER (0..268),

freqHopping SEQUENCE {

c-SRS INTEGER (0..63),

b-SRS INTEGER (0..3),

b-hop INTEGER (0..3)

},

groupOrSequenceHopping ENUMERATED { neither, groupHopping, sequenceHopping },

resourceType CHOICE {

aperiodic SEQUENCE {

...

},

semi-persistent SEQUENCE {

periodicityAndOffset-sp SRS-PeriodicityAndOffset,

...

},

periodic SEQUENCE {

periodicityAndOffset-p SRS-PeriodicityAndOffset,

...

}

},

sequenceId INTEGER (0..1023),

spatialRelationInfo SRS-SpatialRelationInfo OPTIONAL, -- Need R

...,

[[

resourceMapping-r16 SEQUENCE {

startPosition-r16 INTEGER (0..13),

nrofSymbols-r16 ENUMERATED {n1, n2, n4},

repetitionFactor-r16 ENUMERATED {n1, n2, n4}

} OPTIONAL -- Need R

]],

[[

spatialRelationInfo-PDC-r17 SetupRelease { SpatialRelationInfo-PDC-r17 } OPTIONAL, -- Need M

resourceMapping-r17 SEQUENCE {

startPosition-r17 INTEGER (0..13),

nrofSymbols-r17 ENUMERATED {n1, n2, n4, n8, n10, n12, n14},

repetitionFactor-r17 ENUMERATED {n1, n2, n4, n5, n6, n7, n8, n10, n12, n14}

} OPTIONAL, -- Need R

partialFreqSounding-r17 SEQUENCE {

startRBIndexFScaling-r17 CHOICE{

startRBIndexAndFreqScalingFactor2-r17 INTEGER (0..1),

startRBIndexAndFreqScalingFactor4-r17 INTEGER (0..3)

},

enableStartRBHopping-r17 ENUMERATED {enable} OPTIONAL -- Need R

} OPTIONAL, -- Need R

transmissionComb-n8-r17 SEQUENCE {

combOffset-n8-r17 INTEGER (0..7),

cyclicShift-n8-r17 INTEGER (0..5)

} OPTIONAL, -- Need R

srs-TCIState-r17 CHOICE {

srs-UL-TCIState-r17 TCI-UL-State-Id-r17,

srs-DLorJoint-TCIState-r17 TCI-StateId

} OPTIONAL -- Need R

]]

}

-- Editor's note: It is FFS to determine whether to introduce serving cell ID and/or BWP ID to be associated with srs-UL-TCIState-r17

-- or srs DLorJoint-TCIState-r17.

SRS-PosResource-r16::= SEQUENCE {

srs-PosResourceId-r16 SRS-PosResourceId-r16,

transmissionComb-r16 CHOICE {

n2-r16 SEQUENCE {

combOffset-n2-r16 INTEGER (0..1),

cyclicShift-n2-r16 INTEGER (0..7)

},

n4-r16 SEQUENCE {

combOffset-n4-r16 INTEGER (0..3),

cyclicShift-n4-r16 INTEGER (0..11)

},

n8-r16 SEQUENCE {

combOffset-n8-r16 INTEGER (0..7),

cyclicShift-n8-r16 INTEGER (0..5)

},

...

},

resourceMapping-r16 SEQUENCE {

startPosition-r16 INTEGER (0..13),

nrofSymbols-r16 ENUMERATED {n1, n2, n4, n8, n12}

},

freqDomainShift-r16 INTEGER (0..268),

freqHopping-r16 SEQUENCE {

c-SRS-r16 INTEGER (0..63),

...

},

groupOrSequenceHopping-r16 ENUMERATED { neither, groupHopping, sequenceHopping },

resourceType-r16 CHOICE {

aperiodic-r16 SEQUENCE {

slotOffset-r16 INTEGER (1..32) OPTIONAL, -- Need S

...

},

semi-persistent-r16 SEQUENCE {

periodicityAndOffset-sp-r16 SRS-PeriodicityAndOffset-r16,

...,

[[

periodicityAndOffset-sp-Ext-r16 SRS-PeriodicityAndOffsetExt-r16 OPTIONAL -- Need R

]]

},

periodic-r16 SEQUENCE {

periodicityAndOffset-p-r16 SRS-PeriodicityAndOffset-r16,

...,

[[

periodicityAndOffset-p-Ext-r16 SRS-PeriodicityAndOffsetExt-r16 OPTIONAL -- Need R

]]

}

},

sequenceId-r16 INTEGER (0..65535),

spatialRelationInfoPos-r16 SRS-SpatialRelationInfoPos-r16 OPTIONAL, -- Need R

...

}

SRS-SpatialRelationInfo ::= SEQUENCE {

servingCellId ServCellIndex OPTIONAL, -- Need S

referenceSignal CHOICE {

ssb-Index SSB-Index,

csi-RS-Index NZP-CSI-RS-ResourceId,

srs SEQUENCE {

resourceId SRS-ResourceId,

uplinkBWP BWP-Id

}

}

}

SRS-SpatialRelationInfoPos-r16 ::= CHOICE {

servingRS-r16 SEQUENCE {

servingCellId ServCellIndex OPTIONAL, -- Need S

referenceSignal-r16 CHOICE {

ssb-IndexServing-r16 SSB-Index,

csi-RS-IndexServing-r16 NZP-CSI-RS-ResourceId,

srs-SpatialRelation-r16 SEQUENCE {

resourceSelection-r16 CHOICE {

srs-ResourceId-r16 SRS-ResourceId,

srs-PosResourceId-r16 SRS-PosResourceId-r16

},

uplinkBWP-r16 BWP-Id

}

}

},

ssb-Ncell-r16 SSB-InfoNcell-r16,

dl-PRS-r16 DL-PRS-Info-r16

}

SSB-Configuration-r16 ::= SEQUENCE {

ssb-Freq-r16 ARFCN-ValueNR,

halfFrameIndex-r16 ENUMERATED {zero, one},

ssbSubcarrierSpacing-r16 SubcarrierSpacing,

ssb-Periodicity-r16 ENUMERATED { ms5, ms10, ms20, ms40, ms80, ms160, spare2,spare1 } OPTIONAL, -- Need S

sfn0-Offset-r16 SEQUENCE {

sfn-Offset-r16 INTEGER (0..1023),

integerSubframeOffset-r16 INTEGER (0..9) OPTIONAL -- Need R

} OPTIONAL, -- Need R

sfn-SSB-Offset-r16 INTEGER (0..15),

ss-PBCH-BlockPower-r16 INTEGER (-60..50) OPTIONAL -- Cond Pathloss

}

SSB-InfoNcell-r16 ::= SEQUENCE {

physicalCellId-r16 PhysCellId,

ssb-IndexNcell-r16 SSB-Index OPTIONAL, -- Need S

ssb-Configuration-r16 SSB-Configuration-r16 OPTIONAL -- Need S

}

DL-PRS-Info-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

dl-PRS-ResourceSetId-r16 INTEGER (0..7),

dl-PRS-ResourceId-r16 INTEGER (0..63) OPTIONAL -- Need S

}

SRS-ResourceId ::= INTEGER (0..maxNrofSRS-Resources-1)

SRS-PosResourceId-r16 ::= INTEGER (0..maxNrofSRS-PosResources-1-r16)

SRS-PeriodicityAndOffset ::= CHOICE {

sl1 NULL,

sl2 INTEGER(0..1),

sl4 INTEGER(0..3),

sl5 INTEGER(0..4),

sl8 INTEGER(0..7),

sl10 INTEGER(0..9),

sl16 INTEGER(0..15),

sl20 INTEGER(0..19),

sl32 INTEGER(0..31),

sl40 INTEGER(0..39),

sl64 INTEGER(0..63),

sl80 INTEGER(0..79),

sl160 INTEGER(0..159),

sl320 INTEGER(0..319),

sl640 INTEGER(0..639),

sl1280 INTEGER(0..1279),

sl2560 INTEGER(0..2559)

}

SRS-PeriodicityAndOffset-r16 ::= CHOICE {

sl1 NULL,

sl2 INTEGER(0..1),

sl4 INTEGER(0..3),

sl5 INTEGER(0..4),

sl8 INTEGER(0..7),

sl10 INTEGER(0..9),

sl16 INTEGER(0..15),

sl20 INTEGER(0..19),

sl32 INTEGER(0..31),

sl40 INTEGER(0..39),

sl64 INTEGER(0..63),

sl80 INTEGER(0..79),

sl160 INTEGER(0..159),

sl320 INTEGER(0..319),

sl640 INTEGER(0..639),

sl1280 INTEGER(0..1279),

sl2560 INTEGER(0..2559),

sl5120 INTEGER(0..5119),

sl10240 INTEGER(0..10239),

sl40960 INTEGER(0..40959),

sl81920 INTEGER(0..81919),

...

}

SRS-PeriodicityAndOffsetExt-r16 ::= CHOICE {

sl128 INTEGER(0..127),

sl256 INTEGER(0..255),

sl512 INTEGER(0..511),

sl20480 INTEGER(0..20479)

}

SpatialRelationInfo-PDC-r17 ::= SEQUENCE {

referenceSignal CHOICE {

ssb-Index SSB-Index,

csi-RS-Index NZP-CSI-RS-ResourceId,

dl-PRS-PDC NR-DL-PRS-ResourceID-r17,

srs SEQUENCE {

resourceId SRS-ResourceId,

uplinkBWP BWP-Id

},

...

},

...

}

-- TAG-SRS-CONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***SRS-Config* field descriptions** |
| ***tpc-Accumulation***  If the field is absent, UE applies TPC commands via accumulation. If disabled, UE applies the TPC command without accumulation (this applies to SRS when a separate closed loop is configured for SRS) (see TS 38.213 [13], clause 7.3). |

|  |
| --- |
| ***SRS-Resource, SRS-PosResource* field descriptions** |
| ***cyclicShift-n2***  Cyclic shift configuration (see TS 38.214 [19], clause 6.2.1). |
| ***cyclicShift-n4***  Cyclic shift configuration (see TS 38.214 [19], clause 6.2.1). |
| ***enableStartRBHopping***  When this RRC parameter is configured, start RB location hopping is enabled for partial frequency sounding in different SRS frequency hopping periods for periodic/semi-persistent/aperiodic SRS as described in Clause 6.4.1.4 in TS 38.211. |
| ***freqHopping***  Includes parameters capturing SRS frequency hopping (see TS 38.214 [19], clause 6.2.1). For CLI SRS-RSRP measurement, the network always configures this field such that *b-hop* > *b-SRS*. |
| ***groupOrSequenceHopping***  Parameter(s) for configuring group or sequence hopping (see TS 38.211 [16], clause 6.4.1.4.2). For CLI SRS-RSRP measurement, the network always configures this parameter to 'neither'. |
| ***nrofSRS-Ports***  Number of ports. For CLI SRS-RSRP measurement, the network always configures this parameter to 'port1'. |
| ***periodicityAndOffset-p, periodicityAndOffset-p-Ext***  Periodicity and slot offset for this SRS resource. All values are in "number of slots". Value *sl1* corresponds to a periodicity of 1 slot, value *sl2* corresponds to a periodicity of 2 slots, and so on. For each periodicity the corresponding offset is given in number of slots. For periodicity *sl1* the offset is 0 slots (see TS 38.214 [19], clause 6.2.1). For CLI SRS-RSRP measurement, *sl1280* and *sl2560* cannot be configured. For SRS-PosResource, *sl20480*, *sl40960* and *sl81920* cannot be configured for SCS=15kHz, *sl40960* and *sl81920* cannot be configured for SCS=30kHz, and *sl81920* cannot be configured for SCS=60kHz.  When the field *periodicityAndOffset-p-Ext* is present, the field *periodicityAndOffset-p* shall be ignored by the UE. When the field *periodicityAndOffset-p* is present, the field *periodicityAndOffset-p-Ext* shall be absent. |
| ***periodicityAndOffset-sp, periodicityAndOffset-sp-Ext***  Periodicity and slot offset for this SRS resource. All values are in "number of slots". Value *sl1* corresponds to a periodicity of 1 slot, value *sl2* corresponds to a periodicity of 2 slots, and so on. For each periodicity the corresponding offset is given in number of slots. For periodicity *sl1* the offset is 0 slots (see TS 38.214 [19], clause 6.2.1). For SRS-PosResource, *sl20480*, *sl40960* and *sl81920* cannot be configured for SCS=15kHz, *sl40960* and *sl81920* cannot be configured for SCS=30kHz, and *sl81920* cannot be configured for SCS=60kHz.  When the field *periodicityAndOffset-sp-Ext* is present, the field *periodicityAndOffset-sp* shall be ignored by the UE. When the field *periodicityAndOffset-sp* is present, the field *periodicityAndOffset-sp-Ext* shall be absent. |
| ***ptrs-PortIndex***  The PTRS port index for this SRS resource for non-codebook based UL MIMO. This is only applicable when the corresponding *PTRS-UplinkConfig* is set to CP-OFDM. The *ptrs-PortIndex* configured here must be smaller than the *maxNrofPorts* configured in the *PTRS-UplinkConfig* (see TS 38.214 [19], clause 6.2.3.1). This parameter is not applicable to CLI SRS-RSRP measurement. |
| ***resourceMapping***  OFDM symbol location of the SRS resource within a slot including *nrofSymbols* (number of OFDM symbols), *startPosition* (value 0 refers to the last symbol, value 1 refers to the second last symbol, and so on) and *repetitionFactor* (see TS 38.214 [19], clause 6.2.1 and TS 38.211 [16], clause 6.4.1.4). The configured SRS resource does not exceed the slot boundary. If *resourceMapping-r16* is signalled, UE shall ignore the *resourceMapping* (without suffix). If *resourceMapping-r17* is signalled, UE shall ignore the *resourceMapping* (without suffix) and only the values of nrofSymbols which are integer multiples of the configured repetitionFactor can be configured. For CLI SRS-RSRP measurement, the network always configures *nrofSymbols* and *repetitionFactor* to 'n1'. |
| ***resourceType***  Periodicity and offset for semi-persistent and periodic SRS resource (see TS 38.214 [19], clause 6.2.1). For CLI SRS-RSRP measurement, only 'periodic' is applicable for *resourceType*. |
| ***sequenceId***  Sequence ID used to initialize pseudo random group and sequence hopping (see TS 38.214 [19], clause 6.2.1). |
| ***servingCellId***  The serving Cell ID of the source SSB, CSI-RS, or SRS for the spatial relation of the target SRS resource. If this field is absent the SSB, the CSI-RS, or the SRS is from the same serving cell where the SRS is configured. |
| ***spatialRelationInfo***  Configuration of the spatial relation between a reference RS and the target SRS. Reference RS can be SSB/CSI-RS/SRS (see TS 38.214 [19], clause 6.2.1). This parameter is not applicable to CLI SRS-RSRP measurement. |
| ***spatialRelationInfo-PDC***  Configuration of the spatial relation between a reference RS and the target SRS. Reference RS can be SSB/CSI-RS/SRS/DL-PRS-PDC (see TS 38.214 [19], clause 6.2.1). The field is present in case of *resourceType=periodic* and *usagePDC-r17=true* in the *SRS-ResourceSet*, otherwise the field is absent. |
| ***spatialRelationInfoPos***  Configuration of the spatial relation between a reference RS and the target SRS. Reference RS can be SSB/CSI-RS/SRS/DL-PRS (see TS 38.214 [19], clause 6.2.1).  If the IE *srs-ResourceId-Ext* is present, the IE *srs-ResourceId* in *spatialRelationInfoPos* represents the index from 0 to 63. Otherwise the IE *srs-ResourceId* in *spatialRelationInfoPos* represents the index from 0 to 31. |
| ***srs-RequestDCI-0-2***  Indicate the number of bits for "SRS request"in DCI format 0\_2. When the field is absent, then the value of 0 bit for "SRS request" in DCI format 0\_2 is applied. If the parameter *srs-RequestDCI-0-2* is configured to value 1, 1 bit is used to indicate one of the first two rows of Table 7.3.1.1.2-24 in TS 38.212 [17] for triggered aperiodic SRS resource set. If the value 2 is configured, 2 bits are used to indicate one of the rows of Table 7.3.1.1.2-24 in TS 38.212 [17]. When UE is configured with *supplementaryUplink*, an extra bit (the first bit of the SRS request field) is used for the non-SUL/SUL indication. |
| ***srs-RequestDCI-1-2***  Indicate the number of bits for "SRS request" in DCI format 1\_2. When the field is absent, then the value of 0 bit for "SRS request" in DCI format 1\_2 is applied. When the UE is configured with *supplementaryUplink*, an extra bit (the first bit of the SRS request field) is used for the non-SUL/SUL indication (see TS 38.214 [19], clause 6.1.1.2). |
| ***srs-ResourceSetToAddModListDCI-0-2***  List of SRS resource set to be added or modified for DCI format 0\_2 (see TS 38.212 [17], clause 7.3.1). |
| ***srs-ResourceSetToReleaseListDCI-0-2***  List of SRS resource set to be released for DCI format 0\_2 (see TS 38.212 [17], clause 7.3.1). |
| ***srs-TCIState***  Configuration of either a UL TCI state or a joint TCI state for the SRS resource. This field is absent when the SRS resource is in a *SRS-ResourceSet* configured with *followUnifiedTCIstateSRS-r17* or when the field *unifiedTCI-StateType* is not configured to the serving cell which the SRS resource is located in. |
| ***startRBIndexAndFreqScalingFactor***  Configures the UE with the startRBIndex and freqScalingFactor for partial frequency sounding as described in Clause 6.4.1.4 in TS 38.211. The startRBIndexForFScaling2 gives the startRBIndex when freqScalingFactor is 2 and the startRBIndexForFScaling4 gives the startRBIndex when FreqScalingFactor is 4 |
| ***transmissionComb, transmissionComb-n8***  Comb value (2 or 4 or 8) and comb offset (0..combValue-1) (see TS 38.214 [19], clause 6.2.1). |

=======================================================NEXT CHANGE========================================================

### 6.3.3 UE capability information elements

– *Phy-Parameters*

The IE *Phy-Parameters* is used to convey the physical layer capabilities.

***Phy-Parameters* information element**

-- ASN1START

-- TAG-PHY-PARAMETERS-START

Phy-Parameters ::= SEQUENCE {

phy-ParametersCommon Phy-ParametersCommon OPTIONAL,

phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

phy-ParametersFR1 Phy-ParametersFR1 OPTIONAL,

phy-ParametersFR2 Phy-ParametersFR2 OPTIONAL

}

Phy-ParametersCommon ::= SEQUENCE {

csi-RS-CFRA-ForHO ENUMERATED {supported} OPTIONAL,

dynamicPRB-BundlingDL ENUMERATED {supported} OPTIONAL,

sp-CSI-ReportPUCCH ENUMERATED {supported} OPTIONAL,

sp-CSI-ReportPUSCH ENUMERATED {supported} OPTIONAL,

nzp-CSI-RS-IntefMgmt ENUMERATED {supported} OPTIONAL,

type2-SP-CSI-Feedback-LongPUCCH ENUMERATED {supported} OPTIONAL,

precoderGranularityCORESET ENUMERATED {supported} OPTIONAL,

dynamicHARQ-ACK-Codebook ENUMERATED {supported} OPTIONAL,

semiStaticHARQ-ACK-Codebook ENUMERATED {supported} OPTIONAL,

spatialBundlingHARQ-ACK ENUMERATED {supported} OPTIONAL,

dynamicBetaOffsetInd-HARQ-ACK-CSI ENUMERATED {supported} OPTIONAL,

pucch-Repetition-F1-3-4 ENUMERATED {supported} OPTIONAL,

ra-Type0-PUSCH ENUMERATED {supported} OPTIONAL,

dynamicSwitchRA-Type0-1-PDSCH ENUMERATED {supported} OPTIONAL,

dynamicSwitchRA-Type0-1-PUSCH ENUMERATED {supported} OPTIONAL,

pdsch-MappingTypeA ENUMERATED {supported} OPTIONAL,

pdsch-MappingTypeB ENUMERATED {supported} OPTIONAL,

interleavingVRB-ToPRB-PDSCH ENUMERATED {supported} OPTIONAL,

interSlotFreqHopping-PUSCH ENUMERATED {supported} OPTIONAL,

type1-PUSCH-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

type2-PUSCH-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

pusch-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

pdsch-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

downlinkSPS ENUMERATED {supported} OPTIONAL,

configuredUL-GrantType1 ENUMERATED {supported} OPTIONAL,

configuredUL-GrantType2 ENUMERATED {supported} OPTIONAL,

pre-EmptIndication-DL ENUMERATED {supported} OPTIONAL,

cbg-TransIndication-DL ENUMERATED {supported} OPTIONAL,

cbg-TransIndication-UL ENUMERATED {supported} OPTIONAL,

cbg-FlushIndication-DL ENUMERATED {supported} OPTIONAL,

dynamicHARQ-ACK-CodeB-CBG-Retx-DL ENUMERATED {supported} OPTIONAL,

rateMatchingResrcSetSemi-Static ENUMERATED {supported} OPTIONAL,

rateMatchingResrcSetDynamic ENUMERATED {supported} OPTIONAL,

bwp-SwitchingDelay ENUMERATED {type1, type2} OPTIONAL,

...,

[[

dummy ENUMERATED {supported} OPTIONAL

]],

[[

maxNumberSearchSpaces ENUMERATED {n10} OPTIONAL,

rateMatchingCtrlResrcSetDynamic ENUMERATED {supported} OPTIONAL,

maxLayersMIMO-Indication ENUMERATED {supported} OPTIONAL

]],

[[

spCellPlacement CarrierAggregationVariant OPTIONAL

]],

[[

-- R1 9-1: Basic channel structure and procedure of 2-step RACH

twoStepRACH-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-1: Monitoring DCI format 1\_2 and DCI format 0\_2

dci-Format1-2And0-2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-1a: Monitoring both DCI format 0\_1/1\_1 and DCI format 0\_2/1\_2 in the same search space

monitoringDCI-SameSearchSpace-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-10: Type 2 configured grant release by DCI format 0\_1

type2-CG-ReleaseDCI-0-1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-11: Type 2 configured grant release by DCI format 0\_2

type2-CG-ReleaseDCI-0-2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-3: SPS release by DCI format 1\_1

sps-ReleaseDCI-1-1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-3a: SPS release by DCI format 1\_2

sps-ReleaseDCI-1-2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 14-8: CSI trigger states containing non-active BWP

csi-TriggerStateNon-ActiveBWP-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-2: Support up to 4 SMTCs configured for an IAB node MT per frequency location, including IAB-specific SMTC window periodicities

separateSMTC-InterIAB-Support-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-3: Support RACH configuration separately from the RACH configuration for UE access, including new IAB-specific offset and scaling factors

separateRACH-IAB-Support-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-5a: Support semi-static configuration/indication of UL-Flexible-DL slot formats for IAB-MT resources

ul-flexibleDL-SlotFormatSemiStatic-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-5b: Support dynamic indication of UL-Flexible-DL slot formats for IAB-MT resources

ul-flexibleDL-SlotFormatDynamics-IAB-r16 ENUMERATED {supported} OPTIONAL,

dft-S-OFDM-WaveformUL-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-6: Support DCI Format 2\_5 based indication of soft resource availability to an IAB node

dci-25-AI-RNTI-Support-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-7: Support T\_delta reception.

t-DeltaReceptionSupport-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-8: Support of Desired guard symbol reporting and provided guard symbok reception.

guardSymbolReportReception-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-8 HARQ-ACK codebook type and spatial bundling per PUCCH group

harqACK-CB-SpatialBundlingPUCCH-Group-r16 ENUMERATED {supported} OPTIONAL,

-- R1 19-2: Cross Slot Scheduling

crossSlotScheduling-r16 SEQUENCE {

non-SharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL,

sharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

maxNumberSRS-PosPathLossEstimateAllServingCells-r16 ENUMERATED {n1, n4, n8, n16} OPTIONAL,

extendedCG-Periodicities-r16 ENUMERATED {supported} OPTIONAL,

extendedSPS-Periodicities-r16 ENUMERATED {supported} OPTIONAL,

codebookVariantsList-r16 CodebookVariantsList-r16 OPTIONAL,

-- R1 11-6: PUSCH repetition Type A

pusch-RepetitionTypeA-r16 SEQUENCE {

sharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL,

non-SharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 11-4b: DL priority indication in DCI with mixed DCI formats

dci-DL-PriorityIndicator-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-1a: UL priority indication in DCI with mixed DCI formats

dci-UL-PriorityIndicator-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1e: Maximum number of configured pathloss reference RSs for PUSCH/PUCCH/SRS by RRC for MAC-CE based pathloss reference RS update

maxNumberPathlossRS-Update-r16 ENUMERATED {n4, n8, n16, n32, n64} OPTIONAL,

-- R1 18-9: Usage of the PDSCH starting time for HARQ-ACK type 2 codebook

type2-HARQ-ACK-Codebook-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1g-1: Resources for beam management, pathloss measurement, BFD, RLM and new beam identification across frequency ranges

maxTotalResourcesForAcrossFreqRanges-r16 SEQUENCE {

maxNumberResWithinSlotAcrossCC-AcrossFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n64, n128} OPTIONAL,

maxNumberResAcrossCC-AcrossFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n40, n48, n64, n72, n80, n96, n128, n256}

OPTIONAL

} OPTIONAL,

-- R1 16-2a-4: HARQ-ACK for multi-DCI based multi-TRP – separate

harqACK-separateMultiDCI-MultiTRP-r16 SEQUENCE {

maxNumberLongPUCCHs-r16 ENUMERATED {longAndLong, longAndShort, shortAndShort} OPTIONAL

} OPTIONAL,

-- R1 16-2a-4: HARQ-ACK for multi-DCI based multi-TRP – joint

harqACK-jointMultiDCI-MultiTRP-r16 ENUMERATED {supported} OPTIONAL,

-- R4 9-1: BWP switching on multiple CCs RRM requirements

bwp-SwitchingMultiCCs-r16 CHOICE {

type1-r16 ENUMERATED {us100, us200},

type2-r16 ENUMERATED {us200, us400, us800, us1000}

} OPTIONAL

]],

[[

targetSMTC-SCG-r16 ENUMERATED {supported} OPTIONAL,

supportRepetitionZeroOffsetRV-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-12: in-order CBG-based re-transmission

cbg-TransInOrderPUSCH-UL-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R4 6-3: Dormant BWP switching on multiple CCs RRM requirements

bwp-SwitchingMultiDormancyCCs-r16 CHOICE {

type1-r16 ENUMERATED {us100, us200},

type2-r16 ENUMERATED {us200, us400, us800, us1000}

} OPTIONAL,

-- R1 16-2a-8: Indicates that retransmission scheduled by a different CORESETPoolIndex for multi-DCI multi-TRP is not supported.

supportRetx-Diff-CoresetPool-Multi-DCI-TRP-r16 ENUMERATED {notSupported} OPTIONAL,

-- R1 22-10: Support of pdcch-MonitoringAnyOccasionsWithSpanGap in case of cross-carrier scheduling with different SCSs

pdcch-MonitoringAnyOccasionsWithSpanGapCrossCarrierSch-r16 ENUMERATED {mode2, mode3} OPTIONAL

]],

[[

-- R1 16-1j-1: Support of 2 port CSI-RS for new beam identification

newBeamIdentifications2PortCSI-RS-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1j-2: Support of 2 port CSI-RS for pathloss estimation

pathlossEstimation2PortCSI-RS-r16 ENUMERATED {supported} OPTIONAL

]],

[[

mux-HARQ-ACK-withoutPUCCH-onPUSCH-r16 ENUMERATED {supported} OPTIONAL

]],

[[

srs-PeriodicityAndOffsetExt-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 31-1: Support of Desired Guard Symbol reporting and provided guard symbol reception.

guardSymbolReportReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-2: support of restricted IAB-DU beam reception

restricted-IAB-DU-BeamReception-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-3: support of recommended IAB-MT beam transmission for DL and UL beam

recommended-IAB-MT-BeamTransmission-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-4: support of case 6 timing alignment indication reception

case6-TimingAlignmentReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-5: support of case 7 timing offset indication reception and case 7 timing at parent-node indication reception

case7-TimingAlignmentReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-6: support of desired DL Tx power adjustment reporting and DL Tx power adjustment reception

dl-tx-PowerAdjustment-IAB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-7: support of desired IAB-MT PSD range reporting

desired-ul-tx-PowerAdjustment-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-8: support of monitoring DCI Format 2\_5 scrambled by AI-RNTI for indication of FDM soft resource availability to an IAB node

fdm-SoftResourceAvailability-DynamicIndication-r17 ENUMERATED{supported} OPTIONAL,

-- R1 31-10: Support of updated T\_delta range reception

updated-T-DeltaRangeRecption-r17 ENUMERATED{supported} OPTIONAL,

-- R1 30-5: Support slot based dynamic PUCCH repetition indication for PUCCH formats 0/1/2/3/4

slotBasedDynamicPUCCH-Rep-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-1: Support of HARQ-ACK deferral in case of TDD collision

sps-HARQ-ACK-Deferral-r17 SEQUENCE {

non-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

sharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 23-1-1k Maximum number of configured CC lists (per UE)

unifiedJointTCI-commonUpdate-r17 INTEGER (1..4) OPTIONAL,

-- R1 23-2-1c PDCCH repetition with a single span of three contiguous OFDM symbols that is within the first four OFDM symbols in a slot

mTRP-PDCCH-singleSpan-r17 ENUMERATED {supported} OPTIONAL,

-- R1 27-23: Support of more than one activated PRS processing windows across all active DL BWPs

supportedActivatedPRS-ProcessingWindow-r17 ENUMERATED {n2, n3, n4} OPTIONAL,

cg-TimeDomainAllocationExtension-r17 ENUMERATED {supported} OPTIONAL

]]

}

=======================================================END OF CHANGES========================================================