3GPP TSG-RAN WG2 Meeting #119 electronic R2-2208871

Online, 17th August – 29th August, 2022

Agenda Item: 6.1.2

Source: Huawei, HiSilicon

Title: [AT119-e][601][MBS-R17] RRC corrections

Document for: Discussion and Decision

# 1 Introduction

This document aims at summarizing the following offline discussion:

* [AT119-e][601][MBS-R17] RRC corrections (Huawei)

Phase 2 scope: Resolve remaining RRC issues

Phase 2 outcome: Report, 38.331 MBS corrections CR

Deadline (Phase 2): Report available: 2022-08-24 1200 UTC, agreeable CR: EOM

This is a follow up offline discussing of [Pre119-e][601][MBS-R17] Summary of A.I. 6.1.2 RRC corrections (Huawei). The corresponding summary documents can be found in the [draft folder](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119-e/Inbox/Drafts/%5BPre119-e%5D%5B601%5D%5BMBS-R17%5D%20Summary%20of%20A.I.%206.1.2%20%20RRC%20corrections%20%28Huawei%29).

The following deadlines are suggested:

* For initial inputs to questions listed in this document and comments on the 38.331 CR for MBS
	+ Deadline: Tuesday 2022-08-24 0100 UTC
* Summary of the offline and updated 38.331 CR for MBS
	+ Deadline: Wednesday 2022-08-24, 1200 UTC

# 2 Contact information

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 RRC corrections to be discussed

3.1 Correction 01

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2207032 | An MBS capable UE in RRC\_CONNECTED may initiate the procedure in several cases including upon successful connection establishment/resume, upon entering or leaving the broadcast service area, upon MBS broadcast session start or stop, upon change of interest, upon change of priority between MBS broadcast reception and unicast/multicast reception, upon change to a PCell in which the SIB1 scheduling information contains *SIB21*, upon receiving *SIB20* of an SCell via dedicated signalling, upon handover.Upon initiating the procedure, the UE shall:1> if *SIB21* is in the SIB1 scheduling information of the PCell:2> ensure having a valid version of *SIB21* for the PCell;2> if the UE did not transmit MBS Interest Indication since last entering RRC\_CONNECTED state; or2> if since the last time the UE transmitted an MBS Interest Indication, the UE connected to a PCell in which the SIB1 scheduling information does not contain *SIB21*:3> if the set of MBS broadcast frequencies of interest, determined in accordance with 5.9.4.3, is not empty:4> set the contents of MBS Interest Indication according to 5.9.4.5 and initiate transmission of the *MBSInterestIndication* message;2> else:3> if the set of MBS broadcast frequencies of interest, determined in accordance with 5.9.4.3, is different from *mbs-FreqList* included in the last transmission of the MBS Interest Indication; or3> if the prioritisation of reception of all indicated MBS broadcast frequencies compared to reception of any of the established unicast bearers and multicast MRBs has changed since the last transmission of the MBS Interest Indication:4> set the contents of MBS Interest Indication according to 5.9.4.5 and initiate transmission of the *MBSInterestIndication* message;NOTE: The UE may send MBS Interest Indication even when it is able to receive the MBS services it is interested in i.e. to avoid that the network allocates a configuration inhibiting MBS broadcast reception.3> else if *SIB20* is in the SIB1 scheduling information of the PCell or is provided for the SCell:4> if since the last time the UE transmitted the MBS Interest Indication, the UE connected to a PCell in which the SIB1 scheduling information does not contain *SIB20* and the UE was not provided with *SIB20* for an SCell; or4> if the set of MBS broadcast services of interest determined in accordance with 5.9.4.4 is different from *mbs-ServiceList* included in the last transmission of the MBS Interest Indication:5> set the contents of MBS Interest Indication according to 5.9.4.5 and initiate the transmission of *MBSInterestIndication* message. |

This correction is related to MII initiation. Currently, the following changes are agreed:

|  |
| --- |
| 5.9.4.2 InitiationAn MBS capable UE in RRC\_CONNECTED may initiate the procedure in several cases including upon successful connection establishment/resume, upon entering or leaving the broadcast service area, upon MBS broadcast session start or stop, upon change of interest, upon change of priority between MBS broadcast reception and unicast/multicast reception, upon change to a PCell providing *SIB21* (i.e. where the *SIB1* scheduling information contains *SIB21*), upon receiving *SIB20* of an SCell via dedicated signalling, upon handover. |

So in Rapporteur’s understanding, the changes in R2-2207032 on “provide” proposed by Correction 01 are not needed. And “broadcasting” can be changed to “providing” in the following sentence to make the wording consistent:

2> if since the last time the UE transmitted an MBS Interest Indication, the UE connected to a PCell not providing *SIB21*

**Q1: Do you agree with Rapporteur’s understanding?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2: If the answer to Q1 is no, do you agree with Correction1?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.2 Correction 02

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2207033 | ***MBS-SessionInfoList* field descriptions**

|  |
| --- |
| ***mtch-neighbourCell***Indicates neighbour cells which provide this service on MTCH. The first bit is set to 1 if the service is provided on MTCH in the first cell in *mbs-NeighbourCellList*, otherwise it is set to 0. The second bit is set to 1 if the service is provided on MTCH in the second cell in *mbs-NeighbourCellList*, and so on. If the service is not available in any neighbouring cell and *mbs-NeighbourCellList* is signalled, the network sets all bits in this field to 0. The network does not configure this field if *mbs-NeighbourCellList* is not present or empty in the same message. If this field is absent, the related service may or may not be available in any neighbouring cell, i.e. the UE cannot determine the presence or absence of an MBS service in neighbouring cells based on the absence of this field. |
| ***mtch-schedulingInfo***Indicates the index of DRX configuration entry in *drx-ConfigPTM-List* that is used for scheduling the MTCH. The value 0 corresponds to the first entry in *drx-ConfigPTM-List*, the value 1 corresponds to the second entry in *drx-ConfigPTM-List* and so on. The network does not configure this field if *drx-ConfigPTM-List* is not present in the same message. In case *mtch-schedulingInfo* is absent for a G-RNTI (i.e. no PTM DRX), the UE shall monitor for PDCCH scrambled with G-RNTI in any slot according to the search space configured for MTCH [see TS 38.213 [13], clause 10.1]. |

 |

The following has already been clarified for *mbs-NeighbourCellList*:

When an empty *mbs-NeighbourCellList* list is signalled, the UE shall assume that MBS broadcast services signalled in *mbs-SessionInfoList* in the *MBSBroadcastConfiguration* message are not provided in any neighbour cell. When the field *mbs-NeighbourCellList* is absent, the current serving cell does not provide information about MBS broadcast services in the neighbouring cells, i.e. the UE cannot determine the presence or absence of an MBS service in neighbouring cells based on the absence of this field.

**Q3: Do you agree with Correction 02?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.3 Correction 03

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2207034 | **5.3.5.6.6 Multicast MRB release**The UE shall:1> for each *mrb-Identity* value included in the *mrb-ToReleaseList* that is part of the current UE configuration; or1> for each *mrb-Identity* value that is to be released as the result of full configuration according to 5.3.5.11:2> release the PDCP entity and the *mrb-Identity*; |

This correction is originated from some overlap with **5.3.5.6.1:**

|  |
| --- |
| 5.3.5.6.1 GeneralThe UE shall perform the following actions based on a received *RadioBearerConfig* IE:\*\*[Text omitted]\*\*1> if the *RadioBearerConfig* includes the *mrb-ToReleaseList*:2> perform multicast MRB release as specified in 5.3.5.6.6;1> if the *RadioBearerConfig* includes the *mrb-ToAddModList*:2> perform multicast MRB addition or reconfiguration as specified in 5.3.5.6.7;1> release all SDAP entities, if any, that have no associated DRB as specified in TS 37.324 [24] clause 5.1.2, and indicate the release of the user plane resources for PDU Sessions associated with the released SDAP entities to upper layers;1> release all SDAP entities that have no associated multicast MRB as specified in TS 37.324 [24] clause 5.1.2, and indicate the release of user plane resources for these MBS multicast sessions to upper layers. |

In the meantime, apart from the duplication issue, Rapporteur observes that there may be a case where for a TMGI, one MRB is first released and another MRB is added in the same configuration message. In this case, the original description seems not suitable, as it will incorrectly indicate the release of use plane resources to upper layer during the execution of 5.3.5.6.6. Companies can provide their views on this correction.

**Q4: Do you agree with Correction 03?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.4 Correction 04

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2207039 | **5.3.7.5 Reception of the *RRCReestablishment* by the UE**The UE shall:<Omitted Text>1. submit the *RRCReestablishmentComplete* message to lower layers for transmission;

1> if the PCell provides *SIB21*:2> if the UE initiated transmission of a *MBSInterestIndication*message during the last 1 second preceding detection of radio link failure:3> initiate transmission of a *MBSInterestIndication*message in accordance with clause 5.9.4; 1> the procedure ends. |

This correction is related MII reporting during reestablishment.

**Q5: Do you agree with Correction 04?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.5 Correction 05

|  |  |
| --- | --- |
| R2-2207225 | **5.3.5.5.4 RLC bearer addition/modification**NOTE 1: For DRB and SRB, the network does not re-associate an already configured logical channel with another radio bearer. For MRB, the network does not re-associate an already configured logical channel with DBR or SRB. |

The proponent’s understanding is that LCH re-association can happen between MRBs. While Rapporteur thinks LCH re-association shouldn’t be supported between MRBs. So rapporteur’s proposed resolution is to change the NOTE as:

|  |
| --- |
| NOTE 1: For DRB, MRB and SRB, the network does not re-associate an already configured logical channel with another radio bearer. |

**Q6: Which option do you prefer?**

Option 1: Rapporteur’s resolution, i.e. adding “, MRB” in the NOTE1;

Option 2: Correction05 as proposed by R2-2207225

|  |  |  |
| --- | --- | --- |
| **Company** | **Option1/2** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.6 Correction 06

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2207555 | 5.3.2.3 Reception of the *Paging* *message* by the UE or *PagingRecord* by the L2 U2N Remote UE…1> if in RRC\_INACTIVE, for each of the *PagingRecord*, if any, included in the *Paging* message and the *ue-Identity* included in the *PagingRecord* matches the UE's stored *fullI-RNTI*, or1> if in RRC\_INACTIVE, for each of the *PagingRecord*, if any, included in the *UuMessageTransferSidelink* message received from the connected L2 U2N Relay UE and the *ue-Identity* included in the *PagingRecord* matches the UE's stored *fullI-RNTI*:1> if in RRC\_INACTIVE and the UE has joined one or more MBS session(s) indicated by the *TMGI* included in the *pagingGroupList*:2> if the UE is configured by upper layers with Access Identity 1:3> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set to *mps-PriorityAccess*;2> else if the UE is configured by upper layers with Access Identity 2:3> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set to *mcs-PriorityAccess*;2> else if the UE is configured by upper layers with one or more Access Identities equal to 11-15:3> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set to *highPriorityAccess*;2> else:3> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set to *mt-Access*;NOTE: A MUSIM UE may not initiate the RRC connection resumption procedure, e.g. when it decides not to respond to the *Paging* message due to UE implementation constraints as specified in TS 24.501 [23].2> else if the *ue-Identity* included in the *PagingRecord* matches the UE identity allocated by upper layers:3> if upper layers indicate the support of paging cause:4> forward the *ue-Identity*, *accessType* (if present) and paging cause (if determined) to the upper layers;3> else:4> forward the *ue-Identity* and *accessType* (if present) to the upper layers;3> perform the actions upon going to RRC\_IDLE as specified in 5.3.11 with release cause 'other';1> for each *TMGI* included in *pagingGroupList*, if any, included in the *Paging* message:2> if the UE has joined an MBS session indicated by the *TMGI* included in the *pagingGroupList*:3> forward the *TMGI* to the upper layers; |

The correction is some kind of rewording. Rapporteur’s understanding is as follows:

The changes are only to restructure the text (no functional change). However, the reconstruction will affect the Rel-15 wording structure for unicast paging which may cause some potential issues. Separate descriptions for multicast paging are clearer (although has more texts).

Also one company (Samsung) indicates: “Note that proposed changes are not proper as “2> else if the *ue-Identity* included in the…” is left dangling with no proper condition. It is not clear if it pertains to RRC\_INACTIVE but receiving CN paging. Further, going to RRC\_IDLE becomes ambiguous.”

**Q7: Whether Correction 06 is needed or not?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.7 Correction 07

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2207591 | Proposal 1: Confirm the understanding that configuration of MBS broadcast search space to a UE not supporting MBS broadcast in PDCCH-ConfigCommon will not cause inter-operability issue.Proposal 2: If Proposal 1 is not agreed, RAN2 is asked to change MBS broadcast capability from “optional capability without signalling” to “optional capability with signalling”. |

In R2-2207591, it mentions the possibility that the network may configure *searchSpaceMCCH* and *searchSapceMTCH* for a RRC configured BWPto the UE before the MII report, which can avoid potential the second RRC Reconfiguration procedures to configure MBS broadcast search space as a response to the MII report. In this case, the network may configure MBS broadcast search space in PDCCH-ConfigCommon to the UE not supporting MBS broadcast. As there is no UE actions required upon the UE receiving this MBS broadcast search space, proponent think it will not cause inter-operability issue.

**Q8: Do you agree with Proposal 1 in R2-2207591?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

**Q9: If you don’t agree with Proposal 1, do you agree to change MBS broadcast capability from “optional capability without signalling” to “optional capability with signalling”?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.8 Correction 08

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2207592 | * *TMGI*

The IE *TMGI* is used to identify the MBS session.***TMGI* information element**-- ASN1START-- TAG-TMGI-STARTTMGI-r17 ::= SEQUENCE { plmn-Id -r17 CHOICE { plmn-Index INTEGER (1..maxPLMN), explicitValue PLMN-Identity }, serviceId-r17 OCTET STRING (SIZE (3))}-- TAG-TMGI-STOP-- ASN1STOP

|  |
| --- |
| ***TMGI* field descriptions** |
| ***serviceId***Uniquely identifies the identity of an MBS service within a PLMN. The field contains octet 3- 5 of the IE Temporary Mobile Group Identity (TMGI) as defined in TS 24.008 [38]. The first octet contains the third octet of the TMGI, the second octet contains the fourth octet of the TMGI and so on. |
| ***plmn-Id***Uniquely identifies the identity of the PLMN. When this field is included in *MBS-ServiceList* field for MBS Interest Indication, the *explicitValue* shall be always chosen. |

 |

In R2-2207592, it is observed that the target gNB may not correctly comprehend the *plmn-index* in the *mbsInterestIndication* included in the *HandoverPreparationInformation* message during the handover. The reason is that different cells may support different PLMNs and even if the supported PLMNs are the same, the order of PLMNs in the list is very likely to be different as the *plmn-IdentityInfoList*s in SIB1 are generated separately by the source cell and the target cell. So it is proposed UE shall report explicit values of PLMN-IDs for TMGIs in the *MBSInterestIndication* message (this doesn’t affect the plmn-Index being used in MCCH to reduce the MCCH signalling overhead).

**Q10: Do you agree with the issue that the target gNB may not correctly comprehend the *plmn-index* in the *mbsInterestIndication* included in the *HandoverPreparationInformation* message during the handover?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

**Q11: If the answer to Q10 is yes, do you agree with Correction08?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.9 Correction 09

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2208088 | **5.9.4.2 Initiation**…Upon initiating the procedure, the UE shall:1> if *SIB21* is provided by the PCell; or1> if *SIB21* is not provided by the PCell and the frequency is included in the USD for the MBS services of interest:**5.9.4.3 MBS frequencies of interest determination**The UE shall:1> consider a frequency to be part of the MBS frequencies of interest if the following conditions are met:2> at least one MBS session the UE is receiving or interested to receive via a broadcast MRB is ongoing or about to start; andNOTE 1: The UE may determine whether the session is ongoing from the start and stop time indicated in the User Service Description (USD), see TS 38.300 [2] or TS 23.247 [67].2> for at least one of these MBS sessions, *SIB21* acquired from the PCell includes mapping between the concerned frequency and one or more MBS FSAIs indicated in the USD for this session, or for at least one of these MBS sessions, the concerned frequency is not included in *SIB21* but is indicated in the USD for this session, or for at least one of these MBS sessions, the concerned frequency is included in the USD when *SIB21* is absent; andNOTE 2: The UE considers a frequency to be part of the MBS frequencies of interest even though NG-RAN may (temporarily) not employ a broadcast MRB for the concerned session, i.e., the UE does not verify if the session is indicated on MCCH.2> the *supportedBandCombination* the UE included in *UE-NR-Capability* contains at least one band combination including the concerned MBS frequency of interest.5.9.4.4 MBS services of interest determinationThe UE shall:1> consider an MBS service to be part of the MBS services of interest if the following conditions are met:2> the UE is receiving or interested to receive this service via a broadcast MRB; and2> the session of this service is ongoing or about to start; and2> one or more MBS FSAIs in the USD for this service is included in *SIB21* acquired from the PCell for a frequency belonging to the set of MBS frequencies of interest, or no MBS FSAI in the USD for this service is included in *SIB21* and the MBS service is included in the USD for a frequency belonging to the set of MBS frequencies of interest, or *SIB21* is absent and the MBS service is included in the USD for a frequency belonging to the set of MBS frequencies of interest, determined according to 5.9.4.3. |

In R2-2208088, it is proposed UE can send MII when *SIB21* is absent but the frequency info is included in the USD for the MBS service. Correspondingly, UE can also include the frequency/service of interest in the MII message in this case.

Rapporteur’s understanding is that it was discussed and agreed to use the presence/absence of *SIB21* to enable/disable MII reporting in RAN2#116. If MII reporting is allowed without *SIB21,* the NW cannot control MII reporting on/off and a gNB not supporting MBS may also receive the MII message and cause failure.

Then the proponent proposed a way forward to discuss the following:

P1: RAN2 to discuss if MII signalling is supported when SIB21 is absent

P2: RAN2 to discuss how to enable the use case in P1 (e.g. add MII flag in SIB)

Per Rapporteur’s understanding, SIB21 already allows empty list of frequencies, if the network intends not providing any frequencies and allowing MII report, an empty SIB21 can be sent to control MII report. We see no reason to re-discuss this in R17 considering that there is already a clear agreement and R17 is already closed.

**Q12: Do you agree to re-discuss how MII signalling is controlled by NW?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

**Q13: Do you agree with Correction9?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.10 Correction 10

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2208095 | *BWP-UplinkDedicated*The IE *BWP-UplinkDedicated* is used to configure the dedicated (UE specific) parameters of an uplink BWP.*BWP-UplinkDedicated* information element-- ASN1START-- TAG-BWP-UPLINKDEDICATED-STARTBWP-UplinkDedicated ::= SEQUENCE { pucch-Config SetupRelease { PUCCH-Config } OPTIONAL, -- Need M pusch-Config SetupRelease { PUSCH-Config } OPTIONAL, -- Need M configuredGrantConfig SetupRelease { ConfiguredGrantConfig } OPTIONAL, -- Need M srs-Config SetupRelease { SRS-Config } OPTIONAL, -- Need M beamFailureRecoveryConfig SetupRelease { BeamFailureRecoveryConfig } OPTIONAL, -- Cond SpCellOnly ..., [[ sl-PUCCH-Config-r16 SetupRelease { PUCCH-Config } OPTIONAL, -- Need M cp-ExtensionC2-r16 INTEGER (1..28) OPTIONAL, -- Need R cp-ExtensionC3-r16 INTEGER (1..28) OPTIONAL, -- Need R useInterlacePUCCH-PUSCH-r16 ENUMERATED {enabled} OPTIONAL, -- Need R pucch-ConfigurationList-r16 SetupRelease { PUCCH-ConfigurationList-r16 } OPTIONAL, -- Need M lbt-FailureRecoveryConfig-r16 SetupRelease { LBT-FailureRecoveryConfig-r16 } OPTIONAL, -- Need M configuredGrantConfigToAddModList-r16 ConfiguredGrantConfigToAddModList-r16 OPTIONAL, -- Need N configuredGrantConfigToReleaseList-r16 ConfiguredGrantConfigToReleaseList-r16 OPTIONAL, -- Need N configuredGrantConfigType2DeactivationStateList-r16 ConfiguredGrantConfigType2DeactivationStateList-r16 OPTIONAL -- Need R ]], [[ ul-TCI-StateList-r17 CHOICE { explicitlist SEQUENCE { ul-TCI-ToAddModList-r17 SEQUENCE (SIZE (1..maxUL-TCI-r17)) OF TCI-UL-State-r17 OPTIONAL, -- Need N ul-TCI-ToReleaseList-r17 SEQUENCE (SIZE (1..maxUL-TCI-r17)) OF TCI-UL-State-Id-r17 OPTIONAL -- Need N }, unifiedTCI-StateRef-r17 ServingCellAndBWP-Id-r17 } OPTIONAL, -- Need R ul-powerControl-r17 Uplink-powerControlId-r17 OPTIONAL, -- Cond NoTCI-PC pucch-ConfigurationListMulticast1-r17 SetupRelease { PUCCH-ConfigurationList-r16 } OPTIONAL, -- Need M pucch-ConfigurationListMulticast2-r17 SetupRelease { PUCCH-ConfigurationList-r16 } OPTIONAL -- Need M ]], [[ pucch-ConfigMulticast1-r17 SetupRelease { PUCCH-Config } OPTIONAL, -- Need M pucch-ConfigMulticast2-r17 SetupRelease { PUCCH-Config } OPTIONAL -- Need M ]]}ConfiguredGrantConfigToAddModList-r16 ::= SEQUENCE (SIZE (1..maxNrofConfiguredGrantConfig-r16)) OF ConfiguredGrantConfigConfiguredGrantConfigToReleaseList-r16 ::= SEQUENCE (SIZE (1..maxNrofConfiguredGrantConfig-r16)) OF ConfiguredGrantConfigIndex-r16ConfiguredGrantConfigType2DeactivationState-r16 ::= SEQUENCE (SIZE (1..maxNrofConfiguredGrantConfig-r16)) OF ConfiguredGrantConfigIndex-r16ConfiguredGrantConfigType2DeactivationStateList-r16 ::= SEQUENCE (SIZE (1..maxNrofCG-Type2DeactivationState)) OF ConfiguredGrantConfigType2DeactivationState-r16-- TAG-BWP-UPLINKDEDICATED-STOP-- ASN1STOP |

In R2-2208095, it is observed that for multicast, there is no *pucch-ConfigMulticast1/pucch-ConfigMulticast2* when multicast feedback is not configured with a priority value. There are only *pucch-ConfigurationListMulticast1*/*pucch-ConfigurationListMulticast2* applicable when multicast feedback is configured with a priority value.

Companies can check whether current specs is sufficient or there is any case missing.

**Q14: Do you agree with Correction10?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

3.11 Correction 11

|  |  |
| --- | --- |
| TDoc | Detailed RRC corrections |
| R2-2208589 | The procedural text related to counter check in 5.3.6 and ASN. 1 signalling in 6.2.2 are updated to apply counter check to multicast MRB. **(The detailed changes can refer to the paper)** |

In R2-2208589, it is proposed to extend Counter Check Procedure to multicast MRB. Rapporteur’s understanding is as below:

Counter check has been discussed in SA3#106E but not agreed (S3-220292). Companies in SA2 commented that since security including integrity protection of the data traffic is provided at a higher layer above PDCP, what happens at the PDCP layer or below is irrelevant.

From RAN2 point of view, besides for security purpose, counter check is not an essential feature.

Companies can provide their views on this function.

**Q15: Do you think agree to extend Counter Check Procedure to multicast MRB?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

**Q16: If the answer to Q15 is yes, do you agree with the Correction11 made in R2-2208589?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

# 4 Conclusion

**TBD**

*[Easy Agreements]*

*[To be discussed]*

# 4 References

1. R2-2207032 Corrections related to MBS Interest Indication CATT CR Rel-17 38.331 17.1.0 3208 - F NR\_MBS-Core
2. R2-2207033 Corrections on Broadcast Configuration CATT, CBN CR Rel-17 38.331 17.1.0 3209 - F NR\_MBS-Core
3. R2-2207034 Corrections on multicast MRB handling CATT CR Rel-17 38.331 17.1.0 3210 - F NR\_MBS-Core
4. R2-2207035 Miscellaneous Corrections to TS 38.331 CATT CR Rel-17 38.331 17.1.0 3211 - F NR\_MBS-Core
5. R2-2207039 RRC Corrections for MBS Samsung discussion Rel-17 38.331
6. R2-2207225 Clarification on LCH Reassociation vivo discussion Rel-17 NR\_MBS-Core
7. R2-2207555 TMGI handling Nokia, Nokia Shanghai Bell CR Rel-17 38.331 17.1.0 3287 - F NR\_MBS-Core
8. R2-2207591 Clarification on the early configuration of MBS broadcast search space Huawei, CBN, HiSilicon discussion Rel-17 NR\_MBS-Core
9. R2-2207592 Discussion on decoding of the TMGI in MII Huawei, CBN, HiSilicon discussion Rel-17 NR\_MBS-Core
10. R2-2208084 Broadcast sessions with the same MRB configuration Ericsson discussion Rel-17 NR\_MBS-Core (moved from 6.1.3)
11. R2-2208088 MII signalling when SIB21 is absent Ericsson discussion Rel-17 NR\_MBS-Core
12. R2-2208095 Multicast-specific PUCCH-Config when multicast feedback is not configured with a priority value Qualcomm Incorporated CR Rel-17

38.331 17.1.0 3354 - F NR\_MBS-Core

1. R2-2208589 Counter Check Procedure for Multicast Samsung discussion Rel-17 NR\_MBS-Core
2. R2-2208639 Miscellaneous CR to TS 38.331 on NR MBS ZTE, Sanechips CR Rel-17 38.331 17.1.0 3457 - F NR\_MBS-Core