**3GPP TSG-RAN WG2 Meeting #121 *R2-2301688***

**Athens, Greece, 27th February – 3th March, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **3917** | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on the filed descriptions of NeedForGaps in 38.331 |
|  |  |
| ***Source to WG:*** | CATT, ZTE, vivo |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_redcap-Core |  | ***Date:*** | 2023-02-16 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)s*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | In RAN2#118e, RAN2 achieved the following agreement:

|  |
| --- |
| **2. For how to indicate serving cell MO for RedCap UE, adopt solution A-2.**  **Solution A-2: Optionally configures a BWP-specific servingCellMO under BWP-DownlinkDedicated IE when the BWP-DownlinkDedicated contains nonCellDefiningSSB-r17. If the field is present, the UE uses this servingCellMO for serving cell measurements, otherwise, the UE uses legacy servingCellMO IE under ServingCellConfig.** |

That is, for a BWP, a BWP specific servingCellMO can be configured, and if the BWP specific servingCellMO is configured, the UE will use it for serving cell measurements. So if the RedCap UE works on a BWP with BWP specific servingCellMO, no measurement gap is needed. This is not considered in the field descriptions of *NeedForGapsIntraFreq* and *NeedForGapNCSG-InfoNR*.  |
|  |  |
| ***Summary of change:*** | Update the field description of *NeedForGapsIntraFreq* and *NeedForGapNCSG-InfoNR*, to make it clear that, if the RedCap UE works on a BWP with BWP specific servingCellMO, no measurement gap is needed.**Impact analysis:**Impacted 5G architecture options:StandaloneImpacted functionality:Measurement configuration for RedCap UE.Inter-operability:1. If the UE is implemented according to this CR but the network is not, there is no inter-operability issue forseen.2. If the network is implemented according to this CR but the UE is not, there is no inter-operability issue forseen. |
|  |  |
| ***Consequences if not approved:*** | It is not clear how the UE will deal with the BWP with BWP specific servingCellMO when UE evaluates whether a measurement gap is needed or not.  |
|  |  |
| ***Clauses affected:*** | 6.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*Start of change*

– *NeedForGapsInfoNR*

The IE *NeedForGapsInfoNR* indicates whether measurement gap is required for the UE to perform SSB based measurements on an NR target band while NR-DC or NE-DC is not configured.

***NeedForGapsInfoNR* information element**

-- ASN1START

-- TAG-NeedForGapsInfoNR-START

NeedForGapsInfoNR-r16 ::= SEQUENCE {

 intraFreq-needForGap-r16 NeedForGapsIntraFreqList-r16,

 interFreq-needForGap-r16 NeedForGapsBandListNR-r16

}

NeedForGapsIntraFreqList-r16 ::= SEQUENCE (SIZE (1.. maxNrofServingCells)) OF NeedForGapsIntraFreq-r16

NeedForGapsBandListNR-r16 ::= SEQUENCE (SIZE (1..maxBands)) OF NeedForGapsNR-r16

NeedForGapsIntraFreq-r16 ::= SEQUENCE {

 servCellId-r16 ServCellIndex,

 gapIndicationIntra-r16 ENUMERATED {gap, no-gap}

}

NeedForGapsNR-r16 ::= SEQUENCE {

 bandNR-r16 FreqBandIndicatorNR,

 gapIndication-r16 ENUMERATED {gap, no-gap}

}

-- TAG-NeedForGapsInfoNR-STOP

-- ASN1STOP

|  |
| --- |
| ***NeedForGapsInfoNR* field descriptions** |
| ***intraFreq-needForGap***Indicates the measurement gap requirement information for NR intra-frequency measurement. |
| ***interFreq-needForGap***Indicates the measurement gap requirement information for NR inter-frequency measurement. |

|  |
| --- |
| ***NeedForGapsIntraFreq field descriptions*** |
| ***servCellId***Indicates the serving cell which contains the target SSB (associated with the initial DL BWP) to be measured.  |
| ***gapIndicationIntra***Indicates whether measurement gap is required for the UE to perform intra-frequency SSB based measurements on the concerned serving cell. Value *gap* indicates that a measurement gap is needed if any of the UE configured BWPs (except the BWP(s) configured with ServingCellMO associated with NCD-SSB) do not contain the frequency domain resources of the SSB associated to the initial DL BWP (CD-SSB). Value *no-gap* indicates a measurement gap is not needed to measure the SSB associated to the initial DL BWP (CD-SSB) for all configured BWPs (except the BWP(s) configured with ServingCellMO associated with NCD-SSB), no matter the SSB is within the configured BWP or not.  |

|  |
| --- |
| ***NeedForGapsNR* field descriptions** |
| ***bandNR***Indicates the NR target band to be measured. |
| ***gapIndication***Indicates whether measurement gap is required for the UE to perform SSB based measurements on the concerned NR target band while NR-DC or NE-DC is not configured. The UE determines this information based on the resultant configuration of the *RRCReconfiguration* or *RRCResume* message that triggers this response. Value *gap* indicates that a measurement gap is needed, value *no-gap* indicates a measurement gap is not needed.  |

*Next change*

– *NeedForGapNCSG-InfoNR*

The IE *NeedForGapNCSG-InfoNR* indicates whether measurement gap or NCSG is required for the UE to perform SSB based measurements on an NR target band while NR-DC or NE-DC is not configured.

***NeedForGapNCSG-InfoNR* information element**

-- ASN1START

-- TAG-NEEDFORGAPNCSG-INFONR-START

NeedForGapNCSG-InfoNR-r17 ::= SEQUENCE {

 intraFreq-needForNCSG-r17 NeedForNCSG-IntraFreqList-r17,

 interFreq-needForNCSG-r17 NeedForNCSG-BandListNR-r17

}

NeedForNCSG-IntraFreqList-r17 ::= SEQUENCE (SIZE (1.. maxNrofServingCells)) OF NeedForNCSG-IntraFreq-r17

NeedForNCSG-BandListNR-r17 ::= SEQUENCE (SIZE (1..maxBands)) OF NeedForNCSG-NR-r17

NeedForNCSG-IntraFreq-r17 ::= SEQUENCE {

 servCellId-r17 ServCellIndex,

 gapIndicationIntra-r17 ENUMERATED {gap, ncsg, nogap-noncsg}

}

NeedForNCSG-NR-r17 ::= SEQUENCE {

 bandNR-r17 FreqBandIndicatorNR,

 gapIndication-r17 ENUMERATED {gap, ncsg, nogap-noncsg}

}

-- TAG-NEEDFORGAPNCSG-INFONR-STOP

-- ASN1STOP

|  |
| --- |
| ***NeedForGapNCSG-InfoNR* field descriptions** |
| ***intraFreq-needForNCSG***Indicates the measurement gap and NCSG requirement information for NR intra-frequency measurement. |
| ***interFreq-needForNCSG***Indicates the measurement gap and NCSG requirement information for NR inter-frequency measurement. |

|  |
| --- |
| ***NeedForNCSG-IntraFreq field descriptions*** |
| ***servCellId***Indicates the serving cell which contains the target SSB (associated with the initial DL BWP) to be measured. |
| ***gapIndicationIntra***Indicates whether measurement gap or NCSG is required for the UE to perform intra-frequency SSB based measurements on the concerned serving cell. Value *gap* indicates that a measurement gap is needed if any of the UE configured BWPs (except the BWP(s) configured with ServingCellMO associated with NCD-SSB) do not contain the frequency domain resources of the SSB associated to the initial DL BWP (CD-SSB). Value *ncsg* indicates that a NCSG is needed if any of the UE configured BWPs do not contain the frequency domain resources of the SSB associated to the initial DL BWP. Value *nogap-noncsg* indicates that neither a measurement gap nor a NCSG is needed to measure the SSB associated to the initial DL BWP (CD-SSB) for all configured BWPs (except the BWP(s) configured with ServingCellMO associated with NCD-SSB), no matter the SSB is within the configured BWP or not. |

|  |
| --- |
| ***NeedForNCSG-NR* field descriptions** |
| ***bandNR***Indicates the NR target band to be measured. |
| ***gapIndication***Indicates whether measurement gap or NCSG is required for the UE to perform SSB based measurements on the concerned NR target band while NR-DC or NE-DC is not configured. The UE determines this information based on the resultant configuration of the *RRCReconfiguration* or *RRCResume* message that triggers this response. Value *gap* indicates that a measurement gap is needed, value *ncsg* indicates that a NCSG is needed, and value *nogap-noncsg* indicates neither a measurement gap nor a NCSG is needed.  |

*End of change*