**3GPP TSG RAN WG2#121 draft R2-2301973**

**Athens, Greece, February 27th - 3rd March, 2023**

**Source: Samsung**

**Title: [AT121][116][NR NTN] CP corrections (Samsung)**

**Agenda item:** **6.6.3**

**Document for:** **Discussion and Decision**

# Introduction

This document is intended to address CP corrections as per the following email discussion guidelines:

* [AT121][116][NR NTN] CP corrections (Samsung)

Scope: Discuss the CRs in [R2-2300125](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300125%20Remaining%20issue%20on%20PDD%20reporting.docx), [R2-2300234](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300234%20Remaining%20issues%20on%20SMTC.doc) and [R2-2300236](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300236%20CR%20to%2038.331%20on%20event%20D1.docx)

Intended outcome: offline summary (and agreeable CRs, if any)

Deadline for companies' feedback: Thursday 2023-03-02 22:00 EET

Deadline for rapporteur's summary (in R2-2301973): Friday 2023-03-03 08:00 EET

# Discussion

## Remaining issue on PDD reporting

For propagation delay difference (PDD) reporting, the parameter epochTime is included in NeighbourCellInfo in otherConfig. In RAN2 #120 meeting, it has been identified that it is not clear how to apply the epochTime.

|  |
| --- |
| [R2-2211894](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2211894%20Discussion%20on%20propagation%20delay%20difference%20reporting%20in%20TS%2038.331.docx) Discussion on propagation delay difference reporting in TS 38.331 vivo discussionProposal 1b: If RAN2 confirm that the parameter epochTime in Proposal 1 is not used, RAN2 to agree to dummify this parameter.* Nokia agrees it’s not clear why we have Epoch time there.
* HW thinks it was include to provide information, also wonders if the ephemeris are needed
* Postponed to the next meeting
 |

In [R2-2300125](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300125%20Remaining%20issue%20on%20PDD%20reporting.docx), it is explained that this epochTime is associated with the ephermeis provided in NeighbourCellInfo in otherConfig, which is necessary for the UE to derive the satellite position for the corresponding neighbour cell configured in NeighbourCellInfo. Further considering that the UE may be configured in otherConfig with a neighbour cell that is not included in SIB19, it is thus unable to assume that for PDD reporting the UE can always find and reuse the epochTime in the NTN-config in SIB19 for each neighbour cell. Thus, it is necessary to provide this epochTime parameter in otherConfig.

However, how to apply the epochTime in otherConfig for PDD is unclear. Although for the epochTime included in NTN-Config there are some requirements specified in field description on how the epochTime needs to be configured and applied in dedicated configuration (highlighted below), they are specified for handover/CHO configuration.

|  |
| --- |
| ***epochTime***Indicate the epoch time for the NTN assistance information. When explicitly provided through SIB, or through dedicated signaling, the *EpochTime* is the starting time of a DL sub-frame, indicated by a SFN and a sub-frame number signaled together with the assistance information. For serving cell, the field *sfn* indicates the current SFN or the next upcoming SFN after the frame where the message indicating the *epochTime* is received. For neighbour cell, the *sfn* indicates the SFN nearest to the frame where the message indicating the *epochTime* is received. The reference point for epoch time of the serving NTN payload ephemeris and Common TA parameters is the uplink time synchronization reference point. If this field is absent, the epoch time is the end of SI window where this SIB19 is scheduled. This field is mandatory present when provided in dedicated configuration. If this field is absent in *ntn-Config* provided via *NTN-NeighCellConfig* the UE uses epoch time of the serving cell, otherwise the field is based on the timing of the serving cell, i.e. the SFN and sub-frame number indicated in this field refers to the SFN and sub-frame of the serving cell. In case of handover or conditional handover, this field is based on the timing of the target cell, i.e. the SFN and sub-frame number indicated in this field refers to the SFN and sub-frame of the target cell. For the target cell the UE considers epoch time, indicated by the SFN and sub-frame number in this field, to be the frame nearest to the frame in which the message indicating the epoch time is received. This field is excluded when determining changes in system information, i.e. changes to *epochTime* should neither result in system information change notifications nor in a modification of *valueTag* in *SIB1*. |

Note that the epochTime is provided as a separate parameter in the otherConfig, not reusing the one included in NTN-Config, so the field description of epochTime included in NTN-Config cannot directly cover this parameter when provided in otherConfig. Additionally, it is seen that the epochTime included in NeighbourCellInfo in otherConfig is already a mandatory field, so the requirement in above bullet 2 is the extra part that needs to be clarified in the Spec for its usage. Therefore, it is proposed to add a field description for the epochTime in otherConfig to clarify how the parameter is applied for PDD reporting.

**Q1) Do you agree to add a field description for the epochTime in otherConfig to clarify how the parameter is used for PDD reporting?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Samsung | Yes |  |
| Huawei, HiSilicon | Yes |  |
| MediaTek | Yes |  |
| Google | Yes |  |
| Apple | Yes |  |
| Intel | Yes |  |
| CATT | Yes |  |
| Qualcomm | Yes |  |
| Xiaomi | Yes |  |
| Lenovo | Yes |  |
| OPPO | Yes |  |
| LGE  | Yes |  |
| Nokia |  | We are not sure if the problem is real – will there be a mismatch in NW configuration between what is provided in otherConfig and in NeighbourCellInfo |
| Ericsson | yes |  |
| Sequans | Yes |  |

The corresponding TP is provided, see Appendix 1, with a field description added.

| ***NeighbourCellInfo* field descriptions** |
| --- |
| ***epochTime***Indicates the epoch time used along with the *ephemerisInfo* to derive the propagation delay difference for the associated neighbour cell. The UE considers epoch time, indicated by the SFN and sub-frame number in this field, to be the frame nearest to the frame in which the message indicating the epoch time is received. |

**Q2) If Q1 is agreed, do you agree the TP in Appendix 1?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Samsung | Yes |  |
| Huawei, HiSilicon | Yes |  |
| MediaTek | Yes |  |
| Google | Yes |  |
| Apple | Yes with comment | We suggest to add the reference timing in the file description, e.g. This field is based on the timing of the serving cell, i.e. the SFN and sub-frame number indicated in this field refers to the SFN and sub-frame of the serving cell. |
| Intel | Yes |  |
| CATT | Yes |  |
| Qualcomm | Yes |  |
| Xiaomi | Yes |  |
| Lenovo | Yes |  |
| OPPO | Yes | It is OK to introduce epochTime using a separate FD table. |
| LGE | Yes |  |
| Nokia |  | Should be optional |
| Ericsson | Yes |  |
| Sequans | Yes |  |

## Remaining issues on SMTC

### SMTC in SIB2/4

For SMTC adjustment, NW-based solution for RRC\_CONNECTED (e.g., UE follows configured smtc) and UE-based solution for RRC\_IDLE/INACTIVE are supported in Rel-17. For UE-based solution, new smtc fields have been introduced in SIB2/4. After receiving the SMTC, the UE needs to calculate the PDD between serving cell and a neighbour cell, and adjust the SMTC offset by the PDD. According to the current field description (taking the SMTC in SIB2 as an example), the SMTC is assuming service link propagation delay difference is 0 (not mentioning feeder link), and the UE can adjust the smtc offset based on the actual PDD.

|  |
| --- |
| ***smtc***Measurement timing configuration for intra-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms for the intra-frequnecy cells. If the field is broadcast by an NTN cell, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and UE can adjust the actual *offset* based on the actual propagation delay difference. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |

How to handle the feeder link PDD is however not clear in the spec although relevant agreements were maded in 118-e and 119-e.

|  |
| --- |
| 118-e:Common TA parameters and Kmac of the neighbour cell are used to support IDLE/Inactive UEs in NTN to perform SMTC adjustments.119-e:The broadcast SMTC in SIB2/4 assumes PDD = 0 ms. |

Aligning with these agreements, one understanding on how to handle the feeder link PDD is that for the SMTC in SIB2/4 the UE assumes the feeder link PDD between the serving cell and a neighbor cell is 0 ms. The UE derives the actual feeder PDD based on common TA parameters and Kmac for the serving cell and the neighbor cell, and then adjusts the smtc offset based on the actual PDD including service link PDD and feeder link PDD.

In [R2-2300234](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300234%20Remaining%20issues%20on%20SMTC.doc), a second understanding is provided that assuming NW already compensates the FL delay corresponding to an epoch time in SMTC in SIB2/4, the UE checks the FL delay at the moment and the FL delay corresponding to the SMTC in SIB2/4 (which requires to inform the UE the corresponding “epoch time”). The difference between the two values needs to be adjusted by the UE. However, in this case the aforementioned “epoch time” is not clarified in the spec.

Based on above two understandings, several possible solutions are proposed:

- **Option 1**: **Add a separate epochTime (T0) in SIB2/4 for the SMTC**

With this option, UE assumes FL PDD has been compensated in SMTC in SIB2/4 up to T0, and the FL PDD later on needs to be compensated by the UE themselves. However, adding a new parameter leads to potential NBC issue, as the new parameters is invisible for the old UEs to follow (especially considering it is for the IDLE/INACTIVE case)

- **Option 2**: **Clarify in the field description of SMTC in SIB2/4 that the SMTC assumes feeder link PDD = 0ms (i.e. FL PDD is not compensated by NW)**

With this option, when adjusting the real-time SMTC offset, the UE only consider the absolute value of the service link PDD and feeder link PDD, and can add them to the SMTC offset to derive the real-time SMTC. This option clarifies the assumption that FL PDD is 0 ms, but may cause potential NBC issue.

- **Option 3: Clarify in the field description of SMTC that the FL PDD corresponding to the epochTime in SIB19 is compensated (i.e. FL PDD at epoch time is compensated by NW)**

This option is reusing the epochTime in SIB19 as a clarification on how to understand the SMTC in SIB2/4.

**Q3) Please indicate which option is preferred with comments. If none is preferred, please indicate other options in comments.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1/2/3** | **Comments**  |
| Samsung | Option 2 | As the currently FL PDD is not mentioned in the field description, we understand this is only to further clarify FL PDD = 0, which is already agreed before.Technically, option 2 is simpler that only needs UE to calculate absolute FL PDD, while option 3 requires NW to compensate FL PDD at every epoch time and update SMTC in SIB2/4 for every validity duration, and requires UE to calculate relative FL PDD change. |
| Huawei, HiSilicon | Option 3 | We woulde like a consistent behaviour for both Idle and Connected UE: the feeder link delay is always compensated by the NW.Also, we think Option 2 is NBC because the current description assumes feeder link delay is compensated (since feeder link delay is not mentioned in the description).Finally, there was a CR (R2-2210646) in the previous meeting with a change similar to Option 3 and was not approved. Part of the reason was the concern on backward compatibility. |
| MediaTek | Neutral |  |
| Google | Option 2, but | The network actually does not compensate the full FL propagation delay, and hence option 1 is not feasible (network only compensates the propagation delay from the GW to the RP, that’s why common TA is signalled in the sytem information). Our previous CR **R2-2212895** provideds another remedy, which we believe is more accurate. R2-2212895 clarifies in the field description that the SMTC assumes the **common TA difference** between the serving cell and neighbouring cells equals to 0ms.  |
| ZTE | Option 2 | In our understanding this issue has been discussed in RAN2#118 offline 106, and RAN2 agrees on below agreements:***5.Common TA parameters and Kmac of the neighbour cell are used to support IDLE/Inactive UEs in NTN to perform SMTC adjustments.***The intention is to have UE to perform autonomous adjust SMTC based on the estimation of propagation delay difference taking into account on the feeder link delay. |
| Apple | Option 2 | Agree with ZTE that we have discussed it and made such agreement before.  |
| Intel | Option 2 |  |
| CATT | Option 2 with comment | Share a similar view with google. It is more accurate to use common TA, because only when the RP is at the gateway, the common TA refer to the feeder link which need to be compensated by UE.We think option 3 is also NBC in some way, because we nerver defined that. Hence, we preferred the simpler way, i.e., option 2. |
| Qualcomm | Option 3 | We agree with Huawei. Option 3 aligns more with current understanding and we should avoid the changes causing potential issue for UE. |
| Xiaomi | Option 3 | Prefer network to compensate the feederlink delay. |
| Lenovo | Option 2 |  |
| OPPO | Option 2 |  |
| LGE | Option 3 | Agree with ZTE but UE has no idea about the propagation delay. Therefore, we understand that UE uses common TA parameters to compensate change of feeder link PDD after the network compensates feeder link PDD at epoch time. |
| Nokia | Option 2 | It has the lowest specification effort.  |
| Ericsson | Option 2 |  |

A possible TP for **Option 2** is as follows.

|  |
| --- |
| ***smtc***Measurement timing configuration for intra-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms for the intra-frequnecy cells. If the field is broadcast by an NTN cell, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that service link propagation delay differencebetween the serving cell and neighbour cells equals to 0 ms, and feeder link propagation delay difference between the serving cell and neighbour cells equals to 0 ms. The UE can adjust the actual *offset* based on the actual propagation delay difference. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and feeder link propagation delay difference between the serving cell and neighbour cells equals to 0 ms. The UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |

**Q4) If Option 2 is preferred, do you agree the TP above (also see Appendix 3)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Samsung | Yes |  |
| Google | No | Suggest to modify as follows (same as in R2-2212895). If the field is broadcast by an NTN cell, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that service link propagation delay difference, as well as the common TA difference between the serving cell and neighbour cells equals to 0 ms, and UE can adjust the actual *offset* based on the actual service link propagation delay difference and common TA difference. |
| ZTE | Yes |  |
| Apple | Yes |  |
| Intel | Yes |  |
| CATT | No | We can accept the modification proposed by Google. |
| Lenovo | Yes |  |
| OPPO | Yes |  |
| Nokia | Looks OK |  |
|  |  |  |
|  |  |  |

A possible TP for **Option 3** is as follows.

|  |
| --- |
| ***smtc***Measurement timing configuration for intra-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms for the intra-frequnecy cells. If the field is broadcast by an NTN cell, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and the feeder link delay corresponding to *epochTime* in SIB19 is compensated. The UE can adjust the actual *offset* based on the actual propagation delay difference. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and the feeder link delay corresponding to *epochTime* in SIB19 is compensated. The UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |

**Q5) If Option 3 is preferred, do you agree the TP above (also see Appendix 2)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Huawei, HiSilicon | Yes |  |
| Xiaomi | Yes |  |
| LGE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### SMTC in inter-node message

The inter-node message MeasurementTimingConfiguration includes the timing occasions where SSBs are transmitted. In TS 38.331, it is specified that the timing of the SMTC configuration is based on the cell for which the message is included, i.e., the timing is based on the transmitting node.

|  |
| --- |
| ***ssb-MeasurementTimingConfiguration***Indicates the SMTC which can be used to search for SSB of the cell for which the message is included. When the message is included in "Served NR Cell Information" (see TS 36.423 [37]), "Served Cell Information NR" (see TS 38.423 [35]), or "Served Cell Information" (see TS 38.473 [36]), the timing is based on the cell for which the message is included. When the message is included in "NR Neighbour Information" (see TS 36.423 [37]), or "Served Cell Information" (see TS 38.423 [35]), the timing is based on the cell indicated in the "Served NR Cell Information" or "Served Cell Information NR" with which the "NR Neighbour Information" or "Neighbour Information NR" is provided. When the message is included in "CU to DU RRC Information", the timing is based on the cell indicated by SpCell ID with which the message is included. |
|  |

On the other hand, the SMTC configured to the served UEs via Uu interface is based on the timing of the serving cell. For TN, the receiving node needs to compensate the timing difference between the transmitting node and the receiving node (e.g., based on SFTD information) before configuring the SMTC to the UE. In NTN, the timing difference caused by propagation delay needs to be considered for both RRC\_CONNECTED and RRC\_IDLE/INACTIVE.

It is pointed in [R2-2300236](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300236%20CR%20to%2038.331%20on%20event%20D1.docx) that it is not clear whether the FL propagation delay is compensated by the transmitting node or the receiving node. One option is that the FL propagation delay is not compensated by the transmitting node while exchanging the SMTC configuration in the inter-node message, and the receiving gNB is responsible to adjust the received SMTC configuration if necessary before configuring SMTC to the UE.

**Q6) Do you agree that the feeder link propagation delay is not compensated by the transmitting node while exchanging the SMTC configuration in the inter-node message, the receiving gNB can adjust the received SMTC configuration if necessary before configuring SMTC to the UE?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Samsung | Yes | This allow the receiving gNB directly adjust SMTC offset based on FL PDD between cells from transmitting and receiving gNBs. |
| Huawei, HiSilicon | Yes |  |
| MediaTek | Yes |  |
| Google | No | Neither the transmitting gNB nor the receiving gNB needs to adjust the SMTC configuration (UE does!), as long as both sides have the same understanding that the SMTC provided by the transmitting gNB is based on the timing at the reference point. |
| ZTE | No need to specify | This NW inplementation, UE just follows the configuration, no need to capture NW behavior in specs. |
| Apple | Yes |  |
| Intel | No | Agree with ZTE |
| CATT | See the comment | When the RP is at gateway, the feeder link can be compensated by UE. When the RP is at satellite, the feeder link need to be compensated by the receiving gNB, because UE have no idea of the feeder link delay. |
| Lenovo | Yes |  |
| OPPO | No | We cannot assume feeder link delay of transmitting gNB to be 0ms. If assuming so, transmitting gNB may have to frequently update the SMTC config to receving gNB. To reduce the update frequency, receiving gNB may need to know serving cell and neighbor cell’s feeder link delay. But this can be up to NW implementation as pointed out by ZTE, if we don’t want to introduce RAN3 impact. |
| Nokia | No need to specify | Agree with ZTE. |
| Ericsson | No need to specify |  |

If Q6 is the common understanding, a clarification is needed in the field description of ssb-MeasurementTimingConfiguration in the inter-node message. A TP is provided in [R2-2300236](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300236%20CR%20to%2038.331%20on%20event%20D1.docx), assuming **Option 3** in 2.2.1 is agreed.

* **TP-1 if Option 3** **in 2.2.1 is agreed (also see Appendix 2)**

|  |
| --- |
| ***ssb-MeasurementTimingConfiguration***Indicates the SMTC which can be used to search for SSB of the cell for which the message is included. When the message is included in "Served NR Cell Information" (see TS 36.423 [37]), "Served Cell Information NR" (see TS 38.423 [35]), or "Served Cell Information" (see TS 38.473 [36]), the timing is based on the cell for which the message is included. When the message is included in "NR Neighbour Information" (see TS 36.423 [37]), or "Served Cell Information" (see TS 38.423 [35]), the timing is based on the cell indicated in the "Served NR Cell Information" or "Served Cell Information NR" with which the "NR Neighbour Information" or "Neighbour Information NR" is provided. When the message is included in "CU to DU RRC Information", the timing is based on the cell indicated by SpCell ID with which the message is included. If the field is provided by an NTN cell, the offset (derived from parameter *periodicityAndOffset*) is based on the assumption that the feeder link propagation delay of the cell for which the message is included equals to 0 ms, and the receiving gNB can adjust the actual offset based on the actual feeder link propagation delay before configuring SMTC to the UE. |

Note that **TP-1** assumes Option 3 in 2.2.1 (i.e., FL PDD at epoch time is compensated by NW for RRC\_IDLE/INACTIVE) is agreed. To decouple the two issues, an alternative TP is provided as follows to allow flexible adjustments by the receiving gNB if needed. Additionally, the actual offset for connected UE may also need to be adjusted based on service link PDD if reported before configuring SMTC to the UE.

* **TP-2 (also see Appendix 3)**

|  |
| --- |
| ***ssb-MeasurementTimingConfiguration***Indicates the SMTC which can be used to search for SSB of the cell for which the message is included. When the message is included in "Served NR Cell Information" (see TS 36.423 [37]), "Served Cell Information NR" (see TS 38.423 [35]), or "Served Cell Information" (see TS 38.473 [36]), the timing is based on the cell for which the message is included. When the message is included in "NR Neighbour Information" (see TS 36.423 [37]), or "Served Cell Information" (see TS 38.423 [35]), the timing is based on the cell indicated in the "Served NR Cell Information" or "Served Cell Information NR" with which the "NR Neighbour Information" or "Neighbour Information NR" is provided. When the message is included in "CU to DU RRC Information", the timing is based on the cell indicated by SpCell ID with which the message is included. If the field is provided by an NTN cell, the offset (derived from parameter *periodicityAndOffset*) is based on the assumption that the propagation delay of the cell for which the message is included equals to 0 ms, and the receiving gNB can adjust the actual offset before configuring SMTC to the UE. |

**Q7) Do you prefer TP-1 or TP-2? If neither is preferred, please indicate other options in comments.**

|  |  |  |
| --- | --- | --- |
| **Company** | **TP-1/2** | **Comments**  |
| Samsung | TP-2 |  |
| Huawei, HiSilicon | TP-1 | To be consistent with the answers in Q3. |
| MediaTek | TP-1 |  |
| Google | Neither | Changes are not needed. |
| ZTE | Neither |  |
| CATT | Neither | ***ssb-MeasurementTimingConfiguration***Indicates the SMTC which can be used to search for SSB of the cell for which the message is included. When the message is included in "Served NR Cell Information" (see TS 36.423 [37]), "Served Cell Information NR" (see TS 38.423 [35]), or "Served Cell Information" (see TS 38.473 [36]), the timing is based on the cell for which the message is included. When the message is included in "NR Neighbour Information" (see TS 36.423 [37]), or "Served Cell Information" (see TS 38.423 [35]), the timing is based on the cell indicated in the "Served NR Cell Information" or "Served Cell Information NR" with which the "NR Neighbour Information" or "Neighbour Information NR" is provided. When the message is included in "CU to DU RRC Information", the timing is based on the cell indicated by SpCell ID with which the message is included. If the field is provided by an NTN cell, the the timing is based on the RP of the cell for which the message is included. |
| Lenovo | TP-1 |  |
| OPPO | Neither |  |
| Nokia | None |  |
|  |  |  |
|  |  |  |

## EventD1

The IE *ReferenceLocation* specifies the location information used in *eventD1* and *condEventD1*, and the value of reference location is defined in TS 37.355 (*Ellipsoid-Point* in TS 37.355), which does not contain height information:

Ellipsoid-Point ::= SEQUENCE {

 latitudeSign ENUMERATED {north, south},

 degreesLatitude INTEGER (0..8388607), -- 23 bit field

 degreesLongitude INTEGER (-8388608..8388607) -- 24 bit field

}

It is unclear whether the UE needs to take its height into account when calculating the distance to reference location, especially for UEs with a high altitude (e.g., UEs on the mountain or UEs in the plane). CR in [R2-2300236](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300236%20CR%20to%2038.331%20on%20event%20D1.docx) clarifies that when UE calculates the distance between UE and the reference location, the assumption is that the height of the UE is 0.

**Q8) Do you agree the CR in R2-2300236?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Huawei, HiSilicon | Yes |  |
| MediaTek | Yes |  |
| Google | No | The height can be neglected compared to the distance between the satellite and the Earth.  |
| ZTE | Yes, with modification | Since NW is not aware of such information, it shall be fine to take assumption. And we suggest below modification:NOTE: The assumption is that the altitude of UE is zero. |
| Apple | Yes |  |
| Samsung | Yes | ok with ZTE’s wording |
| Intel | No | If there is no altitude parameter within Ellipsoid-Point, it’s already clear it’s not taken into account. |
| CATT | No | It is unnecessary.The *Ellipsoid-Point* in TS 37.355 is reference to a geographic shape as defined in TS 23.032.

|  |
| --- |
| The description of an ellipsoid point is that of a point on the surface of the ellipsoid, and consists of a latitude and a longitude. In practice, such a description can be used to refer to a point on Earth's surface, or close to Earth's surface, with the same longitude and latitude. No provision is made in this version of the standard to give the height of a point.Figure 1: Description of a Point as two co-ordinates |

In our understanding, the description is clear, no more limitation on height is needed.On the other hand, here is no height concept in the definition of *Ellipsoid-Point*, what is the reference coordinate system of the height? the earth's core or surface? It is not clear.  |
| Qualcomm | No | If there is no height information provided, its already clear. Height not considered means it is zero. |
| Xiaomi | No | Agree with Intel. |
| Lenovo | No | Agree with Google |
| OPPO | Yes | OK with ZTE’s wording |
| LGE | No | Same view with Intel. |
| Nokia | No | Agree with Intel and CATT’s explanation. |
| ericsson | No | Agree with Intel and CATT’s explanation. |
| Sequans | No | Same view as Intel/CATT |

## Relaxed measurment

RAN2 has agreed to reuse relaxedMeasurement-r16 field for NTN relaxed measurement based on RAN4 LS R2-2209337.

|  |
| --- |
| Agreements 119bis-e:Reuse the exiting relaxedMeasurement-r16 field to enable the relaxed cell reselection requirements for GEO. |

Regarding the field description of relaxedMeasurement, the LS reply (R2-2210866) was sent to RAN4 for confirmation. RAN4 further replied in R2-2300057.

|  |  |
| --- | --- |
| RAN4 would like to thanks RAN2 for the information in LS R2-2210866. On relaxed measurement, RAN4 reached the following conclusions.

|  |
| --- |
| * For intra-frequency measurement, RAN4 to confirm that the NR NTN relaxed intra-frequency measurements only apply to GSO neighbour cells and can be configured only by GSO serving cell.
* For inter-frequency measurement, RAN4 to confirm that the NR NTN relaxed inter-frequency measurements only apply to GSO neighbour cells and can be configured by GSO and NGSO serving cell.
* (Note) The applicability of the signalling for relaxed RRM measurement for IoT NTN shall be separately discussed and decided under WI of LTE\_NBeMTC\_NTN.
 |

RAN4 respectfully asks RAN2 to take the above information into account.  |

RAN4 confirms that for NTN the relaxed measurement is applied to GSO neighbor cell measurements for cell reselection. It can be configured for intra-frequency measurements by a GSO serving cell and for inter-frequency measurements by a GSO/NGSO serving cell. Clarification for relaxedMeasurement in SIB2 is needed.

In CR R2-2301478, a clarification on NTN relaxed measurement configuration is added in the field description of relaxedMeasurement in SIB2 according to the RAN4 LS reply.” This clarification explaines how the field is configured for relaxed measurement in NTN.

|  |
| --- |
| ***relaxedMeasurement***Configuration to allow relaxation of RRM measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9). In NTN, this field is configured by a GSO serving cell for intra-frequency measurements of GSO neighbour cells or configured by a GSO/NGSO serving cell for inter-frequency measurements of GSO neighbour cells. |

**Q9) Do you agree the CR in R2-2301478?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Samsung | Yes | The RAN4 LS reply should be reflected in both 331 and 304 spec.  |
| Intel | Agree with intention | We prefer Apple CR R2-2300730, i.e., only need to Clarify the relaxedMeasurement configuration is only applied on GSO neighbor cells |
| CATT | See the comment | The RAN4 LS clarifies the restriction on the relax measurement object for intra-frequency and inter-frequency and restriction on the configured serving cell type. This information is not captured in TS38.133, that we need to capture it in RAN2 spec.We prefer to add a NOTE in TS38.304, see our CR R2-2301686NOTE: For NTN access, the relaxed intra-frequency measurements only apply to GSO neighbour cells and can be configured only by GSO serving cell. The relaxed inter-frequency measurements only apply to GSO neighbour cells and can be configured by GSO and NGSO serving cell. |
| Qualcomm |  | It may be sufficient to say this applies only to GSO neighbor cell and can be configured by GSO or NGSO serving cell. |
| Xiaomi | Yes |  |
| Lenovo | Yes |  |
| OPPO | Yes |  |
| ZTE | No | Since in 38.304 it is clearly specified, there is no need to duplicate again the description.  |
| Apple | Yes | We should support both. The RRC CR is to clarify the restriction of the configuration, and the 304 CR is to reflect the reference to RAN4 spec.  |
| LGE | Yes with comments | We suggest to modify it as follow:***relaxedMeasurement***Configuration to allow relaxation of RRM measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9). In NTN, this field is configured by a GSO serving cell for intra-frequency measurements or configured by a GSO/NGSO serving cell for inter-frequency measurements. |
| Nokia | Yes | Seems to be a valid proposal. |
| Ericsson | Yes |  |
| Sequans | Yes |  |

# Conclusions

<To be generated based on company input>

# References

1. [R2-2300125](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300125%20Remaining%20issue%20on%20PDD%20reporting.docx) Remaining issue on PDD reporting vivo, Samsung, Huawei, HiSilicon discussion Rel-17 NR\_NTN\_solutions-Core
2. [R2-2300234](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300234%20Remaining%20issues%20on%20SMTC.doc) Remaining issues on SMTC Huawei, HiSilicon, vivo, Samsung discussion Rel-17 NR\_NTN\_solutions-Core
3. [R2-2300236](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2300236%20CR%20to%2038.331%20on%20event%20D1.docx) CR to 38.331 on event D1 Huawei, HiSilicon CR Rel-17 38.331 17.3.0 3790 - F NR\_NTN\_solutions-Core

# Appendix 1: Proposed TP for the field description of epochTime in otherConfig

================================= TEXT PROPOSAL START =================================

– *OtherConfig*

The IE *OtherConfig* contains configuration related to miscellaneous other configurations.

***OtherConfig* information element**

-- ASN1START

-- TAG-OTHERCONFIG-START

OtherConfig ::= SEQUENCE {

 delayBudgetReportingConfig CHOICE{

 release NULL,

 setup SEQUENCE{

 delayBudgetReportingProhibitTimer ENUMERATED {s0, s0dot4, s0dot8, s1dot6, s3, s6, s12, s30}

 }

 } OPTIONAL -- Need M

}

OtherConfig-v1540 ::= SEQUENCE {

 overheatingAssistanceConfig SetupRelease {OverheatingAssistanceConfig} OPTIONAL, -- Need M

 ...

}

CandidateServingFreqListNR-r16 ::= SEQUENCE (SIZE (1..maxFreqIDC-r16)) OF ARFCN-ValueNR

OtherConfig-v1610 ::= SEQUENCE {

 idc-AssistanceConfig-r16 SetupRelease {IDC-AssistanceConfig-r16} OPTIONAL, -- Need M

 drx-PreferenceConfig-r16 SetupRelease {DRX-PreferenceConfig-r16} OPTIONAL, -- Need M

 maxBW-PreferenceConfig-r16 SetupRelease {MaxBW-PreferenceConfig-r16} OPTIONAL, -- Need M

 maxCC-PreferenceConfig-r16 SetupRelease {MaxCC-PreferenceConfig-r16} OPTIONAL, -- Need M

 maxMIMO-LayerPreferenceConfig-r16 SetupRelease {MaxMIMO-LayerPreferenceConfig-r16} OPTIONAL, -- Need M

 minSchedulingOffsetPreferenceConfig-r16 SetupRelease {MinSchedulingOffsetPreferenceConfig-r16} OPTIONAL, -- Need M

 releasePreferenceConfig-r16 SetupRelease {ReleasePreferenceConfig-r16} OPTIONAL, -- Need M

 referenceTimePreferenceReporting-r16 ENUMERATED {true} OPTIONAL, -- Need R

 btNameList-r16 SetupRelease {BT-NameList-r16} OPTIONAL, -- Need M

 wlanNameList-r16 SetupRelease {WLAN-NameList-r16} OPTIONAL, -- Need M

 sensorNameList-r16 SetupRelease {Sensor-NameList-r16} OPTIONAL, -- Need M

 obtainCommonLocation-r16 ENUMERATED {true} OPTIONAL, -- Need R

 sl-AssistanceConfigNR-r16 ENUMERATED{true} OPTIONAL -- Need R

}

OtherConfig-v1700 ::= SEQUENCE {

 ul-GapFR2-PreferenceConfig-r17 ENUMERATED {true} OPTIONAL, -- Need R

 musim-GapAssistanceConfig-r17 SetupRelease {MUSIM-GapAssistanceConfig-r17} OPTIONAL, -- Need M

 musim-LeaveAssistanceConfig-r17 SetupRelease {MUSIM-LeaveAssistanceConfig-r17} OPTIONAL, -- Need M

 successHO-Config-r17 SetupRelease {SuccessHO-Config-r17} OPTIONAL, -- Need M

 maxBW-PreferenceConfigFR2-2-r17 ENUMERATED {true} OPTIONAL, -- Cond maxBW

 maxMIMO-LayerPreferenceConfigFR2-2-r17 ENUMERATED {true} OPTIONAL, -- Cond maxMIMO

 minSchedulingOffsetPreferenceConfigExt-r17 ENUMERATED {true} OPTIONAL, -- Cond minOffset

 rlm-RelaxationReportingConfig-r17 SetupRelease {RLM-RelaxationReportingConfig-r17} OPTIONAL, -- Need M

 bfd-RelaxationReportingConfig-r17 SetupRelease {BFD-RelaxationReportingConfig-r17} OPTIONAL, -- Need M

 scg-DeactivationPreferenceConfig-r17 SetupRelease {SCG-DeactivationPreferenceConfig-r17} OPTIONAL, -- Cond SCG

 rrm-MeasRelaxationReportingConfig-r17 SetupRelease {RRM-MeasRelaxationReportingConfig-r17} OPTIONAL, -- Need M

 propDelayDiffReportConfig-r17 SetupRelease {PropDelayDiffReportConfig-r17} OPTIONAL -- Need M

}

MUSIM-GapAssistanceConfig-r17 ::= SEQUENCE {

 musim-GapProhibitTimer-r17 ENUMERATED {s0, s0dot1, s0dot2, s0dot3, s0dot4, s0dot5, s1, s2, s3, s4, s5, s6, s7, s8, s9, s10}

}

MUSIM-LeaveAssistanceConfig-r17 ::= SEQUENCE {

 musim-LeaveWithoutResponseTimer-r17 ENUMERATED {ms10, ms20, ms40, ms60, ms80, ms100, spare2, spare1}

}

SuccessHO-Config-r17 ::= SEQUENCE {

 thresholdPercentageT304-r17 ENUMERATED {p40, p60, p80, spare5, spare4, spare3, spare2, spare1} OPTIONAL, --Need R

 thresholdPercentageT310-r17 ENUMERATED {p40, p60, p80, spare5, spare4, spare3, spare2, spare1} OPTIONAL, --Need R

 thresholdPercentageT312-r17 ENUMERATED {p20, p40, p60, p80, spare4, spare3, spare2, spare1} OPTIONAL, --Need R

 sourceDAPS-FailureReporting-r17 ENUMERATED {true} OPTIONAL, --Need R

 ...

}

OverheatingAssistanceConfig ::= SEQUENCE {

 overheatingIndicationProhibitTimer ENUMERATED {s0, s0dot5, s1, s2, s5, s10, s20, s30,

 s60, s90, s120, s300, s600, spare3, spare2, spare1}

}

IDC-AssistanceConfig-r16 ::= SEQUENCE {

 candidateServingFreqListNR-r16 CandidateServingFreqListNR-r16 OPTIONAL, -- Need R

 ...

}

DRX-PreferenceConfig-r16 ::= SEQUENCE {

 drx-PreferenceProhibitTimer-r16 ENUMERATED {

 s0, s0dot5, s1, s2, s3, s4, s5, s6, s7,

 s8, s9, s10, s20, s30, spare2, spare1}

}

MaxBW-PreferenceConfig-r16 ::= SEQUENCE {

 maxBW-PreferenceProhibitTimer-r16 ENUMERATED {

 s0, s0dot5, s1, s2, s3, s4, s5, s6, s7,

 s8, s9, s10, s20, s30, spare2, spare1}

}

MaxCC-PreferenceConfig-r16 ::= SEQUENCE {

 maxCC-PreferenceProhibitTimer-r16 ENUMERATED {

 s0, s0dot5, s1, s2, s3, s4, s5, s6, s7,

 s8, s9, s10, s20, s30, spare2, spare1}

}

MaxMIMO-LayerPreferenceConfig-r16 ::= SEQUENCE {

 maxMIMO-LayerPreferenceProhibitTimer-r16 ENUMERATED {

 s0, s0dot5, s1, s2, s3, s4, s5, s6, s7,

 s8, s9, s10, s20, s30, spare2, spare1}

}

MinSchedulingOffsetPreferenceConfig-r16 ::= SEQUENCE {

 minSchedulingOffsetPreferenceProhibitTimer-r16 ENUMERATED {

 s0, s0dot5, s1, s2, s3, s4, s5, s6, s7,

 s8, s9, s10, s20, s30, spare2, spare1}

}

ReleasePreferenceConfig-r16 ::= SEQUENCE {

 releasePreferenceProhibitTimer-r16 ENUMERATED {

 s0, s0dot5, s1, s2, s3, s4, s5, s6, s7,

 s8, s9, s10, s20, s30, infinity, spare1},

 connectedReporting ENUMERATED {true} OPTIONAL -- Need R

}

RLM-RelaxationReportingConfig-r17 ::= SEQUENCE {

 rlm-RelaxtionReportingProhibitTimer ENUMERATED {s0, s0dot5, s1, s2, s5, s10, s20, s30,

 s60, s90, s120, s300, s600, infinity, spare2, spare1}

}

BFD-RelaxationReportingConfig-r17 ::= SEQUENCE {

 bfd-RelaxtionReportingProhibitTimer ENUMERATED {s0, s0dot5, s1, s2, s5, s10, s20, s30,

 s60, s90, s120, s300, s600, infinity, spare2, spare1}

}

SCG-DeactivationPreferenceConfig-r17 ::= SEQUENCE {

 scg-DeactivationPreferenceProhibitTimer-r17 ENUMERATED {

 s0, s1, s2, s4, s8, s10, s15, s30,

 s60, s120, s180, s240, s300, s600, s900, s1800}

}

RRM-MeasRelaxationReportingConfig-r17 ::= SEQUENCE {

 s-SearchDeltaP-Stationary-r17 ENUMERATED {dB2, dB3, dB6, dB9, dB12, dB15, spare2, spare1},

 t-SearchDeltaP-Stationary-r17 ENUMERATED {s5, s10, s20, s30, s60, s120, s180, s240, s300, spare7, spare6, spare5,

 spare4, spare3, spare2, spare1}

}

PropDelayDiffReportConfig-r17 ::= SEQUENCE {

 threshPropDelayDiff-r17 ENUMERATED {ms0dot5, ms1, ms2, ms3, ms4, ms5, ms6 ,ms7, ms8, ms9, ms10, spare5,

 spare4, spare3, spare2, spare1} OPTIONAL, -- Need M

 neighCellInfoList-r17 SEQUENCE (SIZE (1..maxCellNTN-r17)) OF NeighbourCellInfo-r17 OPTIONAL -- Need M

}

NeighbourCellInfo-r17 ::= SEQUENCE {

epochTime-r17 EpochTime-r17,

ephemerisInfo-r17 EphemerisInfo-r17

}

-- TAG-OTHERCONFIG-STOP

-- ASN1STOP

| ***OtherConfig* field descriptions** |
| --- |
| ***bfd-RelaxationReportingConfig***Configuration for the UE to report the relaxation state of BFD measurements. |
| ***candidateServingFreqListNR***Indicates for each candidate NR serving cells, the center frequency around which UE is requested to report IDC issues. |
| ***connectedReporting***Indicates that the UE can report a preference to remain in RRC\_CONNECTED state following a report to leave RRC\_CONNECTED state. If absent, the UE cannot report a preference to stay in RRC\_CONNECTED state. |
| ***delayBudgetReportingProhibitTimer***Prohibit timer for delay budget reporting. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot4* means prohibit timer is set to 0.4 seconds, and so on. |
| ***drx-PreferenceConfig***Configuration for the UE to report assistance information to inform the gNB about the UE's DRX preferences for power saving. |
| ***drx-PreferenceProhibitTimer***Prohibit timer for DRX preferences assistance information reporting. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot5* means prohibit timer is set to 0.5 seconds, value *s1* means prohibit timer is set to 1 second and so on. |
| ***idc-AssistanceConfig***Configuration for the UE to report assistance information to inform the gNB about UE detected IDC problem. |
| ***maxBW-PreferenceConfig***Configuration for the UE to report assistance information to inform the gNB about the UE's preferred bandwidth for power saving. |
| ***maxBW-PreferenceProhibitTimer***Prohibit timer for preferred bandwidth assistance information reporting. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot5* means prohibit timer is set to 0.5 seconds, value *s1* means prohibit timer is set to 1 second and so on. |
| ***maxCC-PreferenceConfig***Configuration for the UE to report assistance information to inform the gNB about the UE's preferred number of carriers for power saving. |
| ***maxBW-PreferenceConfigFR2-2***Configuration for the UE to report assistance information to inform the gNB about the UE's preferred bandwidth for power saving for FR2-2. |
| ***maxCC-PreferenceProhibitTimer***Prohibit timer for preferred number of carriers assistance information reporting. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot5* means prohibit timer is set to 0.5 seconds, value *s1* means prohibit timer is set to 1 second and so on. |
| ***maxMIMO-LayerPreferenceConfig***Configuration for the UE to report assistance information to inform the gNB about the UE's preferred number of MIMO layers for power saving. |
| ***maxMIMO-LayerPreferenceConfigFR2-2***Configuration for the UE to report assistance information to inform the gNB about the UE's preferred number of MIMO layers for power saving for FR2-2. |
| ***maxMIMO-LayerPreferenceProhibitTimer***Prohibit timer for preferred number of number of MIMO layers assistance information reporting. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot5* means prohibit timer is set to 0.5 seconds, value *s1* means prohibit timer is set to 1 second and so on. |
| ***minSchedulingOffsetPreferenceConfig***Configuration for the UE to report assistance information to inform the gNB about the UE's preferred *minimumSchedulingOffset* value for cross-slot scheduling for power saving. |
| ***minSchedulingOffsetPreferenceConfigExt***Configuration for the UE to report assistance information to inform the gNB about the UE's preferred *minimumSchedulingOffset* value for cross-slot scheduling for power saving for SCS 480 kHz and/or 960 kHz. |
| ***minSchedulingOffsetPreferenceProhibitTimer***Prohibit timer for preferred *minimumSchedulingOffset* assistance information reporting. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot5* means prohibit timer is set to 0.5 seconds, value *s1* means prohibit timer is set to 1 second and so on. |
| ***musim-GapAssistanceConfig***Configuration for the UE to report assistance information for gap preference. |
| ***musim-GapProhibitTimer***Prohibit timer for MUSIM assistance information reporting for gap preference. |
| ***musim-LeaveAssistanceConfig***Configuration for the UE to report assistance information for leaving RRC\_CONNECTED for MUSIM purpose. |
| ***musim-LeaveWithoutResponseTimer***Indicates the timer for the UE to enter RRC\_IDLE for MUSIM purpose as defined in clause 5.3.8.6. |
| ***obtainCommonLocation***Requests the UE to attempt to have detailed location information available using GNSS. NR configures the field if *includeCommonLocationInfo* is configured for one or more measurements. |
| ***overheatingAssistanceConfig***Configuration for the UE to report assistance information to inform the gNB about UE detected internal overheating. |
| ***overheatingIndicationProhibitTimer***Prohibit timer for overheating assistance information reporting. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot5* means prohibit timer is set to 0.5 seconds, value *s1* means prohibit timer is set to 1 second and so on. |
| ***propDelayDiffReportConfig***Configuration for the UE to report service link propagation delay difference between serving cell and neighbour cell(s). |
| ***referenceTimePreferenceReporting***If present, the field indicates the UE is configured to provide reference time assistance information. |
| ***releasePreferenceConfig***Configuration for the UE to report assistance information to inform the gNB about the UE's preference to leave RRC\_CONNECTED state. |
| ***rlm-RelaxationReportingConfig***Configuration for the UE to report the relaxation state of RLM measurements. |
| ***releasePreferenceProhibitTimer***Prohibit timer for release preference assistance information reporting. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot5* means prohibit timer is set to 0.5 seconds, value *s1* means prohibit timer is set to 1 second and so on. Value *infinity* means that once a UE has reported a release preference, the UE cannot report a release preference again during the RRC connection. |
| ***s-SearchDeltaP-Stationary***Parameter "SSearchDeltaP-StationaryConnected" in 5.7.4.4. Value dB2 corresponds to 2 dB, dB3 corresponds to 3 dB and so on. |
| ***scg-DeactivationPreferenceConfig***Configuration of the UE to indicate its preference for SCG deactivation. |
| ***scg -StatePreferenceProhibitTimer***Prohibit timer for UE indication of its preference for SCG deactivation. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s1* means prohibit timer is set to 1 second and so on. |
| ***sensorNameList***Configuration for the UE to report measurements from specific sensors. |
| ***sl-AssistanceConfigNR***Indicate whether UE is configured to provide configured grant assistance information for NR sidelink communication. |
| ***sourceDAPS-FailureReporting***This field indicates whether the UE shall generate the SHR upon successfully completing the DAPS handover to the target cell and if a radio link failure was experienced in the source PCell while executing the DAPS handover. This field is set in the *otherConfig* configured by the source cell of the DAPS handover. |
| ***successHO-Config***Configuration for the UE to report the successful handover information to the network. |
| ***t-SearchDeltaP-Stationary***Parameter "TSearchDeltaP-StationaryConnected" in 5.7.4.4. Value in seconds. Value s5 means 5 seconds, value s10 means 10 seconds and so on. |
| ***thresholdPercentageT304***This field indicates the threshold for the ratio in percentage between the elapsed T304 timer and the configured value of the T304 timer. Value *p40* corresponds to 40%, value *p60* corresponds to 60% and so on. This field is set in the *otherConfig* configured by the target cell of the handover. |
| ***thresholdPercentageT310***This field indicates the threshold for the ratio in percentage between the elapsed T310 timer and the configured value of the T310 timer. Value *p40* corresponds to 40%, value *p60* corresponds to 60% and so on. This field is set in the *otherConfig* configured by the source cell of the handover. |
| ***thresholdPercentageT312***This field indicates the threshold for the ratio in percentage between the elapsed T312 timer and the configured value(s) of the T312 timer. Value *p20* corresponds to 20%, value *p40* corresponds to 40% and so on. This field is set in the *otherConfig* configured by the source cell of the handover. |
| ***threshPropDelayDiff***Threshold for service link propagation delay difference report as specified in 5.7.4.2. |
| ***ul-GapFR2-PreferenceConfig***Indicates whether UE is configured to request for FR2 UL gap activation/deactivation and preferred FR2 UL gap pattern. |

| ***NeighbourCellInfo* field descriptions** |
| --- |
| ***epochTime***Indicates the epoch time used along with the *ephemerisInfo* to derive the propagation delay difference for the associated neighbour cell. The UE considers epoch time, indicated by the SFN and sub-frame number in this field, to be the frame nearest to the frame in which the message indicating the epoch time is received. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *maxBW* | This field is optionally present, need R, if *maxBW-PreferenceConfig-r16* is setup; otherwise it is absent, need R. |
| *maxMIMO* | This field is optionally present, need R, if *maxMIMO-LayerPreferenceConfig-r16* is setup; otherwise it is absent, need R. |
| *minOffset* | This field is optionally present, need R, if *minSchedulingOffsetPreferenceConfig-r16* is setup; otherwise it is absent, need R. |
| *SCG* | This field is optionally present, need M, in an *RRCReconfiguration* message not within *mrdc-SecondaryCellGroup* and received, either via SRB3 within *DLInformationTransferMRDC* or via SRB1. Otherwise, it is absent. |

================================= TEXT PROPOSAL END =================================

# Appendix 2: TP-1 for SMTC and inter-node message

<Start of 1st Change>

6.3.1 System information blocks

– *SIB2*

*SIB2* contains cell re-selection information common for intra-frequency, inter-frequency and/or inter-RAT cell re-selection (i.e. applicable for more than one type of cell re-selection but not necessarily all) as well as intra-frequency cell re-selection information other than neighbouring cell related.

***SIB2* information element**

-- ASN1START

-- TAG-SIB2-START

SIB2 ::= SEQUENCE {

 cellReselectionInfoCommon SEQUENCE {

 nrofSS-BlocksToAverage INTEGER (2..maxNrofSS-BlocksToAverage) OPTIONAL, -- Need S

 absThreshSS-BlocksConsolidation ThresholdNR OPTIONAL, -- Need S

 rangeToBestCell RangeToBestCell OPTIONAL, -- Need R

 q-Hyst ENUMERATED {

 dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,

 dB12, dB14, dB16, dB18, dB20, dB22, dB24},

 speedStateReselectionPars SEQUENCE {

 mobilityStateParameters MobilityStateParameters,

 q-HystSF SEQUENCE {

 sf-Medium ENUMERATED {dB-6, dB-4, dB-2, dB0},

 sf-High ENUMERATED {dB-6, dB-4, dB-2, dB0}

 }

 } OPTIONAL, -- Need R

 ...

 },

 cellReselectionServingFreqInfo SEQUENCE {

 s-NonIntraSearchP ReselectionThreshold OPTIONAL, -- Need S

 s-NonIntraSearchQ ReselectionThresholdQ OPTIONAL, -- Need S

 threshServingLowP ReselectionThreshold,

 threshServingLowQ ReselectionThresholdQ OPTIONAL, -- Need R

 cellReselectionPriority CellReselectionPriority,

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL, -- Need R

 ...

 },

 intraFreqCellReselectionInfo SEQUENCE {

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 s-IntraSearchP ReselectionThreshold,

 s-IntraSearchQ ReselectionThresholdQ OPTIONAL, -- Need S

 t-ReselectionNR T-Reselection,

 frequencyBandList MultiFrequencyBandListNR-SIB OPTIONAL, -- Need S

 frequencyBandListSUL MultiFrequencyBandListNR-SIB OPTIONAL, -- Need R

 p-Max P-Max OPTIONAL, -- Need S

 smtc SSB-MTC OPTIONAL, -- Need S

 ss-RSSI-Measurement SS-RSSI-Measurement OPTIONAL, -- Need R

 ssb-ToMeasure SSB-ToMeasure OPTIONAL, -- Need S

 deriveSSB-IndexFromCell BOOLEAN,

 ...,

 [[

 t-ReselectionNR-SF SpeedStateScaleFactors OPTIONAL -- Need N

 ]],

 [[

 smtc2-LP-r16 SSB-MTC2-LP-r16 OPTIONAL, -- Need R

 ssb-PositionQCL-Common-r16 SSB-PositionQCL-Relation-r16 OPTIONAL -- Cond SharedSpectrum

 ]],

 [[

 ssb-PositionQCL-Common-r17 SSB-PositionQCL-Relation-r17 OPTIONAL -- Cond SharedSpectrum2

 ]],

 [[

 smtc4list-r17 SSB-MTC4List-r17 OPTIONAL -- Need R

 ]]

 },

 ...,

 [[

 relaxedMeasurement-r16 SEQUENCE {

 lowMobilityEvaluation-r16 SEQUENCE {

 s-SearchDeltaP-r16 ENUMERATED {

 dB3, dB6, dB9, dB12, dB15,

 spare3, spare2, spare1},

 t-SearchDeltaP-r16 ENUMERATED {

 s5, s10, s20, s30, s60, s120, s180,

 s240, s300, spare7, spare6, spare5,

 spare4, spare3, spare2, spare1}

 } OPTIONAL, -- Need R

 cellEdgeEvaluation-r16 SEQUENCE {

 s-SearchThresholdP-r16 ReselectionThreshold,

 s-SearchThresholdQ-r16 ReselectionThresholdQ OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 combineRelaxedMeasCondition-r16 ENUMERATED {true} OPTIONAL, -- Need R

 highPriorityMeasRelax-r16 ENUMERATED {true} OPTIONAL -- Need R

 } OPTIONAL -- Need R

 ]],

 [[

 cellEquivalentSize-r17 INTEGER(2..16) OPTIONAL, -- Cond HSDN

 relaxedMeasurement-r17 SEQUENCE {

 stationaryMobilityEvaluation-r17 SEQUENCE {

 s-SearchDeltaP-Stationary-r17 ENUMERATED {dB2, dB3, dB6, dB9, dB12, dB15, spare2, spare1},

 t-SearchDeltaP-Stationary-r17 ENUMERATED {s5, s10, s20, s30, s60, s120, s180, s240, s300, spare7, spare6, spare5,

 spare4, spare3, spare2, spare1}

 },

 cellEdgeEvaluationWhileStationary-r17 SEQUENCE {

 s-SearchThresholdP2-r17 ReselectionThreshold,

 s-SearchThresholdQ2-r17 ReselectionThresholdQ OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 combineRelaxedMeasCondition2-r17 ENUMERATED {true} OPTIONAL -- Need R

 } OPTIONAL -- Need R

 ]]

}

RangeToBestCell ::= Q-OffsetRange

-- TAG-SIB2-STOP

-- ASN1STOP

| ***SIB2* field descriptions** |
| --- |
| ***absThreshSS-BlocksConsolidation***Threshold for consolidation of L1 measurements per RS index. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***cellEdgeEvaluation***Indicates the criteria for a UE to detect that it is not at cell edge, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.2). |
| ***cellEdgeEvaluationWhileStationary***Indicates the criteria for a UE to detect that it is not at cell edge while stationary, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.4). |
| ***cellEquivalentSize***The number of cell count used for mobility state estimation for this cell as specified in TS 38.304 [20]. |
| ***cellReselectionInfoCommon***Cell re-selection information common for intra-frequency, inter-frequency and/ or inter-RAT cell re-selection. |
| ***cellReselectionServingFreqInfo***Information common for non-intra-frequency cell re-selection i.e. cell re-selection to inter-frequency and inter-RAT cells. |
| ***combineRelaxedMeasCondition***When both *lowMobilityEvalutation* and *cellEdgeEvalutation* criteria are present in SIB2, this parameter configures the UE to fulfil both criteria in order to relax measurement requirements for cell reselection. If the field is absent, the UE is allowed to relax measurement requirements for cell reselection when either or both of the criteria are met. (See TS 38.304 [20], clause 5.2.4.9.0) |
| ***combineRelaxedMeasCondition2***When both *stationaryMobilityEvaluation* and *cellEdgeEvaluationWhileStationary* criteria are present in SIB2, this parameter configures the UE to fulfil both criteria in order to relax measurement requirements for cell reselection. If the field is absent, the UE is allowed to relax measurement requirements for cell reselection when only the stationary criteria is met. (See TS 38.304 [20], clause 5.2.4.9.0) |
| ***deriveSSB-IndexFromCell***This field indicates whether the UE can utilize serving cell timing to derive the index of SS block transmitted by neighbour cell. If this field is set to *true*, the UE assumes SFN and frame boundary alignment across cells on the serving frequency as specified in TS 38.133 [14]. |
| ***frequencyBandList***Indicates the list of frequency bands for which the NR cell reselection parameters apply. The UE behaviour in case the field is absent is described in clause 5.2.2.4.3. |
| ***highPriorityMeasRelax***Indicates whether measurements can be relaxed on high priority frequencies. If the field is absent, the UE shall not relax measurements on high priority frequencies beyond "Thigher\_priority\_search" unless both low mobility and not at cell edge criteria are fulfilled (see TS 38.133 [14], clauses 4.2.2.7, 4.2.2.10 and 4.2.2.11). |
| ***intraFreqCellReselectionInfo***Cell re-selection information common for intra-frequency cells. |
| ***lowMobilityEvaluation***Indicates the criteria for a UE to detect low mobility, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.1). |
| ***nrofSS-BlocksToAverage***Number of SS blocks to average for cell measurement derivation. If the field is absent the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***p-Max***Value in dBm applicable for the intra-frequency neighbouring NR cells. If absent the UE applies the maximum power according to TS 38.101-1 [15] in case of an FR1 cell or TS 38.101-2 [39] in case of an FR2 cell. In this release of the specification, if *p-Max* is present on a carrier frequency in FR2, the UE shall ignore the field and applies the maximum power according to TS 38.101-2 [39]. This field is ignored by IAB-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [63]. |
| ***q-Hyst***Parameter "*Qhyst*" in TS 38.304 [20], Value in dB. Value *dB1* corresponds to 1 dB, *dB2* corresponds to 2 dB and so on. |
| ***q-HystSF***Parameter "Speed dependent ScalingFactor for Qhyst" in TS 38.304 [20]. The *sf-Medium* and *sf-High* concern the additional hysteresis to be applied, in Medium and High Mobility state respectively, to Qhyst as defined in TS 38.304 [20]. In dB. Value *dB-6* corresponds to -6dB, *dB-4* corresponds to -4dB and so on. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin.  |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. |
| ***rangeToBestCell***Parameter "rangeToBestCell" in TS 38.304 [20]. The network configures only non-negative (in dB) values. |
| ***relaxedMeasurement***Configuration to allow relaxation of RRM measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9). |
| ***s-IntraSearchP***Parameter "SIntraSearchP" in TS 38.304 [20]. |
| ***s-IntraSearchQ***Parameter "SIntraSearchQ" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of 0 dB for SIntraSearchQ. |
| ***s-NonIntraSearchP***Parameter "SnonIntraSearchP" in TS 38.304 [20]. If this field is absent, the UE applies the (default) value of infinity for SnonIntraSearchP. |
| ***s-NonIntraSearchQ***Parameter "SnonIntraSearchQ" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of 0 dB for SnonIntraSearchQ. |
| ***s-SearchDeltaP***Parameter "SSearchDeltaP" in TS 38.304 [20]. Value dB3 corresponds to 3 dB, dB6 corresponds to 6 dB and so on. |
| ***s-SearchDeltaP-Stationary***Parameter "SSearchDeltaP-Stationary" in TS 38.304 [20]. Value *dB2* corresponds to 2 dB, *dB3* corresponds to 3 dB and so on. |
| ***s-SearchThresholdP, s-SearchThresholdP2***Parameters "SSearchThresholdP" and "SSearchThresholdP2" in TS 38.304 [20]. The network configures *s-SearchThresholdP* and *s-SearchThresholdP2* to be less than or equal to *s-IntraSearchP* and *s-NonIntraSearchP*. |
| ***s-SearchThresholdQ, s-SearchThresholdQ2***Parameters "SSearchThresholdQ" and "SSearchThresholdQ2" in TS 38.304 [20]. The network configures *s-SearchThresholdQ* and *s-SearchThresholdQ2* to be less than or equal to *s-IntraSearchQ* and *s-NonIntraSearchQ*. |
| ***smtc***Measurement timing configuration for intra-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms for the intra-frequnecy cells. If the field is broadcast by an NTN cell, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and the feeder link delay corresponding to *epochTime* in SIB19 is compensated. The UE can adjust the actual *offset* based on the actual propagation delay difference. |
| ***smtc2-LP***Measurement timing configuration for intra-frequency neighbour cells with a Long Periodicity (LP) indicated by periodicity in *smtc2-LP*. The timing offset and duration are equal to the offset and duration indicated in *smtc* in *intraFreqCellReselectionInfo*. The periodicity in *smtc2-LP* can only be set to a value strictly larger than the periodicity in *smtc* in *intraFreqCellReselectionInfo* (e.g. if *smtc* indicates sf20 the Long Periodicity can only be set to sf40, sf80 or sf160, if *smtc* indicates sf160, *smtc2-LP* cannot be configured). The *pci-List*, if present, includes the physical cell identities of the intra-frequency neighbour cells with Long Periodicity. If *smtc2-LP* is absent, the UE assumes that there are no intra-frequency neighbour cells with a Long Periodicity. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and the feeder link delay corresponding to *epochTime* in SIB19 is compensated. The UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |
| ***ssb-PositionQCL-Common***Indicates the QCL relation between SS/PBCH blocks for intra-frequency neighbor cells as specified in TS 38.213 [13], clause 4.1. |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). When the field is absent the UE measures on all SS-blocks. |
| ***stationaryMobilityEvaluation***Indicates the criteria for a UE to detect stationary mobility, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.0). |
| ***t-ReselectionNR***Parameter "TreselectionNR" in TS 38.304 [20]. |
| ***t-ReselectionNR-SF***Parameter "Speed dependent ScalingFactor for TreselectionNR" in TS 38.304 [20]. If the field is absent, the UE behaviour is specified in TS 38.304 [20]. |
| ***threshServingLowP***Parameter "ThreshServing, LowP" in TS 38.304 [20]. |
| ***threshServingLowQ***Parameter "ThreshServing, LowQ" in TS 38.304 [20]. |
| ***t-SearchDeltaP***Parameter "TSearchDeltaP" in TS 38.304 [20]. Value in seconds. Value *s5* means 5 seconds, value *s10* means 10 seconds and so on. |
| ***t-SearchDeltaP-Stationary***Parameter "TSearchDeltaP-Stationary" in TS 38.304 [20]. Value in seconds. Value *s5* means 5 seconds, value *s10* means 10 seconds and so on. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *HSDN* | The field is optionally present, Need R, if *speedStateReselectionPars* is present; otherwise the field is not present. |
| *SharedSpectrum* | This field is mandatory present if this intra-frequency operates with shared spectrum channel access in FR1. Otherwise, it is absent, Need R. |
| *SharedSpectrum2* | This field is optionally present if this intra-frequency operates with shared spectrum channel access in FR2-2, Need R. Otherwise, it is absent, Need R. |

[Unchanged parts omitted]

– *SIB4*

*SIB4* contains information relevant for inter-frequency cell re-selection (i.e. information about other NR frequencies and inter-frequency neighbouring cells relevant for cell re-selection), which can also be used for NR idle/inactive measurements. The IE includes cell re-selection parameters common for a frequency as well as cell specific re-selection parameters.

***SIB4* information element**

-- ASN1START

-- TAG-SIB4-START

SIB4 ::= SEQUENCE {

 interFreqCarrierFreqList InterFreqCarrierFreqList,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 ...,

 [[

 interFreqCarrierFreqList-v1610 InterFreqCarrierFreqList-v1610 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1700 InterFreqCarrierFreqList-v1700 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1720 InterFreqCarrierFreqList-v1720 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1730 InterFreqCarrierFreqList-v1730 OPTIONAL -- Need R

 ]]

}

InterFreqCarrierFreqList ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo

InterFreqCarrierFreqList-v1610 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1610

InterFreqCarrierFreqList-v1700 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1700

InterFreqCarrierFreqList-v1720 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1720

InterFreqCarrierFreqList-v1730 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1730

InterFreqCarrierFreqInfo ::= SEQUENCE {

 dl-CarrierFreq ARFCN-ValueNR,

 frequencyBandList MultiFrequencyBandListNR-SIB OPTIONAL, -- Cond Mandatory

 frequencyBandListSUL MultiFrequencyBandListNR-SIB OPTIONAL, -- Need R

 nrofSS-BlocksToAverage INTEGER (2..maxNrofSS-BlocksToAverage) OPTIONAL, -- Need S

 absThreshSS-BlocksConsolidation ThresholdNR OPTIONAL, -- Need S

 smtc SSB-MTC OPTIONAL, -- Need S

 ssbSubcarrierSpacing SubcarrierSpacing,

 ssb-ToMeasure SSB-ToMeasure OPTIONAL, -- Need S

 deriveSSB-IndexFromCell BOOLEAN,

 ss-RSSI-Measurement SS-RSSI-Measurement OPTIONAL, -- Need R

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 p-Max P-Max OPTIONAL, -- Need S

 t-ReselectionNR T-Reselection,

 t-ReselectionNR-SF SpeedStateScaleFactors OPTIONAL, -- Need S

 threshX-HighP ReselectionThreshold,

 threshX-LowP ReselectionThreshold,

 threshX-Q SEQUENCE {

 threshX-HighQ ReselectionThresholdQ,

 threshX-LowQ ReselectionThresholdQ

 } OPTIONAL, -- Cond RSRQ

 cellReselectionPriority CellReselectionPriority OPTIONAL, -- Need R

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL, -- Need R

 q-OffsetFreq Q-OffsetRange DEFAULT dB0,

 interFreqNeighCellList InterFreqNeighCellList OPTIONAL, -- Need R

 interFreqExcludedCellList InterFreqExcludedCellList OPTIONAL, -- Need R

 ...

}

InterFreqCarrierFreqInfo-v1610 ::= SEQUENCE {

 interFreqNeighCellList-v1610 InterFreqNeighCellList-v1610 OPTIONAL, -- Need R

 smtc2-LP-r16 SSB-MTC2-LP-r16 OPTIONAL, -- Need R

 interFreqAllowedCellList-r16 InterFreqAllowedCellList-r16 OPTIONAL, -- Cond SharedSpectrum2

 ssb-PositionQCL-Common-r16 SSB-PositionQCL-Relation-r16 OPTIONAL, -- Cond SharedSpectrum

 interFreqCAG-CellList-r16 SEQUENCE (SIZE (1..maxPLMN)) OF InterFreqCAG-CellListPerPLMN-r16 OPTIONAL -- Need R

}

InterFreqCarrierFreqInfo-v1700 ::= SEQUENCE {

 interFreqNeighHSDN-CellList-r17 InterFreqNeighHSDN-CellList-r17 OPTIONAL, -- Need R

 highSpeedMeasInterFreq-r17 ENUMERATED {true} OPTIONAL, -- Need R

 redCapAccessAllowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 ssb-PositionQCL-Common-r17 SSB-PositionQCL-Relation-r17 OPTIONAL, -- Cond SharedSpectrum

 interFreqNeighCellList-v1710 InterFreqNeighCellList-v1710 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqCarrierFreqInfo-v1720 ::= SEQUENCE {

 smtc4list-r17 SSB-MTC4List-r17 OPTIONAL -- Need R

}

InterFreqCarrierFreqInfo-v1730 ::= SEQUENCE {

 channelAccessMode2-r17 ENUMERATED {enabled} OPTIONAL -- Need R

}

InterFreqNeighHSDN-CellList-r17 ::= SEQUENCE (SIZE (1..maxCellInter)) OF PCI-Range

InterFreqNeighCellList ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo

InterFreqNeighCellList-v1610 ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo-v1610

InterFreqNeighCellList-v1710 ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo-v1710

InterFreqNeighCellInfo ::= SEQUENCE {

 physCellId PhysCellId,

 q-OffsetCell Q-OffsetRange,

 q-RxLevMinOffsetCell INTEGER (1..8) OPTIONAL, -- Need R

 q-RxLevMinOffsetCellSUL INTEGER (1..8) OPTIONAL, -- Need R

 q-QualMinOffsetCell INTEGER (1..8) OPTIONAL, -- Need R

 ...

}

InterFreqNeighCellInfo-v1610 ::= SEQUENCE {

 ssb-PositionQCL-r16 SSB-PositionQCL-Relation-r16 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqNeighCellInfo-v1710 ::= SEQUENCE {

 ssb-PositionQCL-r17 SSB-PositionQCL-Relation-r17 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqExcludedCellList ::= SEQUENCE (SIZE (1..maxCellExcluded)) OF PCI-Range

InterFreqAllowedCellList-r16 ::= SEQUENCE (SIZE (1..maxCellAllowed)) OF PCI-Range

InterFreqCAG-CellListPerPLMN-r16 ::= SEQUENCE {

 plmn-IdentityIndex-r16 INTEGER (1..maxPLMN),

 cag-CellList-r16 SEQUENCE (SIZE (1..maxCAG-Cell-r16)) OF PCI-Range

}

-- TAG-SIB4-STOP

-- ASN1STOP

| ***SIB4* field descriptions** |
| --- |
| ***absThreshSS-BlocksConsolidation***Threshold for consolidation of L1 measurements per RS index. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***channelAccessMode2***If present, this field indicates that the neighbor cells on the inter-frequency apply channel access mode procedures for operation with shared spectrum channel access in accordance with TS 37.213 [48], clause 4.4 for FR2-2. If absent, the neighbor cells on the inter-frequency do not apply any channel access procedure. |
| ***deriveSSB-IndexFromCell***This field indicates whether the UE may use the timing of any detected cell on that frequency to derive the SSB index of all neighbour cells on that frequency. If this field is set to *true*, the UE assumes SFN and frame boundary alignment across cells on the neighbor frequency as specified in TS 38.133 [14]. |
| ***dl-CarrierFreq***This field indicates center frequency of the SS block of the neighbour cells, where the frequency corresponds to a GSCN value as specified in TS 38.101-1 [15]. |
| ***frequencyBandList***Indicates the list of frequency bands for which the NR cell reselection parameters apply. |
| ***highSpeedMeasInterFreq***If the field is set to *true* and UE supports high speed inter-frequency IDLE/INACTIVE measurements, the UE shall apply the enhanced inter-frequency RRM requirements on the inter-frequency carrier to support high speed up to 500 km/h in RRC\_IDLE/RRC\_INACTIVE as specified in TS 38.133 [14]. |
| ***interFreqAllowedCellList***List of allow-listed inter-frequency neighbouring cells, see TS 38.304 [20], clause 5.2.4. |
| ***interFreqCAG-CellList***List of inter-frequency neighbouring CAG cells (as defined in TS 38.304 [20] per PLMN. |
| ***interFreqCarrierFreqList***List of neighbouring carrier frequencies and frequency specific cell re-selection information. If *interFreqCarrierFreqList-v1610, interFreqCarrierFreqList-v1700, interFreqCarrierFreqList-v1720* or *interFreqCarrierFreqList-v1730* are present, they shall contain the same number of entries, listed in the same order as in *interFreqCarrierFreqList* (without suffix). |
| ***interFreqExcludedCellList***List of exclude-listed inter-frequency neighbouring cells. |
| ***interFreqNeighCellList***List of inter-frequency neighbouring cells with specific cell re-selection parameters. If *interFreqNeighCellList-v1610* is present, it shall contain the same number of entries, listed in the same order as in *interFreqNeighCellList* (without suffix). |
| ***interFreqNeighHSDN-CellList***List of inter-frequency neighbouring HSDN cells as specified in TS 38.304 [20]. |
| ***nrofSS-BlocksToAverage***Number of SS blocks to average for cell measurement derivation. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***p-Max***Value in dBm applicable for the neighbouring NR cells on this carrier frequency. If absent the UE applies the maximum power according to TS 38.101-1 [15] in case of an FR1 cell or TS 38.101-2 [39] in case of an FR2 cell. In this release of the specification, if *p-Max* is present on a carrier frequency in FR2, the UE shall ignore the field and applies the maximum power according to TS 38.101-2 [39]. This field is ignored by IAB-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [63]. |
| ***q-OffsetCell***Parameter "Qoffsets,n" in TS 38.304 [20]. |
| ***q-OffsetFreq***Parameter "Qoffsetfrequency" in TS 38.304 [20]. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin. |
| ***q-QualMinOffsetCell***Parameter "Qqualminoffsetcell" in TS 38.304 [20]. Actual value Qqualminoffsetcell = field value [dB]. |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20]. |
| ***q-RxLevMinOffsetCell***Parameter "Qrxlevminoffsetcell" in TS 38.304 [20]. Actual value Qrxlevminoffsetcell = field value \* 2 [dB]. |
| ***q-RxLevMinOffsetCellSUL***Parameter "QrxlevminoffsetcellSUL" in TS 38.304 [20]. Actual value QrxlevminoffsetcellSUL = field value \* 2 [dB]. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20]. |
| ***redCapAccessAllowed***Indicates whether RedCap UEs are allowed to access the frequency. |
| ***smtc***Measurement timing configuration for inter-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms in this frequency. If the field is broadcast by an NTN cell, the o*ffset* (derived from parameter *periodicityAndOffset*) is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and the feeder link delay corresponding to *epochTime* in SIB19 is compensated. The UE can adjust the actual o*ffset* based on the actual propagation delay difference. |
| ***smtc2-LP***Measurement timing configuration for inter-frequency neighbour cells with a Long Periodicity (LP) indicated by periodicity in *smtc2-LP*. The timing offset and duration are equal to the offset and duration indicated in *smtc* in *InterFreqCarrierFreqInfo*. The periodicity in *smtc2-LP* can only be set to a value strictly larger than the periodicity in *smtc* in *InterFreqCarrierFreqInfo* (e.g. if *smtc* indicates sf20 the Long Periodicity can only be set to sf40, sf80 or sf160, if *smtc* indicates sf160, *smtc2-LP* cannot be configured). The *pci-List*, if present, includes the physical cell identities of the inter-frequency neighbour cells with Long Periodicity. If *smtc2-LP* is absent, the UE assumes that there are no inter-frequency neighbour cells with a Long Periodicity. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and the feeder link delay corresponding to *epochTime* in SIB19 is compensated. The UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |
| ***ssb-PositionQCL***Indicates the QCL relation between SS/PBCH blocks for a specific neighbor cell as specified in TS 38.213 [13], clause 4.1. If provided, the cell specific value overwrites the common value signalled by *ssb-PositionQCL-Common* in *SIB4* for the indicated cell. |
| ***ssb-PositionQCL-Common***Indicates the QCL relation between SS/PBCH blocks for inter-frequency neighbor cells as specified in TS 38.213 [13], clause 4.1. |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). When the field is absent the UE measures on all SS-blocks. |
| ***ssbSubcarrierSpacing***Subcarrier spacing of SSB.Only the following values are applicable depending on the used frequency:FR1: 15 or 30 kHzFR2-1: 120 or 240 kHzFR2-2: 120, 480, or 960 kHz |
| ***threshX-HighP***Parameter "ThreshX, HighP" in TS 38.304 [20]. |
| ***threshX-HighQ***Parameter "ThreshX, HighQ" in TS 38.304 [20]. |
| ***threshX-LowP***Parameter "ThreshX, LowP" in TS 38.304 [20]. |
| ***threshX-LowQ***Parameter "ThreshX, LowQ" in TS 38.304 [20]. |
| ***t-ReselectionNR***Parameter "TreselectionNR" in TS 38.304 [20]. |
| ***t-ReselectionNR-SF***Parameter "Speed dependent ScalingFactor for TreselectionNR" in TS 38.304 [20]. If the field is absent, the UE behaviour is specified in TS 38.304 [20]. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *Mandatory* | The field is mandatory present in SIB4. |
| *RSRQ* | The field is mandatory present if *threshServingLowQ* is present in *SIB2*; otherwise it is absent. |
| *SharedSpectrum* | This field is mandatory present if this inter-frequency operates with shared spectrum channel access. Otherwise, it is absent, Need R. |
| *SharedSpectrum2* | The field is optional present, Need R, if this inter-frequency or neighbor cell operates with shared spectrum channel access. Otherwise, it is absent, Need R. |

<End of 1st Change>

<Start of 2nd Change>

11.2.2 Message definitions

[Unchanged parts omitted]

– *MeasurementTimingConfiguration*

The *MeasurementTimingConfiguration* message is used to convey assistance information for measurement timing.

Direction: en-gNB to eNB, eNB to en-gNB, gNB to gNB, ng-eNB to gNB, gNB to ng-eNB, ng-eNB to ng-eNB, gNB DU to gNB CU, and gNB CU to gNB DU.

***MeasurementTimingConfiguration* message**

-- ASN1START

-- TAG-MEASUREMENT-TIMING-CONFIGURATION-START

MeasurementTimingConfiguration ::= SEQUENCE {

 criticalExtensions CHOICE {

 c1 CHOICE{

 measTimingConf MeasurementTimingConfiguration-IEs,

 spare3 NULL, spare2 NULL, spare1 NULL

 },

 criticalExtensionsFuture SEQUENCE {}

 }

}

MeasurementTimingConfiguration-IEs ::= SEQUENCE {

 measTiming MeasTimingList OPTIONAL,

 nonCriticalExtension MeasurementTimingConfiguration-v1550-IEs OPTIONAL

}

MeasurementTimingConfiguration-v1550-IEs ::= SEQUENCE {

 campOnFirstSSB BOOLEAN,

 psCellOnlyOnFirstSSB BOOLEAN,

 nonCriticalExtension MeasurementTimingConfiguration-v1610-IEs OPTIONAL

}

MeasurementTimingConfiguration-v1610-IEs ::= SEQUENCE {

 csi-RS-Config-r16 SEQUENCE {

 csi-RS-SubcarrierSpacing-r16 SubcarrierSpacing,

 csi-RS-CellMobility-r16 CSI-RS-CellMobility,

 refSSBFreq-r16 ARFCN-ValueNR

 },

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

MeasTimingList ::= SEQUENCE (SIZE (1..maxMeasFreqsMN)) OF MeasTiming

MeasTiming ::= SEQUENCE {

 frequencyAndTiming SEQUENCE {

 carrierFreq ARFCN-ValueNR,

 ssbSubcarrierSpacing SubcarrierSpacing,

 ssb-MeasurementTimingConfiguration SSB-MTC,

 ss-RSSI-Measurement SS-RSSI-Measurement OPTIONAL

 } OPTIONAL,

 ...,

 [[

 ssb-ToMeasure SSB-ToMeasure OPTIONAL,

 physCellId PhysCellId OPTIONAL

 ]]

}

-- TAG-MEASUREMENT-TIMING-CONFIGURATION-STOP

-- ASN1STOP

|  |
| --- |
| ***MeasTiming* field descriptions** |
| ***carrierFreq, ssbSubcarrierSpacing***Indicates the frequency and subcarrier spacing of the SS block of the cell for which this message is included, or of other SS blocks within the same carrier. |
| ***ssb-MeasurementTimingConfiguration***Indicates the SMTC which can be used to search for SSB of the cell for which the message is included. When the message is included in "Served NR Cell Information" (see TS 36.423 [37]), "Served Cell Information NR" (see TS 38.423 [35]), or "Served Cell Information" (see TS 38.473 [36]), the timing is based on the cell for which the message is included. When the message is included in "NR Neighbour Information" (see TS 36.423 [37]), or "Served Cell Information" (see TS 38.423 [35]), the timing is based on the cell indicated in the "Served NR Cell Information" or "Served Cell Information NR" with which the "NR Neighbour Information" or "Neighbour Information NR" is provided. When the message is included in "CU to DU RRC Information", the timing is based on the cell indicated by SpCell ID with which the message is included. If the field is provided by an NTN cell, the offset (derived from parameter *periodicityAndOffset*) is based on the assumption that the feeder link propagation delay of the cell for which the message is included equals to 0 ms, and the receiving gNB can adjust the actual offset based on the actual feeder link propagation delay before configuring SMTC to the UE. |
| ***ss-RSSI-Measurement***Provides the configuration which can be used for RSSI measurements of the cell for which the message is included. |

|  |
| --- |
| ***MeasurementTimingConfiguration* field descriptions** |
| ***campOnFirstSSB***Value *true* indicates that the SSB indicated in the first instance of *MeasTiming* in the *measTiming* list can be used for camping and for a PCell configuration (i.e. in *spCellConfigCommon* of the *masterCellGroup*). |
| ***csi-RS-CellMobility***Indicates the CSI-RS configuration of the cell for which this message is included. The timing of the CSI-RS resources is based on the SSB indicated by *refSSBFreq*. |
| ***csi-RS-SubcarrierSpacing***Indicates the subcarrier spacing of the CSI-RS resources included in *csi-rs-CellMobility*. |
| ***measTiming***A list of SMTC information, SSB RSSI measurement information and associated NR frequency exchanged via EN-DC X2 Setup, EN-DC Configuration Update, Xn Setup and NG-RAN Node Configuration Update procedures, or F1 messages between gNB DU and gNB CU. |
| ***physCellId***Physical Cell Identity of the SSB on the ARFCN indicated by *carrierFreq*. |
| ***psCellOnlyOnFirstSSB***Value *true* indicates that only the SSB indicated in the first instance of *MeasTiming* in the *measTiming* list can be used for a PSCell configuration (i.e. in *spCellConfigCommon* of the *secondaryCellGroup*). |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). |

<End of 2nd Change>

# Appendix 3: TP-2 for SMTC and inter-node message

<Start of 1st Change>

6.3.1 System information blocks

– *SIB2*

*SIB2* contains cell re-selection information common for intra-frequency, inter-frequency and/or inter-RAT cell re-selection (i.e. applicable for more than one type of cell re-selection but not necessarily all) as well as intra-frequency cell re-selection information other than neighbouring cell related.

***SIB2* information element**

-- ASN1START

-- TAG-SIB2-START

SIB2 ::= SEQUENCE {

 cellReselectionInfoCommon SEQUENCE {

 nrofSS-BlocksToAverage INTEGER (2..maxNrofSS-BlocksToAverage) OPTIONAL, -- Need S

 absThreshSS-BlocksConsolidation ThresholdNR OPTIONAL, -- Need S

 rangeToBestCell RangeToBestCell OPTIONAL, -- Need R

 q-Hyst ENUMERATED {

 dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,

 dB12, dB14, dB16, dB18, dB20, dB22, dB24},

 speedStateReselectionPars SEQUENCE {

 mobilityStateParameters MobilityStateParameters,

 q-HystSF SEQUENCE {

 sf-Medium ENUMERATED {dB-6, dB-4, dB-2, dB0},

 sf-High ENUMERATED {dB-6, dB-4, dB-2, dB0}

 }

 } OPTIONAL, -- Need R

 ...

 },

 cellReselectionServingFreqInfo SEQUENCE {

 s-NonIntraSearchP ReselectionThreshold OPTIONAL, -- Need S

 s-NonIntraSearchQ ReselectionThresholdQ OPTIONAL, -- Need S

 threshServingLowP ReselectionThreshold,

 threshServingLowQ ReselectionThresholdQ OPTIONAL, -- Need R

 cellReselectionPriority CellReselectionPriority,

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL, -- Need R

 ...

 },

 intraFreqCellReselectionInfo SEQUENCE {

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 s-IntraSearchP ReselectionThreshold,

 s-IntraSearchQ ReselectionThresholdQ OPTIONAL, -- Need S

 t-ReselectionNR T-Reselection,

 frequencyBandList MultiFrequencyBandListNR-SIB OPTIONAL, -- Need S

 frequencyBandListSUL MultiFrequencyBandListNR-SIB OPTIONAL, -- Need R

 p-Max P-Max OPTIONAL, -- Need S

 smtc SSB-MTC OPTIONAL, -- Need S

 ss-RSSI-Measurement SS-RSSI-Measurement OPTIONAL, -- Need R

 ssb-ToMeasure SSB-ToMeasure OPTIONAL, -- Need S

 deriveSSB-IndexFromCell BOOLEAN,

 ...,

 [[

 t-ReselectionNR-SF SpeedStateScaleFactors OPTIONAL -- Need N

 ]],

 [[

 smtc2-LP-r16 SSB-MTC2-LP-r16 OPTIONAL, -- Need R

 ssb-PositionQCL-Common-r16 SSB-PositionQCL-Relation-r16 OPTIONAL -- Cond SharedSpectrum

 ]],

 [[

 ssb-PositionQCL-Common-r17 SSB-PositionQCL-Relation-r17 OPTIONAL -- Cond SharedSpectrum2

 ]],

 [[

 smtc4list-r17 SSB-MTC4List-r17 OPTIONAL -- Need R

 ]]

 },

 ...,

 [[

 relaxedMeasurement-r16 SEQUENCE {

 lowMobilityEvaluation-r16 SEQUENCE {

 s-SearchDeltaP-r16 ENUMERATED {

 dB3, dB6, dB9, dB12, dB15,

 spare3, spare2, spare1},

 t-SearchDeltaP-r16 ENUMERATED {

 s5, s10, s20, s30, s60, s120, s180,

 s240, s300, spare7, spare6, spare5,

 spare4, spare3, spare2, spare1}

 } OPTIONAL, -- Need R

 cellEdgeEvaluation-r16 SEQUENCE {

 s-SearchThresholdP-r16 ReselectionThreshold,

 s-SearchThresholdQ-r16 ReselectionThresholdQ OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 combineRelaxedMeasCondition-r16 ENUMERATED {true} OPTIONAL, -- Need R

 highPriorityMeasRelax-r16 ENUMERATED {true} OPTIONAL -- Need R

 } OPTIONAL -- Need R

 ]],

 [[

 cellEquivalentSize-r17 INTEGER(2..16) OPTIONAL, -- Cond HSDN

 relaxedMeasurement-r17 SEQUENCE {

 stationaryMobilityEvaluation-r17 SEQUENCE {

 s-SearchDeltaP-Stationary-r17 ENUMERATED {dB2, dB3, dB6, dB9, dB12, dB15, spare2, spare1},

 t-SearchDeltaP-Stationary-r17 ENUMERATED {s5, s10, s20, s30, s60, s120, s180, s240, s300, spare7, spare6, spare5,

 spare4, spare3, spare2, spare1}

 },

 cellEdgeEvaluationWhileStationary-r17 SEQUENCE {

 s-SearchThresholdP2-r17 ReselectionThreshold,

 s-SearchThresholdQ2-r17 ReselectionThresholdQ OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 combineRelaxedMeasCondition2-r17 ENUMERATED {true} OPTIONAL -- Need R

 } OPTIONAL -- Need R

 ]]

}

RangeToBestCell ::= Q-OffsetRange

-- TAG-SIB2-STOP

-- ASN1STOP

| ***SIB2* field descriptions** |
| --- |
| ***absThreshSS-BlocksConsolidation***Threshold for consolidation of L1 measurements per RS index. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***cellEdgeEvaluation***Indicates the criteria for a UE to detect that it is not at cell edge, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.2). |
| ***cellEdgeEvaluationWhileStationary***Indicates the criteria for a UE to detect that it is not at cell edge while stationary, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.4). |
| ***cellEquivalentSize***The number of cell count used for mobility state estimation for this cell as specified in TS 38.304 [20]. |
| ***cellReselectionInfoCommon***Cell re-selection information common for intra-frequency, inter-frequency and/ or inter-RAT cell re-selection. |
| ***cellReselectionServingFreqInfo***Information common for non-intra-frequency cell re-selection i.e. cell re-selection to inter-frequency and inter-RAT cells. |
| ***combineRelaxedMeasCondition***When both *lowMobilityEvalutation* and *cellEdgeEvalutation* criteria are present in SIB2, this parameter configures the UE to fulfil both criteria in order to relax measurement requirements for cell reselection. If the field is absent, the UE is allowed to relax measurement requirements for cell reselection when either or both of the criteria are met. (See TS 38.304 [20], clause 5.2.4.9.0) |
| ***combineRelaxedMeasCondition2***When both *stationaryMobilityEvaluation* and *cellEdgeEvaluationWhileStationary* criteria are present in SIB2, this parameter configures the UE to fulfil both criteria in order to relax measurement requirements for cell reselection. If the field is absent, the UE is allowed to relax measurement requirements for cell reselection when only the stationary criteria is met. (See TS 38.304 [20], clause 5.2.4.9.0) |
| ***deriveSSB-IndexFromCell***This field indicates whether the UE can utilize serving cell timing to derive the index of SS block transmitted by neighbour cell. If this field is set to *true*, the UE assumes SFN and frame boundary alignment across cells on the serving frequency as specified in TS 38.133 [14]. |
| ***frequencyBandList***Indicates the list of frequency bands for which the NR cell reselection parameters apply. The UE behaviour in case the field is absent is described in clause 5.2.2.4.3. |
| ***highPriorityMeasRelax***Indicates whether measurements can be relaxed on high priority frequencies. If the field is absent, the UE shall not relax measurements on high priority frequencies beyond "Thigher\_priority\_search" unless both low mobility and not at cell edge criteria are fulfilled (see TS 38.133 [14], clauses 4.2.2.7, 4.2.2.10 and 4.2.2.11). |
| ***intraFreqCellReselectionInfo***Cell re-selection information common for intra-frequency cells. |
| ***lowMobilityEvaluation***Indicates the criteria for a UE to detect low mobility, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.1). |
| ***nrofSS-BlocksToAverage***Number of SS blocks to average for cell measurement derivation. If the field is absent the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***p-Max***Value in dBm applicable for the intra-frequency neighbouring NR cells. If absent the UE applies the maximum power according to TS 38.101-1 [15] in case of an FR1 cell or TS 38.101-2 [39] in case of an FR2 cell. In this release of the specification, if *p-Max* is present on a carrier frequency in FR2, the UE shall ignore the field and applies the maximum power according to TS 38.101-2 [39]. This field is ignored by IAB-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [63]. |
| ***q-Hyst***Parameter "*Qhyst*" in TS 38.304 [20], Value in dB. Value *dB1* corresponds to 1 dB, *dB2* corresponds to 2 dB and so on. |
| ***q-HystSF***Parameter "Speed dependent ScalingFactor for Qhyst" in TS 38.304 [20]. The *sf-Medium* and *sf-High* concern the additional hysteresis to be applied, in Medium and High Mobility state respectively, to Qhyst as defined in TS 38.304 [20]. In dB. Value *dB-6* corresponds to -6dB, *dB-4* corresponds to -4dB and so on. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin.  |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. |
| ***rangeToBestCell***Parameter "rangeToBestCell" in TS 38.304 [20]. The network configures only non-negative (in dB) values. |
| ***relaxedMeasurement***Configuration to allow relaxation of RRM measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9). |
| ***s-IntraSearchP***Parameter "SIntraSearchP" in TS 38.304 [20]. |
| ***s-IntraSearchQ***Parameter "SIntraSearchQ" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of 0 dB for SIntraSearchQ. |
| ***s-NonIntraSearchP***Parameter "SnonIntraSearchP" in TS 38.304 [20]. If this field is absent, the UE applies the (default) value of infinity for SnonIntraSearchP. |
| ***s-NonIntraSearchQ***Parameter "SnonIntraSearchQ" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of 0 dB for SnonIntraSearchQ. |
| ***s-SearchDeltaP***Parameter "SSearchDeltaP" in TS 38.304 [20]. Value dB3 corresponds to 3 dB, dB6 corresponds to 6 dB and so on. |
| ***s-SearchDeltaP-Stationary***Parameter "SSearchDeltaP-Stationary" in TS 38.304 [20]. Value *dB2* corresponds to 2 dB, *dB3* corresponds to 3 dB and so on. |
| ***s-SearchThresholdP, s-SearchThresholdP2***Parameters "SSearchThresholdP" and "SSearchThresholdP2" in TS 38.304 [20]. The network configures *s-SearchThresholdP* and *s-SearchThresholdP2* to be less than or equal to *s-IntraSearchP* and *s-NonIntraSearchP*. |
| ***s-SearchThresholdQ, s-SearchThresholdQ2***Parameters "SSearchThresholdQ" and "SSearchThresholdQ2" in TS 38.304 [20]. The network configures *s-SearchThresholdQ* and *s-SearchThresholdQ2* to be less than or equal to *s-IntraSearchQ* and *s-NonIntraSearchQ*. |
| ***smtc***Measurement timing configuration for intra-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms for the intra-frequnecy cells. If the field is broadcast by an NTN cell, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that service link propagation delay differencebetween the serving cell and neighbour cells equals to 0 ms, and feeder link propagation delay difference between the serving cell and neighbour cells equals to 0 ms. The UE can adjust the actual *offset* based on the actual propagation delay difference. |
| ***smtc2-LP***Measurement timing configuration for intra-frequency neighbour cells with a Long Periodicity (LP) indicated by periodicity in *smtc2-LP*. The timing offset and duration are equal to the offset and duration indicated in *smtc* in *intraFreqCellReselectionInfo*. The periodicity in *smtc2-LP* can only be set to a value strictly larger than the periodicity in *smtc* in *intraFreqCellReselectionInfo* (e.g. if *smtc* indicates sf20 the Long Periodicity can only be set to sf40, sf80 or sf160, if *smtc* indicates sf160, *smtc2-LP* cannot be configured). The *pci-List*, if present, includes the physical cell identities of the intra-frequency neighbour cells with Long Periodicity. If *smtc2-LP* is absent, the UE assumes that there are no intra-frequency neighbour cells with a Long Periodicity. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and feeder link propagation delay difference between the serving cell and neighbour cells equals to 0 ms. The UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |
| ***ssb-PositionQCL-Common***Indicates the QCL relation between SS/PBCH blocks for intra-frequency neighbor cells as specified in TS 38.213 [13], clause 4.1. |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). When the field is absent the UE measures on all SS-blocks. |
| ***stationaryMobilityEvaluation***Indicates the criteria for a UE to detect stationary mobility, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.0). |
| ***t-ReselectionNR***Parameter "TreselectionNR" in TS 38.304 [20]. |
| ***t-ReselectionNR-SF***Parameter "Speed dependent ScalingFactor for TreselectionNR" in TS 38.304 [20]. If the field is absent, the UE behaviour is specified in TS 38.304 [20]. |
| ***threshServingLowP***Parameter "ThreshServing, LowP" in TS 38.304 [20]. |
| ***threshServingLowQ***Parameter "ThreshServing, LowQ" in TS 38.304 [20]. |
| ***t-SearchDeltaP***Parameter "TSearchDeltaP" in TS 38.304 [20]. Value in seconds. Value *s5* means 5 seconds, value *s10* means 10 seconds and so on. |
| ***t-SearchDeltaP-Stationary***Parameter "TSearchDeltaP-Stationary" in TS 38.304 [20]. Value in seconds. Value *s5* means 5 seconds, value *s10* means 10 seconds and so on. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *HSDN* | The field is optionally present, Need R, if *speedStateReselectionPars* is present; otherwise the field is not present. |
| *SharedSpectrum* | This field is mandatory present if this intra-frequency operates with shared spectrum channel access in FR1. Otherwise, it is absent, Need R. |
| *SharedSpectrum2* | This field is optionally present if this intra-frequency operates with shared spectrum channel access in FR2-2, Need R. Otherwise, it is absent, Need R. |

[Unchanged parts omitted]

– *SIB4*

*SIB4* contains information relevant for inter-frequency cell re-selection (i.e. information about other NR frequencies and inter-frequency neighbouring cells relevant for cell re-selection), which can also be used for NR idle/inactive measurements. The IE includes cell re-selection parameters common for a frequency as well as cell specific re-selection parameters.

***SIB4* information element**

-- ASN1START

-- TAG-SIB4-START

SIB4 ::= SEQUENCE {

 interFreqCarrierFreqList InterFreqCarrierFreqList,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 ...,

 [[

 interFreqCarrierFreqList-v1610 InterFreqCarrierFreqList-v1610 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1700 InterFreqCarrierFreqList-v1700 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1720 InterFreqCarrierFreqList-v1720 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1730 InterFreqCarrierFreqList-v1730 OPTIONAL -- Need R

 ]]

}

InterFreqCarrierFreqList ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo

InterFreqCarrierFreqList-v1610 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1610

InterFreqCarrierFreqList-v1700 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1700

InterFreqCarrierFreqList-v1720 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1720

InterFreqCarrierFreqList-v1730 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1730

InterFreqCarrierFreqInfo ::= SEQUENCE {

 dl-CarrierFreq ARFCN-ValueNR,

 frequencyBandList MultiFrequencyBandListNR-SIB OPTIONAL, -- Cond Mandatory

 frequencyBandListSUL MultiFrequencyBandListNR-SIB OPTIONAL, -- Need R

 nrofSS-BlocksToAverage INTEGER (2..maxNrofSS-BlocksToAverage) OPTIONAL, -- Need S

 absThreshSS-BlocksConsolidation ThresholdNR OPTIONAL, -- Need S

 smtc SSB-MTC OPTIONAL, -- Need S

 ssbSubcarrierSpacing SubcarrierSpacing,

 ssb-ToMeasure SSB-ToMeasure OPTIONAL, -- Need S

 deriveSSB-IndexFromCell BOOLEAN,

 ss-RSSI-Measurement SS-RSSI-Measurement OPTIONAL, -- Need R

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 p-Max P-Max OPTIONAL, -- Need S

 t-ReselectionNR T-Reselection,

 t-ReselectionNR-SF SpeedStateScaleFactors OPTIONAL, -- Need S

 threshX-HighP ReselectionThreshold,

 threshX-LowP ReselectionThreshold,

 threshX-Q SEQUENCE {

 threshX-HighQ ReselectionThresholdQ,

 threshX-LowQ ReselectionThresholdQ

 } OPTIONAL, -- Cond RSRQ

 cellReselectionPriority CellReselectionPriority OPTIONAL, -- Need R

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL, -- Need R

 q-OffsetFreq Q-OffsetRange DEFAULT dB0,

 interFreqNeighCellList InterFreqNeighCellList OPTIONAL, -- Need R

 interFreqExcludedCellList InterFreqExcludedCellList OPTIONAL, -- Need R

 ...

}

InterFreqCarrierFreqInfo-v1610 ::= SEQUENCE {

 interFreqNeighCellList-v1610 InterFreqNeighCellList-v1610 OPTIONAL, -- Need R

 smtc2-LP-r16 SSB-MTC2-LP-r16 OPTIONAL, -- Need R

 interFreqAllowedCellList-r16 InterFreqAllowedCellList-r16 OPTIONAL, -- Cond SharedSpectrum2

 ssb-PositionQCL-Common-r16 SSB-PositionQCL-Relation-r16 OPTIONAL, -- Cond SharedSpectrum

 interFreqCAG-CellList-r16 SEQUENCE (SIZE (1..maxPLMN)) OF InterFreqCAG-CellListPerPLMN-r16 OPTIONAL -- Need R

}

InterFreqCarrierFreqInfo-v1700 ::= SEQUENCE {

 interFreqNeighHSDN-CellList-r17 InterFreqNeighHSDN-CellList-r17 OPTIONAL, -- Need R

 highSpeedMeasInterFreq-r17 ENUMERATED {true} OPTIONAL, -- Need R

 redCapAccessAllowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 ssb-PositionQCL-Common-r17 SSB-PositionQCL-Relation-r17 OPTIONAL, -- Cond SharedSpectrum

 interFreqNeighCellList-v1710 InterFreqNeighCellList-v1710 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqCarrierFreqInfo-v1720 ::= SEQUENCE {

 smtc4list-r17 SSB-MTC4List-r17 OPTIONAL -- Need R

}

InterFreqCarrierFreqInfo-v1730 ::= SEQUENCE {

 channelAccessMode2-r17 ENUMERATED {enabled} OPTIONAL -- Need R

}

InterFreqNeighHSDN-CellList-r17 ::= SEQUENCE (SIZE (1..maxCellInter)) OF PCI-Range

InterFreqNeighCellList ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo

InterFreqNeighCellList-v1610 ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo-v1610

InterFreqNeighCellList-v1710 ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo-v1710

InterFreqNeighCellInfo ::= SEQUENCE {

 physCellId PhysCellId,

 q-OffsetCell Q-OffsetRange,

 q-RxLevMinOffsetCell INTEGER (1..8) OPTIONAL, -- Need R

 q-RxLevMinOffsetCellSUL INTEGER (1..8) OPTIONAL, -- Need R

 q-QualMinOffsetCell INTEGER (1..8) OPTIONAL, -- Need R

 ...

}

InterFreqNeighCellInfo-v1610 ::= SEQUENCE {

 ssb-PositionQCL-r16 SSB-PositionQCL-Relation-r16 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqNeighCellInfo-v1710 ::= SEQUENCE {

 ssb-PositionQCL-r17 SSB-PositionQCL-Relation-r17 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqExcludedCellList ::= SEQUENCE (SIZE (1..maxCellExcluded)) OF PCI-Range

InterFreqAllowedCellList-r16 ::= SEQUENCE (SIZE (1..maxCellAllowed)) OF PCI-Range

InterFreqCAG-CellListPerPLMN-r16 ::= SEQUENCE {

 plmn-IdentityIndex-r16 INTEGER (1..maxPLMN),

 cag-CellList-r16 SEQUENCE (SIZE (1..maxCAG-Cell-r16)) OF PCI-Range

}

-- TAG-SIB4-STOP

-- ASN1STOP

| ***SIB4* field descriptions** |
| --- |
| ***absThreshSS-BlocksConsolidation***Threshold for consolidation of L1 measurements per RS index. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***channelAccessMode2***If present, this field indicates that the neighbor cells on the inter-frequency apply channel access mode procedures for operation with shared spectrum channel access in accordance with TS 37.213 [48], clause 4.4 for FR2-2. If absent, the neighbor cells on the inter-frequency do not apply any channel access procedure. |
| ***deriveSSB-IndexFromCell***This field indicates whether the UE may use the timing of any detected cell on that frequency to derive the SSB index of all neighbour cells on that frequency. If this field is set to *true*, the UE assumes SFN and frame boundary alignment across cells on the neighbor frequency as specified in TS 38.133 [14]. |
| ***dl-CarrierFreq***This field indicates center frequency of the SS block of the neighbour cells, where the frequency corresponds to a GSCN value as specified in TS 38.101-1 [15]. |
| ***frequencyBandList***Indicates the list of frequency bands for which the NR cell reselection parameters apply. |
| ***highSpeedMeasInterFreq***If the field is set to *true* and UE supports high speed inter-frequency IDLE/INACTIVE measurements, the UE shall apply the enhanced inter-frequency RRM requirements on the inter-frequency carrier to support high speed up to 500 km/h in RRC\_IDLE/RRC\_INACTIVE as specified in TS 38.133 [14]. |
| ***interFreqAllowedCellList***List of allow-listed inter-frequency neighbouring cells, see TS 38.304 [20], clause 5.2.4. |
| ***interFreqCAG-CellList***List of inter-frequency neighbouring CAG cells (as defined in TS 38.304 [20] per PLMN. |
| ***interFreqCarrierFreqList***List of neighbouring carrier frequencies and frequency specific cell re-selection information. If *interFreqCarrierFreqList-v1610, interFreqCarrierFreqList-v1700, interFreqCarrierFreqList-v1720* or *interFreqCarrierFreqList-v1730* are present, they shall contain the same number of entries, listed in the same order as in *interFreqCarrierFreqList* (without suffix). |
| ***interFreqExcludedCellList***List of exclude-listed inter-frequency neighbouring cells. |
| ***interFreqNeighCellList***List of inter-frequency neighbouring cells with specific cell re-selection parameters. If *interFreqNeighCellList-v1610* is present, it shall contain the same number of entries, listed in the same order as in *interFreqNeighCellList* (without suffix). |
| ***interFreqNeighHSDN-CellList***List of inter-frequency neighbouring HSDN cells as specified in TS 38.304 [20]. |
| ***nrofSS-BlocksToAverage***Number of SS blocks to average for cell measurement derivation. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***p-Max***Value in dBm applicable for the neighbouring NR cells on this carrier frequency. If absent the UE applies the maximum power according to TS 38.101-1 [15] in case of an FR1 cell or TS 38.101-2 [39] in case of an FR2 cell. In this release of the specification, if *p-Max* is present on a carrier frequency in FR2, the UE shall ignore the field and applies the maximum power according to TS 38.101-2 [39]. This field is ignored by IAB-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [63]. |
| ***q-OffsetCell***Parameter "Qoffsets,n" in TS 38.304 [20]. |
| ***q-OffsetFreq***Parameter "Qoffsetfrequency" in TS 38.304 [20]. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin. |
| ***q-QualMinOffsetCell***Parameter "Qqualminoffsetcell" in TS 38.304 [20]. Actual value Qqualminoffsetcell = field value [dB]. |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20]. |
| ***q-RxLevMinOffsetCell***Parameter "Qrxlevminoffsetcell" in TS 38.304 [20]. Actual value Qrxlevminoffsetcell = field value \* 2 [dB]. |
| ***q-RxLevMinOffsetCellSUL***Parameter "QrxlevminoffsetcellSUL" in TS 38.304 [20]. Actual value QrxlevminoffsetcellSUL = field value \* 2 [dB]. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20]. |
| ***redCapAccessAllowed***Indicates whether RedCap UEs are allowed to access the frequency. |
| ***smtc***Measurement timing configuration for intra-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms for the intra-frequnecy cells. If the field is broadcast by an NTN cell, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that service link propagation delay differencebetween the serving cell and neighbour cells equals to 0 ms, and feeder link propagation delay difference between the serving cell and neighbour cells equals to 0 ms. The UE can adjust the actual *offset* based on the actual propagation delay difference. |
| ***smtc2-LP***Measurement timing configuration for inter-frequency neighbour cells with a Long Periodicity (LP) indicated by periodicity in *smtc2-LP*. The timing offset and duration are equal to the offset and duration indicated in *smtc* in *InterFreqCarrierFreqInfo*. The periodicity in *smtc2-LP* can only be set to a value strictly larger than the periodicity in *smtc* in *InterFreqCarrierFreqInfo* (e.g. if *smtc* indicates sf20 the Long Periodicity can only be set to sf40, sf80 or sf160, if *smtc* indicates sf160, *smtc2-LP* cannot be configured). The *pci-List*, if present, includes the physical cell identities of the inter-frequency neighbour cells with Long Periodicity. If *smtc2-LP* is absent, the UE assumes that there are no inter-frequency neighbour cells with a Long Periodicity. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that service link propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and feeder link propagation delay difference between the serving cell and neighbour cells equals to 0 ms. The UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |
| ***ssb-PositionQCL***Indicates the QCL relation between SS/PBCH blocks for a specific neighbor cell as specified in TS 38.213 [13], clause 4.1. If provided, the cell specific value overwrites the common value signalled by *ssb-PositionQCL-Common* in *SIB4* for the indicated cell. |
| ***ssb-PositionQCL-Common***Indicates the QCL relation between SS/PBCH blocks for inter-frequency neighbor cells as specified in TS 38.213 [13], clause 4.1. |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). When the field is absent the UE measures on all SS-blocks. |
| ***ssbSubcarrierSpacing***Subcarrier spacing of SSB.Only the following values are applicable depending on the used frequency:FR1: 15 or 30 kHzFR2-1: 120 or 240 kHzFR2-2: 120, 480, or 960 kHz |
| ***threshX-HighP***Parameter "ThreshX, HighP" in TS 38.304 [20]. |
| ***threshX-HighQ***Parameter "ThreshX, HighQ" in TS 38.304 [20]. |
| ***threshX-LowP***Parameter "ThreshX, LowP" in TS 38.304 [20]. |
| ***threshX-LowQ***Parameter "ThreshX, LowQ" in TS 38.304 [20]. |
| ***t-ReselectionNR***Parameter "TreselectionNR" in TS 38.304 [20]. |
| ***t-ReselectionNR-SF***Parameter "Speed dependent ScalingFactor for TreselectionNR" in TS 38.304 [20]. If the field is absent, the UE behaviour is specified in TS 38.304 [20]. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *Mandatory* | The field is mandatory present in SIB4. |
| *RSRQ* | The field is mandatory present if *threshServingLowQ* is present in *SIB2*; otherwise it is absent. |
| *SharedSpectrum* | This field is mandatory present if this inter-frequency operates with shared spectrum channel access. Otherwise, it is absent, Need R. |
| *SharedSpectrum2* | The field is optional present, Need R, if this inter-frequency or neighbor cell operates with shared spectrum channel access. Otherwise, it is absent, Need R. |

<End of 1st Change>

<Start of 2nd Change>

11.2.2 Message definitions

[Unchanged parts omitted]

– *MeasurementTimingConfiguration*

The *MeasurementTimingConfiguration* message is used to convey assistance information for measurement timing.

Direction: en-gNB to eNB, eNB to en-gNB, gNB to gNB, ng-eNB to gNB, gNB to ng-eNB, ng-eNB to ng-eNB, gNB DU to gNB CU, and gNB CU to gNB DU.

***MeasurementTimingConfiguration* message**

-- ASN1START

-- TAG-MEASUREMENT-TIMING-CONFIGURATION-START

MeasurementTimingConfiguration ::= SEQUENCE {

 criticalExtensions CHOICE {

 c1 CHOICE{

 measTimingConf MeasurementTimingConfiguration-IEs,

 spare3 NULL, spare2 NULL, spare1 NULL

 },

 criticalExtensionsFuture SEQUENCE {}

 }

}

MeasurementTimingConfiguration-IEs ::= SEQUENCE {

 measTiming MeasTimingList OPTIONAL,

 nonCriticalExtension MeasurementTimingConfiguration-v1550-IEs OPTIONAL

}

MeasurementTimingConfiguration-v1550-IEs ::= SEQUENCE {

 campOnFirstSSB BOOLEAN,

 psCellOnlyOnFirstSSB BOOLEAN,

 nonCriticalExtension MeasurementTimingConfiguration-v1610-IEs OPTIONAL

}

MeasurementTimingConfiguration-v1610-IEs ::= SEQUENCE {

 csi-RS-Config-r16 SEQUENCE {

 csi-RS-SubcarrierSpacing-r16 SubcarrierSpacing,

 csi-RS-CellMobility-r16 CSI-RS-CellMobility,

 refSSBFreq-r16 ARFCN-ValueNR

 },

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

MeasTimingList ::= SEQUENCE (SIZE (1..maxMeasFreqsMN)) OF MeasTiming

MeasTiming ::= SEQUENCE {

 frequencyAndTiming SEQUENCE {

 carrierFreq ARFCN-ValueNR,

 ssbSubcarrierSpacing SubcarrierSpacing,

 ssb-MeasurementTimingConfiguration SSB-MTC,

 ss-RSSI-Measurement SS-RSSI-Measurement OPTIONAL

 } OPTIONAL,

 ...,

 [[

 ssb-ToMeasure SSB-ToMeasure OPTIONAL,

 physCellId PhysCellId OPTIONAL

 ]]

}

-- TAG-MEASUREMENT-TIMING-CONFIGURATION-STOP

-- ASN1STOP

|  |
| --- |
| ***MeasTiming* field descriptions** |
| ***carrierFreq, ssbSubcarrierSpacing***Indicates the frequency and subcarrier spacing of the SS block of the cell for which this message is included, or of other SS blocks within the same carrier. |
| ***ssb-MeasurementTimingConfiguration***Indicates the SMTC which can be used to search for SSB of the cell for which the message is included. When the message is included in "Served NR Cell Information" (see TS 36.423 [37]), "Served Cell Information NR" (see TS 38.423 [35]), or "Served Cell Information" (see TS 38.473 [36]), the timing is based on the cell for which the message is included. When the message is included in "NR Neighbour Information" (see TS 36.423 [37]), or "Served Cell Information" (see TS 38.423 [35]), the timing is based on the cell indicated in the "Served NR Cell Information" or "Served Cell Information NR" with which the "NR Neighbour Information" or "Neighbour Information NR" is provided. When the message is included in "CU to DU RRC Information", the timing is based on the cell indicated by SpCell ID with which the message is included. If the field is provided by an NTN cell, the offset (derived from parameter *periodicityAndOffset*) is based on the assumption that the propagation delay of the cell for which the message is included equals to 0 ms, and the receiving gNB can adjust the actual offset before configuring SMTC to the UE. |
| ***ss-RSSI-Measurement***Provides the configuration which can be used for RSSI measurements of the cell for which the message is included. |

|  |
| --- |
| ***MeasurementTimingConfiguration* field descriptions** |
| ***campOnFirstSSB***Value *true* indicates that the SSB indicated in the first instance of *MeasTiming* in the *measTiming* list can be used for camping and for a PCell configuration (i.e. in *spCellConfigCommon* of the *masterCellGroup*). |
| ***csi-RS-CellMobility***Indicates the CSI-RS configuration of the cell for which this message is included. The timing of the CSI-RS resources is based on the SSB indicated by *refSSBFreq*. |
| ***csi-RS-SubcarrierSpacing***Indicates the subcarrier spacing of the CSI-RS resources included in *csi-rs-CellMobility*. |
| ***measTiming***A list of SMTC information, SSB RSSI measurement information and associated NR frequency exchanged via EN-DC X2 Setup, EN-DC Configuration Update, Xn Setup and NG-RAN Node Configuration Update procedures, or F1 messages between gNB DU and gNB CU. |
| ***physCellId***Physical Cell Identity of the SSB on the ARFCN indicated by *carrierFreq*. |
| ***psCellOnlyOnFirstSSB***Value *true* indicates that only the SSB indicated in the first instance of *MeasTiming* in the *measTiming* list can be used for a PSCell configuration (i.e. in *spCellConfigCommon* of the *secondaryCellGroup*). |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). |

<End of 2nd Change>