**3GPP TSG RAN2 #121 R2-23xxxxx**

**Athens, Greece, 27th Feb – 3rd Mar, 2023**

**Agenda Item:**  **8.14.5 Other topics**

**Source: Huawei (email rapporteur)**

**Title:** **Report of [AT121][201][QoE] Continuity of QoE measurements during intra-5GC inter-RAT HO (Huawei)**

**Document for: Discussion and Decision**

# 1 Introduction

This is the email report of [AT121][201]:

* [AT121][201][QoE] Continuity of QoE measurements during intra-5GC inter-RAT HO (Huawei)

 Scope: Discuss the possible options and identify their impacts to specifications and WGs. Should identify which options have LTE impact (and therefore are not in the current scope of the WI). If possible try to downselect which options could be feasible for this WI.

 Intended outcome: Report in [R2-2302005](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_121/Docs/R2-2302005.zip).

 Deadline: Friday morning (before morning coffee break)

Companies providing input to this email discussion are requested to leave contact information below.

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email Address** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 2 Discussion

## 2.1 List of options

Based on the relevant contributions and online discussions, at least the following options are provided. Companies can add other options if possible.

**Option 1:** (NR -> LTE/5GC -> NR) Source NR node sends RRC message to UE to pause the NR QoE. Later, when the UE goes back to NR, the NR can indicate the UE to continue the previous NR QoE reporting.

**Option 2:** (LTE/5GC -> NR -> LTE/5GC) Source LTE/5GC node sends RRC message to UE to pause the LTE QoE, which has some impacts to TS 36.331. Later, when the UE goes back to LTE/5GC, the LTE/5GC can indicate the UE to continue the previous LTE QoE reporting.

**Option 3:** (NR -> LTE/5GC) When the UE goes to LTE/5GC from NR, one previous QoE measurement can be activated in LTE/5GC (while others can be paused or released), and the QoE measurement and reporting will continue in LTE/5GC.

**Option 4:** (LTE/5GC -> NR) When the UE goes to NR from LTE/5GC, the previous QoE measurement can be continued in NR. During the inter-RAT HO, the target RAT can also configure other QoE measurements to the UE.

**Option 5:** The network can release the QoE configuration before moving UE to LTE/5GC and then reconfigure once UE moves back to NR.

[Other options…]

## 2.2 Discussion on Option 1

For option 1, the technical analysis in [2] are used here.

|  |  |  |  |
| --- | --- | --- | --- |
| **Principle** | **LTE impacts** | **Other RAN2 impacts** | **RAN3 impacts** |
| Source NR node sends RRC message to UE to pause the NR QoE. Later, when the UE goes back to NR, the NR can indicate the UE to continue the previous NR QoE reporting. | TS 36.331: no impacts | TS 38.331: impacts to inter-RAT HO command and QoE configurations storingTS 38.300: stage-2 description | TS 38.423: check whether existing QoE config in HANDOVER REQUEST procedure can cover LTE QoE config or not |

**Q1: For option 1, do companies agree on analysis on principle and specification impacts (including LTE impacts)? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

For the scope of this email discussion, it mentions “If possible try to downselect which options could be feasible for this WI.”, so it is suggested to collect companies’ preferences.

**Q2: Do companies support to select Option 1 for this WI? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.3 Discussion on Option 2

For option 2, the technical analysis in [2] are used here.

|  |  |  |  |
| --- | --- | --- | --- |
| **Principle** | **LTE impacts** | **Other RAN2 impacts** | **RAN3 impacts** |
| Source LTE/5GC node sends RRC message to UE to pause the LTE QoE, which has some impacts to TS 36.331. Later, when the UE goes back to LTE/5GC, the LTE/5GC can indicate the UE to continue the previous LTE QoE reporting. | TS 36.331: impacts due to the introduction of pause/resume mechanism | TS 38.331: no impactsTS 38.300: stage-2 description | TS 38.423: check whether existing QoE config in HANDOVER REQUEST procedure can cover LTE QoE config or not |

**Q3: For option 2, do companies agree on analysis on principle and specification impacts (including LTE impacts)? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q4: Do companies support to select Option 2 for this WI? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.4 Discussion on Option 3

For option 3, the technical analysis in [2] are used here.

|  |  |  |  |
| --- | --- | --- | --- |
| **Principle** | **LTE impacts** | **Other RAN2 impacts** | **RAN3 impacts** |
| When the UE goes to LTE/5GC from NR, one previous QoE measurement can be activated in LTE/5GC (while others can be paused or released), and the QoE measurement and reporting will continue in LTE/5GC. | TS 36.331: impacts related to configuration of the QoE measurements from NR | TS 38.331: impacts to inter-RAT HO commandTS 38.300: stage-2 description | TS 38.423: NR or LTE/5GC can decide which of QoE measurements can be continued and inform NR, which has impacts to Xn. In addition, whether existing QoE config in HANDOVER REQUEST procedure can cover LTE QoE config or not can be checked. |

**Q5: For option 3, do companies agree on analysis on principle and specification impacts (including LTE impacts)? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q6: Do companies support to select Option 3 for this WI? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.5 Discussion on Option 4

For option 1, the technical analysis in [2] are used here.

|  |  |  |  |
| --- | --- | --- | --- |
| **Principle** | **LTE impacts** | **Other RAN2 impacts** | **RAN3 impacts** |
| When the UE goes to NR from LTE/5GC, the previous QoE measurement can be continued in NR. During the inter-RAT HO, the target RAT can also configure other QoE measurements to the UE. | TS 36.331: impacts to inter-RAT HO command | TS 38.331: some impacts related to ensuring continuation of QoE measurement from LTE when the UE moves to NRTS 38.300: stage-2 description | TS 38.423: check whether existing QoE config in HANDOVER REQUEST procedure can cover LTE QoE config or not |

**Q7: For option 4, do companies agree on analysis on principle and specification impacts (including LTE impacts)? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q8: Do companies support to select Option 4 for this WI? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.6 Discussion on Option 5

For option 1, the technical analysis in [2] are used here.

|  |  |  |  |
| --- | --- | --- | --- |
| **Principle** | **LTE impacts** | **Other RAN2 impacts** | **RAN3 impacts** |
| The network can release the QoE configuration before moving UE to LTE/5GC and then reconfigure once UE moves back to NR. | TS 36.331: no impacts | TS 38.331: no impactsTS 38.300: may be no impacts | May be no impacts |

**Q9: For option 5, do companies agree on analysis on principle and specification impacts (including LTE impacts)? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q10: Do companies support to select Option 5 for this WI? Please provide your comments in the comment column if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.7 Discussion on Option XX

[to be added if necessary]

# 3 Conclusion

[To be added]

# 4 References

[1] RAN2-121 LTE MUSIM QoE XR (Tero)\_2023-02-28-1845

[2] R2-2300356 Discussion on Rel-18 other QoE enhancement ZTE Corporation, Sanechips

[3] R2-2300603 QoE continuity between LTE-5GC and NR Huawei, HiSilicon

[4] R2-2300631 Discussion on QoE measurement during intra-5GC inter-RAT handover Lenovo

[5] R2-2300722 QoE Continuity During Intra-5GC Inter-RAT Handover Apple

[6] R2-2301339 QoE measurements at IRAT handover Ericsson

[7] R2-2301641 Discussion on QoE measurement continuity during inter-RAT handover Samsung

[8] R2-2301665 On QoE continuity during inter-RAT handover Nokia, Nokia Shanghai Bell

[9] R2-2301756 Discussion on the QoE continuity during intra-5GC inter-RAT HO China Unicom

[10] R2-2301803 Discussion on the continuity of QoE measurement CATT