**3GPP TSG-RAN WG3 Meeting #115-eR3-222921**

**Feb. 21st ~Mar. 3rd 2022**

**Online**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.423** | **CR** | **0532** | **rev** | **10** | **Current version:** | **16.8.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | BL CR to XnAP on Rel-17 eIAB | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung，Nokia, Nokia Shanghai Bell, Verizon, Qualcomm Incorporated, CATT, ZTE, Fujitsu, AT&T, KDDI, Lenovo, Motorola Mobility, LG Electronics | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_IAB\_enh-Core | | | | |  | | ***Date:*** | | 2022-03-04 |
|  |  | | | |  | | |  | |  |
| ***Category:*** | **B** |  | | | | | | ***Release:*** | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Support Rel-17 eIAB | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * **RAN3#115-e**   **Capture agreed TP R3-222855, R3-222882, R3-222860, R3-222749**   * **RAN3#114bis-e**   **Capture agreed TP R3-221233**   * **RAN3#114e**   **Capture agreements as below:**  **The F1-terminating donor of the boundary node forwards the boundary IAB node’s resource configuration information to the non-F1-terminating donor, via following XnAP procedures:**  **- retrieve UE context procedure,**  **- handover preparation procedure,**  **- SN addition procedure,**  **- MN initiated SN modification procedure.**  **- SN initiated SN modification procedure**  **Following information are exchanged over Xn interface via the procedures in Proposal 1-1**   * + - * **Activated cell list.**       * **H/S/NA resource configurations.**       * **DL/UL resource configurations.**       * **Multiplexing info.**       * **Cell specific signal/channel configurations, including at least: SSB information, CORESET 0, and RACH configurations) from/for different parent nodes.**       * **other higher layer parameters listed in R1-2110573** * **RAN3#111e**   To enable F1-C transfer, a new XnAP procedure, i.e., F1-C Traffic Transfer, is added. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Cannot support Rel-17 eIAB | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.1; 8.2.1.2; 8.2.4.2; 8.3.1.2; 8.3.3.2; 8.3.4.2; 8.x(new); 9.1.1.1; 9.1.1.9; 9.1.2.1; 9.1.2.5; 9.1.2.8; 9.1.x(new);9.2.1.13; 9.2.2.x~x13; 9.3.3; 9.3.4; 9.3.5; 9.3.7 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | |  | | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | TS/TR ... CR ... | | | |
| ***affected:*** | |  | **x** | Test specifications | | | TS/TR ... CR ... | | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | TS/TR ... CR ... | | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |

|  |  |
| --- | --- |
| ***This CR's revision history:*** | Rev#1:   * Add “**Editor Note: FFS on potential revision to this procedure due to, e.g., RAN2 progress, etc**” in section 8.x.1.1.   Rev#2:   * Change the Editor Note to “**Editor Note: FFS on potential revision to this procedure due to, e.g., RAN2 progress regarding simultaneous connectivity to two donors, etc.**”   Rev#3:   * Remove Ericsson as co-signer   Rev#4 (pre-RAN3#112e)   * Update cover page * Re-base on TS38.423v16.5.0 * Incoporate R3-211327 agreed in RAN3#111e   Rev#5 (pre-RAN3#113e)   * Re-base on TS38.423 v16.6.0   Rev#6 (pre-RAN3#114e)  Re-base on TS38.423 v16.7.0  Rev#7(Post-RAN3#114e)   * Incorporate R3-216142 agreed in RAN3#114e * Change ProtocolIE-ID of id-Activated-Cells-List and id-IAB-MT-Cell-List to ‘xxx’   Rev#8 (Pre-RAN3#114bis-e)   * Rebase v16.8.0   Rev#9 (Post-RAN3#114bis-e and submit to RAN3#115-e)   * Incoporate R3-221233 agreed in RAN3#114bis-e * Add ASN.1 related to R3-221233 * Add missed presence for some IEs * Delete presence of the *Activated Cells List* IE * Editorial changes:   + Change first letter of each word in each IE to captial   + Delete "NRCellIdentity ::= BIT STRING (SIZE(36))"   + Change nRCellIdentity NRCellIdentity --> NR-Cell-Identity   Rev#10 (Post-RAN3#115-e)   * Incorporate R3-222855, R3-222882, R3-222860, R3-222749 * Remove editor’s note * Add definition of F1-terminating donor and non-F1-terminating donor * Re-ordering the sections * IAB TRANSPORT MIGRATION MANAGEMENT RESPONSE message   + Add criticality   + Swap “F1-Terminating donor UE XnAP ID” and “Non-F1-Terminating donor UE XnAP ID” in the tabular to align with ASN.1   + remove definition of maxnoofBHInfo * IAB TRANSPORT MIGRATION MODIFICATION RESPONSE message   + Add criticality   + Remove definition for maxnoofBHInfo   + Add 1..< *maxnoofTrafficIndexEntries* > in IAB TRANSPORT MIGRATION MODIFICATION RESPONSE message * Update definition of maxnoofBHInfo to “Maximum no. of BH information corresponding to one Traffic Index assigned to the traffic offloaded to the non-F1-terminating IAB-donor-CU.” to align it with that under 9.2.2.x3 Non-F1-terminating Topology BH Information * Traffic to Be Release Information * Remove definition of maxnoofBHInfo * Slot Index : INTEGER (0.. *maxnoofHSNASlots-1*) 🡪 INTEGER (1.. *maxnoofHSNASlots*) * RB set Index: INTEGER (0.. *maxnoofRBsetsPerCell-1*) 🡪 INTEGER (1.. *maxnoofRBsetsPerCell*) * Resolve FFS on ” maxnoofPhysicalResourceBlocks”, and give its value as 275 * ASN.1 clean-up |

-------------------------------------------Change 1-------------------------------------------

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**CAG Cell**: As defined in TS 38.300 [9].

**Conditional Handover**: As defined in TS 38.300 [9].

**Conditional PSCell Change**: As defined in TS 37.340 [8].

**DAPS Handover**: As defined in TS 38.300 [9].

**Elementary Procedure:** XnAP protocol consists of Elementary Procedures (EPs). An XnAP Elementary Procedure is a unit of interaction between two NG-RAN nodes. An EP consists of an initiating message and possibly a response message. Two kinds of EPs are used:

- **Class 1**: Elementary Procedures with response (success or failure),

- **Class 2**: Elementary Procedures without response.

**Immediate Handover**: Used in the context of Conditional Handover, to refer to a handover that is executed immediately after the UE receives the Handover Command.

**NG-RAN node**: as defined in TS 38.300 [9].

**Non-CAG Cell**: As defined in TS 38.300 [9].

**PDU Session Resource:** As defined in TS 38.401 [2].

**PDU session split:** as defined in TS 37.340 [8].

**Public Network Integrated NPN:** as defined in TS 23.501 [7].

**Stand-alone Non-Public Network:** as defined in TS 23.501 [7].

**F1-terminating IAB-donor**: as defined in TS38.401[2].

**Non-F1-terminating IAB-donor**: as defined in TS38.401[2].

-------------------------------------------Change 1-------------------------------------------

## 8.1 Elementary procedures

In the following tables, all EPs are divided into Class 1 and Class 2 EPs.

-----------------------------------------------------<unchanged part is omitted>-----------------------------------------------------

Table 8.1-1: Class 1 Elementary Procedures

| Elementary Procedure | Initiating Message | Successful Outcome | Unsuccessful Outcome | |
| --- | --- | --- | --- | --- |
| Response message | Response message | |
| Handover Preparation | HANDOVER REQUEST | HANDOVER REQUEST ACKNOWLEDGE | HANDOVER PREPARATION FAILURE |
| Retrieve UE Context | RETRIEVE UE CONTEXT REQUEST | RETRIEVE UE CONTEXT RESPONSE | RETRIEVE UE CONTEXT FAILURE |
| S-NG-RAN node Addition Preparation | S-NODE ADDITION REQUEST | S-NODE ADDITION REQUEST ACKNOWLEDGE | S-NODE ADDITION REQUEST REJECT |
| M-NG-RAN node initiated S-NG-RAN node Modification Preparation | S-NODE MODIFICATION REQUEST | S-NODE MODIFICATION REQUEST ACKNOWLEDGE | S-NODE MODIFICATION REQUEST REJECT |
| S-NG-RAN node initiated S-NG-RAN node Modification | S-NODE MODIFICATION REQUIRED | S-NODE MODIFICATION CONFIRM | S-NODE MODIFICATION REFUSE |
| S-NG-RAN node initiated S-NG-RAN node CHANGE | S-NODE CHANGE REQUIRED | S-NODE CHANGE CONFIRM | S-NODE CHANGE REFUSE |
| M-NG-RAN node initiated S-NG-RAN node Release | S-NODE RELEASE REQUEST | S-NODE RELEASE REQUEST ACKNOWLEDGE | S-NODE RELEASE REJECT |
| S-NG-RAN node initiated S-NG-RAN node Release | S-NODE RELEASE REQUIRED | S-NODE RELEASE CONFIRM |  |
| Xn Setup | XN SETUP REQUEST | XN SETUP RESPONSE | XN SETUP FAILURE |
| NG-RAN node Configuration Update | NG-RAN NODE CONFIGURATION UPDATE | NG-RAN NODE CONFIGURATION UPDATE ACKNOWLEDGE | NG-RAN NODE CONFIGURATION UPDATE FAILURE |
| Cell Activation | CELL ACTIVATION REQUEST | CELL ACTIVATION RESPONSE | CELL ACTIVATION FAILURE |
| Reset | RESET REQUEST | RESET RESPONSE |  |
| Xn Removal | Xn REMOVAL REQUEST | Xn REMOVAL RESPONSE | Xn REMOVAL FAILURE |
| E-UTRA - NR Cell Resource Coordination | E-UTRA - NR CELL RESOURCE COORDINATION REQUEST | E-UTRA - NR CELL RESOURCE COORDINATION RESPONSE |  |
| Resource Status Reporting Initiation | RESOURCE STATUS REQUEST | RESOURCE STATUS RESPONSE | RESOURCE STATUS FAILURE |
| Mobility Settings Change | MOBILITY CHANGE REQUEST | MOBILITY CHANGE ACKNOWLEDGE | MOBILITY CHANGE FAILURE |
| IAB Transport Migration Management | IAB TRANSPORT MIGRATION MANAGEMENT REQUEST | IAB TRANSPORT MIGRATION MANAGEMENT RESPONSE |  |
| IAB RESOURCE COORDINATION | IAB RESOURCE COORDINATION REQUEST | IAB RESOURCE COORDINATION RESPONSE |  |

Table 8.1-2: Class 2 Elementary Procedures

| Elementary Procedure | Initiating Message |
| --- | --- |
| Handover Cancel | HANDOVER CANCEL |
| SN Status Transfer | SN STATUS TRANSFER |
| RAN Paging | RAN PAGING |
| Xn-U Address Indication | XN-U ADDRESS INDICATION |
| S-NG-RAN node Reconfiguration Completion | S-NODE RECONFIGURATION COMPLETE |
| S-NG-RAN node Counter Check | S-NODE COUNTER CHECK REQUEST |
| UE Context Release | UE CONTEXT RELEASE |
| RRC Transfer | RRC TRANSFER |
| Error Indication | ERROR INDICATION |
| Notification Control Indication | NOTIFICATION CONTROL INDICATION |
| Activity Notification | ACTIVITY NOTIFICATION |
| Secondary RAT Data Usage Report | SECONDARY RAT DATA USAGE REPORT |
| Trace Start | TRACE START |
| Deactivate Trace | DEACTIVATE TRACE |
| Handover Success | HANDOVER SUCCESS |
| Conditional Handover Cancel | CONDITIONAL HANDOVER CANCEL |
| Early Status Transfer | EARLY STATUS TRANSFER |
| Failure Indication | FAILURE INDICATION |
| Handover Report | HANDOVER REPORT |
| Resource Status Reporting | RESOURCE STATUS UPDATE |
| Access And Mobility Indication | ACCESS AND MOBILITY INDICATION |
| F1-C Traffic Transfer | F1-C TRAFFIC TRANSFER |

-------------------------------------------Next Change-------------------------------------------

### 8.2.1 Handover Preparation

#### 8.2.1.1 General

This procedure is used to establish necessary resources in an NG-RAN node for an incoming handover. If the procedure concerns a conditional handover, parallel transactions are allowed. Possible parallel requests are identified by the target cell ID when the source UE AP IDs are the same.

The procedure uses UE-associated signalling.

#### 8.2.1.2 Successful Operation



Figure 8.2.1.2-1: Handover Preparation, successful operation

The source NG-RAN node initiates the procedure by sending the HANDOVER REQUEST message to the target NG-RAN node. When the source NG-RAN node sends the HANDOVER REQUEST message, it shall start the timer TXnRELOCprep.

----------------------------------------------<unchanged part is omitted>-----------------------------------------------

If the *IAB Node Indication* IE is contained in the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, consider that the handover is for an IAB node. In addition:

* If the *No PDU Session Indication* IE is contained in the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, consider the UE as an IAB-node which does not have any PDU sessions activated, and ignore the *PDU Session Resources To Be Setup List* IE, and shall not take any action with respect to PDU session setup. Subsequently, the source NG-RAN node shall, if supported, ignore the *PDU Session Resources Admitted To Be Added List* IE in the HANDOVER REQUEST ACKNOWLEDGE message.

If the *UE Radio Capability ID* IE is contained in the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 23.501 [7] and TS 23.502 [13].

-------------------------------------------Next change-------------------------------------------

### 8.2.4 Retrieve UE Context

#### 8.2.4.1 General

The purpose of the Retrieve UE Context procedure is to either retrieve the UE context from the old NG-RAN node and transfer it to the NG-RAN node where the UE RRC Connection has been requested to be established, or to enable the old NG-RAN node to forward an RRC message to the UE via the new NG-RAN node without context transfer.

The procedure uses UE-associated signalling.

#### 8.2.4.2 Successful Operation



Figure 8.2.4.2-1: Retrieve UE Context, successful operation

The new NG-RAN node initiates the procedure by sending the RETRIEVE UE CONTEXT REQUEST message to the old NG-RAN node.

----------------------------------------------<unchanged part is omitted>-----------------------------------------------

If the *UE Radio Capability ID* IE is contained in the RETRIEVE UE CONTEXT RESPONSE message, the new NG- RAN node shall, if supported store this information in the UE context and use it as defined in TS 23.501 [7] and TS 23.502 [13].

If the *IAB Node Indication* IE is contained in the RETRIEVE UE CONTEXT RESPONSE message, the new NG-RAN node shall, if supported, consider that the procedure is performed for an IAB-node. In addition:

* If the *No PDU Session Indication* IE is contained in the *UE Context Information – Retrieve UE Context Response* IE of the RETRIEVE UE CONTEXT RESPONSE message, the new NG-RAN node shall, if supported, consider the UE as an IAB-node which does not have any PDU sessions activated, and ignore the *PDU Session Resources To Be Setup List* IE in the *UE Context Information – Retrieve UE Context Response* IE, and shall not take any action with respect to PDU session setup.

-------------------------------------------Next change-------------------------------------------

### 8.3.1 S-NG-RAN node Addition Preparation

#### 8.3.1.1 General

The purpose of the S-NG-RAN node Addition Preparation procedure is to request the S-NG-RAN node to allocate resources for dual connectivity operation for a specific UE.

The procedure uses UE-associated signalling.

#### 8.3.1.2 Successful Operation



Figure 8.3.1.2-1: S-NG-RAN node Addition Preparation, successful operation

The M-NG-RAN node initiates the procedure by sending the S-NODE ADDITION REQUEST message to the S-NG-RAN node.

----------------------------------------------<unchanged part is omitted>-----------------------------------------------

For each DRB configured as MN-terminated split bearer/SCG bearer, if the *QoS Mapping Information* IE is included in the *DRBs Admitted List* IE in the *PDU Session Resource Setup Response Info – MN terminated* IE of the S-NODE ADDITION REQUEST ACKNOWLEDGE message, the M-NG-RAN node shall, if supported, use it to set DSCP and/or flow label fields for the downlink IP packets which are transmitted from M-NG-RAN node to S-NG-RAN node through the GTP tunnels indicated by the *UP Transport Layer Information* IE.

If the *IAB Node Indication* IE is contained in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall, if supported, consider the dual connectivity is for an IAB-node. In addition:

* If the *No PDU Session Indication* IE is contained in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall, if supported, consider the UE as an IAB-node which does not have any PDU sessions activated, and ignore the *PDU Session Resources To Be Added List* IE, and shall not take any action with respect to PDU session setup. Subsequently, the M-NG-RAN node shall, if supported, ignore the *PDU Session Resources Admitted To Be Added List* IE in the S-NODE ADDITION REQUEST ACKNOWLEDGE message.

-------------------------------------------Next change-------------------------------------------

### 8.3.3 M-NG-RAN node initiated S-NG-RAN node Modification Preparation

#### 8.3.3.1 General

This procedure is used to enable an M-NG-RAN node to request an S-NG-RAN node to either modify the UE context at the S-NG-RAN node or to query the current SCG configuration for supporting delta signalling in M-NG-RAN node initiated S-NG-RAN node change, or to provide the S-RLF-related information to the S-NG-RAN node.

The procedure uses UE-associated signalling.

#### 8.3.3.2 Successful Operation



Figure 8.3.3.2-1: M-NG-RAN node initiated S-NG-RAN node Modification Preparation, successful operation

The M-NG-RAN node initiates the procedure by sending the S-NODE MODIFICATION REQUEST message to the S-NG-RAN node.

----------------------------------------------<unchanged part is omitted>-----------------------------------------------

For each DRB configured as SN-terminated split bearer/MCG bearer, if the *QoS Mapping Information* IE is included in the *DRBs To Be Modified List* IE in the *PDU Session Resource Modification Info – SN terminated* IE of the S-NODE MODIFICATION REQUEST message, the S-NG-RAN node shall, if supported, use it to set DSCP and/or flow label fields for the downlink IP packets which are transmitted from S-NG-RAN node to M-NG-RAN node through the GTP tunnels indicated by the *UP Transport Layer Information* IE.

-------------------------------------------Next change-------------------------------------------

### 8.3.4 S-NG-RAN node initiated S-NG-RAN node Modification

#### 8.3.4.1 General

This procedure is used by the S-NG-RAN node to modify the UE context in the S-NG-RAN node.

The procedure uses UE-associated signalling.

#### 8.3.4.2 Successful Operation



Figure 8.3.4.2-1: S-NG-RAN node initiated S-NG-RAN node Modification, successful operation.

The S-NG-RAN node initiates the procedure by sending the S-NODE MODIFICATION REQUIRED message to the M-NG-RAN node.

----------------------------------------------<unchanged part is omitted>-----------------------------------------------

For each DRB configured as MN-terminated split bearer/SCG bearer, if the *QoS Mapping Information* IE is included in the *DRBs To Be Modified List* IE in the *PDU Session Resource Modification Required Info – MN terminated* IE of the S-NODE MODIFICATION REQUIRED message, the M-NG-RAN node shall, if supported, use it to set DSCP and/or flow label fields for the downlink IP packets which are transmitted from M-NG-RAN node to S-NG-RAN node through the GTP tunnels indicated by the *UP Transport Layer Information* IE.

For each DRB configured as SN-terminated split bearer/MCG bearer, if the *QoS Mapping Information* IE is included in the *DRBs Admitted to be Setup or Modified List* IE in the *PDU Session Resource Modification Confirm Info – SN terminated* IE of the S-NODE MODIFICATION CONFIRM message, the S-NG-RAN node shall, if supported, use it to set DSCP and/or flow label fields for the downlink IP packets which are transmitted from S-NG-RAN node to M-NG-RAN node through the GTP tunnels indicated by the *UP Transport Layer Information* IE.

-------------------------------------------Next Change-------------------------------------------

## 8.x IAB Procedures

### 8.x.1 F1-C Traffic Transfer

#### 8.x.1.1 General

The purpose of the F1-C Traffic Transfer procedure is to deliver F1-C traffic between the M-NG-RAN node and the S-NG-RAN node serving a dual-connected IAB-node, where the F1-C traffic is either received from the IAB-node or sent to the IAB-node.

The procedure uses UE-associated signalling. This procedure is only applicable to IAB-nodes.

#### 8.x.1.2 Successful Operation



Figure 8.x.1.2-1: F1-C Traffic Transfer procedure, successful operation.

Either the M-NG-RAN Node initiates the procedure by sending the F1-C TRAFFIC TRANSFER message to the S-NG-RAN Node, or the S-NG-RAN Node initiates the procedure by sending the F1-C TRAFFIC TRANSFER message to the M-NG-RAN Node.

Upon reception of the F1-C TRAFFIC TRANSFER message, the receiving node, not being the IAB-donor of the IAB-node, shall deliver the contained F1-C traffic to the IAB-node. Alternatively, the receiving node, being the IAB-donor of the IAB-node, shall handle the received F1-C traffic as specified in TS38.473[41].

#### 8.x.1.3 Unsuccessful Operation

Not applicable.

#### 8.x.1.4 Abnormal Conditions

Not Applicable.

### 8.x.2 IAB Transport Migration Management

#### 8.x.2.1 General

The purpose of the IAB Transport Migration Management procedure is to exchange information between the F1-terminating IAB-donor-CU and the non-F1-terminating IAB-donor-CU of a boundary IAB-node, for the purpose of managing the migration of the boundary and descendant IAB-node traffic between the topologies managed by the two IAB-donor-CUs.

The procedure is applicable to inter-donor partial migration, inter-donor RLF recovery and inter-donor topology redundancy cases. The procedure is initiated by the F1-terminating IAB-donor-CU of the boundary IAB-node. The procedure can be used to set up, modify and release (e.g., for the purpose of revoking) the resources under the non-F1-terminating IAB-donor-CU used for serving the offloaded traffic. The procedure uses UE-associated signalling.

#### 8.x.2.2 Successful Operation



Figure 8.x.2.2-1: IAB Transport Migration Management triggered by the F1-terminating donor, successful operation

The F1-terminating donor initiates the procedure by sending the IAB TRANSPORT MIGRATION MANAGEMENT REQUEST message to the non-F1-terminating IAB-donor.

The non-F1-terminating donor may respond with the IAB TRANSPORT MIGRATION MANAGEMENT RESPONSE message by indicating:

- Traffic accepted for offloading, within the *Traffic Added Item* IE;

- Already offloaded traffic accepted for modification , within the *Traffic Modified Item* IE;

- Traffic not accepted for offloading within the *Traffic Not Added List* IE;

- Already offloaded traffic not accepted for modification within the *Traffic Not Modified List* IE.

If the *Traffic to Be Released Information* IE is contained in the IAB TRANSPORT MIGRATION MANAGEMENTREQUEST message, the non-F1-terminating donor should release all offloaded traffic if the *All Traffic Indication* IE in the *Traffic to Be Released Information* IE is set to “true”, or release only the offloaded traffic indicated by the *Traffic to Be Released Item* IE in the *Traffic to Be Released Information* IE.

If the IAB TRANSPORT MIGRATION MANAGEMENT REQUEST message contains the *Traffic to Be Released Information* IE, the non-F1-terminating donor shall include the *Traffic Released List* IE in the IAB TRANSPORT MIGRATION MANAGEMENT RESPONSE message.

If the *IAB TNL Address Request* IE is contained in the IAB TRANSPORT MIGRATION MANAGEMENT REQUEST message, the non-F1-terminating donor should provide the allocated TNL address via the *IAB TNL Address Response* IE in the IAB TRANSPORT MIGRATION MANAGEMENT RESPONSE message.

If the *IAB TNL Address Exception* IE is contained in the IAB TRANSPORT MIGRATION MANAGEMENT REQUEST message, the non-F1-terminating donor shall, if supported, configure the related IAB-donor-DU to enable traffic transfer over the inter-donor-DU tunnel.

#### 8.x.2.3 Unsuccessful Operation

Not applicable.

#### 8.x.2.4 Abnormal Conditions

Not applicable.

8.x.3 IAB Transport Migration Modification

#### 8.x.3.1 General

The purpose of the IAB Transport Migration Modification procedure is to modify the backhaul information of the offloaded traffic in the topology of the non-F1-terminating IAB-donor of a boundary IAB-node. The procedure can also be used to release the resources under the non-F1-terminating IAB-donor-CU used for serving the offloaded traffic.

The procedure is applicable to inter-donor partial migration, inter-donor RLF recovery and inter-donor topology redundancy cases. The procedure is initiated by the non-F1-terminating IAB-donor-CU of the boundary IAB-node.

The procedure uses UE-associated signalling.

#### 8.x.3.2 Successful Operation



**Figure 8.x.3.2-1: IAB Transport Migration Modification, successful operation**

The Non-F1-terminating donor initiates the procedure by sending the IAB TRANSPORT MIGRATION MODIFICATION REQUEST message to the F1-terminating IAB-donor. The F1-terminating IAB-donor responds with the IAB TRANSPORT MIGRATION MODIFICATION RESPONSE message, by indicating already offloaded traffic accepted for modification, within the *Traffic Required Modified List* IE.

If the *Traffic Required To Be Modified List* IE is contained in the IAB TRANSPORT MIGRATION MODIFICATION REQUEST message, the F1-terminating donor shall update the backhaul information in non-F1-terminating topology for each traffic indicated in the list.

If the *Traffic to Be Released Information* IE is contained in the IAB TRANSPORT MIGRATION MODIFICATION REQUEST message, the F1-terminating donor shall consider all offloaded traffic will be released by the non-F1-terminating donor if the *All Traffic Indication* IE in the *Traffic to Be Released Information* IE is set to “true”, or only the traffic indicated by the *Traffic to Be Released Item* IE will be released by the non-F1-terminating donor.

If the IAB TRANSPORT MIGRATION MODIFICATION REQUEST message contains the *Traffic to Be Released Information* IE, the F1-terminating donor shall include the *Traffic Released List* IE in the IAB TRANSPORT MIGRATION MODIFICATION RESPONSE message.

If the *IAB TNL Address To Be Added* IE is contained in the IAB TRANSPORT MIGRATION MODIFICATION REQUEST message, the F1-terminating donor shall allocate the TNL address(es) contained in this IE to the boundary IAB node or the descendant IAB-nodes.

If the *IAB TNL Address To Be Released* IE is contained in the IAB TRANSPORT MIGRATION MODIFICATION REQUEST message, the F1-terminating donor shall release the TNL address(es) contained in this IE for the boundary IAB-node or descendant IAB-node.

8.x.3.3 Unsuccessful Operation

Not applicable.

8.x.3.4 Abnormal Conditions

Not applicable.

8.x.4 IAB RESOURCE COORDINATION

8.x.4.1 General

The purpose of the IAB Resource Coordination procedure is to exchange the semi-static radio resource configuration pertaining to a boundary IAB-node, between the F1-terminating IAB-donor-CU and the non-F1-terminating IAB-donor-CU of a boundary IAB-node, for the purpose of resource multiplexing. The procedure can be initiated by the F1-terminating or non F1-terminating IAB-donor-CU of the boundary IAB-node.

The procedure uses UE-associated signalling.

8.x.4.2 Successful Operation

****

**Figure 8.x.4.2-1: IAB Resource Coordination triggered by the F1-terminating/non-F1-terminating donor, successful operation**

The F1-terminating/non F1-terminating IAB-donor-CU initiates the procedure by sending the IAB RESOURCE COORDINATION REQUEST message to the non-F1-terminating/F1-terminating IAB-donor-CU. The non-F1-terminating/F1-terminating IAB-donor-CU may respond with the IAB RESOURCE COORDINATION RESPONSE message to the F1-terminating/non-F1-terminating IAB-donor-CU.

If the *Boundary-Node Cells List* IE and/or *Parent-Node Cells List* IE is included in the IAB RESOURCE COORDINATION REQUEST or IAB RESOURCE COORDINATION RESPONSE message, the receiving F1-terminating/non F1-terminating IAB-donor-CU should take this information into account for resource coordination with the sending F1-terminating/non F1-terminating IAB-donor-CU.

8.x.4.3 Unsuccessful Operation

Not applicable.

8.x.4.4 Abnormal Conditions

Not applicable.

-------------------------------------------Next Change-------------------------------------------

9.1.1 Messages for Basic Mobility Procedures

9.1.1.1 HANDOVER REQUEST

This message is sent by the source NG-RAN node to the target NG-RAN node to request the preparation of resources for a handover.

Direction: source NG-RAN node → target NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| Source NG-RAN node UE XnAP ID reference | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | Allocated at the source NG-RAN node | YES | reject |
| Cause | M |  | 9.2.3.2 |  | YES | reject |
| Target Cell Global ID | M |  | 9.2.3.25 | Includes either an E-UTRA CGI or an NR CGI | YES | reject |
| GUAMI | M |  | 9.2.3.24 |  | YES | reject |
| <unchanged part is omitted> | | | | | | |
| LTE V2X Services Authorized | O |  | 9.2.3.106 |  | YES | ignore |
| PC5 QoS Parameters | O |  | 9.2.3.109 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| Mobility Information | O |  | BIT STRING (SIZE (32)) | Information related to the handover; the source NG-RAN node provides it in order to enable later analysis of the conditions that led to a wrong HO. | YES | ignore |
| UE History Information from the UE | O |  | 9.2.3.110 |  | YES | ignore |
| IAB Node Indication | O |  | ENUMERATED (true, ...) |  | YES | reject |
| No PDU Session Indication | O |  | ENUMERATED (true, ...) | Applicable to IAB only. | YES | ignore |

|  |  |
| --- | --- |
| **Condition** | **Explanation** |
| ifCHOmod | This IE shall be present if the *CHO Trigger* IE is present and set to "CHO-replace". |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofMDTPLMNs | PLMNs in the Management Based MDT PLMN list. Value is 16. |

------------------------------------------Next change -------------------------------------------

9.1.1.9 RETRIEVE UE CONTEXT RESPONSE

This message is sent by the old NG-RAN node to transfer the UE context to the new NG-RAN node.

Direction: old NG-RAN node → new NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| New NG-RAN node UE XnAP ID reference | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | Allocated at the new NG-RAN node | YES | ignore |
| Old NG-RAN node UE XnAP ID reference | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | Allocated at the old NG-RAN node | YES | ignore |
| GUAMI | M |  | 9.2.3.24 |  | YES | reject |
| UE Context Information – Retrieve UE Context Response | M |  | 9.2.1.13 |  | YES | reject |
| Trace Activation | O |  | 9.2.3.55 |  | YES | ignore |
| Masked IMEISV | O |  | 9.2.3.32 |  | YES | ignore |
| Location Reporting Information | O |  | 9.2.3.47 | Includes the necessary parameters for location reporting. | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.3.3 |  | YES | ignore |
| NR V2X Services Authorized | O |  | 9.2.3.105 |  | YES | ignore |
| LTE V2X Services Authorized | O |  | 9.2.3.106 |  | YES | ignore |
| PC5 QoS Parameters | O |  | 9.2.3.109 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| UE History Information | O |  | 9.2.3.64 |  | YES | ignore |
| UE History Information from the UE | O |  | 9.2.3.110 |  | YES | ignore |
| ManagementBasedMDT PLMN List | O |  | MDT PLMN List  9.2.3.133 |  | YES | ignore |
| IAB Node Indication | O |  | ENUMERATED (true, ...) |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofMDTPLMNs | PLMNs in the Management Based MDT PLMN list. Value is 16. |

-------------------------------------------Next change-------------------------------------------

9.1.2 Messages for Dual Connectivity Procedures

9.1.2.1 S-NODE ADDITION REQUEST

This message is sent by the M-NG-RAN node to the S-NG-RAN node to request the preparation of resources for dual connectivity operation for a specific UE.

Direction: M-NG-RAN node → S-NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| M-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | Allocated at the M-NG-RAN node | YES | reject |
| UE Security Capabilities | M |  | 9.2.3.49 |  | YES | reject |
| S-NG-RAN node Security Key | M |  | 9.2.3.51 |  | YES | reject |
| S-NG-RAN node UE Aggregate Maximum Bit Rate | M |  | UE Aggregate Maximum Bit Rate  9.2.3.17 | The UE Aggregate Maximum Bit Rate is split into M-NG-RAN node UE Aggregate Maximum Bit Rate and S-NG-RAN node UE Aggregate Maximum Bit Rate which are enforced by M-NG-RAN node and S-NG-RAN node respectively. | YES | reject |
| Selected PLMN | O |  | PLMN Identity  9.2.2.4 | The selected PLMN of the SCG in the S-NG-RAN node. | YES | ignore |
| Mobility Restriction List | O |  | 9.2.3.53 |  | YES | ignore |
| Index to RAT/Frequency Selection Priority | O |  | 9.2.3.23 |  | YES | reject |
| <unchanged part is omitted> | | | | | | |
| UE Radio Capability ID | O |  | 9.2.3.138 |  | YES | reject |
| IAB Node Indication | O |  | ENUMERATED (true, ...) |  | YES | ignore |
| No PDU Session Indication | O |  | ENUMERATED (true, ...) | Applicable for IAB only. | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofPDUSessions | Maximum no. of PDU sessions. Value is 256 |

|  |  |
| --- | --- |
| **Condition** | **Explanation** |
| ifSNterminated | This IE shall be present if there is at least one *PDU Session Resource Setup Info – SN terminated* in the *PDU Session Resources To Be Added List* IE. |

-------------------------------------------Next change-------------------------------------------

9.1.2.5 S-NODE MODIFICATION REQUEST

This message is sent by the M-NG-RAN node to the S-NG-RAN node to either request the preparation to modify S-NG-RAN node resources for a specific UE, or to query for the current SCG configuration, or to provide the S-RLF-related information to the S-NG-RAN node.

Direction: M-NG-RAN node → S-NG-RAN node.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.2.3.1 |  | | YES | reject |
| M-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | Allocated at the M-NG-RAN node | | YES | reject |
| S-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID  9.2.3.16 | Allocated at the S-NG-RAN node | | YES | reject |
| Cause | M |  | 9.2.3.2 |  | | YES | ignore |
| PDCP Change Indication | O |  | 9.2.3.74 |  | | YES | ignore |
| Selected PLMN | O |  | PLMN Identity  9.2.2.4 | The selected PLMN of the SCG in the S-NG-RAN node. | | YES | ignore |
| Mobility Restriction List | O |  | 9.2.3.53 |  | | YES | ignore |
| SCG Configuration Query | O |  | 9.2.3.27 |  | | YES | ignore |
| <unchanged part is omitted> | | | | | | | |
| SN triggered | O |  | ENUMERATED (TRUE ...) | |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofPDUSessions | Maximum no. of PDU sessions. Value is 256 |

-------------------------------------------Next change-------------------------------------------

9.1.2.8 S-NODE MODIFICATION REQUIRED

This message is sent by the S-NG-RAN node to the M-NG-RAN node to request the modification of S-NG-RAN node resources for a specific UE.

Direction: S-NG-RAN node → M-NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| M-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID  9.2.3.16 | Allocated at the M-NG-RAN node | YES | reject |
| S-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID  9.2.3.16 | Allocated at the S-NG-RAN node | YES | reject |
| Cause | M |  | 9.2.3.2 |  | YES | ignore |
| PDCP Change Indication | O |  | 9.2.3.74 |  | YES | ignore |
| <unchanged part is omitted> | | | | | | |
| SCG Indicator | O |  | ENUMERATED(released,...) |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofPDUSessions | Maximum no. of PDU sessions. Value is 256 |

-------------------------------------------Next change-------------------------------------------

### 9.1.x Messages for IAB Procedures

#### 9.1.x.1 F1-C TRAFFIC TRANSFER

This message is sent by the M-NG-RAN node to the S-NG-RAN node or by the S-NG-RAN node to the M-NG-RAN node of a dual-connected IAB-node to transfer the F1-C traffic to and from the IAB-node.

Direction: M-NG-RAN node → S-NG-RAN node or S-NG-RAN node → M-NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| M-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID  9.2.3.16 | Allocated at the M-NG-RAN node | YES | reject |
| S-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID  9.2.3.16 | Allocated at the S-NG-RAN node | YES | reject |
| F1-C Traffic Container | M |  | OCTET STRING | Contains an F1-C interface SCTP CHUNK and IP header, or an IP packet to protect the traffic on the F1-C interface as defined in TS 33.501 [28]. | YES | reject |

#### 9.1.x.2 IAB TRANSPORT MIGRATION MANAGEMENT REQUEST

This message is sent by a F1-terminating IAB-donor-CU to a non-F1-terminating IAB-donor-CU of a boundary IAB-node, for the purpose of setting up, modifying, or releasing (e.g., for the purpose of revoking) the configuration for the migration of boundary and descendant node traffic between two IAB-donor-CUs.

Direction: F1-terminating donor CU → non-F1-terminating donor CU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| F1-Terminating donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID  9.2.3.16 | This IE refers to the Source NG-RAN node UE  XnAP ID reference or to the M-NG-RAN node UE XnAP  ID, or to the S-NG-RAN node UE XnAP  ID. | YES | reject |
| Non-F1-Terminating donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID  9.2.3.16 | This IE refers to the Target NG-RAN node UE  XnAP ID reference or to the S-NG-RAN node UE XnAP  ID, or to the M-NG-RAN node UE XnAP  ID. | YES | reject |
| **Traffic To Be Added List** |  | *0..1* |  |  | YES | reject |
| >**Traffic To Be Added Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>Traffic Profile | M |  | 9.2.2.x1 |  | – |  |
| >>F1-terminating Topology BH Information | O |  | 9.2.2.x2 |  | – |  |
| **Traffic To Be Modified List** |  | *0..1* |  |  | YES | reject |
| >**Traffic To Be Modified Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>Traffic Profile | O |  | 9.2.2.x1 |  | – |  |
| >>F1-terminating Topology BH Information | O |  | 9.2.2.x2 |  | – |  |
| Traffic To Be Released Information | O |  | 9.2.2.x4 |  | YES | reject |
| IAB TNL Address Request | O |  | 9.2.2.x5 |  | YES | reject |
| IAB TNL Address Exception | O |  | 9.2.2.x18 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTrafficIndexEntries | Maximum no. of traffic offloaded to the non-F1-terminating IAB-donor-CU. The value is 1024. |

#### 9.1.x.3 IAB TRANSPORT MIGRATION MANAGEMENT RESPONSE

This message is sent by the non-F1-terminating IAB-donor-CU to the F1-terminating IAB-donor-CU of a boundary IAB-node to provide inter-donor transport related configurations for the offloaded traffic.

Direction: non-F1-terminating donor CU → F1-terminating donor CU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| F1-Terminating Donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Source NG-RAN node UE  XnAP ID reference or to the M-NG-RAN node UE XnAP  ID, or to the S-NG-RAN node UE XnAP  ID. | YES | reject |
| Non-F1-Terminating Donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Target NG-RAN node UE  XnAP ID reference or to the S-NG-RAN node UE XnAP  ID, or to the M-NG-RAN node UE XnAP  ID. | YES | reject |
| **Traffic Added List** |  | *0..1* |  |  | YES | reject |
| >**Traffic Added Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>Non-F1-terminating Topology BH Information | M |  | 9.2.2.x3 |  | – |  |
| **Traffic Modified List** |  | *0..1* |  |  | YES | reject |
| >**Traffic Modified Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>Non-F1-terminating Topology BH Information | M |  | 9.2.2.x3 |  | – |  |
| **Traffic Not Added List** |  | *0..1* |  |  | YES | reject |
| >**Traffic Not Added Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>Cause | O |  | 9.2.2.2 |  | – |  |
| **Traffic Not Modified List** |  | *0..1* |  |  | YES | reject |
| >**Traffic Not Modified Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>Cause | O |  | 9.2.3.2 |  | – |  |
| IAB TNL Address Response | O |  | 9.2.2.x6 |  | YES | reject |
| **Traffic Released List** |  | *0..1* |  |  | YES | reject |
| >**Traffic Released Item** |  |  |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>BH Info List | O |  | 9.2.2.x19 |  | – |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTrafficIndexEntries | Maximum no. of traffic offloaded to the non-F1-terminating IAB-donor-CU. The value is 1024. |

#### 9.1.x.4 IAB TRANSPORT MIGRATION MODIFICATION REQUEST

This message is sent by a non-F1-terminating IAB-donor-CU to a F1-terminating IAB-donor-CU of a boundary IAB-node, for the purpose of modifying or releasing the configuration for the migrated traffic of boundary IAB-node or descendant IAB-node.

Direction: non-F1-terminating donor CU → F1-terminating donor CU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| F1-Terminating donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID  9.2.3.16 | This IE refers to the Source NG-RAN node UE  XnAP ID reference or to the M-NG-RAN node UE XnAP  ID, or to the S-NG-RAN node UE XnAP  ID. | YES | reject |
| Non-F1-Terminating donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Target NG-RAN node UE  XnAP ID reference or to the S-NG-RAN node UE XnAP  ID, or to the M-NG-RAN node UE XnAP  ID. | YES | reject |
| **Traffic Required To Be Modified List** |  | *0..1* |  |  | YES | reject |
| >**Traffic Required To Be Modified Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>Non-F1-terminating topology BH information | O |  | 9.2.2.x3 |  | – |  |
| Traffic To Be Released Information | O |  | 9.2.2.x4 |  | YES | reject |
| IAB TNL Address To Be Added | O |  | 9.2.2.x6 |  | YES | reject |
| **IAB TNL Address To Be Released List** |  | *0..1* |  |  | YES | reject |
| **>IAB TNL Address To Be Released Item** |  | *1*..<*maxnoofTLAsIAB*> |  |  | – |  |
| >>IAB TNL Address | M |  | 9.2.2.x12 |  | – |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTrafficIndexEntries | Maximum no. of traffic offloaded to the non-F1-terminating IAB-donor-CU. The value is 1024. |
| maxnoofTLAsIAB | Maximum no. of IPv6 addresses or IPv6 address prefixes and/or individual IPv4 addresses that can be allocated in one procedure execution. The value is 1024. |

#### 9.1.x.5 IAB TRANSPORT MIGRATION MODIFICATION RESPONSE

This message is sent by the F1-terminating IAB-donor-CU to the non-F1-terminating IAB-donor-CU of a boundary IAB-node to acknowledge update of configuration provided by the non-F1-terminating IAB-donor-CU.

Direction: F1-terminating donor CU → non-F1-terminating donor CU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| F1-Terminating donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Source NG-RAN node UE  XnAP ID reference or to the M-NG-RAN node UE XnAP  ID, or to the S-NG-RAN node UE XnAP  ID. | YES | Reject |
| Non-F1-Terminating donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Target NG-RAN node UE  XnAP ID reference or to the S-NG-RAN node UE XnAP  ID, or to the M-NG-RAN node UE XnAP  ID. | YES | reject |
| **Traffic Required Modified List** |  | *0..1* |  |  | YES | reject |
| >**Traffic Required Modified Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| **Traffic Released List IE** |  | *0..1* |  |  | YES | reject |
| **>Traffic Released Item** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  | – |  |
| >>Traffic Index | M |  | 9.2.2.x0 |  | – |  |
| >>BH Info List | O |  | 9.2.2.x19 |  | – |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTrafficIndexEntries | Maximum no. of traffic offloaded to the non-F1-terminating IAB-donor-CU. The value is 1024. |

9.1.x.6 IAB RESOURCE COORDINATION REQUEST

This message is sent by a F1-terminating/non F1-terminating IAB-donor-CU to a non-F1-terminating/F1-terminating IAB-donor-CU of a boundary IAB-node, for the purpose of coordination of the semi-static resources of a single- or dual-connected boundary IAB-node.

Direction: F1-terminating IAB-donor-CU → non-F1-terminating IAB-donor-CU, non-F1-terminating IAB-donor-CU→F1-terminating IAB-donor-CU

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| F1-terminating Donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Source NG-RAN node UE  XnAP ID or to the M-NG-RAN node UE XnAP ID or to the S-NG-RAN node UE XnAP ID. | YES | reject |
| Non F1-terminating Donor UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Target NG-RAN node UE  XnAP ID or to the S-NG-RAN node UE XnAP ID or to the M-NG-RAN node UE XnAP ID. | YES | reject |
| **Boundary Node Cells List** |  | *0..1* |  | List of cells served by the boundary node IAB-DU. | YES | reject |
| **>Boundary Node Cells List Item** |  | *1 .. <maxnoofServedCellsIAB >* |  |  | EACH | reject |
| >>Boundary Node Cell Information | M |  | IAB Cell Information  9.2.2.x14 |  |  |  |
| **Parent Node Cells List** |  | *0..1* |  | List of cells served by the parent node IAB-DU. | YES | reject |
| **>Parent Node Cells List Item** |  | *1 .. <* maxnoofServingCells *>* |  |  | EACH | reject |
| >>Parent Node Cell Information | M |  | IAB Cell Information  9.2.2.x14 |  |  |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofServedCellsIAB | Maximum number of cells served by an IAB-DU or an IAB-donor-DU. Value is 512. |
| maxnoofServingCells | Maximum no. of serving cells for an IAB-MT. Value is 32, as defined by the *maxNrofServingCells* in TS 38.331. |

#### 9.1.x.7 IAB RESOURCE COORDINATION RESPONSE

This message is sent by a non-F1-terminating/F1-terminating IAB-donor-CU to a F1-terminating/non-F1-terminating IAB-donor-CU of a boundary IAB-node, in response to an IAB RESOURCE COORDINATION REQUEST message.

Direction: non-F1-terminating IAB-donor-CU → F1-terminating IAB-donor-CU, F1-terminating IAB-donor-CU → non-F1-terminating IAB-donor-CU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| F1-terminating Donor node UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Source NG-RAN node UE  XnAP ID or to the M-NG-RAN node UE XnAP ID or to the S-NG-RAN node UE XnAP ID. | YES | reject |
| Non F1-terminating Donor node UE XnAP ID | M |  | NG-RAN node UE XnAP ID 9.2.3.16 | This IE refers to the Target NG-RAN node UE  XnAP ID or to the S-NG-RAN node UE XnAP ID or to the M-NG-RAN node UE XnAP ID. | YES | reject |
| **Boundary Node Cells List** |  | *0..1* |  | List of cells served by the boundary node IAB-DU. | YES | reject |
| **>Boundary Node Cells List Item** |  | *1 .. <maxnoofServedCellsIAB >* |  |  | EACH | reject |
| >>Boundary Node cell Information | M |  | IAB Cell Information  9.2.2.x14 |  |  |  |
| **Parent-Node Cells List** |  | *0..1* |  | List of cells served by the parent node IAB-DU. | YES | reject |
| **>Parent-Node Cells List Item** |  | *1 .. <* maxnoofServingCells *>* |  |  | EACH | reject |
| >>Parent Node Cell Information | M |  | IAB Cell Information  9.2.2.x14 |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofServedCellsIAB | Maximum number of cells served by an IAB-DU or an IAB-donor-DU. Value is 512. |
| maxnoofServingCells | Maximum no. of serving cells for an IAB-MT. Value is 32, as defined by the *maxNrofServingCells* in TS 38.331. |

-------------------------------------------Next change-------------------------------------------

#### 9.2.1.13 UE Context Information – Retrieve UE Context Response

This IE contains the UE context information within the RETRIEVE UE CONTEXT RESPONSE message.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| NG-C UE associated Signalling reference | M |  | AMF UE NGAP ID  9.2.3.26 | Allocated at the AMF on the old NG-C connection. | – |  |
| Signalling TNL Association Address at source NG-C side | M |  | CP Transport Layer Information  9.2.3.31 | This IE indicates the AMF’s IP address of the SCTP association used at the source NG-C interface instance.  Note: If no UE TNLA binding exists at the source NG-RAN node, the source NG-RAN node indicates the TNL association address it would have selected if it would have had to create a UE TNLA binding. | – |  |
| UE Security Capabilities | M |  | 9.2.3.49 |  | – |  |
| AS Security Information | M |  | 9.2.3.50 |  | – |  |
| UE Aggregate Maximum Bit Rate | M |  | 9.2.3.17 |  | – |  |
| PDU Session Resources To Be Setup List | M |  | 9.2.1.1 |  | – |  |
| RRC Context | M |  | OCTET STRING | Includes the *HandoverPreparationInformation* message as defined in subclause 11.2.2 of TS 38.331[10] if the old and new serving NG-RAN nodes are gNBs.  Includes either the *HandoverPreparationInformation* message as defined in subclause 10.2.2 of TS 36.331 [14] or the *HandoverPreparationInformation-NB* message as defined in subclause 10.6.2 of TS 36.331 [14], if the old and new serving NG-RAN nodes are ng-eNBs. | – |  |
| Mobility Restriction List | O |  | 9.2.3.53 |  | – |  |
| Index to RAT/Frequency Selection Priority | O |  | 9.2.3.23 |  | – |  |
| 5GC Mobility Restriction List Container | O |  | 9.2.3.100 |  | YES | ignore |
| NR UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.2.3.107 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| LTE UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.2.3.108 | This IE applies only if the UE is authorized for LTE V2X services. | YES | Ignore |
| UE Radio Capability ID | O |  | 9.2.3.138 |  | YES | reject |
| No PDU Session Indication | O |  | ENUMERATED (true, ...) | Applicable to IAB only. | YES | ignore |

-------------------------------------------Next change-------------------------------------------

9.2.2 NG-RAN Node and Cell Configuration related IE definitions

#### 9.2.2.11 Served Cell Information NR

This IE contains cell configuration information of an NR cell that a neighbouring NG-RAN node may need for the Xn AP interface.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| NR-PCI | M |  | INTEGER (0..1007, …) | NR Physical Cell ID | – |  |
| NR CGI | M |  | 9.2.2.7 |  | – |  |
| TAC | M |  | 9.2.2.5 | Tracking Area Code | – |  |
| RANAC | O |  | RAN Area Code  9.2.2.6 |  | – |  |
| **Broadcast PLMNs** |  | *1..<maxnoofBPLMNs>* |  | Broadcast PLMNs in SIB1 associated to the NR Cell Identity in the *NR CGI* IE. | – |  |
| >PLMN Identity | M |  | 9.2.2.4 |  | – |  |
| CHOICE *NR-Mode-Info* | M |  |  |  | – |  |
| >*FDD* |  |  |  |  |  |  |
| >>**FDD Info** |  | *1* |  |  | – |  |
| >>>UL NR Frequency Info | M |  | NR Frequency Info  9.2.2.19 |  | – |  |
| >>>DL NR Frequency Info | M |  | NR Frequency Info  9.2.2.19 |  | – |  |
| >>>UL Transmission Bandwidth | M |  | NR Transmission Bandwidth  9.2.2.20 |  | – |  |
| >>>DL Transmission Bandwidth | M |  | NR Transmission Bandwidth  9.2.2.20 |  | – |  |
| >>>UL Carrier List | O |  | NR Carrier List  9.2.2.63 | If included, the *UL Transmission Bandwidth* IE shall be ignored. | YES | ignore |
| >>>DL Carrier List | O |  | NR Carrier List  9.2.2.63 | If included, the *DL Transmission Bandwidth* IE shall be ignored. | YES | ignore |
| >>>gNB-DU Cell Resource Configuration-FDD-UL | M |  | gNB-DU Cell Resource Configuration  9.2.2.x14 | Contains FDD UL resource configuration of gNB-DU’s cell. Only applicable if the gNB-DU is an IAB-DU or an IAB-donor-DU. | – |  |
| >>>gNB-DU Cell Resource Configuration-FDD-DL | M |  | gNB-DU Cell Resource Configuration  9.2.2.x14 | Contains FDD UL resource configuration of gNB-DU’s cell. Only applicable if the gNB-DU is an IAB-DU or an IAB-donor-DU. | – |  |
| >*TDD* |  |  |  |  |  |  |
| >>**TDD Info** |  | *1* |  |  | – |  |
| >>>Frequency Info | M |  | NR Frequency Info  9.2.2.19 |  | – |  |
| >>>Transmission Bandwidth | M |  | NR Transmission Bandwidth  9.2.2.20 |  | – |  |
| >>>Intended TDD DL-UL Configuration NR | O |  | 9.2.2.40 |  | YES | ignore |
| >>>TDD UL-DL Configuration Common NR | O |  | OCTET STRING | The *tdd-UL-DL-ConfigurationCommon* as defined in TS 38.331 [10] | YES | ignore |
| >>>Carrier List | O |  | NR Carrier List  9.2.2.63 | If included, the *Transmission Bandwidth* IE shall be ignored. | YES | ignore |
| >>>gNB-DU Cell Resource Configuration-TDD | M |  | gNB-DU Cell Resource Configuration  9.2.2.x14 | Contains FDD UL resource configuration of gNB-DU’s cell. Only applicable if the gNB-DU is an IAB-DU or an IAB-donor-DU. | – |  |
| Measurement Timing Configuration | M |  | OCTET STRING | Contains the *MeasurementTimingConfiguration* inter-node message for the served cell, as defined in TS 38.331 [10]. | – |  |
| Connectivity Support | M |  | 9.2.2.28 |  | – |  |
| **Broadcast PLMN Identity Info List NR** |  | *0..<maxnoofBPLMNs>* |  | This IE corresponds to the *PLMN-IdentityInfoList* IE and the *NPN-IdentityInfoList* IE (if available) in *SIB1* as specified in TS 38.331 [8]. All PLMN Identities and associated information contained in the *PLMN-IdentityInfoList* IE and NPN identities and associated information contained in the *NPN-IdentityInfoList* IE (if available) are included and provided in the same order as broadcast in SIB1.  NOTE: In case of NPN-only cell, the PLMN Identities and associated information contained in the *PLMN-IdentityInfoList* IE are not included. | YES | ignore |
| **>Broadcast PLMNs** |  | *1..<maxnoofBPLMNs>* |  | Broadcast PLMNs in SIB1 associated to the *NR Cell Identity* IE. | – |  |
| >>PLMN Identity | M |  | 9.2.2.4 |  | – |  |
| >TAC | M |  | 9.2.2.5 |  | – |  |
| >NR Cell Identity | M |  | BIT STRING (SIZE(36)) |  | – |  |
| >RANAC | O |  | RAN Area Code  9.2.2.6 |  | – |  |
| >Configured TAC Indication | O |  | 9.2.2.39a | NOTE: This IE is associated with the TAC in the *Broadcast PLMN Identity Info List NR* IE | YES | ignore |
| >NPN Broadcast Information | O |  | 9.2.2.71 | If this IE is included the content of the *Broadcast PLMNs* IE in the *Broadcast PLMN Identity Info List NR* IE is ignored. | YES | reject |
| Configured TAC Indication | O |  | 9.2.2.39a | NOTE: This IE is associated with the TAC on top-level of the *Served Cell Information NR* IE | YES | ignore |
| NPN Broadcast Information | O |  | 9.2.2.71 | If this IE is included the content of the *Broadcast PLMNs* IE in the top *Served Cell Information NR* IE is ignored. | YES | reject |
| SSB Positions In Burst | O |  | 9.2.2.64 |  | YES | ignore |
| NR Cell PRACH Configuration | O |  | OCTET STRING | Containing 9.3.1.139 NR Cell PRACH Configuration as of TS 38.473 [41]. | YES | ignore |
| CSI-RS Transmission Indication | O |  | ENUMERATED (activated, deactivated, ...) | This IE indicates the CSI-RS transmission status of the given cell. | YES | ignore |
| SFN Offset | O |  | 9.2.2.75 |  | YES | Ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofBPLMNs | Maximum no. of broadcast PLMNs by a cell. Value is 12. |

#### 9.2.2.40 Intended TDD DL-UL Configuration NR

This IE contains the subcarrier spacing, cyclic prefix and TDD DL-UL slot configuration of an NR cell that a neighbour NG-RAN node needs to take into account for cross-link interference mitigation, and/or for NR-DC power coordination, when operating its own cells.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description | Criticality | Assigned Criticality |
| NR SCS | M |  | ENUMERATED (scs15, scs30, scs60, scs120, …) | The values scs15, scs30, scs60 and scs120 corresponds to the sub carrier spacing in TS 38.104 [24]. |  |  |
| NR Cyclic Prefix | M |  | ENUMERATED (Normal, Extended, …) | The type of cyclic prefix, which determines the number of symbols in a slot. |  |  |
| NR DL-UL Transmission Periodicity | M |  | ENUMERATED (ms0p5, ms0p625, ms1, ms1p25, ms2, ms2p5, ms3, ms4, ms5, ms10, ms20, ms40, ms60, ms80, ms100, ms120, ms140, ms160, …) | The periodicity is expressed in the format msXpYZ, and equals X.YZ milliseconds. |  |  |
| **Slot Configuration List** |  | 1 |  |  |  |  |
| **>Slot Configuration List Item** |  | *1..<maxnoofslots>* |  |  |  |  |
| >>Slot Index |  |  | INTEGER (0.. 5119) |  |  |  |
| >>CHOICE *Symbol Allocation in Slot* | M |  |  |  |  |  |
| >>>*All DL* |  |  |  |  |  |  |
| >>>*All UL* |  |  |  |  |  |  |
| >>>*Both DL and UL* |  |  |  |  |  |  |
| >>>>Number of DL Symbols | M |  | INTEGER (0..13) | Number of consecutive DL symbols at the beginning of the slot identified by Slot Index. If extended cyclic prefix is used, the maximum value is 11. The Permutation IE indicates the location of UL symbols in the slot. |  |  |
| >>>>Number of UL Symbols | M |  | INTEGER (0..13) | Number of consecutive UL symbols in the end of the slot identified by Slot Index. If extended cyclic prefix is used, the maximum value is 11. The Permutation IE indicates the location of UL symbols in the slot. |  |  |
| >>>>Permutation | O |  | ENUMERATED (DFU, UFD, …) | If not present, the default value is DFU. | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofslots | Maximum length of number of slots in a 10-ms period. Value is 5120. |

#### 9.2.2.x Multiplexing Info

This IE contains information about the multiplexing capabilities between the IAB-DU’s cell and the cells configured on the collocated IAB-MT.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **IAB-MT Cell List** |  | *1* |  |  |
| **>IAB-MT Cell Item** |  | *1* .. <*maxnoofServingCells*> |  |  |
| >>NR Cell Identity | M |  | BIT STRING (SIZE(36)) | Cell identity of a serving cell configured for a collocated IAB-MT. |
| >>DU\_RX/MT\_RX | M |  | ENUMERATED (supported, not supported, supported and FDM required) | An indication of whether the IAB-node supports simultaneous reception at its DU and MT side. |
| >>DU\_TX/MT\_TX | M |  | ENUMERATED (supported, not supported, supported and FDM required) | An indication of whether the IAB-node supports simultaneous transmission at its DU and MT side. |
| >>DU\_TX/MT\_RX | M |  | ENUMERATED (supported, not supported, supported and FDM required) | An indication of whether the IAB-node supports simultaneous transmission at its DU and reception at its MT side. |
| >>DU\_RX/MT\_TX | M |  | ENUMERATED (supported, not supported, supported and FDM required) | An indication of whether the IAB-node supports simultaneous reception at its DU and transmission at its MT side. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofServingCells | Maximum no. of serving cells for an IAB-MT. Value is 32, as defined by the *maxNrofServingCells* in TS 38.331 [10]. |

#### 9.2.2.x0 Traffic Index

This IE is used to identify the traffic offloaded to the topology of non-F1-terminating IAB-donor-CU.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Traffic Index | M | INTEGER (1..1024,…) |  |  |

#### 9.2.2.x1 Traffic Profile

This IE is used to indication the Traffic QoS parameters for F1-U traffic or non-UP traffic type. This IE is only applicable to IAB.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *Traffic type* | M |  |  |  |
| *>UP Traffic* |  |  |  |  |
| >>QoS Parameters | M |  | 9.2.3.5 |  |
| >*Non-UP Traffic* |  |  | 9.2.2.x20 |  |

#### 9.2.2.x2 F1-Terminating Topology BH Information

This IE provides the BH information of the traffic used in F1-terminating donor’s topology. This IE is only applicable to IAB.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **F1-terminating BH information list** |  | *1* |  |  |
| >**F1-terminating BH Information item IEs** |  | *1..<maxnoofBHInfo>* |  |  |
| >>BH Info Index | M |  | INTEGER (1..maxnoofBHInfo) |  |
| >>DL TNL Address | O |  | 9.2.2.x12 |  |
| >>DL F1 term BH Info |  | *0..1* |  | This IE indicates the BH information for DL traffic. |
| >>> Egress BAP Routing ID | M |  | 9.2.2.x7 |  |
| >>> Egress BH RLC CH ID | M |  | 9.2.2.x8 |  |
| >>UL F1 term BH Info |  | *0..1* |  | This IE indicates the BH information for UL traffic. |
| >>>Ingress BAP Routing ID | M |  | 9.2.2.x7 |  |
| >>>Ingress BH RLC CH ID | M |  | 9.2.2.x8 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofBHInfo | Maximum no. of BH information corresponding to one Traffic Index assigned to the traffic offloaded to the non-F1-terminating IAB-donor-CU. The value is 1024. |

#### 9.2.2.x3 Non-F1-terminating Topology BH Information

This IE provides the BH information of the traffic used in non-F1-terminating donor’s topology. This IE is only applicable to IAB.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **Non-F1-terminating BH Information list** |  | *1* |  |  |
| **>Non-F1-terminating BH Information item IEs** |  | *1..<maxnoofBHInfo>* |  |  |
| >> BH Info Index | M |  | INTEGER (1..maxnoofBHInfo) |  |
| >>DL non-F1 term BH Info |  | *0..1* |  | This IE indicates the BH information for DL traffic |
| >>>Ingress BAP routing ID | M |  | 9.2.2.x7 |  |
| >>>Ingress BH RLC CH | M |  | 9.2.2.x8 |  |
| >>>Prior-hop BAP address | M |  | 9.2.2.x9 |  |
| >>>QoS mapping information | M |  | 9.2.2.x11 |  |
| >>>UL non-F1 term BH Info |  | *0..1* |  | This IE indicates the BH information for UL traffic |
| >>>Egress BAP Routing ID | M |  | 9.2.2.x7 |  |
| >>>Egress BH RLC CH ID | M |  | 9.2.2.x8 |  |
| >>>Next-hop BAP address | M |  | 9.2.2.x9 |  |
| **BAPControl PDU RLC CH List** |  | *0..1* |  |  |
| >**BAP Control PDU RLC CH Item IEs** |  | *1..<maxnoofBAPControlPDURLCCHs>* |  |  |
| >>BH RLC CH ID | M |  | 9.2.2.x8 |  |
| >>Next-hop BAP Address | M |  | 9.2.2.x9 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofBHInfo | Maximum no. of BH information corresponding to one Traffic Index assigned to the traffic offloaded to the non-F1-terminating IAB-donor-CU. The value is 1024. |
| maxnoofBAPControlPDURLCCHs | Maximum no. of BH RLC CHs to be used for the boundary IAB-node and its parent node in the non-F1-terminating topology. The value is 2. |

#### 9.2.2.x4 Traffic To Be Released Information

This IE is used to indicate the request to release the offloaded traffic.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *Release type* | M |  |  |  |
| >*Full Release* |  |  |  |  |
| >>All Traffic Indication | M |  | ENUMERATED(true, ..) |  |
| >*Partial Release* |  |  |  |  |
| >>**Traffic To Be Released List** |  | *1* |  |  |
| >>>**Traffic To Be Released Item IE** |  | *1 .. <maxnoofTrafficIndexEntries>* |  |  |
| >>>>Traffic Index | M |  | 9.2.2.x0 |  |
| >>>>BH Info List | O |  | 9.2.2.x19 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTrafficIndexEntries | Maximum no. of traffic offloaded to the non-F1-terminating IAB-donor-CU. The value is 1024. |



#### 9.2.2.x5 IAB TNL Address Request

This IE indicates the request of IP address assignment.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| IAB IPv4 Addresses Requested | O |  | IAB TNL Addresses Requested  9.2.2.x13 |  |
| CHOICE *IAB IPv6 Request Type* | O |  |  |  |
| >*IPv6 Address* |  |  |  |  |
| >>IAB IPv6 Addresses Requested | M |  | IAB TNL Addresses Requested  9.2.2.x13 |  |
| >*IPv6 Prefix* |  |  |  |  |
| >>IAB IPv6 Address Prefixes Requested | M |  | IAB TNL Addresses Requested  9.2.2.x13 |  |
| **IAB TNL Address To Remove List** |  | *0..1* |  |  |
| **>IAB TNL Address To Remove Item** |  | *1*..<*maxnoofTLAsIAB*> |  |  |
| >>IAB TNL Address | M |  | 9.2.2.x12 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTLAsIAB | Maximum no. of individual IPv4/IPv6 addresses or IPv6 address prefixes that can be allocated in one procedure execution. The value is 1024. |

#### 9.2.2.x6 IAB TNL Address Response

This IE indicates the assigned IP address to an IAB node.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **IAB Allocated TNL Address List** |  | *1* |  |  |
| **>IAB Allocated TNL Address Item** |  | *1*..<*maxnoofTLAsIAB*> |  |  |
| >>IAB TNL Address | M |  | 9.2.2.x12 |  |
| >>IAB TNL Address Usage | O |  | ENUMERATED (F1-C, F1-U, Non-F1, All, …) | The usage of the allocated IPv4 or IPv6 address or IPv6 address prefix. |
| >>Associated Donor DU Address | O |  | 9.2.2.x9 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTLAsIAB | Maximum no. of IPv6 addresses or IPv6 address prefixes and/or individual IPv4 addresses that can be allocated in one procedure execution. The value is 1024. |

#### 9.2.2.x7 BAP Routing ID

This IE indicates the BAP Routing ID.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| BAP Address | M |  | 9.2.3.x9 |  |
| Path ID | M |  | BAP Path ID  9.2.3.x10 |  |

#### 9.2.2.x8 BH RLC Channel ID

This IE uniquely identifies a BH RLC channel in the link between IAB-MT of the IAB-node and IAB-DU of the parent IAB-node or IAB-donor-DU.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| BH RLC CH ID | M |  | BIT STRING (SIZE(16)) |  |

#### 9.2.2.x9 BAP Address

This IE indicates the BAP address of an IAB-node or of an IAB-donor-DU, and it is part of the BAP Routing ID.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| BAP Address | M |  | BIT STRING (SIZE(10)) | Corresponds to the *bap-Address-r16*, defined in subclause 6.2.2 or subclause 6.3.2 of TS 38.331 [10], *or the iab-donor-DU-BAP-address-r16* defined in subclause 6.2.2 of TS 38.331[10]. |

#### 9.2.2.x10 BAP Path ID

This IE indicates the BAP path ID, which is part of the BAP Routing ID.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| BAP Path ID | M |  | BIT STRING (SIZE(10)) | Corresponds to the *Bap-Pathid-r16* defined in subclause 6.3.2 of TS 38.331 [10]. |

#### 9.2.2.x11 QoS mapping information

This IE indicates the DSCP and/or IPv6 Flow Label field(s) of IP packet which is sent through the GTP-U tunnel of a requested DRB. This IE is only used for IAB.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| DSCP | O |  | BIT STRING (SIZE(6)) |  |
| Flow Label | O |  | BIT STRING (SIZE(20)) |  |

#### 9.2.2.x12 IAB TNL Address

The *IAB TNL Address* IE indicates an IPv4 or IPv6 address or an IPv6 address prefix assigned to an IAB-node.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *IAB TNL Address* | M |  |  |  |
| *>IPv4* |  |  |  |  |
| >>IPv4 Address | M |  | BIT STRING (SIZE(32)) | The IPv4 address allocated to an IAB-node. |
| *>IPv6* |  |  |  |  |
| >>IPv6 Address | M |  | BIT STRING (SIZE(128)) | The IPv6 address allocated to an IAB-node. |
| *>IPv6prefix* |  |  |  |  |
| >>IPv6 Prefix | M |  | BIT STRING (SIZE(64)) | The IPv6 address prefix allocated to an IAB-node. |

#### 9.2.2.x13 IAB TNL Addresses Requested

The *IAB TNL Addresses Requested* IE indicates the number of IPv4 or IPv6 addresses or IPv6 address prefixes requested for the indicated usage.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| TNL Addresses or Prefixes Requested - All Traffic | O |  | INTEGER (1..256) | The number of TNL addresses/ IPv6 prefixes requested for all traffic. |
| TNL Addresses or Prefixes Requested - F1-C traffic | O |  | INTEGER (1..256) | The number of TNL addresses/IPv6 prefixes requested for F1-C traffic. |
| TNL Addresses or Prefixes Requested - F1-U traffic | O |  | INTEGER (1..256) | The number of TNL addresses/ IPv6 prefixes requested for F1-U traffic. |
| TNL Addresses or Prefixes Requested - Non-F1 traffic | O |  | INTEGER (1..256) | The number of TNL addresses/ IPv6 prefixes requested for non-F1 traffic. |

#### 9.2.2.x14 IAB Cell Information

This IE contains IAB-DU cell resource configuration, cell specific signal/channel configuration and multiplexing info of the cell of an IAB-node or IAB-donor-DU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| NR CGI | M |  | 9.2.2.7 |  | - |  |
| CHOICE *IAB-DU Cell Resource Configuration-Mode-Info* | O |  |  |  | - |  |
| >*TDD* |  |  |  |  | - |  |
| >>TDD Info |  | *1* |  |  | - |  |
| >>>gNB-DU Cell Resource Configuration-TDD | M |  | gNB-DU Cell Resource Configuration  9.2.2.x15 | Contains TDD resource configuration of gNB-DU’s cell. | - |  |
| >>>Frequency Info | O |  | NR Frequency Info  9.2.2.19 |  | – |  |
| >>>Transmission Bandwidth | O |  | NR Transmission Bandwidth  9.2.2.20 |  | – |  |
| >>>Carrier List | O |  | NR Carrier List  9.2.2.63 | If included, the *Transmission Bandwidth* IE shall be ignored. | YES | ignore |
| >*FDD* |  |  |  |  | - |  |
| >>FDD Info |  | *1* |  |  | - |  |
| >>>gNB-DU Cell Resource Configuration-FDD-UL | M |  | gNB-DU Cell Resource Configuration  9.2.2.x15 | Contains FDD UL resource configuration of gNB-DU’s cell. | - |  |
| >>>gNB-DU Cell Resource Configuration-FDD-DL | M |  | gNB-DU Cell Resource Configuration  9.2.2.x15 | Contains FDD DL resource configuration of gNB-DU’s cell. | - |  |
| >>>UL Frequency Info | O |  | NR Frequency Info  9.2.2.19 |  | – |  |
| >>>DL Frequency Info | O |  | NR Frequency Info  9.2.2.19 |  | – |  |
| >>>UL Transmission Bandwidth | O |  | NR Transmission Bandwidth  9.2.2.20 |  | – |  |
| >>>DL Transmission Bandwidth | O |  | NR Transmission Bandwidth  9.2.2.20 |  | – |  |
| >>>UL Carrier List | O |  | NR Carrier List  9.2.2.63 | If included, the *UL Transmission Bandwidth* IE shall be ignored. | YES | ignore |
| >>>DL Carrier List | O |  | NR Carrier List  9.2.2.63 | If included, the *DL Transmission Bandwidth* IE shall be ignored. | YES | ignore |
| IAB STC Info | O |  | 9.2.2.x16 | STC configuration of child-node IAB-DU’s cell. | - |  |
| RACH Config Common | O |  | OCTET STRING | Corresponds to the *rach-ConfigCommon* as defined in subclause 6.3.2 of TS 38.331 [8]. | - |  |
| RACH Config Common IAB | O |  | OCTET STRING | Corresponds to the IAB-specific *rach-ConfigCommonIAB-r16* as defined in subclause 6.3.2 of TS 38.331 [8]. | - |  |
| CSI-RS Configuration | O |  | OCTET STRING | Corresponds to the *NZP-CSI-RS-Resource* as defined in subclause 6.3.2 of TS 38.331 [8]. | - |  |
| SR Configuration | O |  | OCTET STRING | Corresponds to the *SchedulingRequestResourceConfig* as defined in subclause 6.3.2 of TS 38.331 [8]. | - |  |
| PDCCH Configuration SIB1 | O |  | OCTET STRING | Corresponds to the *PDCCH-ConfigSIB1* as defined in subclause 6.3.2 of TS 38.331 [8]. | - |  |
| SCS Common | O |  | OCTET STRING | Corresponds to the *subCarrierSpacingCommon* as defined in subclause 6.2.2 of TS 38.331 [8]. | - |  |
| Multiplexing Info | O |  | 9.2.2.x | Contains information on multiplexing with cells configured for collocated IAB-MT, if applicable. | - |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofServedCellsIAB | Maximum number of cells served by an IAB-DU or an IAB-donor-DU. Value is 512. |

#### 9.2.2.x15 gNB-DU Cell Resource Configuration

This IE contains the resource configuration of the cells served by a gNB-DU, i.e. the TDD/FDD resource parameters for each activated cell (TS 38.213 [40], clause 11.1.1). This IE is only applicable if the gNB-DU is an IAB-DU or an IAB-donor-DU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Subcarrier Spacing | M |  | ENUMERATED (kHz15, kHz30, kHz60, kHz120, kHz240, spare3, spare2, spare1, …) | Subcarrier spacing used as reference for the TDD/FDD slot configuration. | YES | reject |
| DUF Transmission Periodicity | O |  | ENUMERATED (ms0p5, ms0p625, ms1, ms1p25, ms2, ms2p5, ms5, ms10, …) |  | YES | reject |
| **DUF Slot Configuration List** |  | *0..1* |  |  | YES | reject |
| >**DUF Slot Configuration Item** |  | *1*..<*maxnoofDUFSlots*> |  | The *maxNrofSlots* in TS 38.331 [8]. | - |  |
| >>CHOICE *DUF Slot Configuration* | M |  |  |  | - |  |
| >>>Explicit Format |  |  |  |  | - |  |
| >>>>Permutation | M |  | ENUMERATED (DFU, UFD, …) |  | - |  |
| >>>>Number of Downlink Symbols | O |  | INTEGER (0..14) |  | - |  |
| >>>>Number of Uplink Symbols | O |  | INTEGER (0..14) |  | - |  |
| >>>Implicit Format |  |  |  |  |  |  |
| >>>>DUF Slot Format Index | M |  | INTEGER (0..254) | Index into Table 11.1.1-1 and Table 14-2 in TS 38.213 [31], excluding the last row in Table 14-2. | - |  |
| HSNA Transmission Periodicity | M |  | ENUMERATED (ms0p5, ms0p625, ms1, ms1p25, ms2, ms2p5, ms5, ms10, ms20, ms40, ms80, ms160, …) |  | YES | reject |
| **HSNA Slot Configuration List** |  | 0..1 |  |  | YES | reject |
| >**HSNA Slot Configuration Item** |  | 1..<*maxnoofHSNASlots*> |  |  |  |  |
| >>HSNA Downlink | O |  | ENUMERATED (HARD, SOFT, NOTAVAILABLE) | HSNA value for downlink symbols in a slot. | - |  |
| >>HSNA Uplink | O |  | ENUMERATED (HARD, SOFT, NOTAVAILABLE) | HSNA value for uplink symbols in a slot. | - |  |
| >>HSNA Flexible | O |  | ENUMERATED (HARD, SOFT, NOTAVAILABLE) | HSNA value for flexible symbols in a slot. | - |  |
| RB Set Configuration | O |  | 9.2.2.x17 | Indicates the configuration for up to M non-overlapping RB sets for a given DU cell, used for frequency domain resource allocation. | YES | reject |
| **Frequency-domain HSNA Configuration List** |  | 0..1 |  |  | YES | reject |
| >**Frequency-domain** **HSNA Configuration Item** |  | 1..<*maxnoofRBsetsPerCell*> |  |  | - |  |
| >>RB set Index | M |  | INTEGER (1.. *maxnoofRBsetsPerCell*) | Refers to an RB set defined by RB Set Configuration. | - |  |
| **>>Frequency-domain HSNA Slot Configuration List** |  | 1 |  |  | - |  |
| **>>>Frequency-domain HSNA Slot Configuration item** |  | 1..<*maxnoofHSNASlots*> |  |  | - |  |
| >>>>Slot Index | M |  | INTEGER (.. *maxnoofHSNASlots*) | Index to a slot within the HSNA Transmission Periodicity. \* | - |  |
| >>>>HSNA Downlink | O |  | ENUMERATED (HARD, SOFT, NOTAVAILABLE) | HSNA value for downlink symbols in a slot, for an RB set. | - |  |
| >>>>HSNA Uplink | O |  | ENUMERATED (HARD, SOFT, NOTAVAILABLE) | HSNA value for uplink symbols in a slot, for an RB set. | - |  |
| >>>>HSNA Flexible | O |  | ENUMERATED (HARD, SOFT, NOTAVAILABLE) | HSNA value for flexible symbols in a slot, for an RB set. | - |  |
| **NA cell resource configuration List** |  | 0..1 |  | List of unavailable resources of this cell for the dual-connected boundary node. | YES | reject |
| >**NA cell resource configuration Item** |  | 1..<*maxnoofHSNASlots*> |  |  | - |  |
| >>NA Downlink | O |  | ENUMERATED (true, false, …) | Indicates whether downlink symbols, in a slot, are unavailable to serve the boundary IAB-node. | - |  |
| >>NA Uplink | O |  | ENUMERATED (true, false, …) | Indicates whether uplink symbols, in a slot, are unavailable to serve the boundary IAB-node. | - |  |
| >>NA Flexible | O |  | ENUMERATED (true, false, …) | Indicates whether flexible symbols, in a slot, are unavailable to serve the boundary IAB-node. | - |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDUFSlots | Maximum no. of slots in 10ms. Value is 320. |
| maxnoofSymbols | Maximum no. of symbols in a slot. Value is 14. |
| maxnoofHSNASlots | Maximum no of "Hard", "Soft" or "Not available" slots in 160ms. Value is 5120. |
| maxnoofRBsetsPerCell | Maximum no. of RB sets per DU cell. Value is 8. |
| maxnoofChildIABNodes | Maximum number of child nodes served by an IAB-DU or IAB-donor-DU. Value is 1024. |

#### 9.2.2.x16 IAB STC Info

This IE contains cell SSB Transmission Configuration (STC) information of an IAB-DU or an IAB-donor-DU.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **IAB STC-Info List** |  | *1* |  |  |
| **>IAB STC-Info Item** |  | *1* ..<*maxnoofIABSTCInfo*> |  |  |
| >>SSB Frequency Info | M |  | INTEGER (0.. maxNRARFCN) | The SSB central frequency. |
| >>SSB Subcarrier Spacing | M |  | ENUMERATED (kHz15, kHz30, kHz120, kHz240, spare3, spare2, spare1, …) | The SSB subcarrier spacing. |
| >>SSB Transmission Periodicity | M |  | ENUMERATED (sf5, sf10, sf20, sf40, sf80, sf160, sf320, sf640, ,,,) |  |
| >>SSB Transmission Timing Offset | M |  | INTEGER (0.. 127, …) | SSB transmission timing offset in number of half-frames. |
| >>CHOICE *SSB Transmission Bitmap* | M |  |  | The *SSB-ToMeasure* IE defined in TS 38.331 [10]. |
| >>>Short Bitmap | M |  | BIT STRING (SIZE (4)) |  |
| >>>Medium Bitmap | M |  | BIT STRING (SIZE (8)) |  |
| >>>Long Bitmap | M |  | BIT STRING (SIZE (64)) |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofIABSTCInfo | Maximum no. of STC configurations. Value is 5. This includes 1 STC configuration for access and 4 STC configurations for backhaul. |
| maxNRARFCN | Maximum value of NR ARFCNs. Value is 3279165. |

#### 9.2.2.x17 RB Set Configuration

This IE contains the configuration for up to M non-overlapping RB sets for a given gNB-DU cell, used for frequency domain resource allocation. This IE is only applicable if the gNB-DU is an IAB-DU or an IAB-donor-DU.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Subcarrier Spacing | M |  | ENUMERATED (kHz15, kHz30, kHz60, kHz120, kHz240, spare3, spare2, spare1, …) | Subcarrier spacing used as reference for the RB set configuration. |
| RB Set Size | M |  | ENUMERATED (2, 4, 8, 16, 32, 64) | Number of PRBs in each RB set. |
| **RB Set List** |  | *0..1* |  |  |
| **>RB Set Item** |  | *1*..<*maxnoofRBsetsPerCell*> |  |  |
| >>RB Set Index | M |  | INTEGER (1.. *maxnoofRBsetsPerCell*) |  |
| >>Initial RB Index | M |  | INTEGER (1.. *maxnoofPhysicalResourceBlocks*) |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofRBsetsPerCell | Maximum no. of RB sets per IAB-DU or an IAB-donor-DU cell. Value is 8. |
| maxnoofPhysicalResourceBlocks | Maximum no. of Physical Resource Blocks. Value is 275. |

#### 9.2.2.x18 IAB TNL Address Exception

This IE indicates the list of TNL addresses related to the UL packets to be forwarded over the Inter-donor-DU tunnel and that are exempt from TNL address filtering.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **IAB TNL Address List** |  | *1* |  |  | YES | ignore |
| **>IAB TNL Address Item IEs** |  | *1..< maxnoofTLAsIAB>* |  |  |  |  |
| >>IAB TNL Address | M |  | 9.2.2.X12 |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTLAsIAB | Maximum no. of individual IPv4/IPv6 addresses or IPv6 address prefixes in one procedure execution. The value is 1024. |

#### 9.2.2.x19 BH Info List

This IE indicates a list of BH information index, each of which represents the offloaded traffic with certain configured BH information, e.g., BAP routing ID, BH RLC CH.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| BH Info List |  | *1* |  |  |
| **>BH Info Item IEs** |  | *1..<maxnoofBHInfo>* |  |  |
| >>BH Info Index | M |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofBHInfo | Maximum no. of BH information corresponding to one Traffic Index assigned to the traffic offloaded to the non-F1-terminating IAB-donor-CU.The value is 1024. |

#### 9.2.2.x20 Non-UP traffic

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE non-UP*Traffic* |  |  |  |  |
| >Non-UP Traffic Type | M |  | ENUMERATED(UE-associated F1AP, non-UE-associated F1AP, non-F1, ...) |  |
| >Control Plane Traffic Type | M |  | INTEGER (1..3, ...) | Identified by the different codepoints in this IE, where 1 has the highest priority. |

-------------------------------------------Next Change-------------------------------------------

9.3.3 Elementary Procedure Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedure definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-PDU-Descriptions {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-PDU-Descriptions (0) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Criticality,

ProcedureCode

FROM XnAP-CommonDataTypes

HandoverRequest,

HandoverRequestAcknowledge,

HandoverPreparationFailure,

SNStatusTransfer,

UEContextRelease,

HandoverCancel,

NotificationControlIndication,

RANPaging,

RetrieveUEContextRequest,

RetrieveUEContextResponse,

RetrieveUEContextFailure,

XnUAddressIndication,

SecondaryRATDataUsageReport,

SNodeAdditionRequest,

SNodeAdditionRequestAcknowledge,

SNodeAdditionRequestReject,

SNodeReconfigurationComplete,

SNodeModificationRequest,

SNodeModificationRequestAcknowledge,

SNodeModificationRequestReject,

SNodeModificationRequired,

SNodeModificationConfirm,

SNodeModificationRefuse,

SNodeReleaseRequest,

SNodeReleaseRequestAcknowledge,

SNodeReleaseReject,

SNodeReleaseRequired,

SNodeReleaseConfirm,

SNodeCounterCheckRequest,

SNodeChangeRequired,

SNodeChangeConfirm,

SNodeChangeRefuse,

RRCTransfer,

XnRemovalRequest,

XnRemovalResponse,

XnRemovalFailure,

XnSetupRequest,

XnSetupResponse,

XnSetupFailure,

NGRANNodeConfigurationUpdate,

NGRANNodeConfigurationUpdateAcknowledge,

NGRANNodeConfigurationUpdateFailure,

E-UTRA-NR-CellResourceCoordinationRequest,

E-UTRA-NR-CellResourceCoordinationResponse,

ActivityNotification,

CellActivationRequest,

CellActivationResponse,

CellActivationFailure,

ResetRequest,

ResetResponse,

ErrorIndication,

PrivateMessage,

DeactivateTrace,

TraceStart,

HandoverSuccess,

ConditionalHandoverCancel,

EarlyStatusTransfer,

FailureIndication,

HandoverReport,

ResourceStatusRequest,

ResourceStatusResponse,

ResourceStatusFailure,

ResourceStatusUpdate,

MobilityChangeRequest,

MobilityChangeAcknowledge,

MobilityChangeFailure,

AccessAndMobilityIndication,

F1CTrafficTransfer,

IABTransportMigrationManagementRequest,

IABTransportMigrationManagementResponse,

IABTransportMigrationModificationRequest,

IABTransportMigrationModificationResponse,

IABResourceCoordinationRequest,

IABResourceCoordinationResponse

FROM XnAP-PDU-Contents

id-handoverPreparation,

id-sNStatusTransfer,

id-handoverCancel,

id-notificationControl,

id-retrieveUEContext,

id-rANPaging,

id-xnUAddressIndication,

id-uEContextRelease,

id-secondaryRATDataUsageReport,

id-sNGRANnodeAdditionPreparation,

id-sNGRANnodeReconfigurationCompletion,

id-mNGRANnodeinitiatedSNGRANnodeModificationPreparation,

id-sNGRANnodeinitiatedSNGRANnodeModificationPreparation,

id-mNGRANnodeinitiatedSNGRANnodeRelease,

id-sNGRANnodeinitiatedSNGRANnodeRelease,

id-sNGRANnodeCounterCheck,

id-sNGRANnodeChange,

id-activityNotification,

id-rRCTransfer,

id-xnRemoval,

id-xnSetup,

id-nGRANnodeConfigurationUpdate,

id-e-UTRA-NR-CellResourceCoordination,

id-cellActivation,

id-reset,

id-errorIndication,

id-privateMessage,

id-deactivateTrace,

id-traceStart,

id-handoverSuccess,

id-conditionalHandoverCancel,

id-earlyStatusTransfer,

id-failureIndication,

id-handoverReport,

id-resourceStatusReportingInitiation,

id-resourceStatusReporting,

id-mobilitySettingsChange,

id-accessAndMobilityIndication,

id-f1CTrafficTransfer,

id-iABTransportMigrationManagement,

id-iABTransportMigrationModification,

id-iABResourceCoordination

FROM XnAP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure Class

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XNAP-ELEMENTARY-PROCEDURE ::= CLASS {

&InitiatingMessage ,

&SuccessfulOutcome OPTIONAL,

&UnsuccessfulOutcome OPTIONAL,

&procedureCode ProcedureCode UNIQUE,

&criticality Criticality DEFAULT ignore

}

WITH SYNTAX {

INITIATING MESSAGE &InitiatingMessage

[SUCCESSFUL OUTCOME &SuccessfulOutcome]

[UNSUCCESSFUL OUTCOME &UnsuccessfulOutcome]

PROCEDURE CODE &procedureCode

[CRITICALITY &criticality]

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface PDU Definition

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-PDU ::= CHOICE {

initiatingMessage InitiatingMessage,

successfulOutcome SuccessfulOutcome,

unsuccessfulOutcome UnsuccessfulOutcome,

...

}

InitiatingMessage ::= SEQUENCE {

procedureCode XNAP-ELEMENTARY-PROCEDURE.&procedureCode ({XNAP-ELEMENTARY-PROCEDURES}),

criticality XNAP-ELEMENTARY-PROCEDURE.&criticality ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value XNAP-ELEMENTARY-PROCEDURE.&InitiatingMessage ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

SuccessfulOutcome ::= SEQUENCE {

procedureCode XNAP-ELEMENTARY-PROCEDURE.&procedureCode ({XNAP-ELEMENTARY-PROCEDURES}),

criticality XNAP-ELEMENTARY-PROCEDURE.&criticality ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value XNAP-ELEMENTARY-PROCEDURE.&SuccessfulOutcome ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

UnsuccessfulOutcome ::= SEQUENCE {

procedureCode XNAP-ELEMENTARY-PROCEDURE.&procedureCode ({XNAP-ELEMENTARY-PROCEDURES}),

criticality XNAP-ELEMENTARY-PROCEDURE.&criticality ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value XNAP-ELEMENTARY-PROCEDURE.&UnsuccessfulOutcome ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XNAP-ELEMENTARY-PROCEDURES XNAP-ELEMENTARY-PROCEDURE ::= {

XNAP-ELEMENTARY-PROCEDURES-CLASS-1 |

XNAP-ELEMENTARY-PROCEDURES-CLASS-2 ,

...

}

XNAP-ELEMENTARY-PROCEDURES-CLASS-1 XNAP-ELEMENTARY-PROCEDURE ::= {

handoverPreparation |

retrieveUEContext |

sNGRANnodeAdditionPreparation |

mNGRANnodeinitiatedSNGRANnodeModificationPreparation |

sNGRANnodeinitiatedSNGRANnodeModificationPreparation |

mNGRANnodeinitiatedSNGRANnodeRelease |

sNGRANnodeinitiatedSNGRANnodeRelease |

sNGRANnodeChange |

xnRemoval |

xnSetup |

nGRANnodeConfigurationUpdate |

e-UTRA-NR-CellResourceCoordination |

cellActivation |

reset |

resourceStatusReportingInitiation |

mobilitySettingsChange |

iABTransportMigrationManagement |

iABTransportMigrationModification |

iABResourceCoordination ,

...

}

XNAP-ELEMENTARY-PROCEDURES-CLASS-2 XNAP-ELEMENTARY-PROCEDURE ::= {

sNStatusTransfer |

handoverCancel |

rANPaging |

xnUAddressIndication |

uEContextRelease |

sNGRANnodeReconfigurationCompletion |

sNGRANnodeCounterCheck |

rRCTransfer |

errorIndication |

privateMessage |

notificationControl |

activityNotification |

secondaryRATDataUsageReport |

deactivateTrace |

traceStart |

handoverSuccess |

conditionalHandoverCancel |

earlyStatusTransfer |

failureIndication |

handoverReport |

resourceStatusReporting |

accessAndMobilityIndication |

f1CTrafficTransfer ,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

handoverPreparation XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE HandoverRequest

SUCCESSFUL OUTCOME HandoverRequestAcknowledge

UNSUCCESSFUL OUTCOME HandoverPreparationFailure

PROCEDURE CODE id-handoverPreparation

CRITICALITY reject

}

sNStatusTransfer XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNStatusTransfer

PROCEDURE CODE id-sNStatusTransfer

CRITICALITY ignore

}

handoverCancel XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE HandoverCancel

PROCEDURE CODE id-handoverCancel

CRITICALITY ignore

}

retrieveUEContext XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE RetrieveUEContextRequest

SUCCESSFUL OUTCOME RetrieveUEContextResponse

UNSUCCESSFUL OUTCOME RetrieveUEContextFailure

PROCEDURE CODE id-retrieveUEContext

CRITICALITY reject

}

rANPaging XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE RANPaging

PROCEDURE CODE id-rANPaging

CRITICALITY reject

}

xnUAddressIndication XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE XnUAddressIndication

PROCEDURE CODE id-xnUAddressIndication

CRITICALITY reject

}

uEContextRelease XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE UEContextRelease

PROCEDURE CODE id-uEContextRelease

CRITICALITY reject

}

sNGRANnodeAdditionPreparation XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNodeAdditionRequest

SUCCESSFUL OUTCOME SNodeAdditionRequestAcknowledge

UNSUCCESSFUL OUTCOME SNodeAdditionRequestReject

PROCEDURE CODE id-sNGRANnodeAdditionPreparation

CRITICALITY reject

}

sNGRANnodeReconfigurationCompletion XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNodeReconfigurationComplete

PROCEDURE CODE id-sNGRANnodeReconfigurationCompletion

CRITICALITY reject

}

mNGRANnodeinitiatedSNGRANnodeModificationPreparation XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNodeModificationRequest

SUCCESSFUL OUTCOME SNodeModificationRequestAcknowledge

UNSUCCESSFUL OUTCOME SNodeModificationRequestReject

PROCEDURE CODE id-mNGRANnodeinitiatedSNGRANnodeModificationPreparation

CRITICALITY reject

}

sNGRANnodeinitiatedSNGRANnodeModificationPreparation XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNodeModificationRequired

SUCCESSFUL OUTCOME SNodeModificationConfirm

UNSUCCESSFUL OUTCOME SNodeModificationRefuse

PROCEDURE CODE id-sNGRANnodeinitiatedSNGRANnodeModificationPreparation

CRITICALITY reject

}

mNGRANnodeinitiatedSNGRANnodeRelease XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNodeReleaseRequest

SUCCESSFUL OUTCOME SNodeReleaseRequestAcknowledge

UNSUCCESSFUL OUTCOME SNodeReleaseReject

PROCEDURE CODE id-mNGRANnodeinitiatedSNGRANnodeRelease

CRITICALITY reject

}

sNGRANnodeinitiatedSNGRANnodeRelease XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNodeReleaseRequired

SUCCESSFUL OUTCOME SNodeReleaseConfirm

PROCEDURE CODE id-sNGRANnodeinitiatedSNGRANnodeRelease

CRITICALITY reject

}

sNGRANnodeCounterCheck XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNodeCounterCheckRequest

PROCEDURE CODE id-sNGRANnodeCounterCheck

CRITICALITY reject

}

sNGRANnodeChange XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNodeChangeRequired

SUCCESSFUL OUTCOME SNodeChangeConfirm

UNSUCCESSFUL OUTCOME SNodeChangeRefuse

PROCEDURE CODE id-sNGRANnodeChange

CRITICALITY reject

}

rRCTransfer XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE RRCTransfer

PROCEDURE CODE id-rRCTransfer

CRITICALITY reject

}

xnRemoval XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE XnRemovalRequest

SUCCESSFUL OUTCOME XnRemovalResponse

UNSUCCESSFUL OUTCOME XnRemovalFailure

PROCEDURE CODE id-xnRemoval

CRITICALITY reject

}

xnSetup XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE XnSetupRequest

SUCCESSFUL OUTCOME XnSetupResponse

UNSUCCESSFUL OUTCOME XnSetupFailure

PROCEDURE CODE id-xnSetup

CRITICALITY reject

}

nGRANnodeConfigurationUpdate XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE NGRANNodeConfigurationUpdate

SUCCESSFUL OUTCOME NGRANNodeConfigurationUpdateAcknowledge

UNSUCCESSFUL OUTCOME NGRANNodeConfigurationUpdateFailure

PROCEDURE CODE id-nGRANnodeConfigurationUpdate

CRITICALITY reject

}

e-UTRA-NR-CellResourceCoordination XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE E-UTRA-NR-CellResourceCoordinationRequest

SUCCESSFUL OUTCOME E-UTRA-NR-CellResourceCoordinationResponse

PROCEDURE CODE id-e-UTRA-NR-CellResourceCoordination

CRITICALITY reject

}

cellActivation XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE CellActivationRequest

SUCCESSFUL OUTCOME CellActivationResponse

UNSUCCESSFUL OUTCOME CellActivationFailure

PROCEDURE CODE id-cellActivation

CRITICALITY reject

}

reset XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ResetRequest

SUCCESSFUL OUTCOME ResetResponse

PROCEDURE CODE id-reset

CRITICALITY reject

}

errorIndication XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ErrorIndication

PROCEDURE CODE id-errorIndication

CRITICALITY ignore

}

notificationControl XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE NotificationControlIndication

PROCEDURE CODE id-notificationControl

CRITICALITY ignore

}

activityNotification XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ActivityNotification

PROCEDURE CODE id-activityNotification

CRITICALITY ignore

}

privateMessage XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PrivateMessage

PROCEDURE CODE id-privateMessage

CRITICALITY ignore

}

secondaryRATDataUsageReport XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SecondaryRATDataUsageReport

PROCEDURE CODE id-secondaryRATDataUsageReport

CRITICALITY reject

}

deactivateTrace XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE DeactivateTrace

PROCEDURE CODE id-deactivateTrace

CRITICALITY ignore

}

traceStart XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE TraceStart

PROCEDURE CODE id-traceStart

CRITICALITY ignore

}

handoverSuccess XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE HandoverSuccess

PROCEDURE CODE id-handoverSuccess

CRITICALITY ignore

}

conditionalHandoverCancel XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ConditionalHandoverCancel

PROCEDURE CODE id-conditionalHandoverCancel

CRITICALITY ignore

}

earlyStatusTransfer XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE EarlyStatusTransfer

PROCEDURE CODE id-earlyStatusTransfer

CRITICALITY ignore

}

failureIndication XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE FailureIndication

PROCEDURE CODE id-failureIndication

CRITICALITY ignore

}

handoverReport XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE HandoverReport

PROCEDURE CODE id-handoverReport

CRITICALITY ignore

}

resourceStatusReportingInitiation XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ResourceStatusRequest

SUCCESSFUL OUTCOME ResourceStatusResponse

UNSUCCESSFUL OUTCOME ResourceStatusFailure

PROCEDURE CODE id-resourceStatusReportingInitiation

CRITICALITY reject

}

resourceStatusReporting XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ResourceStatusUpdate

PROCEDURE CODE id-resourceStatusReporting

CRITICALITY ignore

}

mobilitySettingsChange XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE MobilityChangeRequest

SUCCESSFUL OUTCOME MobilityChangeAcknowledge

UNSUCCESSFUL OUTCOME MobilityChangeFailure

PROCEDURE CODE id-mobilitySettingsChange

CRITICALITY reject

}

accessAndMobilityIndication XNAP-ELEMENTARY-PROCEDURE ::={

INITIATING MESSAGE AccessAndMobilityIndication

PROCEDURE CODE id-accessAndMobilityIndication

CRITICALITY ignore

}

f1CTrafficTransfer XNAP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE F1CTrafficTransfer

PROCEDURE CODE id-f1CTrafficTransfer

CRITICALITY ignore

}

iABTransportMigrationManagement XNAP-ELEMENTARY-PROCEDURE ::={

INITIATING MESSAGE IABTransportMigrationManagementRequest

SUCCESSFUL OUTCOME IABTransportMigrationManagementResponse

PROCEDURE CODE id-iABTransportMigrationManagement

CRITICALITY reject

}

iABTransportMigrationModification XNAP-ELEMENTARY-PROCEDURE ::={

INITIATING MESSAGE IABTransportMigrationModificationRequest

SUCCESSFUL OUTCOME IABTransportMigrationModificationResponse

PROCEDURE CODE id-iABTransportMigrationModification

CRITICALITY reject

}

iABResourceCoordination XNAP-ELEMENTARY-PROCEDURE ::={

INITIATING MESSAGE IABResourceCoordinationRequest

SUCCESSFUL OUTCOME IABResourceCoordinationResponse

PROCEDURE CODE id-iABResourceCoordination

CRITICALITY reject

}

END

-- ASN1STOP

9.3.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for XnAP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

ActivationIDforCellActivation,

AMF-Region-Information,

AMF-UE-NGAP-ID,

AS-SecurityInformation,

AssistanceDataForRANPaging,

BitRate,

Cause,

CellAndCapacityAssistanceInfo-EUTRA,

CellAndCapacityAssistanceInfo-NR,

CellAssistanceInfo-EUTRA,

CellAssistanceInfo-NR,

CHOinformation-Req,

CHOinformation-Ack,

CHO-MRDC-EarlyDataForwarding,

CHO-MRDC-Indicator,

CPTransportLayerInformation,

TNLA-To-Add-List,

TNLA-To-Update-List,

TNLA-To-Remove-List,

TNLA-Setup-List,

TNLA-Failed-To-Setup-List,

CriticalityDiagnostics,

XnUAddressInfoperPDUSession-List,

DAPSResponseInfo-List,

DataTrafficResourceIndication,

DeliveryStatus,

DesiredActNotificationLevel,

DRB-ID,

DRB-List,

DRB-Number,

DRBsSubjectToDLDiscarding-List,

DRBsSubjectToEarlyStatusTransfer-List,

DRBsSubjectToStatusTransfer-List,

DRBToQoSFlowMapping-List,

E-UTRA-CGI,

ExpectedUEActivityBehaviour,

ExpectedUEBehaviour,

ExtendedUEIdentityIndexValue,

FiveGCMobilityRestrictionListContainer,

GlobalCell-ID,

GlobalNG-RANNode-ID,

GlobalNG-RANCell-ID,

GUAMI,

InterfaceInstanceIndication,

I-RNTI,

LocationInformationSNReporting,

LocationReportingInformation,

LowerLayerPresenceStatusChange,

LTEUESidelinkAggregateMaximumBitRate,

LTEV2XServicesAuthorized,

MR-DC-ResourceCoordinationInfo,

ServedCells-E-UTRA,

ServedCells-NR,

ServedCellsToUpdate-E-UTRA,

ServedCellsToUpdate-NR,

MAC-I,

MaskedIMEISV,

MDT-Configuration,

MDTPLMNList,

MobilityRestrictionList,

NG-RAN-Cell-Identity,

NG-RANnodeUEXnAPID,

NR-CGI,

NE-DC-TDM-Pattern,

NRUESidelinkAggregateMaximumBitRate,

NRV2XServicesAuthorized,

PagingDRX,

PagingeDRXInformation,

PagingPriority,

PartialListIndicator,

PLMN-Identity,

PDCPChangeIndication,

PDUSessionAggregateMaximumBitRate,

PDUSession-ID,

PDUSession-List,

PDUSession-List-withCause,

PDUSession-List-withDataForwardingFromTarget,

PDUSession-List-withDataForwardingRequest,

PDUSessionResourcesAdmitted-List,

PDUSessionResourcesNotAdmitted-List,

PDUSessionResourcesToBeSetup-List,

PDUSessionResourceChangeRequiredInfo-SNterminated,

PDUSessionResourceChangeRequiredInfo-MNterminated,

PDUSessionResourceChangeConfirmInfo-SNterminated,

PDUSessionResourceChangeConfirmInfo-MNterminated,

PDUSessionResourceSecondaryRATUsageList,

PDUSessionResourceSetupInfo-SNterminated,

PDUSessionResourceSetupInfo-MNterminated,

PDUSessionResourceSetupResponseInfo-SNterminated,

PDUSessionResourceSetupResponseInfo-MNterminated,

PDUSessionResourceModificationInfo-SNterminated,

PDUSessionResourceModificationInfo-MNterminated,

PDUSessionResourceModificationResponseInfo-SNterminated,

PDUSessionResourceModificationResponseInfo-MNterminated,

PDUSessionResourceModConfirmInfo-SNterminated,

PDUSessionResourceModConfirmInfo-MNterminated,

PDUSessionResourceModRqdInfo-SNterminated,

PDUSessionResourceModRqdInfo-MNterminated,

PDUSessionType,

PC5QoSParameters,

QoSFlowIdentifier,

QoSFlowNotificationControlIndicationInfo,

QoSFlows-List,

RANPagingArea,

ResetRequestTypeInfo,

ResetResponseTypeInfo,

RFSP-Index,

RRCConfigIndication,

RRCResumeCause,

SCGConfigurationQuery,

SecurityIndication,

S-NG-RANnode-SecurityKey,

SpectrumSharingGroupID,

SplitSRBsTypes,

S-NG-RANnode-Addition-Trigger-Ind,

S-NSSAI,

TargetCellList,

TAISupport-List,

Target-CGI,

TimeToWait,

TraceActivation,

UEAggregateMaximumBitRate,

UEContextID,

UEContextInfoRetrUECtxtResp,

UEContextKeptIndicator,

UEHistoryInformation,

UEIdentityIndexValue,

UERadioCapabilityForPaging,

UERadioCapabilityID,

UERANPagingIdentity,

UESecurityCapabilities,

UPTransportLayerInformation,

UserPlaneTrafficActivityReport,

XnBenefitValue,

RANPagingFailure,

TNLConfigurationInfo,

MaximumCellListSize,

MessageOversizeNotification,

NG-RANTraceID,

MobilityInformation,

InitiatingCondition-FailureIndication,

HandoverReportType,

TargetCellinEUTRAN,

C-RNTI,

UERLFReportContainer,

Measurement-ID,

RegistrationRequest,

ReportCharacteristics,

CellToReport,

ReportingPeriodicity,

CellMeasurementResult,

UEHistoryInformationFromTheUE,

MobilityParametersInformation,

MobilityParametersModificationRange,

RACHReportInformation,

IABNodeIndication,

SNTriggered,

SCGIndicator,

UESpecificDRX,

F1CTrafficContainer,

NoPDUSessionIndication,

IAB-TNL-Address-Request,

IAB-TNL-Address-Response,

TrafficIndex,

TrafficProfile,

TrafficToBeReleaseInformation,

F1-TerminatingTopologyBHInformation,

Non-F1-TerminatingTopologyBHInformation,

BHInfoList,

IABTNLAddress,

IABCellInformation,

IABTNLAddressException

FROM XnAP-IEs

PrivateIE-Container{},

ProtocolExtensionContainer{},

ProtocolIE-Container{},

ProtocolIE-ContainerList{},

ProtocolIE-ContainerPair{},

ProtocolIE-ContainerPairList{},

ProtocolIE-Single-Container{},

XNAP-PRIVATE-IES,

XNAP-PROTOCOL-EXTENSION,

XNAP-PROTOCOL-IES,

XNAP-PROTOCOL-IES-PAIR

FROM XnAP-Containers

id-ActivatedServedCells,

id-ActivationIDforCellActivation,

id-AdditionalDRBIDs,

id-AMF-Region-Information,

id-AMF-Region-Information-To-Add,

id-AMF-Region-Information-To-Delete,

id-AssistanceDataForRANPaging,

id-AvailableDRBIDs,

id-Cause,

id-cellAssistanceInfo-EUTRA,

id-cellAssistanceInfo-NR,

id-CellAndCapacityAssistanceInfo-EUTRA,

id-CellAndCapacityAssistanceInfo-NR,

id-ConfigurationUpdateInitiatingNodeChoice,

id-UEContextID,

id-CriticalityDiagnostics,

id-XnUAddressInfoperPDUSession-List,

id-DesiredActNotificationLevel,

id-DRBsSubjectToStatusTransfer-List,

id-ExpectedUEBehaviour,

id-ExtendedUEIdentityIndexValue,

id-FiveGCMobilityRestrictionListContainer,

id-GlobalNG-RAN-node-ID,

id-GUAMI,

id-indexToRatFrequSelectionPriority,

id-List-of-served-cells-E-UTRA,

id-List-of-served-cells-NR,

id-LocationInformationSN,

id-LocationInformationSNReporting,

id-LocationReportingInformation,

id-LTEUESidelinkAggregateMaximumBitRate,

id-LTEV2XServicesAuthorized,

id-MAC-I,

id-MaskedIMEISV,

id-MDT-Configuration,

id-MDTPLMNList,

id-MN-to-SN-Container,

id-MobilityRestrictionList,

id-M-NG-RANnodeUEXnAPID,

id-new-NG-RAN-Cell-Identity,

id-newNG-RANnodeUEXnAPID,

id-NRUESidelinkAggregateMaximumBitRate,

id-NRV2XServicesAuthorized,

id-oldNG-RANnodeUEXnAPID,

id-OldtoNewNG-RANnodeResumeContainer,

id-PagingDRX,

id-PagingeDRXInformation,

id-PagingPriority,

id-PartialListIndicator-EUTRA,

id-PartialListIndicator-NR,

id-PCellID,

id-PDUSessionResourceSecondaryRATUsageList,

id-PDUSessionResourcesActivityNotifyList,

id-PDUSessionResourcesAdmitted-List,

id-PDUSessionResourcesNotAdmitted-List,

id-PDUSessionResourcesNotifyList,

id-PDUSessionToBeAddedAddReq,

id-PDUSessionToBeReleased-RelReqAck,

id-procedureStage,

id-RANPagingArea,

id-requestedSplitSRB,

id-RequiredNumberOfDRBIDs,

id-ResetRequestTypeInfo,

id-ResetResponseTypeInfo,

id-RespondingNodeTypeConfigUpdateAck,

id-RRCResumeCause,

id-selectedPLMN,

id-ServedCellsToActivate,

id-servedCellsToUpdate-E-UTRA,

id-ServedCellsToUpdateInitiatingNodeChoice,

id-servedCellsToUpdate-NR,

id-sourceNG-RANnodeUEXnAPID,

id-SpareDRBIDs,

id-S-NG-RANnodeMaxIPDataRate-UL,

id-S-NG-RANnodeMaxIPDataRate-DL,

id-S-NG-RANnodeUEXnAPID,

id-TAISupport-list,

id-Target2SourceNG-RANnodeTranspContainer,

id-targetCellGlobalID,

id-targetNG-RANnodeUEXnAPID,

id-TimeToWait,

id-TNLA-To-Add-List,

id-TNLA-To-Update-List,

id-TNLA-To-Remove-List,

id-TNLA-Setup-List,

id-TNLA-Failed-To-Setup-List,

id-TraceActivation,

id-UEContextInfoHORequest,

id-UEContextInfoRetrUECtxtResp,

id-UEContextKeptIndicator,

id-UEContextRefAtSN-HORequest,

id-UEHistoryInformation,

id-UEIdentityIndexValue,

id-UERANPagingIdentity,

id-UESecurityCapabilities,

id-UserPlaneTrafficActivityReport,

id-XnRemovalThreshold,

id-PDUSessionAdmittedAddedAddReqAck,

id-PDUSessionNotAdmittedAddReqAck,

id-SN-to-MN-Container,

id-RRCConfigIndication,

id-SplitSRB-RRCTransfer,

id-UEReportRRCTransfer,

id-PDUSessionReleasedList-RelConf,

id-BearersSubjectToCounterCheck,

id-PDUSessionToBeReleasedList-RelRqd,

id-ResponseInfo-ReconfCompl,

id-initiatingNodeType-ResourceCoordRequest,

id-respondingNodeType-ResourceCoordResponse,

id-PDUSessionToBeReleased-RelReq,

id-PDUSession-SNChangeRequired-List,

id-PDUSession-SNChangeConfirm-List,

id-PDCPChangeIndication,

id-PC5QoSParameters,

id-SCGConfigurationQuery,

id-UEContextInfo-SNModRequest,

id-requestedSplitSRBrelease,

id-PDUSessionAdmitted-SNModResponse,

id-PDUSessionNotAdmitted-SNModResponse,

id-admittedSplitSRB,

id-admittedSplitSRBrelease,

id-PDUSessionAdmittedModSNModConfirm,

id-PDUSessionReleasedSNModConfirm,

id-s-ng-RANnode-SecurityKey,

id-PDUSessionToBeModifiedSNModRequired,

id-S-NG-RANnodeUE-AMBR,

id-PDUSessionToBeReleasedSNModRequired,

id-target-S-NG-RANnodeID,

id-S-NSSAI,

id-MR-DC-ResourceCoordinationInfo,

id-RANPagingFailure,

id-UERadioCapabilityForPaging,

id-PDUSessionDataForwarding-SNModResponse,

id-Secondary-MN-Xn-U-TNLInfoatM,

id-NE-DC-TDM-Pattern,

id-InterfaceInstanceIndication,

id-S-NG-RANnode-Addition-Trigger-Ind,

id-SNTriggered,

id-DRBs-transferred-to-MN,

id-TNLConfigurationInfo,

id-MessageOversizeNotification,

id-NG-RANTraceID,

id-FastMCGRecoveryRRCTransfer-SN-to-MN,

id-FastMCGRecoveryRRCTransfer-MN-to-SN,

id-RequestedFastMCGRecoveryViaSRB3,

id-AvailableFastMCGRecoveryViaSRB3,

id-RequestedFastMCGRecoveryViaSRB3Release,

id-ReleaseFastMCGRecoveryViaSRB3,

id-CHOinformation-Req,

id-CHOinformation-Ack,

id-targetCellsToCancel,

id-requestedTargetCellGlobalID,

id-DAPSResponseInfo-List,

id-CHO-MRDC-EarlyDataForwarding,

id-CHO-MRDC-Indicator,

id-MobilityInformation,

id-InitiatingCondition-FailureIndication,

id-UEHistoryInformationFromTheUE,

id-HandoverReportType,

id-HandoverCause,

id-SourceCellCGI,

id-TargetCellCGI,

id-ReEstablishmentCellCGI,

id-TargetCellinEUTRAN,

id-SourceCellCRNTI,

id-UERLFReportContainer,

id-NGRAN-Node1-Measurement-ID,

id-NGRAN-Node2-Measurement-ID,

id-RegistrationRequest,

id-ReportCharacteristics,

id-CellToReport,

id-ReportingPeriodicity,

id-CellMeasurementResult,

id-NG-RANnode1CellID,

id-NG-RANnode2CellID,

id-NG-RANnode1MobilityParameters,

id-NG-RANnode2ProposedMobilityParameters,

id-MobilityParametersModificationRange,

id-RACHReportInformation,

id-IABNodeIndication,

id-UERadioCapabilityID,

id-SCGIndicator,

id-UESpecificDRX,

id-PDUSessionExpectedUEActivityBehaviour,

id-F1CTrafficContainer,

id-NoPDUSessionIndication,

id-F1-Terminating-DonorUEXnAPID,

id-nonF1-Terminating-DonorUEXnAPID,

id-IAB-TNL-Address-Request,

id-IAB-TNL-Address-Response,

id-TrafficToBeAddedList,

id-TrafficToBeModifiedList,

id-TrafficToBeReleaseInformation,

id-TrafficAddedList,

id-TrafficModifiedList,

id-TrafficNotAddedList,

id-TrafficNotModifiedList,

id-TrafficRequiredToBeModifiedList,

id-TrafficRequiredModifiedList,

id-TrafficReleasedList,

id-IABTNLAddressToBeAdded,

id-IABTNLAddressToBeReleasedList, id-BoundaryNodeCellsList,

id-ParentNodeCellsList,

id-IABTNLAddressException,

maxnoofCellsinNG-RANnode,

maxnoofDRBs,

maxnoofPDUSessions,

maxnoofQoSFlows, maxnoofServedCellsIAB,

maxnoofTrafficIndexEntries,

maxnoofTLAsIAB,

maxnoofBAPControlPDURLCCHs, maxnoofServingCells

FROM XnAP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- HANDOVER REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

HandoverRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{HandoverRequest-IEs}},

...

}

HandoverRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY reject TYPE Cause PRESENCE mandatory}|

{ ID id-targetCellGlobalID CRITICALITY reject TYPE Target-CGI PRESENCE mandatory}|

{ ID id-GUAMI CRITICALITY reject TYPE GUAMI PRESENCE mandatory}|

{ ID id-UEContextInfoHORequest CRITICALITY reject TYPE UEContextInfoHORequest PRESENCE mandatory}|

{ ID id-TraceActivation CRITICALITY ignore TYPE TraceActivation PRESENCE optional }|

{ ID id-MaskedIMEISV CRITICALITY ignore TYPE MaskedIMEISV PRESENCE optional }|

{ ID id-UEHistoryInformation CRITICALITY ignore TYPE UEHistoryInformation PRESENCE mandatory}|

{ ID id-UEContextRefAtSN-HORequest CRITICALITY ignore TYPE UEContextRefAtSN-HORequest PRESENCE optional }|

{ ID id-CHOinformation-Req CRITICALITY reject TYPE CHOinformation-Req PRESENCE optional }|

{ ID id-NRV2XServicesAuthorized CRITICALITY ignore TYPE NRV2XServicesAuthorized PRESENCE optional }|

{ ID id-LTEV2XServicesAuthorized CRITICALITY ignore TYPE LTEV2XServicesAuthorized PRESENCE optional }|

{ ID id-PC5QoSParameters CRITICALITY ignore TYPE PC5QoSParameters PRESENCE optional }|

{ ID id-MobilityInformation CRITICALITY ignore TYPE MobilityInformation PRESENCE optional}|

{ ID id-UEHistoryInformationFromTheUE CRITICALITY ignore TYPE UEHistoryInformationFromTheUE PRESENCE optional }|

{ ID id-IABNodeIndication CRITICALITY reject TYPE IABNodeIndication PRESENCE optional}|

{ ID id-NoPDUSessionIndication CRITICALITY ignore TYPE NoPDUSessionIndication PRESENCE optional},

...

}

UEContextInfoHORequest ::= SEQUENCE {

ng-c-UE-reference AMF-UE-NGAP-ID,

cp-TNL-info-source CPTransportLayerInformation,

ueSecurityCapabilities UESecurityCapabilities,

securityInformation AS-SecurityInformation,

indexToRatFrequencySelectionPriority RFSP-Index OPTIONAL,

ue-AMBR UEAggregateMaximumBitRate,

pduSessionResourcesToBeSetup-List PDUSessionResourcesToBeSetup-List,

rrc-Context OCTET STRING,

locationReportingInformation LocationReportingInformation OPTIONAL,

mrl MobilityRestrictionList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {UEContextInfoHORequest-ExtIEs} } OPTIONAL,

...

}

UEContextInfoHORequest-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

{ ID id-FiveGCMobilityRestrictionListContainer CRITICALITY ignore EXTENSION FiveGCMobilityRestrictionListContainer PRESENCE optional }|

{ ID id-NRUESidelinkAggregateMaximumBitRate CRITICALITY ignore EXTENSION NRUESidelinkAggregateMaximumBitRate PRESENCE optional }|

{ ID id-LTEUESidelinkAggregateMaximumBitRate CRITICALITY ignore EXTENSION LTEUESidelinkAggregateMaximumBitRate PRESENCE optional }|

{ ID id-MDTPLMNList CRITICALITY ignore EXTENSION MDTPLMNList PRESENCE optional }|

{ ID id-UERadioCapabilityID CRITICALITY reject EXTENSION UERadioCapabilityID PRESENCE optional },

...

}

UEContextRefAtSN-HORequest ::= SEQUENCE {

globalNG-RANNode-ID GlobalNG-RANNode-ID,

sN-NG-RANnodeUEXnAPID NG-RANnodeUEXnAPID,

iE-Extensions ProtocolExtensionContainer { {UEContextRefAtSN-HORequest-ExtIEs} } OPTIONAL,

...

}

UEContextRefAtSN-HORequest-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- HANDOVER REQUEST ACKNOWLEDGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

HandoverRequestAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{HandoverRequestAcknowledge-IEs}},

...

}

HandoverRequestAcknowledge-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-targetNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSessionResourcesAdmitted-List CRITICALITY ignore TYPE PDUSessionResourcesAdmitted-List PRESENCE mandatory}|

{ ID id-PDUSessionResourcesNotAdmitted-List CRITICALITY ignore TYPE PDUSessionResourcesNotAdmitted-List PRESENCE optional }|

{ ID id-Target2SourceNG-RANnodeTranspContainer CRITICALITY ignore TYPE OCTET STRING PRESENCE mandatory}|

{ ID id-UEContextKeptIndicator CRITICALITY ignore TYPE UEContextKeptIndicator PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-DRBs-transferred-to-MN CRITICALITY ignore TYPE DRB-List PRESENCE optional }|

{ ID id-DAPSResponseInfo-List CRITICALITY reject TYPE DAPSResponseInfo-List PRESENCE optional }|

{ ID id-CHOinformation-Ack CRITICALITY reject TYPE CHOinformation-Ack PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- HANDOVER PREPARATION FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

HandoverPreparationFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{HandoverPreparationFailure-IEs}},

...

}

HandoverPreparationFailure-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-requestedTargetCellGlobalID CRITICALITY reject TYPE Target-CGI PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- SN STATUS TRANSFER

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNStatusTransfer ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{SNStatusTransfer-IEs}},

...

}

SNStatusTransfer-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-targetNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-DRBsSubjectToStatusTransfer-List CRITICALITY ignore TYPE DRBsSubjectToStatusTransfer-List PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- UE CONTEXT RELEASE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UEContextRelease ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{UEContextRelease-IEs}},

...

}

UEContextRelease-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-targetNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- HANDOVER CANCEL

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

HandoverCancel ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{HandoverCancel-IEs}},

...

}

HandoverCancel-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-targetNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE optional }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-targetCellsToCancel CRITICALITY reject TYPE TargetCellList PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- HANDOVER SUCCESS

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

HandoverSuccess ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{HandoverSuccess-IEs}},

...

}

HandoverSuccess-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-targetNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-requestedTargetCellGlobalID CRITICALITY reject TYPE Target-CGI PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- CONDITIONAL HANDOVER CANCEL

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ConditionalHandoverCancel ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ ConditionalHandoverCancel-IEs}},

...

}

ConditionalHandoverCancel-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-targetNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-targetCellsToCancel CRITICALITY reject TYPE TargetCellList PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- EARLY STATUS TRANSFER

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

EarlyStatusTransfer ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ EarlyStatusTransfer-IEs}},

...

}

EarlyStatusTransfer-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-sourceNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-targetNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-procedureStage CRITICALITY reject TYPE ProcedureStageChoice PRESENCE mandatory},

...

}

ProcedureStageChoice ::= CHOICE {

first-dl-count FirstDLCount,

dl-discarding DLDiscarding,

choice-extension ProtocolIE-Single-Container { {ProcedureStageChoice-ExtIEs} }

}

ProcedureStageChoice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

FirstDLCount ::= SEQUENCE {

dRBsSubjectToEarlyStatusTransfer DRBsSubjectToEarlyStatusTransfer-List,

iE-Extension ProtocolExtensionContainer { {FirstDLCount-ExtIEs} } OPTIONAL,

...

}

FirstDLCount-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DLDiscarding ::= SEQUENCE {

dRBsSubjectToDLDiscarding DRBsSubjectToDLDiscarding-List,

iE-Extension ProtocolExtensionContainer { {DLDiscarding-ExtIEs} } OPTIONAL,

...

}

DLDiscarding-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RAN PAGING

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

RANPaging ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{RANPaging-IEs}},

...

}

RANPaging-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-UEIdentityIndexValue CRITICALITY reject TYPE UEIdentityIndexValue PRESENCE mandatory}|

{ ID id-UERANPagingIdentity CRITICALITY ignore TYPE UERANPagingIdentity PRESENCE mandatory}|

{ ID id-PagingDRX CRITICALITY ignore TYPE PagingDRX PRESENCE mandatory}|

{ ID id-RANPagingArea CRITICALITY reject TYPE RANPagingArea PRESENCE mandatory}|

{ ID id-PagingPriority CRITICALITY ignore TYPE PagingPriority PRESENCE optional }|

{ ID id-AssistanceDataForRANPaging CRITICALITY ignore TYPE AssistanceDataForRANPaging PRESENCE optional }|

{ ID id-UERadioCapabilityForPaging CRITICALITY ignore TYPE UERadioCapabilityForPaging PRESENCE optional }|

{ ID id-ExtendedUEIdentityIndexValue CRITICALITY ignore TYPE ExtendedUEIdentityIndexValue PRESENCE optional }|

{ ID id-PagingeDRXInformation CRITICALITY ignore TYPE PagingeDRXInformation PRESENCE optional }|

{ ID id-UESpecificDRX CRITICALITY ignore TYPE UESpecificDRX PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RETRIEVE UE CONTEXT REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

RetrieveUEContextRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{RetrieveUEContextRequest-IEs}},

...

}

RetrieveUEContextRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-newNG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-UEContextID CRITICALITY reject TYPE UEContextID PRESENCE mandatory}|

{ ID id-MAC-I CRITICALITY reject TYPE MAC-I PRESENCE mandatory}|

{ ID id-new-NG-RAN-Cell-Identity CRITICALITY reject TYPE NG-RAN-Cell-Identity PRESENCE mandatory}|

{ ID id-RRCResumeCause CRITICALITY ignore TYPE RRCResumeCause PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RETRIEVE UE CONTEXT RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

RetrieveUEContextResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ RetrieveUEContextResponse-IEs}},

...

}

RetrieveUEContextResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-newNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-oldNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-GUAMI CRITICALITY reject TYPE GUAMI PRESENCE mandatory}|

{ ID id-UEContextInfoRetrUECtxtResp CRITICALITY reject TYPE UEContextInfoRetrUECtxtResp PRESENCE mandatory}|

{ ID id-TraceActivation CRITICALITY ignore TYPE TraceActivation PRESENCE optional }|

{ ID id-MaskedIMEISV CRITICALITY ignore TYPE MaskedIMEISV PRESENCE optional }|

{ ID id-LocationReportingInformation CRITICALITY ignore TYPE LocationReportingInformation PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-NRV2XServicesAuthorized CRITICALITY ignore TYPE NRV2XServicesAuthorized PRESENCE optional}|

{ ID id-LTEV2XServicesAuthorized CRITICALITY ignore TYPE LTEV2XServicesAuthorized PRESENCE optional}|

{ ID id-PC5QoSParameters CRITICALITY ignore TYPE PC5QoSParameters PRESENCE optional }|

{ ID id-UEHistoryInformation CRITICALITY ignore TYPE UEHistoryInformation PRESENCE optional}|

{ ID id-UEHistoryInformationFromTheUE CRITICALITY ignore TYPE UEHistoryInformationFromTheUE PRESENCE optional }|

{ ID id-MDTPLMNList CRITICALITY ignore TYPE MDTPLMNList PRESENCE optional }|

{ ID id-IABNodeIndication CRITICALITY reject TYPE IABNodeIndication PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RETRIEVE UE CONTEXT FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

RetrieveUEContextFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ RetrieveUEContextFailure-IEs}},

...

}

RetrieveUEContextFailure-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-newNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-OldtoNewNG-RANnodeResumeContainer CRITICALITY ignore TYPE OCTET STRING PRESENCE optional }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- XN-U ADDRESS INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnUAddressIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ XnUAddressIndication-IEs}},

...

}

XnUAddressIndication-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-newNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-oldNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-XnUAddressInfoperPDUSession-List CRITICALITY reject TYPE XnUAddressInfoperPDUSession-List PRESENCE mandatory}|

{ ID id-CHO-MRDC-Indicator CRITICALITY reject TYPE CHO-MRDC-Indicator PRESENCE optional }|

{ ID id-CHO-MRDC-EarlyDataForwarding CRITICALITY ignore TYPE CHO-MRDC-EarlyDataForwarding PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE ADDITION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeAdditionRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeAdditionRequest-IEs}},

...

}

SNodeAdditionRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-UESecurityCapabilities CRITICALITY reject TYPE UESecurityCapabilities PRESENCE mandatory}|

{ ID id-s-ng-RANnode-SecurityKey CRITICALITY reject TYPE S-NG-RANnode-SecurityKey PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUE-AMBR CRITICALITY reject TYPE UEAggregateMaximumBitRate PRESENCE mandatory}|

{ ID id-selectedPLMN CRITICALITY ignore TYPE PLMN-Identity PRESENCE optional }|

{ ID id-MobilityRestrictionList CRITICALITY ignore TYPE MobilityRestrictionList PRESENCE optional }|

{ ID id-indexToRatFrequSelectionPriority CRITICALITY reject TYPE RFSP-Index PRESENCE optional }|

{ ID id-PDUSessionToBeAddedAddReq CRITICALITY reject TYPE PDUSessionToBeAddedAddReq PRESENCE mandatory}|

{ ID id-MN-to-SN-Container CRITICALITY reject TYPE OCTET STRING PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE optional }|

{ ID id-ExpectedUEBehaviour CRITICALITY ignore TYPE ExpectedUEBehaviour PRESENCE optional }|

{ ID id-requestedSplitSRB CRITICALITY reject TYPE SplitSRBsTypes PRESENCE optional }|

{ ID id-PCellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE optional }|

{ ID id-DesiredActNotificationLevel CRITICALITY ignore TYPE DesiredActNotificationLevel PRESENCE optional }|

{ ID id-AvailableDRBIDs CRITICALITY reject TYPE DRB-List PRESENCE conditional}

-- The IE shall be present if there is at least one PDUSessionResourceSetupInfo-SNterminated included --|

{ ID id-S-NG-RANnodeMaxIPDataRate-UL CRITICALITY reject TYPE BitRate PRESENCE optional }|

{ ID id-S-NG-RANnodeMaxIPDataRate-DL CRITICALITY reject TYPE BitRate PRESENCE optional }|

{ ID id-LocationInformationSNReporting CRITICALITY ignore TYPE LocationInformationSNReporting PRESENCE optional}|

{ ID id-MR-DC-ResourceCoordinationInfo CRITICALITY ignore TYPE MR-DC-ResourceCoordinationInfo PRESENCE optional }|

{ ID id-MaskedIMEISV CRITICALITY ignore TYPE MaskedIMEISV PRESENCE optional}|

{ ID id-NE-DC-TDM-Pattern CRITICALITY ignore TYPE NE-DC-TDM-Pattern PRESENCE optional}|

{ ID id-S-NG-RANnode-Addition-Trigger-Ind CRITICALITY reject TYPE S-NG-RANnode-Addition-Trigger-Ind PRESENCE optional}|

{ ID id-TraceActivation CRITICALITY ignore TYPE TraceActivation PRESENCE optional}|

{ ID id-RequestedFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE RequestedFastMCGRecoveryViaSRB3 PRESENCE optional}|

{ ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE optional}|

{ ID id-IABNodeIndication CRITICALITY reject TYPE IABNodeIndication PRESENCE optional}|

{ ID id-NoPDUSessionIndication CRITICALITY ignore TYPE NoPDUSessionIndication PRESENCE optional},

...

}

PDUSessionToBeAddedAddReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionToBeAddedAddReq-Item

PDUSessionToBeAddedAddReq-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

s-NSSAI S-NSSAI,

sN-PDUSessionAMBR PDUSessionAggregateMaximumBitRate OPTIONAL,

sn-terminated PDUSessionResourceSetupInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceSetupInfo-MNterminated OPTIONAL,

-- NOTE: If neither the PDU Session Resource Setup Info – SN terminated IE

-- nor the *PDU Session Resource Setup Info – MN terminated* IE is present,

-- abnormal conditions as specified in clause 8.3.1.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSessionToBeAddedAddReq-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionToBeAddedAddReq-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RequestedFastMCGRecoveryViaSRB3 ::= ENUMERATED {true, ...}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE ADDITION REQUEST ACKNOWLEDGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeAdditionRequestAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeAdditionRequestAcknowledge-IEs}},

...

}

SNodeAdditionRequestAcknowledge-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSessionAdmittedAddedAddReqAck CRITICALITY ignore TYPE PDUSessionAdmittedAddedAddReqAck PRESENCE mandatory}|

{ ID id-PDUSessionNotAdmittedAddReqAck CRITICALITY ignore TYPE PDUSessionNotAdmittedAddReqAck PRESENCE optional }|

{ ID id-SN-to-MN-Container CRITICALITY reject TYPE OCTET STRING PRESENCE mandatory}|

{ ID id-admittedSplitSRB CRITICALITY reject TYPE SplitSRBsTypes PRESENCE optional }|

{ ID id-RRCConfigIndication CRITICALITY reject TYPE RRCConfigIndication PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-LocationInformationSN CRITICALITY ignore TYPE Target-CGI PRESENCE optional }|

{ ID id-MR-DC-ResourceCoordinationInfo CRITICALITY ignore TYPE MR-DC-ResourceCoordinationInfo PRESENCE optional }|

{ ID id-AvailableFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE AvailableFastMCGRecoveryViaSRB3 PRESENCE optional },

...

}

PDUSessionAdmittedAddedAddReqAck ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionAdmittedAddedAddReqAck-Item

PDUSessionAdmittedAddedAddReqAck-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

sn-terminated PDUSessionResourceSetupResponseInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceSetupResponseInfo-MNterminated OPTIONAL,

-- NOTE: If neither the *PDU Session Resource Setup Response Info – SN terminated* IE

-- nor the *PDU Session Resource Setup Response Info – MN terminated* IE is present,

-- abnormal conditions as specified in clause 8.3.1.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSessionAdmittedAddedAddReqAck-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionAdmittedAddedAddReqAck-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionNotAdmittedAddReqAck ::= SEQUENCE {

pduSessionResourcesNotAdmitted-SNterminated PDUSessionResourcesNotAdmitted-List OPTIONAL,

pduSessionResourcesNotAdmitted-MNterminated PDUSessionResourcesNotAdmitted-List OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSessionNotAdmittedAddReqAck-ExtIEs} } OPTIONAL,

...

}

PDUSessionNotAdmittedAddReqAck-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

AvailableFastMCGRecoveryViaSRB3 ::= ENUMERATED {true, ...}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE ADDITION REQUEST REJECT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeAdditionRequestReject ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeAdditionRequestReject-IEs}},

...

}

SNodeAdditionRequestReject-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE RECONFIGURATION COMPLETE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeReconfigurationComplete ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeReconfigurationComplete-IEs}},

...

}

SNodeReconfigurationComplete-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-ResponseInfo-ReconfCompl CRITICALITY ignore TYPE ResponseInfo-ReconfCompl PRESENCE mandatory},

...

}

ResponseInfo-ReconfCompl ::= SEQUENCE {

responseType-ReconfComplete ResponseType-ReconfComplete,

iE-Extensions ProtocolExtensionContainer { {ResponseInfo-ReconfCompl-ExtIEs} } OPTIONAL,

...

}

ResponseInfo-ReconfCompl-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResponseType-ReconfComplete ::= CHOICE {

configuration-successfully-applied Configuration-successfully-applied,

configuration-rejected-by-M-NG-RANNode Configuration-rejected-by-M-NG-RANNode,

choice-extension ProtocolIE-Single-Container { {ResponseType-ReconfComplete-ExtIEs} }

}

ResponseType-ReconfComplete-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

Configuration-successfully-applied ::= SEQUENCE {

m-NG-RANNode-to-S-NG-RANNode-Container OCTET STRING OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {Configuration-successfully-applied-ExtIEs} } OPTIONAL,

...

}

Configuration-successfully-applied-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

Configuration-rejected-by-M-NG-RANNode ::= SEQUENCE {

cause Cause,

m-NG-RANNode-to-S-NG-RANNode-Container OCTET STRING OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {Configuration-rejected-by-M-NG-RANNode-ExtIEs} } OPTIONAL,

...

}

Configuration-rejected-by-M-NG-RANNode-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE MODIFICATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeModificationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeModificationRequest-IEs}},

...

}

SNodeModificationRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-PDCPChangeIndication CRITICALITY ignore TYPE PDCPChangeIndication PRESENCE optional }|

{ ID id-selectedPLMN CRITICALITY ignore TYPE PLMN-Identity PRESENCE optional }|

{ ID id-MobilityRestrictionList CRITICALITY ignore TYPE MobilityRestrictionList PRESENCE optional }|

{ ID id-SCGConfigurationQuery CRITICALITY ignore TYPE SCGConfigurationQuery PRESENCE optional }|

{ ID id-UEContextInfo-SNModRequest CRITICALITY reject TYPE UEContextInfo-SNModRequest PRESENCE optional }|

{ ID id-MN-to-SN-Container CRITICALITY ignore TYPE OCTET STRING PRESENCE optional }|

{ ID id-requestedSplitSRB CRITICALITY ignore TYPE SplitSRBsTypes PRESENCE optional }|

{ ID id-requestedSplitSRBrelease CRITICALITY ignore TYPE SplitSRBsTypes PRESENCE optional }|

{ ID id-DesiredActNotificationLevel CRITICALITY ignore TYPE DesiredActNotificationLevel PRESENCE optional }|

{ ID id-AdditionalDRBIDs CRITICALITY reject TYPE DRB-List PRESENCE optional }|

{ ID id-S-NG-RANnodeMaxIPDataRate-UL CRITICALITY reject TYPE BitRate PRESENCE optional }|

{ ID id-S-NG-RANnodeMaxIPDataRate-DL CRITICALITY reject TYPE BitRate PRESENCE optional }|

{ ID id-LocationInformationSNReporting CRITICALITY ignore TYPE LocationInformationSNReporting PRESENCE optional}|

{ ID id-MR-DC-ResourceCoordinationInfo CRITICALITY ignore TYPE MR-DC-ResourceCoordinationInfo PRESENCE optional }|

{ ID id-PCellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE optional }|

{ ID id-NE-DC-TDM-Pattern CRITICALITY ignore TYPE NE-DC-TDM-Pattern PRESENCE optional}|

{ ID id-RequestedFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE RequestedFastMCGRecoveryViaSRB3 PRESENCE optional }|

{ ID id-RequestedFastMCGRecoveryViaSRB3Release CRITICALITY ignore TYPE RequestedFastMCGRecoveryViaSRB3Release PRESENCE optional }|

{ ID id-SNTriggered CRITICALITY ignore TYPE SNTriggered PRESENCE optional},

...

}

UEContextInfo-SNModRequest ::= SEQUENCE {

ueSecurityCapabilities UESecurityCapabilities OPTIONAL,

s-ng-RANnode-SecurityKey S-NG-RANnode-SecurityKey OPTIONAL,

s-ng-RANnodeUE-AMBR UEAggregateMaximumBitRate OPTIONAL,

indexToRatFrequencySelectionPriority RFSP-Index OPTIONAL,

lowerLayerPresenceStatusChange LowerLayerPresenceStatusChange OPTIONAL,

pduSessionResourceToBeAdded PDUSessionsToBeAdded-SNModRequest-List OPTIONAL,

pduSessionResourceToBeModified PDUSessionsToBeModified-SNModRequest-List OPTIONAL,

pduSessionResourceToBeReleased PDUSessionsToBeReleased-SNModRequest-List OPTIONAL,

iE-Extension ProtocolExtensionContainer { {UEContextInfo-SNModRequest-ExtIEs} } OPTIONAL,

...

}

UEContextInfo-SNModRequest-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionsToBeAdded-SNModRequest-List ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionsToBeAdded-SNModRequest-Item

PDUSessionsToBeAdded-SNModRequest-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

s-NSSAI S-NSSAI,

sN-PDUSessionAMBR PDUSessionAggregateMaximumBitRate OPTIONAL,

sn-terminated PDUSessionResourceSetupInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceSetupInfo-MNterminated OPTIONAL,

-- NOTE: If neither the *PDU Session Resource Setup Info – SN terminated* IE

-- nor the *PDU Session Resource Setup Info – MN terminated* IE is present,

-- abnormal conditions as specified in clause 8.3.3.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSessionsToBeAdded-SNModRequest-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionsToBeAdded-SNModRequest-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ID id-PDUSessionExpectedUEActivityBehaviour CRITICALITY ignore EXTENSION ExpectedUEActivityBehaviour PRESENCE optional},

...

}

PDUSessionsToBeModified-SNModRequest-List ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionsToBeModified-SNModRequest-Item

PDUSessionsToBeModified-SNModRequest-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

sN-PDUSessionAMBR PDUSessionAggregateMaximumBitRate OPTIONAL,

sn-terminated PDUSessionResourceModificationInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceModificationInfo-MNterminated OPTIONAL,

-- NOTE: If neither the *PDU Session Resource Modification Info – SN terminated* IE

-- nor the *PDU Session Resource Modification Info – MN terminated* IE is present,

-- abnormal conditions as specified in clause 8.3.3.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSessionsToBeModified-SNModRequest-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionsToBeModified-SNModRequest-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ID id-S-NSSAI CRITICALITY reject EXTENSION S-NSSAI PRESENCE optional}|

{ID id-PDUSessionExpectedUEActivityBehaviour CRITICALITY ignore EXTENSION ExpectedUEActivityBehaviour PRESENCE optional},

...

}

PDUSessionsToBeReleased-SNModRequest-List ::= SEQUENCE {

pdu-session-list PDUSession-List-withCause OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSessionsToBeReleased-SNModRequest-List-ExtIEs} } OPTIONAL,

...

}

PDUSessionsToBeReleased-SNModRequest-List-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RequestedFastMCGRecoveryViaSRB3Release ::= ENUMERATED {true, ...}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE MODIFICATION REQUEST ACKNOWLEDGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeModificationRequestAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeModificationRequestAcknowledge-IEs}},

...

}

SNodeModificationRequestAcknowledge-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSessionAdmitted-SNModResponse CRITICALITY ignore TYPE PDUSessionAdmitted-SNModResponse PRESENCE optional }|

{ ID id-PDUSessionNotAdmitted-SNModResponse CRITICALITY ignore TYPE PDUSessionNotAdmitted-SNModResponse PRESENCE optional }|

{ ID id-SN-to-MN-Container CRITICALITY ignore TYPE OCTET STRING PRESENCE optional }|

{ ID id-admittedSplitSRB CRITICALITY ignore TYPE SplitSRBsTypes PRESENCE optional }|

{ ID id-admittedSplitSRBrelease CRITICALITY ignore TYPE SplitSRBsTypes PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-LocationInformationSN CRITICALITY ignore TYPE Target-CGI PRESENCE optional }|

{ ID id-MR-DC-ResourceCoordinationInfo CRITICALITY ignore TYPE MR-DC-ResourceCoordinationInfo PRESENCE optional }|

{ ID id-PDUSessionDataForwarding-SNModResponse CRITICALITY ignore TYPE PDUSessionDataForwarding-SNModResponse PRESENCE optional }|

{ ID id-RRCConfigIndication CRITICALITY reject TYPE RRCConfigIndication PRESENCE optional }|

{ ID id-AvailableFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE AvailableFastMCGRecoveryViaSRB3 PRESENCE optional }|

{ ID id-ReleaseFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE ReleaseFastMCGRecoveryViaSRB3 PRESENCE optional },

...

}

PDUSessionAdmitted-SNModResponse ::= SEQUENCE {

pduSessionResourcesAdmittedToBeAdded PDUSessionAdmittedToBeAddedSNModResponse OPTIONAL,

pduSessionResourcesAdmittedToBeModified PDUSessionAdmittedToBeModifiedSNModResponse OPTIONAL,

pduSessionResourcesAdmittedToBeReleased PDUSessionAdmittedToBeReleasedSNModResponse OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSessionAdmitted-SNModResponse-ExtIEs} } OPTIONAL,

...

}

PDUSessionAdmitted-SNModResponse-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionAdmittedToBeAddedSNModResponse ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionAdmittedToBeAddedSNModResponse-Item

PDUSessionAdmittedToBeAddedSNModResponse-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

sn-terminated PDUSessionResourceSetupResponseInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceSetupResponseInfo-MNterminated OPTIONAL,

-- NOTE: If neither the *PDU Session Resource Setup Response Info – SN terminated* IE

-- nor the *PDU Session Resource Setup Response Info – MN terminated* IE is present,

-- abnormal conditions as specified in clause 8.3.3.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSessionAdmittedToBeAddedSNModResponse-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionAdmittedToBeAddedSNModResponse-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionAdmittedToBeModifiedSNModResponse::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionAdmittedToBeModifiedSNModResponse-Item

PDUSessionAdmittedToBeModifiedSNModResponse-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

sn-terminated PDUSessionResourceModificationResponseInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceModificationResponseInfo-MNterminated OPTIONAL,

-- NOTE: If neither the *PDU Session Resource Modification Response Info – SN terminated* IE

-- nor the *PDU Session Resource Modification Response Info – MN terminated* IE is present,

-- abnormal conditions as specified in clause 8.3.3.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSessionAdmittedToBeModifiedSNModResponse-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionAdmittedToBeModifiedSNModResponse-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionAdmittedToBeReleasedSNModResponse ::= SEQUENCE {

sn-terminated PDUSession-List-withDataForwardingRequest OPTIONAL,

mn-terminated PDUSession-List-withCause OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSessionAdmittedToBeReleasedSNModResponse-ExtIEs} } OPTIONAL,

...

}

PDUSessionAdmittedToBeReleasedSNModResponse-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionNotAdmitted-SNModResponse ::= SEQUENCE {

pdu-Session-List PDUSession-List OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSessionNotAdmitted-SNModResponse-ExtIEs} } OPTIONAL,

...

}

PDUSessionNotAdmitted-SNModResponse-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionDataForwarding-SNModResponse ::= SEQUENCE {

sn-terminated PDUSession-List-withDataForwardingRequest,

iE-Extensions ProtocolExtensionContainer { {PDUSessionDataForwarding-SNModResponse-ExtIEs} } OPTIONAL,

...

}

PDUSessionDataForwarding-SNModResponse-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ReleaseFastMCGRecoveryViaSRB3 ::= ENUMERATED {true, ...}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE MODIFICATION REQUEST REJECT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeModificationRequestReject ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeModificationRequestReject-IEs}},

...

}

SNodeModificationRequestReject-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE MODIFICATION REQUIRED

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeModificationRequired ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeModificationRequired-IEs}},

...

}

SNodeModificationRequired-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-PDCPChangeIndication CRITICALITY ignore TYPE PDCPChangeIndication PRESENCE optional }|

{ ID id-PDUSessionToBeModifiedSNModRequired CRITICALITY ignore TYPE PDUSessionToBeModifiedSNModRequired PRESENCE optional }|

{ ID id-PDUSessionToBeReleasedSNModRequired CRITICALITY ignore TYPE PDUSessionToBeReleasedSNModRequired PRESENCE optional }|

{ ID id-SN-to-MN-Container CRITICALITY ignore TYPE OCTET STRING PRESENCE optional }|

{ ID id-SpareDRBIDs CRITICALITY ignore TYPE DRB-List PRESENCE optional }|

{ ID id-RequiredNumberOfDRBIDs CRITICALITY ignore TYPE DRB-Number PRESENCE optional }|

{ ID id-LocationInformationSN CRITICALITY ignore TYPE Target-CGI PRESENCE optional }|

{ ID id-MR-DC-ResourceCoordinationInfo CRITICALITY ignore TYPE MR-DC-ResourceCoordinationInfo PRESENCE optional }|

{ ID id-RRCConfigIndication CRITICALITY reject TYPE RRCConfigIndication PRESENCE optional }|

{ ID id-AvailableFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE AvailableFastMCGRecoveryViaSRB3 PRESENCE optional }|

{ ID id-ReleaseFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE ReleaseFastMCGRecoveryViaSRB3 PRESENCE optional }|

{ ID id-SCGIndicator CRITICALITY ignore TYPE SCGIndicator PRESENCE optional },

...

}

PDUSessionToBeModifiedSNModRequired::= SEQUENCE (SIZE (1.. maxnoofPDUSessions)) OF PDUSessionToBeModifiedSNModRequired-Item

PDUSessionToBeModifiedSNModRequired-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

sn-terminated PDUSessionResourceModRqdInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceModRqdInfo-MNterminated OPTIONAL,

-- NOTE: If neither the *PDU Session Resource Modification Required Info – SN terminated* IE

-- nor the *PDU Session Resource Modification Required Info – MN terminated* IE is present,

-- abnormal conditions as specified in clause 8.3.4.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSessionToBeModifiedSNModRequired-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionToBeModifiedSNModRequired-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionToBeReleasedSNModRequired ::= SEQUENCE {

sn-terminated PDUSession-List-withDataForwardingRequest OPTIONAL,

mn-terminated PDUSession-List-withCause OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSessionToBeReleasedSNModRequired-ExtIEs} } OPTIONAL,

...

}

PDUSessionToBeReleasedSNModRequired-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE MODIFICATION CONFIRM

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeModificationConfirm ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeModificationConfirm-IEs}},

...

}

SNodeModificationConfirm-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSessionAdmittedModSNModConfirm CRITICALITY ignore TYPE PDUSessionAdmittedModSNModConfirm PRESENCE optional }|

{ ID id-PDUSessionReleasedSNModConfirm CRITICALITY ignore TYPE PDUSessionReleasedSNModConfirm PRESENCE optional }|

{ ID id-MN-to-SN-Container CRITICALITY ignore TYPE OCTET STRING PRESENCE optional }|

{ ID id-AdditionalDRBIDs CRITICALITY reject TYPE DRB-List PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-MR-DC-ResourceCoordinationInfo CRITICALITY ignore TYPE MR-DC-ResourceCoordinationInfo PRESENCE optional },

...

}

PDUSessionAdmittedModSNModConfirm ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionAdmittedModSNModConfirm-Item

PDUSessionAdmittedModSNModConfirm-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

sn-terminated PDUSessionResourceModConfirmInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceModConfirmInfo-MNterminated OPTIONAL,

-- NOTE: If neither the *PDU Session Resource Modification Confirm Info – SN terminated* IE

-- nor the *PDU Session Resource Modification Confirm Info – MN terminated* IE is present,

-- abnormal conditions as specified in clause 8.3.4.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSessionAdmittedModSNModConfirm-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionAdmittedModSNModConfirm-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionReleasedSNModConfirm ::= SEQUENCE {

sn-terminated PDUSession-List-withDataForwardingFromTarget OPTIONAL,

mn-terminated PDUSession-List OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSessionAdmittedToBeReleasedSNModConfirm-ExtIEs} } OPTIONAL,

...

}

PDUSessionAdmittedToBeReleasedSNModConfirm-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE MODIFICATION REFUSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeModificationRefuse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeModificationRefuse-IEs}},

...

}

SNodeModificationRefuse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-MN-to-SN-Container CRITICALITY ignore TYPE OCTET STRING PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE RELEASE REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeReleaseRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeReleaseRequest-IEs}},

...

}

SNodeReleaseRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE optional }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-PDUSessionToBeReleased-RelReq CRITICALITY ignore TYPE PDUSession-List-withCause PRESENCE mandatory}|

{ ID id-UEContextKeptIndicator CRITICALITY ignore TYPE UEContextKeptIndicator PRESENCE optional }|

{ ID id-MN-to-SN-Container CRITICALITY ignore TYPE OCTET STRING PRESENCE optional }|

{ ID id-DRBs-transferred-to-MN CRITICALITY ignore TYPE DRB-List PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE RELEASE REQUEST ACKNOWLEDGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeReleaseRequestAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeReleaseRequestAcknowledge-IEs}},

...

}

SNodeReleaseRequestAcknowledge-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE optional }|

{ ID id-PDUSessionToBeReleased-RelReqAck CRITICALITY ignore TYPE PDUSessionToBeReleasedList-RelReqAck PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

PDUSessionToBeReleasedList-RelReqAck ::= SEQUENCE {

pduSessionsToBeReleasedList-SNterminated PDUSession-List-withDataForwardingRequest OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionToBeReleasedList-RelReqAck-ExtIEs} } OPTIONAL,

...

}

PDUSessionToBeReleasedList-RelReqAck-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE RELEASE REJECT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeReleaseReject ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeReleaseReject-IEs}},

...

}

SNodeReleaseReject-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE optional }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE RELEASE REQUIRED

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeReleaseRequired ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeReleaseRequired-IEs}},

...

}

SNodeReleaseRequired-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSessionToBeReleasedList-RelRqd CRITICALITY ignore TYPE PDUSessionToBeReleasedList-RelRqd PRESENCE optional }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-SN-to-MN-Container CRITICALITY ignore TYPE OCTET STRING PRESENCE optional },

...

}

PDUSessionToBeReleasedList-RelRqd ::= SEQUENCE {

pduSessionsToBeReleasedList-SNterminated PDUSession-List-withDataForwardingRequest OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionToBeReleasedList-RelRqd-ExtIEs} } OPTIONAL,

...

}

PDUSessionToBeReleasedList-RelRqd-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE RELEASE CONFIRM

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeReleaseConfirm ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeReleaseConfirm-IEs}},

...

}

SNodeReleaseConfirm-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSessionReleasedList-RelConf CRITICALITY ignore TYPE PDUSessionReleasedList-RelConf PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

PDUSessionReleasedList-RelConf ::= SEQUENCE {

pduSessionsReleasedList-SNterminated PDUSession-List-withDataForwardingFromTarget OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionReleasedList-RelConf-ExtIEs} } OPTIONAL,

...

}

PDUSessionReleasedList-RelConf-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE COUNTER CHECK REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeCounterCheckRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeCounterCheckRequest-IEs}},

...

}

SNodeCounterCheckRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-BearersSubjectToCounterCheck CRITICALITY ignore TYPE BearersSubjectToCounterCheck-List PRESENCE mandatory},

...

}

BearersSubjectToCounterCheck-List ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF BearersSubjectToCounterCheck-Item

BearersSubjectToCounterCheck-Item ::= SEQUENCE {

drb-ID DRB-ID,

ul-count INTEGER (0.. 4294967295),

dl-count INTEGER (0.. 4294967295),

iE-Extensions ProtocolExtensionContainer { {BearersSubjectToCounterCheck-Item-ExtIEs} } OPTIONAL,

...

}

BearersSubjectToCounterCheck-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE CHANGE REQUIRED

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeChangeRequired ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeChangeRequired-IEs}},

...

}

SNodeChangeRequired-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-target-S-NG-RANnodeID CRITICALITY reject TYPE GlobalNG-RANNode-ID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-PDUSession-SNChangeRequired-List CRITICALITY ignore TYPE PDUSession-SNChangeRequired-List PRESENCE optional }|

{ ID id-SN-to-MN-Container CRITICALITY reject TYPE OCTET STRING PRESENCE mandatory},

...

}

PDUSession-SNChangeRequired-List ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSession-SNChangeRequired-Item

PDUSession-SNChangeRequired-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

sn-terminated PDUSessionResourceChangeRequiredInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceChangeRequiredInfo-MNterminated OPTIONAL,

-- NOTE: If the *PDU Session Resource Change Required Info – SN terminated* IE is not present,

-- abnormal conditions as specified in clause 8.3.5.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSession-SNChangeRequired-Item-ExtIEs} } OPTIONAL,

...

}

PDUSession-SNChangeRequired-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE CHANGE CONFIRM

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeChangeConfirm ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeChangeConfirm-IEs}},

...

}

SNodeChangeConfirm-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSession-SNChangeConfirm-List CRITICALITY ignore TYPE PDUSession-SNChangeConfirm-List PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

PDUSession-SNChangeConfirm-List ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSession-SNChangeConfirm-Item

PDUSession-SNChangeConfirm-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

sn-terminated PDUSessionResourceChangeConfirmInfo-SNterminated OPTIONAL,

mn-terminated PDUSessionResourceChangeConfirmInfo-MNterminated OPTIONAL,

-- NOTE: If the *PDU Session Resource Change Confirm Info – SN terminated* IE is not present,

-- abnormal conditions as specified in clause 8.3.5.4 apply.

iE-Extension ProtocolExtensionContainer { {PDUSession-SNChangeConfirm-Item-ExtIEs} } OPTIONAL,

...

}

PDUSession-SNChangeConfirm-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE CHANGE REFUSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeChangeRefuse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ SNodeChangeRefuse-IEs}},

...

}

SNodeChangeRefuse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RRC TRANSFER

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

RRCTransfer ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ RRCTransfer-IEs}},

...

}

RRCTransfer-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-SplitSRB-RRCTransfer CRITICALITY reject TYPE SplitSRB-RRCTransfer PRESENCE optional }|

{ ID id-UEReportRRCTransfer CRITICALITY reject TYPE UEReportRRCTransfer PRESENCE optional }|

{ ID id-FastMCGRecoveryRRCTransfer-SN-to-MN CRITICALITY ignore TYPE FastMCGRecoveryRRCTransfer PRESENCE optional}|

{ ID id-FastMCGRecoveryRRCTransfer-MN-to-SN CRITICALITY ignore TYPE FastMCGRecoveryRRCTransfer PRESENCE optional},

...

}

SplitSRB-RRCTransfer ::= SEQUENCE {

rrcContainer OCTET STRING OPTIONAL,

srbType ENUMERATED {srb1, srb2, ...},

deliveryStatus DeliveryStatus OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {SplitSRB-RRCTransfer-ExtIEs} } OPTIONAL,

...

}

SplitSRB-RRCTransfer-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

UEReportRRCTransfer::= SEQUENCE {

rrcContainer OCTET STRING,

iE-Extensions ProtocolExtensionContainer { {UEReportRRCTransfer-ExtIEs} } OPTIONAL,

...

}

UEReportRRCTransfer-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

FastMCGRecoveryRRCTransfer::= SEQUENCE {

rrcContainer OCTET STRING,

iE-Extensions ProtocolExtensionContainer { { FastMCGRecoveryRRCTransfer-ExtIEs} } OPTIONAL,

...

}

FastMCGRecoveryRRCTransfer-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- NOTIFICATION CONTROL INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NotificationControlIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{NotificationControlIndication-IEs}},

...

}

NotificationControlIndication-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSessionResourcesNotifyList CRITICALITY reject TYPE PDUSessionResourcesNotifyList PRESENCE optional },

...

}

PDUSessionResourcesNotifyList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourcesNotify-Item

PDUSessionResourcesNotify-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

qosFlowsNotificationContrIndInfo QoSFlowNotificationControlIndicationInfo,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourcesNotify-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourcesNotify-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- ACTIVITY NOTIFICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ActivityNotification ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ActivityNotification-IEs}},

...

}

ActivityNotification-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-UserPlaneTrafficActivityReport CRITICALITY ignore TYPE UserPlaneTrafficActivityReport PRESENCE optional }|

{ ID id-PDUSessionResourcesActivityNotifyList CRITICALITY ignore TYPE PDUSessionResourcesActivityNotifyList PRESENCE optional }|

{ ID id-RANPagingFailure CRITICALITY ignore TYPE RANPagingFailure PRESENCE optional },

...

}

PDUSessionResourcesActivityNotifyList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourcesActivityNotify-Item

PDUSessionResourcesActivityNotify-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

pduSessionLevelUPactivityreport UserPlaneTrafficActivityReport OPTIONAL,

qosFlowsActivityNotifyList QoSFlowsActivityNotifyList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourcesActivityNotify-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourcesActivityNotify-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

QoSFlowsActivityNotifyList ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF QoSFlowsActivityNotifyItem

QoSFlowsActivityNotifyItem ::= SEQUENCE {

qosFlowIdentifier QoSFlowIdentifier,

pduSessionLevelUPactivityreport UserPlaneTrafficActivityReport,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsActivityNotifyItem-ExtIEs} } OPTIONAL,

...

}

QoSFlowsActivityNotifyItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- XN SETUP REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnSetupRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ XnSetupRequest-IEs}},

...

}

XnSetupRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-GlobalNG-RAN-node-ID CRITICALITY reject TYPE GlobalNG-RANNode-ID PRESENCE mandatory}|

{ ID id-TAISupport-list CRITICALITY reject TYPE TAISupport-List PRESENCE mandatory}|

{ ID id-AMF-Region-Information CRITICALITY reject TYPE AMF-Region-Information PRESENCE mandatory}|

{ ID id-List-of-served-cells-NR CRITICALITY reject TYPE ServedCells-NR PRESENCE optional }|

{ ID id-List-of-served-cells-E-UTRA CRITICALITY reject TYPE ServedCells-E-UTRA PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional }|

{ ID id-TNLConfigurationInfo CRITICALITY ignore TYPE TNLConfigurationInfo PRESENCE optional}|

{ ID id-PartialListIndicator-NR CRITICALITY ignore TYPE PartialListIndicator PRESENCE optional }|

{ ID id-CellAndCapacityAssistanceInfo-NR CRITICALITY ignore TYPE CellAndCapacityAssistanceInfo-NR PRESENCE optional }|

{ ID id-PartialListIndicator-EUTRA CRITICALITY ignore TYPE PartialListIndicator PRESENCE optional }|

{ ID id-CellAndCapacityAssistanceInfo-EUTRA CRITICALITY ignore TYPE CellAndCapacityAssistanceInfo-EUTRA PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- XN SETUP RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnSetupResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ XnSetupResponse-IEs}},

...

}

XnSetupResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-GlobalNG-RAN-node-ID CRITICALITY reject TYPE GlobalNG-RANNode-ID PRESENCE mandatory}|

{ ID id-TAISupport-list CRITICALITY reject TYPE TAISupport-List PRESENCE mandatory}|

{ ID id-List-of-served-cells-NR CRITICALITY reject TYPE ServedCells-NR PRESENCE optional }|

{ ID id-List-of-served-cells-E-UTRA CRITICALITY reject TYPE ServedCells-E-UTRA PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-AMF-Region-Information CRITICALITY reject TYPE AMF-Region-Information PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional }|

{ ID id-TNLConfigurationInfo CRITICALITY ignore TYPE TNLConfigurationInfo PRESENCE optional }|

{ ID id-PartialListIndicator-NR CRITICALITY ignore TYPE PartialListIndicator PRESENCE optional }|

{ ID id-CellAndCapacityAssistanceInfo-NR CRITICALITY ignore TYPE CellAndCapacityAssistanceInfo-NR PRESENCE optional }|

{ ID id-PartialListIndicator-EUTRA CRITICALITY ignore TYPE PartialListIndicator PRESENCE optional }|

{ ID id-CellAndCapacityAssistanceInfo-EUTRA CRITICALITY ignore TYPE CellAndCapacityAssistanceInfo-EUTRA PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- XN SETUP FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnSetupFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ XnSetupFailure-IEs}},

...

}

XnSetupFailure-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-TimeToWait CRITICALITY ignore TYPE TimeToWait PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional }|

{ ID id-MessageOversizeNotification CRITICALITY ignore TYPE MessageOversizeNotification PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- NG-RAN NODE CONFIGURATION UPDATE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGRANNodeConfigurationUpdate ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ NGRANNodeConfigurationUpdate-IEs}},

...

}

NGRANNodeConfigurationUpdate-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-TAISupport-list CRITICALITY reject TYPE TAISupport-List PRESENCE optional }|

{ ID id-ConfigurationUpdateInitiatingNodeChoice CRITICALITY ignore TYPE ConfigurationUpdateInitiatingNodeChoice PRESENCE mandatory}|

{ ID id-TNLA-To-Add-List CRITICALITY ignore TYPE TNLA-To-Add-List PRESENCE optional }|

{ ID id-TNLA-To-Remove-List CRITICALITY ignore TYPE TNLA-To-Remove-List PRESENCE optional }|

{ ID id-TNLA-To-Update-List CRITICALITY ignore TYPE TNLA-To-Update-List PRESENCE optional }|

{ ID id-GlobalNG-RAN-node-ID CRITICALITY reject TYPE GlobalNG-RANNode-ID PRESENCE optional }|

{ ID id-AMF-Region-Information-To-Add CRITICALITY reject TYPE AMF-Region-Information PRESENCE optional }|

{ ID id-AMF-Region-Information-To-Delete CRITICALITY reject TYPE AMF-Region-Information PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional }|

{ ID id-TNLConfigurationInfo CRITICALITY ignore TYPE TNLConfigurationInfo PRESENCE optional },

...

}

ConfigurationUpdateInitiatingNodeChoice ::= CHOICE {

gNB ProtocolIE-Container { {ConfigurationUpdate-gNB} },

ng-eNB ProtocolIE-Container { {ConfigurationUpdate-ng-eNB} },

choice-extension ProtocolIE-Single-Container { {ServedCellsToUpdateInitiatingNodeChoice-ExtIEs} }

}

ServedCellsToUpdateInitiatingNodeChoice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

ConfigurationUpdate-gNB XNAP-PROTOCOL-IES ::= {

{ ID id-servedCellsToUpdate-NR CRITICALITY ignore TYPE ServedCellsToUpdate-NR PRESENCE optional }|

{ ID id-cellAssistanceInfo-NR CRITICALITY ignore TYPE CellAssistanceInfo-NR PRESENCE optional }|

{ ID id-cellAssistanceInfo-EUTRA CRITICALITY ignore TYPE CellAssistanceInfo-EUTRA PRESENCE optional },

...

}

ConfigurationUpdate-ng-eNB XNAP-PROTOCOL-IES ::= {

{ ID id-servedCellsToUpdate-E-UTRA CRITICALITY ignore TYPE ServedCellsToUpdate-E-UTRA PRESENCE optional }|

{ ID id-cellAssistanceInfo-NR CRITICALITY ignore TYPE CellAssistanceInfo-NR PRESENCE optional }|

{ ID id-cellAssistanceInfo-EUTRA CRITICALITY ignore TYPE CellAssistanceInfo-EUTRA PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- NG-RAN NODE CONFIGURATION UPDATE ACKNOWLEDGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGRANNodeConfigurationUpdateAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ NGRANNodeConfigurationUpdateAcknowledge-IEs}},

...

}

NGRANNodeConfigurationUpdateAcknowledge-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-RespondingNodeTypeConfigUpdateAck CRITICALITY ignore TYPE RespondingNodeTypeConfigUpdateAck PRESENCE mandatory}|

{ ID id-TNLA-Setup-List CRITICALITY ignore TYPE TNLA-Setup-List PRESENCE optional }|

{ ID id-TNLA-Failed-To-Setup-List CRITICALITY ignore TYPE TNLA-Failed-To-Setup-List PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional }|

{ ID id-TNLConfigurationInfo CRITICALITY ignore TYPE TNLConfigurationInfo PRESENCE optional },

...

}

RespondingNodeTypeConfigUpdateAck ::= CHOICE {

ng-eNB RespondingNodeTypeConfigUpdateAck-ng-eNB,

gNB RespondingNodeTypeConfigUpdateAck-gNB,

choice-extension ProtocolIE-Single-Container { {RespondingNodeTypeConfigUpdateAck-ExtIEs} }

}

RespondingNodeTypeConfigUpdateAck-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

RespondingNodeTypeConfigUpdateAck-ng-eNB ::= SEQUENCE {

iE-Extension ProtocolExtensionContainer { {RespondingNodeTypeConfigUpdateAck-ng-eNB-ExtIEs} } OPTIONAL,

...

}

RespondingNodeTypeConfigUpdateAck-ng-eNB-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-List-of-served-cells-E-UTRA CRITICALITY ignore EXTENSION ServedCells-E-UTRA PRESENCE optional }|

{ ID id-PartialListIndicator-EUTRA CRITICALITY ignore EXTENSION PartialListIndicator PRESENCE optional }|

{ ID id-CellAndCapacityAssistanceInfo-EUTRA CRITICALITY ignore EXTENSION CellAndCapacityAssistanceInfo-EUTRA PRESENCE optional },

...

}

RespondingNodeTypeConfigUpdateAck-gNB ::= SEQUENCE {

served-NR-Cells ServedCells-NR OPTIONAL,

iE-Extension ProtocolExtensionContainer { {RespondingNodeTypeConfigUpdateAck-gNB-ExtIEs} } OPTIONAL,

...

}

RespondingNodeTypeConfigUpdateAck-gNB-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-PartialListIndicator-NR CRITICALITY ignore EXTENSION PartialListIndicator PRESENCE optional }|

{ ID id-CellAndCapacityAssistanceInfo-NR CRITICALITY ignore EXTENSION CellAndCapacityAssistanceInfo-NR PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- NG-RAN NODE CONFIGURATION UPDATE FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGRANNodeConfigurationUpdateFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{NGRANNodeConfigurationUpdateFailure-IEs}},

...

}

NGRANNodeConfigurationUpdateFailure-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-TimeToWait CRITICALITY ignore TYPE TimeToWait PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E-UTRA NR CELL RESOURCE COORDINATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E-UTRA-NR-CellResourceCoordinationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{E-UTRA-NR-CellResourceCoordinationRequest-IEs}},

...

}

E-UTRA-NR-CellResourceCoordinationRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-initiatingNodeType-ResourceCoordRequest CRITICALITY reject TYPE InitiatingNodeType-ResourceCoordRequest PRESENCE mandatory}|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

InitiatingNodeType-ResourceCoordRequest ::= CHOICE {

ng-eNB ResourceCoordRequest-ng-eNB-initiated,

gNB ResourceCoordRequest-gNB-initiated,

choice-extension ProtocolIE-Single-Container { {InitiatingNodeType-ResourceCoordRequest-ExtIEs} }

}

InitiatingNodeType-ResourceCoordRequest-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

ResourceCoordRequest-ng-eNB-initiated ::= SEQUENCE {

dataTrafficResourceIndication DataTrafficResourceIndication,

spectrumSharingGroupID SpectrumSharingGroupID,

listofE-UTRACells SEQUENCE (SIZE(1.. maxnoofCellsinNG-RANnode)) OF E-UTRA-CGI OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ResourceCoordRequest-ng-eNB-initiated-ExtIEs} } OPTIONAL,

...

}

ResourceCoordRequest-ng-eNB-initiated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResourceCoordRequest-gNB-initiated ::= SEQUENCE {

dataTrafficResourceIndication DataTrafficResourceIndication,

listofE-UTRACells SEQUENCE (SIZE(1.. maxnoofCellsinNG-RANnode)) OF E-UTRA-CGI OPTIONAL,

spectrumSharingGroupID SpectrumSharingGroupID,

listofNRCells SEQUENCE (SIZE(1.. maxnoofCellsinNG-RANnode)) OF NR-CGI OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ResourceCoordRequest-gNB-initiated-ExtIEs} } OPTIONAL,

...

}

ResourceCoordRequest-gNB-initiated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E-UTRA NR CELL RESOURCE COORDINATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E-UTRA-NR-CellResourceCoordinationResponse::= SEQUENCE {

protocolIEs ProtocolIE-Container {{E-UTRA-NR-CellResourceCoordinationResponse-IEs}},

...

}

E-UTRA-NR-CellResourceCoordinationResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-respondingNodeType-ResourceCoordResponse CRITICALITY reject TYPE RespondingNodeType-ResourceCoordResponse PRESENCE mandatory}|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

RespondingNodeType-ResourceCoordResponse ::= CHOICE {

ng-eNB ResourceCoordResponse-ng-eNB-initiated,

gNB ResourceCoordResponse-gNB-initiated,

choice-extension ProtocolIE-Single-Container { {RespondingNodeType-ResourceCoordResponse-ExtIEs} }

}

RespondingNodeType-ResourceCoordResponse-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

ResourceCoordResponse-ng-eNB-initiated ::= SEQUENCE {

dataTrafficResourceIndication DataTrafficResourceIndication,

spectrumSharingGroupID SpectrumSharingGroupID,

listofE-UTRACells SEQUENCE (SIZE(1.. maxnoofCellsinNG-RANnode)) OF E-UTRA-CGI OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ResourceCoordResponse-ng-eNB-initiated-ExtIEs} } OPTIONAL,

...

}

ResourceCoordResponse-ng-eNB-initiated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResourceCoordResponse-gNB-initiated ::= SEQUENCE {

dataTrafficResourceIndication DataTrafficResourceIndication,

spectrumSharingGroupID SpectrumSharingGroupID,

listofNRCells SEQUENCE (SIZE(1.. maxnoofCellsinNG-RANnode)) OF NR-CGI OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ResourceCoordResponse-gNB-initiated-ExtIEs} } OPTIONAL,

...

}

ResourceCoordResponse-gNB-initiated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- SECONDARY RAT DATA USAGE REPORT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SecondaryRATDataUsageReport ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{SecondaryRATDataUsageReport-IEs}},

...

}

SecondaryRATDataUsageReport-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-PDUSessionResourceSecondaryRATUsageList CRITICALITY reject TYPE PDUSessionResourceSecondaryRATUsageList PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- XN REMOVAL REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnRemovalRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ XnRemovalRequest-IEs}},

...

}

XnRemovalRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-GlobalNG-RAN-node-ID CRITICALITY reject TYPE GlobalNG-RANNode-ID PRESENCE mandatory}|

{ ID id-XnRemovalThreshold CRITICALITY reject TYPE XnBenefitValue PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- XN REMOVAL RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnRemovalResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ XnRemovalResponse-IEs}},

...

}

XnRemovalResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-GlobalNG-RAN-node-ID CRITICALITY reject TYPE GlobalNG-RANNode-ID PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- XN REMOVAL FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnRemovalFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ XnRemovalFailure-IEs}},

...

}

XnRemovalFailure-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- CELL ACTIVATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

CellActivationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ CellActivationRequest-IEs}},

...

}

CellActivationRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-ServedCellsToActivate CRITICALITY reject TYPE ServedCellsToActivate PRESENCE mandatory}|

{ ID id-ActivationIDforCellActivation CRITICALITY reject TYPE ActivationIDforCellActivation PRESENCE mandatory}|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

ServedCellsToActivate ::= CHOICE {

nr-cells SEQUENCE (SIZE(1..maxnoofCellsinNG-RANnode)) OF NR-CGI,

e-utra-cells SEQUENCE (SIZE(1..maxnoofCellsinNG-RANnode)) OF E-UTRA-CGI,

choice-extension ProtocolIE-Single-Container { {ServedCellsToActivate-ExtIEs} }

}

ServedCellsToActivate-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- CELL ACTIVATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

CellActivationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{CellActivationResponse-IEs}},

...

}

CellActivationResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-ActivatedServedCells CRITICALITY reject TYPE ActivatedServedCells PRESENCE mandatory}|

{ ID id-ActivationIDforCellActivation CRITICALITY reject TYPE ActivationIDforCellActivation PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

ActivatedServedCells ::= CHOICE {

nr-cells SEQUENCE (SIZE(1..maxnoofCellsinNG-RANnode)) OF NR-CGI,

e-utra-cells SEQUENCE (SIZE(1..maxnoofCellsinNG-RANnode)) OF E-UTRA-CGI,

choice-extension ProtocolIE-Single-Container { {ActivatedServedCells-ExtIEs} }

}

ActivatedServedCells-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- CELL ACTIVATION FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

CellActivationFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{CellActivationFailure-IEs}},

...

}

CellActivationFailure-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-ActivationIDforCellActivation CRITICALITY reject TYPE ActivationIDforCellActivation PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RESET REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ResetRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ResetRequest-IEs}},

...

}

ResetRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-ResetRequestTypeInfo CRITICALITY reject TYPE ResetRequestTypeInfo PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RESET RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ResetResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ResetResponse-IEs}},

...

}

ResetResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-ResetResponseTypeInfo CRITICALITY reject TYPE ResetResponseTypeInfo PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- ERROR INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ErrorIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ErrorIndication-IEs}},

...

}

ErrorIndication-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-oldNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE optional }|

{ ID id-newNG-RANnodeUEXnAPID CRITICALITY ignore TYPE NG-RANnodeUEXnAPID PRESENCE optional }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-InterfaceInstanceIndication CRITICALITY reject TYPE InterfaceInstanceIndication PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PRIVATE MESSAGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PrivateMessage ::= SEQUENCE {

privateIEs PrivateIE-Container {{PrivateMessage-IEs}},

...

}

PrivateMessage-IEs XNAP-PRIVATE-IES ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TRACE START

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TraceStart ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {TraceStartIEs} },

...

}

TraceStartIEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-TraceActivation CRITICALITY ignore TYPE TraceActivation PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- DEACTIVATE TRACE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

DeactivateTrace ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {DeactivateTraceIEs} },

...

}

DeactivateTraceIEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-NG-RANTraceID CRITICALITY ignore TYPE NG-RANTraceID PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- FAILURE INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

FailureIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{FailureIndication-IEs}},

...

}

FailureIndication-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-InitiatingCondition-FailureIndication CRITICALITY reject TYPE InitiatingCondition-FailureIndication PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- HANDOVER REPORT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

HandoverReport ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ HandoverReport-IEs}},

...

}

HandoverReport-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-HandoverReportType CRITICALITY ignore TYPE HandoverReportType PRESENCE mandatory}|

{ ID id-HandoverCause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-SourceCellCGI CRITICALITY ignore TYPE GlobalNG-RANCell-ID PRESENCE mandatory }|

{ ID id-TargetCellCGI CRITICALITY ignore TYPE GlobalNG-RANCell-ID PRESENCE mandatory }|

{ ID id-ReEstablishmentCellCGI CRITICALITY ignore TYPE GlobalCell-ID PRESENCE conditional }|

-- This IE shall be present if the *Handover Report Type* IE is set to the value "HO to wrong cell"

{ ID id-TargetCellinEUTRAN CRITICALITY ignore TYPE TargetCellinEUTRAN PRESENCE conditional }|

-- This IE shall be present if the *Handover Report Type* IE is set to the value "Inter-system ping-pong"

{ ID id-SourceCellCRNTI CRITICALITY ignore TYPE C-RNTI PRESENCE optional }|

{ ID id-MobilityInformation CRITICALITY ignore TYPE MobilityInformation PRESENCE optional }|

{ ID id-UERLFReportContainer CRITICALITY ignore TYPE UERLFReportContainer PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RESOURCE STATUS REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ResourceStatusRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ResourceStatusRequest-IEs}},

...

}

ResourceStatusRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-NGRAN-Node1-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-NGRAN-Node2-Measurement-ID CRITICALITY ignore TYPE Measurement-ID PRESENCE conditional}|

-- This IE shall be present if the *Registration Request* IE is set to the value "stop", "partial stop" or "add".

{ ID id-RegistrationRequest CRITICALITY reject TYPE RegistrationRequest PRESENCE mandatory}|

{ ID id-ReportCharacteristics CRITICALITY reject TYPE ReportCharacteristics PRESENCE conditional}|

-- This IE shall be present if the *Registration Request* IE is set to the value "start".

{ ID id-CellToReport CRITICALITY ignore TYPE CellToReport PRESENCE optional}|

{ ID id-ReportingPeriodicity CRITICALITY ignore TYPE ReportingPeriodicity PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RESOURCE STATUS RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ResourceStatusResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ResourceStatusResponse-IEs}},

...

}

ResourceStatusResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-NGRAN-Node1-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-NGRAN-Node2-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RESOURCE STATUS FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ResourceStatusFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ResourceStatusFailure-IEs}},

...

}

ResourceStatusFailure-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-NGRAN-Node1-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-NGRAN-Node2-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RESOURCE STATUS UPDATE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ResourceStatusUpdate ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ResourceStatusUpdate-IEs}},

...

}

ResourceStatusUpdate-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-NGRAN-Node1-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-NGRAN-Node2-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-CellMeasurementResult CRITICALITY ignore TYPE CellMeasurementResult PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MOBILITY CHANGE REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MobilityChangeRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MobilityChangeRequest-IEs}},

...

}

MobilityChangeRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-NG-RANnode1CellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE mandatory}|

{ ID id-NG-RANnode2CellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE mandatory}|

{ ID id-NG-RANnode1MobilityParameters CRITICALITY reject TYPE MobilityParametersInformation PRESENCE optional}|

{ ID id-NG-RANnode2ProposedMobilityParameters CRITICALITY reject TYPE MobilityParametersInformation PRESENCE optional}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MOBILITY CHANGE ACKNOWLEDGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MobilityChangeAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MobilityChangeAcknowledge-IEs}},

...

}

MobilityChangeAcknowledge-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-NG-RANnode1CellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE mandatory}|

{ ID id-NG-RANnode2CellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MOBILITY CHANGE FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MobilityChangeFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MobilityChangeFailure-IEs}},

...

}

MobilityChangeFailure-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-NG-RANnode1CellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE mandatory}|

{ ID id-NG-RANnode2CellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-MobilityParametersModificationRange CRITICALITY reject TYPE MobilityParametersModificationRange PRESENCE optional}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- ACCESS AND MOBILITY INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

AccessAndMobilityIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ AccessAndMobilityIndication-IEs}},

...

}

AccessAndMobilityIndication-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-RACHReportInformation CRITICALITY ignore TYPE RACHReportInformation PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- F1-C TRAFFIC TRANSFER

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1CTrafficTransfer ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ F1CTrafficTransfer-IEs}},

...

}

F1CTrafficTransfer-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-F1CTrafficContainer CRITICALITY reject TYPE F1CTrafficContainer PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IAB TRANSPORT MIGRATION MANAGEMENT REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IABTransportMigrationManagementRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ IABTransportMigrationManagementRequest-IEs}},

...

}

IABTransportMigrationManagementRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-F1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-nonF1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-TrafficToBeAddedList CRITICALITY reject TYPE TrafficToBeAddedList PRESENCE optional }|

{ ID id-TrafficToBeModifiedList CRITICALITY reject TYPE TrafficToBeModifiedList PRESENCE optional }|

{ ID id-TrafficToBeReleaseInformation CRITICALITY reject TYPE TrafficToBeReleaseInformation PRESENCE optional }|

{ ID id-IAB-TNL-Address-Request CRITICALITY reject TYPE IAB-TNL-Address-Request PRESENCE optional }|

{ ID id-IABTNLAddressException CRITICALITY ignore TYPE IABTNLAddressException PRESENCE optional },

...

}

TrafficToBeAddedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficToBeAdded-Item

TrafficToBeAdded-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

trafficProfile TrafficProfile,

f1-TerminatingTopologyBHInformation F1-TerminatingTopologyBHInformation OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {TrafficToBeAdded-Item-ExtIEs} } OPTIONAL,

...

}

TrafficToBeAdded-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TrafficToBeModifiedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficToBeModified-Item

TrafficToBeModified-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

trafficProfile TrafficProfile OPTIONAL,

f1-TerminatingTopologyBHInformation F1-TerminatingTopologyBHInformation OPTIONAL,

iE-Extension ProtocolExtensionContainer { {TrafficToBeModified-Item-ExtIEs} } OPTIONAL,

...

}

TrafficToBeModified-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IAB TRANSPORT MIGRATION MANAGEMENT RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IABTransportMigrationManagementResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ IABTransportMigrationManagementResponse-IEs}},

...

}

IABTransportMigrationManagementResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-F1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-nonF1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-TrafficAddedList CRITICALITY reject TYPE TrafficAddedList PRESENCE optional }|

{ ID id-TrafficModifiedList CRITICALITY reject TYPE TrafficModifiedList PRESENCE optional }|

{ ID id-TrafficNotAddedList CRITICALITY reject TYPE TrafficNotAddedList PRESENCE optional }|

{ ID id-TrafficNotModifiedList CRITICALITY reject TYPE TrafficNotModifiedList PRESENCE optional }|

{ ID id-IAB-TNL-Address-Response CRITICALITY reject TYPE IAB-TNL-Address-Response PRESENCE optional }|

{ ID id-TrafficReleasedList CRITICALITY reject TYPE TrafficReleasedList PRESENCE optional },

...

}

TrafficAddedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficAdded-Item

TrafficAdded-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

non-F1-TerminatingTopologyBHInformation Non-F1-TerminatingTopologyBHInformation,

iE-Extensions ProtocolExtensionContainer { {TrafficAdded-Item-ExtIEs} } OPTIONAL,

...

}

TrafficAdded-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TrafficModifiedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficModified-Item

TrafficModified-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

non-F1-TerminatingTopologyBHInformation Non-F1-TerminatingTopologyBHInformation,

iE-Extensions ProtocolExtensionContainer { {TrafficModified-Item-ExtIEs} } OPTIONAL,

...

}

TrafficModified-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TrafficNotAddedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficNotAdded-Item

TrafficNotAdded-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

casue Cause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {TrafficNotAdded-Item-ExtIEs} } OPTIONAL,

...

}

TrafficNotAdded-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TrafficNotModifiedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficNotModified-Item

TrafficNotModified-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

cause Cause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {TrafficNotModified-Item-ExtIEs} } OPTIONAL,

...

}

TrafficNotModified-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TrafficReleasedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficReleased-Item

TrafficReleased-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

bHInfoList BHInfoList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { TrafficReleased-Item-ExtIEs} } OPTIONAL,

...

}

TrafficReleased-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IAB TRANSPORT MIGRATION MODIFICATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IABTransportMigrationModificationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ IABTransportMigrationModificationRequest-IEs}},

...

}

IABTransportMigrationModificationRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-F1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-nonF1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-TrafficRequiredToBeModifiedList CRITICALITY reject TYPE TrafficRequiredToBeModifiedList PRESENCE optional }|

{ ID id-TrafficToBeReleaseInformation CRITICALITY reject TYPE TrafficToBeReleaseInformation PRESENCE optional }|

{ ID id-IABTNLAddressToBeAdded CRITICALITY reject TYPE IAB-TNL-Address-Response PRESENCE optional }|

{ ID id-IABTNLAddressToBeReleasedList CRITICALITY reject TYPE IABTNLAddressToBeReleasedList PRESENCE optional },

...

}

TrafficRequiredToBeModifiedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficRequiredToBeModified-Item

TrafficRequiredToBeModified-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

non-f1-TerminatingTopologyBHInformation Non-F1-TerminatingTopologyBHInformation OPTIONAL,

iE-Extensions ProtocolExtensionContainer{ { TrafficRequiredToBeModified-Item-ExtIEs} } OPTIONAL,

...

}

TrafficRequiredToBeModified-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IABTNLAddressToBeReleasedList ::= SEQUENCE (SIZE(1..maxnoofTLAsIAB)) OF IABTNLAddressToBeReleased-Item

IABTNLAddressToBeReleased-Item ::= SEQUENCE {

iabTNLAddress IABTNLAddress,

iE-Extensions ProtocolExtensionContainer{ { IABTNLAddressToBeReleased-Item-ExtIEs} } OPTIONAL,

...

}

IABTNLAddressToBeReleased-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IAB TRANSPORT MIGRATION MODIFICATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IABTransportMigrationModificationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ IABTransportMigrationModificationResponse-IEs}},

...

}

IABTransportMigrationModificationResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-F1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-nonF1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-TrafficRequiredModifiedList CRITICALITY reject TYPE TrafficRequiredModifiedList PRESENCE optional }|

{ ID id-TrafficReleasedList CRITICALITY reject TYPE TrafficReleasedList PRESENCE optional },

...

}

TrafficRequiredModifiedList ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficRequiredModified-Item

TrafficRequiredModified-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

iE-Extensions ProtocolExtensionContainer { { TrafficRequiredModified-Item-ExtIEs} } OPTIONAL,

...

}

TrafficRequiredModified-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IAB RESOURCE COORDINATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IABResourceCoordinationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ IABResourceCoordinationRequest-IEs}},

...

}

IABResourceCoordinationRequest-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-F1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-nonF1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-BoundaryNodeCellsList CRITICALITY reject TYPE BoundaryNodeCellsList PRESENCE optional }|

{ ID id-ParentNodeCellsList CRITICALITY reject TYPE ParentNodeCellsList PRESENCE optional },

...

}

BoundaryNodeCellsList ::= SEQUENCE (SIZE(1..maxnoofServedCellsIAB)) OF BoundaryNodeCellsList-Item

BoundaryNodeCellsList-Item ::= SEQUENCE {

boundaryNodeCellInformation IABCellInformation,

iE-Extensions ProtocolExtensionContainer { {BoundaryNodeCellsList-Item-ExtIEs} } OPTIONAL,

...

}

BoundaryNodeCellsList-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ParentNodeCellsList ::= SEQUENCE (SIZE(1..maxnoofServingCells)) OF ParentNodeCellsList-Item

ParentNodeCellsList-Item ::= SEQUENCE {

parentNodeCellInformation IABCellInformation,

iE-Extensions ProtocolExtensionContainer { {ParentNodeCellsList-Item-ExtIEs} } OPTIONAL,

...

}

ParentNodeCellsList-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IAB RESOURCE COORDINATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IABResourceCoordinationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ IABResourceCoordinationResponse-IEs}},

...

}

IABResourceCoordinationResponse-IEs XNAP-PROTOCOL-IES ::= {

{ ID id-F1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-nonF1-Terminating-DonorUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

{ ID id-BoundaryNodeCellsList CRITICALITY reject TYPE BoundaryNodeCellsList PRESENCE optional }|

{ ID id-ParentNodeCellsList CRITICALITY reject TYPE ParentNodeCellsList PRESENCE optional },

...

}

END

-- ASN1STOP

9.3.5 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

id-CNTypeRestrictionsForEquivalent,

id-CNTypeRestrictionsForServing,

id-Additional-UL-NG-U-TNLatUPF-List,

id-ConfiguredTACIndication,

id-AlternativeQoSParaSetList,

id-CurrentQoSParaSetIndex,

id-DefaultDRB-Allowed,

id-DLCarrierList,

id-EndpointIPAddressAndPort,

id-ExtendedTAISliceSupportList,

id-FiveGCMobilityRestrictionListContainer,

id-SecondarydataForwardingInfoFromTarget-List,

id-LastE-UTRANPLMNIdentity,

id-IntendedTDD-DL-ULConfiguration-NR,

id-MaxIPrate-DL,

id-SecurityResult,

id-OldQoSFlowMap-ULendmarkerexpected,

id-PDUSessionCommonNetworkInstance,

id-BPLMN-ID-Info-EUTRA,

id-BPLMN-ID-Info-NR,

id-DRBsNotAdmittedSetupModifyList,

id-Secondary-MN-Xn-U-TNLInfoatM,

id-ULForwardingProposal,

id-DRB-IDs-takenintouse,

id-SplitSessionIndicator,

id-NonGBRResources-Offered,

id-MDT-Configuration,

id-TraceCollectionEntityURI,

id-NPN-Broadcast-Information,

id-NPNPagingAssistanceInformation,

id-NPNMobilityInformation,

id-NPN-Support,

id-LTEUESidelinkAggregateMaximumBitRate,

id-NRUESidelinkAggregateMaximumBitRate,

id-ExtendedRATRestrictionInformation,

id-QoSMonitoringRequest,

id-QoSMonitoringDisabled,

id-QosMonitoringReportingFrequency,

id-DAPSRequestInfo,

id-OffsetOfNbiotChannelNumberToDL-EARFCN,

id-OffsetOfNbiotChannelNumberToUL-EARFCN,

id-NBIoT-UL-DL-AlignmentOffset,

id-TDDULDLConfigurationCommonNR,

id-CarrierList,

id-ULCarrierList,

id-FrequencyShift7p5khz,

id-SSB-PositionsInBurst,

id-NRCellPRACHConfig,

id-Redundant-UL-NG-U-TNLatUPF,

id-Redundant-DL-NG-U-TNLatNG-RAN,

id-CNPacketDelayBudgetDownlink,

id-CNPacketDelayBudgetUplink,

id-ExtendedPacketDelayBudget,

id-Additional-Redundant-UL-NG-U-TNLatUPF-List,

id-RedundantCommonNetworkInstance,

id-TSCTrafficCharacteristics,

id-RedundantQoSFlowIndicator,

id-Additional-PDCP-Duplication-TNL-List,

id-RedundantPDUSessionInformation,

id-UsedRSNInformation,

id-RLCDuplicationInformation,

id-CSI-RSTransmissionIndication,

id-UERadioCapabilityID,

id-secondary-SN-UL-PDCP-UP-TNLInfo,

id-pdcpDuplicationConfiguration,

id-duplicationActivation,

id-NPRACHConfiguration,

id-QoSFlowsMappedtoDRB-SetupResponse-MNterminated,

id-DL-scheduling-PDCCH-CCE-usage,

id-UL-scheduling-PDCCH-CCE-usage,

id-SFN-Offset,

id-QoS-Mapping-Information,

id-AdditionLocationInformation,

id-dataForwardingInfoFromTargetE-UTRANnode,

id-Cause,

id-IAB-MT-Cell-List,

id-NoPDUSessionIndication,

id-permutation,

id-UL-GNB-DU-Cell-Resource-Configuration,

id-DL-GNB-DU-Cell-Resource-Configuration,

maxEARFCN,

maxnoofAllowedAreas,

maxnoofAMFRegions,

maxnoofAoIs,

maxnoofBPLMNs,

maxnoofCAGs,

maxnoofCAGsperPLMN,

maxnoofCellsinAoI,

maxnoofCellsinNG-RANnode,

maxnoofCellsinRNA,

maxnoofCellsinUEHistoryInfo,

maxnoofCellsUEMovingTrajectory,

maxnoofDRBs,

maxnoofEPLMNs,

maxnoofEPLMNsplus1,

maxnoofEUTRABands,

maxnoofEUTRABPLMNs,

maxnoofForbiddenTACs,

maxnoofMBSFNEUTRA,

maxnoofMultiConnectivityMinusOne,

maxnoofNeighbours,

maxnoofNIDs,

maxnoofNRCellBands,

maxnoofPDUSessions,

maxnoofPLMNs,

maxnoofProtectedResourcePatterns,

maxnoofQoSFlows,

maxnoofQoSParaSets,

maxnoofRANAreaCodes,

maxnoofRANAreasinRNA,

maxnoofSCellGroups,

maxnoofSCellGroupsplus1,

maxnoofSliceItems,

maxnoofExtSliceItems,

maxnoofSNPNIDs,

maxnoofsupportedTACs,

maxnoofsupportedPLMNs,

maxnoofTAI,

maxnoofTAIsinAoI,

maxnoofTNLAssociations,

maxnoofUEContexts,

maxNRARFCN,

maxNrOfErrors,

maxnoofRANNodesinAoI,

maxnooftimeperiods,

maxnoofslots,

maxnoofExtTLAs,

maxnoofGTPTLAs,

maxnoofCHOcells,

maxnoofPC5QoSFlows,

maxnoofSSBAreas,

maxnoofNRSCSs,

maxnoofPhysicalResourceBlocks,

maxnoofRACHReports,

maxnoofAdditionalPDCPDuplicationTNL,

maxnoofRLCDuplicationstate,

maxnoofBluetoothName,

maxnoofCellIDforMDT,

maxnoofMDTPLMNs,

maxnoofTAforMDT,

maxnoofWLANName,

maxnoofSensorName,

maxnoofNeighPCIforMDT,

maxnoofFreqforMDT,

maxnoofNonAnchorCarrierFreqConfig,

maxnoofDataForwardingTunneltoE-UTRAN,

maxnoofServingCells,

maxnoofBHInfo,

maxnoofTLAsIAB,

maxnoofTrafficIndexEntries,

maxnoofBAPControlPDURLCCHs,

maxnoofServedCellsIAB,

maxnoofDUFSlots,

maxnoofSymbols,

maxnoofHSNASlots,

maxnoofRBsetsPerCell,

maxnoofChildIABNodes,

maxnoofIABSTCInfo

FROM XnAP-Constants

Criticality,

ProcedureCode,

ProtocolIE-ID,

TriggeringMessage

FROM XnAP-CommonDataTypes

ProtocolExtensionContainer{},

ProtocolIE-Single-Container{},

XNAP-PROTOCOL-EXTENSION,

XNAP-PROTOCOL-IES

FROM XnAP-Containers;

-- A

AdditionLocationInformation ::= ENUMERATED {

includePSCell,

...

}

Additional-PDCP-Duplication-TNL-List ::= SEQUENCE (SIZE(1..maxnoofAdditionalPDCPDuplicationTNL)) OF Additional-PDCP-Duplication-TNL-Item

Additional-PDCP-Duplication-TNL-Item ::= SEQUENCE {  
 additional-PDCP-Duplication-UP-TNL-Information UPTransportLayerInformation,  
 iE-Extensions ProtocolExtensionContainer { { Additional-PDCP-Duplication-TNL-ExtIEs} } OPTIONAL,  
 ...  
}

Additional-PDCP-Duplication-TNL-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {  
 ...  
}

Additional-UL-NG-U-TNLatUPF-Item ::= SEQUENCE {

additional-UL-NG-U-TNLatUPF UPTransportLayerInformation,

iE-Extensions ProtocolExtensionContainer { { Additional-UL-NG-U-TNLatUPF-Item-ExtIEs} } OPTIONAL,

...

}

Additional-UL-NG-U-TNLatUPF-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-PDUSessionCommonNetworkInstance CRITICALITY ignore EXTENSION PDUSessionCommonNetworkInstance PRESENCE optional},

...

}

Additional-UL-NG-U-TNLatUPF-List ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF Additional-UL-NG-U-TNLatUPF-Item

ActivationIDforCellActivation ::= INTEGER (0..255)

AllocationandRetentionPriority ::= SEQUENCE {

priorityLevel INTEGER (0..15,...),

pre-emption-capability ENUMERATED {shall-not-trigger-preemptdatDion, may-trigger-preemption, ...},

pre-emption-vulnerability ENUMERATED {not-preemptable, preemptable, ...},

iE-Extensions ProtocolExtensionContainer { {AllocationandRetentionPriority-ExtIEs} } OPTIONAL,

...

}

AllocationandRetentionPriority-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ActivationSFN ::= INTEGER (0..1023)

AllowedCAG-ID-List-perPLMN ::= SEQUENCE (SIZE(1..maxnoofCAGsperPLMN)) OF CAG-Identifier

AllowedPNI-NPN-ID-List ::= SEQUENCE (SIZE(1..maxnoofEPLMNsplus1)) OF AllowedPNI-NPN-ID-Item

AllowedPNI-NPN-ID-Item ::= SEQUENCE {

plmn-id PLMN-Identity,

pni-npn-restricted-information PNI-NPN-Restricted-Information,

allowed-CAG-id-list-per-plmn AllowedCAG-ID-List-perPLMN,

iE-Extensions ProtocolExtensionContainer { {AllowedPNI-NPN-ID-Item-ExtIEs} } OPTIONAL,

...

}

AllowedPNI-NPN-ID-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

AllTrafficIndication ::= ENUMERATED {true,...}

AlternativeQoSParaSetList ::= SEQUENCE (SIZE(1..maxnoofQoSParaSets)) OF AlternativeQoSParaSetItem

AlternativeQoSParaSetItem ::= SEQUENCE {

alternativeQoSParaSetIndex QoSParaSetIndex,

guaranteedFlowBitRateDL BitRate OPTIONAL,

guaranteedFlowBitRateUL BitRate OPTIONAL,

packetDelayBudget PacketDelayBudget OPTIONAL,

packetErrorRate PacketErrorRate OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {AlternativeQoSParaSetItem-ExtIEs} } OPTIONAL,

...

}

AlternativeQoSParaSetItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

AMF-Region-Information ::= SEQUENCE (SIZE (1..maxnoofAMFRegions)) OF GlobalAMF-Region-Information

GlobalAMF-Region-Information ::= SEQUENCE {

plmn-ID PLMN-Identity,

amf-region-id BIT STRING (SIZE (8)),

iE-Extensions ProtocolExtensionContainer { {GlobalAMF-Region-Information-ExtIEs} } OPTIONAL,

...

}

GlobalAMF-Region-Information-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

AMF-UE-NGAP-ID ::= INTEGER (0..1099511627775)

AreaOfInterestInformation ::= SEQUENCE (SIZE(1..maxnoofAoIs)) OF AreaOfInterest-Item

AreaOfInterest-Item ::= SEQUENCE {

listOfTAIsinAoI ListOfTAIsinAoI OPTIONAL,

listOfCellsinAoI ListOfCells OPTIONAL,

listOfRANNodesinAoI ListOfRANNodesinAoI OPTIONAL,

requestReferenceID RequestReferenceID,

iE-Extensions ProtocolExtensionContainer { {AreaOfInterest-Item-ExtIEs} } OPTIONAL,

...

}

AreaOfInterest-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

AreaScopeOfMDT-NR ::= CHOICE {

cellBased CellBasedMDT-NR,

tABased TABasedMDT,

tAIBased TAIBasedMDT,

...

}

AreaScopeOfMDT-EUTRA ::= CHOICE {

cellBased CellBasedMDT-EUTRA,

tABased TABasedMDT,

tAIBased TAIBasedMDT,

...

}

AreaScopeOfNeighCellsList ::= SEQUENCE (SIZE(1..maxnoofFreqforMDT)) OF AreaScopeOfNeighCellsItem

AreaScopeOfNeighCellsItem ::= SEQUENCE {

nrFrequencyInfo NRFrequencyInfo,

pciListForMDT PCIListForMDT OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { AreaScopeOfNeighCellsItem-ExtIEs} } OPTIONAL,

...

}

AreaScopeOfNeighCellsItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

AS-SecurityInformation ::= SEQUENCE {

key-NG-RAN-Star BIT STRING (SIZE(256)),

ncc INTEGER (0..7),

iE-Extensions ProtocolExtensionContainer { {AS-SecurityInformation-ExtIEs} } OPTIONAL,

...

}

AS-SecurityInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

AssistanceDataForRANPaging ::= SEQUENCE {

ran-paging-attempt-info RANPagingAttemptInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {AssistanceDataForRANPaging-ExtIEs} } OPTIONAL,

...

}

AssistanceDataForRANPaging-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-NPNPagingAssistanceInformation CRITICALITY ignore EXTENSION NPNPagingAssistanceInformation PRESENCE optional },

...

}

AvailableCapacity ::= INTEGER (1.. 100,...)

AvailableRRCConnectionCapacityValue ::= INTEGER (0..100)

AveragingWindow ::= INTEGER (0..4095, ...)

-- B

BAPAddress ::= BIT STRING (SIZE(10))

BAPPathID ::= BIT STRING (SIZE(10))

BAPRoutingID ::= SEQUENCE {

bAPAddress BAPAddress,

bAPPathID BAPPathID,

iE-Extensions ProtocolExtensionContainer { {BAPRoutingID-ExtIEs} } OPTIONAL,

...

}

BAPRoutingID-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

BHInfoIndex ::= INTEGER (1..maxnoofBHInfo)

BHInfoList ::= SEQUENCE (SIZE(1.. maxnoofBHInfo)) OF BHInfo-Item

BHInfo-Item ::= SEQUENCE {

bHInfoIndex BHInfoIndex,

iE-Extensions ProtocolExtensionContainer { { BHInfo-Item-ExtIEs} } OPTIONAL,

...

}

BHInfo-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

BHRLCChannelID ::= BIT STRING (SIZE(16))

BAPControlPDURLCCH-List ::= SEQUENCE (SIZE(1.. maxnoofBAPControlPDURLCCHs)) OF BAPControlPDURLCCH-Item

BAPControlPDURLCCH-Item ::= SEQUENCE {

bHRLCCHID BHRLCChannelID,

nexthopBAPAddress BAPAddress,

iE-Extensions ProtocolExtensionContainer { { BAPControlPDURLCCH-Item-ExtIEs} } OPTIONAL,

...

}

BAPControlPDURLCCH-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

BluetoothMeasurementConfiguration ::= SEQUENCE {

bluetoothMeasConfig BluetoothMeasConfig,

bluetoothMeasConfigNameList BluetoothMeasConfigNameList OPTIONAL,

bt-rssi ENUMERATED {true, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { BluetoothMeasurementConfiguration-ExtIEs } } OPTIONAL,

...

}

BluetoothMeasurementConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

BluetoothMeasConfigNameList ::= SEQUENCE (SIZE(1..maxnoofBluetoothName)) OF BluetoothName

BluetoothMeasConfig::= ENUMERATED {setup,...}

BluetoothName ::= OCTET STRING (SIZE (1..248))

BPLMN-ID-Info-EUTRA ::= SEQUENCE (SIZE(1..maxnoofEUTRABPLMNs)) OF BPLMN-ID-Info-EUTRA-Item

BPLMN-ID-Info-EUTRA-Item ::= SEQUENCE {

broadcastPLMNs BroadcastEUTRAPLMNs,

tac TAC,

e-utraCI E-UTRA-Cell-Identity,

ranac RANAC OPTIONAL,

iE-Extension ProtocolExtensionContainer { {BPLMN-ID-Info-EUTRA-Item-ExtIEs} } OPTIONAL,

...

}

BPLMN-ID-Info-EUTRA-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

BPLMN-ID-Info-NR ::= SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF BPLMN-ID-Info-NR-Item

BPLMN-ID-Info-NR-Item ::= SEQUENCE {

broadcastPLMNs BroadcastPLMNs,

tac TAC,

nr-CI NR-Cell-Identity,

ranac RANAC OPTIONAL,

iE-Extension ProtocolExtensionContainer { {BPLMN-ID-Info-NR-Item-ExtIEs} } OPTIONAL,

...

}

BPLMN-ID-Info-NR-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-ConfiguredTACIndication CRITICALITY ignore EXTENSION ConfiguredTACIndication PRESENCE optional }|

{ ID id-NPN-Broadcast-Information CRITICALITY reject EXTENSION NPN-Broadcast-Information PRESENCE optional },

...

}

BitRate ::= INTEGER (0..4000000000000,...)

BroadcastCAG-Identifier-List ::= SEQUENCE (SIZE(1..maxnoofCAGs)) OF BroadcastCAG-Identifier-Item

BroadcastCAG-Identifier-Item ::= SEQUENCE {

cag-Identifier CAG-Identifier,

iE-Extension ProtocolExtensionContainer { {BroadcastCAG-Identifier-Item-ExtIEs} } OPTIONAL,

...

}

BroadcastCAG-Identifier-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

BroadcastNID-List ::= SEQUENCE (SIZE(1..maxnoofNIDs)) OF BroadcastNID-Item

BroadcastNID-Item ::= SEQUENCE {

nid NID,

iE-Extension ProtocolExtensionContainer { {BroadcastNID-Item-ExtIEs} } OPTIONAL,

...

}

BroadcastNID-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

BroadcastPLMNs ::= SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF PLMN-Identity

BroadcastEUTRAPLMNs ::= SEQUENCE (SIZE(1..maxnoofEUTRABPLMNs)) OF PLMN-Identity

BroadcastPLMNinTAISupport-Item ::= SEQUENCE {

plmn-id PLMN-Identity,

tAISliceSupport-List SliceSupport-List,

iE-Extension ProtocolExtensionContainer { {BroadcastPLMNinTAISupport-Item-ExtIEs} } OPTIONAL,

...

}

BroadcastPLMNinTAISupport-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-NPN-Support CRITICALITY reject EXTENSION NPN-Support PRESENCE optional}|

{ ID id-ExtendedTAISliceSupportList CRITICALITY reject EXTENSION ExtendedSliceSupportList PRESENCE optional},

...

}

BroadcastPNI-NPN-ID-Information ::= SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF BroadcastPNI-NPN-ID-Information-Item

BroadcastPNI-NPN-ID-Information-Item ::= SEQUENCE {

plmn-id PLMN-Identity,

broadcastCAG-Identifier-List BroadcastCAG-Identifier-List,

iE-Extension ProtocolExtensionContainer { {BroadcastPNI-NPN-ID-Information-Item-ExtIEs} } OPTIONAL,

...

}

BroadcastPNI-NPN-ID-Information-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

BroadcastSNPNID-List ::= SEQUENCE (SIZE(1..maxnoofSNPNIDs)) OF BroadcastSNPNID

BroadcastSNPNID ::= SEQUENCE {

plmn-id PLMN-Identity,

broadcastNID-List BroadcastNID-List,

iE-Extension ProtocolExtensionContainer { {BroadcastSNPNID-ExtIEs} } OPTIONAL,

...

}

BroadcastSNPNID-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- C

CAG-Identifier ::= BIT STRING (SIZE (32))

CapacityValue ::= INTEGER (0..100)

CapacityValueInfo ::= SEQUENCE {

capacityValue CapacityValue,

ssbAreaCapacityValueList SSBAreaCapacityValue-List OPTIONAL,

iE-Extension ProtocolExtensionContainer { {CapacityValueInfo-ExtIEs} } OPTIONAL,

...

}

CapacityValueInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

Cause ::= CHOICE {

radioNetwork CauseRadioNetworkLayer,

transport CauseTransportLayer,

protocol CauseProtocol,

misc CauseMisc,

choice-extension ProtocolIE-Single-Container { {Cause-ExtIEs} }

}

Cause-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

CauseRadioNetworkLayer ::= ENUMERATED {

cell-not-available,

handover-desirable-for-radio-reasons,

handover-target-not-allowed,

invalid-AMF-Set-ID,

no-radio-resources-available-in-target-cell,

partial-handover,

reduce-load-in-serving-cell,

resource-optimisation-handover,

time-critical-handover,

tXnRELOCoverall-expiry,

tXnRELOCprep-expiry,

unknown-GUAMI-ID,

unknown-local-NG-RAN-node-UE-XnAP-ID,

inconsistent-remote-NG-RAN-node-UE-XnAP-ID,

encryption-and-or-integrity-protection-algorithms-not-supported,

protection-algorithms-not-supported,

multiple-PDU-session-ID-instances,

unknown-PDU-session-ID,

unknown-QoS-Flow-ID,

multiple-QoS-Flow-ID-instances,

switch-off-ongoing,

not-supported-5QI-value,

tXnDCoverall-expiry,

tXnDCprep-expiry,

action-desirable-for-radio-reasons,

reduce-load,

resource-optimisation,

time-critical-action,

target-not-allowed,

no-radio-resources-available,

invalid-QoS-combination,

encryption-algorithms-not-supported,

procedure-cancelled,

rRM-purpose,

improve-user-bit-rate,

user-inactivity,

radio-connection-with-UE-lost,

failure-in-the-radio-interface-procedure,

bearer-option-not-supported,

up-integrity-protection-not-possible,

up-confidentiality-protection-not-possible,

resources-not-available-for-the-slice-s,

ue-max-IP-data-rate-reason,

cP-integrity-protection-failure,

uP-integrity-protection-failure,

slice-not-supported-by-NG-RAN,

mN-Mobility,

sN-Mobility,

count-reaches-max-value,

unknown-old-NG-RAN-node-UE-XnAP-ID,

pDCP-Overload,

drb-id-not-available,

unspecified,

...,

ue-context-id-not-known,

non-relocation-of-context,

cho-cpc-resources-tobechanged,

rSN-not-available-for-the-UP,

npn-access-denied,

report-characteristics-empty,

existing-measurement-ID,

measurement-temporarily-not-available,

measurement-not-supported-for-the-object,

ue-power-saving,

unknown-NG-RAN-node2-Measurement-ID,

insufficient-ue-capabilities,

normal-release

}

CauseTransportLayer ::= ENUMERATED {

transport-resource-unavailable,

unspecified,

...

}

CauseProtocol ::= ENUMERATED {

transfer-syntax-error,

abstract-syntax-error-reject,

abstract-syntax-error-ignore-and-notify,

message-not-compatible-with-receiver-state,

semantic-error,

abstract-syntax-error-falsely-constructed-message,

unspecified,

...

}

CauseMisc ::= ENUMERATED {

control-processing-overload,

hardware-failure,

o-and-M-intervention,

not-enough-user-plane-processing-resources,

unspecified,

...

}

CellAssistanceInfo-NR ::= CHOICE {

limitedNR-List SEQUENCE (SIZE(1..maxnoofCellsinNG-RANnode)) OF NR-CGI,

full-List ENUMERATED {all-served-cells-NR, ...},

choice-extension ProtocolIE-Single-Container { {CellAssistanceInfo-NR-ExtIEs} }

}

CellAssistanceInfo-NR-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

CellAndCapacityAssistanceInfo-NR ::= SEQUENCE {

maximumCellListSize MaximumCellListSize OPTIONAL,

cellAssistanceInfo-NR CellAssistanceInfo-NR OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { CellAndCapacityAssistanceInfo-NR-ExtIEs} } OPTIONAL,

...

}

CellAndCapacityAssistanceInfo-NR-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CellAndCapacityAssistanceInfo-EUTRA ::= SEQUENCE {

maximumCellListSize MaximumCellListSize OPTIONAL,

cellAssistanceInfo-EUTRA CellAssistanceInfo-EUTRA OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { CellAndCapacityAssistanceInfo-EUTRA-ExtIEs} } OPTIONAL,

...

}

CellAndCapacityAssistanceInfo-EUTRA-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CellAssistanceInfo-EUTRA ::= CHOICE {

limitedEUTRA-List SEQUENCE (SIZE(1..maxnoofCellsinNG-RANnode)) OF E-UTRA-CGI,

full-List ENUMERATED {all-served-cells-E-UTRA, ...},

choice-extension ProtocolIE-Single-Container { {CellAssistanceInfo-EUTRA-ExtIEs} }

}

CellAssistanceInfo-EUTRA-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

CellBasedMDT-NR::= SEQUENCE {

cellIdListforMDT-NR CellIdListforMDT-NR,

iE-Extensions ProtocolExtensionContainer { {CellBasedMDT-NR-ExtIEs} } OPTIONAL,

...

}

CellBasedMDT-NR-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CellIdListforMDT-NR ::= SEQUENCE (SIZE(1..maxnoofCellIDforMDT)) OF NR-CGI

CellBasedMDT-EUTRA::= SEQUENCE {

cellIdListforMDT-EUTRA CellIdListforMDT-EUTRA,

iE-Extensions ProtocolExtensionContainer { {CellBasedMDT-EUTRA-ExtIEs} } OPTIONAL,

...

}

CellBasedMDT-EUTRA-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CellIdListforMDT-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellIDforMDT)) OF E-UTRA-CGI

CellCapacityClassValue ::= INTEGER (1..100,...)

CellGroupID ::= INTEGER (0..maxnoofSCellGroups)

CellMeasurementResult ::= SEQUENCE (SIZE(1..maxnoofCellsinNG-RANnode)) OF CellMeasurementResult-Item

CellMeasurementResult-Item ::= SEQUENCE {

cell-ID GlobalNG-RANCell-ID,

radioResourceStatus RadioResourceStatus OPTIONAL,

tNLCapacityIndicator TNLCapacityIndicator OPTIONAL,

compositeAvailableCapacityGroup CompositeAvailableCapacityGroup OPTIONAL,

sliceAvailableCapacity SliceAvailableCapacity OPTIONAL,

numberofActiveUEs NumberofActiveUEs OPTIONAL,

rRCConnections RRCConnections OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { CellMeasurementResult-Item-ExtIEs} } OPTIONAL,

...

}

CellMeasurementResult-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CellToReport ::= SEQUENCE (SIZE(1..maxnoofCellsinNG-RANnode)) OF CellToReport-Item

CellToReport-Item ::= SEQUENCE {

cell-ID GlobalNG-RANCell-ID,

sSBToReport-List SSBToReport-List OPTIONAL,

sliceToReport-List SliceToReport-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { CellToReport-Item-ExtIEs} } OPTIONAL,

...

}

CellToReport-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

Cell-Type-Choice ::= CHOICE {

ng-ran-e-utra E-UTRA-Cell-Identity,

ng-ran-nr NR-Cell-Identity,

e-utran E-UTRA-Cell-Identity,

choice-extension ProtocolIE-Single-Container { { Cell-Type-Choice-ExtIEs} }

}

Cell-Type-Choice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

CompositeAvailableCapacityGroup ::= SEQUENCE {

compositeAvailableCapacityDownlink CompositeAvailableCapacity,

compositeAvailableCapacityUplink CompositeAvailableCapacity,

iE-Extensions ProtocolExtensionContainer { { CompositeAvailableCapacityGroup-ExtIEs} } OPTIONAL,

...

}

CompositeAvailableCapacityGroup-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CompositeAvailableCapacity ::= SEQUENCE {

cellCapacityClassValue CellCapacityClassValue OPTIONAL,

capacityValueInfo CapacityValueInfo, -- this IE represents the IE "CapacityValue" in 9.2.2.a, it’s used to distinguish the "CapacityValue" in 9.2.2.c

iE-Extensions ProtocolExtensionContainer { { CompositeAvailableCapacity-ExtIEs} }OPTIONAL,

...

}

CompositeAvailableCapacity-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ControlPlaneTrafficType ::= INTEGER (1..3, ...)

CHO-MRDC-EarlyDataForwarding ::= ENUMERATED {stop, ...}

CHO-MRDC-Indicator ::= ENUMERATED {true, ...}

CHOtrigger ::= ENUMERATED {

cho-initiation,

cho-replace,

...

}

CHOinformation-Req ::= SEQUENCE {

cho-trigger CHOtrigger,

targetNG-RANnodeUEXnAPID NG-RANnodeUEXnAPID OPTIONAL

-- This IE shall be present if the cho-trigger IE is present and set to "CHO-replace" --,

cHO-EstimatedArrivalProbability CHO-Probability OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { CHOinformation-Req-ExtIEs} } OPTIONAL,

...

}

CHOinformation-Req-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

CHOinformation-Ack ::= SEQUENCE {

requestedTargetCellGlobalID Target-CGI,

maxCHOoperations MaxCHOpreparations OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { CHOinformation-Ack-ExtIEs} } OPTIONAL,

...

}

CHOinformation-Ack-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

CHO-Probability ::= INTEGER (1..100)

ConfiguredTACIndication ::= ENUMERATED {

true,

...

}

Connectivity-Support ::= SEQUENCE {

eNDC-Support ENUMERATED {supported, not-supported, ...},

iE-Extensions ProtocolExtensionContainer { {Connectivity-Support-ExtIEs} } OPTIONAL,

...

}

Connectivity-Support-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

COUNT-PDCP-SN12 ::= SEQUENCE {

pdcp-SN12 INTEGER (0..4095),

hfn-PDCP-SN12 INTEGER (0..1048575),

iE-Extensions ProtocolExtensionContainer { {COUNT-PDCP-SN12-ExtIEs} } OPTIONAL,

...

}

COUNT-PDCP-SN12-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

COUNT-PDCP-SN18 ::= SEQUENCE {

pdcp-SN18 INTEGER (0..262143),

hfn-PDCP-SN18 INTEGER (0..16383),

iE-Extensions ProtocolExtensionContainer { {COUNT-PDCP-SN18-ExtIEs} } OPTIONAL,

...

}

COUNT-PDCP-SN18-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CPTransportLayerInformation ::= CHOICE {

endpointIPAddress TransportLayerAddress,

choice-extension ProtocolIE-Single-Container { {CPTransportLayerInformation-ExtIEs} }

}

CPTransportLayerInformation-ExtIEs XNAP-PROTOCOL-IES ::= {

{ ID id-EndpointIPAddressAndPort CRITICALITY reject TYPE EndpointIPAddressAndPort PRESENCE mandatory},

...

}

CriticalityDiagnostics ::= SEQUENCE {

procedureCode ProcedureCode OPTIONAL,

triggeringMessage TriggeringMessage OPTIONAL,

procedureCriticality Criticality OPTIONAL,

iEsCriticalityDiagnostics CriticalityDiagnostics-IE-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {CriticalityDiagnostics-ExtIEs} } OPTIONAL,

...

}

CriticalityDiagnostics-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CriticalityDiagnostics-IE-List ::= SEQUENCE (SIZE (1..maxNrOfErrors)) OF

SEQUENCE {

iECriticality Criticality,

iE-ID ProtocolIE-ID,

typeOfError TypeOfError,

iE-Extensions ProtocolExtensionContainer { {CriticalityDiagnostics-IE-List-ExtIEs} } OPTIONAL,

...

}

CriticalityDiagnostics-IE-List-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

C-RNTI ::= BIT STRING (SIZE(16))

CyclicPrefix-E-UTRA-DL ::= ENUMERATED {

normal,

extended,

...

}

CyclicPrefix-E-UTRA-UL ::= ENUMERATED {

normal,

extended,

...

}

CSI-RSTransmissionIndication ::= ENUMERATED {

activated,

deactivated,

...

}

-- D

XnUAddressInfoperPDUSession-List ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF XnUAddressInfoperPDUSession-Item

XnUAddressInfoperPDUSession-Item ::= SEQUENCE {

pduSession-ID PDUSession-ID,

dataForwardingInfoFromTargetNGRANnode DataForwardingInfoFromTargetNGRANnode OPTIONAL,

pduSessionResourceSetupCompleteInfo-SNterm PDUSessionResourceBearerSetupCompleteInfo-SNterminated OPTIONAL,

iE-Extension ProtocolExtensionContainer { { XnUAddressInfoperPDUSession-Item-ExtIEs} } OPTIONAL,

...

}

XnUAddressInfoperPDUSession-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-SecondarydataForwardingInfoFromTarget-List CRITICALITY ignore EXTENSION SecondarydataForwardingInfoFromTarget-List PRESENCE optional}|

{ ID id-DRB-IDs-takenintouse CRITICALITY reject EXTENSION DRB-List PRESENCE optional}|

{ ID id-dataForwardingInfoFromTargetE-UTRANnode CRITICALITY ignore EXTENSION DataForwardingInfoFromTargetE-UTRANnode PRESENCE optional},

...

}

DataForwardingAccepted ::= ENUMERATED {data-forwarding-accepted, ...}

DataForwardingInfoFromTargetE-UTRANnode ::= SEQUENCE {

dataForwardingInfoFromTargetE-UTRANnode-List DataForwardingInfoFromTargetE-UTRANnode-List,

iE-Extension ProtocolExtensionContainer { { DataForwardingInfoFromTargetE-UTRANnode-ExtIEs} } OPTIONAL,

...

}

DataForwardingInfoFromTargetE-UTRANnode-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DataForwardingInfoFromTargetE-UTRANnode-List ::= SEQUENCE (SIZE(1.. maxnoofDataForwardingTunneltoE-UTRAN)) OF DataForwardingInfoFromTargetE-UTRANnode-Item

DataForwardingInfoFromTargetE-UTRANnode-Item ::= SEQUENCE {

dlForwardingUPTNLInformation UPTransportLayerInformation,

qosFlowsToBeForwarded-List QoSFlowsToBeForwarded-List,

iE-Extension ProtocolExtensionContainer { { DataForwardingInfoFromTargetE-UTRANnode-Item-ExtIEs} } OPTIONAL,

...

}

DataForwardingInfoFromTargetE-UTRANnode-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

QoSFlowsToBeForwarded-List ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF QoSFlowsToBeForwarded-Item

QoSFlowsToBeForwarded-Item ::= SEQUENCE {

qosFlowIdentifier QoSFlowIdentifier,

iE-Extension ProtocolExtensionContainer { { QoSFlowsToBeForwarded-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsToBeForwarded-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DataForwardingInfoFromTargetNGRANnode ::= SEQUENCE {

qosFlowsAcceptedForDataForwarding-List QoSFLowsAcceptedToBeForwarded-List,

pduSessionLevelDLDataForwardingInfo UPTransportLayerInformation OPTIONAL,

pduSessionLevelULDataForwardingInfo UPTransportLayerInformation OPTIONAL,

dataForwardingResponseDRBItemList DataForwardingResponseDRBItemList OPTIONAL,

iE-Extension ProtocolExtensionContainer { {DataForwardingInfoFromTargetNGRANnode-ExtIEs} } OPTIONAL,

...

}

DataForwardingInfoFromTargetNGRANnode-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

QoSFLowsAcceptedToBeForwarded-List ::= SEQUENCE (SIZE(1.. maxnoofQoSFlows)) OF QoSFLowsAcceptedToBeForwarded-Item

QoSFLowsAcceptedToBeForwarded-Item ::= SEQUENCE {

qosFlowIdentifier QoSFlowIdentifier,

iE-Extension ProtocolExtensionContainer { {QoSFLowsAcceptedToBeForwarded-Item-ExtIEs} } OPTIONAL,

...

}

QoSFLowsAcceptedToBeForwarded-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DataforwardingandOffloadingInfofromSource ::= SEQUENCE {

qosFlowsToBeForwarded QoSFLowsToBeForwarded-List,

sourceDRBtoQoSFlowMapping DRBToQoSFlowMapping-List OPTIONAL,

iE-Extension ProtocolExtensionContainer { {DataforwardingandOffloadingInfofromSource-ExtIEs} } OPTIONAL,

...

}

DataforwardingandOffloadingInfofromSource-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

QoSFLowsToBeForwarded-List ::= SEQUENCE (SIZE(1.. maxnoofQoSFlows)) OF QoSFLowsToBeForwarded-Item

QoSFLowsToBeForwarded-Item ::= SEQUENCE {

qosFlowIdentifier QoSFlowIdentifier,

dl-dataforwarding DLForwarding,

ul-dataforwarding ULForwarding,

iE-Extension ProtocolExtensionContainer { {QoSFLowsToBeForwarded-Item-ExtIEs} } OPTIONAL,

...

}

QoSFLowsToBeForwarded-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-ULForwardingProposal CRITICALITY ignore EXTENSION ULForwardingProposal PRESENCE optional },

...

}

DataForwardingResponseDRBItemList ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DataForwardingResponseDRBItem

DataForwardingResponseDRBItem ::= SEQUENCE {

drb-ID DRB-ID,

dlForwardingUPTNL UPTransportLayerInformation OPTIONAL,

ulForwardingUPTNL UPTransportLayerInformation OPTIONAL,

iE-Extension ProtocolExtensionContainer { {DataForwardingResponseDRBItem-ExtIEs} } OPTIONAL,

...

}

DataForwardingResponseDRBItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DataTrafficResources ::= BIT STRING (SIZE(6..17600))

DataTrafficResourceIndication ::= SEQUENCE {

activationSFN ActivationSFN,

sharedResourceType SharedResourceType,

reservedSubframePattern ReservedSubframePattern OPTIONAL,

iE-Extension ProtocolExtensionContainer { {DataTrafficResourceIndication-ExtIEs} } OPTIONAL,

...

}

DataTrafficResourceIndication-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DAPSRequestInfo ::= SEQUENCE {

dapsIndicator ENUMERATED {daps-HO-required, ...},

iE-Extensions ProtocolExtensionContainer { {DAPSRequestInfo-ExtIEs} } OPTIONAL,

...

}

DAPSRequestInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DAPSResponseInfo-List ::= SEQUENCE (SIZE (1..maxnoofDRBs)) OF DAPSResponseInfo-Item

DAPSResponseInfo-Item ::= SEQUENCE {

drbID DRB-ID,

dapsResponseIndicator ENUMERATED {daps-HO-accepted, daps-HO-not-accepted, ...},

iE-Extensions ProtocolExtensionContainer { {DAPSResponseInfo-Item-ExtIEs} } OPTIONAL,

...

}

DAPSResponseInfo-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DeliveryStatus ::= INTEGER (0..4095, ...)

DesiredActNotificationLevel ::= ENUMERATED {none, qos-flow, pdu-session, ue-level, ...}

DefaultDRB-Allowed ::= ENUMERATED {true, false, ...}

DLCountChoice ::= CHOICE {

count12bits COUNT-PDCP-SN12,

count18bits COUNT-PDCP-SN18,

choice-extension ProtocolIE-Single-Container { {DLCountChoice-ExtIEs} }

}

DLCountChoice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

DLForwarding ::= ENUMERATED {dl-forwarding-proposed, ...}

DL-GBR-PRB-usage::= INTEGER (0..100)

DL-non-GBR-PRB-usage::= INTEGER (0..100)

DLF1Term-BHInfo ::= SEQUENCE {

egressBAPRoutingID BAPRoutingID,

egressBHRLCCHID BHRLCChannelID,

iE-Extensions ProtocolExtensionContainer { { DLF1Term-BHInfo-ExtIEs} } OPTIONAL,

...

}

DLF1Term-BHInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DLNonF1Term-BHInfo ::= SEQUENCE {

ingressBAPRoutingID BAPRoutingID,

ingressBHRLCCHID BHRLCChannelID,

priorhopBAPAddress BAPAddress,

qosMappingInformation QoS-Mapping-Information,

iE-Extensions ProtocolExtensionContainer { { DLNonF1Term-BHInfo-ExtIEs} } OPTIONAL,

...

}

DLNonF1Term-BHInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DL-Total-PRB-usage::= INTEGER (0..100)

DRB-ID ::= INTEGER (1..32, ...)

DRB-List ::= SEQUENCE (SIZE (1..maxnoofDRBs)) OF DRB-ID

DRB-List-withCause ::= SEQUENCE (SIZE (1..maxnoofDRBs)) OF DRB-List-withCause-Item

DRB-List-withCause-Item ::= SEQUENCE {

drb-id DRB-ID,

cause Cause,

rLC-Mode RLCMode OPTIONAL,

iE-Extension ProtocolExtensionContainer { {DRB-List-withCause-Item-ExtIEs} } OPTIONAL,

...

}

DRB-List-withCause-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Number ::= INTEGER (1..32, ...)

DRBsSubjectToDLDiscarding-List ::= SEQUENCE (SIZE (1..maxnoofDRBs)) OF DRBsSubjectToDLDiscarding-Item

DRBsSubjectToDLDiscarding-Item ::= SEQUENCE {

drbID DRB-ID,

dlCount DLCountChoice,

iE-Extension ProtocolExtensionContainer { { DRBsSubjectToDLDiscarding-Item-ExtIEs} } OPTIONAL,

...

}

DRBsSubjectToDLDiscarding-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsSubjectToEarlyStatusTransfer-List ::= SEQUENCE (SIZE (1..maxnoofDRBs)) OF DRBsSubjectToEarlyStatusTransfer-Item

DRBsSubjectToEarlyStatusTransfer-Item ::= SEQUENCE {

drbID DRB-ID,

dlCount DLCountChoice,

iE-Extension ProtocolExtensionContainer { { DRBsSubjectToEarlyStatusTransfer-Item-ExtIEs} } OPTIONAL,

...

}

DRBsSubjectToEarlyStatusTransfer-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsSubjectToStatusTransfer-List ::= SEQUENCE (SIZE (1..maxnoofDRBs)) OF DRBsSubjectToStatusTransfer-Item

DRBsSubjectToStatusTransfer-Item ::= SEQUENCE {

drbID DRB-ID,

pdcpStatusTransfer-UL DRBBStatusTransferChoice,

pdcpStatusTransfer-DL DRBBStatusTransferChoice,

iE-Extension ProtocolExtensionContainer { {DRBsSubjectToStatusTransfer-Item-ExtIEs} } OPTIONAL,

...

}

DRBsSubjectToStatusTransfer-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-OldQoSFlowMap-ULendmarkerexpected CRITICALITY reject EXTENSION QoSFlows-List PRESENCE optional },

...

}

DRBBStatusTransferChoice ::= CHOICE {

pdcp-sn-12bits DRBBStatusTransfer12bitsSN,

pdcp-sn-18bits DRBBStatusTransfer18bitsSN,

choice-extension ProtocolIE-Single-Container { {DRBBStatusTransferChoice-ExtIEs} }

}

DRBBStatusTransferChoice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

DRBBStatusTransfer12bitsSN ::= SEQUENCE {

receiveStatusofPDCPSDU BIT STRING (SIZE(1..2048)) OPTIONAL,

cOUNTValue COUNT-PDCP-SN12,

iE-Extension ProtocolExtensionContainer { {DRBBStatusTransfer12bitsSN-ExtIEs} } OPTIONAL,

...

}

DRBBStatusTransfer12bitsSN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBBStatusTransfer18bitsSN ::= SEQUENCE {

receiveStatusofPDCPSDU BIT STRING (SIZE(1..131072)) OPTIONAL,

cOUNTValue COUNT-PDCP-SN18,

iE-Extension ProtocolExtensionContainer { {DRBBStatusTransfer18bitsSN-ExtIEs} } OPTIONAL,

...

}

DRBBStatusTransfer18bitsSN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBToQoSFlowMapping-List ::= SEQUENCE (SIZE (1..maxnoofDRBs)) OF DRBToQoSFlowMapping-Item

DRBToQoSFlowMapping-Item ::= SEQUENCE {

drb-ID DRB-ID,

qosFlows-List QoSFlows-List,

rLC-Mode RLCMode OPTIONAL,

iE-Extension ProtocolExtensionContainer { {DRBToQoSFlowMapping-Item-ExtIEs} } OPTIONAL,

...

}

DRBToQoSFlowMapping-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-DAPSRequestInfo CRITICALITY ignore EXTENSION DAPSRequestInfo PRESENCE optional },

...

}

DUF-Slot-Config-List ::= SEQUENCE (SIZE(1..maxnoofDUFSlots)) OF DUF-Slot-Config-Item

DUF-Slot-Config-Item ::= CHOICE {

explicitFormat ExplicitFormat,

implicitFormat ImplicitFormat,

choice-extension ProtocolIE-Single-Container { { DUF-Slot-Config-Item-ExtIEs} }

}

DUF-Slot-Config-Item-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

DUFSlotformatIndex ::= INTEGER(0..254)

DUFTransmissionPeriodicity ::= ENUMERATED { ms0p5, ms0p625, ms1, ms1p25, ms2, ms2p5, ms5, ms10, ...}

DU-RX-MT-RX ::= ENUMERATED {supported, not-supported, supported-FDM-required}

DU-TX-MT-TX ::= ENUMERATED {supported, not-supported, supported-FDM-required}

DU-RX-MT-TX ::= ENUMERATED {supported, not-supported, supported-FDM-required}

DU-TX-MT-RX ::= ENUMERATED {supported, not-supported, supported-FDM-required}

DuplicationActivation ::= ENUMERATED {active, inactive, ...}

Dynamic5QIDescriptor ::= SEQUENCE {

priorityLevelQoS PriorityLevelQoS,

packetDelayBudget PacketDelayBudget,

packetErrorRate PacketErrorRate,

fiveQI FiveQI OPTIONAL,

delayCritical ENUMERATED {delay-critical, non-delay-critical, ...} OPTIONAL,

-- This IE shall be present if the *GBR QoS Flow Information* IE is present in the *QoS Flow Level QoS Parameters* IE.

averagingWindow AveragingWindow OPTIONAL,

-- This IE shall be present if the *GBR QoS Flow Information* IE is present in the *QoS Flow Level QoS Parameters* IE.

maximumDataBurstVolume MaximumDataBurstVolume OPTIONAL,

iE-Extension ProtocolExtensionContainer { {Dynamic5QIDescriptor-ExtIEs } } OPTIONAL,

...

}

Dynamic5QIDescriptor-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-ExtendedPacketDelayBudget CRITICALITY ignore EXTENSION ExtendedPacketDelayBudget PRESENCE optional}|

{ ID id-CNPacketDelayBudgetDownlink CRITICALITY ignore EXTENSION ExtendedPacketDelayBudget PRESENCE optional}|

{ ID id-CNPacketDelayBudgetUplink CRITICALITY ignore EXTENSION ExtendedPacketDelayBudget PRESENCE optional},

...

}

-- E

E-RAB-ID ::= INTEGER (0..15, ...)

E-UTRAARFCN ::= INTEGER (0..maxEARFCN)

E-UTRA-Cell-Identity ::= BIT STRING (SIZE(28))

E-UTRA-CGI ::= SEQUENCE {

plmn-id PLMN-Identity,

e-utra-CI E-UTRA-Cell-Identity,

iE-Extension ProtocolExtensionContainer { {E-UTRA-CGI-ExtIEs} } OPTIONAL,

...

}

E-UTRA-CGI-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

E-UTRAFrequencyBandIndicator ::= INTEGER (1..256, ...)

E-UTRAMultibandInfoList ::= SEQUENCE (SIZE(1..maxnoofEUTRABands)) OF E-UTRAFrequencyBandIndicator

E-UTRAPCI ::= INTEGER (0..503, ...)

E-UTRAPRACHConfiguration ::= SEQUENCE {

rootSequenceIndex INTEGER (0..837),

zeroCorrelationIndex INTEGER (0..15),

highSpeedFlag ENUMERATED {true, false, ...},

prach-FreqOffset INTEGER (0..94),

prach-ConfigIndex INTEGER (0..63) OPTIONAL,

-- C-ifTDD: This IE shall be present if the EUTRA-Mode-Info IE in the Served Cell Information IE is set to the value "TDD" --

iE-Extensions ProtocolExtensionContainer { {E-UTRAPRACHConfiguration-ExtIEs} } OPTIONAL,

...

}

E-UTRAPRACHConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

E-UTRATransmissionBandwidth ::= ENUMERATED {bw6, bw15, bw25, bw50, bw75, bw100, ..., bw1}

EndpointIPAddressAndPort ::=SEQUENCE {

endpointIPAddress TransportLayerAddress,

portNumber PortNumber,

iE-Extensions ProtocolExtensionContainer { { EndpointIPAddressAndPort-ExtIEs} } OPTIONAL

}

EndpointIPAddressAndPort-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

EventTriggered ::= SEQUENCE {

loggedEventTriggeredConfig LoggedEventTriggeredConfig,

iE-Extensions ProtocolExtensionContainer { { EventTriggered-ExtIEs} } OPTIONAL,

...

}

EventTriggered-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

EventType ::= ENUMERATED {

report-upon-change-of-serving-cell,

report-UE-moving-presence-into-or-out-of-the-Area-of-Interest,

...,

report-upon-change-of-serving-cell-and-Area-of-Interest

}

EventTypeTrigger ::= CHOICE {

outOfCoverage ENUMERATED {true, ...},

eventL1 EventL1,

choice-Extensions ProtocolIE-Single-Container { {EventTypeTrigger-ExtIEs} }

}

EventTypeTrigger-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

EventL1 ::= SEQUENCE {

l1Threshold MeasurementThresholdL1LoggedMDT,

hysteresis Hysteresis,

timeToTrigger TimeToTrigger,

iE-Extensions ProtocolExtensionContainer { { EventL1-ExtIEs} } OPTIONAL,

...

}

EventL1-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

MeasurementThresholdL1LoggedMDT ::= CHOICE {

threshold-RSRP Threshold-RSRP,

threshold-RSRQ Threshold-RSRQ,

...

}

ExpectedActivityPeriod ::= INTEGER (1..30|40|50|60|80|100|120|150|180|181, ...)

ExpectedHOInterval ::= ENUMERATED {

sec15, sec30, sec60, sec90, sec120, sec180, long-time,

...

}

ExpectedIdlePeriod ::= INTEGER (1..30|40|50|60|80|100|120|150|180|181, ...)

ExpectedUEActivityBehaviour ::= SEQUENCE {

expectedActivityPeriod ExpectedActivityPeriod OPTIONAL,

expectedIdlePeriod ExpectedIdlePeriod OPTIONAL,

sourceOfUEActivityBehaviourInformation SourceOfUEActivityBehaviourInformation OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ExpectedUEActivityBehaviour-ExtIEs} } OPTIONAL,

...

}

ExpectedUEActivityBehaviour-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ExpectedUEBehaviour ::= SEQUENCE {

expectedUEActivityBehaviour ExpectedUEActivityBehaviour OPTIONAL,

expectedHOInterval ExpectedHOInterval OPTIONAL,

expectedUEMobility ExpectedUEMobility OPTIONAL,

expectedUEMovingTrajectory ExpectedUEMovingTrajectory OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ExpectedUEBehaviour-ExtIEs} } OPTIONAL,

...

}

ExpectedUEBehaviour-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ExpectedUEMobility ::= ENUMERATED {

stationary,

mobile,

...

}

ExpectedUEMovingTrajectory ::= SEQUENCE (SIZE(1..maxnoofCellsUEMovingTrajectory)) OF ExpectedUEMovingTrajectoryItem

ExpectedUEMovingTrajectoryItem ::= SEQUENCE {

nGRAN-CGI GlobalNG-RANCell-ID,

timeStayedInCell INTEGER (0..4095) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ExpectedUEMovingTrajectoryItem-ExtIEs} } OPTIONAL,

...

}

ExpectedUEMovingTrajectoryItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SourceOfUEActivityBehaviourInformation ::= ENUMERATED {

subscription-information,

statistics,

...

}

ExplicitFormat ::= SEQUENCE {

permutation Permutation,

noofDownlinkSymbols INTEGER(0..14) OPTIONAL,

noofUplinkSymbols INTEGER(0..14) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ExplicitFormat-ExtIEs} } OPTIONAL,

...

}

ExplicitFormat-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ExtendedRATRestrictionInformation ::= SEQUENCE {

primaryRATRestriction BIT STRING (SIZE(8, ...)),

secondaryRATRestriction BIT STRING (SIZE(8, ...)),

iE-Extensions ProtocolExtensionContainer { {ExtendedRATRestrictionInformation-ExtIEs} } OPTIONAL,

...

}

ExtendedRATRestrictionInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ExtendedPacketDelayBudget ::= INTEGER (0..65535, ...)

ExtendedSliceSupportList ::= SEQUENCE (SIZE(1..maxnoofExtSliceItems)) OF S-NSSAI

ExtendedUEIdentityIndexValue ::= BIT STRING (SIZE(16))

ExtTLAs ::= SEQUENCE (SIZE(1..maxnoofExtTLAs)) OF ExtTLA-Item

ExtTLA-Item ::= SEQUENCE {

iPsecTLA TransportLayerAddress OPTIONAL,

gTPTransportLayerAddresses GTPTLAs OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ExtTLA-Item-ExtIEs} } OPTIONAL,

...

}

ExtTLA-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

GTPTLAs ::= SEQUENCE (SIZE(1.. maxnoofGTPTLAs)) OF GTPTLA-Item

GTPTLA-Item ::= SEQUENCE {

gTPTransportLayerAddresses TransportLayerAddress,

iE-Extensions ProtocolExtensionContainer { { GTPTLA-Item-ExtIEs } } OPTIONAL,

...

}

GTPTLA-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- F

F1CTrafficContainer ::= OCTET STRING

F1-TerminatingTopologyBHInformation ::= SEQUENCE {

f1TerminatingBHInformation-List F1TerminatingBHInformation-List,

iE-Extensions ProtocolExtensionContainer { {F1-TerminatingTopologyBHInformation-ExtIEs} } OPTIONAL,

...

}

F1-TerminatingTopologyBHInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

F1TerminatingBHInformation-List ::= SEQUENCE (SIZE(1..maxnoofBHInfo)) OF F1TerminatingBHInformation-Item

F1TerminatingBHInformation-Item ::= SEQUENCE {

bHInfoIndex BHInfoIndex,

dLTNLAddress IABTNLAddress,

dlF1TermBHInfo DLF1Term-BHInfo OPTIONAL,

ulF1TermBHInfo ULF1Term-BHInfo OPTIONAL,

iE-Extension ProtocolExtensionContainer { { F1TerminatingBHInformation-Item-ExtIEs} } OPTIONAL,

...

}

F1TerminatingBHInformation-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

FiveGCMobilityRestrictionListContainer ::= OCTET STRING

-- This octets of the OCTET STRING contain the Mobility Restriction List IE as specified in TS 38.413 [5]. --

FiveQI ::= INTEGER (0..255, ...)

FreqDomainHSNAconfiguration-List ::= SEQUENCE (SIZE(1.. maxnoofHSNASlots)) OF FreqDomainHSNAconfiguration-List-Item

FreqDomainHSNAconfiguration-List-Item ::= SEQUENCE {

rBsetIndex INTEGER(1.. maxnoofRBsetsPerCell),

freqDomainSlotHSNAconfiguration-List FreqDomainSlotHSNAconfiguration-List,

iE-Extensions ProtocolExtensionContainer { { FreqDomainHSNAconfiguration-List-Item-ExtIEs} } OPTIONAL,

...

}

FreqDomainHSNAconfiguration-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

FreqDomainSlotHSNAconfiguration-List ::= SEQUENCE (SIZE(1.. maxnoofHSNASlots)) OF FreqDomainSlotHSNAconfiguration-List-Item

FreqDomainSlotHSNAconfiguration-List-Item ::= SEQUENCE {

slotIndex INTEGER(1..maxnoofHSNASlots), hSNADownlink HSNADownlink OPTIONAL,

hSNAUplink HSNAUplink OPTIONAL,

hSNAFlexible HSNAFlexible OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { FreqDomainSlotHSNAconfiguration-List-Item-ExtIEs} } OPTIONAL,

...

}

FreqDomainSlotHSNAconfiguration-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

FrequencyShift7p5khz ::= ENUMERATED {false, true, ...}

-- G

GBRQoSFlowInfo ::= SEQUENCE {

maxFlowBitRateDL BitRate,

maxFlowBitRateUL BitRate,

guaranteedFlowBitRateDL BitRate,

guaranteedFlowBitRateUL BitRate,

notificationControl ENUMERATED {notification-requested, ...} OPTIONAL,

maxPacketLossRateDL PacketLossRate OPTIONAL,

maxPacketLossRateUL PacketLossRate OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {GBRQoSFlowInfo-ExtIEs} } OPTIONAL,

...

}

GBRQoSFlowInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-AlternativeQoSParaSetList CRITICALITY ignore EXTENSION AlternativeQoSParaSetList PRESENCE optional },

...

}

GlobalgNB-ID ::= SEQUENCE {

plmn-id PLMN-Identity,

gnb-id GNB-ID-Choice,

iE-Extensions ProtocolExtensionContainer { {GlobalgNB-ID-ExtIEs} } OPTIONAL,

...

}

GlobalgNB-ID-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

GNB-DU-Cell-Resource-Configuration ::= SEQUENCE {

subcarrierSpacing SSB-subcarrierSpacing,

dUFTransmissionPeriodicity DUFTransmissionPeriodicity OPTIONAL,

dUF-Slot-Config-List DUF-Slot-Config-List OPTIONAL,

hSNATransmissionPeriodicity HSNATransmissionPeriodicity OPTIONAL,

hNSASlotConfigList HSNASlotConfigList OPTIONAL,

rBsetConfiguration RBsetConfiguration OPTIONAL,

freqDomainHSNAconfiguration-List FreqDomainHSNAconfiguration-List OPTIONAL,

nACellResourceConfigurationList NACellResourceConfigurationList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { GNB-DU-Cell-Resource-Configuration-ExtIEs } } OPTIONAL,

...

}

GNB-DU-Cell-Resource-Configuration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

GNB-ID-Choice ::= CHOICE {

gnb-ID BIT STRING (SIZE(22..32)),

choice-extension ProtocolIE-Single-Container { {GNB-ID-Choice-ExtIEs} }

}

GNB-ID-Choice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

GNB-RadioResourceStatus ::= SEQUENCE {

ssbAreaRadioResourceStatus-List SSBAreaRadioResourceStatus-List,

iE-Extensions ProtocolExtensionContainer { { GNB-RadioResourceStatus-ExtIEs} } OPTIONAL,

...

}

GNB-RadioResourceStatus-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

GlobalCell-ID ::= SEQUENCE {

plmn-id PLMN-Identity,

cell-type Cell-Type-Choice,

iE-Extensions ProtocolExtensionContainer { { GlobalCell-ID-ExtIEs} } OPTIONAL,

...

}

GlobalCell-ID-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

GlobalngeNB-ID ::= SEQUENCE {

plmn-id PLMN-Identity,

enb-id ENB-ID-Choice,

iE-Extensions ProtocolExtensionContainer { {GlobaleNB-ID-ExtIEs} } OPTIONAL,

...

}

GlobaleNB-ID-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ENB-ID-Choice ::= CHOICE {

enb-ID-macro BIT STRING (SIZE(20)),

enb-ID-shortmacro BIT STRING (SIZE(18)),

enb-ID-longmacro BIT STRING (SIZE(21)),

choice-extension ProtocolIE-Single-Container { {ENB-ID-Choice-ExtIEs} }

}

ENB-ID-Choice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

GlobalNG-RANCell-ID ::= SEQUENCE {

plmn-id PLMN-Identity,

ng-RAN-Cell-id NG-RAN-Cell-Identity,

iE-Extensions ProtocolExtensionContainer { {GlobalNG-RANCell-ID-ExtIEs} } OPTIONAL,

...

}

GlobalNG-RANCell-ID-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

GlobalNG-RANNode-ID ::= CHOICE {

gNB GlobalgNB-ID,

ng-eNB GlobalngeNB-ID,

choice-extension ProtocolIE-Single-Container { {GlobalNG-RANNode-ID-ExtIEs} }

}

GlobalNG-RANNode-ID-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

GTP-TEID ::= OCTET STRING (SIZE(4))

GTPtunnelTransportLayerInformation ::= SEQUENCE {

tnl-address TransportLayerAddress,

gtp-teid GTP-TEID,

iE-Extensions ProtocolExtensionContainer { {GTPtunnelTransportLayerInformation-ExtIEs} } OPTIONAL,

...

}

GTPtunnelTransportLayerInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

GUAMI ::= SEQUENCE {

plmn-ID PLMN-Identity,

amf-region-id BIT STRING (SIZE (8)),

amf-set-id BIT STRING (SIZE (10)),

amf-pointer BIT STRING (SIZE (6)),

iE-Extensions ProtocolExtensionContainer { {GUAMI-ExtIEs} } OPTIONAL,

...

}

GUAMI-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- H

HandoverReportType ::= ENUMERATED {

hoTooEarly,

hoToWrongCell,

intersystempingpong,

...

}

HSNASlotConfigList ::= SEQUENCE (SIZE(1..maxnoofHSNASlots)) OF HSNASlotConfigItem

HSNASlotConfigItem ::= SEQUENCE {

hSNADownlink HSNADownlink OPTIONAL,

hSNAUplink HSNAUplink OPTIONAL,

hSNAFlexible HSNAFlexible OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { HSNASlotConfigItem-ExtIEs } } OPTIONAL,

...

}

HSNASlotConfigItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

HSNADownlink ::= ENUMERATED { hard, soft, notavailable }

HSNAFlexible ::= ENUMERATED { hard, soft, notavailable }

HSNAUplink ::= ENUMERATED { hard, soft, notavailable }

HSNATransmissionPeriodicity ::= ENUMERATED { ms0p5, ms0p625, ms1, ms1p25, ms2, ms2p5, ms5, ms10, ms20, ms40, ms80, ms160, ...}

Hysteresis ::= INTEGER (0..30)

-- I

IABCellInformation::= SEQUENCE{

nRCGI NR-CGI,

iAB-DU-Cell-Resource-Configuration-Mode-Info IAB-DU-Cell-Resource-Configuration-Mode-Info OPTIONAL,

iAB-STC-Info IAB-STC-Info OPTIONAL,

rACH-Config-Common RACH-Config-Common OPTIONAL,

rACH-Config-Common-IAB RACH-Config-Common-IAB OPTIONAL,

cSI-RS-Configuration OCTET STRING OPTIONAL,

sR-Configuration OCTET STRING OPTIONAL,

pDCCH-ConfigSIB1 OCTET STRING OPTIONAL,

sCS-Common OCTET STRING OPTIONAL,

multiplexingInfo MultiplexingInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { IABCellInformation-ExtIEs} } OPTIONAL,

...

}

IABCellInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IAB-DU-Cell-Resource-Configuration-Mode-Info ::= CHOICE {

tDD IAB-DU-Cell-Resource-Configuration-TDD-Info,

fDD IAB-DU-Cell-Resource-Configuration-FDD-Info,

choice-extension ProtocolIE-Single-Container { { IAB-DU-Cell-Resource-Configuration-Mode-Info-ExtIEs} }

}

IAB-DU-Cell-Resource-Configuration-Mode-Info-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

IAB-DU-Cell-Resource-Configuration-FDD-Info ::= SEQUENCE {

gNB-DU-Cell-Resource-Configuration-FDD-UL GNB-DU-Cell-Resource-Configuration,

gNB-DU-Cell-Resource-Configuration-FDD-DL GNB-DU-Cell-Resource-Configuration,

uLFrequencyInfo NRFrequencyInfo OPTIONAL,

dLFrequencyInfo NRFrequencyInfo OPTIONAL,

uLTransmissionBandwidth NRTransmissionBandwidth OPTIONAL,

dlTransmissionBandwidth NRTransmissionBandwidth OPTIONAL,

uLCarrierList NRCarrierList OPTIONAL,

dlCarrierList NRCarrierList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {IAB-DU-Cell-Resource-Configuration-FDD-Info-ExtIEs} } OPTIONAL,

...

}

IAB-DU-Cell-Resource-Configuration-FDD-Info-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IAB-DU-Cell-Resource-Configuration-TDD-Info ::= SEQUENCE {

gNB-DU-Cell-Resource-Configuration-TDD GNB-DU-Cell-Resource-Configuration,

frequencyInfo NRFrequencyInfo OPTIONAL,

transmissionBandwidth NRTransmissionBandwidth OPTIONAL,

carrierList NRCarrierList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {IAB-DU-Cell-Resource-Configuration-TDD-Info-ExtIEs} } OPTIONAL,

...

}

IAB-DU-Cell-Resource-Configuration-TDD-Info-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IAB-MT-Cell-List ::= SEQUENCE (SIZE(1..maxnoofServingCells)) OF IAB-MT-Cell-List-Item

IAB-MT-Cell-List-Item ::= SEQUENCE {

nRCellIdentity NR-Cell-Identity,

dU-RX-MT-RX DU-RX-MT-RX,

dU-TX-MT-TX DU-TX-MT-TX,

dU-RX-MT-TX DU-RX-MT-TX,

dU-TX-MT-RX DU-TX-MT-RX,

iE-Extensions ProtocolExtensionContainer { { IAB-MT-Cell-List-Item-ExtIEs } } OPTIONAL,

...

}

IAB-MT-Cell-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IABNodeIndication ::= ENUMERATED {true,...}

IAB-STC-Info ::= SEQUENCE{

iAB-STC-Info-List IAB-STC-Info-List,

iE-Extensions ProtocolExtensionContainer { { IAB-STC-Info-ExtIEs } } OPTIONAL,

...

}

IAB-STC-Info-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IAB-STC-Info-List ::= SEQUENCE (SIZE(1..maxnoofIABSTCInfo)) OF IAB-STC-Info-Item

IAB-STC-Info-Item::= SEQUENCE {

sSB-freqInfo SSB-freqInfo,

sSB-subcarrierSpacing SSB-subcarrierSpacing,

sSB-transmissionPeriodicity SSB-transmissionPeriodicity,

sSB-transmissionTimingOffset SSB-transmissionTimingOffset,

sSB-transmissionBitmap SSB-transmissionBitmap,

iE-Extensions ProtocolExtensionContainer { { IAB-STC-Info-Item-ExtIEs } } OPTIONAL,

...

}

IAB-STC-Info-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IAB-TNL-Address-Request ::= SEQUENCE {

iABIPv4AddressesRequested IABTNLAddressesRequested,

iABIPv6RequestType IABIPv6RequestType,

iABTNLAddressToRemove-List IABTNLAddressToRemove-List,

iE-Extensions ProtocolExtensionContainer { {IAB-TNL-Address-Request-ExtIEs} } OPTIONAL,

...

}

IAB-TNL-Address-Request-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IABIPv6RequestType ::= CHOICE {

iPv6Address IABTNLAddressesRequested,

iPv6Prefix IABTNLAddressesRequested,

choice-extension ProtocolIE-Single-Container { {IABIPv6RequestType-ExtIEs} }

}

IABIPv6RequestType-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

IAB-TNL-Address-Response ::= SEQUENCE {

iABAllocatedTNLAddress-List IABAllocatedTNLAddress-List,

iE-Extensions ProtocolExtensionContainer { {IAB-TNL-Address-Response-ExtIEs} } OPTIONAL,

...

}

IAB-TNL-Address-Response-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IABAllocatedTNLAddress-List ::= SEQUENCE (SIZE(1..maxnoofTLAsIAB)) OF IABAllocatedTNLAddress-Item

IABAllocatedTNLAddress-Item ::= SEQUENCE {

iABTNLAddress IABTNLAddress,

iABTNLAddressUsage IABTNLAddressUsage OPTIONAL,

associatedDonorDUAddress BAPAddress OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {IABAllocatedTNLAddress-Item-ExtIEs} } OPTIONAL,

...

}

IABAllocatedTNLAddress-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IABTNLAddress ::= CHOICE {

iPv4Address BIT STRING (SIZE(32)),

iPv6Address BIT STRING (SIZE(128)),

iPv6Prefix BIT STRING (SIZE(64)),

choice-extension ProtocolIE-Single-Container { {IABTNLAddress-ExtIEs} }

}

IABTNLAddress-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

IABTNLAddressesRequested ::= SEQUENCE {

tNLAddressesOrPrefixesRequestedAllTraffic INTEGER (1..256) OPTIONAL,

tNLAddressesOrPrefixesRequestedF1-C INTEGER (1..256) OPTIONAL,

tNLAddressesOrPrefixesRequestedF1-U INTEGER (1..256) OPTIONAL,

tNLAddressesOrPrefixesRequestedNoNF1 INTEGER (1..256) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {IABTNLAddressesRequested-ExtIEs} } OPTIONAL

}

IABTNLAddressesRequested-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IABTNLAddressToRemove-List ::= SEQUENCE (SIZE(1..maxnoofTLAsIAB)) OF IABTNLAddressToRemove-Item

IABTNLAddressToRemove-Item ::= SEQUENCE {

iABTNLAddress IABTNLAddress,

iE-Extension ProtocolExtensionContainer { {IABTNLAddressToRemove-Item-ExtIEs} } OPTIONAL,

...

}

IABTNLAddressToRemove-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

IABTNLAddressUsage ::= ENUMERATED {

f1-c,

f1-u,

non-f1,

...

}

IABTNLAddressException ::= SEQUENCE (SIZE(1..maxnoofTLAsIAB)) OF IABTNLAddress-Item

IABTNLAddress-Item ::= SEQUENCE {

iABTNLAddress IABTNLAddress OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { IABTNLAddress-ItemExtIEs } } OPTIONAL,

...}

IABTNLAddress-ItemExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ImmediateMDT-EUTRA ::= OCTET STRING

ImmediateMDT-NR ::= SEQUENCE {

measurementsToActivate MeasurementsToActivate,

m1Configuration M1Configuration OPTIONAL,

m4Configuration M4Configuration OPTIONAL,

m5Configuration M5Configuration OPTIONAL,

mDT-Location-Info MDT-Location-Info OPTIONAL,

m6Configuration M6Configuration OPTIONAL,

m7Configuration M7Configuration OPTIONAL,

bluetoothMeasurementConfiguration BluetoothMeasurementConfiguration OPTIONAL,

wLANMeasurementConfiguration WLANMeasurementConfiguration OPTIONAL,

sensorMeasurementConfiguration SensorMeasurementConfiguration OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ImmediateMDT-NR-ExtIEs} } OPTIONAL,

...

}

ImmediateMDT-NR-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ImplicitFormat ::= SEQUENCE {

dUFSlotformatIndex DUFSlotformatIndex,

iE-Extensions ProtocolExtensionContainer { { ImplicitFormat-ExtIEs } } OPTIONAL,

...

}

ImplicitFormat-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

InitiatingCondition-FailureIndication ::= CHOICE {

rRCReestab RRCReestab-initiated,

rRCSetup RRCSetup-initiated,

choice-extension ProtocolIE-Single-Container { {InitiatingCondition-FailureIndication-ExtIEs} }

}

InitiatingCondition-FailureIndication-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

IntendedTDD-DL-ULConfiguration-NR ::= SEQUENCE {

nrscs NRSCS,

nrCyclicPrefix NRCyclicPrefix,

nrDL-ULTransmissionPeriodicity NRDL-ULTransmissionPeriodicity,

slotConfiguration-List SlotConfiguration-List,

iE-Extensions ProtocolExtensionContainer { {IntendedTDD-DL-ULConfiguration-NR-ExtIEs} } OPTIONAL,

...

}

IntendedTDD-DL-ULConfiguration-NR-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

InterfaceInstanceIndication ::= INTEGER (0..255, ...)

InterfacesToTrace ::= BIT STRING { ng-c (0), x-nc (1), uu (2), f1-c (3), e1 (4)} (SIZE(8))

I-RNTI ::= CHOICE {

i-RNTI-full BIT STRING (SIZE(40)),

i-RNTI-short BIT STRING (SIZE(24)),

choice-extension ProtocolIE-Single-Container { {I-RNTI-ExtIEs} }

}

I-RNTI-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

-- J

-- K

-- L

LastVisitedCell-Item ::= CHOICE {

nG-RAN-Cell LastVisitedNGRANCellInformation,

e-UTRAN-Cell LastVisitedEUTRANCellInformation,

uTRAN-Cell LastVisitedUTRANCellInformation,

gERAN-Cell LastVisitedGERANCellInformation,

choice-extension ProtocolIE-Single-Container { { LastVisitedCell-Item-ExtIEs} }

}

LastVisitedCell-Item-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

LastVisitedEUTRANCellInformation ::= OCTET STRING

LastVisitedGERANCellInformation ::= OCTET STRING

LastVisitedNGRANCellInformation ::= OCTET STRING

LastVisitedUTRANCellInformation ::= OCTET STRING

LCID ::= INTEGER (1..32, ...)

Links-to-log ::= ENUMERATED {uplink, downlink, both-uplink-and-downlink, ...}

ListOfCells ::= SEQUENCE (SIZE(1..maxnoofCellsinAoI)) OF CellsinAoI-Item

CellsinAoI-Item ::= SEQUENCE {

pLMN-Identity PLMN-Identity,

ng-ran-cell-id NG-RAN-Cell-Identity,

iE-Extensions ProtocolExtensionContainer { {CellsinAoI-Item-ExtIEs} } OPTIONAL,

...

}

CellsinAoI-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ListOfRANNodesinAoI ::= SEQUENCE (SIZE(1.. maxnoofRANNodesinAoI)) OF GlobalNG-RANNodesinAoI-Item

GlobalNG-RANNodesinAoI-Item ::= SEQUENCE {

global-NG-RAN-Node-ID GlobalNG-RANNode-ID,

iE-Extensions ProtocolExtensionContainer { {GlobalNG-RANNodesinAoI-Item-ExtIEs} } OPTIONAL,

...

}

GlobalNG-RANNodesinAoI-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ListOfTAIsinAoI ::= SEQUENCE (SIZE(1..maxnoofTAIsinAoI)) OF TAIsinAoI-Item

TAIsinAoI-Item ::= SEQUENCE {

pLMN-Identity PLMN-Identity,

tAC TAC,

iE-Extensions ProtocolExtensionContainer { {TAIsinAoI-Item-ExtIEs} } OPTIONAL,

...

}

TAIsinAoI-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

LocationInformationSNReporting ::= ENUMERATED {

pSCell,

...

}

LocationReportingInformation ::= SEQUENCE {

eventType EventType,

reportArea ReportArea,

areaOfInterest AreaOfInterestInformation OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {LocationReportingInformation-ExtIEs} } OPTIONAL,

...

}

LocationReportingInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

{ ID id-AdditionLocationInformation CRITICALITY ignore EXTENSION AdditionLocationInformation PRESENCE optional},

...

}

LoggedMDT-EUTRA ::= SEQUENCE {

loggingInterval LoggingInterval,

loggingDuration LoggingDuration,

bluetoothMeasurementConfiguration BluetoothMeasurementConfiguration OPTIONAL,

wLANMeasurementConfiguration WLANMeasurementConfiguration OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {LoggedMDT-EUTRA-ExtIEs} } OPTIONAL,

...

}

LoggedMDT-EUTRA-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

LoggedEventTriggeredConfig ::= SEQUENCE {

eventTypeTrigger EventTypeTrigger,

iE-Extensions ProtocolExtensionContainer { { LoggedEventTriggeredConfig-ExtIEs} } OPTIONAL,

...

}

LoggedEventTriggeredConfig-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

LoggedMDT-NR ::= SEQUENCE {

loggingInterval LoggingInterval,

loggingDuration LoggingDuration,

reportType ReportType,

bluetoothMeasurementConfiguration BluetoothMeasurementConfiguration OPTIONAL,

wLANMeasurementConfiguration WLANMeasurementConfiguration OPTIONAL,

sensorMeasurementConfiguration SensorMeasurementConfiguration OPTIONAL,

areaScopeOfNeighCellsList AreaScopeOfNeighCellsList OPTIONAL, iE-Extensions ProtocolExtensionContainer { {LoggedMDT-NR-ExtIEs} } OPTIONAL,

...

}

LoggedMDT-NR-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

LoggingInterval ::= ENUMERATED { ms320, ms640, ms1280, ms2560, ms5120, ms10240, ms20480, ms30720, ms40960, ms61440}

LoggingDuration ::= ENUMERATED {m10, m20, m40, m60, m90, m120}

LowerLayerPresenceStatusChange ::= ENUMERATED {

release-lower-layers,

re-establish-lower-layers,

...,

suspend-lower-layers,

resume-lower-layers

}

LTEV2XServicesAuthorized ::= SEQUENCE {

vehicleUE VehicleUE OPTIONAL,

pedestrianUE PedestrianUE OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {LTEV2XServicesAuthorized-ExtIEs} } OPTIONAL,

...

}

LTEV2XServicesAuthorized-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

LTEUESidelinkAggregateMaximumBitRate ::= SEQUENCE {

uESidelinkAggregateMaximumBitRate BitRate,

iE-Extensions ProtocolExtensionContainer { {LTEUESidelinkAggregateMaximumBitRate-ExtIEs} } OPTIONAL,

...

}

LTEUESidelinkAggregateMaximumBitRate-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- M

M1Configuration ::= SEQUENCE {

m1reportingTrigger M1ReportingTrigger,

m1thresholdeventA2 M1ThresholdEventA2 OPTIONAL,

-- Included in case of event-triggered, or event-triggered periodic reporting for measurement M1

m1periodicReporting M1PeriodicReporting OPTIONAL,

-- Included in case of periodic or event-triggered periodic reporting

iE-Extensions ProtocolExtensionContainer { { M1Configuration-ExtIEs} } OPTIONAL,

...

}

M1Configuration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

M1PeriodicReporting ::= SEQUENCE {

reportInterval ReportIntervalMDT,

reportAmount ReportAmountMDT,

iE-Extensions ProtocolExtensionContainer { { M1PeriodicReporting-ExtIEs} } OPTIONAL,

...

}

M1PeriodicReporting-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

M1ReportingTrigger ::= ENUMERATED{

periodic,

a2eventtriggered,

a2eventtriggered-periodic,

...

}

M1ThresholdEventA2 ::= SEQUENCE {

measurementThreshold MeasurementThresholdA2,

iE-Extensions ProtocolExtensionContainer { { M1ThresholdEventA2-ExtIEs} } OPTIONAL,

...

}

M1ThresholdEventA2-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

M4Configuration ::= SEQUENCE {

m4period M4period,

m4-links-to-log Links-to-log,

iE-Extensions ProtocolExtensionContainer { { M4Configuration-ExtIEs} } OPTIONAL,

...

}

M4Configuration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

M4period ::= ENUMERATED {ms1024, ms2048, ms5120, ms10240, min1, ... }

M5Configuration ::= SEQUENCE {

m5period M5period,

m5-links-to-log Links-to-log,

iE-Extensions ProtocolExtensionContainer { { M5Configuration-ExtIEs} } OPTIONAL,

...

}

M5Configuration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

M5period ::= ENUMERATED {ms1024, ms2048, ms5120, ms10240, min1, ... }

M6Configuration ::= SEQUENCE {

m6report-Interval M6report-Interval,

m6-links-to-log Links-to-log,

iE-Extensions ProtocolExtensionContainer { { M6Configuration-ExtIEs} } OPTIONAL,

...

}

M6Configuration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

M6report-Interval ::= ENUMERATED { ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240, ms20480, ms40960, min1, min6, min12, min30,... }

M7Configuration ::= SEQUENCE {

m7period M7period,

m7-links-to-log Links-to-log,

iE-Extensions ProtocolExtensionContainer { { M7Configuration-ExtIEs} } OPTIONAL,

...

}

M7Configuration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

M7period ::= INTEGER(1..60, ...)

MAC-I ::= BIT STRING (SIZE(16))

MaskedIMEISV ::= BIT STRING (SIZE(64))

MaxCHOpreparations ::= INTEGER (1..8, ...)

MaximumDataBurstVolume ::= INTEGER (0..4095, ..., 4096.. 2000000)

MaximumIPdatarate ::= SEQUENCE {

maxIPrate-UL MaxIPrate,

iE-Extensions ProtocolExtensionContainer { {MaximumIPdatarate-ExtIEs} } OPTIONAL,

...

}

MaximumIPdatarate-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-MaxIPrate-DL CRITICALITY ignore EXTENSION MaxIPrate PRESENCE optional},

...

}

MaxIPrate ::= ENUMERATED {

bitrate64kbs,

max-UErate,

...

}

MBSFNControlRegionLength ::= INTEGER (0..3)

MBSFNSubframeAllocation-E-UTRA ::= CHOICE {

oneframe BIT STRING (SIZE(6)),

fourframes BIT STRING (SIZE(24)),

choice-extension ProtocolIE-Single-Container { {MBSFNSubframeAllocation-E-UTRA-ExtIEs} }

}

MBSFNSubframeAllocation-E-UTRA-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

MBSFNSubframeInfo-E-UTRA ::= SEQUENCE (SIZE(1..maxnoofMBSFNEUTRA)) OF MBSFNSubframeInfo-E-UTRA-Item

MBSFNSubframeInfo-E-UTRA-Item ::= SEQUENCE {

radioframeAllocationPeriod ENUMERATED{n1,n2,n4,n8,n16,n32,...},

radioframeAllocationOffset INTEGER (0..7, ...),

subframeAllocation MBSFNSubframeAllocation-E-UTRA,

iE-Extensions ProtocolExtensionContainer { {MBSFNSubframeInfo-E-UTRA-Item-ExtIEs} } OPTIONAL,

...

}

MBSFNSubframeInfo-E-UTRA-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

MDT-Activation ::= ENUMERATED {

immediate-MDT-only,

immediate-MDT-and-Trace,

logged-MDT-only,

...

}

MDT-Configuration ::= SEQUENCE {

mDT-Configuration-NR MDT-Configuration-NR OPTIONAL,

mDT-Configuration-EUTRA MDT-Configuration-EUTRA OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { MDT-Configuration-ExtIEs} } OPTIONAL,

...

}

MDT-Configuration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

MDT-Configuration-NR ::= SEQUENCE {

mdt-Activation MDT-Activation,

areaScopeOfMDT-NR AreaScopeOfMDT-NR OPTIONAL,

mDTMode-NR MDTMode-NR,

signallingBasedMDTPLMNList MDTPLMNList,

iE-Extensions ProtocolExtensionContainer { { MDT-Configuration-NR-ExtIEs} } OPTIONAL,

...

}

MDT-Configuration-NR-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

MDT-Configuration-EUTRA ::= SEQUENCE {

mdt-Activation MDT-Activation,

areaScopeOfMDT-EUTRA AreaScopeOfMDT-EUTRA OPTIONAL,

mDTMode-EUTRA MDTMode-EUTRA,

signallingBasedMDTPLMNList MDTPLMNList,

iE-Extensions ProtocolExtensionContainer { { MDT-Configuration-EUTRA-ExtIEs} } OPTIONAL,

...

}

MDT-Configuration-EUTRA-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

MDT-Location-Info ::= BIT STRING (SIZE (8))

MDTPLMNList ::= SEQUENCE (SIZE(1..maxnoofMDTPLMNs)) OF PLMN-Identity

MDTMode-NR ::= CHOICE {

immediateMDT ImmediateMDT-NR,

loggedMDT LoggedMDT-NR,

...,

mDTMode-NR-Extension MDTMode-NR-Extension

}

MDTMode-NR-Extension ::= ProtocolIE-Single-Container {{ MDTMode-NR-ExtensionIE }}

MDTMode-NR-ExtensionIE XNAP-PROTOCOL-IES ::= {

...

}

MDTMode-EUTRA ::= CHOICE {

immediateMDT ImmediateMDT-EUTRA,

loggedMDT LoggedMDT-EUTRA,

...,

mDTMode-EUTRA-Extension MDTMode-EUTRA-Extension

}

MDTMode-EUTRA-Extension ::= ProtocolIE-Single-Container {{ MDTMode-EUTRA-ExtensionIE }}

MDTMode-EUTRA-ExtensionIE XNAP-PROTOCOL-IES ::= {

...

}

MeasurementsToActivate ::= BIT STRING (SIZE (8))

MeasurementThresholdA2 ::= CHOICE {

threshold-RSRP Threshold-RSRP,

threshold-RSRQ Threshold-RSRQ,

threshold-SINR Threshold-SINR,

choice-extension ProtocolIE-Single-Container { { MeasurementThresholdA2-ExtIEs} }

}

MeasurementThresholdA2-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

Measurement-ID ::= INTEGER (1..4095,...)

MobilityInformation ::= BIT STRING (SIZE(32))

MobilityParametersModificationRange ::= SEQUENCE {

handoverTriggerChangeLowerLimit INTEGER (-20..20),

handoverTriggerChangeUpperLimit INTEGER (-20..20),

...

}

MobilityParametersInformation ::= SEQUENCE {

handoverTriggerChange INTEGER (-20..20),

...

}

MobilityRestrictionList ::= SEQUENCE {

serving-PLMN PLMN-Identity,

equivalent-PLMNs SEQUENCE (SIZE(1..maxnoofEPLMNs)) OF PLMN-Identity OPTIONAL,

rat-Restrictions RAT-RestrictionsList OPTIONAL,

forbiddenAreaInformation ForbiddenAreaList OPTIONAL,

serviceAreaInformation ServiceAreaList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {MobilityRestrictionList-ExtIEs} } OPTIONAL,

...

}

MobilityRestrictionList-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

{ ID id-LastE-UTRANPLMNIdentity CRITICALITY ignore EXTENSION PLMN-Identity PRESENCE optional }|

{ ID id-CNTypeRestrictionsForServing CRITICALITY ignore EXTENSION CNTypeRestrictionsForServing PRESENCE optional }|

{ ID id-CNTypeRestrictionsForEquivalent CRITICALITY ignore EXTENSION CNTypeRestrictionsForEquivalent PRESENCE optional }|

{ ID id-NPNMobilityInformation CRITICALITY reject EXTENSION NPNMobilityInformation PRESENCE optional },

...

}

CNTypeRestrictionsForEquivalent ::= SEQUENCE (SIZE(1..maxnoofEPLMNs)) OF CNTypeRestrictionsForEquivalentItem

CNTypeRestrictionsForEquivalentItem ::= SEQUENCE {

plmn-Identity PLMN-Identity,

cn-Type ENUMERATED {epc-forbidden, fiveGC-forbidden, ...},

iE-Extensions ProtocolExtensionContainer { {CNTypeRestrictionsForEquivalentItem-ExtIEs} } OPTIONAL,

...

}

CNTypeRestrictionsForEquivalentItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

CNTypeRestrictionsForServing ::= ENUMERATED {

epc-forbidden,

...

}

RAT-RestrictionsList ::= SEQUENCE (SIZE(1..maxnoofPLMNs)) OF RAT-RestrictionsItem

RAT-RestrictionsItem ::= SEQUENCE {

plmn-Identity PLMN-Identity,

rat-RestrictionInformation RAT-RestrictionInformation,

iE-Extensions ProtocolExtensionContainer { {RAT-RestrictionsItem-ExtIEs} } OPTIONAL,

...

}

RAT-RestrictionsItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

{ ID id-ExtendedRATRestrictionInformation CRITICALITY ignore EXTENSION ExtendedRATRestrictionInformation PRESENCE optional},

...

}

RAT-RestrictionInformation ::= BIT STRING {e-UTRA (0),nR (1)} (SIZE(8, ...))

ForbiddenAreaList ::= SEQUENCE (SIZE(1..maxnoofPLMNs)) OF ForbiddenAreaItem

ForbiddenAreaItem ::= SEQUENCE {

plmn-Identity PLMN-Identity,

forbidden-TACs SEQUENCE (SIZE(1..maxnoofForbiddenTACs)) OF TAC,

iE-Extensions ProtocolExtensionContainer { {ForbiddenAreaItem-ExtIEs} } OPTIONAL,

...

}

ForbiddenAreaItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

ServiceAreaList ::= SEQUENCE (SIZE(1..maxnoofPLMNs)) OF ServiceAreaItem

ServiceAreaItem ::= SEQUENCE {

plmn-Identity PLMN-Identity,

allowed-TACs-ServiceArea SEQUENCE (SIZE(1..maxnoofAllowedAreas)) OF TAC OPTIONAL,

not-allowed-TACs-ServiceArea SEQUENCE (SIZE(1..maxnoofAllowedAreas)) OF TAC OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ServiceAreaItem-ExtIEs} } OPTIONAL,

...

}

ServiceAreaItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

MR-DC-ResourceCoordinationInfo ::= SEQUENCE {

ng-RAN-Node-ResourceCoordinationInfo NG-RAN-Node-ResourceCoordinationInfo,

iE-Extension ProtocolExtensionContainer { {MR-DC-ResourceCoordinationInfo-ExtIEs}} OPTIONAL,

...

}

MR-DC-ResourceCoordinationInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NG-RAN-Node-ResourceCoordinationInfo ::= CHOICE {

eutra-resource-coordination-info E-UTRA-ResourceCoordinationInfo,

nr-resource-coordination-info NR-ResourceCoordinationInfo

}

E-UTRA-ResourceCoordinationInfo ::= SEQUENCE {

e-utra-cell E-UTRA-CGI,

ul-coordination-info BIT STRING (SIZE (6..4400)),

dl-coordination-info BIT STRING (SIZE (6..4400)) OPTIONAL,

nr-cell NR-CGI OPTIONAL,

e-utra-coordination-assistance-info E-UTRA-CoordinationAssistanceInfo OPTIONAL,

iE-Extension ProtocolExtensionContainer { {E-UTRA-ResourceCoordinationInfo-ExtIEs} } OPTIONAL,

...

}

E-UTRA-ResourceCoordinationInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

E-UTRA-CoordinationAssistanceInfo ::= ENUMERATED {coordination-not-required, ...}

NR-ResourceCoordinationInfo ::= SEQUENCE {

nr-cell NR-CGI,

ul-coordination-info BIT STRING (SIZE (6..4400)),

dl-coordination-info BIT STRING (SIZE (6..4400)) OPTIONAL,

e-utra-cell E-UTRA-CGI OPTIONAL,

nr-coordination-assistance-info NR-CoordinationAssistanceInfo OPTIONAL,

iE-Extension ProtocolExtensionContainer { {NR-ResourceCoordinationInfo-ExtIEs} } OPTIONAL,

...

}

NR-ResourceCoordinationInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NR-CoordinationAssistanceInfo ::= ENUMERATED {coordination-not-required, ...}

MessageOversizeNotification ::= SEQUENCE {

maximumCellListSize MaximumCellListSize,

iE-Extension ProtocolExtensionContainer { {MessageOversizeNotification-ExtIEs}} OPTIONAL,

...

}

MessageOversizeNotification-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

MaximumCellListSize ::= INTEGER(1..16384, ...)

MultiplexingInfo ::= SEQUENCE{

iAB-MT-Cell-List IAB-MT-Cell-List,

iE-Extensions ProtocolExtensionContainer { {MultiplexingInfo-ExtIEs} } OPTIONAL,

...

}

MultiplexingInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- N

NACellResourceConfigurationList ::= SEQUENCE (SIZE(1..maxnoofHSNASlots)) OF NACellResourceConfiguration-Item

NACellResourceConfiguration-Item ::= SEQUENCE {

nAdownlink ENUMERATED {true, false, ...} OPTIONAL,

nAuplink ENUMERATED {true, false, ...} OPTIONAL,

nAflexible ENUMERATED {true, false, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { NACellResourceConfiguration-Item-ExtIEs} } OPTIONAL,

...

}

NACellResourceConfiguration-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NBIoT-UL-DL-AlignmentOffset ::= ENUMERATED {

khz-7dot5,

khz0,

khz7dot5,

...

}

NE-DC-TDM-Pattern ::= SEQUENCE {

subframeAssignment ENUMERATED {sa0,sa1,sa2,sa3,sa4,sa5,sa6},

harqOffset INTEGER (0..9),

iE-Extension ProtocolExtensionContainer { {NE-DC-TDM-Pattern-ExtIEs}} OPTIONAL,

...

}

NE-DC-TDM-Pattern-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NeighbourInformation-E-UTRA ::= SEQUENCE (SIZE(1..maxnoofNeighbours)) OF NeighbourInformation-E-UTRA-Item

NeighbourInformation-E-UTRA-Item ::= SEQUENCE {

e-utra-PCI E-UTRAPCI,

e-utra-cgi E-UTRA-CGI,

earfcn E-UTRAARFCN,

tac TAC,

ranac RANAC OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {NeighbourInformation-E-UTRA-Item-ExtIEs} } OPTIONAL,

...

}

NeighbourInformation-E-UTRA-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

NeighbourInformation-NR ::= SEQUENCE (SIZE(1..maxnoofNeighbours)) OF NeighbourInformation-NR-Item

NeighbourInformation-NR-Item ::= SEQUENCE {

nr-PCI NRPCI,

nr-cgi NR-CGI,

tac TAC,

ranac RANAC OPTIONAL,

nr-mode-info NeighbourInformation-NR-ModeInfo,

connectivitySupport Connectivity-Support,

measurementTimingConfiguration OCTET STRING,

iE-Extensions ProtocolExtensionContainer { {NeighbourInformation-NR-Item-ExtIEs} } OPTIONAL,

...

}

NeighbourInformation-NR-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::={

...

}

NeighbourInformation-NR-ModeInfo ::= CHOICE {

fdd-info NeighbourInformation-NR-ModeFDDInfo,

tdd-info NeighbourInformation-NR-ModeTDDInfo,

choice-extension ProtocolIE-Single-Container { {NeighbourInformation-NR-ModeInfo-ExtIEs} }

}

NeighbourInformation-NR-ModeInfo-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NeighbourInformation-NR-ModeFDDInfo ::= SEQUENCE {

ul-NR-FreqInfo NRFrequencyInfo,

dl-NR-FequInfo NRFrequencyInfo,

ie-Extensions ProtocolExtensionContainer { {NeighbourInformation-NR-ModeFDDInfo-ExtIEs} } OPTIONAL,

...

}

NeighbourInformation-NR-ModeFDDInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NeighbourInformation-NR-ModeTDDInfo ::= SEQUENCE {

nr-FreqInfo NRFrequencyInfo,

ie-Extensions ProtocolExtensionContainer { {NeighbourInformation-NR-ModeTDDInfo-ExtIEs} } OPTIONAL,

...

}

NeighbourInformation-NR-ModeTDDInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NID ::= BIT STRING (SIZE(44))

NRCarrierList ::= SEQUENCE (SIZE(1..maxnoofNRSCSs)) OF NRCarrierItem

NRCarrierItem ::= SEQUENCE {

carrierSCS NRSCS,

offsetToCarrier INTEGER (0..2199, ...),

carrierBandwidth INTEGER (0..maxnoofPhysicalResourceBlocks, ...),

iE-Extension ProtocolExtensionContainer { {NRCarrierItem-ExtIEs} } OPTIONAL,

...

}

NRCarrierItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NRCellPRACHConfig ::= OCTET STRING

NG-RAN-Cell-Identity ::= CHOICE {

nr NR-Cell-Identity,

e-utra E-UTRA-Cell-Identity,

choice-extension ProtocolIE-Single-Container { {NG-RAN-Cell-Identity-ExtIEs} }

}

NG-RAN-Cell-Identity-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NG-RAN-CellPCI ::= CHOICE {

nr NRPCI,

e-utra E-UTRAPCI,

choice-extension ProtocolIE-Single-Container { {NG-RAN-CellPCI-ExtIEs} }

}

NG-RAN-CellPCI-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NG-RANnodeUEXnAPID ::= INTEGER (0.. 4294967295)

NumberofActiveUEs::= INTEGER(0..16777215, ...)

NoofRRCConnections ::= INTEGER (1..65536,...)

NonDynamic5QIDescriptor ::= SEQUENCE {

fiveQI FiveQI,

priorityLevelQoS PriorityLevelQoS OPTIONAL,

averagingWindow AveragingWindow OPTIONAL,

maximumDataBurstVolume MaximumDataBurstVolume OPTIONAL,

iE-Extension ProtocolExtensionContainer { {NonDynamic5QIDescriptor-ExtIEs } } OPTIONAL,

...

}

NonDynamic5QIDescriptor-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-CNPacketDelayBudgetDownlink CRITICALITY ignore EXTENSION ExtendedPacketDelayBudget PRESENCE optional}|

{ ID id-CNPacketDelayBudgetUplink CRITICALITY ignore EXTENSION ExtendedPacketDelayBudget PRESENCE optional},

...

}

NRARFCN ::= INTEGER (0.. maxNRARFCN)

NG-eNB-RadioResourceStatus ::= SEQUENCE {

dL-GBR-PRB-usage DL-GBR-PRB-usage,

uL-GBR-PRB-usage UL-GBR-PRB-usage,

dL-non-GBR-PRB-usage DL-non-GBR-PRB-usage,

uL-non-GBR-PRB-usage UL-non-GBR-PRB-usage,

dL-Total-PRB-usage DL-Total-PRB-usage,

uL-Total-PRB-usage UL-Total-PRB-usage,

iE-Extensions ProtocolExtensionContainer { { NG-eNB-RadioResourceStatus-ExtIEs} } OPTIONAL,

...

}

NG-eNB-RadioResourceStatus-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-DL-scheduling-PDCCH-CCE-usage CRITICALITY ignore EXTENSION DL-scheduling-PDCCH-CCE-usage PRESENCE optional}|

{ ID id-UL-scheduling-PDCCH-CCE-usage CRITICALITY ignore EXTENSION UL-scheduling-PDCCH-CCE-usage PRESENCE optional},

...

}

DL-scheduling-PDCCH-CCE-usage ::= INTEGER (0.. 100)

UL-scheduling-PDCCH-CCE-usage ::= INTEGER (0.. 100)

TNLCapacityIndicator ::= SEQUENCE {

dLTNLOfferedCapacity OfferedCapacity,

dLTNLAvailableCapacity AvailableCapacity,

uLTNLOfferedCapacity OfferedCapacity,

uLTNLAvailableCapacity AvailableCapacity,

iE-Extensions ProtocolExtensionContainer { { TNLCapacityIndicator-ExtIEs} } OPTIONAL,

...

}

TNLCapacityIndicator-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

Non-F1-TerminatingTopologyBHInformation ::= SEQUENCE {

nonF1TerminatingBHInformation-List NonF1TerminatingBHInformation-List,

bAPControlPDURLCCH-List BAPControlPDURLCCH-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {Non-F1-TerminatingTopologyBHInformation-ExtIEs} } OPTIONAL,

...

}

Non-F1-TerminatingTopologyBHInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NonF1TerminatingBHInformation-List ::= SEQUENCE (SIZE(1..maxnoofBHInfo)) OF NonF1TerminatingBHInformation-Item

NonF1TerminatingBHInformation-Item ::= SEQUENCE {

bHInfoIndex BHInfoIndex,

dlNon-F1TermBHInfo DLNonF1Term-BHInfo OPTIONAL,

ulNon-F1TermBHInfo ULNonF1Term-BHInfo OPTIONAL,

iE-Extension ProtocolExtensionContainer { { NonF1TerminatingBHInformation-Item-ExtIEs} } OPTIONAL,

...

}

NonF1TerminatingBHInformation-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NonUPTraffic ::= CHOICE {

nonUPTrafficType NonUPTrafficType,

controlPlaneTrafficType ControlPlaneTrafficType,

choice-extension ProtocolIE-Single-Container { { NonUPTraffic-ExtIEs} }

}

NonUPTraffic-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NonUPTrafficType ::= ENUMERATED {ueassociatedf1ap, nonueassociatedf1ap, nonf1, ...}

NoPDUSessionIndication ::= ENUMERATED {true, ...}

NPN-Broadcast-Information ::= CHOICE {

snpn-Information NPN-Broadcast-Information-SNPN,

pni-npn-Information NPN-Broadcast-Information-PNI-NPN,

choice-extension ProtocolIE-Single-Container { {NPN-Broadcast-Information-ExtIEs} }

}

NPN-Broadcast-Information-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NPN-Broadcast-Information-SNPN ::= SEQUENCE {

broadcastSNPNID-List BroadcastSNPNID-List,

iE-Extension ProtocolExtensionContainer { {NPN-Broadcast-Information-SNPN-ExtIEs} } OPTIONAL,

...

}

NPN-Broadcast-Information-SNPN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NPN-Broadcast-Information-PNI-NPN ::= SEQUENCE {

broadcastPNI-NPN-ID-Information BroadcastPNI-NPN-ID-Information,

iE-Extension ProtocolExtensionContainer { {NPN-Broadcast-Information-PNI-NPN-ExtIEs} } OPTIONAL,

...

}

NPN-Broadcast-Information-PNI-NPN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NPNMobilityInformation::= CHOICE {

snpn-mobility-information NPNMobilityInformation-SNPN,

pni-npn-mobility-information NPNMobilityInformation-PNI-NPN,

choice-extension ProtocolIE-Single-Container { {NPNMobilityInformation-ExtIEs} }

}

NPNMobilityInformation-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NPNMobilityInformation-SNPN ::= SEQUENCE {

serving-NID NID,

iE-Extension ProtocolExtensionContainer { {NPNMobilityInformation-SNPN-ExtIEs} } OPTIONAL,

...

}

NPNMobilityInformation-SNPN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NPNMobilityInformation-PNI-NPN ::= SEQUENCE {

allowedPNI-NPN-ID-List AllowedPNI-NPN-ID-List,

iE-Extension ProtocolExtensionContainer { {NPNMobilityInformation-PNI-NPN-ExtIEs} } OPTIONAL,

...

}

NPNMobilityInformation-PNI-NPN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NPNPagingAssistanceInformation ::= CHOICE {

pni-npn-Information NPNPagingAssistanceInformation-PNI-NPN,

choice-extension ProtocolIE-Single-Container { {NPNPagingAssistanceInformation-ExtIEs} }

}

NPNPagingAssistanceInformation-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NPNPagingAssistanceInformation-PNI-NPN ::= SEQUENCE {

allowedPNI-NPN-ID-List AllowedPNI-NPN-ID-List,

iE-Extension ProtocolExtensionContainer { {NPNPagingAssistanceInformation-PNI-NPN-ExtIEs} } OPTIONAL,

...

}

NPNPagingAssistanceInformation-PNI-NPN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NPN-Support ::= CHOICE {

sNPN NPN-Support-SNPN,

choice-Extensions ProtocolIE-Single-Container { {NPN-Support-ExtIEs} }

}

NPN-Support-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NPN-Support-SNPN ::= SEQUENCE {

nid NID,

ie-Extension ProtocolExtensionContainer { {NPN-Support-SNPN-ExtIEs} } OPTIONAL,

...

}

NPN-Support-SNPN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NPRACHConfiguration::= SEQUENCE {

fdd-or-tdd CHOICE {

fdd NPRACHConfiguration-FDD,

tdd NPRACHConfiguration-TDD,

choice-extension ProtocolIE-Single-Container { { FDD-or-TDD-in-NPRACHConfiguration-Choice-ExtIEs} }

},

iE-Extensions ProtocolExtensionContainer { { NPRACHConfiguration-ExtIEs} } OPTIONAL,

...

}

NPRACHConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

FDD-or-TDD-in-NPRACHConfiguration-Choice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NPRACHConfiguration-FDD::= SEQUENCE {

nprach-CP-length NPRACH-CP-Length,

anchorCarrier-NPRACHConfig OCTET STRING,

anchorCarrier-EDT-NPRACHConfig OCTET STRING OPTIONAL,

anchorCarrier-Format2-NPRACHConfig OCTET STRING OPTIONAL,

anchorCarrier-Format2-EDT-NPRACHConfig OCTET STRING OPTIONAL,

non-anchorCarrier-NPRACHConfig OCTET STRING OPTIONAL,

non-anchorCarrier-Format2-NPRACHConfig OCTET STRING OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { NPRACHConfiguration-FDD-ExtIEs} } OPTIONAL,

...

}

NPRACHConfiguration-FDD-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NPRACHConfiguration-TDD::= SEQUENCE {

nprach-preambleFormat NPRACH-preambleFormat,

anchorCarrier-NPRACHConfigTDD OCTET STRING,

non-anchorCarrierFequencyConfiglist Non-AnchorCarrierFrequencylist OPTIONAL,

non-anchorCarrier-NPRACHConfigTDD OCTET STRING OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { NPRACHConfiguration-TDD-ExtIEs} } OPTIONAL,

...

}

NPRACHConfiguration-TDD-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NPRACH-CP-Length::= ENUMERATED {

us66dot7,

us266dot7,

...

}

NPRACH-preambleFormat::= ENUMERATED {fmt0,fmt1,fmt2,fmt0a,fmt1a,...}

Non-AnchorCarrierFrequencylist ::= SEQUENCE (SIZE(1..maxnoofNonAnchorCarrierFreqConfig)) OF

SEQUENCE {

non-anchorCarrierFrquency OCTET STRING,

iE-Extensions ProtocolExtensionContainer { { Non-AnchorCarrierFrequencylist-ExtIEs} } OPTIONAL,

...

}

Non-AnchorCarrierFrequencylist-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NR-Cell-Identity ::= BIT STRING (SIZE (36))

NG-RAN-Cell-Identity-ListinRANPagingArea ::= SEQUENCE (SIZE (1..maxnoofCellsinRNA)) OF NG-RAN-Cell-Identity

NR-CGI ::= SEQUENCE {

plmn-id PLMN-Identity,

nr-CI NR-Cell-Identity,

iE-Extension ProtocolExtensionContainer { {NR-CGI-ExtIEs} } OPTIONAL,

...

}

NR-CGI-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NRCyclicPrefix ::= ENUMERATED {normal, extended, ...}

NRDL-ULTransmissionPeriodicity ::= ENUMERATED {ms0p5, ms0p625, ms1, ms1p25, ms2, ms2p5, ms3, ms4, ms5, ms10, ms20, ms40, ms60, ms80, ms100, ms120, ms140, ms160, ...}

NRFrequencyBand ::= INTEGER (1..1024, ...)

NRFrequencyBand-List ::= SEQUENCE (SIZE(1..maxnoofNRCellBands)) OF NRFrequencyBandItem

NRFrequencyBandItem ::= SEQUENCE {

nr-frequency-band NRFrequencyBand,

supported-SUL-Band-List SupportedSULBandList OPTIONAL,

iE-Extension ProtocolExtensionContainer { {NRFrequencyBandItem-ExtIEs} } OPTIONAL,

...

}

NRFrequencyBandItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NRFrequencyInfo ::= SEQUENCE {

nrARFCN NRARFCN,

sul-information SUL-Information OPTIONAL,

frequencyBand-List NRFrequencyBand-List,

iE-Extension ProtocolExtensionContainer { {NRFrequencyInfo-ExtIEs} } OPTIONAL,

...

}

NRFrequencyInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-FrequencyShift7p5khz CRITICALITY ignore EXTENSION FrequencyShift7p5khz PRESENCE optional },...

}

NRMobilityHistoryReport ::= OCTET STRING

NRModeInfo ::= CHOICE {

fdd NRModeInfoFDD,

tdd NRModeInfoTDD,

choice-extension ProtocolIE-Single-Container { {NRModeInfo-ExtIEs} }

}

NRModeInfo-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

NRModeInfoFDD ::= SEQUENCE {

ulNRFrequencyInfo NRFrequencyInfo,

dlNRFrequencyInfo NRFrequencyInfo,

ulNRTransmissonBandwidth NRTransmissionBandwidth,

dlNRTransmissonBandwidth NRTransmissionBandwidth,

iE-Extension ProtocolExtensionContainer { {NRModeInfoFDD-ExtIEs} } OPTIONAL,

...

}

NRModeInfoFDD-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-ULCarrierList CRITICALITY ignore EXTENSION NRCarrierList PRESENCE optional }|

{ ID id-DLCarrierList CRITICALITY ignore EXTENSION NRCarrierList PRESENCE optional }|

{ ID id-UL-GNB-DU-Cell-Resource-Configuration CRITICALITY ignore EXTENSION GNB-DU-Cell-Resource-Configuration PRESENCE optional }|

{ ID id-DL-GNB-DU-Cell-Resource-Configuration CRITICALITY ignore EXTENSION GNB-DU-Cell-Resource-Configuration PRESENCE optional },

...

}

NRModeInfoTDD ::= SEQUENCE {

nrFrequencyInfo NRFrequencyInfo,

nrTransmissonBandwidth NRTransmissionBandwidth,

iE-Extension ProtocolExtensionContainer { {NRModeInfoTDD-ExtIEs} } OPTIONAL,

...

}

NRModeInfoTDD-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ID id-IntendedTDD-DL-ULConfiguration-NR CRITICALITY ignore EXTENSION IntendedTDD-DL-ULConfiguration-NR PRESENCE optional }|

{ID id-TDDULDLConfigurationCommonNR CRITICALITY ignore EXTENSION TDDULDLConfigurationCommonNR PRESENCE optional }|

{ ID id-CarrierList CRITICALITY ignore EXTENSION NRCarrierList PRESENCE optional }|

{ID id-tdd-GNB-DU-Cell-Resource-Configuration CRITICALITY ignore EXTENSION GNB-DU-Cell-Resource-Configuration PRESENCE optional },

...

}

NRNRB ::= ENUMERATED { nrb11, nrb18, nrb24, nrb25, nrb31, nrb32, nrb38, nrb51, nrb52, nrb65, nrb66, nrb78, nrb79, nrb93, nrb106, nrb107, nrb121, nrb132, nrb133, nrb135, nrb160, nrb162, nrb189, nrb216, nrb217, nrb245, nrb264, nrb270, nrb273, ...}

NRPCI ::= INTEGER (0..1007, ...)

NRSCS ::= ENUMERATED { scs15, scs30, scs60, scs120, ...}

NRTransmissionBandwidth ::= SEQUENCE {

nRSCS NRSCS,

nRNRB NRNRB,

iE-Extensions ProtocolExtensionContainer { {NRTransmissionBandwidth-ExtIEs} } OPTIONAL,

...

}

NRTransmissionBandwidth-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NumberOfAntennaPorts-E-UTRA ::= ENUMERATED {an1, an2, an4, ...}

NG-RANTraceID ::=OCTET STRING (SIZE (8))

NonGBRResources-Offered ::= ENUMERATED {true, ...}

NRV2XServicesAuthorized ::= SEQUENCE {

vehicleUE VehicleUE OPTIONAL,

pedestrianUE PedestrianUE OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {NRV2XServicesAuthorized-ExtIEs} } OPTIONAL,

...

}

NRV2XServicesAuthorized-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NRUESidelinkAggregateMaximumBitRate ::= SEQUENCE {

uESidelinkAggregateMaximumBitRate BitRate,

iE-Extensions ProtocolExtensionContainer { {NRUESidelinkAggregateMaximumBitRate-ExtIEs} } OPTIONAL,

...

}

NRUESidelinkAggregateMaximumBitRate-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- O

OfferedCapacity ::= INTEGER (1.. 16777216,...)

OffsetOfNbiotChannelNumberToEARFCN ::= ENUMERATED {

minusTen,

minusNine,

minusEightDotFive,

minusEight,

minusSeven,

minusSix,

minusFive,

minusFourDotFive,

minusFour,

minusThree,

minusTwo,

minusOne,

minusZeroDotFive,

zero,

one,

two,

three,

threeDotFive,

four,

five,

six,

seven,

sevenDotFive,

eight,

nine,

...

}

-- P

PacketDelayBudget ::= INTEGER (0..1023, ...)

PacketErrorRate ::= SEQUENCE {

pER-Scalar PER-Scalar,

pER-Exponent PER-Exponent,

iE-Extensions ProtocolExtensionContainer { {PacketErrorRate-ExtIEs} } OPTIONAL,

...

}

PacketErrorRate-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PedestrianUE ::= ENUMERATED {

authorized,

not-authorized,

...

}

PER-Scalar ::= INTEGER (0..9, ...)

PER-Exponent ::= INTEGER (0..9, ...)

PacketLossRate ::= INTEGER (0..1000, ...)

PagingDRX ::= ENUMERATED {

v32,

v64,

v128,

v256,

... ,

v512,

v1024

}

PagingeDRXInformation ::= SEQUENCE {

paging-eDRX-Cycle Paging-eDRX-Cycle,

paging-Time-Window Paging-Time-Window OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PagingeDRXInformation-ExtIEs} } OPTIONAL,

...

}

PagingeDRXInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

Paging-eDRX-Cycle ::= ENUMERATED {

hfhalf, hf1, hf2, hf4, hf6,

hf8, hf10, hf12, hf14, hf16,

hf32, hf64, hf128, hf256,

...

}

Paging-Time-Window ::= ENUMERATED {

s1, s2, s3, s4, s5,

s6, s7, s8, s9, s10,

s11, s12, s13, s14, s15, s16,

...

}

PagingPriority ::= ENUMERATED {

priolevel1,

priolevel2,

priolevel3,

priolevel4,

priolevel5,

priolevel6,

priolevel7,

priolevel8,

...

}

PartialListIndicator ::= ENUMERATED {partial, ...}

PC5QoSParameters ::= SEQUENCE {

pc5QoSFlowList PC5QoSFlowList,

pc5LinkAggregateBitRates BitRate OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PC5QoSParameters-ExtIEs} } OPTIONAL,

...

}

PC5QoSParameters-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PC5QoSFlowList ::= SEQUENCE (SIZE(1..maxnoofPC5QoSFlows)) OF PC5QoSFlowItem

PC5QoSFlowItem::= SEQUENCE {

pQI FiveQI,

pc5FlowBitRates PC5FlowBitRates OPTIONAL,

range Range OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PC5QoSFlowItem-ExtIEs} } OPTIONAL,

...

}

PC5QoSFlowItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PC5FlowBitRates ::= SEQUENCE {

guaranteedFlowBitRate BitRate,

maximumFlowBitRate BitRate,

iE-Extensions ProtocolExtensionContainer { { PC5FlowBitRates-ExtIEs} } OPTIONAL,

...

}

PC5FlowBitRates-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDCPChangeIndication ::= CHOICE {

from-S-NG-RAN-node ENUMERATED {s-ng-ran-node-key-update-required, pdcp-data-recovery-required, ...},

from-M-NG-RAN-node ENUMERATED {pdcp-data-recovery-required, ...},

choice-extension ProtocolIE-Single-Container { {PDCPChangeIndication-ExtIEs} }

}

PDCPChangeIndication-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

PDCPDuplicationConfiguration ::= ENUMERATED {

configured,

de-configured,

...

}

PDCPSNLength ::= SEQUENCE {

ulPDCPSNLength ENUMERATED {v12bits, v18bits, ...},

dlPDCPSNLength ENUMERATED {v12bits, v18bits, ...},

iE-Extension ProtocolExtensionContainer { {PDCPSNLength-ExtIEs} } OPTIONAL,

...

}

PDCPSNLength-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionAggregateMaximumBitRate ::= SEQUENCE {

downlink-session-AMBR BitRate,

uplink-session-AMBR BitRate,

iE-Extensions ProtocolExtensionContainer { {PDUSessionAggregateMaximumBitRate-ExtIEs} } OPTIONAL,

...

}

PDUSessionAggregateMaximumBitRate-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSession-List ::= SEQUENCE (SIZE (1.. maxnoofPDUSessions)) OF PDUSession-ID

PDUSession-List-withCause ::= SEQUENCE (SIZE (1.. maxnoofPDUSessions)) OF PDUSession-List-withCause-Item

PDUSession-List-withCause-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

cause Cause OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSession-List-withCause-Item-ExtIEs} } OPTIONAL,

...

}

PDUSession-List-withCause-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSession-List-withDataForwardingFromTarget ::= SEQUENCE (SIZE (1.. maxnoofPDUSessions)) OF

PDUSession-List-withDataForwardingFromTarget-Item

PDUSession-List-withDataForwardingFromTarget-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

dataforwardinginfoTarget DataForwardingInfoFromTargetNGRANnode,

iE-Extension ProtocolExtensionContainer { {PDUSession-List-withDataForwardingFromTarget-Item-ExtIEs} } OPTIONAL,

...

}

PDUSession-List-withDataForwardingFromTarget-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-DRB-IDs-takenintouse CRITICALITY reject EXTENSION DRB-List PRESENCE optional},

...

}

PDUSession-List-withDataForwardingRequest ::= SEQUENCE (SIZE (1.. maxnoofPDUSessions)) OF

PDUSession-List-withDataForwardingRequest-Item

PDUSession-List-withDataForwardingRequest-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

dataforwardingInfofromSource DataforwardingandOffloadingInfofromSource OPTIONAL,

dRBtoBeReleasedList DRBToQoSFlowMapping-List OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSession-List-withDataForwardingRequest-Item-ExtIEs} } OPTIONAL,

...

}

PDUSession-List-withDataForwardingRequest-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ID id-Cause CRITICALITY ignore EXTENSION Cause PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session related message level IEs BEGIN

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resources Admitted List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourcesAdmitted-List ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourcesAdmitted-Item

PDUSessionResourcesAdmitted-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

pduSessionResourceAdmittedInfo PDUSessionResourceAdmittedInfo,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourcesAdmitted-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourcesAdmitted-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionResourceAdmittedInfo ::= SEQUENCE {

dL-NG-U-TNL-Information-Unchanged ENUMERATED {true, ...} OPTIONAL,

qosFlowsAdmitted-List QoSFlowsAdmitted-List,

qosFlowsNotAdmitted-List QoSFlows-List-withCause OPTIONAL,

dataForwardingInfoFromTarget DataForwardingInfoFromTargetNGRANnode OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceAdmittedInfo-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceAdmittedInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-SecondarydataForwardingInfoFromTarget-List CRITICALITY ignore EXTENSION SecondarydataForwardingInfoFromTarget-List PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resources Not Admitted List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourcesNotAdmitted-List ::= SEQUENCE (SIZE (1..maxnoofPDUSessions)) OF PDUSessionResourcesNotAdmitted-Item

PDUSessionResourcesNotAdmitted-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

cause Cause OPTIONAL,

iE-Extension ProtocolExtensionContainer { {PDUSessionResourcesNotAdmitted-Item-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourcesNotAdmitted-Item-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resources To Be Setup List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourcesToBeSetup-List ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourcesToBeSetup-Item

PDUSessionResourcesToBeSetup-Item ::= SEQUENCE {

pduSessionId PDUSession-ID,

s-NSSAI S-NSSAI,

pduSessionAMBR PDUSessionAggregateMaximumBitRate OPTIONAL,

uL-NG-U-TNLatUPF UPTransportLayerInformation,

source-DL-NG-U-TNL-Information UPTransportLayerInformation OPTIONAL,

securityIndication SecurityIndication OPTIONAL,

pduSessionType PDUSessionType,

pduSessionNetworkInstance PDUSessionNetworkInstance OPTIONAL,

qosFlowsToBeSetup-List QoSFlowsToBeSetup-List,

dataforwardinginfofromSource DataforwardingandOffloadingInfofromSource OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourcesToBeSetup-Item-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourcesToBeSetup-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-UL-NG-U-TNLatUPF-List CRITICALITY ignore EXTENSION Additional-UL-NG-U-TNLatUPF-List PRESENCE optional}|

{ ID id-PDUSessionCommonNetworkInstance CRITICALITY ignore EXTENSION PDUSessionCommonNetworkInstance PRESENCE optional}|

{ ID id-Redundant-UL-NG-U-TNLatUPF CRITICALITY ignore EXTENSION UPTransportLayerInformation PRESENCE optional}|

{ ID id-Additional-Redundant-UL-NG-U-TNLatUPF-List CRITICALITY ignore EXTENSION Additional-UL-NG-U-TNLatUPF-List PRESENCE optional}|

{ ID id-RedundantCommonNetworkInstance CRITICALITY ignore EXTENSION PDUSessionCommonNetworkInstance PRESENCE optional}|

{ ID id-RedundantPDUSessionInformation CRITICALITY ignore EXTENSION RedundantPDUSessionInformation PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Setup Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceSetupInfo-SNterminated ::= SEQUENCE {

uL-NG-U-TNLatUPF UPTransportLayerInformation,

pduSessionType PDUSessionType,

pduSessionNetworkInstance PDUSessionNetworkInstance OPTIONAL,

qosFlowsToBeSetup-List QoSFlowsToBeSetup-List-Setup-SNterminated,

dataforwardinginfofromSource DataforwardingandOffloadingInfofromSource OPTIONAL,

securityIndication SecurityIndication OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceSetupInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceSetupInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-SecurityResult CRITICALITY reject EXTENSION SecurityResult PRESENCE optional}|

{ ID id-PDUSessionCommonNetworkInstance CRITICALITY ignore EXTENSION PDUSessionCommonNetworkInstance PRESENCE optional}|

{ID id-DefaultDRB-Allowed CRITICALITY ignore EXTENSION DefaultDRB-Allowed PRESENCE optional}|

{ ID id-SplitSessionIndicator CRITICALITY reject EXTENSION SplitSessionIndicator PRESENCE optional}|

{ID id-NonGBRResources-Offered CRITICALITY ignore EXTENSION NonGBRResources-Offered PRESENCE optional}|

{ ID id-Redundant-UL-NG-U-TNLatUPF CRITICALITY ignore EXTENSION UPTransportLayerInformation PRESENCE optional}|

{ ID id-RedundantCommonNetworkInstance CRITICALITY ignore EXTENSION PDUSessionCommonNetworkInstance PRESENCE optional}|

{ ID id-RedundantPDUSessionInformation CRITICALITY ignore EXTENSION RedundantPDUSessionInformation PRESENCE optional},

...

}

QoSFlowsToBeSetup-List-Setup-SNterminated ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF QoSFlowsToBeSetup-List-Setup-SNterminated-Item

QoSFlowsToBeSetup-List-Setup-SNterminated-Item ::= SEQUENCE {

qfi QoSFlowIdentifier,

qosFlowLevelQoSParameters QoSFlowLevelQoSParameters,

offeredGBRQoSFlowInfo GBRQoSFlowInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsToBeSetup-List-Setup-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsToBeSetup-List-Setup-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-TSCTrafficCharacteristics CRITICALITY ignore EXTENSION TSCTrafficCharacteristics PRESENCE optional}|

{ ID id-RedundantQoSFlowIndicator CRITICALITY ignore EXTENSION RedundantQoSFlowIndicator PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Setup Response Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceSetupResponseInfo-SNterminated ::= SEQUENCE {

dL-NG-U-TNLatNG-RAN UPTransportLayerInformation,

dRBsToBeSetup DRBsToBeSetupList-SetupResponse-SNterminated OPTIONAL,

dataforwardinginfoTarget DataForwardingInfoFromTargetNGRANnode OPTIONAL,

qosFlowsNotAdmittedList QoSFlows-List-withCause OPTIONAL,

securityResult SecurityResult OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceSetupResponseInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceSetupResponseInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-DRB-IDs-takenintouse CRITICALITY reject EXTENSION DRB-List PRESENCE optional}|

{ ID id-Redundant-DL-NG-U-TNLatNG-RAN CRITICALITY ignore EXTENSION UPTransportLayerInformation PRESENCE optional}|

{ ID id-UsedRSNInformation CRITICALITY ignore EXTENSION RedundantPDUSessionInformation PRESENCE optional},

...

}

DRBsToBeSetupList-SetupResponse-SNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToBeSetupList-SetupResponse-SNterminated-Item

DRBsToBeSetupList-SetupResponse-SNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

sN-UL-PDCP-UP-TNLInfo UPTransportParameters,

dRB-QoS QoSFlowLevelQoSParameters,

pDCP-SNLength PDCPSNLength OPTIONAL,

rLC-Mode RLCMode,

uL-Configuration ULConfiguration OPTIONAL,

secondary-SN-UL-PDCP-UP-TNLInfo UPTransportParameters OPTIONAL,

duplicationActivation DuplicationActivation OPTIONAL,

qoSFlowsMappedtoDRB-SetupResponse-SNterminated QoSFlowsMappedtoDRB-SetupResponse-SNterminated,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeSetupList-SetupResponse-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeSetupList-SetupResponse-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional}|

{ ID id-RLCDuplicationInformation CRITICALITY ignore EXTENSION RLCDuplicationInformation PRESENCE optional},

...

}

QoSFlowsMappedtoDRB-SetupResponse-SNterminated ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF

QoSFlowsMappedtoDRB-SetupResponse-SNterminated-Item

QoSFlowsMappedtoDRB-SetupResponse-SNterminated-Item ::= SEQUENCE {

qoSFlowIdentifier QoSFlowIdentifier,

mCGRequestedGBRQoSFlowInfo GBRQoSFlowInfo OPTIONAL,

qosFlowMappingIndication QoSFlowMappingIndication OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsMappedtoDRB-SetupResponse-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsMappedtoDRB-SetupResponse-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-CurrentQoSParaSetIndex CRITICALITY ignore EXTENSION QoSParaSetIndex PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Setup Info - MN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceSetupInfo-MNterminated ::= SEQUENCE {

pduSessionType PDUSessionType,

dRBsToBeSetup DRBsToBeSetupList-Setup-MNterminated,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceSetupInfo-MNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceSetupInfo-MNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsToBeSetupList-Setup-MNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToBeSetupList-Setup-MNterminated-Item

DRBsToBeSetupList-Setup-MNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

mN-UL-PDCP-UP-TNLInfo UPTransportParameters,

rLC-Mode RLCMode,

uL-Configuration ULConfiguration OPTIONAL,

dRB-QoS QoSFlowLevelQoSParameters,

pDCP-SNLength PDCPSNLength OPTIONAL,

secondary-MN-UL-PDCP-UP-TNLInfo UPTransportParameters OPTIONAL,

duplicationActivation DuplicationActivation OPTIONAL,

qoSFlowsMappedtoDRB-Setup-MNterminated QoSFlowsMappedtoDRB-Setup-MNterminated,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeSetupList-Setup-MNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeSetupList-Setup-MNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional}|

{ ID id-RLCDuplicationInformation CRITICALITY ignore EXTENSION RLCDuplicationInformation PRESENCE optional},

...

}

QoSFlowsMappedtoDRB-Setup-MNterminated ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF QoSFlowsMappedtoDRB-Setup-MNterminated-Item

QoSFlowsMappedtoDRB-Setup-MNterminated-Item ::= SEQUENCE {

qoSFlowIdentifier QoSFlowIdentifier,

qoSFlowLevelQoSParameters QoSFlowLevelQoSParameters,

qosFlowMappingIndication QoSFlowMappingIndication OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsMappedtoDRB-Setup-MNterminated-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsMappedtoDRB-Setup-MNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-TSCTrafficCharacteristics CRITICALITY ignore EXTENSION TSCTrafficCharacteristics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Setup Response Info - MN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceSetupResponseInfo-MNterminated ::= SEQUENCE {

dRBsAdmittedList DRBsAdmittedList-SetupResponse-MNterminated,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceSetupResponseInfo-MNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceSetupResponseInfo-MNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ID id-DRBsNotAdmittedSetupModifyList CRITICALITY ignore EXTENSION DRB-List-withCause PRESENCE optional},

...

}

DRBsAdmittedList-SetupResponse-MNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsAdmittedList-SetupResponse-MNterminated-Item

DRBsAdmittedList-SetupResponse-MNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

sN-DL-SCG-UP-TNLInfo UPTransportParameters,

secondary-SN-DL-SCG-UP-TNLInfo UPTransportParameters OPTIONAL,

lCID LCID OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DRBsAdmittedList-SetupResponse-MNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsAdmittedList-SetupResponse-MNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional}|

{ ID id-QoSFlowsMappedtoDRB-SetupResponse-MNterminated CRITICALITY ignore EXTENSION QoSFlowsMappedtoDRB-SetupResponse-MNterminated PRESENCE optional},

...

}

QoSFlowsMappedtoDRB-SetupResponse-MNterminated ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF QoSFlowsMappedtoDRB-SetupResponse-MNterminated-Item

QoSFlowsMappedtoDRB-SetupResponse-MNterminated-Item ::= SEQUENCE {

qoSFlowIdentifier QoSFlowIdentifier,

currentQoSParaSetIndex QoSParaSetIndex,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsMappedtoDRB-SetupResponse-MNterminated-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsMappedtoDRB-SetupResponse-MNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Modification Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceModificationInfo-SNterminated ::= SEQUENCE {

uL-NG-U-TNLatUPF UPTransportLayerInformation OPTIONAL,

pduSessionNetworkInstance PDUSessionNetworkInstance OPTIONAL,

qosFlowsToBeSetup-List QoSFlowsToBeSetup-List-Setup-SNterminated OPTIONAL,

dataforwardinginfofromSource DataforwardingandOffloadingInfofromSource OPTIONAL,

qosFlowsToBeModified-List QoSFlowsToBeSetup-List-Modified-SNterminated OPTIONAL,

qoSFlowsToBeReleased-List QoSFlows-List-withCause OPTIONAL,

drbsToBeModifiedList DRBsToBeModified-List-Modified-SNterminated OPTIONAL,

dRBsToBeReleased DRB-List-withCause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceModificationInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceModificationInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-PDUSessionCommonNetworkInstance CRITICALITY ignore EXTENSION PDUSessionCommonNetworkInstance PRESENCE optional}|

{ID id-DefaultDRB-Allowed CRITICALITY ignore EXTENSION DefaultDRB-Allowed PRESENCE optional}|

{ID id-NonGBRResources-Offered CRITICALITY ignore EXTENSION NonGBRResources-Offered PRESENCE optional}|

{ID id-Redundant-UL-NG-U-TNLatUPF CRITICALITY ignore EXTENSION UPTransportLayerInformation PRESENCE optional}|

{ID id-RedundantCommonNetworkInstance CRITICALITY ignore EXTENSION PDUSessionCommonNetworkInstance PRESENCE optional},

...

}

QoSFlowsToBeSetup-List-Modified-SNterminated ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF QoSFlowsToBeSetup-List-Modified-SNterminated-Item

QoSFlowsToBeSetup-List-Modified-SNterminated-Item ::= SEQUENCE {

qfi QoSFlowIdentifier,

qosFlowLevelQoSParameters QoSFlowLevelQoSParameters OPTIONAL,

offeredGBRQoSFlowInfo GBRQoSFlowInfo OPTIONAL,

qosFlowMappingIndication QoSFlowMappingIndication OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsToBeSetup-List-Modified-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsToBeSetup-List-Modified-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-TSCTrafficCharacteristics CRITICALITY ignore EXTENSION TSCTrafficCharacteristics PRESENCE optional}|

{ ID id-RedundantQoSFlowIndicator CRITICALITY ignore EXTENSION RedundantQoSFlowIndicator PRESENCE optional},

...

}

DRBsToBeModified-List-Modified-SNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToBeModified-List-Modified-SNterminated-Item

DRBsToBeModified-List-Modified-SNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

mN-DL-SCG-UP-TNLInfo UPTransportParameters OPTIONAL,

secondary-MN-DL-SCG-UP-TNLInfo UPTransportParameters OPTIONAL,

lCID LCID OPTIONAL,

rlc-status RLC-Status OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeModified-List-Modified-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeModified-List-Modified-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Modification Response Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceModificationResponseInfo-SNterminated ::= SEQUENCE {

dL-NG-U-TNLatNG-RAN UPTransportLayerInformation OPTIONAL,

dRBsToBeSetup DRBsToBeSetupList-SetupResponse-SNterminated OPTIONAL,

dataforwardinginfoTarget DataForwardingInfoFromTargetNGRANnode OPTIONAL,

dRBsToBeModified DRBsToBeModifiedList-ModificationResponse-SNterminated OPTIONAL,

dRBsToBeReleased DRB-List-withCause OPTIONAL,

dataforwardinginfofromSource DataforwardingandOffloadingInfofromSource OPTIONAL,

qosFlowsNotAdmittedTBAdded QoSFlows-List-withCause OPTIONAL,

qosFlowsReleased QoSFlows-List-withCause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceModificationResponseInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceModificationResponseInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-DRB-IDs-takenintouse CRITICALITY reject EXTENSION DRB-List PRESENCE optional}|

{ ID id-Redundant-DL-NG-U-TNLatNG-RAN CRITICALITY ignore EXTENSION UPTransportLayerInformation PRESENCE optional},

...

}

DRBsToBeModifiedList-ModificationResponse-SNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF

DRBsToBeModifiedList-ModificationResponse-SNterminated-Item

DRBsToBeModifiedList-ModificationResponse-SNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

sN-UL-PDCP-UP-TNLInfo UPTransportParameters OPTIONAL,

dRB-QoS QoSFlowLevelQoSParameters OPTIONAL,

qoSFlowsMappedtoDRB-SetupResponse-SNterminated QoSFlowsMappedtoDRB-SetupResponse-SNterminated OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeModifiedList-ModificationResponse-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeModifiedList-ModificationResponse-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional}|

{ ID id-RLCDuplicationInformation CRITICALITY ignore EXTENSION RLCDuplicationInformation PRESENCE optional}|

{ ID id-secondary-SN-UL-PDCP-UP-TNLInfo CRITICALITY ignore EXTENSION UPTransportParameters PRESENCE optional}|

{ ID id-pdcpDuplicationConfiguration CRITICALITY ignore EXTENSION PDCPDuplicationConfiguration PRESENCE optional}|

{ ID id-duplicationActivation CRITICALITY ignore EXTENSION DuplicationActivation PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Modification Info - MN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceModificationInfo-MNterminated ::= SEQUENCE {

pduSessionType PDUSessionType,

dRBsToBeSetup DRBsToBeSetupList-Setup-MNterminated OPTIONAL,

dRBsToBeModified DRBsToBeModifiedList-Modification-MNterminated OPTIONAL,

dRBsToBeReleased DRB-List-withCause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceModificationInfo-MNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceModificationInfo-MNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsToBeModifiedList-Modification-MNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF

DRBsToBeModifiedList-Modification-MNterminated-Item

DRBsToBeModifiedList-Modification-MNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

mN-UL-PDCP-UP-TNLInfo UPTransportParameters OPTIONAL,

dRB-QoS QoSFlowLevelQoSParameters OPTIONAL,

secondary-MN-UL-PDCP-UP-TNLInfo UPTransportParameters OPTIONAL,

uL-Configuration ULConfiguration OPTIONAL,

pdcpDuplicationConfiguration PDCPDuplicationConfiguration OPTIONAL,

duplicationActivation DuplicationActivation OPTIONAL,

qoSFlowsMappedtoDRB-Setup-MNterminated QoSFlowsMappedtoDRB-Setup-MNterminated OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeModifiedList-Modification-MNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeModifiedList-Modification-MNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional}|

{ ID id-RLCDuplicationInformation CRITICALITY ignore EXTENSION RLCDuplicationInformation PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Modification Response Info - MN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceModificationResponseInfo-MNterminated ::= SEQUENCE {

dRBsAdmittedList DRBsAdmittedList-ModificationResponse-MNterminated,

dRBsReleasedList DRB-List OPTIONAL,

dRBsNotAdmittedSetupModifyList DRB-List-withCause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceModificationResponseInfo-MNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceModificationResponseInfo-MNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsAdmittedList-ModificationResponse-MNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsAdmittedList-ModificationResponse-MNterminated-Item

DRBsAdmittedList-ModificationResponse-MNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

sN-DL-SCG-UP-TNLInfo UPTransportParameters OPTIONAL,

secondary-SN-DL-SCG-UP-TNLInfo UPTransportParameters OPTIONAL,

lCID LCID OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DRBsAdmittedList-ModificationResponse-MNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsAdmittedList-ModificationResponse-MNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional}|

{ ID id-QoSFlowsMappedtoDRB-SetupResponse-MNterminated CRITICALITY ignore EXTENSION QoSFlowsMappedtoDRB-SetupResponse-MNterminated PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Change Required Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceChangeRequiredInfo-SNterminated ::= SEQUENCE {

dataforwardinginfofromSource DataforwardingandOffloadingInfofromSource OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceChangeRequiredInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceChangeRequiredInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Change Confirm Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceChangeConfirmInfo-SNterminated ::= SEQUENCE {

dataforwardinginfoTarget DataForwardingInfoFromTargetNGRANnode OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceChangeConfirmInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceChangeConfirmInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-DRB-IDs-takenintouse CRITICALITY reject EXTENSION DRB-List PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Change Required Info - MN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceChangeRequiredInfo-MNterminated ::= SEQUENCE {

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceChangeRequiredInfo-MNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceChangeRequiredInfo-MNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Change Confirm Info - MN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceChangeConfirmInfo-MNterminated ::= SEQUENCE {

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceChangeConfirmInfo-MNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceChangeConfirmInfo-MNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Modification Required Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceModRqdInfo-SNterminated ::= SEQUENCE {

dL-NG-U-TNLatNG-RAN UPTransportLayerInformation OPTIONAL,

qoSFlowsToBeReleased-List QoSFlows-List-withCause OPTIONAL,

dataforwardinginfofromSource DataforwardingandOffloadingInfofromSource OPTIONAL,

drbsToBeSetupList DRBsToBeSetup-List-ModRqd-SNterminated OPTIONAL,

drbsToBeModifiedList DRBsToBeModified-List-ModRqd-SNterminated OPTIONAL,

dRBsToBeReleased DRB-List-withCause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceModRqdInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceModRqdInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsToBeSetup-List-ModRqd-SNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToBeSetup-List-ModRqd-SNterminated-Item

DRBsToBeSetup-List-ModRqd-SNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

pDCP-SNLength PDCPSNLength OPTIONAL,

sn-UL-PDCP-UPTNLinfo UPTransportParameters,

dRB-QoS QoSFlowLevelQoSParameters,

secondary-SN-UL-PDCP-UP-TNLInfo UPTransportParameters OPTIONAL,

duplicationActivation DuplicationActivation OPTIONAL,

uL-Configuration ULConfiguration OPTIONAL,

qoSFlowsMappedtoDRB-ModRqd-SNterminated QoSFlowsSetupMappedtoDRB-ModRqd-SNterminated,

rLC-Mode RLCMode,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeSetup-List-ModRqd-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeSetup-List-ModRqd-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional}|

{ ID id-RLCDuplicationInformation CRITICALITY ignore EXTENSION RLCDuplicationInformation PRESENCE optional},

...

}

QoSFlowsSetupMappedtoDRB-ModRqd-SNterminated ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF

QoSFlowsSetupMappedtoDRB-ModRqd-SNterminated-Item

QoSFlowsSetupMappedtoDRB-ModRqd-SNterminated-Item ::= SEQUENCE {

qoSFlowIdentifier QoSFlowIdentifier,

mCGRequestedGBRQoSFlowInfo GBRQoSFlowInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsSetupMappedtoDRB-ModRqd-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsSetupMappedtoDRB-ModRqd-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsToBeModified-List-ModRqd-SNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToBeModified-List-ModRqd-SNterminated-Item

DRBsToBeModified-List-ModRqd-SNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

sN-UL-PDCP-UP-TNLInfo UPTransportParameters OPTIONAL,

dRB-QoS QoSFlowLevelQoSParameters OPTIONAL,

secondary-SN-UL-PDCP-UP-TNLInfo UPTransportParameters OPTIONAL,

uL-Configuration ULConfiguration OPTIONAL,

pdcpDuplicationConfiguration PDCPDuplicationConfiguration OPTIONAL,

duplicationActivation DuplicationActivation OPTIONAL,

qoSFlowsMappedtoDRB-ModRqd-SNterminated QoSFlowsModifiedMappedtoDRB-ModRqd-SNterminated OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeModified-List-ModRqd-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeModified-List-ModRqd-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional}|

{ ID id-RLCDuplicationInformation CRITICALITY ignore EXTENSION RLCDuplicationInformation PRESENCE optional},

...

}

QoSFlowsModifiedMappedtoDRB-ModRqd-SNterminated ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF

QoSFlowsModifiedMappedtoDRB-ModRqd-SNterminated-Item

QoSFlowsModifiedMappedtoDRB-ModRqd-SNterminated-Item ::= SEQUENCE {

qoSFlowIdentifier QoSFlowIdentifier,

mCGRequestedGBRQoSFlowInfo GBRQoSFlowInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsModifiedMappedtoDRB-ModRqd-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsModifiedMappedtoDRB-ModRqd-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Modification Confirm Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceModConfirmInfo-SNterminated ::= SEQUENCE {

uL-NG-U-TNLatUPF UPTransportLayerInformation OPTIONAL,

dRBsAdmittedList DRBsAdmittedList-ModConfirm-SNterminated,

dRBsNotAdmittedSetupModifyList DRB-List-withCause OPTIONAL,

dataforwardinginfoTarget DataForwardingInfoFromTargetNGRANnode OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceModConfirmInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceModConfirmInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-DRB-IDs-takenintouse CRITICALITY reject EXTENSION DRB-List PRESENCE optional},

...

}

DRBsAdmittedList-ModConfirm-SNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF

DRBsAdmittedList-ModConfirm-SNterminated-Item

DRBsAdmittedList-ModConfirm-SNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

mN-DL-CG-UP-TNLInfo UPTransportParameters OPTIONAL,

secondary-MN-DL-CG-UP-TNLInfo UPTransportParameters OPTIONAL,

lCID LCID OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DRBsAdmittedList-ModConfirm-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsAdmittedList-ModConfirm-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Modification Required Info - MN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceModRqdInfo-MNterminated ::= SEQUENCE {

dRBsToBeModified DRBsToBeModified-List-ModRqd-MNterminated OPTIONAL,

dRBsToBeReleased DRB-List-withCause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceModRqdInfo-MNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceModRqdInfo-MNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsToBeModified-List-ModRqd-MNterminated ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToBeModified-List-ModRqd-MNterminated-Item

DRBsToBeModified-List-ModRqd-MNterminated-Item ::= SEQUENCE {

drb-ID DRB-ID,

sN-DL-SCG-UP-TNLInfo UPTransportLayerInformation,

secondary-SN-DL-SCG-UP-TNLInfo UPTransportLayerInformation OPTIONAL,

lCID LCID OPTIONAL,

rlc-status RLC-Status OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeModified-List-ModRqd-MNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeModified-List-ModRqd-MNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-Additional-PDCP-Duplication-TNL-List CRITICALITY ignore EXTENSION Additional-PDCP-Duplication-TNL-List PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Modification Confirm Info - MN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceModConfirmInfo-MNterminated ::= SEQUENCE {

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceModConfirmInfo-MNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceModConfirmInfo-MNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session Resource Setup Complete Info - SN terminated

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceBearerSetupCompleteInfo-SNterminated ::= SEQUENCE {

dRBsToBeSetupList SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToBeSetupList-BearerSetupComplete-SNterminated-Item,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceBearerSetupCompleteInfo-SNterminated-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceBearerSetupCompleteInfo-SNterminated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

DRBsToBeSetupList-BearerSetupComplete-SNterminated-Item ::= SEQUENCE {

dRB-ID DRB-ID,

mN-Xn-U-TNLInfoatM UPTransportLayerInformation,

iE-Extensions ProtocolExtensionContainer { {DRBsToBeSetupList-BearerSetupComplete-SNterminated-Item-ExtIEs} } OPTIONAL,

...

}

DRBsToBeSetupList-BearerSetupComplete-SNterminated-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ID id-Secondary-MN-Xn-U-TNLInfoatM CRITICALITY ignore EXTENSION UPTransportLayerInformation PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU Session related message level IEs END

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PDUSessionResourceSecondaryRATUsageList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSecondaryRATUsageItem

PDUSessionResourceSecondaryRATUsageItem ::= SEQUENCE {

pDUSessionID PDUSession-ID,

secondaryRATUsageInformation SecondaryRATUsageInformation,

iE-Extensions ProtocolExtensionContainer { {PDUSessionResourceSecondaryRATUsageItem-ExtIEs} } OPTIONAL,

...

}

PDUSessionResourceSecondaryRATUsageItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionUsageReport ::= SEQUENCE {

rATType ENUMERATED {nr, eutra, ..., nr-unlicensed, e-utra-unlicensed},

pDUSessionTimedReportList VolumeTimedReportList,

iE-Extensions ProtocolExtensionContainer { {PDUSessionUsageReport-ExtIEs} } OPTIONAL,

...

}

PDUSessionUsageReport-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

PDUSessionType ::= ENUMERATED {ipv4, ipv6, ipv4v6, ethernet, unstructured, ...}

PDUSession-ID ::= INTEGER (0..255)

PDUSessionNetworkInstance ::= INTEGER (1..256, ...)

PDUSessionCommonNetworkInstance ::= OCTET STRING

Periodical ::= SEQUENCE {

iE-Extensions ProtocolExtensionContainer { { Periodical-ExtIEs} } OPTIONAL,

...

}

Periodical-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

Permutation ::= ENUMERATED {dfu, ufd, ...}

PLMN-Identity ::= OCTET STRING (SIZE(3))

PCIListForMDT ::= SEQUENCE (SIZE(1.. maxnoofNeighPCIforMDT)) OF NRPCI

PNI-NPN-Restricted-Information ::= ENUMERATED { restriced, not-restricted, ...}

PortNumber ::= BIT STRING (SIZE (16))

PriorityLevelQoS ::= INTEGER (1..127, ...)

ProtectedE-UTRAResourceIndication ::= SEQUENCE {

activationSFN ActivationSFN,

protectedResourceList ProtectedE-UTRAResourceList,

mbsfnControlRegionLength MBSFNControlRegionLength OPTIONAL,

pDCCHRegionLength INTEGER (1..3),

iE-Extensions ProtocolExtensionContainer { {ProtectedE-UTRAResourceIndication-ExtIEs} } OPTIONAL,

...

}

ProtectedE-UTRAResourceIndication-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ProtectedE-UTRAResourceList ::= SEQUENCE (SIZE (1.. maxnoofProtectedResourcePatterns)) OF ProtectedE-UTRAResource-Item

ProtectedE-UTRAResource-Item ::= SEQUENCE {

resourceType ENUMERATED {downlinknonCRS, cRS, uplink, ...},

intra-PRBProtectedResourceFootprint BIT STRING (SIZE(84, ...)),

protectedFootprintFrequencyPattern BIT STRING (SIZE(6..110, ...)),

protectedFootprintTimePattern ProtectedE-UTRAFootprintTimePattern,

iE-Extensions ProtocolExtensionContainer { {ProtectedE-UTRAResource-Item-ExtIEs} } OPTIONAL,

...

}

ProtectedE-UTRAResource-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ProtectedE-UTRAFootprintTimePattern ::= SEQUENCE {

protectedFootprintTimeperiodicity INTEGER (1..320, ...),

protectedFootrpintStartTime INTEGER (1..20, ...),

iE-Extensions ProtocolExtensionContainer { {ProtectedE-UTRAFootprintTimePattern-ExtIEs} } OPTIONAL,

...

}

ProtectedE-UTRAFootprintTimePattern-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- Q

QoSCharacteristics ::= CHOICE {

non-dynamic NonDynamic5QIDescriptor,

dynamic Dynamic5QIDescriptor,

choice-extension ProtocolIE-Single-Container { {QoSCharacteristics-ExtIEs} }

}

QoSCharacteristics-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

QoSFlowIdentifier ::= INTEGER (0..63, ...)

QoSFlowLevelQoSParameters ::= SEQUENCE {

qos-characteristics QoSCharacteristics,

allocationAndRetentionPrio AllocationandRetentionPriority,

gBRQoSFlowInfo GBRQoSFlowInfo OPTIONAL,

relectiveQoS ReflectiveQoSAttribute OPTIONAL,

additionalQoSflowInfo ENUMERATED {more-likely, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {QoSFlowLevelQoSParameters-ExtIEs} } OPTIONAL,

...

}

QoSFlowLevelQoSParameters-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ID id-QoSMonitoringRequest CRITICALITY ignore EXTENSION QosMonitoringRequest PRESENCE optional}|

{ID id-QosMonitoringReportingFrequency CRITICALITY ignore EXTENSION QosMonitoringReportingFrequency PRESENCE optional}|

{ID id-QoSMonitoringDisabled CRITICALITY ignore EXTENSION QoSMonitoringDisabled PRESENCE optional},

...

}

QoSFlowMappingIndication ::= ENUMERATED {

ul,

dl,

...

}

QoSFlowNotificationControlIndicationInfo ::= SEQUENCE (SIZE (1..maxnoofQoSFlows)) OF QoSFlowNotify-Item

QoSFlowNotify-Item ::= SEQUENCE {

qosFlowIdentifier QoSFlowIdentifier,

notificationInformation ENUMERATED {fulfilled, not-fulfilled, ...},

iE-Extensions ProtocolExtensionContainer { {QoSFlowNotificationControlIndicationInfo-ExtIEs} } OPTIONAL,

...

}

QoSFlowNotificationControlIndicationInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-CurrentQoSParaSetIndex CRITICALITY ignore EXTENSION QoSParaSetNotifyIndex PRESENCE optional },

...

}

QoSFlows-List ::= SEQUENCE (SIZE (1..maxnoofQoSFlows)) OF QoSFlow-Item

QoSFlow-Item ::= SEQUENCE {

qfi QoSFlowIdentifier,

qosFlowMappingIndication QoSFlowMappingIndication OPTIONAL,

iE-Extension ProtocolExtensionContainer { {QoSFlow-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlow-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

QoSFlows-List-withCause ::= SEQUENCE (SIZE (1..maxnoofQoSFlows)) OF QoSFlowwithCause-Item

QoSFlowwithCause-Item ::= SEQUENCE {

qfi QoSFlowIdentifier,

cause Cause OPTIONAL,

iE-Extension ProtocolExtensionContainer { {QoSFlowwithCause-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowwithCause-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

QoS-Mapping-Information ::= SEQUENCE {

dscp BIT STRING (SIZE(6)) OPTIONAL,

flow-label BIT STRING (SIZE(20)) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {QoS-Mapping-Information-ExtIEs} } OPTIONAL,

...

}

QoS-Mapping-Information-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

QoSParaSetIndex ::= INTEGER (1..8,...)

QoSParaSetNotifyIndex ::= INTEGER (0..8,...)

QoSFlowsAdmitted-List ::= SEQUENCE (SIZE (1..maxnoofQoSFlows)) OF QoSFlowsAdmitted-Item

QoSFlowsAdmitted-Item ::= SEQUENCE {

qfi QoSFlowIdentifier,

iE-Extension ProtocolExtensionContainer { {QoSFlowsAdmitted-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsAdmitted-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-CurrentQoSParaSetIndex CRITICALITY ignore EXTENSION QoSParaSetIndex PRESENCE optional },

...

}

QoSFlowsToBeSetup-List ::= SEQUENCE (SIZE (1..maxnoofQoSFlows)) OF QoSFlowsToBeSetup-Item

QoSFlowsToBeSetup-Item ::= SEQUENCE {

qfi QoSFlowIdentifier,

qosFlowLevelQoSParameters QoSFlowLevelQoSParameters,

e-RAB-ID E-RAB-ID OPTIONAL,

iE-Extension ProtocolExtensionContainer { {QoSFlowsToBeSetup-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsToBeSetup-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-TSCTrafficCharacteristics CRITICALITY ignore EXTENSION TSCTrafficCharacteristics PRESENCE optional}|

{ ID id-RedundantQoSFlowIndicator CRITICALITY ignore EXTENSION RedundantQoSFlowIndicator PRESENCE optional},

...

}

QoSFlowsUsageReportList ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF QoSFlowsUsageReport-Item

QoSFlowsUsageReport-Item ::= SEQUENCE {

qosFlowIdentifier QoSFlowIdentifier,

rATType ENUMERATED {nr, eutra, ..., nr-unlicensed, e-utra-unlicensed},

qoSFlowsTimedReportList VolumeTimedReportList,

iE-Extensions ProtocolExtensionContainer { {QoSFlowsUsageReport-Item-ExtIEs} } OPTIONAL,

...

}

QoSFlowsUsageReport-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

QosMonitoringRequest ::= ENUMERATED {ul, dl, both}

QoSMonitoringDisabled ::= ENUMERATED {true, ...}

QosMonitoringReportingFrequency ::= INTEGER (1..1800, ...)

-- R

RACH-Config-Common ::= OCTET STRING

RACH-Config-Common-IAB ::= OCTET STRING

RACHReportInformation ::= SEQUENCE (SIZE(1.. maxnoofRACHReports)) OF RACHReportList-Item

RACHReportList-Item ::= SEQUENCE {

rACHReport RACHReportContainer,

iE-Extensions ProtocolExtensionContainer { { RACHReportList-Item-ExtIEs} } OPTIONAL,

...

}

RACHReportList-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RACHReportContainer ::= OCTET STRING

RadioResourceStatus ::= CHOICE {

ng-eNB-RadioResourceStatus NG-eNB-RadioResourceStatus,

gNB-RadioResourceStatus GNB-RadioResourceStatus,

choice-extension ProtocolIE-Single-Container { { RadioResourceStatus-ExtIEs} }

}

RadioResourceStatus-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

RANAC ::= INTEGER (0..255)

RANAreaID ::= SEQUENCE {

tAC TAC,

rANAC RANAC OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {RANAreaID-ExtIEs} } OPTIONAL,

...

}

RANAreaID-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RANAreaID-List ::= SEQUENCE (SIZE(1..maxnoofRANAreasinRNA)) OF RANAreaID

Range ::= ENUMERATED {m50, m80, m180, m200, m350, m400, m500, m700, m1000, ...}

RANPagingArea ::= SEQUENCE {

pLMN-Identity PLMN-Identity,

rANPagingAreaChoice RANPagingAreaChoice,

iE-Extensions ProtocolExtensionContainer { {RANPagingArea-ExtIEs} } OPTIONAL,

...

}

RANPagingArea-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RANPagingAreaChoice ::= CHOICE {

cell-List NG-RAN-Cell-Identity-ListinRANPagingArea,

rANAreaID-List RANAreaID-List,

choice-extension ProtocolIE-Single-Container { {RANPagingAreaChoice-ExtIEs} }

}

RANPagingAreaChoice-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

RANPagingAttemptInfo ::= SEQUENCE {

pagingAttemptCount INTEGER (1..16, ...),

intendedNumberOfPagingAttempts INTEGER (1..16, ...),

nextPagingAreaScope ENUMERATED {same, changed, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {RANPagingAttemptInfo-ExtIEs} } OPTIONAL,

...

}

RANPagingAttemptInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RANPagingFailure ::= ENUMERATED {

true,

...

}

RBsetConfiguration ::= SEQUENCE {

subcarrierSpacing SSB-subcarrierSpacing,

rBsetSize ENUMERATED {size-2, size-4, size-8, size-16, size-32, size-64},

rB-Set-List RB-Set-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { RBsetConfiguration-ExtIEs} } OPTIONAL,

...

}

RBsetConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RB-Set-List ::= SEQUENCE (SIZE(1..maxnoofRBsetsPerCell)) OF RB-Set-List-Item

RB-Set-List-Item ::= SEQUENCE {

rBsetIndex INTEGER (1..maxnoofRBsetsPerCell),

initialRbIndex INTEGER (1..maxnoofPhysicalResourceBlocks),

iE-Extensions ProtocolExtensionContainer { { RB-Set-List-Item-ExtIEs} } OPTIONAL,

...

}

RB-Set-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RedundantQoSFlowIndicator ::= ENUMERATED {true, false}

RedundantPDUSessionInformation ::= SEQUENCE {

rSN RSN,

iE-Extensions ProtocolExtensionContainer { {RedundantPDUSessionInformation-ExtIEs} } OPTIONAL,

...

}

RedundantPDUSessionInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RSN ::= ENUMERATED {v1, v2, ...}

ReferenceID ::= INTEGER (1..64, ...) -- This IE may need to be refined.

ReflectiveQoSAttribute ::= ENUMERATED {subject-to-reflective-QoS, ...}

ReportAmountMDT ::= ENUMERATED{r1, r2, r4, r8, r16, r32, r64, infinity, ...}

ReportArea ::= ENUMERATED {

cell,

...

}

ReportIntervalMDT ::= ENUMERATED {ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240, min1, min6, min12, min30, min60, ...}

ReportType ::= CHOICE {

periodical Periodical,

eventTriggered EventTriggered,

...

}

ReportCharacteristics ::= BIT STRING(SIZE(32))

ReportingPeriodicity ::= ENUMERATED {

half-thousand-ms,

one-thousand-ms,

two-thousand-ms,

five-thousand-ms,

ten-thousand-ms,

...

}

RegistrationRequest ::= ENUMERATED {start, stop, add, ... }

RequestReferenceID ::= INTEGER (1..64, ...)

ReservedSubframePattern ::= SEQUENCE {

subframeType ENUMERATED {mbsfn, non-mbsfn, ...},

reservedSubframePattern BIT STRING (SIZE(10..160)),

mbsfnControlRegionLength MBSFNControlRegionLength OPTIONAL,

iE-Extension ProtocolExtensionContainer { {ReservedSubframePattern-ExtIEs} } OPTIONAL,

...

}

ReservedSubframePattern-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResetRequestTypeInfo ::= CHOICE {

fullReset ResetRequestTypeInfo-Full,

partialReset ResetRequestTypeInfo-Partial,

choice-extension ProtocolIE-Single-Container { {ResetRequestTypeInfo-ExtIEs} }

}

ResetRequestTypeInfo-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

ResetRequestTypeInfo-Full ::= SEQUENCE {

iE-Extension ProtocolExtensionContainer { {ResetRequestTypeInfo-Full-ExtIEs} } OPTIONAL,

...

}

ResetRequestTypeInfo-Full-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResetRequestTypeInfo-Partial ::= SEQUENCE {

ue-contexts-ToBeReleasedList ResetRequestPartialReleaseList,

iE-Extension ProtocolExtensionContainer { {ResetRequestTypeInfo-Partial-ExtIEs} } OPTIONAL,

...

}

ResetRequestTypeInfo-Partial-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResetRequestPartialReleaseList ::= SEQUENCE (SIZE(1..maxnoofUEContexts)) OF ResetRequestPartialReleaseItem

ResetRequestPartialReleaseItem ::= SEQUENCE {

ng-ran-node1UEXnAPID NG-RANnodeUEXnAPID OPTIONAL,

ng-ran-node2UEXnAPID NG-RANnodeUEXnAPID OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ResetRequestPartialReleaseItem-ExtIEs} } OPTIONAL,

...

}

ResetRequestPartialReleaseItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResetResponseTypeInfo ::= CHOICE {

fullReset ResetResponseTypeInfo-Full,

partialReset ResetResponseTypeInfo-Partial,

choice-extension ProtocolIE-Single-Container { {ResetResponseTypeInfo-ExtIEs} }

}

ResetResponseTypeInfo-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

ResetResponseTypeInfo-Full ::= SEQUENCE {

iE-Extension ProtocolExtensionContainer { {ResetResponseTypeInfo-Full-ExtIEs} } OPTIONAL,

...

}

ResetResponseTypeInfo-Full-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResetResponseTypeInfo-Partial ::= SEQUENCE {

ue-contexts-AdmittedToBeReleasedList ResetResponsePartialReleaseList,

iE-Extension ProtocolExtensionContainer { {ResetResponseTypeInfo-Partial-ExtIEs} } OPTIONAL,

...

}

ResetResponseTypeInfo-Partial-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ResetResponsePartialReleaseList ::= SEQUENCE (SIZE(1..maxnoofUEContexts)) OF ResetResponsePartialReleaseItem

ResetResponsePartialReleaseItem ::= SEQUENCE {

ng-ran-node1UEXnAPID NG-RANnodeUEXnAPID OPTIONAL,

ng-ran-node2UEXnAPID NG-RANnodeUEXnAPID OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ResetResponsePartialReleaseItem-ExtIEs} } OPTIONAL,

...

}

ResetResponsePartialReleaseItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RLCMode ::= ENUMERATED {

rlc-am,

rlc-um-bidirectional,

rlc-um-unidirectional-ul,

rlc-um-unidirectional-dl,

...

}

RLC-Status ::= SEQUENCE {

reestablishment-Indication Reestablishment-Indication,

iE-Extensions ProtocolExtensionContainer { {RLC-Status-ExtIEs} } OPTIONAL,

...

}

RLC-Status-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RLCDuplicationInformation ::= SEQUENCE {

rLCDuplicationStateList RLCDuplicationStateList,

rLC-PrimaryIndicator ENUMERATED {true, false} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {RLCDuplicationInformation-ItemExtIEs} } OPTIONAL

}

RLCDuplicationInformation-ItemExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RLCDuplicationStateList ::= SEQUENCE (SIZE(1..maxnoofRLCDuplicationstate)) OF RLCDuplicationState-Item

RLCDuplicationState-Item ::= SEQUENCE {

duplicationState ENUMERATED {active,inactive, ...},

iE-Extensions ProtocolExtensionContainer { {RLCDuplicationState-ItemExtIEs } } OPTIONAL,

...

}

RLCDuplicationState-ItemExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

Reestablishment-Indication ::= ENUMERATED {

reestablished,

...

}

RFSP-Index ::= INTEGER (1..256)

RRCConfigIndication ::= ENUMERATED {

full-config,

delta-config,

...

}

RRCConnections::= SEQUENCE {

noofRRCConnections NoofRRCConnections,

availableRRCConnectionCapacityValue AvailableRRCConnectionCapacityValue,

iE-Extensions ProtocolExtensionContainer { { RRCConnections-ExtIEs} } OPTIONAL,

...

}

RRCConnections-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RRCReestab-initiated ::= SEQUENCE {

rRRCReestab-initiated-reporting RRCReestab-Initiated-Reporting,

iE-Extensions ProtocolExtensionContainer { { RRCReestab-initiated-ExtIEs} } OPTIONAL,

...

}

RRCReestab-initiated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RRCReestab-Initiated-Reporting ::= CHOICE {

rRCReestab-reporting-wo-UERLFReport RRCReestab-Initiated-Reporting-wo-UERLFReport,

rRCReestab-reporting-with-UERLFReport RRCReestab-Initiated-Reporting-with-UERLFReport,

choice-extension ProtocolIE-Single-Container { {RRCReestab-Initiated-Reporting-ExtIEs} }

}

RRCReestab-Initiated-Reporting-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

RRCReestab-Initiated-Reporting-wo-UERLFReport ::= SEQUENCE {

failureCellPCI NG-RAN-CellPCI,

reestabCellCGI GlobalNG-RANCell-ID,

c-RNTI C-RNTI,

shortMAC-I MAC-I,

iE-Extensions ProtocolExtensionContainer { { RRCReestab-Initiated-Reporting-wo-UERLFReport-ExtIEs} } OPTIONAL,

...

}

RRCReestab-Initiated-Reporting-wo-UERLFReport-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RRCReestab-Initiated-Reporting-with-UERLFReport ::= SEQUENCE {

uERLFReportContainer UERLFReportContainer,

iE-Extensions ProtocolExtensionContainer { {RRCReestab-Initiated-Reporting-with-UERLFReport-ExtIEs} } OPTIONAL,

...

}

RRCReestab-Initiated-Reporting-with-UERLFReport-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RRCSetup-initiated ::= SEQUENCE {

rRRCSetup-Initiated-Reporting RRCSetup-Initiated-Reporting,

uERLFReportContainer UERLFReportContainer OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { RRCSetup-initiated-ExtIEs} } OPTIONAL,

...

}

RRCSetup-initiated-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RRCSetup-Initiated-Reporting ::= CHOICE {

rRCSetup-reporting-with-UERLFReport RRCSetup-Initiated-Reporting-with-UERLFReport,

choice-extension ProtocolIE-Single-Container { {RRCSetup-Initiated-Reporting-ExtIEs} }

}

RRCSetup-Initiated-Reporting-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

RRCSetup-Initiated-Reporting-with-UERLFReport ::= SEQUENCE {

uERLFReportContainer UERLFReportContainer,

iE-Extensions ProtocolExtensionContainer { {RRCSetup-Initiated-Reporting-with-UERLFReport-ExtIEs} } OPTIONAL,

...

}

RRCSetup-Initiated-Reporting-with-UERLFReport-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

RRCResumeCause ::= ENUMERATED {

rna-Update,

...

}

-- S

SecondarydataForwardingInfoFromTarget-Item::= SEQUENCE {

secondarydataForwardingInfoFromTarget DataForwardingInfoFromTargetNGRANnode,

iE-Extensions ProtocolExtensionContainer { { SecondarydataForwardingInfoFromTarget-Item-ExtIEs} } OPTIONAL,

...

}

SecondarydataForwardingInfoFromTarget-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SecondarydataForwardingInfoFromTarget-List ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF SecondarydataForwardingInfoFromTarget-Item

SCGConfigurationQuery ::= ENUMERATED {true, ...}

SCGIndicator ::= ENUMERATED{released, ...}

SecondaryRATUsageInformation ::= SEQUENCE {

pDUSessionUsageReport PDUSessionUsageReport OPTIONAL,

qosFlowsUsageReportList QoSFlowsUsageReportList OPTIONAL,

iE-Extension ProtocolExtensionContainer { {SecondaryRATUsageInformation-ExtIEs} } OPTIONAL,

...

}

SecondaryRATUsageInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SecurityIndication ::= SEQUENCE {

integrityProtectionIndication ENUMERATED {required, preferred, not-needed, ...},

confidentialityProtectionIndication ENUMERATED {required, preferred, not-needed, ...},

maximumIPdatarate MaximumIPdatarate OPTIONAL,

-- This IE shall be present if the *Integrity Protection* IE within the *Security Indication* IE is present and set to "required" or "preferred". --

iE-Extensions ProtocolExtensionContainer { {SecurityIndication-ExtIEs} } OPTIONAL,

...

}

SecurityIndication-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SecurityResult ::= SEQUENCE {

integrityProtectionResult ENUMERATED {performed, not-performed, ...},

confidentialityProtectionResult ENUMERATED {performed, not-performed, ...},

iE-Extensions ProtocolExtensionContainer { {SecurityResult-ExtIEs} } OPTIONAL,

...

}

SecurityResult-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SensorMeasurementConfiguration ::= SEQUENCE {

sensorMeasConfig SensorMeasConfig,

sensorMeasConfigNameList SensorMeasConfigNameList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { SensorMeasurementConfiguration-ExtIEs } } OPTIONAL,

...

}

SensorMeasurementConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SensorMeasConfigNameList ::= SEQUENCE (SIZE(1..maxnoofSensorName)) OF SensorName

SensorMeasConfig::= ENUMERATED {setup,...}

SensorName ::= SEQUENCE {

uncompensatedBarometricConfig ENUMERATED {true, ...} OPTIONAL,

ueSpeedConfig ENUMERATED {true, ...} OPTIONAL,

ueOrientationConfig ENUMERATED {true, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {SensorNameConfig-ExtIEs} } OPTIONAL,

...

}

SensorNameConfig-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- Served Cells E-UTRA IEs

ServedCellInformation-E-UTRA ::= SEQUENCE {

e-utra-pci E-UTRAPCI,

e-utra-cgi E-UTRA-CGI,

tac TAC,

ranac RANAC OPTIONAL,

broadcastPLMNs SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF ServedCellInformation-E-UTRA-perBPLMN,

e-utra-mode-info ServedCellInformation-E-UTRA-ModeInfo,

numberofAntennaPorts NumberOfAntennaPorts-E-UTRA OPTIONAL,

prach-configuration E-UTRAPRACHConfiguration OPTIONAL,

mBSFNsubframeInfo MBSFNSubframeInfo-E-UTRA OPTIONAL,

multibandInfo E-UTRAMultibandInfoList OPTIONAL,

freqBandIndicatorPriority ENUMERATED {not-broadcast, broadcast, ...} OPTIONAL,

bandwidthReducedSI ENUMERATED {scheduled, ...} OPTIONAL,

protectedE-UTRAResourceIndication ProtectedE-UTRAResourceIndication OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ServedCellInformation-E-UTRA-ExtIEs} } OPTIONAL,

...

}

ServedCellInformation-E-UTRA-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-BPLMN-ID-Info-EUTRA CRITICALITY ignore EXTENSION BPLMN-ID-Info-EUTRA PRESENCE optional }|

{ ID id-NPRACHConfiguration CRITICALITY ignore EXTENSION NPRACHConfiguration PRESENCE optional},

...

}

ServedCellInformation-E-UTRA-perBPLMN ::= SEQUENCE {

plmn-id PLMN-Identity,

iE-Extensions ProtocolExtensionContainer { {ServedCellInformation-E-UTRA-perBPLMN-ExtIEs} } OPTIONAL,

...

}

ServedCellInformation-E-UTRA-perBPLMN-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ServedCellInformation-E-UTRA-ModeInfo ::= CHOICE {

fdd ServedCellInformation-E-UTRA-FDDInfo,

tdd ServedCellInformation-E-UTRA-TDDInfo,

choice-extension ProtocolIE-Single-Container{ {ServedCellInformation-E-UTRA-ModeInfo-ExtIEs} }

}

ServedCellInformation-E-UTRA-ModeInfo-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

ServedCellInformation-E-UTRA-FDDInfo ::= SEQUENCE {

ul-earfcn E-UTRAARFCN,

dl-earfcn E-UTRAARFCN,

ul-e-utraTxBW E-UTRATransmissionBandwidth,

dl-e-utraTxBW E-UTRATransmissionBandwidth,

iE-Extensions ProtocolExtensionContainer { {ServedCellInformation-E-UTRA-FDDInfo-ExtIEs} } OPTIONAL,

...

}

ServedCellInformation-E-UTRA-FDDInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-OffsetOfNbiotChannelNumberToDL-EARFCN CRITICALITY reject EXTENSION OffsetOfNbiotChannelNumberToEARFCN PRESENCE optional}|

{ ID id-OffsetOfNbiotChannelNumberToUL-EARFCN CRITICALITY reject EXTENSION OffsetOfNbiotChannelNumberToEARFCN PRESENCE optional},

...

}

ServedCellInformation-E-UTRA-TDDInfo ::= SEQUENCE {

earfcn E-UTRAARFCN,

e-utraTxBW E-UTRATransmissionBandwidth,

subframeAssignmnet ENUMERATED {sa0,sa1,sa2,sa3,sa4,sa5,sa6,...},

specialSubframeInfo SpecialSubframeInfo-E-UTRA,

iE-Extensions ProtocolExtensionContainer { {ServedCellInformation-E-UTRA-TDDInfo-ExtIEs} } OPTIONAL,

...

}

ServedCellInformation-E-UTRA-TDDInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-OffsetOfNbiotChannelNumberToDL-EARFCN CRITICALITY reject EXTENSION OffsetOfNbiotChannelNumberToEARFCN PRESENCE optional}|

{ ID id-NBIoT-UL-DL-AlignmentOffset CRITICALITY reject EXTENSION NBIoT-UL-DL-AlignmentOffset PRESENCE optional},

...

}

ServedCells-E-UTRA ::= SEQUENCE (SIZE (1..maxnoofCellsinNG-RANnode)) OF ServedCells-E-UTRA-Item

ServedCells-E-UTRA-Item ::= SEQUENCE {

served-cell-info-E-UTRA ServedCellInformation-E-UTRA,

neighbour-info-NR NeighbourInformation-NR OPTIONAL,

neighbour-info-E-UTRA NeighbourInformation-E-UTRA OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ServedCells-E-UTRA-Item-ExtIEs} } OPTIONAL,

...

}

ServedCells-E-UTRA-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-SFN-Offset CRITICALITY ignore EXTENSION SFN-Offset PRESENCE optional },

...

}

ServedCellsToUpdate-E-UTRA ::= SEQUENCE {

served-Cells-ToAdd-E-UTRA ServedCells-E-UTRA OPTIONAL,

served-Cells-ToModify-E-UTRA ServedCells-ToModify-E-UTRA OPTIONAL,

served-Cells-ToDelete-E-UTRA SEQUENCE (SIZE (1..maxnoofCellsinNG-RANnode)) OF E-UTRA-CGI OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ServedCellsToUpdate-E-UTRA-ExtIEs} } OPTIONAL,

...

}

ServedCellsToUpdate-E-UTRA-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ServedCells-ToModify-E-UTRA ::= SEQUENCE (SIZE (1..maxnoofCellsinNG-RANnode)) OF ServedCells-ToModify-E-UTRA-Item

ServedCells-ToModify-E-UTRA-Item ::= SEQUENCE {

old-ECGI E-UTRA-CGI,

served-cell-info-E-UTRA ServedCellInformation-E-UTRA,

neighbour-info-NR NeighbourInformation-NR OPTIONAL,

neighbour-info-E-UTRA NeighbourInformation-E-UTRA OPTIONAL,

deactivation-indication ENUMERATED {deactivated, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {Served-cells-ToModify-E-UTRA-Item-ExtIEs} } OPTIONAL,

...

}

Served-cells-ToModify-E-UTRA-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- Served Cells NR IEs

ServedCellInformation-NR ::= SEQUENCE {

nrPCI NRPCI,

cellID NR-CGI,

tac TAC,

ranac RANAC OPTIONAL,

broadcastPLMN BroadcastPLMNs,

nrModeInfo NRModeInfo,

measurementTimingConfiguration OCTET STRING,

connectivitySupport Connectivity-Support,

iE-Extensions ProtocolExtensionContainer { {ServedCellInformation-NR-ExtIEs} } OPTIONAL,

...

}

ServedCellInformation-NR-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-BPLMN-ID-Info-NR CRITICALITY ignore EXTENSION BPLMN-ID-Info-NR PRESENCE optional }|

{ ID id-ConfiguredTACIndication CRITICALITY ignore EXTENSION ConfiguredTACIndication PRESENCE optional }|

{ ID id-SSB-PositionsInBurst CRITICALITY ignore EXTENSION SSB-PositionsInBurst PRESENCE optional }|

{ ID id-NRCellPRACHConfig CRITICALITY ignore EXTENSION NRCellPRACHConfig PRESENCE optional }|

{ ID id-NPN-Broadcast-Information CRITICALITY reject EXTENSION NPN-Broadcast-Information PRESENCE optional }|

{ ID id-CSI-RSTransmissionIndication CRITICALITY ignore EXTENSION CSI-RSTransmissionIndication PRESENCE optional } |

{ ID id-SFN-Offset CRITICALITY ignore EXTENSION SFN-Offset PRESENCE optional },

...

}

SFN-Offset ::= SEQUENCE {

sFN-Time-Offset BIT STRING (SIZE(24)),

iE-Extensions ProtocolExtensionContainer { {SFN-Offset-ExtIEs} } OPTIONAL,

...

}

SFN-Offset-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ServedCells-NR ::= SEQUENCE (SIZE (1..maxnoofCellsinNG-RANnode)) OF ServedCells-NR-Item

ServedCells-NR-Item ::= SEQUENCE {

served-cell-info-NR ServedCellInformation-NR,

neighbour-info-NR NeighbourInformation-NR OPTIONAL,

neighbour-info-E-UTRA NeighbourInformation-E-UTRA OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ServedCells-NR-Item-ExtIEs} } OPTIONAL,

...

}

ServedCells-NR-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ServedCells-ToModify-NR ::= SEQUENCE (SIZE (1..maxnoofCellsinNG-RANnode)) OF ServedCells-ToModify-NR-Item

ServedCells-ToModify-NR-Item ::= SEQUENCE {

old-NR-CGI NR-CGI,

served-cell-info-NR ServedCellInformation-NR,

neighbour-info-NR NeighbourInformation-NR OPTIONAL,

neighbour-info-E-UTRA NeighbourInformation-E-UTRA OPTIONAL,

deactivation-indication ENUMERATED {deactivated, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {Served-cells-ToModify-NR-Item-ExtIEs} } OPTIONAL,

...

}

Served-cells-ToModify-NR-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ServedCellsToUpdate-NR ::= SEQUENCE {

served-Cells-ToAdd-NR ServedCells-NR OPTIONAL,

served-Cells-ToModify-NR ServedCells-ToModify-NR OPTIONAL,

served-Cells-ToDelete-NR SEQUENCE (SIZE (1..maxnoofCellsinNG-RANnode)) OF NR-CGI OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {ServedCellsToUpdate-NR-ExtIEs} } OPTIONAL,

...

}

ServedCellsToUpdate-NR-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SharedResourceType ::= CHOICE {

ul-onlySharing SharedResourceType-UL-OnlySharing,

ul-and-dl-Sharing SharedResourceType-ULDL-Sharing,

choice-extension ProtocolIE-Single-Container { {SharedResourceType-ExtIEs} }

}

SharedResourceType-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

SharedResourceType-UL-OnlySharing ::= SEQUENCE {

ul-resourceBitmap DataTrafficResources,

iE-Extensions ProtocolExtensionContainer { {SharedResourceType-UL-OnlySharing-ExtIEs} } OPTIONAL,

...

}

SharedResourceType-UL-OnlySharing-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SharedResourceType-ULDL-Sharing ::= CHOICE {

ul-resources SharedResourceType-ULDL-Sharing-UL-Resources,

dl-resources SharedResourceType-ULDL-Sharing-DL-Resources,

choice-extension ProtocolIE-Single-Container { {SharedResourceType-ULDL-Sharing-ExtIEs} }

}

SharedResourceType-ULDL-Sharing-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

SharedResourceType-ULDL-Sharing-UL-Resources ::= CHOICE {

unchanged NULL,

changed SharedResourceType-ULDL-Sharing-UL-ResourcesChanged,

choice-extension ProtocolIE-Single-Container { {SharedResourceType-ULDL-Sharing-UL-Resources-ExtIEs} }

}

SharedResourceType-ULDL-Sharing-UL-Resources-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

SharedResourceType-ULDL-Sharing-UL-ResourcesChanged ::= SEQUENCE {

ul-resourceBitmap DataTrafficResources,

iE-Extensions ProtocolExtensionContainer { {SharedResourceType-ULDL-Sharing-UL-ResourcesChanged-ExtIEs} } OPTIONAL,

...

}

SharedResourceType-ULDL-Sharing-UL-ResourcesChanged-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SharedResourceType-ULDL-Sharing-DL-Resources ::= CHOICE {

unchanged NULL,

changed SharedResourceType-ULDL-Sharing-DL-ResourcesChanged,

choice-extension ProtocolIE-Single-Container { {SharedResourceType-ULDL-Sharing-DL-Resources-ExtIEs} }

}

SharedResourceType-ULDL-Sharing-DL-Resources-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

SharedResourceType-ULDL-Sharing-DL-ResourcesChanged ::= SEQUENCE {

dl-resourceBitmap DataTrafficResources,

iE-Extensions ProtocolExtensionContainer { {SharedResourceType-ULDL-Sharing-DL-ResourcesChanged-ExtIEs} } OPTIONAL,

...

}

SharedResourceType-ULDL-Sharing-DL-ResourcesChanged-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SliceAvailableCapacity ::= SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF SliceAvailableCapacity-Item

SliceAvailableCapacity-Item ::= SEQUENCE {

pLMNIdentity PLMN-Identity,

sNSSAIAvailableCapacity-List SNSSAIAvailableCapacity-List,

iE-Extensions ProtocolExtensionContainer { { SliceAvailableCapacity-Item-ExtIEs} } OPTIONAL,

...

}

SliceAvailableCapacity-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SNSSAIAvailableCapacity-List ::= SEQUENCE (SIZE(1.. maxnoofSliceItems)) OF SNSSAIAvailableCapacity-Item

SNSSAIAvailableCapacity-Item ::= SEQUENCE {

sNSSAI S-NSSAI,

sliceAvailableCapacityValueDownlink INTEGER (0..100),

sliceAvailableCapacityValueUplink INTEGER (0..100),

iE-Extensions ProtocolExtensionContainer { { SNSSAIAvailableCapacity-Item-ExtIEs } } OPTIONAL

}

SNSSAIAvailableCapacity-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SliceSupport-List ::= SEQUENCE (SIZE(1..maxnoofSliceItems)) OF S-NSSAI

SliceToReport-List ::= SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF SliceToReport-List-Item

SliceToReport-List-Item ::= SEQUENCE {

pLMNIdentity PLMN-Identity,

sNSSAIlist SNSSAI-list,

iE-Extensions ProtocolExtensionContainer { { SliceToReport-List-Item-ExtIEs} } OPTIONAL,

...

}

SliceToReport-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SNSSAI-list ::= SEQUENCE (SIZE(1.. maxnoofSliceItems)) OF SNSSAI-Item

SNSSAI-Item ::= SEQUENCE {

sNSSAI S-NSSAI,

iE-Extensions ProtocolExtensionContainer { { SNSSAI-Item-ExtIEs } } OPTIONAL

}

SNSSAI-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SlotConfiguration-List ::= SEQUENCE (SIZE (1..maxnoofslots)) OF SlotConfiguration-List-Item

SlotConfiguration-List-Item ::= SEQUENCE {

slotIndex INTEGER (0..5119),

symbolAllocation-in-Slot SymbolAllocation-in-Slot,

iE-Extensions ProtocolExtensionContainer { {SlotConfiguration-List-Item-ExtIEs} } OPTIONAL,

...

}

SlotConfiguration-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

S-NG-RANnode-SecurityKey ::= BIT STRING (SIZE(256))

S-NG-RANnode-Addition-Trigger-Ind ::= ENUMERATED {

sn-change,

inter-MN-HO,

intra-MN-HO,

...

}

S-NSSAI ::= SEQUENCE {

sst OCTET STRING (SIZE(1)),

sd OCTET STRING (SIZE(3)) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {S-NSSAI-ExtIEs} } OPTIONAL,

...

}

S-NSSAI-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SNTriggered ::=ENUMERATED{

true,

...

}

SpecialSubframeInfo-E-UTRA ::= SEQUENCE {

specialSubframePattern SpecialSubframePatterns-E-UTRA,

cyclicPrefixDL CyclicPrefix-E-UTRA-DL,

cyclicPrefixUL CyclicPrefix-E-UTRA-UL,

iE-Extensions ProtocolExtensionContainer { {SpecialSubframeInfo-E-UTRA-ExtIEs} } OPTIONAL,

...

}

SpecialSubframeInfo-E-UTRA-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SpecialSubframePatterns-E-UTRA ::= ENUMERATED {

ssp0,

ssp1,

ssp2,

ssp3,

ssp4,

ssp5,

ssp6,

ssp7,

ssp8,

ssp9,

ssp10,

...

}

SpectrumSharingGroupID ::= INTEGER (1..maxnoofCellsinNG-RANnode)

SplitSessionIndicator ::= ENUMERATED {

split,

...

}

SplitSRBsTypes ::= ENUMERATED {srb1, srb2, srb1and2, ...}

SSBAreaCapacityValue-List ::= SEQUENCE (SIZE(1..maxnoofSSBAreas)) OF SSBAreaCapacityValue-List-Item

SSBAreaCapacityValue-List-Item ::= SEQUENCE {

sSBIndex INTEGER(0..63),

ssbAreaCapacityValue INTEGER (0..100),

iE-Extensions ProtocolExtensionContainer { { SSBAreaCapacityValue-List-Item-ExtIEs} } OPTIONAL,

...

}

SSBAreaCapacityValue-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SSBAreaRadioResourceStatus-List ::= SEQUENCE (SIZE(1..maxnoofSSBAreas)) OF SSBAreaRadioResourceStatus-List-Item

SSBAreaRadioResourceStatus-List-Item ::= SEQUENCE {

sSBIndex INTEGER(0..63),

ssb-Area-DL-GBR-PRB-usage DL-GBR-PRB-usage,

ssb-Area-UL-GBR-PRB-usage UL-GBR-PRB-usage,

ssb-Area-dL-non-GBR-PRB-usage DL-non-GBR-PRB-usage,

ssb-Area-uL-non-GBR-PRB-usage UL-non-GBR-PRB-usage,

ssb-Area-dL-Total-PRB-usage DL-Total-PRB-usage,

ssb-Area-uL-Total-PRB-usage UL-Total-PRB-usage,

iE-Extensions ProtocolExtensionContainer { { SSBAreaRadioResourceStatus-List-Item-ExtIEs} } OPTIONAL,

...

}

SSBAreaRadioResourceStatus-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-DL-scheduling-PDCCH-CCE-usage CRITICALITY ignore EXTENSION DL-scheduling-PDCCH-CCE-usage PRESENCE optional}|

{ ID id-UL-scheduling-PDCCH-CCE-usage CRITICALITY ignore EXTENSION UL-scheduling-PDCCH-CCE-usage PRESENCE optional},

...

}

SSB-PositionsInBurst ::= CHOICE {

shortBitmap BIT STRING (SIZE (4)),

mediumBitmap BIT STRING (SIZE (8)),

longBitmap BIT STRING (SIZE (64)),

choice-extension ProtocolIE-Single-Container { {SSB-PositionsInBurst-ExtIEs} }

}

SSB-PositionsInBurst-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

SSB-freqInfo ::= INTEGER (0..maxNRARFCN)

SSB-subcarrierSpacing ::= ENUMERATED {kHz15, kHz30, kHz120, kHz240, spare3, spare2, spare1, ...}

SSBToReport-List ::= SEQUENCE (SIZE(1..maxnoofSSBAreas)) OF SSBToReport-List-Item

SSBToReport-List-Item ::= SEQUENCE {

sSBIndex INTEGER(0..63),

iE-Extensions ProtocolExtensionContainer { { SSBToReport-List-Item-ExtIEs} } OPTIONAL,

...

}

SSBToReport-List-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SSB-transmissionPeriodicity ::= ENUMERATED {sf10, sf20, sf40, sf80, sf160, sf320, sf640, ...}

SSB-transmissionTimingOffset ::= INTEGER (0..127, ...)

SSB-transmissionBitmap ::= CHOICE {

shortBitmap BIT STRING (SIZE (4)),

mediumBitmap BIT STRING (SIZE (8)),

longBitmap BIT STRING (SIZE (64)),

choice-extension ProtocolIE-Single-Container { { SSB-transmisisonBitmap-ExtIEs} }

}

SSB-transmisisonBitmap-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

SUL-FrequencyBand ::= INTEGER (1..1024)

SUL-Information ::= SEQUENCE {

sulFrequencyInfo NRARFCN,

sulTransmissionBandwidth NRTransmissionBandwidth,

iE-Extensions ProtocolExtensionContainer { {SUL-Information-ExtIEs} } OPTIONAL,

...

}

SUL-Information-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-CarrierList CRITICALITY ignore EXTENSION NRCarrierList PRESENCE optional }|

{ ID id-FrequencyShift7p5khz CRITICALITY ignore EXTENSION FrequencyShift7p5khz PRESENCE optional },

...

}

SupportedSULBandList ::= SEQUENCE (SIZE(1..maxnoofNRCellBands)) OF SupportedSULBandItem

SupportedSULBandItem ::= SEQUENCE {

sulBandItem SUL-FrequencyBand,

iE-Extensions ProtocolExtensionContainer { {SupportedSULBandItem-ExtIEs} } OPTIONAL,

...

}

SupportedSULBandItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SymbolAllocation-in-Slot ::= CHOICE {

allDL SymbolAllocation-in-Slot-AllDL,

allUL SymbolAllocation-in-Slot-AllUL,

bothDLandUL SymbolAllocation-in-Slot-BothDLandUL,

choice-extension ProtocolIE-Single-Container { {SymbolAllocation-in-Slot-ExtIEs} }

}

SymbolAllocation-in-Slot-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

SymbolAllocation-in-Slot-AllDL ::= SEQUENCE {

iE-Extension ProtocolExtensionContainer { {SymbolAllocation-in-Slot-AllDL-ExtIEs} } OPTIONAL,

...

}

SymbolAllocation-in-Slot-AllDL-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SymbolAllocation-in-Slot-AllUL ::= SEQUENCE {

iE-Extension ProtocolExtensionContainer { {SymbolAllocation-in-Slot-AllUL-ExtIEs} } OPTIONAL,

...

}

SymbolAllocation-in-Slot-AllUL-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

SymbolAllocation-in-Slot-BothDLandUL ::= SEQUENCE {

numberofDLSymbols INTEGER (0..13),

numberofULSymbols INTEGER (0..13),

iE-Extension ProtocolExtensionContainer { {SymbolAllocation-in-Slot-BothDLandUL-ExtIEs} } OPTIONAL,

...

}

SymbolAllocation-in-Slot-BothDLandUL-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-permutation CRITICALITY ignore EXTENSION Permutation PRESENCE optional },

...

}

-- T

TABasedMDT ::= SEQUENCE {

tAListforMDT TAListforMDT,

iE-Extensions ProtocolExtensionContainer { {TABasedMDT-ExtIEs} } OPTIONAL,

...

}

TABasedMDT-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TAIBasedMDT ::= SEQUENCE {

tAIListforMDT TAIListforMDT,

iE-Extensions ProtocolExtensionContainer { {TAIBasedMDT-ExtIEs} } OPTIONAL,

...

}

TAIBasedMDT-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TAIListforMDT ::= SEQUENCE (SIZE(1..maxnoofTAforMDT)) OF TAIforMDT-Item

TAIforMDT-Item ::= SEQUENCE {

plmn-ID PLMN-Identity,

tAC TAC,

iE-Extensions ProtocolExtensionContainer { {TAIforMDT-Item-ExtIEs} } OPTIONAL,

...

}

TAIforMDT-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TAC ::= OCTET STRING (SIZE (3))

TAISupport-List ::= SEQUENCE (SIZE(1..maxnoofsupportedTACs)) OF TAISupport-Item

TAISupport-Item ::= SEQUENCE {

tac TAC,

broadcastPLMNs SEQUENCE (SIZE(1..maxnoofsupportedPLMNs)) OF BroadcastPLMNinTAISupport-Item,

iE-Extensions ProtocolExtensionContainer { {TAISupport-Item-ExtIEs} } OPTIONAL,

...

}

TAISupport-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TAListforMDT ::= SEQUENCE (SIZE(1..maxnoofTAforMDT)) OF TAC

TargetCellinEUTRAN ::= OCTET STRING -- This IE is to be encoded according to *Global Cell ID* in the *Last Visited E-UTRAN Cell Information* IE, as defined in in TS 36.413 [31]

Target-CGI ::= CHOICE {

nr NR-CGI,

e-utra E-UTRA-CGI,

choice-extension ProtocolIE-Single-Container { {TargetCGI-ExtIEs} }

}

TargetCGI-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

TDDULDLConfigurationCommonNR ::= OCTET STRING

TargetCellList ::= SEQUENCE (SIZE(1..maxnoofCHOcells)) OF TargetCellList-Item

TargetCellList-Item ::= SEQUENCE {

target-cell Target-CGI,

iE-Extensions ProtocolExtensionContainer { { TargetCellList-Item-ExtIEs} } OPTIONAL

}

TargetCellList-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

Threshold-RSRQ ::= INTEGER(0..34)

Threshold-RSRP ::= INTEGER(0..97)

Threshold-SINR ::= INTEGER(0..127)

TimeToTrigger ::= ENUMERATED {ms0, ms40, ms64, ms80, ms100, ms128, ms160, ms256, ms320, ms480, ms512, ms640, ms1024, ms1280, ms2560, ms5120}

TimeToWait ::= ENUMERATED {

v1s,

v2s,

v5s,

v10s,

v20s,

v60s,

...

}

TNLConfigurationInfo ::= SEQUENCE {

extendedUPTransportLayerAddressesToAdd ExtTLAs OPTIONAL,

extendedUPTransportLayerAddressesToRemove ExtTLAs OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {TNLConfigurationInfo-ExtIEs} } OPTIONAL,

...

}

TNLConfigurationInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TNLA-To-Add-List ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF TNLA-To-Add-Item

TNLA-To-Add-Item ::= SEQUENCE {

tNLAssociationTransportLayerAddress CPTransportLayerInformation,

tNLAssociationUsage TNLAssociationUsage,

iE-Extensions ProtocolExtensionContainer { { TNLA-To-Add-Item-ExtIEs} } OPTIONAL

}

TNLA-To-Add-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TNLA-To-Update-List ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF TNLA-To-Update-Item

TNLA-To-Update-Item::= SEQUENCE {

tNLAssociationTransportLayerAddress CPTransportLayerInformation,

tNLAssociationUsage TNLAssociationUsage OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { TNLA-To-Update-Item-ExtIEs} } OPTIONAL

}

TNLA-To-Update-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TNLA-To-Remove-List ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF TNLA-To-Remove-Item

TNLA-To-Remove-Item::= SEQUENCE {

tNLAssociationTransportLayerAddress CPTransportLayerInformation,

iE-Extensions ProtocolExtensionContainer { { TNLA-To-Remove-Item-ExtIEs} } OPTIONAL

}

TNLA-To-Remove-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TNLA-Setup-List ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF TNLA-Setup-Item

TNLA-Setup-Item ::= SEQUENCE {

tNLAssociationTransportLayerAddress CPTransportLayerInformation,

iE-Extensions ProtocolExtensionContainer { { TNLA-Setup-Item-ExtIEs} } OPTIONAL,

...

}

TNLA-Setup-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TNLA-Failed-To-Setup-List ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF TNLA-Failed-To-Setup-Item

TNLA-Failed-To-Setup-Item ::= SEQUENCE {

tNLAssociationTransportLayerAddress CPTransportLayerInformation,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { TNLA-Failed-To-Setup-Item-ExtIEs} } OPTIONAL

}

TNLA-Failed-To-Setup-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TNLAssociationUsage ::= ENUMERATED {

ue,

non-ue,

both,

...

}

TransportLayerAddress ::= BIT STRING (SIZE(1..160, ...))

TraceActivation ::= SEQUENCE {

ng-ran-TraceID NG-RANTraceID,

interfaces-to-trace BIT STRING { ng-c (0), x-nc (1), uu (2), f1-c (3), e1 (4)} (SIZE(8)),

trace-depth Trace-Depth,

trace-coll-address TransportLayerAddress,

ie-Extension ProtocolExtensionContainer { {TraceActivation-ExtIEs} } OPTIONAL,

...

}

TraceActivation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

-- Extension to support MDT –

{ ID id-TraceCollectionEntityURI CRITICALITY ignore EXTENSION URIaddress PRESENCE optional}|

{ ID id-MDT-Configuration CRITICALITY ignore EXTENSION MDT-Configuration PRESENCE optional},

...

}

Trace-Depth ::= ENUMERATED {

minimum,

medium,

maximum,

minimumWithoutVendorSpecificExtension,

mediumWithoutVendorSpecificExtension,

maximumWithoutVendorSpecificExtension,

...

}

TrafficIndex ::= INTEGER (1..1024, ...)

TrafficProfile ::= CHOICE {

uPTraffic QoSFlowLevelQoSParameters,

nonUPTraffic NonUPTraffic,

choice-extension ProtocolIE-Single-Container { {TrafficProfile-ExtIEs} }

}

TrafficProfile-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

TrafficReleaseType ::= CHOICE {

fullRelease AllTrafficIndication,

partialRelease TrafficToBeRelease-List,

choice-extension ProtocolIE-Single-Container { {TrafficReleaseType-ExtIEs} }

}

TrafficReleaseType-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

TrafficToBeReleaseInformation ::= SEQUENCE {

releaseType TrafficReleaseType,

ie-Extensions ProtocolExtensionContainer { {TrafficToBeReleaseInformation-ExtIEs} } OPTIONAL,

...

}

TrafficToBeReleaseInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TrafficToBeRelease-List ::= SEQUENCE (SIZE(1..maxnoofTrafficIndexEntries)) OF TrafficToBeRelease-Item

TrafficToBeRelease-Item ::= SEQUENCE {

trafficIndex TrafficIndex,

bHInfoList BHInfoList OPTIONAL,

iE-Extension ProtocolExtensionContainer { {TrafficToBeRelease-Item-ExtIEs} } OPTIONAL,

...

}

TrafficToBeRelease-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TSCTrafficCharacteristics ::= SEQUENCE {

tSCAssistanceInformationDownlink TSCAssistanceInformation OPTIONAL,

tSCAssistanceInformationUplink TSCAssistanceInformation OPTIONAL,

ie-Extension ProtocolExtensionContainer { {TSCTrafficCharacteristics-ExtIEs} } OPTIONAL,

...

}

TSCTrafficCharacteristics-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TSCAssistanceInformation ::= SEQUENCE {

periodicity INTEGER (0.. 640000, ...),

burstArrivalTime OCTET STRING OPTIONAL,

ie-Extension ProtocolExtensionContainer { { TSCAssistanceInformation-ExtIEs} } OPTIONAL,

...

}

TSCAssistanceInformation-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

TypeOfError ::= ENUMERATED {

not-understood,

missing,

...

}

-- U

UEAggregateMaximumBitRate ::= SEQUENCE {

dl-UE-AMBR BitRate,

ul-UE-AMBR BitRate,

iE-Extension ProtocolExtensionContainer { {UEAggregateMaximumBitRate-ExtIEs} } OPTIONAL,

...

}

UEAggregateMaximumBitRate-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

UEContextKeptIndicator ::= ENUMERATED {true, ...}

UEContextID ::= CHOICE {

rRCResume UEContextIDforRRCResume,

rRRCReestablishment UEContextIDforRRCReestablishment,

choice-extension ProtocolIE-Single-Container { {UEContextID-ExtIEs} }

}

UEContextID-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

UEContextIDforRRCResume ::= SEQUENCE {

i-rnti I-RNTI,

allocated-c-rnti C-RNTI,

accessPCI NG-RAN-CellPCI,

iE-Extension ProtocolExtensionContainer { {UEContextIDforRRCResume-ExtIEs} } OPTIONAL,

...

}

UEContextIDforRRCResume-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

UEContextIDforRRCReestablishment ::= SEQUENCE {

c-rnti C-RNTI,

failureCellPCI NG-RAN-CellPCI,

iE-Extension ProtocolExtensionContainer { {UEContextIDforRRCReestablishment-ExtIEs} } OPTIONAL,

...

}

UEContextIDforRRCReestablishment-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

UEContextInfoRetrUECtxtResp ::= SEQUENCE {

ng-c-UE-signalling-ref AMF-UE-NGAP-ID,

signalling-TNL-at-source CPTransportLayerInformation,

ueSecurityCapabilities UESecurityCapabilities,

securityInformation AS-SecurityInformation,

ue-AMBR UEAggregateMaximumBitRate,

pduSessionResourcesToBeSetup-List PDUSessionResourcesToBeSetup-List,

rrc-Context OCTET STRING,

mobilityRestrictionList MobilityRestrictionList OPTIONAL,

indexToRatFrequencySelectionPriority RFSP-Index OPTIONAL,

iE-Extension ProtocolExtensionContainer { {UEContextInfoRetrUECtxtResp-ExtIEs} } OPTIONAL,

...

}

UEContextInfoRetrUECtxtResp-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ ID id-FiveGCMobilityRestrictionListContainer CRITICALITY ignore EXTENSION FiveGCMobilityRestrictionListContainer PRESENCE optional }|

{ ID id-NRUESidelinkAggregateMaximumBitRate CRITICALITY ignore EXTENSION NRUESidelinkAggregateMaximumBitRate PRESENCE optional }|

{ ID id-LTEUESidelinkAggregateMaximumBitRate CRITICALITY ignore EXTENSION LTEUESidelinkAggregateMaximumBitRate PRESENCE optional }|

{ ID id-UERadioCapabilityID CRITICALITY reject EXTENSION UERadioCapabilityID PRESENCE optional }|

{ ID id-NoPDUSessionIndication CRITICALITY ignore EXTENSION NoPDUSessionIndication PRESENCE optional},

...

}

UEHistoryInformation ::= SEQUENCE (SIZE(1..maxnoofCellsinUEHistoryInfo)) OF LastVisitedCell-Item

UEHistoryInformationFromTheUE ::= CHOICE {

nR NRMobilityHistoryReport,

choice-extension ProtocolIE-Single-Container { {UEHistoryInformationFromTheUE-ExtIEs} }

}

UEHistoryInformationFromTheUE-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

UEIdentityIndexValue ::= CHOICE {

indexLength10 BIT STRING (SIZE(10)),

choice-extension ProtocolIE-Single-Container { {UEIdentityIndexValue-ExtIEs} }

}

UEIdentityIndexValue-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

UERadioCapabilityForPaging ::= SEQUENCE {

uERadioCapabilityForPagingOfNR UERadioCapabilityForPagingOfNR OPTIONAL,

uERadioCapabilityForPagingOfEUTRA UERadioCapabilityForPagingOfEUTRA OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {UERadioCapabilityForPaging-ExtIEs} } OPTIONAL,

...

}

UERadioCapabilityForPaging-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

UERadioCapabilityForPagingOfNR ::= OCTET STRING

UERadioCapabilityForPagingOfEUTRA ::= OCTET STRING

UERadioCapabilityID ::= OCTET STRING

UERANPagingIdentity ::= CHOICE {

i-RNTI-full BIT STRING ( SIZE (40)),

choice-extension ProtocolIE-Single-Container { {UERANPagingIdentity-ExtIEs} }

}

UERANPagingIdentity-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

UERLFReportContainer ::= CHOICE {

nR-UERLFReportContainer UERLFReportContainerNR,

lTE-UERLFReportContainer UERLFReportContainerLTE,

choice-Extension ProtocolIE-Single-Container { {UERLFReportContainer-ExtIEs} }

}

UERLFReportContainer-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

UERLFReportContainerLTE ::= OCTET STRING

-- This IE is a transparent container and shall be encoded as the *RLF-Report-r9* IE contained in the UEInformationResponse message (TS 36.331 [14])

UERLFReportContainerNR ::= OCTET STRING

-- This IE is a transparent container and shall be encoded as the *nr-RLF-Report-r*16 IE contained in the UEInformationResponse message (TS 38.331 [10])

UESecurityCapabilities ::= SEQUENCE {

nr-EncyptionAlgorithms BIT STRING {nea1-128(1),

nea2-128(2),

nea3-128(3)} (SIZE(16, ...)),

nr-IntegrityProtectionAlgorithms BIT STRING {nia1-128(1),

nia2-128(2),

nia3-128(3)} (SIZE(16, ...)),

e-utra-EncyptionAlgorithms BIT STRING {eea1-128(1),

eea2-128(2),

eea3-128(3)} (SIZE(16, ...)),

e-utra-IntegrityProtectionAlgorithms BIT STRING {eia1-128(1),

eia2-128(2),

eia3-128(3)} (SIZE(16, ...)),

iE-Extension ProtocolExtensionContainer { {UESecurityCapabilities-ExtIEs} } OPTIONAL,

...

}

UESecurityCapabilities-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

UESpecificDRX ::= ENUMERATED {

v32,

v64,

v128,

v256,

...

}

ULConfiguration::= SEQUENCE {

uL-PDCP UL-UE-Configuration,

iE-Extensions ProtocolExtensionContainer { {ULConfiguration-ExtIEs} } OPTIONAL,

...

}

ULConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

UL-UE-Configuration::= ENUMERATED {no-data, shared, only, ...}

ULF1Term-BHInfo ::= SEQUENCE {

ingressBAPRoutingID BAPRoutingID,

ingressBHRLCCHID BHRLCChannelID,

iE-Extensions ProtocolExtensionContainer { { ULF1Term-BHInfo-ExtIEs} } OPTIONAL,

...

}

ULF1Term-BHInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ULNonF1Term-BHInfo ::= SEQUENCE {

egressBAPRoutingID BAPRoutingID,

egressBHRLCCHID BHRLCChannelID,

nexthopBAPAddress BAPAddress,

iE-Extensions ProtocolExtensionContainer { { ULNonF1Term-BHInfo-ExtIEs} } OPTIONAL,

...

}

ULNonF1Term-BHInfo-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

ULForwarding ::= ENUMERATED {ul-forwarding-proposed, ...}

ULForwardingProposal ::= ENUMERATED {ul-forwarding-proposed, ...}

UL-GBR-PRB-usage::= INTEGER (0..100)

UL-non-GBR-PRB-usage::= INTEGER (0..100)

UL-Total-PRB-usage::= INTEGER (0..100)

UPTransportLayerInformation ::= CHOICE {

gtpTunnel GTPtunnelTransportLayerInformation,

choice-extension ProtocolIE-Single-Container { {UPTransportLayerInformation-ExtIEs} }

}

UPTransportLayerInformation-ExtIEs XNAP-PROTOCOL-IES ::= {

...

}

UPTransportParameters ::= SEQUENCE (SIZE(1..maxnoofSCellGroupsplus1)) OF UPTransportParametersItem

UPTransportParametersItem ::= SEQUENCE {

upTNLInfo UPTransportLayerInformation,

cellGroupID CellGroupID,

iE-Extension ProtocolExtensionContainer { {UPTransportParametersItem-ExtIEs} } OPTIONAL,

...

}

UPTransportParametersItem-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

{ID id-QoS-Mapping-Information CRITICALITY reject EXTENSION QoS-Mapping-Information PRESENCE optional},

...

}

UserPlaneTrafficActivityReport ::= ENUMERATED {inactive, re-activated, ...}

URIaddress ::= VisibleString

-- V

VehicleUE ::= ENUMERATED {

authorized,

not-authorized,

...

}

VolumeTimedReportList ::= SEQUENCE (SIZE(1..maxnooftimeperiods)) OF VolumeTimedReport-Item

VolumeTimedReport-Item ::= SEQUENCE {

startTimeStamp OCTET STRING (SIZE(4)),

endTimeStamp OCTET STRING (SIZE(4)),

usageCountUL INTEGER (0..18446744073709551615),

usageCountDL INTEGER (0..18446744073709551615),

iE-Extensions ProtocolExtensionContainer { {VolumeTimedReport-Item-ExtIEs} } OPTIONAL,

...

}

VolumeTimedReport-Item-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

-- W

WLANMeasurementConfiguration ::= SEQUENCE {

wlanMeasConfig WLANMeasConfig,

wlanMeasConfigNameList WLANMeasConfigNameList OPTIONAL,

wlan-rssi ENUMERATED {true, ...} OPTIONAL,

wlan-rtt ENUMERATED {true, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { WLANMeasurementConfiguration-ExtIEs } } OPTIONAL,

...

}

WLANMeasurementConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

WLANMeasConfigNameList ::= SEQUENCE (SIZE(1..maxnoofWLANName)) OF WLANName

WLANMeasConfig::= ENUMERATED {setup,...}

WLANName ::= OCTET STRING (SIZE (1..32))

-- X

XnBenefitValue ::= INTEGER (1..8, ...)

-- Y

-- Z

END

-- ASN1STOP

9.3.6 Common definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Common definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-CommonDataTypes {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-CommonDataTypes (3) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Extension constants

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxPrivateIEs INTEGER ::= 65535

maxProtocolExtensions INTEGER ::= 65535

maxProtocolIEs INTEGER ::= 65535

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Common Data Types

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Criticality ::= ENUMERATED { reject, ignore, notify }

Presence ::= ENUMERATED { optional, conditional, mandatory }

PrivateIE-ID ::= CHOICE {

local INTEGER (0.. maxPrivateIEs),

global OBJECT IDENTIFIER

}

ProcedureCode ::= INTEGER (0..255)

ProtocolIE-ID ::= INTEGER (0..maxProtocolIEs)

TriggeringMessage ::= ENUMERATED { initiating-message, successful-outcome, unsuccessful-outcome}

END

-- ASN1STOP

9.3.7 Constant definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) xnap (2) version1 (1) xnap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

ProcedureCode,

ProtocolIE-ID

FROM XnAP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-handoverPreparation ProcedureCode ::= 0

id-sNStatusTransfer ProcedureCode ::= 1

id-handoverCancel ProcedureCode ::= 2

id-retrieveUEContext ProcedureCode ::= 3

id-rANPaging ProcedureCode ::= 4

id-xnUAddressIndication ProcedureCode ::= 5

id-uEContextRelease ProcedureCode ::= 6

id-sNGRANnodeAdditionPreparation ProcedureCode ::= 7

id-sNGRANnodeReconfigurationCompletion ProcedureCode ::= 8

id-mNGRANnodeinitiatedSNGRANnodeModificationPreparation ProcedureCode ::= 9

id-sNGRANnodeinitiatedSNGRANnodeModificationPreparation ProcedureCode ::= 10

id-mNGRANnodeinitiatedSNGRANnodeRelease ProcedureCode ::= 11

id-sNGRANnodeinitiatedSNGRANnodeRelease ProcedureCode ::= 12

id-sNGRANnodeCounterCheck ProcedureCode ::= 13

id-sNGRANnodeChange ProcedureCode ::= 14

id-rRCTransfer ProcedureCode ::= 15

id-xnRemoval ProcedureCode ::= 16

id-xnSetup ProcedureCode ::= 17

id-nGRANnodeConfigurationUpdate ProcedureCode ::= 18

id-cellActivation ProcedureCode ::= 19

id-reset ProcedureCode ::= 20

id-errorIndication ProcedureCode ::= 21

id-privateMessage ProcedureCode ::= 22

id-notificationControl ProcedureCode ::= 23

id-activityNotification ProcedureCode ::= 24

id-e-UTRA-NR-CellResourceCoordination ProcedureCode ::= 25

id-secondaryRATDataUsageReport ProcedureCode ::= 26

id-deactivateTrace ProcedureCode ::= 27

id-traceStart ProcedureCode ::= 28

id-handoverSuccess ProcedureCode ::= 29

id-conditionalHandoverCancel ProcedureCode ::= 30

id-earlyStatusTransfer ProcedureCode ::= 31

id-failureIndication ProcedureCode ::= 32

id-handoverReport ProcedureCode ::= 33

id-resourceStatusReportingInitiation ProcedureCode ::= 34

id-resourceStatusReporting ProcedureCode ::= 35

id-mobilitySettingsChange ProcedureCode ::= 36

id-accessAndMobilityIndication ProcedureCode ::= 37

id-f1CTrafficTransfer ProcedureCode ::= xx

id-iABTransportMigrationManagement ProcedureCode ::= xx

id-iABTransportMigrationModification ProcedureCode ::= xx

id-iABResourceCoordination ProcedureCode ::= xx

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxEARFCN INTEGER ::= 262143

maxnoofAllowedAreas INTEGER ::= 16

maxnoofAMFRegions INTEGER ::= 16

maxnoofAoIs INTEGER ::= 64

maxnoofBluetoothName INTEGER ::= 4

maxnoofBPLMNs INTEGER ::= 12

maxnoofCAGs INTEGER ::= 12

maxnoofCAGsperPLMN INTEGER ::= 256

maxnoofCellIDforMDT INTEGER ::= 32

maxnoofCellsinAoI INTEGER ::= 256

maxnoofCellsinUEHistoryInfo INTEGER ::= 16

maxnoofCellsinNG-RANnode INTEGER ::= 16384

maxnoofCellsinRNA INTEGER ::= 32

maxnoofCellsUEMovingTrajectory INTEGER ::= 16

maxnoofDRBs INTEGER ::= 32

maxnoofEUTRABands INTEGER ::= 16

maxnoofEUTRABPLMNs INTEGER ::= 6

maxnoofEPLMNs INTEGER ::= 15

maxnoofExtSliceItems INTEGER ::= 65535

maxnoofEPLMNsplus1 INTEGER ::= 16

maxnoofForbiddenTACs INTEGER ::= 4096

maxnoofFreqforMDT INTEGER ::= 8

maxnoofMBSFNEUTRA INTEGER ::= 8

maxnoofMDTPLMNs INTEGER ::= 16

maxnoofMultiConnectivityMinusOne INTEGER ::= 3

maxnoofNeighbours INTEGER ::= 1024

maxnoofNeighPCIforMDT INTEGER ::= 32

maxnoofNIDs INTEGER ::= 12

maxnoofNRCellBands INTEGER ::= 32

maxnoofPLMNs INTEGER ::= 16

maxnoofPDUSessions INTEGER ::= 256

maxnoofProtectedResourcePatterns INTEGER ::= 16

maxnoofQoSFlows INTEGER ::= 64

maxnoofQoSParaSets INTEGER ::= 8

maxnoofRANAreaCodes INTEGER ::= 32

maxnoofRANAreasinRNA INTEGER ::= 16

maxnoofRANNodesinAoI INTEGER ::= 64

maxnoofSCellGroups INTEGER ::= 3

maxnoofSCellGroupsplus1 INTEGER ::= 4

maxnoofSensorName INTEGER ::= 3

maxnoofSliceItems INTEGER ::= 1024

maxnoofSNPNIDs INTEGER ::= 12

maxnoofsupportedPLMNs INTEGER ::= 12

maxnoofsupportedTACs INTEGER ::= 256

maxnoofTAforMDT INTEGER ::= 8

maxnoofTAI INTEGER ::= 16

maxnoofTAIsinAoI INTEGER ::= 16

maxnooftimeperiods INTEGER ::= 2

maxnoofTNLAssociations INTEGER ::= 32

maxnoofUEContexts INTEGER ::= 8192

maxNRARFCN INTEGER ::= 3279165

maxNrOfErrors INTEGER ::= 256

maxnoofslots INTEGER ::= 5120

maxnoofExtTLAs INTEGER ::= 16

maxnoofGTPTLAs INTEGER ::= 16

maxnoofCHOcells INTEGER ::= 8

maxnoofPC5QoSFlows INTEGER ::= 2064

maxnoofSSBAreas INTEGER ::= 64

maxnoofRACHReports INTEGER ::= 64

maxnoofNRSCSs INTEGER ::= 5

maxnoofPhysicalResourceBlocks INTEGER ::= 275

maxnoofAdditionalPDCPDuplicationTNL INTEGER ::= 2

maxnoofRLCDuplicationstate INTEGER ::= 3

maxnoofWLANName INTEGER ::= 4

maxnoofNonAnchorCarrierFreqConfig INTEGER ::= 15

maxnoofDataForwardingTunneltoE-UTRAN INTEGER ::= 256

maxnoofServedCellsIAB INTEGER ::= 512

maxnoofServingCells INTEGER ::= 32

maxnoofBHInfo INTEGER ::= 1024

maxnoofTrafficIndexEntries INTEGER ::= 1024

maxnoofTLAsIAB INTEGER ::= 1024

maxnoofBAPControlPDURLCCHs INTEGER ::= 2

maxnoofIABSTCInfo INTEGER ::= 45

maxnoofSymbols INTEGER ::= 14

maxnoofDUFSlots INTEGER ::= 320

maxnoofHSNASlots INTEGER ::= 5120

maxnoofRBsetsPerCell INTEGER ::= 8

maxnoofChildIABNodes INTEGER ::=1024

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-ActivatedServedCells ProtocolIE-ID ::= 0

id-ActivationIDforCellActivation ProtocolIE-ID ::= 1

id-admittedSplitSRB ProtocolIE-ID ::= 2

id-admittedSplitSRBrelease ProtocolIE-ID ::= 3

id-AMF-Region-Information ProtocolIE-ID ::= 4

id-AssistanceDataForRANPaging ProtocolIE-ID ::= 5

id-BearersSubjectToCounterCheck ProtocolIE-ID ::= 6

id-Cause ProtocolIE-ID ::= 7

id-cellAssistanceInfo-NR ProtocolIE-ID ::= 8

id-ConfigurationUpdateInitiatingNodeChoice ProtocolIE-ID ::= 9

id-CriticalityDiagnostics ProtocolIE-ID ::= 10

id-XnUAddressInfoperPDUSession-List ProtocolIE-ID ::= 11

id-DRBsSubjectToStatusTransfer-List ProtocolIE-ID ::= 12

id-ExpectedUEBehaviour ProtocolIE-ID ::= 13

id-GlobalNG-RAN-node-ID ProtocolIE-ID ::= 14

id-GUAMI ProtocolIE-ID ::= 15

id-indexToRatFrequSelectionPriority ProtocolIE-ID ::= 16

id-initiatingNodeType-ResourceCoordRequest ProtocolIE-ID ::= 17

id-List-of-served-cells-E-UTRA ProtocolIE-ID ::= 18

id-List-of-served-cells-NR ProtocolIE-ID ::= 19

id-LocationReportingInformation ProtocolIE-ID ::= 20

id-MAC-I ProtocolIE-ID ::= 21

id-MaskedIMEISV ProtocolIE-ID ::= 22

id-M-NG-RANnodeUEXnAPID ProtocolIE-ID ::= 23

id-MN-to-SN-Container ProtocolIE-ID ::= 24

id-MobilityRestrictionList ProtocolIE-ID ::= 25

id-new-NG-RAN-Cell-Identity ProtocolIE-ID ::= 26

id-newNG-RANnodeUEXnAPID ProtocolIE-ID ::= 27

id-UEReportRRCTransfer ProtocolIE-ID ::= 28

id-oldNG-RANnodeUEXnAPID ProtocolIE-ID ::= 29

id-OldtoNewNG-RANnodeResumeContainer ProtocolIE-ID ::= 30

id-PagingDRX ProtocolIE-ID ::= 31

id-PCellID ProtocolIE-ID ::= 32

id-PDCPChangeIndication ProtocolIE-ID ::= 33

id-PDUSessionAdmittedAddedAddReqAck ProtocolIE-ID ::= 34

id-PDUSessionAdmittedModSNModConfirm ProtocolIE-ID ::= 35

id-PDUSessionAdmitted-SNModResponse ProtocolIE-ID ::= 36

id-PDUSessionNotAdmittedAddReqAck ProtocolIE-ID ::= 37

id-PDUSessionNotAdmitted-SNModResponse ProtocolIE-ID ::= 38

id-PDUSessionReleasedList-RelConf ProtocolIE-ID ::= 39

id-PDUSessionReleasedSNModConfirm ProtocolIE-ID ::= 40

id-PDUSessionResourcesActivityNotifyList ProtocolIE-ID ::= 41

id-PDUSessionResourcesAdmitted-List ProtocolIE-ID ::= 42

id-PDUSessionResourcesNotAdmitted-List ProtocolIE-ID ::= 43

id-PDUSessionResourcesNotifyList ProtocolIE-ID ::= 44

id-PDUSession-SNChangeConfirm-List ProtocolIE-ID ::= 45

id-PDUSession-SNChangeRequired-List ProtocolIE-ID ::= 46

id-PDUSessionToBeAddedAddReq ProtocolIE-ID ::= 47

id-PDUSessionToBeModifiedSNModRequired ProtocolIE-ID ::= 48

id-PDUSessionToBeReleasedList-RelRqd ProtocolIE-ID ::= 49

id-PDUSessionToBeReleased-RelReq ProtocolIE-ID ::= 50

id-PDUSessionToBeReleasedSNModRequired ProtocolIE-ID ::= 51

id-RANPagingArea ProtocolIE-ID ::= 52

id-PagingPriority ProtocolIE-ID ::= 53

id-requestedSplitSRB ProtocolIE-ID ::= 54

id-requestedSplitSRBrelease ProtocolIE-ID ::= 55

id-ResetRequestTypeInfo ProtocolIE-ID ::= 56

id-ResetResponseTypeInfo ProtocolIE-ID ::= 57

id-RespondingNodeTypeConfigUpdateAck ProtocolIE-ID ::= 58

id-respondingNodeType-ResourceCoordResponse ProtocolIE-ID ::= 59

id-ResponseInfo-ReconfCompl ProtocolIE-ID ::= 60

id-RRCConfigIndication ProtocolIE-ID ::= 61

id-RRCResumeCause ProtocolIE-ID ::= 62

id-SCGConfigurationQuery ProtocolIE-ID ::= 63

id-selectedPLMN ProtocolIE-ID ::= 64

id-ServedCellsToActivate ProtocolIE-ID ::= 65

id-servedCellsToUpdate-E-UTRA ProtocolIE-ID ::= 66

id-ServedCellsToUpdateInitiatingNodeChoice ProtocolIE-ID ::= 67

id-servedCellsToUpdate-NR ProtocolIE-ID ::= 68

id-s-ng-RANnode-SecurityKey ProtocolIE-ID ::= 69

id-S-NG-RANnodeUE-AMBR ProtocolIE-ID ::= 70

id-S-NG-RANnodeUEXnAPID ProtocolIE-ID ::= 71

id-SN-to-MN-Container ProtocolIE-ID ::= 72

id-sourceNG-RANnodeUEXnAPID ProtocolIE-ID ::= 73

id-SplitSRB-RRCTransfer ProtocolIE-ID ::= 74

id-TAISupport-list ProtocolIE-ID ::= 75

id-TimeToWait ProtocolIE-ID ::= 76

id-Target2SourceNG-RANnodeTranspContainer ProtocolIE-ID ::= 77

id-targetCellGlobalID ProtocolIE-ID ::= 78

id-targetNG-RANnodeUEXnAPID ProtocolIE-ID ::= 79

id-target-S-NG-RANnodeID ProtocolIE-ID ::= 80

id-TraceActivation ProtocolIE-ID ::= 81

id-UEContextID ProtocolIE-ID ::= 82

id-UEContextInfoHORequest ProtocolIE-ID ::= 83

id-UEContextInfoRetrUECtxtResp ProtocolIE-ID ::= 84

id-UEContextInfo-SNModRequest ProtocolIE-ID ::= 85

id-UEContextKeptIndicator ProtocolIE-ID ::= 86

id-UEContextRefAtSN-HORequest ProtocolIE-ID ::= 87

id-UEHistoryInformation ProtocolIE-ID ::= 88

id-UEIdentityIndexValue ProtocolIE-ID ::= 89

id-UERANPagingIdentity ProtocolIE-ID ::= 90

id-UESecurityCapabilities ProtocolIE-ID ::= 91

id-UserPlaneTrafficActivityReport ProtocolIE-ID ::= 92

id-XnRemovalThreshold ProtocolIE-ID ::= 93

id-DesiredActNotificationLevel ProtocolIE-ID ::= 94

id-AvailableDRBIDs ProtocolIE-ID ::= 95

id-AdditionalDRBIDs ProtocolIE-ID ::= 96

id-SpareDRBIDs ProtocolIE-ID ::= 97

id-RequiredNumberOfDRBIDs ProtocolIE-ID ::= 98

id-TNLA-To-Add-List ProtocolIE-ID ::= 99

id-TNLA-To-Update-List ProtocolIE-ID ::= 100

id-TNLA-To-Remove-List ProtocolIE-ID ::= 101

id-TNLA-Setup-List ProtocolIE-ID ::= 102

id-TNLA-Failed-To-Setup-List ProtocolIE-ID ::= 103

id-PDUSessionToBeReleased-RelReqAck ProtocolIE-ID ::= 104

id-S-NG-RANnodeMaxIPDataRate-UL ProtocolIE-ID ::= 105

id-PDUSessionResourceSecondaryRATUsageList ProtocolIE-ID ::= 107

id-Additional-UL-NG-U-TNLatUPF-List ProtocolIE-ID ::= 108

id-SecondarydataForwardingInfoFromTarget-List ProtocolIE-ID ::= 109

id-LocationInformationSNReporting ProtocolIE-ID ::= 110

id-LocationInformationSN ProtocolIE-ID ::= 111

id-LastE-UTRANPLMNIdentity ProtocolIE-ID ::= 112

id-S-NG-RANnodeMaxIPDataRate-DL ProtocolIE-ID ::= 113

id-MaxIPrate-DL ProtocolIE-ID ::= 114

id-SecurityResult ProtocolIE-ID ::= 115

id-S-NSSAI ProtocolIE-ID ::= 116

id-MR-DC-ResourceCoordinationInfo ProtocolIE-ID ::= 117

id-AMF-Region-Information-To-Add ProtocolIE-ID ::= 118

id-AMF-Region-Information-To-Delete ProtocolIE-ID ::= 119

id-OldQoSFlowMap-ULendmarkerexpected ProtocolIE-ID ::= 120

id-RANPagingFailure ProtocolIE-ID ::= 121

id-UERadioCapabilityForPaging ProtocolIE-ID ::= 122

id-PDUSessionDataForwarding-SNModResponse ProtocolIE-ID ::= 123

id-DRBsNotAdmittedSetupModifyList ProtocolIE-ID ::= 124

id-Secondary-MN-Xn-U-TNLInfoatM ProtocolIE-ID ::= 125

id-NE-DC-TDM-Pattern ProtocolIE-ID ::= 126

id-PDUSessionCommonNetworkInstance ProtocolIE-ID ::= 127

id-BPLMN-ID-Info-EUTRA ProtocolIE-ID ::= 128

id-BPLMN-ID-Info-NR ProtocolIE-ID ::= 129

id-InterfaceInstanceIndication ProtocolIE-ID ::= 130

id-S-NG-RANnode-Addition-Trigger-Ind ProtocolIE-ID ::= 131

id-DefaultDRB-Allowed ProtocolIE-ID ::= 132

id-DRB-IDs-takenintouse ProtocolIE-ID ::= 133

id-SplitSessionIndicator ProtocolIE-ID ::= 134

id-CNTypeRestrictionsForEquivalent ProtocolIE-ID ::= 135

id-CNTypeRestrictionsForServing ProtocolIE-ID ::= 136

id-DRBs-transferred-to-MN ProtocolIE-ID ::= 137

id-ULForwardingProposal ProtocolIE-ID ::= 138

id-EndpointIPAddressAndPort ProtocolIE-ID ::= 139

id-IntendedTDD-DL-ULConfiguration-NR ProtocolIE-ID ::= 140

id-TNLConfigurationInfo ProtocolIE-ID ::= 141

id-PartialListIndicator-NR ProtocolIE-ID ::= 142

id-MessageOversizeNotification ProtocolIE-ID ::= 143

id-CellAndCapacityAssistanceInfo-NR ProtocolIE-ID ::= 144

id-NG-RANTraceID ProtocolIE-ID ::= 145

id-NonGBRResources-Offered ProtocolIE-ID ::= 146

id-FastMCGRecoveryRRCTransfer-SN-to-MN ProtocolIE-ID ::= 147

id-RequestedFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 148

id-AvailableFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 149

id-RequestedFastMCGRecoveryViaSRB3Release ProtocolIE-ID ::= 150

id-ReleaseFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 151

id-FastMCGRecoveryRRCTransfer-MN-to-SN ProtocolIE-ID ::= 152

id-ExtendedRATRestrictionInformation ProtocolIE-ID ::= 153

id-QoSMonitoringRequest ProtocolIE-ID ::= 154

id-FiveGCMobilityRestrictionListContainer ProtocolIE-ID ::= 155

id-PartialListIndicator-EUTRA ProtocolIE-ID ::= 156

id-CellAndCapacityAssistanceInfo-EUTRA ProtocolIE-ID ::= 157

id-CHOinformation-Req ProtocolIE-ID ::= 158

id-CHOinformation-Ack ProtocolIE-ID ::= 159

id-targetCellsToCancel ProtocolIE-ID ::= 160

id-requestedTargetCellGlobalID ProtocolIE-ID ::= 161

id-procedureStage ProtocolIE-ID ::= 162

id-DAPSRequestInfo ProtocolIE-ID ::= 163

id-DAPSResponseInfo-List ProtocolIE-ID ::= 164

id-CHO-MRDC-Indicator ProtocolIE-ID ::= 165

id-OffsetOfNbiotChannelNumberToDL-EARFCN ProtocolIE-ID ::= 166

id-OffsetOfNbiotChannelNumberToUL-EARFCN ProtocolIE-ID ::= 167

id-NBIoT-UL-DL-AlignmentOffset ProtocolIE-ID ::= 168

id-LTEV2XServicesAuthorized ProtocolIE-ID ::= 169

id-NRV2XServicesAuthorized ProtocolIE-ID ::= 170

id-LTEUESidelinkAggregateMaximumBitRate ProtocolIE-ID ::= 171

id-NRUESidelinkAggregateMaximumBitRate ProtocolIE-ID ::= 172

id-PC5QoSParameters ProtocolIE-ID ::= 173

id-AlternativeQoSParaSetList ProtocolIE-ID ::= 174

id-CurrentQoSParaSetIndex ProtocolIE-ID ::= 175

id-MobilityInformation ProtocolIE-ID ::= 176

id-InitiatingCondition-FailureIndication ProtocolIE-ID ::= 177

id-UEHistoryInformationFromTheUE ProtocolIE-ID ::= 178

id-HandoverReportType ProtocolIE-ID ::= 179

id-HandoverCause ProtocolIE-ID ::= 180

id-SourceCellCGI ProtocolIE-ID ::= 181

id-TargetCellCGI ProtocolIE-ID ::= 182

id-ReEstablishmentCellCGI ProtocolIE-ID ::= 183

id-TargetCellinEUTRAN ProtocolIE-ID ::= 184

id-SourceCellCRNTI ProtocolIE-ID ::= 185

id-UERLFReportContainer ProtocolIE-ID ::= 186

id-NGRAN-Node1-Measurement-ID ProtocolIE-ID ::= 187

id-NGRAN-Node2-Measurement-ID ProtocolIE-ID ::= 188

id-RegistrationRequest ProtocolIE-ID ::= 189

id-ReportCharacteristics ProtocolIE-ID ::= 190

id-CellToReport ProtocolIE-ID ::= 191

id-ReportingPeriodicity ProtocolIE-ID ::= 192

id-CellMeasurementResult ProtocolIE-ID ::= 193

id-NG-RANnode1CellID ProtocolIE-ID ::= 194

id-NG-RANnode2CellID ProtocolIE-ID ::= 195

id-NG-RANnode1MobilityParameters ProtocolIE-ID ::= 196

id-NG-RANnode2ProposedMobilityParameters ProtocolIE-ID ::= 197

id-MobilityParametersModificationRange ProtocolIE-ID ::= 198

id-TDDULDLConfigurationCommonNR ProtocolIE-ID ::= 199

id-CarrierList ProtocolIE-ID ::= 200

id-ULCarrierList ProtocolIE-ID ::= 201

id-FrequencyShift7p5khz ProtocolIE-ID ::= 202

id-SSB-PositionsInBurst ProtocolIE-ID ::= 203

id-NRCellPRACHConfig ProtocolIE-ID ::= 204

id-RACHReportInformation ProtocolIE-ID ::= 205

id-IABNodeIndication ProtocolIE-ID ::= 206

id-Redundant-UL-NG-U-TNLatUPF ProtocolIE-ID ::= 207

id-CNPacketDelayBudgetDownlink ProtocolIE-ID ::= 208

id-CNPacketDelayBudgetUplink ProtocolIE-ID ::= 209

id-Additional-Redundant-UL-NG-U-TNLatUPF-List ProtocolIE-ID ::= 210

id-RedundantCommonNetworkInstance ProtocolIE-ID ::= 211

id-TSCTrafficCharacteristics ProtocolIE-ID ::= 212

id-RedundantQoSFlowIndicator ProtocolIE-ID ::= 213

id-Redundant-DL-NG-U-TNLatNG-RAN ProtocolIE-ID ::= 214

id-ExtendedPacketDelayBudget ProtocolIE-ID ::= 215

id-Additional-PDCP-Duplication-TNL-List ProtocolIE-ID ::= 216

id-RedundantPDUSessionInformation ProtocolIE-ID ::= 217

id-UsedRSNInformation ProtocolIE-ID ::= 218

id-RLCDuplicationInformation ProtocolIE-ID ::= 219

id-NPN-Broadcast-Information ProtocolIE-ID ::= 220

id-NPNPagingAssistanceInformation ProtocolIE-ID ::= 221

id-NPNMobilityInformation ProtocolIE-ID ::= 222

id-NPN-Support ProtocolIE-ID ::= 223

id-MDT-Configuration ProtocolIE-ID ::= 224

id-MDTPLMNList ProtocolIE-ID ::= 225

id-TraceCollectionEntityURI ProtocolIE-ID ::= 226

id-UERadioCapabilityID ProtocolIE-ID ::= 227

id-CSI-RSTransmissionIndication ProtocolIE-ID ::= 228

id-SNTriggered ProtocolIE-ID ::= 229

id-DLCarrierList ProtocolIE-ID ::= 230

id-ExtendedTAISliceSupportList ProtocolIE-ID ::= 231

id-cellAssistanceInfo-EUTRA ProtocolIE-ID ::= 232

id-ConfiguredTACIndication ProtocolIE-ID ::= 233

id-secondary-SN-UL-PDCP-UP-TNLInfo ProtocolIE-ID ::= 234

id-pdcpDuplicationConfiguration ProtocolIE-ID ::= 235

id-duplicationActivation ProtocolIE-ID ::= 236

id-NPRACHConfiguration ProtocolIE-ID ::= 237

id-QosMonitoringReportingFrequency ProtocolIE-ID ::= 238

id-QoSFlowsMappedtoDRB-SetupResponse-MNterminated ProtocolIE-ID ::= 239

id-DL-scheduling-PDCCH-CCE-usage ProtocolIE-ID ::= 240

id-UL-scheduling-PDCCH-CCE-usage ProtocolIE-ID ::= 241

id-SFN-Offset ProtocolIE-ID ::= 242

id-QoSMonitoringDisabled ProtocolIE-ID ::= 243

id-ExtendedUEIdentityIndexValue ProtocolIE-ID ::= 244

id-PagingeDRXInformation ProtocolIE-ID ::= 245

id-CHO-MRDC-EarlyDataForwarding ProtocolIE-ID ::= 246

id-SCGIndicator ProtocolIE-ID ::= 247

id-UESpecificDRX ProtocolIE-ID ::= 248

id-PDUSessionExpectedUEActivityBehaviour ProtocolIE-ID ::= 249

id-QoS-Mapping-Information ProtocolIE-ID ::= 250

id-AdditionLocationInformation ProtocolIE-ID ::= 251

id-dataForwardingInfoFromTargetE-UTRANnode ProtocolIE-ID ::= 252

id-F1CTrafficContainer ProtocolIE-ID ::= xxx

id-Activated-Cells-List ProtocolIE-ID ::= xxx

id-IAB-MT-Cell-List ProtocolIE-ID ::= xxx

id-NoPDUSessionIndication ProtocolIE-ID ::= xxx

id-IAB-TNL-Address-Request ProtocolIE-ID ::= xxx

id-IAB-TNL-Address-Response ProtocolIE-ID ::= xxx

id-TrafficToBeAddedList ProtocolIE-ID ::= xxx

id-TrafficToBeModifiedList ProtocolIE-ID ::= xxx

id-TrafficToBeReleaseInformation ProtocolIE-ID ::= xxx

id-TrafficAddedList ProtocolIE-ID ::= xxx

id-TrafficModifiedList ProtocolIE-ID ::= xxx

id-TrafficNotAddedList ProtocolIE-ID ::= xxx

id-TrafficNotModifiedList ProtocolIE-ID ::= xxx

id-TrafficRequiredToBeModifiedList ProtocolIE-ID ::= xxx

id-TrafficRequiredModifiedList ProtocolIE-ID ::= xxx

id-TrafficReleasedList ProtocolIE-ID ::= xxx

id-IABTNLAddressToBeAdded ProtocolIE-ID ::= xxx

id-IABTNLAddressToBeReleasedList ProtocolIE-ID ::= xxx

id-nonF1-Terminating-DonorUEXnAPID ProtocolIE-ID ::= xxx

id-F1-Terminating-DonorUEXnAPID ProtocolIE-ID ::= xxx

id-BoundaryNodeCellsList ProtocolIE-ID ::= xxx

id-ParentNodeCellsList ProtocolIE-ID ::= xxx

id-tdd-GNB-DU-Cell-Resource-Configuration ProtocolIE-ID ::= xxx

id-UL-GNB-DU-Cell-Resource-Configuration ProtocolIE-ID ::= xxx

id-DL-GNB-DU-Cell-Resource-Configuration ProtocolIE-ID ::= xxx

id-permutation ProtocolIE-ID ::= xxx

id-IABTNLAddressException ProtocolIE-ID ::= xxx

END

-- ASN1STOP

9.3.8 Container definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-Containers {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-Containers (5) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

maxPrivateIEs,

maxProtocolExtensions,

maxProtocolIEs,

Criticality,

Presence,

PrivateIE-ID,

ProtocolIE-ID

FROM XnAP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XNAP-PROTOCOL-IES ::= CLASS {

&id ProtocolIE-ID UNIQUE,

&criticality Criticality,

&Value,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

TYPE &Value

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol IE pairs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XNAP-PROTOCOL-IES-PAIR ::= CLASS {

&id ProtocolIE-ID UNIQUE,

&firstCriticality Criticality,

&FirstValue,

&secondCriticality Criticality,

&SecondValue,

&presence Presence

}

WITH SYNTAX {

ID &id

FIRST CRITICALITY &firstCriticality

FIRST TYPE &FirstValue

SECOND CRITICALITY &secondCriticality

SECOND TYPE &SecondValue

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol Extensions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XNAP-PROTOCOL-EXTENSION ::= CLASS {

&id ProtocolIE-ID UNIQUE,

&criticality Criticality,

&Extension,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

EXTENSION &Extension

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Private IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XNAP-PRIVATE-IES ::= CLASS {

&id PrivateIE-ID,

&criticality Criticality,

&Value,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

TYPE &Value

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-Container {XNAP-PROTOCOL-IES : IEsSetParam} ::=

SEQUENCE (SIZE (0..maxProtocolIEs)) OF

ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-Single-Container {XNAP-PROTOCOL-IES : IEsSetParam} ::= ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-Field {XNAP-PROTOCOL-IES : IEsSetParam} ::= SEQUENCE {

id XNAP-PROTOCOL-IES.&id ({IEsSetParam}),

criticality XNAP-PROTOCOL-IES.&criticality ({IEsSetParam}{@id}),

value XNAP-PROTOCOL-IES.&Value ({IEsSetParam}{@id})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol IE Pairs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-ContainerPair {XNAP-PROTOCOL-IES-PAIR : IEsSetParam} ::=

SEQUENCE (SIZE (0..maxProtocolIEs)) OF

ProtocolIE-FieldPair {{IEsSetParam}}

ProtocolIE-FieldPair {XNAP-PROTOCOL-IES-PAIR : IEsSetParam} ::= SEQUENCE {

id XNAP-PROTOCOL-IES-PAIR.&id ({IEsSetParam}),

firstCriticality XNAP-PROTOCOL-IES-PAIR.&firstCriticality ({IEsSetParam}{@id}),

firstValue XNAP-PROTOCOL-IES-PAIR.&FirstValue ({IEsSetParam}{@id}),

secondCriticality XNAP-PROTOCOL-IES-PAIR.&secondCriticality ({IEsSetParam}{@id}),

secondValue XNAP-PROTOCOL-IES-PAIR.&SecondValue ({IEsSetParam}{@id})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container Lists for Protocol IE Containers

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-ContainerList {INTEGER : lowerBound, INTEGER : upperBound, XNAP-PROTOCOL-IES : IEsSetParam} ::=

SEQUENCE (SIZE (lowerBound..upperBound)) OF

ProtocolIE-Container {{IEsSetParam}}

ProtocolIE-ContainerPairList {INTEGER : lowerBound, INTEGER : upperBound, XNAP-PROTOCOL-IES-PAIR : IEsSetParam} ::=

SEQUENCE (SIZE (lowerBound..upperBound)) OF

ProtocolIE-ContainerPair {{IEsSetParam}}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol Extensions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolExtensionContainer {XNAP-PROTOCOL-EXTENSION : ExtensionSetParam} ::= SEQUENCE (SIZE (1..maxProtocolExtensions)) OF

ProtocolExtensionField {{ExtensionSetParam}}

ProtocolExtensionField {XNAP-PROTOCOL-EXTENSION : ExtensionSetParam} ::= SEQUENCE {

id XNAP-PROTOCOL-EXTENSION.&id ({ExtensionSetParam}),

criticality XNAP-PROTOCOL-EXTENSION.&criticality ({ExtensionSetParam}{@id}),

extensionValue XNAP-PROTOCOL-EXTENSION.&Extension ({ExtensionSetParam}{@id})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Private IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PrivateIE-Container {XNAP-PRIVATE-IES : IEsSetParam} ::=

SEQUENCE (SIZE (1..maxPrivateIEs)) OF

PrivateIE-Field {{IEsSetParam}}

PrivateIE-Field {XNAP-PRIVATE-IES : IEsSetParam} ::= SEQUENCE {

id XNAP-PRIVATE-IES.&id ({IEsSetParam}),

criticality XNAP-PRIVATE-IES.&criticality ({IEsSetParam}{@id}),

value XNAP-PRIVATE-IES.&Value ({IEsSetParam}{@id})

}

END

-- ASN1STOP