**3GPP TSG-RAN WG3 Meeting #123 *R3-240308***

**Athens, GR, 26 Feb – 01 Mar, 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.473** | **CR** | **1292** | **rev** |  | **Current version:** | **18.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction of timing synchronisation status reporting procedure | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, Nokia, Nokia Shanghai Bell, ZTE | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TRS\_URLLC-NR-Core | | | | |  | ***Date:*** | | | 2024-02-19 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The Timing Synchronisation Status Reporting procedure is introduced to enable the gNB-CU to request the gNB-DU to start or stop reporting of RAN timing synchronisation status information.  The Transaction ID is needed for the non-UE associated signalling as per the section 10 (copied below), in case of any abstract syntax error, or the logical error.  Clause 10 of TS 38.413 [3] is applicable for the purposes of the present document, with the following additions for non-UE-associated procedures:  - In case of Abstract Syntax Error, when reporting the *Criticality Diagnostics* IE for not comprehended IE/IEgroups or missing IE/IE groups, the *Transaction ID* IE shall also be included;  - In case of Logical Error, when reporting the *Criticality Diagnostics* IE, the *Transaction ID* IE shall also be included; | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * Add the Transaction ID in the timing synchronisation status reporting messages. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not follow the general rule of Clause 10 for non-UE-associated procedure. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 9.2.17.1, 9.2.17.2, 9.2.17.3, 9.2.17.4, 9.4.4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specification | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **Change Begins** |

### 9.2.17 Timing Synchronisation Status Reporting Messages

#### 9.2.17.1 TIMING SYNCHRONISATION STATUS REQUEST

This message is sent by the gNB-CU to request the gNB-DU to start or stop reporting of RAN timing synchronization status information.

Direction: gNB-CU  gNB-DU

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| RAN TSS Request Type | M |  | ENUMERATED  (start, stop, …) |  | YES | reject |

#### 9.2.17.2 TIMING SYNCHRONISATION STATUS RESPONSE

This message is sent by the gNB-DU to confirm the request to start or stop reporting of RAN timing synchronization status information.

Direction: gNB-DU gNB-CU

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | ignore |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.17.3 TIMING SYNCHRONISATION STATUS FAILURE

This message is sent by the gNB-DU to indicate that reporting of RAN timing synchronisation status information cannot be initiated.

Direction: gNB-DU  gNB-CU

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | ignore |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | Ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.17.4 TIMING SYNCHRONISATION STATUS REPORT

This message is sent by the gNB-DU to report RAN timing synchronisation status information.

Direction: gNB-DU  gNB-CU

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | ignore |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| RAN Timing Synchronisation Status Information | M |  | 9.3.1.298 |  | YES | ignore |

<<<<<<<<<<<<<<<<<<<< Unmodified Text Omitted >>>>>>>>>>>>>>>>>>>>

### 9.4.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for F1AP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1AP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) f1ap (3) version1 (1) f1ap-PDU-Contents (1) }

<<<<<<<<<<<<<<<<<<<< Unmodified Text Omitted >>>>>>>>>>>>>>>>>>>>

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Timing Synchronisation Status Elementary Procedure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TIMING SYNCHRONISATION STATUS REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TimingSynchronisationStatusRequest::= SEQUENCE {

protocolIEs ProtocolIE-Container {{TimingSynchronisationStatusRequest-IEs}},

...

}

TimingSynchronisationStatusRequest-IEs F1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-RANTSSRequestType CRITICALITY reject TYPE RANTSSRequestType PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TIMING SYNCHRONISATION STATUS RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TimingSynchronisationStatusResponse::= SEQUENCE {

protocolIEs ProtocolIE-Container {{TimingSynchronisationStatusResponse-IEs}},

...

}

TimingSynchronisationStatusResponse-IEs F1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TIMING SYNCHRONISATION STATUS FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TimingSynchronisationStatusFailure::= SEQUENCE {

protocolIEs ProtocolIE-Container {{TimingSynchronisationStatusFailure-IEs}},

...

}

TimingSynchronisationStatusFailure-IEs F1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Timing Synchronisation Status Reporting Elementary Procedure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TIMING SYNCHRONISATION STATUS REPORT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TimingSynchronisationStatusReport::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ TimingSynchronisationStatusReport-IEs}},

...

}

TimingSynchronisationStatusReport-IEs F1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-RANTimingSynchronisationStatusInfo CRITICALITY ignore TYPE RANTimingSynchronisationStatusInfo PRESENCE mandatory },

...

}

|  |
| --- |
| **Change Ends** |