**3GPP TSG-RAN WG3 Meeting #123R3-240822**

**Athens, Greece, 26th Feb – 1st Mar 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **-** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Introduction of new SPID value for 2RX XR UE [2Rx\_XR\_UE] |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, ZTE, Apple, Ericsson, Qualcomm, Deutsche Telekom, Vodafone, CATT, CMCC, China Telecom, Huawei |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | TEI18 |  | ***Date:*** | 2024-02-26 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)****S*** *(adding to the sourcing companies’ CR statistics)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | RAN#102 agreed the way forward to support 2Rx XR UE: - SPID indication from the Core Network to gNB. [RAN3]A new reference SPID value needs to be defined for 2Rx XR UE.  |
|  |  |
| ***Summary of change:*** | Introduces a new Reference SPID value for 2Rx XR UE. |
|  |  |
| ***Consequences if not approved:*** | Cannot support 2Rx XR UE. |
|  |  |
| ***Clauses affected:*** | Annex D |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.300 CR 00xx |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*Start of Change*

## 3.2 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1], in TS 36.300 [2] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1] and TS 36.300 [2].

**A2X communication**: A communication to support A2X services leveraging PC5 reference points. A2X services are realized by various types of A2X applications, i.e. BRID or DAA.

**Aerial UE communication:** functionality enabling Aerial UE function, as defined in 16.18.

**Air to Ground network:** An NG-RAN consisting of ground-based gNBs, which provide cell towers that send signals up to an aircraft’s antenna(s) of onboard ATG terminal, with typical vertical altitude of around 10,000m and take-off/landing altitudes down to 3000m.

**BH RLC channel**: an RLC channel between two nodes, which is used to transport backhaul packets**.**

**Boundary IAB-node:** as defined in TS 38.401 [4].

**Broadcast MRB**:A radio bearer configured for MBS broadcast delivery.

**CAG Cell**:a PLMN cell broadcasting at least one Closed Access Group identity.

**CAG Member Cell**:for a UE, a CAG cell broadcasting the identity of the selected PLMN, registered PLMN or equivalent PLMN, and for that PLMN, a CAG identifier belonging to the Allowed CAG list of the UE for that PLMN.

**CAG-only cell**: a CAG cell that is only available for normal service for CAG UEs.

**Cell-Defining SSB**: an SSB with an RMSI associated.

**Child node**: IAB-DU's and IAB-donor-DU's next hop neighbour node; the child node is also an IAB-node.

**Conditional Handover (CHO**): a handover procedure that is executed only when execution condition(s) are met.

**CORESET#0**: the control resource set for at least SIB1 scheduling, can be configured either via MIB or via dedicated RRC signalling.

**DAPS Handover**: a handover procedure that maintains the source gNB connection after reception of RRC message for handover and until releasing the source cell after successful random access to the target gNB.

**Data Burst:** A set of multiple PDUs generated and sent by the application in a short period of time, as defined in TS 23.501 [3].

**Direct Path**: a type of UE-to-Network transmission path, where data is transmitted between a UE and the network without sidelink relaying.

**Downstream**: direction toward child node or UE in IAB-topology.

**Early Data Forwarding**: data forwarding that is initiated before the UE executes the handover.

**Earth-centered, earth-fixed**: a global geodetic reference system for the Earth intended for practical applications of mapping, charting, geopositioning and navigation, as specified in NIMA TR 8350.2 [51].

**eRedCap UE**: a UE with enhanced reduced capabilities as specified in clause 4.2.22.1 in TS 38.306 [11].

**Feeder link**: wireless link between the NTN Gateway and the NTN payload.

**Geosynchronous Orbit**: earth-centered orbit at approximately 35786 kilometres above Earth's surface and synchronised with Earth's rotation. A geostationary orbit is a non-inclined geosynchronous orbit, i.e. in the Earth's equator plane.

**Group ID for Network Selection**: an identifier used during SNPN selection to enhance the likelihood of selecting a preferred SNPN that supports a Default Credentials Server or a Credentials Holder, as specified in TS 23.501 [3].

**gNB**: node providing NR user plane and control plane protocol terminations towards the UE, and connected via the NG interface to the 5GC.

**High Altitude Platform Station**: airborne vehicle embarking the NTN payload placed at an altitude between 8 and 50 km.

**IAB-donor**:gNB that provides network access to UEs via a network of backhaul and access links.

**IAB-donor-CU**: as defined in TS 38.401 [4].

**IAB-donor-DU**:as defined in TS 38.401 [4].

**IAB-DU**: gNB-DU functionality supported by the IAB-node to terminate the NR access interface to UEs and next-hop IAB-nodes, and to terminate the F1 protocol to the gNB-CU functionality, as defined in TS 38.401 [4], on the IAB-donor.

**IAB-MT**: IAB-node function that terminates the Uu interface to the parent node using the procedures and behaviours specified for UEs unless stated otherwise. IAB-MT function used in 38-series of 3GPP Specifications corresponds to IAB-UE function defined in TS 23.501 [3].

**IAB-node**: RAN node that supports NR access links to UEs and NR backhaul links to parent nodes and child nodes. The IAB-node does not support backhauling via LTE.

**IAB topology**: the unison of all IAB-nodes and IAB-donor-DUs whose F1 and/or RRC connections are terminated at the same IAB-donor-CU.

**Indirect Path**: a type of UE-to-Network transmission path, where data is forwarded via a U2N Relay UE between a U2N Remote UE and the network.

**Inter-donor partial migration:** migration of an IAB-MT to a parent node underneath a different IAB-donor-CU while the collocated IAB-DU and its descendant IAB-node(s), if any, are terminated at the initial IAB-donor-CU. The procedure renders the said IAB-node as a boundary IAB-node.

**Intra-system Handover**:handover that does not involve a CN change (EPC or 5GC).

**Inter-system Handover**:handover that involves a CN change (EPC or 5GC).

**Late Data Forwarding**: data forwarding that is initiated after the source NG-RAN node knows that the UE has successfully accessed a target NG-RAN node.

**L1/L2 Triggered Mobility**: a cell switch procedure that the network triggers via MAC CE based on L1 measurements.

**Mapped Cell ID**: in NTN, it corresponds to a fixed geographical area.

**MBS Radio Bearer**: A radio bearer configured for MBS delivery.

**Mobile-IAB cell**: a cell of a mobile IAB-DU.

**Mobile IAB-DU**: gNB-DU functionality supported by the mobile IAB-node to terminate the NR access interface to UEs, and to terminate the F1 protocol to the gNB-CU functionality on the IAB-donor, as defined in TS 38.401 [4].

**Mobile IAB-DU migration**: procedure for a mobile IAB-node as defined in TS 38.401 [4].

**Mobile IAB-MT**: mobile IAB-node function that terminates the Uu interface to the parent node using the procedures and behaviours specified for UEs unless stated otherwise.

**Mobile IAB-MT migration**: procedure for a mobile IAB-MT as defined in TS 38.401 [4].

**Mobile IAB-node**: RAN node that supports NR access links to UEs and an NR backhaul link to a parent node, and that can conduct physical mobility across the RAN area. The mobile IAB-node function used in 38-series of 3GPP Specifications corresponds to the MBSR function defined in TS 23.501 [3].

**MP Relay UE**: a UE that provides functionality to support connectivity to the network for MP Remote UE(s).

**MP Remote UE**: a UE that communicates with the network via a direct Uu link and a MP Relay UE.

**MSG1**: preamble transmission of the random access procedure for 4-step random access (RA) type.

**MSG3**: first scheduled transmission of the random access procedure.

**MSGA**:preamble and payload transmissions of the random access procedure for 2-step RA type.

**MSGB**:response to MSGA in the 2-step random access procedure. MSGB may consist of response(s) for contention resolution, fallback indication(s), and backoff indication.

**Multicast/Broadcast Service**: A point-to-multipoint service as defined in TS 23.247 [45].

**Multicast MRB**:A radio bearer configured for MBS multicast delivery.

**Multi-hop backhauling**: using a chain of NR backhaul links between an IAB-node and an IAB-donor.

**NCR-Fwd**: Network-Controlled Repeater node function, which performs amplifying-and-forwarding of UL/DL RF signals between gNB and UE. The behaviour of the NCR-Fwd is controlled according to the side control information received by the NCR-MT from a gNB.

**NCR-Fwd access link**: link used for transmissions between the NCR-Fwd and UEs.

**NCR-Fwd backhaul link**: link used for backhauling between the NCR-Fwd and gNB.

**NCR-MT**: NCR-node entity which communicates with a gNB via a control link to receive side control information. The control link is based on NR Uu interface.

**NCR-node**: RAN node comprising NCR-MT and NCR-Fwd.

**ng-eNB**: node providing E-UTRA user plane and control plane protocol terminations towards the UE, and connected via the NG interface to the 5GC.

**NG-C**: control plane interface between NG-RAN and 5GC.

**NG-U**: user plane interface between NG-RAN and 5GC.

**NG-RAN node**: either a gNB or an ng-eNB.

**Non-CAG Cell**: a PLMN cell which does not broadcast any Closed Access Group identity.

**Non-Cell Defining SSB**: an SSB without an RMSI associated.

**Non-Geosynchronous orbit**: earth-centered orbit with an orbital period that does not match Earth's rotation on its axis. This includes Low and Medium Earth Orbit (LEO and MEO). LEO operates at altitudes between 300 km and 1500 km and MEO at altitudes between 7000 km and 25000 km, approximately.

**Non-terrestrial network**: an NG-RAN consisting of gNBs, which provide non-terrestrial NR access to UEs by means of an NTN payload embarked on an airborne or space-borne NTN vehicle and an NTN Gateway.

**NR backhaul link**: NR link used for backhauling between an IAB-node and an IAB-donor, and between IAB-nodes in case of a multi-hop backhauling.

**NR sidelink communication**: AS functionality enabling at least V2X communication as defined in TS 23.287 [40] and the ProSe communication (including ProSe non-Relay and UE-to-Network Relay communication) as defined in TS 23.304 [48], between two or more nearby UEs, using NR technology but not traversing any network node.

**NR sidelink discovery**: AS functionality enabling ProSe non-Relay Discovery and ProSe UE-to-Network Relay discovery for Proximity based Services as defined in TS 23.304 [48] between two or more nearby UEs, using NR technology but not traversing any network node.

**NTN Gateway**: an earth station located at the surface of the earth, providing connectivity to the NTN payload using the feeder link. An NTN Gateway is a TNL node.

**NTN payload**: a network node, embarked on board a satellite or high altitude platform station, providing connectivity functions, between the service link and the feeder link. In the current version of this specification, the NTN payload is a TNL node.

**Numerology**: corresponds to one subcarrier spacing in the frequency domain. By scaling a reference subcarrier spacing by an integer *N*, different numerologies can be defined.

**Parent node**: IAB-MT's next hop neighbour node; the parent node can be IAB-node or IAB-donor-DU

**PC5 Relay RLC channel**: an RLC channel between L2 U2N Remote UE and L2 U2N Relay UE, or between L2 U2U Remote UE and L2 U2U Relay UE, which is used to transport packets over PC5 for L2 UE-to-Network/UE-to-UE Relay**.**

**PDU Set**: one or more PDUs carrying the payload of one unit of information generated at the application level (e.g. frame(s) or video slice(s) for XR Services), as defined in TS 23.501 [3].

**PLMN Cell**: a cell of the PLMN.

**RACH-less LTM**: an LTM cell switch procedure where UE skips the random access procedure.

**RedCap UE**: a UE with reduced capabilities as specified in clause 4.2.21.1 in TS 38.306 [11].

**Relay discovery**: AS functionality enabling 5G ProSe UE-to-Network Relay Discovery as defined in TS 23.304 [48], using NR technology but not traversing any network node.

**Satellite**:a space-borne vehicle orbiting the Earth embarking the NTN payload.

**Service link**:wireless link between the NTN payload and UE.

**Sidelink Discovery RSRP:** RSRP measurements on PC5 link related to NR sidelink discovery.

**Sidelink RSRP:** RSRP measurements on PC5 link related to NR sidelink communication.

**SNPN Access Mode**: mode of operation whereby a UE only accesses SNPNs.

**SNPN-only cell**: a cell that is only available for normal service for SNPN subscribers.

**SNPN Identity**: the identity of Stand-alone NPN defined by the pair (PLMN ID, NID).

**Subsequent LTM**: LTM cell switch procedures between candidate cells without RRC reconfiguration by the network in between.

**Transmit/Receive Point**:part of the gNB transmitting and receiving radio signals to/from UE according to physical layer properties and parameters inherent to that element.

**U2N Relay UE**: a UE that provides functionality to support connectivity to the network for U2N Remote UE(s).

**U2N Remote UE**: a UE that communicates with the network via a U2N Relay UE.

**U2U Relay UE**: a UE that provides functionality to support connectivity between two U2U Remote UEs.

**U2U Remote UE**: a UE that communicates with other UE(s) via a U2U Relay UE.

**Upstream**: direction toward parent node in IAB-topology.

**Uu Relay RLC channel**: an RLC channel between L2 U2N Relay UE and gNB, which is used to transport packets over Uu for L2 UE-to-Network Relay**.**

**V2X sidelink communication**: AS functionality enabling V2X communication as defined in TS 23.285 [41], between nearby UEs, using E-UTRA technology but not traversing any network node.

**Xn**: network interface between NG-RAN nodes.

**2Rx non-RedCap XR UE**: a non-RedCap UE used for XR applications with only 2Rx branches, as defined in TS 38.101-1 [18].

*NEXT CHANGE*

Annex D (informative):
SPID ranges and mapping of SPID values to cell reselection and inter-RAT/inter frequency handover priorities

The SPID, i.e. Index to RAT/Frequency Selection Priority as defined in TS23.501 [3], values are defined in Annex I of TS 36.300 [2].

From the SPID reference values defined in TS 36.300 [2], the SPID=253 also applies for 5GC.

The SPID=x defined below applies for 5GC.

SPID = x

Table I.x: gNB local configuration for SPID = X

|  |  |  |
| --- | --- | --- |
| Configuration parameter | Value | Meaning |
| 2Rx non-RedCap XR device subscriber | true | The selection provides information that subscriber is an XR device and is permitted to utilise a minimum of two Rx antenna ports for the NR bands where four Rx antenna ports are baseline as given in TS 38.101-1 [88]. |

*End of Change*