**3GPP TSG-RAN WG3 Meeting #123R3-241194**

**Athens, Greece, Feb 26 – Mar 1, 2024**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.413** | **CR** | **0991** | **rev** | **10** | **Current version:** |  **18.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | (BL CR to 38.413) Support of NR Positioning Enhancements |
|  |  |
| ***Source to WG:*** | ZTE, CATT, Huawei, Nokia, Nokia Shanghai Bell, Ericsson |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_pos\_enh2-Core |  | ***Date:*** | 2023-03-05 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The CR aims at introducing functionally support for Expanded and Improved NR Positioning. |
|  |  |
| ***Summary of change:*** | **RAN3#119bise:**- SL Positioning and Ranging service authorization information is signalled in the following messages:NG: - INITIAL CONTEXT SETUP REQUEST- UE CONTEXT MODIFICATION REQUEST- HANDOVER REQUEST- PATH SWITCH REQUEST ACKNOWLEDGE**RAN3#120 (Incheon)*** SLPP/RSPP Transport QoS parameters are introduced with authorization information

**RAN3#121bis (Xiamen)** - Add semantic description for the clarification of Ranging and Sidelink Positioning Service Information - New procedure LPHAP Information Transfer**RAN3#122 (Chicago)*** Add semantics descriptions i.e. “This IE applies only if the UE is authorized for NR V2X services and/or 5G ProSe services.” in the Ranging and Sidelink Positioning Service Information.

**RAN3#123 (Athens)*** Update the name of IEs, and editorial issue.
 |
|  |  |
| ***Consequences if not approved:*** |  Missing support of NR Positioning Enhancements |
|  |  |
| ***Clauses affected:*** | 3.2, 8.3.1, 8.3.4, 8.4.2, 8.4.4, 8.10.1, 9.2.2.1, 9.2.2.7, 9.2.3.4, 9.2.3.9, 9.3, 9.4.4, 9.4.5, 9.4.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS38.473 CR1180TS38.423 CR1058TS38.455 CR0113TS38.423 CR1061TS38.470 CR0122TS38.305 CR |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev1:Merge the agreed TP R3-233458 in the RAN3#120.Rev2:Re-submission.Rev3:Re-submission.Rev4:Update the cover pageRev5:Merge the agreed TPs in RAN3#121bis, R3-235792, R3-235815Rev6:Re-submission.Rev7:Merge the agreed TP in RAN3#122, R3-237387Rev8:Re-submission.Rev9:Update the meeting information. |

<<<<<<<<<<<<<<<<<<<< Changes Begin >>>>>>>>>>>>>>>>>>>>

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GC 5G Core Network

5QI 5G QoS Identifier

ACL Access Control List

AMF Access and Mobility Management Function

CAG Closed Access Group

CGI Cell Global Identifier

CP Control Plane

DAPS Dual Active Protocol Stacks

DC Dual Connectivity

DL Downlink

EPC Evolved Packet Core

FN-RG Fixed Network Residential Gateway

GUAMI Globally Unique AMF Identifier

HFC Hybrid Fiber-Coax

IAB Integrated Access and Backhaul

IMEISV International Mobile station Equipment Identity and Software Version number

LMF Location Management Function

MBS Multicast/Broadcast Service

N3IWF Non 3GPP InterWorking Function

NB-IoT Narrow Band Internet of Things

NID Network Identifier

NGAP NG Application Protocol

NPN Non-Public Network

NRPPa NR Positioning Protocol Annex

NSAG Network Slice AS Group

NSCI New Security Context Indicator

NSSAI Network Slice Selection Assistance Information

OTDOA Observed Time Difference of Arrival

PEIPS Paging Early Indication with Paging Subgrouping

PNI-NPN Public Network Integrated Non-Public Network

ProSe Proximity Services

PSCell Primary SCG Cell

PTP Point to Point

PTM Point to Multipoint

QMC QoE Measurement Collection

QoE Quality of Experience

RedCap Reduced Capability

RIM Remote Interference Management

RIM-RS RIM Reference Signal

RSN Redundancy Sequence Number

RSPP Ranging/SL Positioning Protocol

SCG Secondary Cell Group

SCTP Stream Control Transmission Protocol

SgNB Secondary gNB

SMF Session Management Function

S-NG-RAN node Secondary NG-RAN node

SNPN Stand-alone Non-Public Network

S-NSSAI Single Network Slice Selection Assistance Information

TAC Tracking Area Code

TAI Tracking Area Identity

TSS Timing Synchronisation Status

TNAP Trusted Non-3GPP Access Point

TNGF Trusted Non-3GPP Gateway Function

TNLA Transport Network Layer Association

TWAP Trusted WLAN Access Point

TWIF Trusted WLAN Interworking Function

UL Uplink

UP User Plane

UPF User Plane Function

V2X Vehicle-to-Everything

W-AGF Wireline Access Gateway Function

WUS Wake Up Signal

**<Unchanged Text Omitted>**

## 8.3 UE Context Management Procedures

### 8.3.1 Initial Context Setup

#### 8.3.1.1 General

The purpose of the Initial Context Setup procedure is to establish the necessary overall initial UE context at the NG-RAN node, when required, including PDU session context, the Security Key, Mobility Restriction List, UE Radio Capability and UE Security Capabilities, etc. The AMF may initiate the Initial Context Setup procedure if a UE-associated logical NG-connection exists for the UE or if the AMF has received the *RAN UE NGAP ID* IE in an INITIAL UE MESSAGE message or if the NG-RAN node has already initiated a UE-associated logical NG-connection by sending an INITIAL UE MESSAGE message via another NG interface instance. The procedure uses UE-associated signalling.

For signalling only connections and if the *UE Context Request* IE is not received in the Initial UE Message, the AMF may be configured to trigger the procedure for all NAS procedures or on a per NAS procedure basis depending on operator’s configuration.

#### 8.3.1.2 Successful Operation

Figure 8.3.1.2-1: Initial context setup: successful operation

In case of the establishment of a PDU session the 5GC shall be prepared to receive user data before the INITIAL CONTEXT SETUP RESPONSE message has been received by the AMF. If no UE-associated logical NG-connection exists, the UE-associated logical NG-connection shall be established at reception of the INITIAL CONTEXT SETUP REQUEST message.

The INITIAL CONTEXT SETUP REQUEST message shall contain the *Index to RAT/Frequency Selection Priority* IE, if available in the AMF.

If the *NAS-PDU* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall pass it transparently towards the UE.

If the *Masked IMEISV* IE is contained in the INITIAL CONTEXT SETUP REQUEST message the target NG-RAN node shall, if supported, use it to determine the characteristics of the UE for subsequent handling.

Upon receipt of the INITIAL CONTEXT SETUP REQUEST message the NG-RAN node shall

- attempt to execute the requested PDU session configuration;

- store the received UE Aggregate Maximum Bit Rate in the UE context, and use the received UE Aggregate Maximum Bit Rate for Non-GBR QoS flows for the concerned UE as specified in TS 23.501 [9];

- store the received Mobility Restriction List in the UE context;

- store the received UE Radio Capability in the UE context;

- store the received Index to RAT/Frequency Selection Priority in the UE context and use it as defined in TS 23.501 [9];

- store the received UE Security Capabilities in the UE context;

- store the received Security Key in the UE context and, if the NG-RAN node is required to activate security for the UE, take this security key into use;

- if supported, store the received SRVCC Operation Possible in the UE context and use it as defined in TS 23.216 [31];

- store the received NR V2X Services Authorization information, if supported, in the UE context;

- store the received LTE V2X Services Authorization information, if supported, in the UE context;

- store the received NR UE Sidelink Aggregate Maximum Bit Rate, if supported, in the UE context, and use it for the concerned UE’s sidelink communication in network scheduled mode for NR V2X services;

- store the received LTE UE Sidelink Aggregate Maximum Bit Rate, if supported, in the UE context, and use it for the concerned UE’s sidelink communication in network scheduled mode for LTE V2X services;

- store the received PC5 QoS Parameters, if supported, in the UE context and use it as defined in TS 23.287 [33];

- store the received Management Based MDT PLMN List information, if supported, in the UE context;

- if supported, store the received IAB Authorization information in the UE context, and use it accordingly for the IAB-MT;

- store the received 5G ProSe Authorization information in the UE context, if supported, and use it for the concerned UE’s sidelink communication in network scheduled mode for 5G ProSe services;

- store the 5G ProSe UE PC5 Aggregate Maximum Bit Rate in the UE context, if supported, and use it for the concerned UE’s sidelink communication in network scheduled mode for 5G ProSe services;

- store the 5G ProSe PC5 QoS Parameters, if supported, in the UE context and use it as defined in TS 23.304 [47];

- store the received Ranging and Sidelink Positioning service information, if supported, in the UE context;

- store the received Network Controlled Repeater Authorization, if supported, in the UE context;

- if supported, store the received Mobile IAB Authorization information in the UE context, and use it accordingly for the mobile IAB-MT;

- store the received PDU Set QoS parameters, if supported, in the UE context and use it as specified in TS 23.501 [9].

For the Initial Context Setup an initial value for the Next Hop Chaining Count is stored in the UE context.

If the *PDU Session Resource Setup Request List* IE is contained in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall behave the same as defined in the PDU Session Resource Setup procedure. The NG-RAN node shall report to the AMF in the INITIAL CONTEXT SETUP RESPONSE message the result for each PDU session resource requested to be setup as defined in the PDU Session Resource Setup procedure.

Upon reception of the INITIAL CONTEXT SETUP RESPONSE message the AMF shall, for each PDU session indicated in the *PDU Session ID* IE, transfer transparently the *PDU Session Resource Setup Response Transfer* IE or *PDU Session Resource Setup Unsuccessful Transfer* IE to the SMF associated with the concerned PDU session. In case the splitting PDU session is not used by the NG-RAN node, the SMF should remove the Additional Transport Layer Information, if any.

The NG-RAN node shall use the information in the *Mobility Restriction List* IE if present in the INITIAL CONTEXT SETUP REQUEST message to

- determine a target for subsequent mobility action for which the NG-RAN node provides information about the target of the mobility action towards the UE;

- select a proper SCG during dual connectivity operation;

- assign proper RNA(s) for the UE when moving the UE to RRC\_INACTIVE state.

If the *Mobility Restriction List* IE is not contained in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall consider that no roaming and no access restriction apply to the UE except for the PNI NPN mobility as described in TS 23.501 [9]. The NG-RAN node shall also consider that no roaming and no access restriction apply to the UE when:

- one of the QoS flows includes a particular ARP value (TS 23.501 [9]).

The NG-RAN node shall consider that roaming or access to CAG cells is only allowed if the *Allowed PNI-NPN List* IE is contained in the INITIAL CONTEXT SETUP REQUEST message, as described in TS 23.501 [9].

If the *Trace Activation* IE is included in the INITIAL CONTEXT SETUP REQUEST message the NG-RAN node shall, if supported, initiate the requested trace function as described in TS 32.422 [11]. In particular, the NG-RAN node shall, if supported:

- if the *Trace Activation* IE includes the *MDT Activation* IE set to "Immediate MDT and Trace", initiate the requested trace session and MDT session as described in TS 32.422 [11];

- if the *Trace Activation* IE includes the *MDT Activation* IE set to "Immediate MDT Only", "Logged MDT only", initiate the requested MDT session as described in TS 32.422 [11] and the NG-RAN node shall ignore the *Interfaces To Trace* IE and the *Trace Depth* IE;

- if the *Trace Activation* IE includes the *MDT Location Information* IE within the *MDT Configuration* IE, store this information and take it into account in the requested MDT session;

- if the *Trace Activation* IE includes the *Signalling Based MDT PLMN List* IE within the *MDT Configuration* IE, the NG-RAN node may use it to propagate the MDT Configuration as described in TS 37.320 [41].

- if the *Trace Activation* IE includes the *Bluetooth Measurement Configuration* IE within the *MDT Configuration* IE, take it into account for MDT Configuration as described in TS 37.320 [41].

- if the *Trace Activation* IE includes the *WLAN Measurement Configuration* IE within the *MDT Configuration* IE, take it into account for MDT Configuration as described in TS 37.320 [41].

- if the *Trace Activation* IE includes the *Sensor Measurement Configuration* IE within the *MDT Configuration* IE, take it into account for MDT Configuration as described in TS 37.320 [41].

- if the *Trace Activation* IE includes the *MDT Configuration* IE and if the NG-RAN node is a gNB at least the *MDT Configuration-NR* IE shall be present, while if the NG-RAN node is an ng-eNB at least the *MDT Configuration-EUTRA* IE shall be present.

If the *UE Security Capabilities* IE included in the INITIAL CONTEXT SETUP REQUEST message only contains the EIA0 or NIA0 algorithm as defined in TS 33.501 [13] and if the EIA0 or NIA0 algorithm is defined in the configured list of allowed integrity protection algorithms in the NG-RAN node (TS 33.501 [13]), the NG-RAN node shall take it into use and ignore the keys received in the *Security Key* IE.

If the *QMC Configuration Information* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, use it for QoE management, as described in TS 38.300 [8].

If the *Core Network Assistance Information* *for RRC INACTIVE* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context and use it for the RRC\_INACTIVE state decision and RNA configuration for the UE and RAN paging if any for a UE in RRC\_INACTIVE state, as specified in TS 38.300 [8]. If the *MICO All PLMN* IE is included in the *Core Network Assistance Information* *for RRC INACTIVE* IE the NG-RAN node shall, if supported, consider that the registration area for the UE is the full PLMN and ignore the *TAI List for RRC Inactive* IE. If the *Paging Cause Indication for Voice Service* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store and use it as specified in 38.300 [8]. If the *PEIPS Assistance Information* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store it and use it for paging subgrouping the UE in RRC\_INACTIVE state, as specified in TS 38.300 [8].

If the *CN Assisted RAN Parameters Tuning* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node may use it as described in TS 23.501 [9].

If the *RRC Inactive Transition Report Request* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context.

If the *Emergency Fallback Indicator* IE is included in the INITIAL CONTEXT SETUP REQUEST message, it indicates that the UE context to be set up is subject to emergency service fallback as described in TS 23.501 [9] and the NG-RAN node may, if supported, take the appropriate mobility actions.

If the *Old AMF* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall consider that this UE-associated logical NG-connection was redirected to this AMF from another AMF identified by the *Old AMF* IE.

If the *Redirection for Voice EPS Fallback* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, store it and use it in a subsequent decision of EPS fallback for voice as specified in TS 23.502 [10].

If the *Location Reporting Request Type* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node should perform the requested location reporting functionality for the UE as described in subclause 8.12.

If the *Enhanced Coverage Restriction* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 23.501 [9].

If the *Extended Connected Time* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, use it as described in TS 23.501 [9].

If the *UE Differentiation Information* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context for further use according to TS 23.501 [9].

If the *CE-mode-B Restricted* IE is included in the INITIAL CONTEXT SETUP REQUEST message and the *Enhanced Coverage Restriction* IE is not set to "restricted"and the Enhanced Coverage Restriction information stored in the UE context is not set to "restricted", the NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 23.501 [9].

If the *UE User Plane CIoT Support Indicator* IE is included in the INITIAL CONTEXT SETUP REQUEST message the NG-RAN node shall, if supported, store this information in the UE context and consider that User Plane CIoT 5GS Optimisation as specified in TS 23.501 [9] is supported for the UE.

If the *Management Based MDT PLMN List* IE is contained in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, use it to allow subsequent selection of the UE for management based MDT defined in TS 32.422 [11].

If the INITIAL CONTEXT SETUP REQUEST message contains the *UE Radio Capability ID* IE, the NG-RAN node shall, if supported, use it as specified in TS 23.501 [9] and TS 23.502 [10].

For each PDU session, if the *PDU Session Expected UE Activity Behaviour* IE is included in the INTIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, handle this information as specified in TS 23.501 [9].

If the *Time Synchronisation Assistance Information* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, store the information in the UE context and use it as defined in TS 23.501 [9].

If the *Target NSSAI Information* IE is contained in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node may use this information as specified in TS 23.501 [9].

If the *UE Slice Maximum Bit Rate List* IE is included in the INITIAL CONTEXT SETUP REQUEST message, the NG-RAN node shall, if supported, store the received UE Slice Maximum Bit Rate List in the UE context, and use it for each S-NSSAI for the concerned UE as specified in TS 23.501 [9].

**Interactions with Initial UE Message procedure:**

The NG-RAN node shall use the *AMF UE NGAP ID* IE and *RAN UE NGAP ID* IE received in the INITIAL CONTEXT SETUP REQUEST message as identification of the logical connection even if the *RAN UE NGAP ID* IE had been allocated in an INITIAL UE MESSAGE message sent over a different NG interface instance.

**Interactions with RRC Inactive Transition Report procedure:**

If the *RRC Inactive Transition Report Request* IE is included in the INITIAL CONTEXT SETUP REQUEST message and set to "subsequent state transition report", the NG-RAN node shall, if supported, send the RRC INACTIVE TRANSITION REPORT message to the AMF to report the RRC state of the UE when the UE enters or leaves RRC\_INACTIVE state.

**<Unchanged Text Omitted>**

### 8.3.4 UE Context Modification

#### 8.3.4.1 General

The purpose of the UE Context Modification procedure is to partly modify the established UE context. The procedure uses UE-associated signalling.

#### 8.3.4.2 Successful Operation

Figure 8.3.4.2-1: UE context modification: successful operation

Upon receipt of the UE CONTEXT MODIFICATION REQUEST message the NG-RAN node shall

- if supported, store the received IAB Authorization information in the UE context. If the *IAB Authorized* IE is set to "not authorized" for an IAB-MT, the NG-RAN node shall, if supported, initiate actions to ensure that the IAB node will not serve any UE(s).

If the *Security Key* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall store it and perform AS key re-keying according to TS 33.501 [13].

If the *UE Security Capabilities* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall store them and take them into use together with the received keys according to TS 33.501 [13].

If the *Index to RAT/Frequency Selection Priority* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, use it as defined in TS 23.501 [9].

If the *RAN Paging Priority* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node may use it to determine a priority for paging the UE in RRC\_INACTIVE state.

If the *UE Aggregate Maximum Bit Rate* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall

- replace the previously provided UE Aggregate Maximum Bit Rate by the received UE Aggregate Maximum Bit Rate in the UE context;

- use the received UE Aggregate Maximum Bit Rate for all Non-GBR QoS flows for the concerned UE as specified in TS 23.501 [9].

If the *Core Network Assistance Information for RRC INACTIVE* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, replace the previously provided Core Network Assistance Information for RRC INACTIVE and use it for the RRC\_INACTIVE state decision and RNA configuration for the UE and RAN paging if any for a UE in RRC\_INACTIVE state, as specified in TS 38.300 [8]. If the *MICO All PLMN* IE is included in the *Core Network Assistance Information* *for RRC INACTIVE* IE the NG-RAN node shall, if supported, consider that the registration area for the UE is the full PLMN and ignore the *TAI List for RRC Inactive* IE. If the *Paging Cause Indication for Voice Service* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store and use it as specified in TS 38.300 [8]. If the *PEIPS Assistance Information* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store it and use it for paging subgrouping the UE in RRC\_INACTIVE state, as specified in TS 38.300 [8].

If the *CN Assisted RAN Parameters Tuning* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node may use it as described in TS 23.501 [9].

If the *RRC Inactive Transition Report Request* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context and report to the AMF the *User Location Information* IE and the *RRC State* IE in the UE CONTEXT MODIFICATION RESPONSE message.

If the *RRC Inactive Transition Report Request* IE is included in the UE CONTEXT MODIFICATION REQUEST message and set to "cancel report", the NG-RAN node shall, if supported, stop reporting to the AMF the RRC state of the UE.

The NG-RAN node shall report, in the UE CONTEXT MODIFICATION RESPONSE message to the AMF, the successful update of the UE context.

If the *Emergency Fallback Indicator* IE is included in the UE CONTEXT MODIFICATION REQUEST message, it indicates that the concerned UE context is subject to emergency service fallback as described in TS 23.501 [9] and the NG-RAN node may, if supported, take the appropriate mobility actions taking into account the *Emergency Service Target CN* IE if provided.

If the *New AMF UE NGAP ID* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall use the received value for future signalling with the AMF.

If the *New GUAMI* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall replace the previously stored GUAMI as specified in TS 23.501 [9].

If the *SRVCC Operation Possible* IE is included in UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, store the content of the received *SRVCC Operation Possible* IE in the UE context and use it as defined in TS 23.216 [31].

If the *NR V2X Services Authorized* IE is contained in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, update its V2X services authorization information for the UE accordingly. If the *NR V2X Services Authorized* IE includes one or more IEs set to "not authorized", the NG-RAN node shall, if supported, initiate actions to ensure that the UE is no longer accessing the relevant service(s).

If the *LTE V2X Services Authorized* IE is contained in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, update its V2X services authorization information for the UE accordingly. If the *LTE V2X Services Authorized* IE includes one or more IEs set to "not authorized", the NG-RAN node shall, if supported, initiate actions to ensure that the UE is no longer accessing the relevant service(s).

If the *NR UE Sidelink Aggregate Maximum Bit Rate* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported:

- replace the previously provided NR UE Sidelink Aggregate Maximum Bit Rate, if available in the UE context, with the received value;

use the received value for the concerned UE’s sidelink communication in network scheduled mode for NR V2X services.

If the *LTE UE Sidelink Aggregate Maximum Bit Rate* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported:

- replace the previously provided LTE UE Sidelink Aggregate Maximum Bit Rate, if available in the UE context, with the received value;

- use the received value for the concerned UE’s sidelink communication in network scheduled mode for LTE V2X services.

If the *PC5 QoS Parameters* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, use it as defined in TS 23.287 [33].

If the UE CONTEXT MODIFICATION REQUEST message contains the *UE Radio Capability ID* IE, the NG-RAN node shall, if supported, use it as specified in TS 23.501 [9] and TS 23.502 [10].

If the *Time Synchronisation Assistance Information* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, store the information in the UE context and use it as defined in TS 23.501 [9].

If the *QMC Configuration Information* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, use it for QoE management, as described in TS 38.300 [8].

If the *QMC Deactivation* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, deactivate the QMC configurations therein.

If the *UE Slice Maximum Bit Rate List* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported:

- store and replace the previously provided UE Slice Maximum Bit Rate List, if any, by the received UE Slice Maximum Bit Rate List in the UE context;

- use the received UE Slice Maximum Bit Rate List for each S-NSSAI for the concerned UE as specified in TS 23.501 [9].

If the *Management Based MDT PLMN Modification* *List* IE is contained in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, overwrite any previously stored Management Based MDT PLMN List information in the UE context and use the received information to determine subsequent selection of the UE for management based MDT defined in TS 32.422 [11].

If the *5G ProSe Authorized* IE is included in UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, update the 5G ProSe authorization information for the UE accordingly. If the *5G ProSe Authorized* IE includes one or more IEs set to “not authorized”, the NG-RAN node shall, if supported, initiate actions to ensure that the UE is no longer accessing the relevant 5G ProSe service(s).

If the *5G ProSe UE PC5 Aggregate Maximum Bit Rate* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported:

- replace the previously provided 5G ProSe UE PC5 Aggregate Maximum Bit Rate, if available in the UE context, with the received value;

- use the received value for the concerned UE’s sidelink communication in network scheduled mode for 5G ProSe services.

If the *5G ProSe PC5 QoS Parameters* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, use it as defined in TS 23.304 [47].

If the *Network Controlled Repeater Authorized* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, update its Network Controlled Repeater Authorization information for the UE accordingly and take it into account when configuring UE information.

If the *Aerial UE Subscription Information* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, store the information or overwrite any previously stored information in the UE context and use it as defined in TS 38.300 [8].

If the *Ranging and Sidelink Positioning Service Information* IE is included in the UE CONTEXT MODIFICATION REQUEST message, the NG-RAN node shall, if supported, update the Ranging and Sidelink Positioning service information for the UE accordingly. If the *Ranging and Sidelink Positioning Authorized* IE within the *Ranging and Sidelink Positioning Service Information* IE is set to "not authorized", the NG-RAN node shall, if supported, initiate actions to ensure that the UE is no longer accessing the Ranging and Sidelink Positioning service.

**Interactions with RRC Inactive Transition Report procedure:**

If the *RRC Inactive Transition Report Request* IE is included in the UE CONTEXT MODIFICATION REQUEST message and set to "single RRC connected state report", the NG-RAN node shall, if supported and if the UE is in RRC\_INACTIVE state, send one subsequent RRC INACTIVE TRANSITION REPORT message to the AMF when the RRC state transitions to RRC\_CONNECTED state.

If the *RRC Inactive Transition Report Request* IE is included in the UE CONTEXT MODIFICATION REQUEST message and set to "subsequent state transition report", the NG-RAN node shall, if supported, send the RRC INACTIVE TRANSITION REPORT message to the AMF to report the RRC state of the UE when the UE enters or leaves RRC\_INACTIVE state.

**<Unchanged Text Omitted>**

### 8.4.2 Handover Resource Allocation

#### 8.4.2.1 General

The purpose of the Handover Resource Allocation procedure is to reserve resources at the target NG-RAN node for the handover of a UE. The procedure uses UE-associated signalling.

#### 8.4.2.2 Successful Operation

Figure 8.4.2.2-1: Handover resource allocation: successful operation

The AMF initiates the procedure by sending the HANDOVER REQUEST message to the target NG-RAN node.

If the *Masked IMEISV* IE is contained in the HANDOVER REQUEST message the target NG-RAN node shall, if supported, use it to determine the characteristics of the UE for subsequent handling.

Upon receipt of the HANDOVER REQUEST message the target NG-RAN node shall

- attempt to execute the requested PDU session configuration and associated security;

- store the received UE Aggregate Maximum Bit Rate in the UE context, and use the received UE Aggregate Maximum Bit Rate for all Non-GBR QoS flows for the concerned UE as specified in TS 23.501 [9];

- store the received Mobility Restriction List in the UE context;

- store the received UE Security Capabilities in the UE context;

- store the received Security Context in the UE context and take it into use as defined in TS 33.501 [13];

- if supported, store the received UE Slice Maximum Bit Rate List in the UE context and use the received UE Slice Maximum Bit Rate List for each S-NSSAI for the concerned UE as specified in TS 23.501 [9].

- if supported, store the received PDU Set QoS parameters in the UE context and use it as specified in TS 23.501 [9].

Upon reception of the *UE History Information* IE, which is included within the *Source to Target Transparent Container* IE of the HANDOVER REQUEST message, the target NG-RAN node shall collect the information defined as mandatory in the *UE History Information* IE and shall, if supported, collect the information defined as optional in the *UE History Information* IE, for as long as the UE stays in one of its cells, and store the collected information to be used for future handover preparations.

Upon receiving the *PDU Session Resource Setup List* IE contained in the HANDOVER REQUEST message and the HANDOVER REQUEST message does not contain the *No PDU Session Indication* IE, the target NG-RAN node shall behave the same as defined in the PDU Session Resource Setup procedure. The target NG-RAN node shall report to the AMF in the HANDOVER REQUEST ACKNOWLEDGE message the result for each PDU session resource requested to be setup. In particular, for each PDU session resource successfully setup, it shall include the *Handover Request Acknowledge Transfer* IE containing the following information:

- The list of QoS flows which have been successfully established in the *QoS Flow Setup Response List* IE.

- The *Data Forwarding Accepted* IE if the data forwarding for the QoS flow is accepted.

- The list of QoS flows which have failed to be established, if any, in the *QoS Flow Failed to Setup List* IE.

- The UP transport layer information to be used for the PDU session.

- The security result associated to the PDU session.

- The redundant UP transport layer information to be used for the redundant transmission for the PDU session.

- The PDU Set based Handling Indicator if the HANDOVER REQUEST message includes the *PDU Set QoS Parameters* IE.

For each PDU session resource which failed to be setup, the *Handover Resource Allocation Unsuccessful Transfer* IE shall be included in the HANDOVER REQUEST ACKNOWLEDGE message containing a cause value that should be precise enough to enable the SMF to know the reason for the unsuccessful establishment.

For each PDU session included in the HANDOVER REQUEST ACKNOWLEDGE message, if the *Current QoS Parameters Set Index* IE is included for a QoS flow in the *QoS Flow Setup Response List* IE within the *Handover Request Acknowledge Transfer* IE the SMF shall consider it as the currently fulfilled QoS parameters set among the alternative QoS parameters for the involved QoS flow.

Upon reception of the HANDOVER REQUEST ACKNOWLEDGE message the AMF shall, for each PDU session indicated in the *PDU Session ID* IE, transfer transparently the *Handover Request Acknowledge Transfer* IE or *Handover Resource Allocation Unsuccessful Transfer* IE to the SMF associated with the concerned PDU session.

If the HANDOVER REQUEST message contains the *Data Forwarding Not Possible* IE associated with a given PDU session within the *Handover Request Transfer* IE set to "data forwarding not possible", the target NG-RAN node may not include the *DL Forwarding UP TNL Information* IE and for intra-system handover the *Data Forwarding Response DRB List* IE within the *Handover Request Acknowledge Transfer* IE in the HANDOVER REQUEST ACKNOWLEDGE message for that PDU session.

If the HANDOVER REQUEST message contains the *Redundant PDU Session Information* IE associated with a given PDU session within the *Handover Request Transfer* IE, the target NG-RAN node shall, if supported, store the received information in the UE context and use it for redundant PDU session setup as specified in TS38.300 [8] and TS 23.501 [9]. If the *PDU Session Type* IE is set to “ethernet” and the redundancy requirement is fulfilled using a secondary NG-RAN node, the NG-RAN node shall, if supported, include the *Global RAN Node ID of Secondary NG-RAN Node* IE in the *Handover Request Acknowledge Transfer* IE of the HANDOVER REQUEST ACKNOWLEDGE message. If the *PDU Session Pair ID* IE is included in the *Redundant PDU Session Information* IE, the NG-RAN node may use it to identify the paired PDU sessions.

For each PDU session for which the *Global RAN Node ID of Secondary NG-RAN Node* IE is included in the *Handover Request Acknowledge Transfer* IE of the HANDOVER REQUEST ACKNOWLEDGE message, the SMF shall, if supported, handle this information as specified in TS 23.501 [9].

In case of intra-system handover, if the target NG-RAN node accepts the downlink data forwarding for at least one QoS flow for which the *DL Forwarding* IE is set to "DL forwarding proposed", it may include the *DL Forwarding UP TNL Information* IE in the *Handover Request Acknowledge Transfer* IE as forwarding tunnel for the QoS flows listed in the *QoS Flow Setup Response List* IE of the HANDOVER REQUEST ACKNOWLEDGE message.

In case of intra-system handover, if the target NG-RAN node accepts the uplink data forwarding for at least one QoS flow for which the *UL Forwarding* IE is set to "UL forwarding proposed", it may include the *UL Forwarding UP TNL Information* IE in the *Handover Request Acknowledge Transfer* IE for the PDU session within the *PDU Session Resource Admitted List* IE of the HANDOVER REQUEST ACKNOWLEDGE message.

In case of intra-system handover, for each PDU session for which the *Additional DL UP TNL Information for HO List* IE is included in the *Handover Request Acknowledge Transfer* IE of the HANDOVER REQUEST ACKNOWLEDGE message, the SMF shall consider the included *Additional DL NG-U UP TNL Information* IE as the downlink termination point for the associated flows indicated in the *Additional QoS Flow Setup Response List* IE for this PDU session split in different tunnels and shall consider the *Additional DL Forwarding UP TNL Information* IE, if included, as the forwarding tunnel associated to these QoS flows.

In case of intra-system handover, for each PDU session for which the *Additional UL Forwarding UP TNL Information* IE is included in the *Handover Request Acknowledge Transfer* IE of the HANDOVER REQUEST ACKNOWLEDGE message, the SMF shall consider it as the termination points for the uplink forwarding tunnels for this PDU session split in different tunnels.

In case of intra-system handover, if the target NG-RAN node accepts the data forwarding for a successfully configured DRB, the target NG-RAN node may include the *DL Forwarding UP TNL Information* IE for the DRB within the *Data Forwarding Response DRB List* IE within *Handover Request Acknowledge Transfer* IE of the HANDOVER REQUEST ACKNOWLEDGE message.

In case of intra-system handover, if the target NG-RAN node receives the *Direct Forwarding Path Availability* IE set to "direct path available" within the *PDU Session Resource Setup Request Transfer* IE, the target NG-RAN node shall, if supported, assign the UP Transport Layer Information for intra-system direct data forwarding from the appropriate address space, if applicable.

If the HANDOVER REQUEST ACKNOWLEDGE message contains the *UL Forwarding UP TNL Information* IE for a given DRB in the *Data Forwarding Response DRB List* IE within the *Handover Request Acknowledge Transfer* IE, it indicates the target NG-RAN node has requested the forwarding of uplink data for the DRB.

In case of inter-system handover from E-UTRAN, if the *PDU Session Resource Setup Request Transfer* IE contains the *Direct Forwarding Path Availability* IE set to "direct path available", the target NG-RAN node shall, if supported, and if it accepts downlink data forwarding for the QoS flows mapped to an E-RAB of an admitted PDU session, include the *DL Forwarding UP TNL Information* IE in the *Data Forwarding Response E-RAB List* IE in the *Handover Request Acknowledge Transfer* IE in the HANDOVER REQUEST ACKNOWLEDGE message for that mapped E-RAB.

In case of inter-system handover from E-UTRAN, the target NG-RAN node includes the *Data Forwarding Accepted* IE for each QoS flow that the *DL Forwarding* IE is set to "DL forwarding proposed" for the corresponding E-RAB in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE and that the target NG-RAN node has admitted the proposed forwarding of downlink data for the QoS flow. If indirect data forwarding is applied for inter-system handover, if the target NG-RAN node accepts the downlink data forwarding for at least one QoS flow of an admitted PDU session it shall include the *DL Forwarding UP TNL Information* IE in the *PDU Session Resource Setup Response Transfer* IE for that PDU session within the *PDU Session Resources Admitted List* IE of the HANDOVER REQUEST ACKNOWLEDGE message.

In case of inter-system handover from E-UTRAN with direct forwarding, if the target NG-RAN node receives the *SgNB UE X2AP ID* IE in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE, it may use it for internal forwarding as described in TS 37.340 [32].

In case of inter-system handover from E-UTRAN, if the target cell is a CAG cell, the target NG-RAN node shall include the *NPN Access Information* IE in the HANDOVER REQUEST ACKNOWLEDGE message, and the AMF shall consider that the included information is associated to the target cell and to the UE’s serving PLMN identity, and use it as specified in TS 23.501 [9].

The target NG-RAN node shall use the information in the *Mobility Restriction List* IE if present in the HANDOVER REQUEST message to

- determine a target for subsequent mobility action for which the target NG-RAN node provides information about the target of the mobility action towards the UE;

- select a proper SCG during dual connectivity operation;

- assign proper RNA(s) for the UE when moving the UE to RRC\_INACTIVE state.

If the *Mobility Restriction List* IE is not contained in the HANDOVER REQUEST message, the target NG-RAN node shall consider that no roaming and no access restriction apply to the UE except for the PNI NPN mobility as described in TS 23.501 [9]. The target NG-RAN node shall also consider that no roaming and no access restriction apply to the UE when:

- one of the QoS flows includes a particular ARP value (TS 23.501 [9]).

The NG-RAN node shall consider that roaming or access to CAG cells is only allowed if the *Allowed PNI-NPN List* IE is contained in the HANDOVER REQUEST message, as described in TS 23.501 [9].

If the *Trace Activation* IE is included in the HANDOVER REQUEST message the target NG-RAN node shall, if supported, initiate the requested trace function as described in TS 32.422 [11]. In particular, the NG-RAN node shall, if supported:

- if the *Trace Activation* IE includes the *MDT Activation* IE set to "Immediate MDT and Trace", initiate the requested trace session and MDT session as described in TS 32.422 [11];

- if the *Trace Activation* IE includes the *MDT Activation* IE set to "Immediate MDT Only", "Logged MDT only", initiate the requested MDT session as described in TS 32.422 [11] and the target NG-RAN node shall ignore the *Interfaces To Trace* IE and the *Trace Depth* IE;

- if the *Trace Activation* IE includes the *MDT Location Information* IE within the *MDT Configuration* IE, store this information and take it into account in the requested MDT session;

- if the *Trace Activation* IE includes the *Signalling Based MDT PLMN List* IE within the *MDT Configuration* IE, the NG-RAN node may use it to propagate the MDT Configuration as described in TS 37.320 [41].

- if the *Trace Activation* IE includes the *Bluetooth Measurement Configuration* IE within the *MDT Configuration* IE, take it into account for MDT Configuration as described in TS 37.320 [41].

- if the *Trace Activation* IE includes the *WLAN Measurement Configuration* IE within the *MDT Configuration* IE, take it into account for MDT Configuration as described in TS 37.320 [41].

- if the *Trace Activation* IE includes the *Sensor Measurement Configuration* IE within the *MDT Configuration* IE, take it into account for MDT Configuration as described in TS 37.320 [41].

- if the *Trace Activation* IE includes the *MDT Configuration* IE and if the NG-RAN node is a gNB at least the *MDT Configuration-NR* IE shall be present, while if the NG-RAN node is an ng-eNB at least the *MDT Configuration-EUTRA* IE shall be present.

If the *Location Reporting Request Type* IE is included in the HANDOVER REQUEST message, the target NG-RAN node should perform the requested location reporting functionality for the UE as described in subclause 8.12.

If the *Core Network Assistance Information for RRC INACTIVE* IE is included in the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store this information in the UE context and use it for the RRC\_INACTIVE state decision and RNA configuration for the UE and RAN paging if any for a UE in RRC\_INACTIVE state, as specified in TS 38.300 [8]. If the *MICO All PLMN* IE is included in the *Core Network Assistance Information* *for RRC INACTIVE* IE the NG-RAN node shall, if supported, consider that the registration area for the UE is the full PLMN and ignore the *TAI List for RRC Inactive* IE. If the *Paging Cause Indication for Voice Service* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store and use it as specified in TS 38.300 [8]. If the *PEIPS Assistance Information* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store it and use it for paging subgrouping the UE in RRC\_INACTIVE state, as specified in TS 38.300 [8]. If the *CN MT Communication Handling* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store it and may subsequently request, based on implementation, the CN for mobile terminated communication handling as described in TS 23.502 [10].

If the *CN Assisted RAN Parameters Tuning* IE is included in the HANDOVER REQUEST message, the NG-RAN node may use it as described in TS 23.501 [9].

If the *New Security Context Indicator* IE is included in the HANDOVER REQUEST message, the target NG-RAN node shall use the information as specified in TS 33.501 [13].

If the *NASC* IE is included in the HANDOVER REQUEST message, the target NG-RAN node shall use it towards the UE as specified in TS 33.501 [13].

If the *RRC Inactive Transition Report Request* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context.

If the *Redirection for Voice EPS Fallback* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, store it and use it in a subsequent decision of EPS fallback for voice as specified in TS 23.502 [10].

If the *SRVCC Operation Possible* IE is included in the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store the content of the received *SRVCC Operation Possible* IE in the UE context and use it as defined in TS 23.216 [31].

If the *IAB Authorized* IE is contained in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, consider that the handover is for an IAB node.

If the *Mobile IAB Authorized* IE is contained in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, consider that the handover is for a mobile IAB-node. In addition, if the *No PDU Session Indication* IE is contained in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, consider the mobile IAB-MT does not have any PDU sessions activated, ignore the *PDU Session Resource Setup List* IE, and it shall not take any action with respect to PDU session setup.

If the *Enhanced Coverage Restriction* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 23.501 [9].

If the *UE Differentiation Information* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context for further use according to TS 23.501 [9].

If the *UE User Plane CIoT Support Indicator* IE is included in the HANDOVER REQUEST message the NG-RAN node shall, if supported, store this information in the UE context and consider that User Plane CIoT 5GS Optimisation as specified in TS 23.501 [9] is supported for the UE.

Upon reception of the *UE History Information from UE* IE, which is included within the *Source to Target Transparent Container* IE of the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store the collected information and use it for future handover preparations.

After all necessary resources for the admitted PDU session resources have been allocated, the target NG-RAN node shall generate the HANDOVER REQUEST ACKNOWLEDGE message.

If the *RedCap Indication* IE is included in the HANDOVER REQUEST ACKNOWLEDGE message, the AMF shall, if supported, consider the UE as a RedCap UE that was previously served by a E-UTRA cell, and use the IE according to TS 23.501 [9].

For each QoS flow which has been established in the target NG-RAN node, if the *QoS Monitoring Request* IE was included in the *QoS Flow Level QoS Parameters* IE contained in the HANDOVER REQUEST message, the target NG-RAN node shall store this information, and, if supported, perform delay measurement and QoS monitoring, as specified in TS 23.501 [9]. If the *QoS Monitoring Reporting Frequency* IE was included in the *QoS Flow Level QoS Parameters* IE contained in the HANDOVER REQUEST message, the target NG-RAN node shall store this information and, if supported, use it for RAN part delay reporting.

If the *NR V2X Services Authorized* IE is contained in the HANDOVER REQUEST message and it contains one or more IEs set to "authorized", the NG-RAN node shall, if supported, consider that the UE is authorized for the relevant service(s).

If the *LTE V2X Services Authorized* IE is contained in the HANDOVER REQUEST message and it contains one or more IEs set to "authorized", the NG-RAN node shall, if supported, consider that the UE is authorized for the relevant service(s).

If the *NR A2X Services Authorized* IE is contained in the HANDOVER REQUEST message and it contains one or more IEs set to "authorized", the NG-RAN node shall, if supported, consider that the UE is authorized for the relevant service(s).

If the *LTE A2X Services Authorized* IE is contained in the HANDOVER REQUEST message and it contains one or more IEs set to "authorized", the NG-RAN node shall, if supported, consider that the UE is authorized for the relevant service(s).

If the *NR UE Sidelink Aggregate Maximum Bit Rate* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use the received value for the concerned UE’s sidelink communication in network scheduled mode for NR V2X services.

If the *LTE UE Sidelink Aggregate Maximum Bit Rate* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use the received value for the concerned UE’s sidelink communication in network scheduled mode for LTE V2X services.

If the *NR A2X UE PC5Aggregate Maximum Bit Rate* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use the received value for the concerned UE’s sidelink communication in network scheduled mode for NR A2X services.

If the *LTE A2X UE PC5 Aggregate Maximum Bit Rate* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use the received value for the concerned UE’s sidelink communication in network scheduled mode for LTE A2X services.

If the *PC5 QoS Parameters* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use it as defined in TS 23.287 [33].

If the *A2X PC5 QoS Parameters* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use it as defined in TS 23.256 [54].

If the *CE-mode-B Restricted* IE is included in the HANDOVER REQUEST message and the *Enhanced Coverage Restriction* IE is not set to "restricted"and the Enhanced Coverage Restriction information stored in the UE context is not set to "restricted", the NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 23.501 [9].

If the *Management Based MDT PLMN List* IE is contained in the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store the received information in the UE context, and use this information to allow subsequent selections of the UE for management based MDT defined in TS 32.422 [11].

If the HANDOVER REQUEST message contains the *UE Radio Capability ID* IE, the NG-RAN node shall, if supported, use it as specified in TS 23.501 [9] and TS 23.502 [10].

If the *DAPS Request Information* IE is included for a DRB in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST message, the target NG-RAN node shall consider that the request concerns a DAPS Handover for that DRB, as described in in TS 38.300 [8]. The target NG-RAN node shall include the *DAPS Response information List* IE in the *Target NG-RAN Node to Source NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST ACKNOWLEDGE message, containing the *DAPS Response Information* IE for each DRB requested to be configured with DAPS Handover.

If the *Extended Connected Time* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use it as described in TS 23.501 [9].

If the target NG-RAN node receives the *UE Context Reference at Source* IE in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST message, it may use it to identify an existing UE.

If the *Source Node ID* IE is included in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, use it to decide whether direct forwarding path is available between the target NG-RAN node and this source RAN node. If the direct forwarding path is available, the target NG-RAN node shall include the *Direct Forwarding Path Availability* IE in the *Target NG-RAN Node to Source NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST ACKNOWLEDGE message.

In case there are MBS sessions the UE has joined, for all the MBS sessions the UE has joined, the SMF shall, if supported, include the *MBS Session Setup Request List* IE within the *PDU Session Resource Setup Request Transfer* IE in the HANDOVER REQUEST message.

If the HANDOVER REQUEST message contains the *MBS Session Setup Request List* IE in a *PDU Session Resource Setup Request Transfer* IE the NG-RAN node shall, if supported, use it as specified in TS 23.247 [44] and TS 38.300 [8].

If the *MBS Active Session Information Source to Target List* IE is contained in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, assume the indicated MBS sessions to be active and establish MBS session resources as specified in TS 23.247 [44] and TS 38.300 [8], if applicable. The target NG-RAN node shall, if supported, consider that the MBS sessions the UE has joined which are not included in the *MBS Active Session Information Source to Target List* IE are inactive.

If the *MBS Area Session ID* IE is included in the *MBS Active Session Information Source to Target List* IE in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST message, the target NG-RAN shall use this information as indication from which MBS Area Session ID the UE is handed over.

If the *MBS Service Area* IE is included in the *MBS Active Session Information Source to Target List* IE in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST message, the target NG-RAN shall use this information to setup respective MBS session resources, if applicable.

If the target NG-RAN node decides to allocate resource for data forwarding for an active MBS session, respective information is provided for that MBS session within the *Data Forwarding Response MRB List* IE in the *MBS Active Session Information Target to Source List* IE in the *Target NG-RAN Node to Source NG-RAN Node Transparent Container* IE.

If the *Time Synchronisation Assistance Information* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, store the information in the UE context and use it as defined in TS 23.501 [9].

If the *5G ProSe Authorized* IE is contained in the HANDOVER REQUEST message and it contains one or more IEs set to "authorized", the NG-RAN node shall, if supported, consider that the UE is authorized for the relevant service(s).

If the *5G ProSe UE PC5 Aggregate Maximum Bit Rate* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use the received value for the concerned UE’s sidelink communication in network scheduled mode for 5G ProSe services.

If the *5G ProSe PC5 QoS Parameters* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use it as defined in TS 23.304 [47].

If for a given QoS flow the *Source Transport Layer Address* IE is included within the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE of the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store this information and use it as part of its ACL functionality configuration actions for direct data forwarding, if such ACL functionality is deployed and if direct forwarding path is available between the target NG-RAN node and this source RAN node.

If for a given QoS flow the *Source Node Transport Layer Address* IE is included within the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE of the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store this information and use it as part of its ACL functionality configuration actions for direct data forwarding, if such ACL functionality is deployed and if direct forwarding path is available between the target NG-RAN node and this source RAN node.

If for a given E-RAB the *Source Transport Layer Address* IE is included within the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE of the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store this information and use it as part of its ACL functionality configuration actions for direct data forwarding, if such ACL functionality is deployed and if direct forwarding path is available between the target NG-RAN node and this source RAN node.

If for a given E-RAB the *Source Node Transport Layer Address* IE is included within the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE of the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, store this information and use it as part of its ACL functionality configuration actions for direct data forwarding, if such ACL functionality is deployed and if direct forwarding path is available between the target NG-RAN node and this source RAN node.

If the HANDOVER REQUEST message contains within the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IEthe *NGAP IE Support Information Request List* IE, the target NG-RAN node shall, if supported and the target NG-RAN node accepts the request for handover, for each included NGAP Protocol IE-Id provided within the *Target NG-RAN Node to Source NG-RAN Node Transparent Container* IE in the HANDOVER REQUEST ACKNOWLEDGE message

- set the *NGAP Protocol IE Support Information* IE to "supported" if the target NG-RAN node has information that the functionality associated with the indicated IE is supported

- set the *NGAP Protocol IE Support Information* IE to "not-supported" if the target NG-RAN node has information that the functionality associated with the indicated IE is not supported

on the interface instance via which the HANDOVER REQUEST message has been received, and

- set the *NGAP Protocol IE Presence Information* IE to "present" if the target NG-RAN node has received the respective NGAP Protocol IE-Id in the HANDOVER REQUEST message, and “not-present” otherwise.

If the HANDOVER REQUEST message contains within the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE the *Time Based Handover Information* IE, the target NG-RAN node may use this information to allocate necessary resources for the incoming handover.

If the *Candidate Relay UE* *Information List* IE is included in the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE within the HANDOVER REQUEST message, the target NG-RAN node shall, if supported, use it to configure the path switch to indirect path as specified in TS 38.300 [8].

If the *Aerial UE Subscription Information* IE is included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 38.300 [8].

If the *PNI-NPN Area Scope of MDT* IE is included in the *MDT Configuration-NR* IE included in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, use it to derive the MDT area scope for MDT measurement collection in PNI-NPN areas. Upon reception of the *PNI-NPN Area Scope of MDT* IE, the NG-RAN node shall consider that the area scope for MDT measurement collection in PNI-NPN areas is defined only by the areas included in the *PNI-NPN Area Scope of MDT* IE.

If the *Partially Allowed NSSAI* IE is contained in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, deduce from it the partially allowed network slices for the UE, store and replace any previously received Partially Allowed NSSAI and use it as specified in TS 23.501 [9].

If the *Ranging and Sidelink Positioning Service Information* IE is contained in the HANDOVER REQUEST message, the NG-RAN node shall, if supported, take it into account for the Ranging and Sidelink Positioning service.

**Interactions with RRC Inactive Transition Report procedure:**

If the *RRC Inactive Transition Report Request* IE is included in the HANDOVER REQUEST message and set to "subsequent state transition report", the NG-RAN node shall, if supported, send the RRC INACTIVE TRANSITION REPORT message to the AMF to report the RRC state of the UE when the UE enters or leaves RRC\_INACTIVE state.

**<Unchanged Text Omitted>**

### 8.4.4 Path Switch Request

#### 8.4.4.1 General

The purpose of the Path Switch Request procedure is to establish a UE associated signalling connection to the 5GC and, if applicable, to request the switch of the downlink termination point of the NG-U transport bearer towards a new termination point. The procedure uses UE-associated signalling.

#### 8.4.4.2 Successful Operation

Figure 8.4.4.2-1: Path switch request: successful operation

The NG-RAN node initiates the procedure by sending the PATH SWITCH REQUEST message to the AMF. Upon reception of the PATH SWITCH REQUEST message the AMF shall, for each PDU session indicated in the *PDU Session ID* IE, transparently transfer the *Path Switch Request Transfer* IE to the SMF associated with the concerned PDU session.

When the NG-RAN node has received from the radio interface the *RRC Resume Cause* IE, it shall include it in the PATH SWITCH REQUEST message.

If the *RedCap Indication* IE is included in the PATH SWITCH REQUEST message, the AMF shall, if supported, consider the UE as a RedCap UE that was previously served by a E-UTRA cell, and use the IE according to TS 23.501 [9].

After all necessary updates including the UP path switch have been successfully completed in the 5GC for at least one of the PDU session resources included in the PATH SWITCH REQUEST, the AMF shall send the PATH SWITCH REQUEST ACKNOWLEDGE message to the NG-RAN node and the procedure ends.

The list of accepted QoS flows shall be included in the PATH SWITCH REQUEST message within the *Path Switch Request Transfer* IE. The SMF shall handle this information as specified in TS 23.502 [10].

For each PDU session for which the *Additional DL QoS Flow per TNL Information* IE is included in the *Path Switch Request Transfer* IE of the PATH SWITCH REQUEST message, the SMF may use each included UP transport layer information as the downlink termination point for the included associated QoS flows for this PDU session split in different tunnels.

The list of PDU sessions which failed to be setup, if any, shall be included in the PATH SWITCH REQUEST message within the *Path Switch Request Setup Failed Transfer* IE. The AMF shall handle this information as specified in TS 23.502 [10].

For each PDU session for which the *User Plane Security Information* IE is included in the *Path Switch Request Transfer* IE of the PATH SWITCH REQUEST message, the SMF shall behave as specified in TS 33.501 [13] and may send back the *Security Indication* IE within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message.

For each PDU session for which the *DL NG-U TNL Information Reused* IE set to "true" is included in the *Path Switch Request Transfer* IE of the PATH SWITCH REQUEST message, the SMF shall, if supported, consider that the DL TNL information contained in the *DL NG-U UP TNL Information* IE has been reused.

For each PDU session for which the *Additional Redundant DL QoS Flow per TNL Information* IE is included in the *Path Switch Request Transfer* IE of the PATH SWITCH REQUEST message, the SMF may use each included UP transport layer information as the downlink termination point for the included associated QoS flows for this PDU session split in different tunnels for the redundant transmission.

For each PDU session for which the *Redundant DL NG-U TNL Information Reused* IE is included in the *Path Switch Request Transfer* IE of the PATH SWITCH REQUEST message, the SMF shall, if supported, consider the included DL transport layer address as the DL transport layer address for the redundant transmission as specified in TS 23.501 [9].

For each PDU session for which the *Global RAN Node ID of Secondary NG-RAN Node* IE is included in the *Path Switch Request Transfer* IE of the PATH SWITCH REQUEST message, the SMF shall, if supported, handle this information as specified in TS 23.501 [9].

For each PDU session included in the PATH SWITCH REQUEST message, if the *Current QoS Parameters Set Index* IE is included in the *Path Switch Request Transfer* IE the SMF shall consider it as the currently fulfilled QoS parameters set among the alternative QoS parameters for the involved QoS flow.

If the *Security Indication* IE is included within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall behave as specified in TS 33.501 [13].

If the *UL NG-U UP TNL Information* IE is included within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall store this information and use it as the uplink termination point for the user plane data for this PDU session.

If the *Additional NG-U* *UP TNL Information* IE is included within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall store this information and use the included *UL NG-U UP TNL Information* IE(s) as the uplink termination point(s) of the user plane data for this PDU session split in different tunnel.

If the *Redundant UL NG-U UP TNL Information* IE is included within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store this information and use it as the uplink termination point for the user plane data for the redundant transmission for this PDU session as specified in TS 23.501 [9].

If the *Additional Redundant NG-U* *UP TNL Information* IE is included within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store this information and use the included *UL NG-U UP TNL Information* IE(s) as the uplink termination point(s) of the user plane data for this PDU session split in different tunnel.

If the *CN Packet Delay Budget Downlink* IE is included within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, replace the previously provided CN Packet Delay Budget Downlink if any and use it as specified in TS 23.502 [10].

If the *CN Packet Delay Budget Uplink* IE is included within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, replace the previously provided CN Packet Delay Budget Uplink if any and use it as specified in TS 23.502 [10].

If the *Burst Arrival Time Downlink* IE is included within the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, replace the previously provided value if any and use it as specified in TS 23.502 [10].

If the *Core Network Assistance Information for RRC INACTIVE* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store this information in the UE context and use it for the RRC\_INACTIVE state decision and RNA configuration for the UE and RAN paging if any for a UE in RRC\_INACTIVE state, as specified in TS 38.300 [8]. If the *MICO All PLMN* IE is included in the *Core Network Assistance Information* *for RRC INACTIVE* IE the NG-RAN node shall, if supported, consider that the registration area for the UE is the full PLMN and ignore the *TAI List for RRC Inactive* IE. If the *Paging Cause Indication for Voice Service* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store and use it as specified in TS 38.300 [8]. If the *PEIPS Assistance Information* IE is included in the *Core Network Assistance Information for RRC INACTIVE* IE, the NG-RAN node shall, if supported, store it and use it for paging subgrouping the UE in RRC\_INACTIVE state, as specified in TS 38.300 [8].

If the *CN Assisted RAN Parameters Tuning* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node may use it as described in TS 23.501 [9].

If the *RRC Inactive Transition Report Request* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store this information in the UE context.

If the *New Security Context Indicator* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall use the information as specified in TS 33.501 [13].

Upon reception of the PATH SWITCH REQUEST ACKNOWLEDGE message the NG-RAN node shall store the received *Security Context* IE in the UE context and the NG-RAN node shall use it as specified in TS 33.501 [13].

If the *UE Security Capabilities* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall handle it accordingly (TS 33.501 [13]).

If the *Redirection for Voice EPS Fallback* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store it and use it in a subsequent decision of EPS fallback for voice as specified in TS 23.502 [10].

If the *PDU Session Resource Released List* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall release the corresponding QoS flows and regard the PDU session(s) indicated in the *PDU Session Resource Released List* IE as being released. The appropriate cause value for each PDU session released is included in the *Path Switch Request Unsuccessful Transfer* IE contained in the PATH SWITCH REQUEST ACKNOWLEDGE message.

If the *SRVCC Operation Possible* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store the content of the received *SRVCC Operation Possible* IE in the UE context and use it as defined in TS 23.216 [31].

If the *Enhanced Coverage Restriction* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 23.501 [9].

If the *Extended Connected Time* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, use it as described in TS 23.501 [9].

If the *UE Differentiation Information* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store this information in the UE context for further use according to TS 23.501 [9].

If the *NR V2X Services Authorized* IE is contained in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, update its NR V2X services authorization information for the UE accordingly. If the *NR V2X Services Authorized* IE includes one or more IEs set to "not authorized", the NG-RAN node shall, if supported, initiate actions to ensure that the UE is no longer accessing the relevant service(s).

If the *LTE V2X Services Authorized* IE is contained in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, update its LTE V2X services authorization information for the UE accordingly. If the *LTE V2X Services Authorized* IE includes one or more IEs set to "not authorized", the NG-RAN node shall, if supported, initiate actions to ensure that the UE is no longer accessing the relevant service(s).

If the *NR UE Sidelink Aggregate Maximum Bit Rate* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported:

- replace the previously provided UE Sidelink Aggregate Maximum Bit Rate, if available in the UE context, with the received value;

- use the received value for the concerned UE’s sidelink communication in network scheduled mode for NR V2X services.

If the *LTE UE Sidelink Aggregate Maximum Bit Rate* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported:

- replace the previously provided UE Sidelink Aggregate Maximum Bit Rate, if available in the UE context, with the received value;

- use the received value for the concerned UE’s sidelink communication in network scheduled mode for LTE V2X services.

If the *PC5 QoS Parameters* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, use it as defined in TS 23.287 [33].

If the *CE-mode-B Restricted* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message and the *Enhanced Coverage Restriction* IE is not set to "restricted"and the Enhanced Coverage Restriction information stored in the UE context is not set to "restricted", the NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 23.501 [9].

If the *UE User Plane CIoT Support Indicator* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message the NG-RAN node shall, if supported, store this information in the UE context and consider that User Plane CIoT 5GS Optimisation as specified in TS 23.501 [9] is supported for the UE.

If the PATH SWITCH REQUEST ACKNOWLEDGE message contains the *UE Radio Capability ID* IE, the NG-RAN node shall, if supported, use it as specified in TS 23.501 [9] and TS 23.502 [10].

If the PATH SWITCH REQUEST ACKNOWLEDGE message contains the *Alternative QoS Parameters Set List* IE, the NG-RAN node shall, if supported, use it as specified in TS 23.502 [10].

For each PDU session, if the *PDU Session Expected UE Activity Behaviour* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, handle this information as specified in TS 23.501 [9].

If the PATH SWITCH REQUEST ACKNOWLEDGE message contains the *Management Based MDT PLMN List* IE, the NG-RAN node shall store it in the UE context, and if supported, use it to allow subsequent selection of the UE for management based MDT defined in TS 32.422 [11].

If the PATH SWITCH REQUEST ACKNOWLEDGE message contains the *Management Based MDT PLMN Modification List* IE, the NG-RAN node shall, if supported, use it to overwrite any previously stored management based MDT PLMN list information in the UE context and use the received information to allow subsequent selection of the UE for management based MDT defined in TS 32.422 [11].

If the *Time Synchronisation Assistance Information* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store the information in the UE context and use it as defined in TS 23.501 [9].

If the *5G ProSe Authorized* IE is contained in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, update its ProSe authorization information for the UE accordingly. If the *5G ProSe Authorized* IEincludes one and more IEs set to "not authorized", the NG-RAN node shall, if supported, initiate actions to ensure that the UE is no longer accessing the relevant 5G ProSe service(s).

If the *5G ProSe UE PC5 Aggregate Maximum Bit Rate* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported:

- replace the previously provided 5G ProSe UE PC5 Aggregate Maximum Bit Rate, if available in the UE context, with the received value;

- use the received value for the concerned UE’s sidelink communication in network scheduled mode for 5G ProSe services.

If the *5G ProSe PC5 QoS Parameters* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, use it as defined in TS 23.304 [47].

If the *Aerial UE Subscription Information* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store the information or overwrite any previously stored information in the UE context and use it as defined in TS 38.300 [8].

If the *IAB Authorized* IE is contained in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store the received IAB Authorization information in the UE context. If the *IAB Authorized* IE is set to "not authorized" for an IAB-MT, the NG-RAN node shall, if supported, initiate actions to ensure that the IAB node will not serve any UE(s).

If the *Mobile* *IAB Authorized* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, store the received mobile IAB Authorization status in the UE context of the mobile IAB-MT. If the *Mobile* *IAB Authorized* IE for a mobile IAB-MT is set to "not authorized", the NG-RAN node shall, if supported, ensure that the mobile IAB-node will not serve any UE(s).

If the *Partially Allowed NSSAI* IE is contained in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, deduce from it the partially allowed network slices for the UE, store and replace any previously received Partially Allowed NSSAI and use it as specified in TS 23.501 [9].

If the *Ranging and Sidelink Positioning Service Information* IE is contained in the PATH SWITCH REQUEST ACKNOWLEDGE message, the NG-RAN node shall, if supported, update the Ranging and Sidelink Positioning service information for the UE accordingly. If the *Ranging and Sidelink Positioning Authorized* IEwithin the *Ranging and Sidelink Positioning Service Information* IE is set to "not authorized", the NG-RAN node shall, if supported, initiate actions to ensure that the UE is no longer accessing the Ranging and Sidelink Positioning service.

**Interactions with RRC Inactive Transition Report procedure:**

If the *RRC Inactive Transition Report Request* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message and set to "single RRC connected state report" and the UE is in RRC\_CONNECTED state, the NG-RAN node shall, if supported, send one RRC INACTIVE TRANSITION REPORT message to the AMF to report the RRC state of the UE.

If the *RRC Inactive Transition Report Request* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message and set to "single RRC connected state report" and the UE is in RRC\_INACTIVE state, the NG-RAN node shall, if supported, send to the AMF one RRC INACTIVE TRANSITION REPORT message plus one subsequent RRC INACTIVE TRANSITION REPORT message when the RRC state transitions to RRC\_CONNECTED state.

If the *RRC Inactive Transition Report Request* IE is included in the PATH SWITCH REQUEST ACKNOWLEDGE message and set to "subsequent state transition report", the NG-RAN node shall, if supported, send one RRC INACTIVE TRANSITION REPORT message to the AMF to report the RRC state of the UE and subsequent RRC INACTIVE TRANSITION REPORT messages to report the RRC state of the UE when the UE enters or leaves RRC\_INACTIVE state.

**Interactions with PDU Session Resource Notify procedure:**

If the QoS related parameters (e.g. the *CN Packet Delay Budget Downlink* IE or the *CN Packet Delay Budget Uplink* IE) are included in the *Path Switch Request Acknowledge Transfer* IE of the PATH SWITCH REQUEST ACKNOWLEDGE message, but can not be succesfully accepted by the NG-RAN node, the NG-RAN node should continue to use the old values received from the source NG-RAN node, if any. The NG-RAN node shall, if supported, send the PDU SESSION RESOURCE NOTIFY message to notify the AMF.

**<Unchanged Text Omitted>**

## 8.10 NRPPa Transport Procedures

### 8.10.1 General

The purpose of the NRPPa Transport procedures is to carry NRPPa signalling (defined in TS 38.455 [19]) between the NG-RAN node and the LMF over the NG interface.

The Downlink UE Associated NRPPa Transport procedure and the Uplink UE Associated NRPPa Transport procedure use UE-associated signalling. The UE-associated signalling is used to support E-CID Location Information Transfer, Positioning Information Transfer, Measurement Preconfiguration Information Transfer, and Reporting of General Error Situations due to reception of an NRPPa message that utilized UE-associated signalling.

The Downlink Non UE Associated NRPPa Transport procedure and the Uplink Non UE Associated NRPPa Transport procedure use non-UE associated signalling. The non-UE associated signalling is used to support OTDOA Information Transfer, Assistance Information Transfer, TRP Information Transfer, Measurement Information Transfer, PRS Information Transfer, Area-specifc Information Transfer and Reporting of General Error Situations due to reception of an NRPPa message that utilized non-UE associated signalling.

**<Unchanged Text Omitted>**

### 9.2.2 UE Context Management Messages

#### 9.2.2.1 INITIAL CONTEXT SETUP REQUEST

This message is sent by the AMF to request the setup of a UE context.

Direction: AMF → NG-RAN node

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| AMF UE NGAP ID | M |  | 9.3.3.1 |  | YES | reject |
| RAN UE NGAP ID | M |  | 9.3.3.2 |  | YES | reject |
| Old AMF | O |  | AMF Name9.3.3.21 |  | YES | reject |
| UE Aggregate Maximum Bit Rate | C-ifPDUsessionResourceSetup |  | 9.3.1.58 |  | YES | reject |
| Core Network Assistance Information for RRC INACTIVE | O |  | 9.3.1.15 |  | YES | ignore |
| GUAMI | M |  | 9.3.3.3 |  | YES | reject |
| **PDU Session Resource Setup Request List** |  | *0..1* |  |  | YES | reject |
| **>PDU Session Resource Setup Request Item** |  | *1..<maxnoofPDUSessions>* |  |  | - |  |
| >>PDU Session ID | M |  | 9.3.1.50 |  | - |  |
| >>PDU Session NAS-PDU | O |  | NAS-PDU9.3.3.4 |  | - |  |
| >>S-NSSAI  | M |  | 9.3.1.24 |  | - |  |
| >>PDU Session Resource Setup Request Transfer | M |  | OCTET STRING | Containing the *PDU Session Resource Setup Request Transfer* IE specified in subclause 9.3.4.1. | - |  |
| >>PDU Session Expected UE Activity Behaviour | O |  | Expected UE Activity Behaviour9.3.1.94 | Expected UE Activity Behaviour for the PDU Session. | YES | ignore |
| Allowed NSSAI | M |  | 9.3.1.31 | Indicates the S-NSSAIs permitted by the network | YES | reject |
| UE Security Capabilities | M |  | 9.3.1.86 |  | YES | reject |
| Security Key | M |  | 9.3.1.87 |  | YES | reject |
| Trace Activation | O |  | 9.3.1.14 |  | YES | ignore |
| Mobility Restriction List | O |  | 9.3.1.85 |  | YES | ignore |
| UE Radio Capability | O |  | 9.3.1.74 |  | YES | ignore |
| Index to RAT/Frequency Selection Priority | O |  | 9.3.1.61 |  | YES | ignore |
| Masked IMEISV | O |  | 9.3.1.54 |  | YES | ignore |
| NAS-PDU | O |  | 9.3.3.4 |  | YES | ignore |
| Emergency Fallback Indicator | O |  | 9.3.1.26 |  | YES | reject |
| RRC Inactive Transition Report Request | O |  | 9.3.1.91 |  | YES | ignore |
| UE Radio Capability for Paging | O |  | 9.3.1.68 |  | YES | ignore |
| Redirection for Voice EPS Fallback  | O |  | 9.3.1.116 |  | YES | ignore |
| Location Reporting Request Type | O |  | 9.3.1.65 |  | YES | ignore |
| CN Assisted RAN Parameters Tuning | O |  | 9.3.1.119 |  | YES | ignore |
| SRVCC Operation Possible | O |  | 9.3.1.128 |  | YES | ignore |
| IAB Authorized | O |  | 9.3.1.129 |  | YES | ignore |
| Enhanced Coverage Restriction | O |  | 9.3.1.140 |  | YES | ignore |
| Extended Connected Time | O |  | 9.3.3.31 |  | YES | ignore |
| UE Differentiation Information | O |  | 9.3.1.144 |  | YES | ignore |
| NR V2X Services Authorized | O |  | 9.3.1.146 |  | YES | ignore |
| LTE V2X Services Authorized | O |  | 9.3.1.147 |  | YES | ignore |
| NR UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.3.1.148 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| LTE UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.3.1.149 | This IE applies only if the UE is authorized for LTE V2X services. | YES | ignore |
| PC5 QoS Parameters | O |  | 9.3.1.150 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| CE-mode-B Restricted | O |  | 9.3.1.155 |  | YES | ignore |
| UE User Plane CIoT Support Indicator | O |  | 9.3.1.160 |  | YES | ignore |
| RG Level Wireline Access Characteristics | O |  | OCTET STRING | Specified in TS 23.316 [34]. Indicates the wireline access technology specific QoS information corresponding to a specific wireline access subscription. | YES | ignore |
| Management Based MDT PLMN List | O |  | MDT PLMN List9.3.1.168 |  | YES | ignore |
| UE Radio Capability ID | O |  | 9.3.1.142 |  | YES | reject |
| Time Synchronisation Assistance Information | O |  | 9.3.1.220 |  | YES | ignore |
| QMC Configuration Information | O |  | 9.3.1.223 |  | YES | ignore |
| Target NSSAI Information | O |  | 9.3.1.229 |  | YES | ignore |
| UE Slice Maximum Bit Rate List | O |  | 9.3.1.231 |  | YES | ignore |
| 5G ProSe Authorized | O |  | 9.3.1.233 |  | YES | ignore |
| 5G ProSe UE PC5 Aggregate Maximum Bit Rate | O |  | NR UE Sidelink Aggregate Maximum Bit Rate9.3.1.148 | This IE applies only if the UE is authorized for 5G ProSe services. | YES | ignore |
| 5G ProSe PC5 QoS Parameters | O |  | 9.3.1.234 | This IE applies only if the UE is authorized for 5G ProSe services. | YES | ignore |
| Network Controlled Repeater Authorized | O |  | 9.3.1.245 |  | YES | ignore |
| Aerial UE Subscription Information | O |  | 9.3.1.246 |  | YES | ignore |
| NR A2X Services Authorized | O |  | 9.3.1.247 |  | YES | ignore |
| LTE A2X Services Authorized | O |  | 9.3.1.248 |  | YES | ignore |
| NR A2X UE PC5 Aggregate Maximum Bit Rate | O |  | NR UE Sidelink Aggregate Maximum Bit Rate9.3.1.148 | This IE applies only if the UE is authorized for NR A2X services. | YES | ignore |
| LTE A2X UE PC5 Aggregate Maximum Bit Rate | O |  | LTE UE Sidelink Aggregate Maximum Bit Rate9.3.1.149 | This IE applies only if the UE is authorized for LTE A2X services. | YES | ignore |
| A2X PC5 QoS Parameters | O |  | 9.3.1.249 | This IE applies only if the UE is authorized for A2X services. | YES | ignore |
| Mobile IAB Authorized | O |  | 9.3.1.259 |  | YES | ignore |
| Partially Allowed NSSAI | O |  | 9.3.1.261 | Indicates the S-NSSAIs partially permitted by the network. | YES | ignore |
| Ranging and Sidelink Positioning Service Information  | O |  | 9.3.1.xx1 | This IE applies only if the UE is authorized for NR V2X services and/or 5G ProSe services. | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofPDUSessions | Maximum no. of PDU sessions allowed towards one UE. Value is 256. |

|  |  |
| --- | --- |
| Condition | Explanation |
| ifPDUsessionResourceSetup | This IE shall be present if the *PDU Session Resource Setup List* IE is present. |

**<Unchanged Text Omitted>**

#### 9.2.2.7 UE CONTEXT MODIFICATION REQUEST

This message is sent by the AMF to provide UE Context information changes to the NG-RAN node.

Direction: AMF → NG-RAN node

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| AMF UE NGAP ID | M |  | 9.3.3.1 |  | YES | reject |
| RAN UE NGAP ID | M |  | 9.3.3.2 |  | YES | reject |
| RAN Paging Priority | O  |  | 9.3.3.15 |  | YES | ignore |
| Security Key | O |  | 9.3.1.87 |  | YES | reject |
| Index to RAT/Frequency Selection Priority | O |  | 9.3.1.61 |  | YES | ignore |
| UE Aggregate Maximum Bit Rate | O |  | 9.3.1.58 |  | YES | ignore |
| UE Security Capabilities | O |  | 9.3.1.86 |  | YES | reject |
| Core Network Assistance Information for RRC INACTIVE | O |  | 9.3.1.15 |  | YES | ignore |
| Emergency Fallback Indicator | O |  | 9.3.1.26 |  | YES | reject |
| New AMF UE NGAP ID | O |  | AMF UE NGAP ID9.3.3.1 |  | YES | reject |
| RRC Inactive Transition Report Request | O |  | 9.3.1.91 |  | YES | ignore |
| New GUAMI | O |  | GUAMI9.3.3.3 |  | YES | reject |
| CN Assisted RAN Parameters Tuning | O |  | 9.3.1.119 |  | YES | ignore |
| SRVCC Operation Possible | O |  | 9.3.1.128 |  | YES | ignore |
| IAB Authorized | O |  | 9.3.1.129 |  | YES | ignore |
| NR V2X Services Authorized | O |  | 9.3.1.146 |  | YES | ignore |
| LTE V2X Services Authorized | O |  | 9.3.1.147 |  | YES | ignore |
| NR UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.3.1.148 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| LTE UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.3.1.149 | This IE applies only if the UE is authorized for LTE V2X services. | YES | ignore |
| PC5 QoS Parameters | O |  | 9.3.1.150 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| UE Radio Capability ID | O |  | 9.3.1.142 |  | YES | reject |
| RG Level Wireline Access Characteristics | O |  | OCTET STRING | Specified in TS 23. 316 [34]. Indicates the wireline access technology specific QoS information corresponding to a specific wireline access subscription. | YES | ignore |
| Time Synchronisation Assistance Information | O |  | 9.3.1.220 |  | YES | ignore |
| QMC Configuration Information | O |  | 9.3.1.223 |  | YES | ignore |
| QMC Deactivation | O |  | 9.3.1.222 |  | YES | ignore |
| UE Slice Maximum Bit Rate List | O |  | 9.3.1.231 |  | YES | ignore |
| Management Based MDT PLMN Modification List | O |  | MDT PLMN Modification List9.3.1.243 |  | YES | ignore |
| 5G ProSe Authorized | O |  | 9.3.1.233 |  | YES | ignore |
| 5G ProSe UE PC5 Aggregate Maximum Bit Rate | O |  | NR UE Sidelink Aggregate Maximum Bit Rate9.3.1.148 | This IE applies only if the UE is authorized for 5G ProSe services. | YES | ignore |
| 5G ProSe PC5 QoS Parameters | O |  | 9.3.1.234 | This IE applies only if the UE is authorized for 5G ProSe services. | YES | ignore |
| Network Controlled Repeater Authorized | O |  | 9.3.1.245 |  | YES | ignore |
| Aerial UE Subscription Information | O |  | 9.3.1.246 |  | YES | ignore |
| NR A2X Services Authorized | O |  | 9.3.1.247 |  | YES | ignore |
| LTE A2X Services Authorized | O |  | 9.3.1.248 |  | YES | ignore |
| NR A2X UE PC5 Aggregate Maximum Bit Rate | O |  | NR UE Sidelink Aggregate Maximum Bit Rate9.3.1.148 | This IE applies only if the UE is authorized for NR A2X services. | YES | ignore |
| LTE A2X UE PC5 Aggregate Maximum Bit Rate | O |  | LTE UE Sidelink Aggregate Maximum Bit Rate9.3.1.149 | This IE applies only if the UE is authorized for LTE A2X services. | YES | ignore |
| A2X PC5 QoS Parameters | O |  | 9.3.1.249 | This IE applies only if the UE is authorized for A2X services. | YES | ignore |
| Mobile IAB Authorized | O |  | 9.3.1.259 |  | YES | ignore |
| Ranging and Sidelink Positioning Service Information  | O |  | 9.3.1.xx1 | This IE applies only if the UE is authorized for NR V2X services and/or 5G ProSe services. | YES | ignore |

**<Unchanged Text Omitted>**

#### 9.2.3.4 HANDOVER REQUEST

This message is sent by the AMF to the target NG-RAN node to request the preparation of resources.

Direction: AMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| AMF UE NGAP ID | M |  | 9.3.3.1 |  | YES | reject |
| Handover Type | M |  | 9.3.1.22 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| UE Aggregate Maximum Bit Rate | M |  | 9.3.1.58 |  | YES | reject |
| Core Network Assistance Information for RRC INACTIVE | O |  | 9.3.1.15 |  | YES | ignore |
| UE Security Capabilities  | M |  | 9.3.1.86 |  | YES | reject |
| Security Context | M |  | 9.3.1.88 |  | YES | reject |
| New Security Context Indicator | O |  | 9.3.1.55 |  | YES | reject |
| NASC | O |  | NAS-PDU9.3.3.4 | Refers to either the “Intra N1 mode NAS transparent container” or the “S1 mode to N1 mode NAS transparent container”, the details of the IE definition and the encoding arespecified in TS 24.501 [26]. | YES | reject |
| **PDU Session Resource Setup List** |  | *1* |  |  | YES | reject |
| **>PDU Session Resource Setup Item** |  | *1..<maxnoofPDUSessions>* |  |  | - |  |
| >>PDU Session ID  | M |  | 9.3.1.50 |  | - |  |
| >>S-NSSAI | M |  | 9.3.1.24 |  | - |  |
| >>Handover Request Transfer | M |  | OCTET STRING | Containing the *PDU Session Resource Setup Request Transfer* IE specified in subclause 9.3.4.1. | - |  |
| >>PDU Session Expected UE Activity Behaviour | O |  | Expected UE Activity Behaviour9.3.1.94 | Expected UE Activity Behaviour for the PDU Session. | YES | ignore |
| Allowed NSSAI | M |  | 9.3.1.31 | Indicates the S-NSSAIs permitted by the network. | YES | reject |
| Trace Activation | O |  | 9.3.1.14 |  | YES | ignore |
| Masked IMEISV | O |  | 9.3.1.54 |  | YES | ignore |
| Source to Target Transparent Container | M |  | 9.3.1.20 |  | YES | reject |
| Mobility Restriction List | O |  | 9.3.1.85 |  | YES | ignore |
| Location Reporting Request Type | O |  | 9.3.1.65 |  | YES | ignore |
| RRC Inactive Transition Report Request | O |  | 9.3.1.91 |  | YES | ignore |
| GUAMI | M |  | 9.3.3.3 |  | YES | reject |
| Redirection for Voice EPS Fallback  | O |  | 9.3.1.116 |  | YES | ignore |
| CN Assisted RAN Parameters Tuning | O |  | 9.3.1.119 |  | YES | ignore |
| SRVCC Operation Possible | O |  | 9.3.1.128 |  | YES | ignore |
| IAB Authorized | O |  | 9.3.1.129 |  | YES | reject |
| Enhanced Coverage Restriction | O |  | 9.3.1.140 |  | YES | ignore |
| UE Differentiation Information | O |  | 9.3.1.144 |  | YES | ignore |
| NR V2X Services Authorized | O |  | 9.3.1.146 |  | YES | ignore |
| LTE V2X Services Authorized | O |  | 9.3.1.147 |  | YES | ignore |
| NR UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.3.1.148 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| LTE UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.3.1.149 | This IE applies only if the UE is authorized for LTE V2X services. | YES | ignore |
| PC5 QoS Parameters | O |  | 9.3.1.150 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| CE-mode-B Restricted | O |  | 9.3.1.155 |  | YES | ignore |
| UE User Plane CIoT Support Indicator | O |  | 9.3.1.160 |  | YES | ignore |
| Management Based MDT PLMN List | O |  | MDT PLMN List9.3.1.168 |  | YES | ignore |
| UE Radio Capability ID | O |  | 9.3.1.142 |  | YES | reject |
| Extended Connected Time | O |  | 9.3.3.31 |  | YES | ignore |
| Time Synchronisation Assistance Information | O |  | 9.3.1.220 |  | YES | ignore |
| UE Slice Maximum Bit Rate List | O |  | 9.3.1.231 |  | YES | ignore |
| 5G ProSe Authorized | O |  | 9.3.1.233 |  | YES | ignore |
| 5G ProSe UE PC5 Aggregate Maximum Bit Rate | O |  | NR UE Sidelink Aggregate Maximum Bit Rate9.3.1.148 | This IE applies only if the UE is authorized for 5G ProSe services. | YES | ignore |
| 5G ProSe PC5 QoS Parameters | O |  | 9.3.1.234 | This IE applies only if the UE is authorized for 5G ProSe services. | YES | ignore |
| Aerial UE Subscription Information | O |  | 9.3.1.246 |  | YES | ignore |
| NR A2X Services Authorized | O |  | 9.3.1.247 |  | YES | ignore |
| LTE A2X Services Authorized | O |  | 9.3.1.248 |  | YES | ignore |
| NR A2X UE PC5 Aggregate Maximum Bit Rate | O |  | NR UE Sidelink Aggregate Maximum Bit Rate9.3.1.148 | This IE applies only if the UE is authorized for NR A2X services. | YES | ignore |
| LTE A2X UE PC5 Aggregate Maximum Bit Rate | O |  | LTE UE Sidelink Aggregate Maximum Bit Rate9.3.1.149 | This IE applies only if the UE is authorized for LTE A2X services. | YES | ignore |
| A2X PC5 QoS Parameters | O |  | 9.3.1.249 | This IE applies only if the UE is authorized for A2X services. | YES | ignore |
| Mobile IAB Authorized | O |  | 9.3.1.259 |  | YES | ignore |
| No PDU Session Indication | O |  | ENUMERATED (true, ...) | This IE applies only if the UE is a mobile IAB-MT. | YES | ignore |
| Partially Allowed NSSAI | O |  | 9.3.1.261 | Indicates the S-NSSAIs partially permitted by the network. | YES | ignore |
| Ranging and Sidelink Positioning Service Information  | O |  | 9.3.1.xx1 | This IE applies only if the UE is authorized for NR V2X services and/or 5G ProSe services. | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofPDUSessions | Maximum no. of PDU sessions allowed towards one UE. Value is 256. |

**<Unchanged Text Omitted>**

#### 9.2.3.9 PATH SWITCH REQUEST ACKNOWLEDGE

This message is sent by the AMF to inform the NG-RAN node that the path switch has been successfully completed in the 5GC.

Direction: AMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| AMF UE NGAP ID | M |  | 9.3.3.1 |  | YES | ignore |
| RAN UE NGAP ID | M |  | 9.3.3.2 |  | YES | ignore |
| UE Security Capabilities | O |  | 9.3.1.86 |  | YES | reject |
| Security Context | M |  | 9.3.1.88 |  | YES | reject |
| New Security Context Indicator | O |  | 9.3.1.55 |  | YES | reject |
| **PDU Session Resource Switched List** |  | *1*  |  |  | YES | ignore |
| **>PDU Session Resource Switched Item** |  | *1..<maxnoofPDUSessions>*  |  |  | - |  |
| >>PDU Session ID  | M |  | 9.3.1.50 |  | - |  |
| >>Path Switch Request Acknowledge Transfer | M |  | OCTET STRING | Containing the *Path Switch Request Acknowledge Transfer* IE specified in subclause 9.3.4.9. | - |  |
| >>PDU Session Expected UE Activity Behaviour | O |  | Expected UE Activity Behaviour9.3.1.94 | Expected UE Activity Behaviour for the PDU Session. | YES | ignore |
| **PDU Session Resource Released List** |  | *0..1* |  |  | YES | ignore |
| **>PDU Session Resource Released Item** |  | *1..<maxnoofPDUSessions>* |  |  | - |  |
| >>PDU Session ID | M |  | 9.3.1.50 |  | - |  |
| >>Path Switch Request Unsuccessful Transfer | M |  | OCTET STRING | Containing the *Path Switch Request Unsuccessful Transfer* IE specified in subclause 9.3.4.20. | - |  |
| Allowed NSSAI | M |  | 9.3.1.31 | Indicates the S-NSSAIs permitted by the network. | YES | reject |
| Core Network Assistance Information for RRC INACTIVE | O |  | 9.3.1.15 |  | YES | ignore |
| RRC Inactive Transition Report Request | O |  | 9.3.1.91 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |
| Redirection for Voice EPS Fallback  | O |  | 9.3.1.116 |  | YES | ignore |
| CN Assisted RAN Parameters Tuning | O |  | 9.3.1.119 |  | YES | ignore |
| SRVCC Operation Possible | O |  | 9.3.1.128 |  | YES | ignore |
| Enhanced Coverage Restriction | O |  | 9.3.1.140 |  | YES | ignore |
| Extended Connected Time | O |  | 9.3.3.31 |  | YES | ignore |
| UE Differentiation Information | O |  | 9.3.1.144 |  | YES | ignore |
| NR V2X Services Authorized | O |  | 9.3.1.146 |  | YES | ignore |
| LTE V2X Services Authorized | O |  | 9.3.1.147 |  | YES | ignore |
| NR UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.3.1.148 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| LTE UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.3.1.149 | This IE applies only if the UE is authorized for LTE V2X services. | YES | ignore |
| PC5 QoS Parameters | O |  | 9.3.1.150 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| CE-mode-B Restricted | O |  | 9.3.1.155 |  | YES | ignore |
| UE User Plane CIoT Support Indicator | O |  | 9.3.1.160 |  | YES | ignore |
| UE Radio Capability ID | O |  | 9.3.1.142 |  | YES | reject |
| Management Based MDT PLMN List | O |  | MDT PLMN List9.3.1.168 | This IE is ignored if the *Management Based MDT PLMN Modification List* IE is present. | YES | ignore |
| Time Synchronisation Assistance Information | O |  | 9.3.1.220 |  | YES | ignore |
| 5G ProSe Authorized | O |  | 9.3.1.233 |  | YES | ignore |
| 5G ProSe UE PC5 Aggregate Maximum Bit Rate | O |  | NR UE Sidelink Aggregate Maximum Bit Rate9.3.1.148 | This IE applies only if the UE is authorized for 5G ProSe services. | YES | ignore |
| 5G ProSe PC5 QoS Parameters | O |  | 9.3.1.234 | This IE applies only if the UE is authorized for 5G ProSe services. | YES | ignore |
| Management Based MDT PLMN Modification List | O |  | MDT PLMN Modification List9.3.1.243 |  | YES | ignore |
| IAB Authorized | O |  | 9.3.1.129 |  | YES | ignore |
| Aerial UE Subscription Information | O |  | 9.3.1.246 |  | YES | ignore |
| NR A2X Services Authorized | O |  | 9.3.1.247 |  | YES | ignore |
| LTE A2X Services Authorized | O |  | 9.3.1.248 |  | YES | ignore |
| NR A2X UE PC5 Aggregate Maximum Bit Rate | O |  | NR UE Sidelink Aggregate Maximum Bit Rate9.3.1.148 | This IE applies only if the UE is authorized for NR A2X services. | YES | ignore |
| LTE A2X UE PC5 Aggregate Maximum Bit Rate | O |  | LTE UE Sidelink Aggregate Maximum Bit Rate9.3.1.149 | This IE applies only if the UE is authorized for LTE A2X services. | YES | ignore |
| A2X PC5 QoS Parameters | O |  | 9.3.1.249 | This IE applies only if the UE is authorized for A2X services. | YES | ignore |
| Mobile IAB Authorized | O |  | 9.3.1.259 |  | YES | ignore |
| Partially Allowed NSSAI | O |  | 9.3.1.261 | Indicates the S-NSSAIs partially permitted by the network. | YES | ignore |
| Ranging and Sidelink Positioning Service Information | O |  | 9.3.1.xx1 | This IE applies only if the UE is authorized for NR V2X services and/or 5G ProSe services. | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofPDUSessions | Maximum no. of PDU sessions allowed towards one UE. Value is 256. |

**<Unchanged Text Omitted>**

## 9.3 Information Element Definitions

**<Unchanged Text Omitted>**

#### 9.3.1.xx1 Ranging and Sidelink Positioning Service Information

This IE provides information on the UE for Ranging and Sidelink Positioning service.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Ranging and Sidelink Positioning Authorized | M |  | ENUMERATED (authorized, not authorized, ...) | This IE indicates whether the UE is authorized to use RSPP communication resources and SL-PRS resources. |
| RSPP Transport QoS Parameters | O |  | 9.3.1.xx2 | This IE applies only if the UE is authorized for Ranging and Sidelink Positioning service. |

#### 9.3.1.xx2 RSPP Transport QoS Parameters

This IE provides information on the RSPP transport QoS parameters.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **RSPP Transport QoS Flow List** |  | *1* |  |  |
| **>RSPP Transport QoS Flow Item** |  | *1..<maxnoofRSPPQoSFlows>* |  |  |
| >>PQI | M |  | INTEGER (0..255, …) | PQI is a special 5QI as specified in TS 23.501 [9]. |
| **>>RSPP Transport Bit Rates** |  | *0..1* |  | Only applies for GBR QoS flows. |
| >>>Guaranteed Flow Bit Rate | M |  | Bit Rate9.3.1.4 | Guaranteed Bit Rate for the RSPP QoS flow. Details in TS 23.501 [9]. |
| >>>Maximum Flow Bit Rate | M |  | Bit Rate9.3.1.4 | Maximum Bit Rate for the RSPP QoS flow. Details in TS 23.501 [9]. |
| >>Range | O |  | ENUMERATED (m50, m80, m180, m200, m350, m400, m500, m700, m1000, …) | Only applies for groupcast. |
| RSPP Transport Link Aggregate Bit Rates | O |  | Bit Rate9.3.1.4 | Only applies for Non-GBR QoS flows. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| *maxnoofRSPPQoSFlows* | Maximum no. of RSPP QoS flows allowed towards one UE. Value is 2048. |

**<Unchanged Text Omitted>**

###

### 9.4.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for NGAP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGAP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 A2X-PC5-QoS-Parameters,

 AerialUEsubscriptionInformation,

 AllowedNSSAI,

 AMFName,

 AMFSetID,

 AMF-TNLAssociationSetupList,

 AMF-TNLAssociationToAddList,

 AMF-TNLAssociationToRemoveList,

 AMF-TNLAssociationToUpdateList,

 AMF-UE-NGAP-ID,

 AssistanceDataForPaging,

 AssociatedSessionID,

 AuthenticatedIndication,

 BroadcastCancelledAreaList,

 BroadcastCompletedAreaList,

 BroadcastTransportFailureTransfer,

 BroadcastTransportRequestTransfer,

 BroadcastTransportResponseTransfer,

 CancelAllWarningMessages,

 Cause,

 CellIDListForRestart,

 CEmodeBrestricted,

 CEmodeBSupport-Indicator,

 CNAssistedRANTuning,

 ConcurrentWarningMessageInd,

 CoreNetworkAssistanceInformationForInactive,

 CPTransportLayerInformation,

 CriticalityDiagnostics,

 DataCodingScheme,

 DirectForwardingPathAvailability,

 DL-CP-SecurityInformation,

 DL-Signalling,

 EarlyStatusTransfer-TransparentContainer,

 EDT-Session,

 EmergencyAreaIDListForRestart,

 EmergencyFallbackIndicator,

 EN-DCSONConfigurationTransfer,

 EndIndication,

 Enhanced-CoverageRestriction,

 EUTRA-CGI,

 EUTRA-PagingeDRXInformation,

 Extended-AMFName,

 Extended-ConnectedTime,

 Extended-RANNodeName,

 FiveGCAction,

 FiveG-ProSeAuthorized,

 FiveG-ProSePC5QoSParameters,

 FiveG-S-TMSI,

 GlobalRANNodeID,

 GUAMI,

 HandoverFlag,

 HandoverType,

 IAB-Authorized,

 IABNodeIndication,

 IAB-Supported,

 IMSVoiceSupportIndicator,

 IndexToRFSP,

 InfoOnRecommendedCellsAndRANNodesForPaging,

 IntersystemSONConfigurationTransfer,

 LAI,

 LocationReportingRequestType,

 LTE-A2X-ServicesAuthorized,

 LTEM-Indication,

 LTEUESidelinkAggregateMaximumBitrate,

 LTEV2XServicesAuthorized,

 MaskedIMEISV,

 MBS-AreaSessionID,

 MBS-DistributionReleaseRequestTransfer,

 MBS-DistributionSetupRequestTransfer,

 MBS-DistributionSetupResponseTransfer,

 MBS-DistributionSetupUnsuccessfulTransfer,

 MBS-ServiceArea,

 MBS-SessionID,

 MBSSessionReleaseResponseTransfer,

 MBSSessionSetupOrModFailureTransfer,

 MBSSessionSetupOrModRequestTransfer,

 MBSSessionSetupOrModResponseTransfer,

 MDTPLMNList,

 MDTPLMNModificationList,

 MessageIdentifier,

 MobileIAB-Authorized,

 MobileIABNodeIndication,

 MobileIAB-Supported,

 MobilityRestrictionList,

 MulticastGroupPagingAreaList,

 MulticastSessionActivationRequestTransfer,

 MulticastSessionDeactivationRequestTransfer,

 MulticastSessionUpdateRequestTransfer,

 NAS-PDU,

 NASSecurityParametersFromNGRAN,

 NB-IoT-DefaultPagingDRX,

 NB-IoT-PagingDRX,

 NB-IoT-Paging-eDRXInfo,

 NB-IoT-UEPriority,

 NetworkControlledRepeaterAuthorized,

 NewSecurityContextInd,

 NGRAN-CGI,

 NGRAN-TNLAssociationToRemoveList,

 NGRANTraceID,

 NID,

 NoPDUSessionIndication,

 NotifySourceNGRANNode,

 NPN-AccessInformation,

 NR-A2X-ServicesAuthorized,

 NR-CGI,

 NR-PagingeDRXInformation,

 NRPPa-PDU,

 NRUESidelinkAggregateMaximumBitrate,

 NRV2XServicesAuthorized,

 NumberOfBroadcastsRequested,

 OverloadResponse,

 OverloadStartNSSAIList,

 PagingAssisDataforCEcapabUE,

 PagingCause,

 PagingDRX,

 PagingOrigin,

 PagingPolicyDifferentiation,

 PagingPriority,

 Partially-Allowed-NSSAI,

 PC5QoSParameters,

 PDUSessionAggregateMaximumBitRate,

 PDUSessionResourceAdmittedList,

 PDUSessionResourceFailedToModifyListModCfm,

 PDUSessionResourceFailedToModifyListModRes,

 PDUSessionResourceFailedToResumeListRESReq,

 PDUSessionResourceFailedToResumeListRESRes,

 PDUSessionResourceFailedToSetupListCxtFail,

 PDUSessionResourceFailedToSetupListCxtRes,

 PDUSessionResourceFailedToSetupListHOAck,

 PDUSessionResourceFailedToSetupListPSReq,

 PDUSessionResourceFailedToSetupListSURes,

 PDUSessionResourceHandoverList,

 PDUSessionResourceListCxtRelCpl,

 PDUSessionResourceListCxtRelReq,

 PDUSessionResourceListHORqd,

 PDUSessionResourceModifyListModCfm,

 PDUSessionResourceModifyListModInd,

 PDUSessionResourceModifyListModReq,

 PDUSessionResourceModifyListModRes,

 PDUSessionResourceNotifyList,

 PDUSessionResourceReleasedListNot,

 PDUSessionResourceReleasedListPSAck,

 PDUSessionResourceReleasedListPSFail,

 PDUSessionResourceReleasedListRelRes,

 PDUSessionResourceResumeListRESReq,

 PDUSessionResourceResumeListRESRes,

 PDUSessionResourceSecondaryRATUsageList,

 PDUSessionResourceSetupListCxtReq,

 PDUSessionResourceSetupListCxtRes,

 PDUSessionResourceSetupListHOReq,

 PDUSessionResourceSetupListSUReq,

 PDUSessionResourceSetupListSURes,

 PDUSessionResourceSuspendListSUSReq,

 PDUSessionResourceSwitchedList,

 PDUSessionResourceToBeSwitchedDLList,

 PDUSessionResourceToReleaseListHOCmd,

 PDUSessionResourceToReleaseListRelCmd,

 PEIPSassistanceInformation,

 PLMNIdentity,

 PLMNSupportList,

 PrivacyIndicator,

 PWSFailedCellIDList,

 QMCConfigInfo,

 QMCDeactivation,

 RANNodeName,

 RANPagingPriority,

 RANStatusTransfer-TransparentContainer,

 RANTimingSynchronisationStatusInfo,

 RAN-TSSRequestType,

 RAN-TSSScope,

 RAN-UE-NGAP-ID,

 RedCapIndication,

 RedirectionVoiceFallback,

 RelativeAMFCapacity,

 RepetitionPeriod,

 ResetType,

 RGLevelWirelineAccessCharacteristics,

 RIMInformationTransfer,

 RoutingID,

 RRCEstablishmentCause,

 RRCInactiveTransitionReportRequest,

 RRCState,

 SecurityContext,

 SecurityKey,

 SerialNumber,

 ServedGUAMIList,

 SliceSupportList,

 SLPositioningRangingServiceInfo,

 S-NSSAI,

 SONConfigurationTransfer,

 SourceToTarget-AMFInformationReroute,

 SourceToTarget-TransparentContainer,

 SRVCCOperationPossible,

 SupportedTAList,

 Suspend-Request-Indication,

 Suspend-Response-Indication,

 TAI,

 TAIListForPaging,

 TAIListForRestart,

 TargetID,

 TargetNSSAIInformation,

 TargettoSource-Failure-TransparentContainer,

 TargetToSource-TransparentContainer,

 TimeSyncAssistanceInfo,

 TimeToWait,

 TNLAssociationList,

 TraceActivation,

 TrafficLoadReductionIndication,

 TransportLayerAddress,

 UEAggregateMaximumBitRate,

 UE-associatedLogicalNG-connectionList,

 UECapabilityInfoRequest,

 UEContextRequest,

 UE-DifferentiationInfo,

 UE-NGAP-IDs,

 UEPagingIdentity,

 UEPresenceInAreaOfInterestList,

 UERadioCapability,

 UERadioCapabilityForPaging,

 UERadioCapabilityID,

 UERetentionInformation,

 UESecurityCapabilities,

 UESliceMaximumBitRateList,

 UE-UP-CIoT-Support,

 UL-CP-SecurityInformation,

 UnavailableGUAMIList,

 URI-address,

 UserLocationInformation,

 WarningAreaCoordinates,

 WarningAreaList,

 WarningMessageContents,

 WarningSecurityInfo,

 WarningType,

 WUS-Assistance-Information

FROM NGAP-IEs

 PrivateIE-Container{},

 ProtocolExtensionContainer{},

 ProtocolIE-Container{},

 ProtocolIE-ContainerList{},

 ProtocolIE-ContainerPair{},

 ProtocolIE-SingleContainer{},

 NGAP-PRIVATE-IES,

 NGAP-PROTOCOL-EXTENSION,

 NGAP-PROTOCOL-IES,

 NGAP-PROTOCOL-IES-PAIR

FROM NGAP-Containers

 id-A2X-PC5-QoS-Parameters,

 id-AerialUEsubscriptionInformation,

 id-AllowedNSSAI,

 id-AMFName,

 id-AMFOverloadResponse,

 id-AMFSetID,

 id-AMF-TNLAssociationFailedToSetupList,

 id-AMF-TNLAssociationSetupList,

 id-AMF-TNLAssociationToAddList,

 id-AMF-TNLAssociationToRemoveList,

 id-AMF-TNLAssociationToUpdateList,

 id-AMFTrafficLoadReductionIndication,

 id-AMF-UE-NGAP-ID,

 id-AssistanceDataForPaging,

 id-AssociatedSessionID,

 id-AuthenticatedIndication,

 id-BroadcastCancelledAreaList,

 id-BroadcastCompletedAreaList,

 id-BroadcastTransportFailureTransfer,

 id-BroadcastTransportRequestTransfer,

 id-BroadcastTransportResponseTransfer,

 id-CancelAllWarningMessages,

 id-Cause,

 id-CellIDListForRestart,

 id-CEmodeBrestricted,

 id-CEmodeBSupport-Indicator,

 id-CNAssistedRANTuning,

 id-ConcurrentWarningMessageInd,

 id-CoreNetworkAssistanceInformationForInactive,

 id-CriticalityDiagnostics,

 id-DataCodingScheme,

 id-DefaultPagingDRX,

 id-DirectForwardingPathAvailability,

 id-DL-CP-SecurityInformation,

 id-DL-Signalling,

 id-EarlyStatusTransfer-TransparentContainer,

 id-EDT-Session,

 id-EmergencyAreaIDListForRestart,

 id-EmergencyFallbackIndicator,

 id-ENDC-SONConfigurationTransferDL,

 id-ENDC-SONConfigurationTransferUL,

 id-EndIndication,

 id-Enhanced-CoverageRestriction,

 id-EUTRA-CGI,

 id-EUTRA-PagingeDRXInformation,

 id-Extended-AMFName,

 id-Extended-ConnectedTime,

 id-Extended-RANNodeName,

 id-FiveGCAction,

 id-FiveG-ProSeAuthorized,

 id-FiveG-ProSePC5QoSParameters,

 id-FiveG-ProSeUEPC5AggregateMaximumBitRate,

 id-FiveG-S-TMSI,

 id-GlobalRANNodeID,

 id-GUAMI,

 id-HandoverFlag,

 id-HandoverType,

 id-IAB-Authorized,

 id-IABNodeIndication,

 id-IAB-Supported,

 id-IMSVoiceSupportIndicator,

 id-IndexToRFSP,

 id-InfoOnRecommendedCellsAndRANNodesForPaging,

 id-IntersystemSONConfigurationTransferDL,

 id-IntersystemSONConfigurationTransferUL,

 id-LocationReportingRequestType,

 id-LTE-A2X-ServicesAuthorized,

 id-LTE-A2X-UE-PC5-AggregateMaximumBitRate,

 id-LTEM-Indication,

 id-LTEUESidelinkAggregateMaximumBitrate,

 id-LTEV2XServicesAuthorized,

 id-ManagementBasedMDTPLMNList,

 id-ManagementBasedMDTPLMNModificationList,

 id-MaskedIMEISV,

 id-MBS-AreaSessionID,

 id-MBS-DistributionReleaseRequestTransfer,

 id-MBS-DistributionSetupRequestTransfer,

 id-MBS-DistributionSetupResponseTransfer,

 id-MBS-DistributionSetupUnsuccessfulTransfer,

 id-MBS-ServiceArea,

 id-MBS-SessionID,

 id-MBSSessionModificationFailureTransfer,

 id-MBSSessionModificationRequestTransfer,

 id-MBSSessionModificationResponseTransfer,

 id-MBSSessionReleaseResponseTransfer,

 id-MBSSessionSetupFailureTransfer,

 id-MBSSessionSetupRequestTransfer,

 id-MBSSessionSetupResponseTransfer,

 id-MessageIdentifier,

 id-MobileIAB-Authorized,

 id-MobileIABNodeIndication,

 id-MobileIAB-Supported,

 id-MobilityRestrictionList,

 id-MulticastGroupPagingAreaList,

 id-MulticastSessionActivationRequestTransfer,

 id-MulticastSessionDeactivationRequestTransfer,

 id-MulticastSessionUpdateRequestTransfer,

 id-NASC,

 id-NAS-PDU,

 id-NASSecurityParametersFromNGRAN,

 id-NB-IoT-DefaultPagingDRX,

 id-NB-IoT-PagingDRX,

 id-NB-IoT-Paging-eDRXInfo,

 id-NB-IoT-UEPriority,

 id-NetworkControlledRepeaterAuthorized,

 id-NewAMF-UE-NGAP-ID,

 id-NewGUAMI,

 id-NewSecurityContextInd,

 id-NGAP-Message,

 id-NGRAN-CGI,

 id-NGRAN-TNLAssociationToRemoveList,

 id-NGRANTraceID,

 id-NoPDUSessionIndication,

 id-NotifySourceNGRANNode,

 id-NPN-AccessInformation,

 id-NR-A2X-ServicesAuthorized,

 id-NR-A2X-UE-PC5-AggregateMaximumBitRate,

 id-NR-PagingeDRXInformation,

 id-NRPPa-PDU,

 id-NRUESidelinkAggregateMaximumBitrate,

 id-NRV2XServicesAuthorized,

 id-NumberOfBroadcastsRequested,

 id-OldAMF,

 id-OverloadStartNSSAIList,

 id-PagingAssisDataforCEcapabUE,

 id-PagingCause,

 id-PagingDRX,

 id-PagingOrigin,

 id-PagingPolicyDifferentiation,

 id-PagingPriority,

 id-Partially-Allowed-NSSAI,

 id-PC5QoSParameters,

 id-PDUSessionResourceAdmittedList,

 id-PDUSessionResourceFailedToModifyListModCfm,

 id-PDUSessionResourceFailedToModifyListModRes,

 id-PDUSessionResourceFailedToResumeListRESReq,

 id-PDUSessionResourceFailedToResumeListRESRes,

 id-PDUSessionResourceFailedToSetupListCxtFail,

 id-PDUSessionResourceFailedToSetupListCxtRes,

 id-PDUSessionResourceFailedToSetupListHOAck,

 id-PDUSessionResourceFailedToSetupListPSReq,

 id-PDUSessionResourceFailedToSetupListSURes,

 id-PDUSessionResourceHandoverList,

 id-PDUSessionResourceListCxtRelCpl,

 id-PDUSessionResourceListCxtRelReq,

 id-PDUSessionResourceListHORqd,

 id-PDUSessionResourceModifyListModCfm,

 id-PDUSessionResourceModifyListModInd,

 id-PDUSessionResourceModifyListModReq,

 id-PDUSessionResourceModifyListModRes,

 id-PDUSessionResourceNotifyList,

 id-PDUSessionResourceReleasedListNot,

 id-PDUSessionResourceReleasedListPSAck,

 id-PDUSessionResourceReleasedListPSFail,

 id-PDUSessionResourceReleasedListRelRes,

 id-PDUSessionResourceResumeListRESReq,

 id-PDUSessionResourceResumeListRESRes,

 id-PDUSessionResourceSecondaryRATUsageList,

 id-PDUSessionResourceSetupListCxtReq,

 id-PDUSessionResourceSetupListCxtRes,

 id-PDUSessionResourceSetupListHOReq,

 id-PDUSessionResourceSetupListSUReq,

 id-PDUSessionResourceSetupListSURes,

 id-PDUSessionResourceSuspendListSUSReq,

 id-PDUSessionResourceSwitchedList,

 id-PDUSessionResourceToBeSwitchedDLList,

 id-PDUSessionResourceToReleaseListHOCmd,

 id-PDUSessionResourceToReleaseListRelCmd,

 id-PEIPSassistanceInformation,

 id-PLMNSupportList,

 id-PrivacyIndicator,

 id-PWSFailedCellIDList,

 id-QMCConfigInfo,

 id-QMCDeactivation,

 id-RANNodeName,

 id-RANPagingPriority,

 id-RANStatusTransfer-TransparentContainer,

 id-RANTimingSynchronisationStatusInfo,

 id-RAN-TSSRequestType,

 id-RAN-TSSScope,

 id-RAN-UE-NGAP-ID,

 id-RedCapIndication,

 id-RedirectionVoiceFallback,

 id-RelativeAMFCapacity,

 id-RepetitionPeriod,

 id-ResetType,

 id-RGLevelWirelineAccessCharacteristics,

 id-RIMInformationTransfer,

 id-RoutingID,

 id-RRCEstablishmentCause,

 id-RRCInactiveTransitionReportRequest,

 id-RRC-Resume-Cause,

 id-RRCState,

 id-SecurityContext,

 id-SecurityKey,

 id-SelectedNID,

 id-SelectedPLMNIdentity,

 id-SerialNumber,

 id-ServedGUAMIList,

 id-SliceSupportList,

 id-S-NSSAI,

 id-SONConfigurationTransferDL,

 id-SONConfigurationTransferUL,

 id-SourceAMF-UE-NGAP-ID,

 id-SourceToTarget-AMFInformationReroute,

 id-SourceToTarget-TransparentContainer,

 id-SRVCCOperationPossible,

 id-SupportedTAList,

 id-Suspend-Request-Indication,

 id-Suspend-Response-Indication,

 id-TAI,

 id-TAIListForPaging,

 id-TAIListForRestart,

 id-TargetID,

 id-TargetNSSAIInformation,

 id-TargettoSource-Failure-TransparentContainer,

 id-TargetToSource-TransparentContainer,

 id-TimeSyncAssistanceInfo,

 id-TimeToWait,

 id-TNGFIdentityInformation,

 id-TraceActivation,

 id-TraceCollectionEntityIPAddress,

 id-TraceCollectionEntityURI,

 id-TWIFIdentityInformation,

 id-UEAggregateMaximumBitRate,

 id-UE-associatedLogicalNG-connectionList,

 id-UECapabilityInfoRequest,

 id-UEContextRequest,

 id-UE-DifferentiationInfo,

 id-UE-NGAP-IDs,

 id-UEPagingIdentity,

 id-UEPresenceInAreaOfInterestList,

 id-UERadioCapability,

 id-UERadioCapability-EUTRA-Format,

 id-UERadioCapabilityForPaging,

 id-UERadioCapabilityID,

 id-UERetentionInformation,

 id-UESecurityCapabilities,

 id-UESliceMaximumBitRateList,

 id-UE-UP-CIoT-Support,

 id-UL-CP-SecurityInformation,

 id-UnavailableGUAMIList,

 id-UserLocationInformation,

 id-W-AGFIdentityInformation,

 id-WarningAreaCoordinates,

 id-WarningAreaList,

 id-WarningMessageContents,

 id-WarningSecurityInfo,

 id-WarningType,

 id-WUS-Assistance-Information,

 id-SLPositioningRangingServiceInfo

**<Unchanged Text Omitted>**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- INITIAL CONTEXT SETUP REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

InitialContextSetupRequest ::= SEQUENCE {

 protocolIEs ProtocolIE-Container { {InitialContextSetupRequestIEs} },

 ...

}

InitialContextSetupRequestIEs NGAP-PROTOCOL-IES ::= {

 { ID id-AMF-UE-NGAP-ID CRITICALITY reject TYPE AMF-UE-NGAP-ID PRESENCE mandatory }|

 { ID id-RAN-UE-NGAP-ID CRITICALITY reject TYPE RAN-UE-NGAP-ID PRESENCE mandatory }|

 { ID id-OldAMF CRITICALITY reject TYPE AMFName PRESENCE optional }|

 { ID id-UEAggregateMaximumBitRate CRITICALITY reject TYPE UEAggregateMaximumBitRate PRESENCE conditional }|

 { ID id-CoreNetworkAssistanceInformationForInactive CRITICALITY ignore TYPE CoreNetworkAssistanceInformationForInactive PRESENCE optional }|

 { ID id-GUAMI CRITICALITY reject TYPE GUAMI PRESENCE mandatory }|

 { ID id-PDUSessionResourceSetupListCxtReq CRITICALITY reject TYPE PDUSessionResourceSetupListCxtReq PRESENCE optional }|

 { ID id-AllowedNSSAI CRITICALITY reject TYPE AllowedNSSAI PRESENCE mandatory }|

 { ID id-UESecurityCapabilities CRITICALITY reject TYPE UESecurityCapabilities PRESENCE mandatory }|

 { ID id-SecurityKey CRITICALITY reject TYPE SecurityKey PRESENCE mandatory }|

 { ID id-TraceActivation CRITICALITY ignore TYPE TraceActivation PRESENCE optional }|

 { ID id-MobilityRestrictionList CRITICALITY ignore TYPE MobilityRestrictionList PRESENCE optional }|

 { ID id-UERadioCapability CRITICALITY ignore TYPE UERadioCapability PRESENCE optional }|

 { ID id-IndexToRFSP CRITICALITY ignore TYPE IndexToRFSP PRESENCE optional }|

 { ID id-MaskedIMEISV CRITICALITY ignore TYPE MaskedIMEISV PRESENCE optional }|

 { ID id-NAS-PDU CRITICALITY ignore TYPE NAS-PDU PRESENCE optional }|

 { ID id-EmergencyFallbackIndicator CRITICALITY reject TYPE EmergencyFallbackIndicator PRESENCE optional }|

 { ID id-RRCInactiveTransitionReportRequest CRITICALITY ignore TYPE RRCInactiveTransitionReportRequest PRESENCE optional }|

 { ID id-UERadioCapabilityForPaging CRITICALITY ignore TYPE UERadioCapabilityForPaging PRESENCE optional }|

 { ID id-RedirectionVoiceFallback CRITICALITY ignore TYPE RedirectionVoiceFallback PRESENCE optional }|

 { ID id-LocationReportingRequestType CRITICALITY ignore TYPE LocationReportingRequestType PRESENCE optional }|

 { ID id-CNAssistedRANTuning CRITICALITY ignore TYPE CNAssistedRANTuning PRESENCE optional }|

 { ID id-SRVCCOperationPossible CRITICALITY ignore TYPE SRVCCOperationPossible PRESENCE optional }|

 { ID id-IAB-Authorized CRITICALITY ignore TYPE IAB-Authorized PRESENCE optional }|

 { ID id-Enhanced-CoverageRestriction CRITICALITY ignore TYPE Enhanced-CoverageRestriction PRESENCE optional }|

 { ID id-Extended-ConnectedTime CRITICALITY ignore TYPE Extended-ConnectedTime PRESENCE optional }|

 { ID id-UE-DifferentiationInfo CRITICALITY ignore TYPE UE-DifferentiationInfo PRESENCE optional }|

 { ID id-NRV2XServicesAuthorized CRITICALITY ignore TYPE NRV2XServicesAuthorized PRESENCE optional }|

 { ID id-LTEV2XServicesAuthorized CRITICALITY ignore TYPE LTEV2XServicesAuthorized PRESENCE optional }|

 { ID id-NRUESidelinkAggregateMaximumBitrate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-LTEUESidelinkAggregateMaximumBitrate CRITICALITY ignore TYPE LTEUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-PC5QoSParameters CRITICALITY ignore TYPE PC5QoSParameters PRESENCE optional }|

 { ID id-CEmodeBrestricted CRITICALITY ignore TYPE CEmodeBrestricted PRESENCE optional }|

 { ID id-UE-UP-CIoT-Support CRITICALITY ignore TYPE UE-UP-CIoT-Support PRESENCE optional }|

 { ID id-RGLevelWirelineAccessCharacteristics CRITICALITY ignore TYPE RGLevelWirelineAccessCharacteristics PRESENCE optional }|

 { ID id-ManagementBasedMDTPLMNList CRITICALITY ignore TYPE MDTPLMNList PRESENCE optional }|

 { ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE optional }|

 { ID id-TimeSyncAssistanceInfo CRITICALITY ignore TYPE TimeSyncAssistanceInfo PRESENCE optional }|

 { ID id-QMCConfigInfo CRITICALITY ignore TYPE QMCConfigInfo PRESENCE optional }|

 { ID id-TargetNSSAIInformation CRITICALITY ignore TYPE TargetNSSAIInformation PRESENCE optional }|

 { ID id-UESliceMaximumBitRateList CRITICALITY ignore TYPE UESliceMaximumBitRateList PRESENCE optional }|

 { ID id-FiveG-ProSeAuthorized CRITICALITY ignore TYPE FiveG-ProSeAuthorized PRESENCE optional }|

 { ID id-FiveG-ProSeUEPC5AggregateMaximumBitRate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-FiveG-ProSePC5QoSParameters CRITICALITY ignore TYPE FiveG-ProSePC5QoSParameters PRESENCE optional }|

 { ID id-NetworkControlledRepeaterAuthorized CRITICALITY ignore TYPE NetworkControlledRepeaterAuthorized PRESENCE optional }|

 { ID id-AerialUEsubscriptionInformation CRITICALITY ignore TYPE AerialUEsubscriptionInformation PRESENCE optional }|

 { ID id-NR-A2X-ServicesAuthorized CRITICALITY ignore TYPE NR-A2X-ServicesAuthorized PRESENCE optional }|

 { ID id-LTE-A2X-ServicesAuthorized CRITICALITY ignore TYPE LTE-A2X-ServicesAuthorized PRESENCE optional }|

 { ID id-NR-A2X-UE-PC5-AggregateMaximumBitRate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-LTE-A2X-UE-PC5-AggregateMaximumBitRate CRITICALITY ignore TYPE LTEUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-A2X-PC5-QoS-Parameters CRITICALITY ignore TYPE A2X-PC5-QoS-Parameters PRESENCE optional }|

 { ID id-MobileIAB-Authorized CRITICALITY ignore TYPE MobileIAB-Authorized PRESENCE optional }|

 { ID id-Partially-Allowed-NSSAI CRITICALITY ignore TYPE Partially-Allowed-NSSAI PRESENCE optional },|

 { ID id-SLPositioningRangingServiceInfo CRITICALITY ignore TYPE SLPositioningRangingServiceInfo PRESENCE optional },

 ...

}

**<Unchanged Text Omitted>**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- UE CONTEXT MODIFICATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UEContextModificationRequest ::= SEQUENCE {

 protocolIEs ProtocolIE-Container { {UEContextModificationRequestIEs} },

 ...

}

UEContextModificationRequestIEs NGAP-PROTOCOL-IES ::= {

 { ID id-AMF-UE-NGAP-ID CRITICALITY reject TYPE AMF-UE-NGAP-ID PRESENCE mandatory }|

 { ID id-RAN-UE-NGAP-ID CRITICALITY reject TYPE RAN-UE-NGAP-ID PRESENCE mandatory }|

 { ID id-RANPagingPriority CRITICALITY ignore TYPE RANPagingPriority PRESENCE optional }|

 { ID id-SecurityKey CRITICALITY reject TYPE SecurityKey PRESENCE optional }|

 { ID id-IndexToRFSP CRITICALITY ignore TYPE IndexToRFSP PRESENCE optional }|

 { ID id-UEAggregateMaximumBitRate CRITICALITY ignore TYPE UEAggregateMaximumBitRate PRESENCE optional }|

 { ID id-UESecurityCapabilities CRITICALITY reject TYPE UESecurityCapabilities PRESENCE optional }|

 { ID id-CoreNetworkAssistanceInformationForInactive CRITICALITY ignore TYPE CoreNetworkAssistanceInformationForInactive PRESENCE optional }|

 { ID id-EmergencyFallbackIndicator CRITICALITY reject TYPE EmergencyFallbackIndicator PRESENCE optional }|

 { ID id-NewAMF-UE-NGAP-ID CRITICALITY reject TYPE AMF-UE-NGAP-ID PRESENCE optional }|

 { ID id-RRCInactiveTransitionReportRequest CRITICALITY ignore TYPE RRCInactiveTransitionReportRequest PRESENCE optional }|

 { ID id-NewGUAMI CRITICALITY reject TYPE GUAMI PRESENCE optional }|

 { ID id-CNAssistedRANTuning CRITICALITY ignore TYPE CNAssistedRANTuning PRESENCE optional }|

 { ID id-SRVCCOperationPossible CRITICALITY ignore TYPE SRVCCOperationPossible PRESENCE optional }|

 { ID id-IAB-Authorized CRITICALITY ignore TYPE IAB-Authorized PRESENCE optional }|

 { ID id-NRV2XServicesAuthorized CRITICALITY ignore TYPE NRV2XServicesAuthorized PRESENCE optional }|

 { ID id-LTEV2XServicesAuthorized CRITICALITY ignore TYPE LTEV2XServicesAuthorized PRESENCE optional }|

 { ID id-NRUESidelinkAggregateMaximumBitrate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-LTEUESidelinkAggregateMaximumBitrate CRITICALITY ignore TYPE LTEUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-PC5QoSParameters CRITICALITY ignore TYPE PC5QoSParameters PRESENCE optional }|

 { ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE optional }|

 { ID id-RGLevelWirelineAccessCharacteristics CRITICALITY ignore TYPE RGLevelWirelineAccessCharacteristics PRESENCE optional }|

 { ID id-TimeSyncAssistanceInfo CRITICALITY ignore TYPE TimeSyncAssistanceInfo PRESENCE optional }|

 { ID id-QMCConfigInfo CRITICALITY ignore TYPE QMCConfigInfo PRESENCE optional }|

 { ID id-QMCDeactivation CRITICALITY ignore TYPE QMCDeactivation PRESENCE optional }|

 { ID id-UESliceMaximumBitRateList CRITICALITY ignore TYPE UESliceMaximumBitRateList PRESENCE optional }|

 { ID id-ManagementBasedMDTPLMNModificationList CRITICALITY ignore TYPE MDTPLMNModificationList PRESENCE optional }|

 { ID id-FiveG-ProSeAuthorized CRITICALITY ignore TYPE FiveG-ProSeAuthorized PRESENCE optional }|

 { ID id-FiveG-ProSeUEPC5AggregateMaximumBitRate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-FiveG-ProSePC5QoSParameters CRITICALITY ignore TYPE FiveG-ProSePC5QoSParameters PRESENCE optional }|

 { ID id-NetworkControlledRepeaterAuthorized CRITICALITY ignore TYPE NetworkControlledRepeaterAuthorized PRESENCE optional }|

 { ID id-AerialUEsubscriptionInformation CRITICALITY ignore TYPE AerialUEsubscriptionInformation PRESENCE optional }|

 { ID id-NR-A2X-ServicesAuthorized CRITICALITY ignore TYPE NR-A2X-ServicesAuthorized PRESENCE optional }|

 { ID id-LTE-A2X-ServicesAuthorized CRITICALITY ignore TYPE LTE-A2X-ServicesAuthorized PRESENCE optional }|

 { ID id-NR-A2X-UE-PC5-AggregateMaximumBitRate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-LTE-A2X-UE-PC5-AggregateMaximumBitRate CRITICALITY ignore TYPE LTEUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-A2X-PC5-QoS-Parameters CRITICALITY ignore TYPE A2X-PC5-QoS-Parameters PRESENCE optional }|

 { ID id-MobileIAB-Authorized CRITICALITY ignore TYPE MobileIAB-Authorized PRESENCE optional }|

 { ID id-SLPositioningRangingServiceInfo CRITICALITY ignore TYPE SLPositioningRangingServiceInfo PRESENCE optional },

 ...

}

**<Unchanged Text Omitted>**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Handover Resource Allocation Elementary Procedure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- HANDOVER REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

HandoverRequest ::= SEQUENCE {

 protocolIEs ProtocolIE-Container { {HandoverRequestIEs} },

 ...

}

HandoverRequestIEs NGAP-PROTOCOL-IES ::= {

 { ID id-AMF-UE-NGAP-ID CRITICALITY reject TYPE AMF-UE-NGAP-ID PRESENCE mandatory }|

 { ID id-HandoverType CRITICALITY reject TYPE HandoverType PRESENCE mandatory }|

 { ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

 { ID id-UEAggregateMaximumBitRate CRITICALITY reject TYPE UEAggregateMaximumBitRate PRESENCE mandatory }|

 { ID id-CoreNetworkAssistanceInformationForInactive CRITICALITY ignore TYPE CoreNetworkAssistanceInformationForInactive PRESENCE optional }|

 { ID id-UESecurityCapabilities CRITICALITY reject TYPE UESecurityCapabilities PRESENCE mandatory }|

 { ID id-SecurityContext CRITICALITY reject TYPE SecurityContext PRESENCE mandatory }|

 { ID id-NewSecurityContextInd CRITICALITY reject TYPE NewSecurityContextInd PRESENCE optional }|

 { ID id-NASC CRITICALITY reject TYPE NAS-PDU PRESENCE optional }|

 { ID id-PDUSessionResourceSetupListHOReq CRITICALITY reject TYPE PDUSessionResourceSetupListHOReq PRESENCE mandatory }|

 { ID id-AllowedNSSAI CRITICALITY reject TYPE AllowedNSSAI PRESENCE mandatory }|

 { ID id-TraceActivation CRITICALITY ignore TYPE TraceActivation PRESENCE optional }|

 { ID id-MaskedIMEISV CRITICALITY ignore TYPE MaskedIMEISV PRESENCE optional }|

 { ID id-SourceToTarget-TransparentContainer CRITICALITY reject TYPE SourceToTarget-TransparentContainer PRESENCE mandatory }|

 { ID id-MobilityRestrictionList CRITICALITY ignore TYPE MobilityRestrictionList PRESENCE optional }|

 { ID id-LocationReportingRequestType CRITICALITY ignore TYPE LocationReportingRequestType PRESENCE optional }|

 { ID id-RRCInactiveTransitionReportRequest CRITICALITY ignore TYPE RRCInactiveTransitionReportRequest PRESENCE optional }|

 { ID id-GUAMI CRITICALITY reject TYPE GUAMI PRESENCE mandatory }|

 { ID id-RedirectionVoiceFallback CRITICALITY ignore TYPE RedirectionVoiceFallback PRESENCE optional }|

 { ID id-CNAssistedRANTuning CRITICALITY ignore TYPE CNAssistedRANTuning PRESENCE optional }|

 { ID id-SRVCCOperationPossible CRITICALITY ignore TYPE SRVCCOperationPossible PRESENCE optional }|

 { ID id-IAB-Authorized CRITICALITY reject TYPE IAB-Authorized PRESENCE optional }|

 { ID id-Enhanced-CoverageRestriction CRITICALITY ignore TYPE Enhanced-CoverageRestriction PRESENCE optional }|

 { ID id-UE-DifferentiationInfo CRITICALITY ignore TYPE UE-DifferentiationInfo PRESENCE optional }|

 { ID id-NRV2XServicesAuthorized CRITICALITY ignore TYPE NRV2XServicesAuthorized PRESENCE optional }|

 { ID id-LTEV2XServicesAuthorized CRITICALITY ignore TYPE LTEV2XServicesAuthorized PRESENCE optional }|

 { ID id-NRUESidelinkAggregateMaximumBitrate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-LTEUESidelinkAggregateMaximumBitrate CRITICALITY ignore TYPE LTEUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-PC5QoSParameters CRITICALITY ignore TYPE PC5QoSParameters PRESENCE optional }|

 { ID id-CEmodeBrestricted CRITICALITY ignore TYPE CEmodeBrestricted PRESENCE optional }|

 { ID id-UE-UP-CIoT-Support CRITICALITY ignore TYPE UE-UP-CIoT-Support PRESENCE optional }|

 { ID id-ManagementBasedMDTPLMNList CRITICALITY ignore TYPE MDTPLMNList PRESENCE optional }|

 { ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE optional }|

 { ID id-Extended-ConnectedTime CRITICALITY ignore TYPE Extended-ConnectedTime PRESENCE optional }|

 { ID id-TimeSyncAssistanceInfo CRITICALITY ignore TYPE TimeSyncAssistanceInfo PRESENCE optional }|

 { ID id-UESliceMaximumBitRateList CRITICALITY ignore TYPE UESliceMaximumBitRateList PRESENCE optional }|

 { ID id-FiveG-ProSeAuthorized CRITICALITY ignore TYPE FiveG-ProSeAuthorized PRESENCE optional }|

 { ID id-FiveG-ProSeUEPC5AggregateMaximumBitRate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-FiveG-ProSePC5QoSParameters CRITICALITY ignore TYPE FiveG-ProSePC5QoSParameters PRESENCE optional }|

 { ID id-AerialUEsubscriptionInformation CRITICALITY ignore TYPE AerialUEsubscriptionInformation PRESENCE optional }|

 { ID id-NR-A2X-ServicesAuthorized CRITICALITY ignore TYPE NR-A2X-ServicesAuthorized PRESENCE optional }|

 { ID id-LTE-A2X-ServicesAuthorized CRITICALITY ignore TYPE LTE-A2X-ServicesAuthorized PRESENCE optional }|

 { ID id-NR-A2X-UE-PC5-AggregateMaximumBitRate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-LTE-A2X-UE-PC5-AggregateMaximumBitRate CRITICALITY ignore TYPE LTEUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-A2X-PC5-QoS-Parameters CRITICALITY ignore TYPE A2X-PC5-QoS-Parameters PRESENCE optional }|

 { ID id-MobileIAB-Authorized CRITICALITY ignore TYPE MobileIAB-Authorized PRESENCE optional }|

 { ID id-NoPDUSessionIndication CRITICALITY ignore TYPE NoPDUSessionIndication PRESENCE optional }|

 { ID id-Partially-Allowed-NSSAI CRITICALITY ignore TYPE Partially-Allowed-NSSAI PRESENCE optional }|

 { ID id-SLPositioningRangingServiceInfo CRITICALITY ignore TYPE SLPositioningRangingServiceInfo PRESENCE optional },

 ...

}

**<Unchanged Text Omitted>**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PATH SWITCH REQUEST ACKNOWLEDGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PathSwitchRequestAcknowledge ::= SEQUENCE {

 protocolIEs ProtocolIE-Container { { PathSwitchRequestAcknowledgeIEs} },

 ...

}

PathSwitchRequestAcknowledgeIEs NGAP-PROTOCOL-IES ::= {

 { ID id-AMF-UE-NGAP-ID CRITICALITY ignore TYPE AMF-UE-NGAP-ID PRESENCE mandatory }|

 { ID id-RAN-UE-NGAP-ID CRITICALITY ignore TYPE RAN-UE-NGAP-ID PRESENCE mandatory }|

 { ID id-UESecurityCapabilities CRITICALITY reject TYPE UESecurityCapabilities PRESENCE optional }|

 { ID id-SecurityContext CRITICALITY reject TYPE SecurityContext PRESENCE mandatory }|

 { ID id-NewSecurityContextInd CRITICALITY reject TYPE NewSecurityContextInd PRESENCE optional }|

 { ID id-PDUSessionResourceSwitchedList CRITICALITY ignore TYPE PDUSessionResourceSwitchedList PRESENCE mandatory }|

 { ID id-PDUSessionResourceReleasedListPSAck CRITICALITY ignore TYPE PDUSessionResourceReleasedListPSAck PRESENCE optional }|

 { ID id-AllowedNSSAI CRITICALITY reject TYPE AllowedNSSAI PRESENCE mandatory }|

 { ID id-CoreNetworkAssistanceInformationForInactive CRITICALITY ignore TYPE CoreNetworkAssistanceInformationForInactive PRESENCE optional }|

 { ID id-RRCInactiveTransitionReportRequest CRITICALITY ignore TYPE RRCInactiveTransitionReportRequest PRESENCE optional }|

 { ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

 { ID id-RedirectionVoiceFallback CRITICALITY ignore TYPE RedirectionVoiceFallback PRESENCE optional }|

 { ID id-CNAssistedRANTuning CRITICALITY ignore TYPE CNAssistedRANTuning PRESENCE optional }|

 { ID id-SRVCCOperationPossible CRITICALITY ignore TYPE SRVCCOperationPossible PRESENCE optional }|

 { ID id-Enhanced-CoverageRestriction CRITICALITY ignore TYPE Enhanced-CoverageRestriction PRESENCE optional }|

 { ID id-Extended-ConnectedTime CRITICALITY ignore TYPE Extended-ConnectedTime PRESENCE optional }|

 { ID id-UE-DifferentiationInfo CRITICALITY ignore TYPE UE-DifferentiationInfo PRESENCE optional }|

 { ID id-NRV2XServicesAuthorized CRITICALITY ignore TYPE NRV2XServicesAuthorized PRESENCE optional }|

 { ID id-LTEV2XServicesAuthorized CRITICALITY ignore TYPE LTEV2XServicesAuthorized PRESENCE optional }|

 { ID id-NRUESidelinkAggregateMaximumBitrate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-LTEUESidelinkAggregateMaximumBitrate CRITICALITY ignore TYPE LTEUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-PC5QoSParameters CRITICALITY ignore TYPE PC5QoSParameters PRESENCE optional }|

 { ID id-CEmodeBrestricted CRITICALITY ignore TYPE CEmodeBrestricted PRESENCE optional }|

 { ID id-UE-UP-CIoT-Support CRITICALITY ignore TYPE UE-UP-CIoT-Support PRESENCE optional }|

 { ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE optional }|

 { ID id-ManagementBasedMDTPLMNList CRITICALITY ignore TYPE MDTPLMNList PRESENCE optional }|

 { ID id-TimeSyncAssistanceInfo CRITICALITY ignore TYPE TimeSyncAssistanceInfo PRESENCE optional }|

 { ID id-FiveG-ProSeAuthorized CRITICALITY ignore TYPE FiveG-ProSeAuthorized PRESENCE optional }|

 { ID id-FiveG-ProSeUEPC5AggregateMaximumBitRate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-FiveG-ProSePC5QoSParameters CRITICALITY ignore TYPE FiveG-ProSePC5QoSParameters PRESENCE optional }|

 { ID id-ManagementBasedMDTPLMNModificationList CRITICALITY ignore TYPE MDTPLMNModificationList PRESENCE optional }|

 { ID id-IAB-Authorized CRITICALITY ignore TYPE IAB-Authorized PRESENCE optional }|

 { ID id-AerialUEsubscriptionInformation CRITICALITY ignore TYPE AerialUEsubscriptionInformation PRESENCE optional }|

 { ID id-NR-A2X-ServicesAuthorized CRITICALITY ignore TYPE NR-A2X-ServicesAuthorized PRESENCE optional }|

 { ID id-LTE-A2X-ServicesAuthorized CRITICALITY ignore TYPE LTE-A2X-ServicesAuthorized PRESENCE optional }|

 { ID id-NR-A2X-UE-PC5-AggregateMaximumBitRate CRITICALITY ignore TYPE NRUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-LTE-A2X-UE-PC5-AggregateMaximumBitRate CRITICALITY ignore TYPE LTEUESidelinkAggregateMaximumBitrate PRESENCE optional }|

 { ID id-A2X-PC5-QoS-Parameters CRITICALITY ignore TYPE A2X-PC5-QoS-Parameters PRESENCE optional }|

 { ID id-MobileIAB-Authorized CRITICALITY ignore TYPE MobileIAB-Authorized PRESENCE optional }|

 { ID id-Partially-Allowed-NSSAI CRITICALITY ignore TYPE Partially-Allowed-NSSAI PRESENCE optional }|

 { ID id-SLPositioningRangingServiceInfo CRITICALITY ignore TYPE SLPositioningRangingServiceInfo PRESENCE optional },

 ...

}

**<Unchanged Text Omitted>**

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGAP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 id-AdditionalDLForwardingUPTNLInformation,

 id-AdditionalULForwardingUPTNLInformation,

 id-AdditionalDLQosFlowPerTNLInformation,

 id-AdditionalDLUPTNLInformationForHOList,

 id-AdditionalNGU-UP-TNLInformation,

 id-AdditionalRedundantDL-NGU-UP-TNLInformation,

 id-AdditionalRedundantDLQosFlowPerTNLInformation,

 id-AdditionalRedundantNGU-UP-TNLInformation,

 id-AdditionalRedundantUL-NGU-UP-TNLInformation,

 id-AdditionalUL-NGU-UP-TNLInformation,

 id-AlternativeQoSParaSetList,

 id-BurstArrivalTimeDownlink,

 id-Cause,

 id-CNPacketDelayBudgetDL,

 id-CNPacketDelayBudgetUL,

 id-CNTypeRestrictionsForEquivalent,

 id-CNTypeRestrictionsForServing,

 id-CommonNetworkInstance,

 id-ConfiguredTACIndication,

 id-CurrentQoSParaSetIndex,

 id-DAPSRequestInfo,

 id-DAPSResponseInfoList,

 id-DataForwardingNotPossible,

 id-DataForwardingResponseERABList,

 id-DirectForwardingPathAvailability,

 id-DL-NGU-UP-TNLInformation,

 id-EndpointIPAddressAndPort,

 id-EnergySavingIndication,

 id-ExtendedMobilityInformation,

 id-ExtendedPacketDelayBudget,

 id-ExtendedRATRestrictionInformation,

 id-ExtendedReportIntervalMDT,

 id-ExtendedSliceSupportList,

 id-ExtendedTAISliceSupportList,

 id-ExtendedUEIdentityIndexValue,

 id-EUTRA-PagingeDRXInformation,

 id-GlobalCable-ID,

 id-GlobalRANNodeID,

 id-GlobalTNGF-ID,

 id-GlobalTWIF-ID,

 id-GlobalW-AGF-ID,

 id-GUAMIType,

 id-HashedUEIdentityIndexValue,

 id-IncludeBeamMeasurementsIndication,

 id-IntersystemSONInformationRequest,

 id-IntersystemSONInformationReply,

 id-IntersystemResourceStatusUpdate,

 id-LastEUTRAN-PLMNIdentity,

 id-LastVisitedPSCellList,

 id-LocationReportingAdditionalInfo,

 id-M4ReportAmount,

 id-M5ReportAmount,

 id-M6ReportAmount,

 id-ExcessPacketDelayThresholdConfiguration,

 id-M7ReportAmount,

 id-MaximumIntegrityProtectedDataRate-DL,

 id-MBS-AreaSessionID,

 id-MBS-QoSFlowsToBeSetupList,

 id-MBS-QoSFlowsToBeSetupModList,

 id-MBS-QoSFlowToReleaseList,

 id-MBS-ServiceArea,

 id-MBS-SessionFSAIDList,

 id-MBS-SessionID,

 id-MBS-ActiveSessionInformation-SourcetoTargetList,

 id-MBS-ActiveSessionInformation-TargettoSourceList,

 id-MBS-SessionTNLInfo5GC,

 id-MBS-SupportIndicator,

 id-MBSSessionFailedtoSetupList,

 id-MBSSessionFailedtoSetuporModifyList,

 id-MBSSessionSetupResponseList,

 id-MBSSessionSetuporModifyResponseList,

 id-MBSSessionToReleaseList,

 id-MBSSessionSetupRequestList,

 id-MBSSessionSetuporModifyRequestList,

 id-MDTConfiguration,

 id-MicoAllPLMN,

 id-NetworkInstance,

 id-NGAPIESupportInformationRequestList,

 id-NGAPIESupportInformationResponseList,

 id-NID,

 id-NR-CGI,

 id-NRNTNTAIInformation,

 id-NPN-MobilityInformation,

 id-NPN-PagingAssistanceInformation,

 id-NPN-Support,

 id-NR-PagingeDRXInformation,

 id-OldAssociatedQosFlowList-ULendmarkerexpected,

 id-OnboardingSupport,

 id-PagingAssisDataforCEcapabUE,

 id-PagingCauseIndicationForVoiceService,

 id-PDUSessionAggregateMaximumBitRate,

 id-PduSessionExpectedUEActivityBehaviour,

 id-PDUSessionPairID,

 id-PDUSessionResourceFailedToSetupListCxtFail,

 id-PDUSessionResourceReleaseResponseTransfer,

 id-PDUSessionType,

 id-PEIPSassistanceInformation,

 id-PSCellInformation,

 id-QMCConfigInfo,

 id-QosFlowAddOrModifyRequestList,

 id-QosFlowFailedToSetupList,

 id-QosFlowFeedbackList,

 id-QosFlowParametersList,

 id-QosFlowSetupRequestList,

 id-QosFlowToReleaseList,

 id-QosMonitoringRequest,

 id-QosMonitoringReportingFrequency,

 id-SuccessfulHandoverReportList,

 id-UEContextReferenceAtSource,

 id-RAT-Information,

 id-RedundantCommonNetworkInstance,

 id-RedundantDL-NGU-TNLInformationReused,

 id-RedundantDL-NGU-UP-TNLInformation,

 id-RedundantDLQosFlowPerTNLInformation,

 id-RedundantPDUSessionInformation,

 id-RedundantQosFlowIndicator,

 id-RedundantUL-NGU-UP-TNLInformation,

 id-SCTP-TLAs,

 id-SecondaryRATUsageInformation,

 id-SecurityIndication,

 id-SecurityResult,

 id-SgNB-UE-X2AP-ID,

 id-S-NSSAI,

 id-SONInformationReport,

 id-SourceNodeID,

 id-SourceNodeTNLAddrInfo,

 id-SourceTNLAddrInfo,

 id-SurvivalTime,

 id-TNLAssociationTransportLayerAddressNGRAN,

 id-TAINSAGSupportList,

 id-TargetHomeENB-ID,

 id-TargetRNC-ID,

 id-TraceCollectionEntityURI,

 id-TSCTrafficCharacteristics,

 id-UEHistoryInformationFromTheUE,

 id-UERadioCapabilityForPaging,

 id-UERadioCapabilityForPagingOfNB-IoT,

 id-UL-NGU-UP-TNLInformation,

 id-UL-NGU-UP-TNLModifyList,

 id-ULForwarding,

 id-ULForwardingUP-TNLInformation,

 id-UsedRSNInformation,

 id-UserLocationInformationTNGF,

 id-UserLocationInformationTWIF,

 id-UserLocationInformationW-AGF,

 id-EarlyMeasurement,

 id-BeamMeasurementsReportConfiguration,

 id-TAI,

 id-HFCNode-ID-new,

 id-GlobalCable-ID-new,

 maxnoofAllowedAreas,

 maxnoofAllowedCAGsperPLMN,

 maxnoofAllowedS-NSSAIs,

 maxnoofBluetoothName,

 maxnoofBPLMNs,

 maxnoofCAGSperCell,

 maxnoofCandidateCells,

 maxnoofCellIDforMDT,

 maxnoofCellIDforQMC,

 maxnoofCellIDforWarning,

 maxnoofCellinAoI,

 maxnoofCellinEAI,

 maxnoofCellsforMBS,

 maxnoofCellsingNB,

 maxnoofCellsinngeNB,

 maxnoofCellsinNGRANNode,

 maxnoofCellinTAI,

 maxnoofCellsinUEHistoryInfo,

 maxnoofCellsUEMovingTrajectory,

 maxnoofDRBs,

 maxnoofEmergencyAreaID,

 maxnoofEAIforRestart,

 maxnoofEPLMNs,

 maxnoofEPLMNsPlusOne,

 maxnoofE-RABs,

 maxnoofErrors,

 maxnoofExtSliceItems,

 maxnoofForbTACs,

 maxnoofFreqforMDT,

 maxnoofMBSFSAs,

 maxnoofMBSQoSFlows,

 maxnoofMBSServiceAreaInformation,

 maxnoofMBSAreaSessionIDs,

 maxnoofMBSSessions,

 maxnoofMBSSessionsofUE,

 maxnoofMDTPLMNs,

 maxnoofMRBs,

 maxnoofMultiConnectivity,

 maxnoofMultiConnectivityMinusOne,

 maxnoofNeighPCIforMDT,

 maxnoofNGAPIESupportInfo,

 maxnoofNGConnectionsToReset,

 maxNRARFCN,

 maxnoofNRCellBands,

 maxnoofNSAGs,

 maxnoofPagingAreas,

 maxnoofPC5QoSFlows,

 maxnoofPDUSessions,

 maxnoofPLMNs,

 maxnoofPLMNforQMC,

 maxnoofQosFlows,

 maxnoofQosParaSets,

 maxnoofRANNodeinAoI,

 maxnoofRecommendedCells,

 maxnoofRecommendedRANNodes,

 maxnoofAoI,

 maxnoofPSCellsPerPrimaryCellinUEHistoryInfo,

 maxnoofReportedCells,

 maxnoofSensorName,

 maxnoofServedGUAMIs,

 maxnoofSliceItems,

 maxnoofSNSSAIforQMC,

 maxnoofSuccessfulHOReports,

 maxnoofTACs,

 maxnoofTACsinNTN,

 maxnoofTAforMDT,

 maxnoofTAforQMC,

 maxnoofTAIforInactive,

 maxnoofTAIforMBS,

 maxnoofTAIforPaging,

 maxnoofTAIforRestart,

 maxnoofTAIforWarning,

 maxnoofTAIinAoI,

 maxnoofTargetS-NSSAIs,

 maxnoofTimePeriods,

 maxnoofTNLAssociations,

 maxnoofUEAppLayerMeas,

 maxnoofUEsforPaging,

 maxnoofWLANName,

 maxnoofXnExtTLAs,

 maxnoofXnGTP-TLAs,

 maxnoofXnTLAs,

 maxnoofThresholdsForExcessPacketDelay,

 maxnoofRSPPQoSFlows

FROM NGAP-Constants

 Criticality,

 ProcedureCode,

 ProtocolIE-ID,

 TriggeringMessage

FROM NGAP-CommonDataTypes

 ProtocolExtensionContainer{},

 ProtocolIE-Container{},

 NGAP-PROTOCOL-EXTENSION,

 ProtocolIE-SingleContainer{},

 NGAP-PROTOCOL-IES

FROM NGAP-Containers;

**<Unchanged Text Omitted>**

-- S

**<Unchanged Text Omitted>**

SLPositioningRangingServiceInfo ::= SEQUENCE{

 sLPositioningRangingAuthorized SLPositioningRangingAuthorized,

 sLPositioningRangingQoSParameters SLPositioningRangingQoSParameters OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { {SLPositioningRangingServiceInfo-ExtIEs} } OPTIONAL

}

SLPositioningRangingServiceInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 ...

}

SLPositioningRangingAuthorized ::= ENUMERATED {

 authorized,

 not-authorized,

 ...

}

SLPositioningRangingQoSParameters ::= SEQUENCE {

 rSPPQoSFlowList RSPPQoSFlowList,

 rSPPLinkAggregateBitRates BitRate OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { { SLPositioningRangingQoSParameters-ExtIEs} } OPTIONAL,

 ...

}

SLPositioningRangingQoSParameters-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 ...

}

**<Unchanged Text Omitted>**

-- R

**<Unchanged Text Omitted>**

RSPPQoSFlowList ::= SEQUENCE (SIZE(1..maxnoofRSPPQoSFlows)) OF RSPPQoSFlowItem

RSPPQoSFlowItem ::= SEQUENCE {

 pQI FiveQI,

 rSPPFlowBitRates RSPPFlowBitRates OPTIONAL,

 range Range OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { { RSPPQoSFlowItem-ExtIEs} } OPTIONAL,

 ...

}

RSPPQoSFlowItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 ...

}

RSPPFlowBitRates ::= SEQUENCE {

 guaranteedFlowBitRate BitRate,

 maximumFlowBitRate BitRate,

 iE-Extensions ProtocolExtensionContainer { { RSPPFlowBitRates-ExtIEs} } OPTIONAL,

 ...

}

RSPPFlowBitRates-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 ...

}

**<Unchanged Text Omitted>**

### 9.4.7 Constant Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGAP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM NGAP-CommonDataTypes;

**<Unchanged Text Omitted>**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

 maxnoofAllowedAreas INTEGER ::= 16

 maxnoofAllowedCAGsperPLMN INTEGER ::= 256

 maxnoofAllowedS-NSSAIs INTEGER ::= 8

 maxnoofBluetoothName INTEGER ::= 4

 maxnoofBPLMNs INTEGER ::= 12

 maxnoofCAGSperCell INTEGER ::= 64

 maxnoofCellIDforMDT INTEGER ::= 32

 maxnoofCellIDforWarning INTEGER ::= 65535

 maxnoofCellinAoI INTEGER ::= 256

 maxnoofCellinEAI INTEGER ::= 65535

 maxnoofCellinTAI INTEGER ::= 65535

 maxnoofCellsforMBS INTEGER ::= 8192

 maxnoofCellsingNB INTEGER ::= 16384

 maxnoofCellsinngeNB INTEGER ::= 256

 maxnoofCellsinNGRANNode INTEGER ::= 16384

 maxnoofCellsinUEHistoryInfo INTEGER ::= 16

 maxnoofCellsUEMovingTrajectory INTEGER ::= 16

 maxnoofDRBs INTEGER ::= 32

 maxnoofEmergencyAreaID INTEGER ::= 65535

 maxnoofEAIforRestart INTEGER ::= 256

 maxnoofEPLMNs INTEGER ::= 15

 maxnoofEPLMNsPlusOne INTEGER ::= 16

 maxnoofE-RABs INTEGER ::= 256

 maxnoofErrors INTEGER ::= 256

 maxnoofExtSliceItems INTEGER ::= 65535

 maxnoofForbTACs INTEGER ::= 4096

 maxnoofFreqforMDT INTEGER ::= 8

 maxnoofMBSAreaSessionIDs INTEGER ::= 256

 maxnoofMBSFSAs INTEGER ::= 64

 maxnoofMBSQoSFlows INTEGER ::= 64

 maxnoofMBSSessions INTEGER ::= 32

 maxnoofMBSSessionsofUE INTEGER ::= 256

 maxnoofMBSServiceAreaInformation INTEGER ::= 256

 maxnoofMDTPLMNs INTEGER ::= 16

 maxnoofMRBs INTEGER ::= 32

 maxnoofMultiConnectivity INTEGER ::= 4

 maxnoofMultiConnectivityMinusOne INTEGER ::= 3

 maxnoofNeighPCIforMDT INTEGER ::= 32

 maxnoofNGAPIESupportInfo INTEGER ::= 32

 maxnoofNGConnectionsToReset INTEGER ::= 65536

 maxnoofNRCellBands INTEGER ::= 32

 maxnoofNSAGs INTEGER ::= 256

 maxnoofPagingAreas INTEGER ::= 64

 maxnoofPC5QoSFlows INTEGER ::= 2048

 maxnoofPDUSessions INTEGER ::= 256

 maxnoofPLMNs INTEGER ::= 12

 maxnoofPSCellsPerPrimaryCellinUEHistoryInfo INTEGER ::= 8

 maxnoofQosFlows INTEGER ::= 64

 maxnoofQosParaSets INTEGER ::= 8

 maxnoofRANNodeinAoI INTEGER ::= 64

 maxnoofRecommendedCells INTEGER ::= 16

 maxnoofRecommendedRANNodes INTEGER ::= 16

 maxnoofAoI INTEGER ::= 64

 maxnoofAoIMinusOne INTEGER ::= 63

 maxnoofReportedCells INTEGER ::= 256

 maxnoofSensorName INTEGER ::= 3

 maxnoofServedGUAMIs INTEGER ::= 256

 maxnoofSliceItems INTEGER ::= 1024

 maxnoofSuccessfulHOReports INTEGER ::= 64

 maxnoofTACs INTEGER ::= 256

 maxnoofTACsinNTN INTEGER ::= 12

 maxnoofTAforMDT INTEGER ::= 8

 maxnoofTAIforInactive INTEGER ::= 16

 maxnoofTAIforMBS INTEGER ::= 1024

 maxnoofTAIforPaging INTEGER ::= 16

 maxnoofTAIforRestart INTEGER ::= 2048

 maxnoofTAIforWarning INTEGER ::= 65535

 maxnoofTAIinAoI INTEGER ::= 16

 maxnoofTimePeriods INTEGER ::= 2

 maxnoofTNLAssociations INTEGER ::= 32

 maxnoofUEsforPaging INTEGER ::= 4096

 maxnoofUETypes INTEGER ::= 8

 maxnoofWLANName INTEGER ::= 4

 maxnoofXnExtTLAs INTEGER ::= 16

 maxnoofXnGTP-TLAs INTEGER ::= 16

 maxnoofXnTLAs INTEGER ::= 2

 maxnoofCandidateCells INTEGER ::= 32

 maxnoofTargetS-NSSAIs INTEGER ::= 8

 maxNRARFCN INTEGER ::= 3279165

 maxnoofCellIDforQMC INTEGER ::= 32

 maxnoofPLMNforQMC INTEGER ::= 16

 maxnoofUEAppLayerMeas INTEGER ::= 16

 maxnoofSNSSAIforQMC INTEGER ::= 16

 maxnoofTAforQMC INTEGER ::= 8

 maxnoofThresholdsForExcessPacketDelay INTEGER ::= 255

 maxnoofESNPNs INTEGER ::= 15

 maxnoofCandidateRelayUEs INTEGER ::= 32

 maxnoofSuccessfulPSCellChangeReports INTEGER ::= 64

 maxnoofCellsTSS INTEGER ::= 16384

 maxnoofPeriodicities INTEGER ::= 8

 maxnoofCAGforMDT INTEGER ::= 256

 maxnoofMDTSNPNs INTEGER ::= 16

 maxnoofPartiallyAllowedS-NSSAIs INTEGER ::= 8

 maxnoofRSPPQoSFlows INTEGER ::= 2048

**<Unchanged Text Omitted>**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

 id-AllowedNSSAI ProtocolIE-ID ::= 0

 id-AMFName ProtocolIE-ID ::= 1

 id-AMFOverloadResponse ProtocolIE-ID ::= 2

 id-AMFSetID ProtocolIE-ID ::= 3

 id-AMF-TNLAssociationFailedToSetupList ProtocolIE-ID ::= 4

 id-AMF-TNLAssociationSetupList ProtocolIE-ID ::= 5

 id-AMF-TNLAssociationToAddList ProtocolIE-ID ::= 6

 id-AMF-TNLAssociationToRemoveList ProtocolIE-ID ::= 7

 id-AMF-TNLAssociationToUpdateList ProtocolIE-ID ::= 8

 id-AMFTrafficLoadReductionIndication ProtocolIE-ID ::= 9

 id-AMF-UE-NGAP-ID ProtocolIE-ID ::= 10

 id-AssistanceDataForPaging ProtocolIE-ID ::= 11

 id-BroadcastCancelledAreaList ProtocolIE-ID ::= 12

 id-BroadcastCompletedAreaList ProtocolIE-ID ::= 13

 id-CancelAllWarningMessages ProtocolIE-ID ::= 14

 id-Cause ProtocolIE-ID ::= 15

 id-CellIDListForRestart ProtocolIE-ID ::= 16

 id-ConcurrentWarningMessageInd ProtocolIE-ID ::= 17

 id-CoreNetworkAssistanceInformationForInactive ProtocolIE-ID ::= 18

 id-CriticalityDiagnostics ProtocolIE-ID ::= 19

 id-DataCodingScheme ProtocolIE-ID ::= 20

 id-DefaultPagingDRX ProtocolIE-ID ::= 21

 id-DirectForwardingPathAvailability ProtocolIE-ID ::= 22

 id-EmergencyAreaIDListForRestart ProtocolIE-ID ::= 23

 id-EmergencyFallbackIndicator ProtocolIE-ID ::= 24

 id-EUTRA-CGI ProtocolIE-ID ::= 25

 id-FiveG-S-TMSI ProtocolIE-ID ::= 26

 id-GlobalRANNodeID ProtocolIE-ID ::= 27

 id-GUAMI ProtocolIE-ID ::= 28

 id-HandoverType ProtocolIE-ID ::= 29

 id-IMSVoiceSupportIndicator ProtocolIE-ID ::= 30

 id-IndexToRFSP ProtocolIE-ID ::= 31

 id-InfoOnRecommendedCellsAndRANNodesForPaging ProtocolIE-ID ::= 32

 id-LocationReportingRequestType ProtocolIE-ID ::= 33

 id-MaskedIMEISV ProtocolIE-ID ::= 34

 id-MessageIdentifier ProtocolIE-ID ::= 35

 id-MobilityRestrictionList ProtocolIE-ID ::= 36

 id-NASC ProtocolIE-ID ::= 37

 id-NAS-PDU ProtocolIE-ID ::= 38

 id-NASSecurityParametersFromNGRAN ProtocolIE-ID ::= 39

 id-NewAMF-UE-NGAP-ID ProtocolIE-ID ::= 40

 id-NewSecurityContextInd ProtocolIE-ID ::= 41

 id-NGAP-Message ProtocolIE-ID ::= 42

 id-NGRAN-CGI ProtocolIE-ID ::= 43

 id-NGRANTraceID ProtocolIE-ID ::= 44

 id-NR-CGI ProtocolIE-ID ::= 45

 id-NRPPa-PDU ProtocolIE-ID ::= 46

 id-NumberOfBroadcastsRequested ProtocolIE-ID ::= 47

 id-OldAMF ProtocolIE-ID ::= 48

 id-OverloadStartNSSAIList ProtocolIE-ID ::= 49

 id-PagingDRX ProtocolIE-ID ::= 50

 id-PagingOrigin ProtocolIE-ID ::= 51

 id-PagingPriority ProtocolIE-ID ::= 52

 id-PDUSessionResourceAdmittedList ProtocolIE-ID ::= 53

 id-PDUSessionResourceFailedToModifyListModRes ProtocolIE-ID ::= 54

 id-PDUSessionResourceFailedToSetupListCxtRes ProtocolIE-ID ::= 55

 id-PDUSessionResourceFailedToSetupListHOAck ProtocolIE-ID ::= 56

 id-PDUSessionResourceFailedToSetupListPSReq ProtocolIE-ID ::= 57

 id-PDUSessionResourceFailedToSetupListSURes ProtocolIE-ID ::= 58

 id-PDUSessionResourceHandoverList ProtocolIE-ID ::= 59

 id-PDUSessionResourceListCxtRelCpl ProtocolIE-ID ::= 60

 id-PDUSessionResourceListHORqd ProtocolIE-ID ::= 61

 id-PDUSessionResourceModifyListModCfm ProtocolIE-ID ::= 62

 id-PDUSessionResourceModifyListModInd ProtocolIE-ID ::= 63

 id-PDUSessionResourceModifyListModReq ProtocolIE-ID ::= 64

 id-PDUSessionResourceModifyListModRes ProtocolIE-ID ::= 65

 id-PDUSessionResourceNotifyList ProtocolIE-ID ::= 66

 id-PDUSessionResourceReleasedListNot ProtocolIE-ID ::= 67

 id-PDUSessionResourceReleasedListPSAck ProtocolIE-ID ::= 68

 id-PDUSessionResourceReleasedListPSFail ProtocolIE-ID ::= 69

 id-PDUSessionResourceReleasedListRelRes ProtocolIE-ID ::= 70

 id-PDUSessionResourceSetupListCxtReq ProtocolIE-ID ::= 71

 id-PDUSessionResourceSetupListCxtRes ProtocolIE-ID ::= 72

 id-PDUSessionResourceSetupListHOReq ProtocolIE-ID ::= 73

 id-PDUSessionResourceSetupListSUReq ProtocolIE-ID ::= 74

 id-PDUSessionResourceSetupListSURes ProtocolIE-ID ::= 75

 id-PDUSessionResourceToBeSwitchedDLList ProtocolIE-ID ::= 76

 id-PDUSessionResourceSwitchedList ProtocolIE-ID ::= 77

 id-PDUSessionResourceToReleaseListHOCmd ProtocolIE-ID ::= 78

 id-PDUSessionResourceToReleaseListRelCmd ProtocolIE-ID ::= 79

 id-PLMNSupportList ProtocolIE-ID ::= 80

 id-PWSFailedCellIDList ProtocolIE-ID ::= 81

 id-RANNodeName ProtocolIE-ID ::= 82

 id-RANPagingPriority ProtocolIE-ID ::= 83

 id-RANStatusTransfer-TransparentContainer ProtocolIE-ID ::= 84

 id-RAN-UE-NGAP-ID ProtocolIE-ID ::= 85

 id-RelativeAMFCapacity ProtocolIE-ID ::= 86

 id-RepetitionPeriod ProtocolIE-ID ::= 87

 id-ResetType ProtocolIE-ID ::= 88

 id-RoutingID ProtocolIE-ID ::= 89

 id-RRCEstablishmentCause ProtocolIE-ID ::= 90

 id-RRCInactiveTransitionReportRequest ProtocolIE-ID ::= 91

 id-RRCState ProtocolIE-ID ::= 92

 id-SecurityContext ProtocolIE-ID ::= 93

 id-SecurityKey ProtocolIE-ID ::= 94

 id-SerialNumber ProtocolIE-ID ::= 95

 id-ServedGUAMIList ProtocolIE-ID ::= 96

 id-SliceSupportList ProtocolIE-ID ::= 97

 id-SONConfigurationTransferDL ProtocolIE-ID ::= 98

 id-SONConfigurationTransferUL ProtocolIE-ID ::= 99

 id-SourceAMF-UE-NGAP-ID ProtocolIE-ID ::= 100

 id-SourceToTarget-TransparentContainer ProtocolIE-ID ::= 101

 id-SupportedTAList ProtocolIE-ID ::= 102

 id-TAIListForPaging ProtocolIE-ID ::= 103

 id-TAIListForRestart ProtocolIE-ID ::= 104

 id-TargetID ProtocolIE-ID ::= 105

 id-TargetToSource-TransparentContainer ProtocolIE-ID ::= 106

 id-TimeToWait ProtocolIE-ID ::= 107

 id-TraceActivation ProtocolIE-ID ::= 108

 id-TraceCollectionEntityIPAddress ProtocolIE-ID ::= 109

 id-UEAggregateMaximumBitRate ProtocolIE-ID ::= 110

 id-UE-associatedLogicalNG-connectionList ProtocolIE-ID ::= 111

 id-UEContextRequest ProtocolIE-ID ::= 112

 id-UE-NGAP-IDs ProtocolIE-ID ::= 114

 id-UEPagingIdentity ProtocolIE-ID ::= 115

 id-UEPresenceInAreaOfInterestList ProtocolIE-ID ::= 116

 id-UERadioCapability ProtocolIE-ID ::= 117

 id-UERadioCapabilityForPaging ProtocolIE-ID ::= 118

 id-UESecurityCapabilities ProtocolIE-ID ::= 119

 id-UnavailableGUAMIList ProtocolIE-ID ::= 120

 id-UserLocationInformation ProtocolIE-ID ::= 121

 id-WarningAreaList ProtocolIE-ID ::= 122

 id-WarningMessageContents ProtocolIE-ID ::= 123

 id-WarningSecurityInfo ProtocolIE-ID ::= 124

 id-WarningType ProtocolIE-ID ::= 125

 id-AdditionalUL-NGU-UP-TNLInformation ProtocolIE-ID ::= 126

 id-DataForwardingNotPossible ProtocolIE-ID ::= 127

 id-DL-NGU-UP-TNLInformation ProtocolIE-ID ::= 128

 id-NetworkInstance ProtocolIE-ID ::= 129

 id-PDUSessionAggregateMaximumBitRate ProtocolIE-ID ::= 130

 id-PDUSessionResourceFailedToModifyListModCfm ProtocolIE-ID ::= 131

 id-PDUSessionResourceFailedToSetupListCxtFail ProtocolIE-ID ::= 132

 id-PDUSessionResourceListCxtRelReq ProtocolIE-ID ::= 133

 id-PDUSessionType ProtocolIE-ID ::= 134

 id-QosFlowAddOrModifyRequestList ProtocolIE-ID ::= 135

 id-QosFlowSetupRequestList ProtocolIE-ID ::= 136

 id-QosFlowToReleaseList ProtocolIE-ID ::= 137

 id-SecurityIndication ProtocolIE-ID ::= 138

 id-UL-NGU-UP-TNLInformation ProtocolIE-ID ::= 139

 id-UL-NGU-UP-TNLModifyList ProtocolIE-ID ::= 140

 id-WarningAreaCoordinates ProtocolIE-ID ::= 141

 id-PDUSessionResourceSecondaryRATUsageList ProtocolIE-ID ::= 142

 id-HandoverFlag ProtocolIE-ID ::= 143

 id-SecondaryRATUsageInformation ProtocolIE-ID ::= 144

 id-PDUSessionResourceReleaseResponseTransfer ProtocolIE-ID ::= 145

 id-RedirectionVoiceFallback ProtocolIE-ID ::= 146

 id-UERetentionInformation ProtocolIE-ID ::= 147

 id-S-NSSAI ProtocolIE-ID ::= 148

 id-PSCellInformation ProtocolIE-ID ::= 149

 id-LastEUTRAN-PLMNIdentity ProtocolIE-ID ::= 150

 id-MaximumIntegrityProtectedDataRate-DL ProtocolIE-ID ::= 151

 id-AdditionalDLForwardingUPTNLInformation ProtocolIE-ID ::= 152

 id-AdditionalDLUPTNLInformationForHOList ProtocolIE-ID ::= 153

 id-AdditionalNGU-UP-TNLInformation ProtocolIE-ID ::= 154

 id-AdditionalDLQosFlowPerTNLInformation ProtocolIE-ID ::= 155

 id-SecurityResult ProtocolIE-ID ::= 156

 id-ENDC-SONConfigurationTransferDL ProtocolIE-ID ::= 157

 id-ENDC-SONConfigurationTransferUL ProtocolIE-ID ::= 158

 id-OldAssociatedQosFlowList-ULendmarkerexpected ProtocolIE-ID ::= 159

 id-CNTypeRestrictionsForEquivalent ProtocolIE-ID ::= 160

 id-CNTypeRestrictionsForServing ProtocolIE-ID ::= 161

 id-NewGUAMI ProtocolIE-ID ::= 162

 id-ULForwarding ProtocolIE-ID ::= 163

 id-ULForwardingUP-TNLInformation ProtocolIE-ID ::= 164

 id-CNAssistedRANTuning ProtocolIE-ID ::= 165

 id-CommonNetworkInstance ProtocolIE-ID ::= 166

 id-NGRAN-TNLAssociationToRemoveList ProtocolIE-ID ::= 167

 id-TNLAssociationTransportLayerAddressNGRAN ProtocolIE-ID ::= 168

 id-EndpointIPAddressAndPort ProtocolIE-ID ::= 169

 id-LocationReportingAdditionalInfo ProtocolIE-ID ::= 170

 id-SourceToTarget-AMFInformationReroute ProtocolIE-ID ::= 171

 id-AdditionalULForwardingUPTNLInformation ProtocolIE-ID ::= 172

 id-SCTP-TLAs ProtocolIE-ID ::= 173

 id-SelectedPLMNIdentity ProtocolIE-ID ::= 174

 id-RIMInformationTransfer ProtocolIE-ID ::= 175

 id-GUAMIType ProtocolIE-ID ::= 176

 id-SRVCCOperationPossible ProtocolIE-ID ::= 177

 id-TargetRNC-ID ProtocolIE-ID ::= 178

 id-RAT-Information ProtocolIE-ID ::= 179

 id-ExtendedRATRestrictionInformation ProtocolIE-ID ::= 180

 id-QosMonitoringRequest ProtocolIE-ID ::= 181

 id-SgNB-UE-X2AP-ID ProtocolIE-ID ::= 182

 id-AdditionalRedundantDL-NGU-UP-TNLInformation ProtocolIE-ID ::= 183

 id-AdditionalRedundantDLQosFlowPerTNLInformation ProtocolIE-ID ::= 184

 id-AdditionalRedundantNGU-UP-TNLInformation ProtocolIE-ID ::= 185

 id-AdditionalRedundantUL-NGU-UP-TNLInformation ProtocolIE-ID ::= 186

 id-CNPacketDelayBudgetDL ProtocolIE-ID ::= 187

 id-CNPacketDelayBudgetUL ProtocolIE-ID ::= 188

 id-ExtendedPacketDelayBudget ProtocolIE-ID ::= 189

 id-RedundantCommonNetworkInstance ProtocolIE-ID ::= 190

 id-RedundantDL-NGU-TNLInformationReused ProtocolIE-ID ::= 191

 id-RedundantDL-NGU-UP-TNLInformation ProtocolIE-ID ::= 192

 id-RedundantDLQosFlowPerTNLInformation ProtocolIE-ID ::= 193

 id-RedundantQosFlowIndicator ProtocolIE-ID ::= 194

 id-RedundantUL-NGU-UP-TNLInformation ProtocolIE-ID ::= 195

 id-TSCTrafficCharacteristics ProtocolIE-ID ::= 196

 id-RedundantPDUSessionInformation ProtocolIE-ID ::= 197

 id-UsedRSNInformation ProtocolIE-ID ::= 198

 id-IAB-Authorized ProtocolIE-ID ::= 199

 id-IAB-Supported ProtocolIE-ID ::= 200

 id-IABNodeIndication ProtocolIE-ID ::= 201

 id-NB-IoT-PagingDRX ProtocolIE-ID ::= 202

 id-NB-IoT-Paging-eDRXInfo ProtocolIE-ID ::= 203

 id-NB-IoT-DefaultPagingDRX ProtocolIE-ID ::= 204

 id-Enhanced-CoverageRestriction ProtocolIE-ID ::= 205

 id-Extended-ConnectedTime ProtocolIE-ID ::= 206

 id-PagingAssisDataforCEcapabUE ProtocolIE-ID ::= 207

 id-WUS-Assistance-Information ProtocolIE-ID ::= 208

 id-UE-DifferentiationInfo ProtocolIE-ID ::= 209

 id-NB-IoT-UEPriority ProtocolIE-ID ::= 210

 id-UL-CP-SecurityInformation ProtocolIE-ID ::= 211

 id-DL-CP-SecurityInformation ProtocolIE-ID ::= 212

 id-TAI ProtocolIE-ID ::= 213

 id-UERadioCapabilityForPagingOfNB-IoT ProtocolIE-ID ::= 214

 id-LTEV2XServicesAuthorized ProtocolIE-ID ::= 215

 id-NRV2XServicesAuthorized ProtocolIE-ID ::= 216

 id-LTEUESidelinkAggregateMaximumBitrate ProtocolIE-ID ::= 217

 id-NRUESidelinkAggregateMaximumBitrate ProtocolIE-ID ::= 218

 id-PC5QoSParameters ProtocolIE-ID ::= 219

 id-AlternativeQoSParaSetList ProtocolIE-ID ::= 220

 id-CurrentQoSParaSetIndex ProtocolIE-ID ::= 221

 id-CEmodeBrestricted ProtocolIE-ID ::= 222

 id-EUTRA-PagingeDRXInformation ProtocolIE-ID ::= 223

 id-CEmodeBSupport-Indicator ProtocolIE-ID ::= 224

 id-LTEM-Indication ProtocolIE-ID ::= 225

 id-EndIndication ProtocolIE-ID ::= 226

 id-EDT-Session ProtocolIE-ID ::= 227

 id-UECapabilityInfoRequest ProtocolIE-ID ::= 228

 id-PDUSessionResourceFailedToResumeListRESReq ProtocolIE-ID ::= 229

 id-PDUSessionResourceFailedToResumeListRESRes ProtocolIE-ID ::= 230

 id-PDUSessionResourceSuspendListSUSReq ProtocolIE-ID ::= 231

 id-PDUSessionResourceResumeListRESReq ProtocolIE-ID ::= 232

 id-PDUSessionResourceResumeListRESRes ProtocolIE-ID ::= 233

 id-UE-UP-CIoT-Support ProtocolIE-ID ::= 234

 id-Suspend-Request-Indication ProtocolIE-ID ::= 235

 id-Suspend-Response-Indication ProtocolIE-ID ::= 236

 id-RRC-Resume-Cause ProtocolIE-ID ::= 237

 id-RGLevelWirelineAccessCharacteristics ProtocolIE-ID ::= 238

 id-W-AGFIdentityInformation ProtocolIE-ID ::= 239

 id-GlobalTNGF-ID ProtocolIE-ID ::= 240

 id-GlobalTWIF-ID ProtocolIE-ID ::= 241

 id-GlobalW-AGF-ID ProtocolIE-ID ::= 242

 id-UserLocationInformationW-AGF ProtocolIE-ID ::= 243

 id-UserLocationInformationTNGF ProtocolIE-ID ::= 244

 id-AuthenticatedIndication ProtocolIE-ID ::= 245

 id-TNGFIdentityInformation ProtocolIE-ID ::= 246

 id-TWIFIdentityInformation ProtocolIE-ID ::= 247

 id-UserLocationInformationTWIF ProtocolIE-ID ::= 248

 id-DataForwardingResponseERABList ProtocolIE-ID ::= 249

 id-IntersystemSONConfigurationTransferDL ProtocolIE-ID ::= 250

 id-IntersystemSONConfigurationTransferUL ProtocolIE-ID ::= 251

 id-SONInformationReport ProtocolIE-ID ::= 252

 id-UEHistoryInformationFromTheUE ProtocolIE-ID ::= 253

 id-ManagementBasedMDTPLMNList ProtocolIE-ID ::= 254

 id-MDTConfiguration ProtocolIE-ID ::= 255

 id-PrivacyIndicator ProtocolIE-ID ::= 256

 id-TraceCollectionEntityURI ProtocolIE-ID ::= 257

 id-NPN-Support ProtocolIE-ID ::= 258

 id-NPN-AccessInformation ProtocolIE-ID ::= 259

 id-NPN-PagingAssistanceInformation ProtocolIE-ID ::= 260

 id-NPN-MobilityInformation ProtocolIE-ID ::= 261

 id-TargettoSource-Failure-TransparentContainer ProtocolIE-ID ::= 262

 id-NID ProtocolIE-ID ::= 263

 id-UERadioCapabilityID ProtocolIE-ID ::= 264

 id-UERadioCapability-EUTRA-Format ProtocolIE-ID ::= 265

 id-DAPSRequestInfo ProtocolIE-ID ::= 266

 id-DAPSResponseInfoList ProtocolIE-ID ::= 267

 id-EarlyStatusTransfer-TransparentContainer ProtocolIE-ID ::= 268

 id-NotifySourceNGRANNode ProtocolIE-ID ::= 269

 id-ExtendedSliceSupportList ProtocolIE-ID ::= 270

 id-ExtendedTAISliceSupportList ProtocolIE-ID ::= 271

 id-ConfiguredTACIndication ProtocolIE-ID ::= 272

 id-Extended-RANNodeName ProtocolIE-ID ::= 273

 id-Extended-AMFName ProtocolIE-ID ::= 274

 id-GlobalCable-ID ProtocolIE-ID ::= 275

 id-QosMonitoringReportingFrequency ProtocolIE-ID ::= 276

 id-QosFlowParametersList ProtocolIE-ID ::= 277

 id-QosFlowFeedbackList ProtocolIE-ID ::= 278

 id-BurstArrivalTimeDownlink ProtocolIE-ID ::= 279

 id-ExtendedUEIdentityIndexValue ProtocolIE-ID ::= 280

 id-PduSessionExpectedUEActivityBehaviour ProtocolIE-ID ::= 281

 id-MicoAllPLMN ProtocolIE-ID ::= 282

 id-QosFlowFailedToSetupList ProtocolIE-ID ::= 283

 id-SourceTNLAddrInfo ProtocolIE-ID ::= 284

 id-ExtendedReportIntervalMDT ProtocolIE-ID ::= 285

 id-SourceNodeID ProtocolIE-ID ::= 286

 id-NRNTNTAIInformation ProtocolIE-ID ::= 287

 id-UEContextReferenceAtSource ProtocolIE-ID ::= 288

 id-LastVisitedPSCellList ProtocolIE-ID ::= 289

 id-IntersystemSONInformationRequest ProtocolIE-ID ::= 290

 id-IntersystemSONInformationReply ProtocolIE-ID ::= 291

 id-EnergySavingIndication ProtocolIE-ID ::= 292

 id-IntersystemResourceStatusUpdate ProtocolIE-ID ::= 293

 id-SuccessfulHandoverReportList ProtocolIE-ID ::= 294

 id-MBS-AreaSessionID ProtocolIE-ID ::= 295

 id-MBS-QoSFlowsToBeSetupList ProtocolIE-ID ::= 296

 id-MBS-QoSFlowsToBeSetupModList ProtocolIE-ID ::= 297

 id-MBS-ServiceArea ProtocolIE-ID ::= 298

 id-MBS-SessionID ProtocolIE-ID ::= 299

 id-MBS-DistributionReleaseRequestTransfer ProtocolIE-ID ::= 300

 id-MBS-DistributionSetupRequestTransfer ProtocolIE-ID ::= 301

 id-MBS-DistributionSetupResponseTransfer ProtocolIE-ID ::= 302

 id-MBS-DistributionSetupUnsuccessfulTransfer ProtocolIE-ID ::= 303

 id-MulticastSessionActivationRequestTransfer ProtocolIE-ID ::= 304

 id-MulticastSessionDeactivationRequestTransfer ProtocolIE-ID ::= 305

 id-MulticastSessionUpdateRequestTransfer ProtocolIE-ID ::= 306

 id-MulticastGroupPagingAreaList ProtocolIE-ID ::= 307

 id-MBS-SupportIndicator ProtocolIE-ID ::= 309

 id-MBSSessionFailedtoSetupList ProtocolIE-ID ::= 310

 id-MBSSessionFailedtoSetuporModifyList ProtocolIE-ID ::= 311

 id-MBSSessionSetupResponseList ProtocolIE-ID ::= 312

 id-MBSSessionSetuporModifyResponseList ProtocolIE-ID ::= 313

 id-MBSSessionSetupFailureTransfer ProtocolIE-ID ::= 314

 id-MBSSessionSetupRequestTransfer ProtocolIE-ID ::= 315

 id-MBSSessionSetupResponseTransfer ProtocolIE-ID ::= 316

 id-MBSSessionToReleaseList ProtocolIE-ID ::= 317

 id-MBSSessionSetupRequestList ProtocolIE-ID ::= 318

 id-MBSSessionSetuporModifyRequestList ProtocolIE-ID ::= 319

 id-MBS-ActiveSessionInformation-SourcetoTargetList ProtocolIE-ID ::= 323

 id-MBS-ActiveSessionInformation-TargettoSourceList ProtocolIE-ID ::= 324

 id-OnboardingSupport ProtocolIE-ID ::= 325

 id-TimeSyncAssistanceInfo ProtocolIE-ID ::= 326

 id-SurvivalTime ProtocolIE-ID ::= 327

 id-QMCConfigInfo ProtocolIE-ID ::= 328

 id-QMCDeactivation ProtocolIE-ID ::= 329

 id-PDUSessionPairID ProtocolIE-ID ::= 331

 id-NR-PagingeDRXInformation ProtocolIE-ID ::= 332

 id-RedCapIndication ProtocolIE-ID ::= 333

 id-TargetNSSAIInformation ProtocolIE-ID ::= 334

 id-UESliceMaximumBitRateList ProtocolIE-ID ::= 335

 id-M4ReportAmount ProtocolIE-ID ::= 336

 id-M5ReportAmount ProtocolIE-ID ::= 337

 id-M6ReportAmount ProtocolIE-ID ::= 338

 id-M7ReportAmount ProtocolIE-ID ::= 339

 id-IncludeBeamMeasurementsIndication ProtocolIE-ID ::= 340

 id-ExcessPacketDelayThresholdConfiguration ProtocolIE-ID ::= 341

 id-PagingCause ProtocolIE-ID ::= 342

 id-PagingCauseIndicationForVoiceService ProtocolIE-ID ::= 343

 id-PEIPSassistanceInformation ProtocolIE-ID ::= 344

 id-FiveG-ProSeAuthorized ProtocolIE-ID ::= 345

 id-FiveG-ProSeUEPC5AggregateMaximumBitRate ProtocolIE-ID ::= 346

 id-FiveG-ProSePC5QoSParameters ProtocolIE-ID ::= 347

 id-MBSSessionModificationFailureTransfer ProtocolIE-ID ::= 348

 id-MBSSessionModificationRequestTransfer ProtocolIE-ID ::= 349

 id-MBSSessionModificationResponseTransfer ProtocolIE-ID ::= 350

 id-MBS-QoSFlowToReleaseList ProtocolIE-ID ::= 351

 id-MBS-SessionTNLInfo5GC ProtocolIE-ID ::= 352

 id-TAINSAGSupportList ProtocolIE-ID ::= 353

 id-SourceNodeTNLAddrInfo ProtocolIE-ID ::= 354

 id-NGAPIESupportInformationRequestList ProtocolIE-ID ::= 355

 id-NGAPIESupportInformationResponseList ProtocolIE-ID ::= 356

 id-MBS-SessionFSAIDList ProtocolIE-ID ::= 357

 id-MBSSessionReleaseResponseTransfer ProtocolIE-ID ::= 358

 id-ManagementBasedMDTPLMNModificationList ProtocolIE-ID ::= 359

 id-EarlyMeasurement ProtocolIE-ID ::= 360

 id-BeamMeasurementsReportConfiguration ProtocolIE-ID ::= 361

 id-HFCNode-ID-new ProtocolIE-ID ::= 362

 id-GlobalCable-ID-new ProtocolIE-ID ::= 363

 id-TargetHomeENB-ID ProtocolIE-ID ::= 364

 id-HashedUEIdentityIndexValue ProtocolIE-ID ::= 365

 id-ExtendedMobilityInformation ProtocolIE-ID ::= 366

 id-NetworkControlledRepeaterAuthorized ProtocolIE-ID ::= 367

 id-AdditionalCancelledlocationReportingReferenceIDList ProtocolIE-ID ::= 368

 id-Selected-Target-SNPN-Identity ProtocolIE-ID ::= 369

 id-EquivalentSNPNsList ProtocolIE-ID ::= 370

 id-SelectedNID ProtocolIE-ID ::= 371

 id-SupportedUETypeList ProtocolIE-ID ::= 372

 id-AerialUEsubscriptionInformation ProtocolIE-ID ::= 373

 id-NR-A2X-ServicesAuthorized ProtocolIE-ID ::= 374

 id-LTE-A2X-ServicesAuthorized ProtocolIE-ID ::= 375

 id-NR-A2X-UE-PC5-AggregateMaximumBitRate ProtocolIE-ID ::= 376

 id-LTE-A2X-UE-PC5-AggregateMaximumBitRate ProtocolIE-ID ::= 377

 id-A2X-PC5-QoS-Parameters ProtocolIE-ID ::= 378

 id-FiveGProSeLayer2Multipath ProtocolIE-ID ::= 379

 id-FiveGProSeLayer2UEtoUERelay ProtocolIE-ID ::= 380

 id-FiveGProSeLayer2UEtoUERemote ProtocolIE-ID ::= 381

 id-CandidateRelayUEInformationList ProtocolIE-ID ::= 382

 id-SuccessfulPSCellChangeReportList ProtocolIE-ID ::= 383

 id-IntersystemMobilityFailureforVoiceFallback ProtocolIE-ID ::= 384

 id-TargetCellCRNTI ProtocolIE-ID ::= 385

 id-TimeSinceFailure ProtocolIE-ID ::= 386

 id-RANTimingSynchronisationStatusInfo ProtocolIE-ID ::= 387

 id-RAN-TSSRequestType ProtocolIE-ID ::= 388

 id-RAN-TSSScope ProtocolIE-ID ::= 389

 id-ClockQualityReportingControlInfo ProtocolIE-ID ::= 390

 id-RANfeedbacktype ProtocolIE-ID ::= 391

 id-QoSFlowTSCList ProtocolIE-ID ::= 392

 id-TSCTrafficCharacteristicsFeedback ProtocolIE-ID ::= 393

 id-DownlinkTLContainer ProtocolIE-ID ::= 394

 id-UplinkTLContainer ProtocolIE-ID ::= 395

 id-ANPacketDelayBudgetUL ProtocolIE-ID ::= 396

 id-QosFlowAdditionalInfoList ProtocolIE-ID ::= 397

 id-AssistanceInformationQoE-Meas ProtocolIE-ID ::= 398

 id-MBSCommServiceType ProtocolIE-ID ::= 399

 id-MobileIAB-Authorized ProtocolIE-ID ::= 400

 id-IAB-MTUserLocationInformation ProtocolIE-ID ::= 401

 id-MobileIABNodeIndication ProtocolIE-ID ::= 402

 id-NoPDUSessionIndication ProtocolIE-ID ::= 403

 id-MobileIAB-Supported ProtocolIE-ID ::= 404

 id-CN-MT-CommunicationHandling ProtocolIE-ID ::= 405

 id-FiveGCAction ProtocolIE-ID ::= 406

 id-PagingPolicyDifferentiation ProtocolIE-ID ::= 407

 id-DL-Signalling ProtocolIE-ID ::= 408

 id-PNI-NPN-AreaScopeofMDT ProtocolIE-ID ::= 409

 id-PNI-NPNBasedMDT ProtocolIE-ID ::= 410

 id-SNPN-CellBasedMDT ProtocolIE-ID ::= 411

 id-SNPN-TAIBasedMDT ProtocolIE-ID ::= 412

 id-SNPN-BasedMDT ProtocolIE-ID ::= 413

 id-Partially-Allowed-NSSAI ProtocolIE-ID ::= 414

 id-AssociatedSessionID ProtocolIE-ID ::= 415

 id-MBS-AssistanceInformation ProtocolIE-ID ::= 416

 id-BroadcastTransportFailureTransfer ProtocolIE-ID ::= 417

 id-BroadcastTransportRequestTransfer ProtocolIE-ID ::= 418

 id-BroadcastTransportResponseTransfer ProtocolIE-ID ::= 419

 id-TimeBasedHandoverInformation ProtocolIE-ID ::= 420

 id-DLDiscarding ProtocolIE-ID ::= 421

 id-PDUsetQoSParameters ProtocolIE-ID ::= 422

 id-PDUSetbasedHandlingIndicator ProtocolIE-ID ::= 423

 id-N6JitterInformation ProtocolIE-ID ::= 424

 id-ECNMarkingorCongestionInformationReportingRequest ProtocolIE-ID ::= 425

 id-ECNMarkingorCongestionInformationReportingStatus ProtocolIE-ID ::= 426

 id-SLPositioningRangingServiceInfo ProtocolIE-ID ::= xxx

 <<<<<<<<<<<<<<<<<<<< Changes End >>>>>>>>>>>>>>>>>>>>