**3GPP TSG-RAN WG4 Meeting #100-e *R4-211xxxx***

**Electronic Meeting, August 16-27, 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** |  | **rev** | **1** | **Current version:** | **16.8.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on measurement requirements in relaxed measurement  |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_UE\_pow\_sav-Core |  | ***Date:*** | 2021-08-06 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Change #1:SMTC-LP2 is added in SIB2/SIB4 in TEI-16 WI (R2-2000302). Then RAN4 had modified the intra-freq/inter-freq measurement delay requirements under idle/inactive state accordingly, e.g.However, relaxed measurements are discussed under a parallel WI so the impact of SMTC-LP2 is missed in 38.133 cl.4.2.2.9. In our opinion it is natrual for relaxed measurement to consider SMTC-LP2 too.Change #2:In the approved WF [R4-2009265], it is indicated that if T331 is running, the carriers which are configured for EMR shall not be performed with relaxed measurement. For these carriers which are configured for mobility (not for EMR), if UE has fulfilled low mobility or not-at-cell edge criteria, UE shall perform relaxed measurement. If a UE is configured with both EMR measurement carriers (T331 is running) and mobility measurement carriers, and the UE fulfills relaxed measurement criterion (either low mobility or not-at-cell edge criteria), when Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ, the measurement requirements are not defined. |
|  |  |
| ***Summary of change:*** | 1. Requirements for relaxed intra-freq measurement is updated to consider SMTC-LP2.
2. Specify the requirements when there are both non-relaxed measurement carriers and relaxed measurement carriers.

- Detection requirements: Ncarrier\_Relax \* Tdetect,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tdetect,NR\_Inter. - Measurements requirements: Ncarrier\_Relax \* Tmeasure,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tmeasure,NR\_Inter. - Evaluation requirements: Ncarrier\_Relax \* Tevaluate,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tevaluate,NR\_Inter.- The parameter Ncarrier\_Relax is the total number of configured inter-frequency carriers indicated by the serving cell and the number of NR inter-frequency carriers configured for idle mode CA measurements (while T331 is not running). - The parameter Ncarrier\_Non\_relax is the total number of NR inter-frequency carriers configured for idle mode CA measurements (while T331 is running). |
|  |  |
| ***Consequences if not approved:*** | The specification is not correct. |
|  |  |
| ***Clauses affected:*** |  4.2.2.9, 4.2.2.10; 4.2.2.11 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.533 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

----------------------------------------------------- Beginning of Change 1 ------------------------------------------------------------

#### 4.2.2.9 Measurements of intra-frequency NR cells for UE configured with relaxed measurement criterion

##### 4.2.2.9.1 Introduction

This clause contains the requirements for measurements on intra-frequency NR cells when Srxlev ≤ SIntraSearchP or Squal ≤ SIntraSearchQ and when the UE is configured any of the following relaxed measurement critera:

- Relaxed measurement criterion for UE with low mobility defined in clause 5.2.4.9.1 in [1],

- Relaxed measurement criterion for UE not-at-cell edge defined in clause 5.2.4.9.2 in [1],

- Both low mobility criterion and not-at-cell edge criterion as defined in clauses 5.2.4.9.1 and 5.2.4.9.2 in [1] respectively.

##### 4.2.2.9.2 Measurements for UE fulfilling low mobility criterion

This clause contains requirements for measurements on intra-frequency NR cells provided that:

- UE is configured with *lowMobilityEvalutation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured, and UE has fulfilled only the *lowMobilityEvalutation* [2] criterion.

The requirements defined in clause 4.2.2.3 apply for this clause except that:

- Tdetect,NR\_Intraas specified in Table 4.2.2.9.2-1.

- Tmeasure,NR\_Intra as specified in Table 4.2.2.9.2-1.

- Tevaluate,NR\_Intra as specified in Table 4.2.2.9.2-1.

Table 4.2.2.9.2-1: Tdetect,NR\_Intra, Tmeasure,NR\_Intra and Tevaluate,NR\_Intra

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DRX cycle length [s] | Scaling Factor (N1) | Tdetect,NR\_Intra [s] (number of DRX cycles) | Tmeasure,NR\_Intra [s] (number of DRX cycles) | Tevaluate,NR\_Intra[s] (number of DRX cycles) |
|  | FR1 | FR2Note1 |
| 0.32 | 1 | 8 | 11.52 x N1 x M2 x K1 (36 x N1 x M2 x K1) | 1.28 x N1 x M2 x K1 (4 x N1 x M2 x K1) | 5.12 x N1 x M2 x K1 (16 x N1 x M2 x K1) |
| 0.64 |  | 5 | 17.92 x N1 x K1 (28 x N1 x K1) | 1.28 x N1 x K1 (2 x N1 x K1) | 5.12 x N1 x K1 (8 x N1 x K1) |
| 1.28 |  | 4 | 32 x N1 x K1 (25 x N1 x K1) | 1.28 x N1 x K1 (1 x N1 x K1) | 6.4 x N1 x K1 (5 x N1 x K1) |
| 2.56 |  | 3 | 58.88 x N1 x K1 (23 x N1 x K1) | 2.56 x N1 x K1 (1 x N1 x K1) | 7.68 x N1 x K1 (3 x N1 x K1) |
| Note 1: Applies for UE supporting power class 2&3&4. For UE supporting power class 1, N1 = 8 for all DRX cycle length.Note 2: M2 = 1.5 if SMTC periodicity of measured intra-frequency cell > 20 ms; otherwise M2=1. When multiple SMTCs are configured, the SMTC periodicity in this note is the one used by the cell being identified.Note 3: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *lowMobilityEvalutation* [2] criterion. |

##### 4.2.2.9.3 Measurements for UE fulfilling not-at-cell edge criterion

This clause contains requirements for measurements on intra-frequency NR cells provided that:

- UE is configured with *cellEdgeEvaluation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criteria and *combineRelaxedMeasCondition* [2] not configured, and UE has fulfilled only the *cellEdgeEvaluation* [2] criterion.

The requirements defined in clause 4.2.2.3 apply for this clause except that:

- Tdetect,NR\_Intraas specified in Table 4.2.2.9.3-1.

- Tmeasure,NR\_Intra as specified in Table 4.2.2.9.3-1.

- Tevaluate,NR\_Intra as specified in Table 4.2.2.9.3-1.

Table 4.2.2.9.3-1: Tdetect,NR\_Intra, Tmeasure,NR\_Intra and Tevaluate,NR\_Intra

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DRX cycle length [s] | Scaling Factor (N1) | Tdetect,NR\_Intra [s] (number of DRX cycles) | Tmeasure,NR\_Intra [s] (number of DRX cycles) | Tevaluate,NR\_Intra[s] (number of DRX cycles) |
|  | FR1 | FR2Note1 |
| 0.32 | 1 | 8 | 11.52 x N1 x M2 x K1 (36 x N1 x M2 x K1) | 1.28 x N1 x M2 x K1 (4 x N1 x M2 x K1) | 5.12 x N1 x M2 x K1 (16 x N1 x M2 x K1) |
| 0.64 |  | 5 | 17.92 x N1 x K1 (28 x N1 x K1) | 1.28 x N1 x K1 (2 x N1 x K1) | 5.12 x N1 x K1 (8 x N1 x K1) |
| 1.28 |  | 4 | 32 x N1 x K1 (25 x N1 x K1) | 1.28 x N1 x K1 (1 x N1 x K1) | 6.4 x N1 x K1 (5 x N1 x K1) |
| 2.56 |  | 3 | 58.88 x N1 x K1 (23 x N1 x K1) | 2.56 x N1 x K1 (1 x N1 x K1) | 7.68 x N1 x K1 (3 x N1 x K1) |
| Note 1: Applies for UE supporting power class 2&3&4. For UE supporting power class 1, N1 = 8 for all DRX cycle length.Note 2: M2 = 1.5 if SMTC periodicity of measured intra-frequency cell > 20 ms; otherwise M2=1. When multiple SMTCs are configured, the SMTC periodicity in this note is the one used by the cell being identified.Note 3: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *cellEdgeEvaluation* [2] criterion. |

##### 4.2.2.9.4 Measurements for UE fulfilling low mobility and not-at-cell edge criteria

This clause contains requirements for measurements on intra-frequency NR cells provided that:

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion, and

- has also fulfilled both criteria, and

- less than 1 hour have passed since measurements for cell reselection were last performed

In this case the UE is not required to meet Tdetect,NR\_Intra, Tmeasure,NR\_Intra and Tevaluate,NR\_Intra as defined in Table 4.2.2.3-1.

------------------------------------------------------------- End of change 1 ------------------------------------------------------------

----------------------------------------------------- Beginning of Change 2 ------------------------------------------------------------

#### 4.2.2.10 Measurements of inter-frequency NR cells for UE configured with relaxed measurement criterion

##### 4.2.2.10.1 Introduction

This clause contains the requirements for measurements on inter-frequency NR cells when the UE is configured with any of following relaxed measurement criteria:

- Relaxed measurement criterion for UE with low mobility defined in clause 5.2.4.9.1 in [1],

- Relaxed measurement criterion for UE not-at-cell edge defined in clause 5.2.4. 9.2 in [1],

- Both low mobility criterion and not-at-cell edge criterion as defined in clauses 5.2.4. 9.1 and 5.2.4.9.2 in [1] respectively.

##### 4.2.2.10.2 Measurements for UE fulfilling low mobility criterion

This clause contains requirements for measurements on inter-frequency NR cells provided that:

- UE is configured with *lowMobilityEvalutation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured, and

- UE has fulfilled only the *lowMobilityEvalutation* [2] criterion.

The UE shall not relax measurements on NR inter-frequency carriers configured for idle mode CA/DC measurements (defined in clause 4.4) while T331 is running.

When Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ then the requirements are defined as follows: :

- Tdetect,NR\_Inter\_Relaxas specified in Table 4.2.2.10.2-1.

- Tmeasure,NR\_Inter\_Relax as specified in Table 4.2.2.10.2-1.

- Tevaluate,NR\_Inter\_Relax as specified in Table 4.2.2.10.2-1.

- The UE shall be able to evaluate whether a newly detectable inter-frequency NR cell meets the reselection criteria defined in TS38.304 [1] within Ncarrier\_Relax \* Tdetect,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tdetect,NR\_Inter. Cells which have been detected shall be measured at least every Ncarrier\_Relax \* Tmeasure,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tmeasure,NR\_Inter. The UE shall be able to evaluate that an already identified inter-frequency NR cell has met reselection criterion defined in TS 38.304 [1] within Ncarrier\_Relax \*Tevaluate,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tevaluate,NR\_Inter.

- The parameter Ncarrier\_Relax is the total number of inter-frequency carriers configured for mobility measurements and the number of inter-frequency carriers configured for mobility measurement and for idle mode CA/DC measurements (while T331 is not running).

- The parameter Ncarrier\_Non\_relax is the total number of NR inter-frequency carriers configured for idle mode CA/DC measurements (while T331 is running).

When Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ and the UE is configured with *highPriorityMeasRelax* [2] then the UE shall search for inter-frequency layers of higher priority at least every K2\*Thigher\_priority\_search seconds where Thigher\_priority\_search is described in clause 4.2.2.7 and, K2 = 60. Otherwise if the UE is not configured with *highPriorityMeasRelax* [2] then the UE shall search for inter-frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2.2.7.

Table 4.2.2.10.2-1: Tdetect,NR\_Inter\_Relax, Tmeasure,NR\_Inter\_Relax and Tevaluate,NR\_Inter\_Relax

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DRX cycle length [s] | Scaling Factor (N1) | Tdetect,NR\_Inter\_Relax [s] (number of DRX  | Tmeasure,NR\_Inter\_Relax [s] (number of DRX cycles) | Tevaluate,NR\_Inter\_Relax [s] (number of DRX cycles) |
|  | FR1 | FR2Note1 | cycles) |  |  |
| 0.32 | 1 | 8 | 11.52 x N1 x 1.5 x K1 (36 x N1 x 1.5 x K1) | 1.28 x N1 x 1.5 x K1 (4 x N1 x 1.5 x K1) | 5.12 x N1 x 1.5 x K1 (16 x N1 x 1.5 x K1) |
| 0.64 |  | 5 | 17.92x N1 x K1 (28 x N1 x K1) | 1.28 x N1 x K1 (2 x N1 x K1) | 5.12 x N1 x K1 (8 x N1 x K1) |
| 1.28 |  | 4 | 32 x N1 x K1 (25 x N1 x K1) | 1.28 x N1 x K1 (1 x N1 x K1) | 6.4 x N1 x K1 (5 x N1 x K1) |
| 2.56 |  | 3 | 58.88 x N1 x K1 (23 x N1 x K1) | 2.56 x N1 x K1 (1 x N1 x K1) | 7.68 x N1 x K1 (3 x N1 x K1) |
| Note 1: Applies for UE supporting power class 2&3&4. For UE supporting power class 1, N1 = 8 for all DRX cycle length.Note 2: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the low mobility. |

##### 4.2.2.10.3 Measurements for UE fulfilling not-at-cell edge criterion

This clause contains requirements for measurements on inter-frequency NR cells provided that:

- UE is configured with *cellEdgeEvaluation* [2] criterion, and UE has fulfilled or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured, and

- UE has fulfilled only the *cellEdgeEvaluation* [2] criterion.

The UE shall not relax measurements on NR inter-frequency carriers configured for idle mode CA/DC measurements (defined in clause 4.4) while T331 is running.

When Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ then the requirements defined in clause 4.2.2.4 apply for this clause except that:

- Tdetect,NR\_Inter\_Relaxas specified in Table 4.2.2.10.3-1.

- Tmeasure,NR\_Inter\_Relax as specified in Table 4.2.2.10.3-1.

- Tevaluate,NR\_Inter\_Relax as specified in Table 4.2.2.10.3-1.- The UE shall be able to evaluate whether a newly detectable inter-frequency NR cell meets the reselection criteria defined in TS38.304 [1] within Ncarrier\_Relax \* Tdetect,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tdetect,NR\_Inter. Cells which have been detected shall be measured at least every Ncarrier\_Relax \* Tmeasure,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tmeasure,NR\_Inter. The UE shall be able to evaluate that an already identified inter-frequency NR cell has met reselection criterion defined in TS 38.304 [1] within Ncarrier\_Relax \* Tevaluate,NR\_Inter\_Relax + Ncarrier\_Non\_relax \* Tevaluate,NR\_Inter.

- The parameter Ncarrier\_Relax is the total number of inter-frequency carriers configured for mobility measurements and the number of inter-frequency carriers configured for mobility measurement and for idle mode CA/DC measurements (while T331 is not running).

- The parameter Ncarrier\_Non\_relax is the total number of NR inter-frequency carriers configured for idle mode CA/DC measurements (while T331 is running).

When Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ and regardless of whether the UE is configured with *highPriorityMeasRelax* [2] or not, the UE shall search for inter-frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2.2.7

Table 4.2.2.10.3-1: Tdetect,NR\_Inter\_Relax, Tmeasure,NR\_Inter\_Relax and Tevaluate,NR\_Inter\_Relax

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DRX cycle length [s] | Scaling Factor (N1) | Tdetect,NR\_Inter\_Relax [s] (number of DRX  | Tmeasure,NR\_Inter\_Relax [s] (number of DRX cycles) | Tevaluate,NR\_Inter\_Relax [s] (number of DRX cycles) |
|  | FR1 | FR2Note1 | cycles) |  |  |
| 0.32 | 1 | 8 | 11.52 x N1 x 1.5 x K1 (36 x N1 x 1.5 x K1) | 1.28 x N1 x 1.5 x K1 (4 x N1 x 1.5 x K1) | 5.12 x N1 x 1.5 x K1 (16 x N1 x 1.5 x K1) |
| 0.64 |  | 5 | 17.92x N1 x K1 (28 x N1 x K1) | 1.28 x N1 x K1 (2 x N1 x K1) | 5.12 x N1 x K1 (8 x N1 x K1) |
| 1.28 |  | 4 | 32 x N1 x K1 (25 x N1 x K1) | 1.28 x N1 x K1 (1 x N1 x K1) | 6.4 x N1 x K1 (5 x N1 x K1) |
| 2.56 |  | 3 | 58.88 x N1 x K1 (23 x N1 x K1) | 2.56 x N1 x K1 (1 x N1 x K1) | 7.68 x N1 x K1 (3 x N1 x K1) |
| Note 1: Applies for UE supporting power class 2&3&4. For UE supporting power class 1, N1 = 8 for all DRX cycle length.Note 2: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *cellEdgeEvaluation* [2] criterion. |

##### 4.2.2.10.4 Measurements for UE fulfilling low mobility and not-at-cell edge criterion

This clause contains requirements for measurements on inter-frequency NR cells provided that:

- T331 timer is not running for EMR measurements on inter-frequency NR carrier, and

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion, and

- Has also fulfilled both criteria, and

- less than 1 hour have passed since measurements for cell reselection were last performed

In this case the UE is not required to meet Tdetect,NR\_Inter, Tmeasure,NR\_Inter and Tevaluate,NR\_Inter as defined in Table 4.2.2.4-1.

##### 4.2.2.11 Measurements of inter-RAT E-UTRAN cells for UE configured with relaxed measurement criterion

4.2.2.11.1 Introduction

This clause contains the requirements for measurements on inter-RAT E-UTRAN cells when the UE is configured with any of following relaxed measurement critera:

- Relaxed measurement criterion for UE with low mobility defined in clause 5.2.4.9.1 in [1],

- Relaxed measurement criterion for UE not-at-cell edge defined in clause 5.2.4.9.2 in [1],

- Both low mobility criterion and not-at-cell edge criterion as defined in clauses 5.2.4.9.1 and 5.2.4.9.2 in [1] respectively.

##### 4.2.2.11.2 Measurements for UE fulfilling low mobility criterion

This clause contains requirements for measurements on inter-RAT E-UTRAN cells provided that:

- T331 timer is not running for EMR measurements on inter-RAT E-UTRAN, and

- UE is configured with *lowMobilityEvalutation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured, and

- UE has fulfilled only the *lowMobilityEvalutation* [2] criterion.

The UE shall not relax measurements on inter-RAT E-UTRAN carriers configured for idle mode CA/DC measurements (defined in clause 4.4) while T331 is running.

When Srxlev ≤ SnonIntraSearchP and Squal ≤ SnonIntraSearchQ then the requirements defined in clause 4.2.2.5 apply for this clause except that:

- Tdetect,EUTRAN\_Relaxas specified in Table 4.2.2.11.2-1.

- Tmeasure,EUTRAN\_Relax as specified in Table 4.2.2.11.2-1.

- Tevaluate,EUTRAN\_Relax as specified in Table 4.2.2.11.2-1.

- The UE shall be able to evaluate whether a newly detectable inter-RAT E-UTRAN cell meets the reselection criteria defined in TS38.304 [1] within Ncarrier\_Relax \* Tdetect,EUTRAN\_Relax + Ncarrier\_Non\_relax \* Tdetect,EUTRAN. Cells which have been detected shall be measured at least every Ncarrier\_Relax \* Tmeasure,EUTRAN\_Relax + Ncarrier\_Non\_relax \* Tmeasure,EUTRAN. The UE shall be able to evaluate that an already identified inter-RAT E-UTRAN cell has met reselection criterion defined in TS 38.304 [1] within NEUTRAN carrier\_Relax \* Tevaluate,EUTRAN\_Relax + NEUTRAN carrier\_Non\_relax \* Tevaluate,EUTRAN.

- The parameter NEUTRAN carrier\_Relax is the total number of inter-RAT E-UTRAN carriers configured for mobility measurements and the number of inter-RAT E-UTRAN carriers configured for mobility measurement and for idle mode CA/DC measurements (while T331 is not running)

- The parameter NEUTRAN carrier\_Non\_relax is the total number of inter-RAT E-UTRAN carriers configured for idle mode CA/DC measurements (while T331 is running).

When Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ and the UE is configured with *highPriorityMeasRelax* [2] then the UE shall search for E-UTRA inter-RAT frequency layers of higher priority at least every K2\*Thigher\_priority\_search seconds where Thigher\_priority\_search is described in clause 4.2.2.7 and, K2 = 60. Otherwise if the UE is not configured with *highPriorityMeasRelax* [2] then the UE shall search for E-UTRA inter-RAT frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2.2.7.

Table 4.2.2.11.2-1: Tdetect,EUTRAN\_Relax, Tmeasure,EUTRAN\_Relax, and Tevaluate,EUTRAN\_Relax

|  |  |  |  |
| --- | --- | --- | --- |
| DRX cycle length [s] | Tdetect,EUTRAN\_Relax [s] (number of DRX cycles) | Tmeasure,EUTRAN\_Relax [s] (number of DRX cycles) | Tevaluate,EUTRAN\_Relax[s] (number of DRX cycles) |
| 0.32 | 11.52 x K1 (36 x K1) | 1.28 x K1 (4 x K1) | 5.12 x K1 (16 x K1) |
| 0.64 | 17.92 x K1 (28 x K1) | 1.28 x K1 (2 x K1) | 5.12 x K1 (8 x K1) |
| 1.28 | 32 x K1 (25 x K1) | 1.28 x K1 (1 x K1) | 6.4 x K1 (5 x K1) |
| 2.56 | 58.88 x K1 (23 x K1) | 2.56 (1 x K1) | 7.68 x K1 (3 x K1) |
| Note 1: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *lowMobilityEvalutation* [2] criterion. |

##### 4.2.2.11.3 Measurements for UE fulfilling with not-at-cell edge criterion

This clause contains requirements for measurements on inter-RAT E-UTRAN cells provided that:

- T331 timer is not running for EMR measurements on inter-RAT E-UTRAN, and

- UE is configured with *cellEdgeEvaluation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured, and

- UE has fulfilled only the *cellEdgeEvaluation* [2] criterion.

The UE shall not relax measurements on inter-RAT E-UTRAN carriers configured for idle mode CA/DC measurements (defined in clause 4.4) while T331 is running.

When Srxlev ≤ SnonIntraSearchP and Squal ≤ SnonIntraSearchQ then the requirements defined in clause 4.2.2.5 apply for this clause except that:

- Tdetect,EUTRAN\_Relaxas specified in Table 4.2.2.11.3-1.

- Tmeasure,EUTRAN\_Relax as specified in Table 4.2.2.11.3-1.

- Tevaluate,EUTRAN\_Relax as specified in Table 4.2.2.11.3-1.

- The UE shall be able to evaluate whether a newly detectable inter-RAT E-UTRAN cell meets the reselection criteria defined in TS38.304 [1] within Ncarrier\_Relax \* Tdetect,EUTRAN\_Relax + Ncarrier\_Non\_relax \* Tdetect,EUTRAN. Cells which have been detected shall be measured at least every Ncarrier\_Relax \* Tmeasure,EUTRAN\_Relax + Ncarrier\_Non\_relax \* Tmeasure,EUTRAN. The UE shall be able to evaluate that an already identified inter-RAT E-UTRAN cell has met reselection criterion defined in TS 38.304 [1] within NEUTRAN carrier\_Relax \* Tevaluate,EUTRAN\_Relax + NEUTRAN carrier\_Non\_relax \* Tevaluate,EUTRAN.

- The parameter NEUTRAN carrier\_Relax is the total number of inter-RAT E-UTRAN carriers configured for mobility measurements and the number of inter-RAT E-UTRAN carriers configured for mobility measurement and for idle mode CA/DC measurements (while T331 is not running)

- The parameter NEUTRAN carrier\_Non\_relax is the total number of inter-RAT E-UTRAN carriers configured for idle mode CA/DC measurements (while T331 is running).

When Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ and regardless of whether the UE is configured with *highPriorityMeasRelax* [2] or not, the UE shall search for inter-RAT E-UTRAN frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2.2.7.

Table 4.2.2.11.3-1: Tdetect,EUTRAN\_Relax, Tmeasure,EUTRAN\_Relax, and Tevaluate,EUTRAN\_Relax

|  |  |  |  |
| --- | --- | --- | --- |
| DRX cycle length [s] | Tdetect,EUTRAN [s] (number of DRX cycles) | Tmeasure,EUTRAN [s] (number of DRX cycles) | Tevaluate,EUTRAN[s] (number of DRX cycles) |
| 0.32 | 11.52 x K1 (36 x K1) | 1.28 x K1 (4 x K1) | 5.12 x K1 (16 x K1) |
| 0.64 | 17.92 x K1 (28 x K1) | 1.28 x K1 (2 x K1) | 5.12 x K1 (8 x K1) |
| 1.28 | 32 x K1 (25 x K1) | 1.28 x K1 (1 x K1) | 6.4 x K1 (5 x K1) |
| 2.56 | 58.88 x K1 (23 x K1) | 2.56 x K1 (1 x K1) | 7.68 x K1 (3 x K1) |
| Note 1: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *lowMobilityEvalutation* [2] criterion. |

##### 4.2.2.11.4 Measurements for UE fulfilling low mobility and not-at-cell edge criterion

This clause contains requirements for measurements on inter-RAT E-UTRAN cells provided that:

- T331 timer is not running for EMR measurements on inter-RAT E-UTRAN, and

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion, and

- has also fulfilled both criteria, and

- less than 1 hour have passed since measurements for cell reselection were last performed,

In this case the UE is not required to meet Tdetect,EUTRAN , Tmeasure,EUTRAN and Tevaluate,EUTRAN as defined in Table 4.2.2.5-1.

------------------------------------------------------------- End of change 2 ------------------------------------------------------------