**3GPP TSG-RAN WG4 Meeting #100-eR4-21xxxxx**

**Electronic Meeting, 16 – 27 August, 2021**

**Agenda item:** 6.1.6.1

**Source:** Moderator (Huawei)

**Title:** Email discussion summary for [100-e][209] NR\_pos\_1

**Document for:** Information

# Introduction

The scope of this email discussion includes the following agenda items:

|  |
| --- |
| 6.1.6.1 RRM core requirements maintenance (38.133) [NR\_pos-Core]6.1.6.1.1 PRS-RSTD measurement requirements [NR\_pos-Core]6.1.6.1.2 PRS-RSRP measurement requirements [NR\_pos-Core]6.1.6.1.3 UE Rx-Tx time difference measurement requirements [NR\_pos-Core]6.1.6.1.4 Other requirements |

In providing comments, companies are encouraged to:

* Ensure that the comments are inserted in the latest version of the document by checking the folder before uploading
* Use “Track changes” to help identify added comments/changes
* Pay attention to the rule for shortening file name

# Topic #1: RSTD measurement period

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc** | **Company** | **Proposals / Observations** |
| [**R4-2111983**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2111983.zip) | CATT | **Proposal 1: No relation between the observation window of N and observation window of Lavailable\_PRS。****Proposal 2: Suggest the following text for the Lavailable\_PRS captured in the specification:** **“**$ L\_{available\\_PRS,i}$ **is the time duration of available PRS to be measured in** $T\_{available\\_PRS,i}$**, and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26].** * **For calculating**$ L\_{available\\_PRS,i}$**, only the resources unmuted and fully or partially covered by the MG are considered.”**

**Proposal 3: When multiple PFLs are configured, which PFL is assumed measured is up to UE implementation. But the PFL with long periodicity PRS is always prioritized.** **Proposal 4: Measurement requirements do not apply if some of the PRS resources in the PFL can be measured with periodicity shorter than or equal to 160 ms. i.e. none of the PRS resources in the PFL would be measured.** |
| [**R4-2111985**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2111985.zip) | CATT | CR |
| [**R4-2112540**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112540.zip) | vivo | **Proposal 1: The measurement period requirements when muting option 1 is configured are applicable when there are PRS resources available during min (10240 ms, *Tprs \* dl-PRS-MutingBitRepetitionFactor-r16*)**. **Proposal 2: No****further enhancement for the case where *Tprs \* dl-PRS-MutingBitRepetitionFactor-r16 \* L < 10240.*****Proposal 3: When muting option 2 is configured, the measurement accuracy requirements may not be met if the least number of repetitions defined in accuracy requirements cannot be ensured.****Proposal 4: Relation between the observation windows of Lavailable\_PRS** **and UE processing capability ‘N’ has already taken into account in the existing measurement period requirements.****Proposal 5: If MG pattern is reconfigured during measurement period, the UE shall continue and complete the on-going RSTD measurements with updated MG pattern. No measurement period requirements for reconfiguration are specified.** |
| [**R4-2112563**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112563.zip) | vivo | CR |
| [**R4-2113153**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2113153.zip) | Intel Corporation | ***Proposal 1: The measurement period defined in [2] can be applicable for PRS configuration cases with muting Option 2******Proposal 2: Measurement requirements do not apply if some of the PRS resources in the PFL can be measured with periodicity shorter or equal to 160 ms. i.e. none of the PRS resources in the PFL would be measured.*** |
| [**R4-2113257**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2113257.zip) | OPPO | **Proposal 1: Requirement applicability for PRS muting pattern is not necessary and network should guarantee that each PRS resource configured to the UE is available for measurement.** **Proposal 2: Do not discuss further enhancement when Tprs\*L\**dl-PRS-MutingBitRepetitionFactor-r16*<10240ms, and keep the current agreements in this release.****Proposal 3: Do not introduce additional clarification for muting option 2.****Proposal 4: There is no relation between the observation windows Lavailable\_PRS,i and window T.** |
| [**R4-2113258**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2113258.zip) | OPPO | CR |
| [**R4-2114193**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114193.zip) | Qualcomm Incorporated | **Proposal 1: Clarify in TS 38.133 that Rel-16 PRS-based measurements are supported with per-UE measurement gaps only. Tables 9.1.2-2 and 9.1.2-3 would be modified to exclude the applicability of per-FR measurement gaps for positioning measurements. Applicability conditions for positioning measurements in sec 9.9.1 would explicitly mention per-UE measurement gaps.** |
| [**R4-2114233**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114233.zip) | Nokia, Nokia Shanghai Bell | Observation 1 : The two windows of *P* and *T* are related to measurement period, especially when T > Tavailable\_PRS,i, . The option-2 “no relation between the two observation windows” is incorrect.Observation 2 : If a UE processing time *T* exceeds *P* *(* T > Tavailable\_PRS,i), some of allocated PRS resources in every Tms cannot be measured. It is not clear if the missed PRS resource is included in the set of measurement PRS resource slots or not.Observation 3 : Although we share the problem statement in observation-1 and -2, this issue is close to measurement period optimization issue as enhancement.Proposal 1 : We agree to keep the current settings of $\left⌈\frac{L\_{PRS,i}}{N}\right⌉$ without any change in Rel-16.  - Further enhancement related to the observation window and UE processing capability are discussed in Rel-17. |
| [**R4-2114269**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114269.zip) | Huawei, HiSilicon | **Proposal 1: Muting requirements apply for a resource provided that the first** $min(L,\frac{10240}{T\_{per}^{PRS}\*T\_{muting}^{PRS}}) $**bits of the muting pattern for the resource is not all-zero.****Proposal 2: Do not introduce further enhancement to muting requirements in Rel-16.****Proposal 3: Do not introduce additional clarification regarding option 2 muting.** **Proposal 4: Confirm the observation window of Lprs is Tavailable\_PRS,i, and do not introduce additional scaling factor to current requirements.** **Proposal 5: Clarify the definition of Lprs:**$L\_{available\\_PRS,i}$ **is the time duration of PRS resources to be measured in the positioning frequency layer i that fall within MGs and are not muted over the time period Tavailable\_PRS,i, and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]****Proposal 6: Clarify that the requirements do not apply if PRS configuration exceeds any of the UE capabilities in *NR-DL-PRS-ResourcesCapability*.** |
| [**R4-2114270**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114270.zip) | Huawei, HiSilicon | CR |

## Open issues summary

*Proposal 3&4 from CATT R4-2111983, Proposal 1 from QC R4-2114193, and Proposal 2 from Intel R4-2113153 are treated in Topic #4.*

### Sub-topic 1-1: Remaining issues with PRS muting

#### Issue 1-1-1: Applicability condition for option-1 muting

* Proposals
	+ Option 1a (vivo)
		- Define Applicability condition for option-1 muting:
			* The measurement period requirements when muting option 1 is configured are applicable when there are PRS resources available during min (10240 ms, Tprs \* dl-PRS-MutingBitRepetitionFactor-r16).
	+ Option 1b (HW)
		- Define Applicability condition for option-1 muting:
			* The requirements apply provided that
				+ none of the PRS resource instances is muted in case $T\_{per,j}^{PRS}\*T\_{muting,j}^{PRS}>10240ms$; or
				+ the first $min(L,\frac{10240}{T\_{per,j}^{PRS}\*T\_{muting,j}^{PRS}})$ bits of $\left\{b^{1}\right\}$ is not all-zero in case $T\_{per,j}^{PRS}\*T\_{muting,j}^{PRS} \leq 10240ms$
	+ Option 2 (OPPO)
		- Requirement applicability for PRS muting pattern is not necessary and network should guarantee that each PRS resource configured to the UE is available for measurement.
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 1-1-2: Enhancement for the case $T\_{per,j}^{PRS}\*T\_{muting,j}^{PRS} \leq 10240ms$

* Proposals
	+ Option 1 (vivo, OPPO, HW, QC)
		- No further enhancement for the case where Tprs \* dl-PRS-MutingBitRepetitionFactor-r16 \* L < 10240.
* Recommended WF
	+ It seems all contributing companies suggest no further enhancement, so moderator suggests to agree on the following statement:
		- No further enhancement on the requirements for the case where Tprs \* dl-PRS-MutingBitRepetitionFactor-r16 \* L < 10240 would be introduced in Rel-16.
	+ Discuss if the Recommended WF is agreeable or not.

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 1-1-3: Considration of muting option-2

* Proposals
	+ Option 1 (vivo)
		- When muting option 2 is configured, the measurement accuracy requirements may not be met if the least number of repetitions defined in accuracy requirements cannot be ensured.
	+ Option 2 (OPPO, Intel, HW, QC)
		- Do not introduce additional clarification for muting option 2.
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 1-1-4: General applicability with PRS muting

* Proposals
	+ Option 1 (QC)
		- When all the resources from a PRS resource set or PFL are muted, then that PRS resource set or PFL can be ignored for the purpose of the measurement requirements.
		- Measurement requirements do not apply to any PRS resources that are muted, they are not transmitted by the TRP and cannot be measured by the UE.
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

### Sub-topic 1-2: Parameter $L\_{available\\_PRS,i} $

#### Issue 1-2-1: Observation window

* Proposals
	+ Option 1a (CATT, OPPO)
		- No relation between the observation window of N and observation window of $L\_{available\\_PRS,i}$
	+ Option 1b (vivo, HW)
		- Relation between the observation windows of Lavailable\_PRS and UE processing capability ‘N’ has already taken into account in the existing measurement period requirements
	+ Option 2 (Nokia)
		- We agree to keep the current settings of $\left⌈\frac{L\_{PRS,i}}{N}\right⌉ $without any change in Rel-16.
		- Further enhancement related to the observation window and UE processing capability are discussed in Rel-17
* Recommended WF
	+ 4 companies (CATT, OPPO, vivo, HW) suggest that there is no relation between the two observation windows, or the relation is already considered in the current requirements, so suggest no change to the current requirements.
	+ 1 company (Nokia) suggests that there is some relation between the two observation windows, and some additional scaling to the current requirements may be needed, but agrees to keep the current requirements and further discuss in Rel-17
	+ Based on the status, moderator suggests to agree on the following statement and close the issue for Rel-16:
		- No update to requirements for the relation between observation window of $L\_{available\\_PRS,i}$ and observation window of capability N would be introduced in Rel-16.
	+ Discuss if the Recommended WF is agreeable or not.

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 1-2-1: Update to the definition of $L\_{available\\_PRS,i}$

* Proposals
	+ Option 1a (CATT)
		- $L\_{available\\_PRS,i}$ is the time duration of available PRS to be measured in $T\_{available\\_PRS,i}$, and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26].
			* For calculating$ L\_{available\\_PRS,i}$, only the resources unmuted and fully or partially covered by the MG are considered.
	+ Option 1b (HW)
		- $L\_{available\\_PRS,i}$ is the time duration of PRS resources to be measured in the positioning frequency layer i that fall within MGs and are not muted over the time period Tavailable\_PRS,i, and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]
* Recommended WF
	+ The two options are rather similar, so moderators suggests to agree on the following updated definition of $L\_{available\\_PRS,i}$ based on a merge between them:
		- $L\_{available\\_PRS,i}$ is the time duration of available PRS in the positioning frequency layer i to be measured in $T\_{available\\_PRS,i}$, and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26].
			* For calculating$ L\_{available\\_PRS,i}$, only the resources unmuted and fully or partially covered by the MG are considered.
	+ Discuss if the Recommended WF is agreeable or not.

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

### Sub-topic 1-3: Others

#### Issue 1-3-1: Impact of MG reconfiguration

* Proposals
	+ Option 1 (vivo)
		- If MG pattern is reconfigured during measurement period, the UE shall continue and complete the on-going RSTD measurements with updated MG pattern. No measurement period requirements for reconfiguration are specified..
* Recommended WF
	+ In RAN4#99-e, the following was agreed in WF R4-2108294, and it seems option 1 is a bit different from the agreement.

|  |
| --- |
| * MG reconfiguration per UE request
	+ RAN4 does not specify the exact measurement period extension due to MG reconfiguration during the measurement period
	+ Add the following text to TS 38.133 sections 9.9.2.5, 9.9.3.5 and 9.9.4.5:
		- If during the measurement period of one or more positioning frequency layers, the MG pattern is reconfigured, the measurement period can be longer.
	+ For MG reconfiguration during measurement period not per UE request, apply same requirements as MG reconfiguration based on UE request.
 |

* + Further discuss whether to adopt option 1 or keep the existing agreement.

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 1-3-2: Applicability condition on measurement capability

* Proposals
	+ Option 1 (HW)
		- Clarify that the requirements do not apply if PRS configuration exceeds any of the UE capabilities in *NR-DL-PRS-ResourcesCapability*
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

## Companies views’ collection for 1st round

### Open issues

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2111985 (CATT) |  |
|  |
|  |
| R4-2112563 (vivo) |  |
|  |
|  |
| R4-2113258 (OPPO) |  |
|  |
|  |
| R4-2114270 (HW) |  |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | *Tentative agreements:**Candidate options:**Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #2: Other issues

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc** | **Company** | **Proposals / Observations** |
| [**R4-2111987**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2111987.zip) | CATT | CR |
| [**R4-2112543**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112543.zip) | vivo | **Proposal 1: When multiple PFLs are configured, the PFL under measurement for positioning is assumed for CCSF calculation for an RRM frequency layer.****Proposal 2: CCSF calculation for an RRM frequency layer is the same as Rel-15 by assuming the PFL under measurement as the candidate positioning frequency layer.****Proposal 3: Long periodicity measurement requirements apply even if some of the PRS resources in the PFL can be measured with periodicity shorter or equal to 160ms.****Proposal 4: If at least part of a PRS resource, including at least the minimum number of repetitions specified in the accuracy requirements, is fully covered by MGL excluding RF switching time, then the PRS resource is considered being fully covered by MGL.** **Proposal 5: If the search window defined by *nr-DL-PRS-ExpectedRSTD* and *nr-DL-PRS-ExpectedRSTD-Uncertainty* together is not covered by MGL, the UE is supposed to do PRS measurement within the entire MGL.** |
| [**R4-2112569**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112569.zip) | vivo | CR |
| [**R4-2113263**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2113263.zip) | OPPO | **Proposal 1: Support option 2: long-periodicity measurement requirements do not apply if some of the PRS resources in the PFL can be measured with periodicity shorter or equal to 160ms.****Proposal 2: Further discuss the following methods to calculate the CSSF for an RRM layer when multiple PFLs are configured:*** **Use the maximum of intermediate CSSF(i) values and each of the intermediate CSSF(i) is calculated assuming that PFL-i and all RRM layers are being measured.**
* **Calculate the CSSF for RRM frequency layers assuming the merged PFL is measured**

**Proposal 3: A PRS resource is overlapped with MG if the minimum number of repetitions specified in the accuracy requirements are covered by the MGL excluding RF switching time.** **Proposal 4: The measurement delay and accuracy requirements do not apply for a PRS resource not overlapped with MG.****Proposal 5: For the calculation of CSSF, a PFL should be excluded if none of PRS resources in this PFL are overlapped with MG.** |
| [**R4-2114065**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114065.zip) | Nokia, Nokia Shanghai Bell | 1. The statement ‘When multiple PFLs are configured by the LMF, the order of measurement and processing of the PFLs is up to UE implementation’ needs to be specified in TS 38.133.
2. When multiple PFLs are configured by the LMF, CSSF for an RRM frequency layer MO *i* is determined by:

a) excluding MG occasions for long periodicity measurements for which no RRM frequency layers need to be measured; b) adjusting for the remaining MG occasions the ratio Ri accordingly for RRM frequency layer MO *i*; c) defining Mintra and Minter MO candidates for these remaining MG occasions, applying, depending on MG sharing scheme, coefficients Kintra and Kinter, thereby accounting for maximum one PFL contributing to Minter, which does not qualify for a long periodicity measurement, as MO candidate per MG occasion and d) selecting the maximum out of these remaining MG occasions.1. Regarding long periodicity measurement, we support option 2, i.e. measurement requirements do not apply if some of the PRS resources in the PFL can be measured with periodicity shorter or equal to 160 ms.
2. Add a definition of the term ‘PRS resource instance’ in TS 38.133.
 |
| [**R4-2114066**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114066.zip) | Nokia, Nokia Shanghai Bell | CR |
| [**R4-2114195**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114195.zip) | Qualcomm Incorporated | **Observation 1: In the extreme (corner) case in which all the resources within a PRS resource set or PFL are muted, then that PRS resource set or PFL can be ignored for the purpose of the measurement requirements.****Observation 2: Overestimation of N\_muting can be avoided by the network by configuring a muting bitmap of the minimum possible length so that the muting pattern does not repeat within the bitmap.****Proposal 1: The starting point for the PRS-RSTD measurement period should be as follows: “The time**$ T\_{RSTD, Total}$ ***s*tarts from the first MG instance aligned with a DL PRS resource(s) in the assistance data after both the *NR-TDOA-ProvideAssistanceData* message and *NR-TDOA-RequestLocationInformation* message are delivered from LMF to the physical layer of UE via LPP [34].”****Proposal 2: The starting point for the PRS-RSRP measurement period should be as follows: “When PRS-RSRP measurements are configured for DL-AoD, the time** $T\_{PRS-RSRP,total}$ **starts from the first MG instance aligned with DL PRS resources in the assistance data after both the *NR-DL-AoD-RequestLocationInformation* message and *NR-DL-AoD-ProvideAssistanceData* message from LMF via LPP [34] are delivered to the physical layer of UE.”****Proposal 3:** **The starting point for the UE Rx-Tx measurement period should be as follows:** **“The time** $T\_{UERxTx,Total}$ **starts from the first MG instance aligned with DL PRS resources in the assistance data after both the *NR-Multi-RTT-RequestLocationInformation* message and *NR-Multi-RTT-ProvideAssistanceData* message from LMF via LPP [34] are delivered to the physical layer of UE.”****Proposal 4: The current measurement period requirement is directly proportional to** $\left⌈\frac{L\_{available\\_PRS,i}}{N\_{i}}\right⌉\left⌈\frac{T\_{i}}{T\_{available\\_PRS,i}}\right⌉$**. No further adjustment is needed to account for the ratio** $\frac{T\_{i}}{T\_{available\\_PRS,i}}$**.****Proposal 5: When multiple PFLs are configured,**$ $**CSSF within gap would be calculated as follows:**1. **Let M be the number of PFLs configured by the LMF. M iterations are performed to calculate the final CSSF within gap for RRM measurements and PFLs.**
2. **In each iteration select one of the M PFLs and calculate CSSF within gap as agreed by RAN4 for the case of a single PFL.**
3. **Repeat step b M times, each time selecting a different PFL.**
4. **After all the iterations are completed, we have M values of** $CSSF\_{withn\\_gap, i}$ **for each RRM measurement object** $i$ **and M values for PFLs.**
5. **For each measurement object** $i$ **set** $CSSF\_{withn\\_gap, i}$ **to the maximum of the M values is step d. For all the PFLs set** $CSSF\_{withn\\_gap, i}$ **to the maximum of the M values calculated in step d.**

**Proposal 6: Measurement requirements do not apply if some of the PRS resources in the PFL can be measured with periodicity shorter or equal to 160 ms. i.e. none of the PRS resources in the PFL would be measured.****Proposal 7: A PRS resource is considered to be “fully covered by the MG”** **if at least the minimum number of repetitions specified in the accuracy requirements are covered by the MGL excluding RF switching time.****Proposal 8: Measurement requirements apply only for PRS resources that are “fully covered by the MG.”** |
| [**R4-2114278**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114278.zip) | Huawei, HiSilicon | **Proposal 1: For defining CSSF for an RRM frequency layer,*** **N intermediate CSSF values would be calculated, where N is the number of PFLs and each intermediate CSSF value accounts for only one of the PFLs.**
* **The CSSF value for the RRM frequency layer is the highest one among the N intermediate CSSF values.**

**Proposal 2: Measurement requirements do not apply if some of the PRS resources in a PFL with Tavailable\_PRS,i > 160ms can be measured with periodicity <= 160ms.****Proposal 3: Take into account expected RSTD and expected RSTD uncertainty in defining overlap between PRS resource and MG.** |
| [**R4-2114279**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114279.zip) | Huawei, HiSilicon | CR |

## Open issues summary

*QC CR R4-2114205 is treated in this topic. Observation 1&2 and Proposal 4 of QC R4-2114195 are treated under Topic #1.*

### Sub-topic 2-1 CSSF

#### Issue 2-1-1: Selection of one PFL in CSSF calculation

* Proposals
	+ Option 1 (vivo)
		- When multiple PFLs are configured, the PFL under measurement for positioning is assumed for CCSF calculation for an RRM frequency layer.
		- CCSF calculation for an RRM frequency layer is the same as Rel-15 by assuming the PFL under measurement as the candidate positioning frequency layer.
	+ Option 2a (OPPO, HW)
		- For defining CSSF for an RRM frequency layer,
			* N intermediate CSSF values would be calculated, where N is the number of PFLs and each intermediate CSSF value accounts for only one of the PFLs.
			* The CSSF value for the RRM frequency layer is the highest one among the N intermediate CSSF values.
	+ Option 2b (QC)
		- When multiple PFLs are configured, CSSF within gap would be calculated as follows:
			* Let M be the number of PFLs configured by the LMF. M iterations are performed to calculate the final CSSF within gap for RRM measurements and PFLs.
			* In each iteration select one of the M PFLs and calculate CSSF within gap as agreed by RAN4 for the case of a single PFL.
			* Repeat step b M times, each time selecting a different PFL.
			* After all the iterations are completed, we have M values of $CSSF\_{withn\\_gap, i}$ for each RRM measurement object $i$ and M values for PFLs.
			* For each measurement object $i$ set $CSSF\_{withn\\_gap, i}$ to the maximum of the M values is step d. For all the PFLs set $CSSF\_{withn\\_gap, i}$ to the maximum of the M values calculated in step d.
	+ Option 3a (OPPO)
		- Calculate the CSSF for RRM frequency layers assuming the merged (short periodicity) PFL is measured.
	+ Option 3b (Nokia)
		- The statement ‘When multiple PFLs are configured by the LMF, the order of measurement and processing of the PFLs is up to UE implementation’ needs to be specified in TS 38.133.
		- When multiple PFLs are configured by the LMF, CSSF for an RRM frequency layer MO i is determined by:
			* a) excluding MG occasions for long periodicity measurements for which no RRM frequency layers need to be measured;
			* b) adjusting for the remaining MG occasions the ratio Ri accordingly for RRM frequency layer MO i;
			* c) defining Mintra and Minter MO candidates for these remaining MG occasions, applying, depending on MG sharing scheme, coefficients Kintra and Kinter, thereby accounting for maximum one PFL contributing to Minter, which does not qualify for a long periodicity measurement, as MO candidate per MG occasion and
			* d) selecting the maximum out of these remaining MG occasions.
* Recommended WF
	+ Further discuss
	+ The difference between option 2a and 2b is that in option 2a the ‘max’ approach is only used to derive CSSF for RRM, while in option 2b it is also used to derive CSSF for PFL
	+ The difference between option 3a and 3b is that in option 3a the ‘merge’ is only among short periodicity PFLs, while in option 3b it is also among all PFLs

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 2-1-2: Requirement applicability for long periodicity measurement

* Proposals
	+ Option 1 (CATT, Intel, OPPO, Nokia, QC, HW)
		- Measurement requirements do not apply if some of the PRS resources in the PFL can be measured with periodicity shorter than or equal to 160 ms. i.e. none of the PRS resources in the PFL would be measured.
	+ Option 2 (vivo)
		- Long periodicity measurement requirements apply even if some of the PRS resources in the PFL can be measured with periodicity shorter or equal to 160ms
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

### Sub-topic 2-2 PRS resource being oberlapped with MG

#### Issue 2-2-1: Definition

* Proposals
	+ Option 1 (vivo)
		- If at least part of a PRS resource, including at least the minimum number of repetitions specified in the accuracy requirements, is fully covered by MGL excluding RF switching time, then the PRS resource is considered being fully covered by MGL.
	+ Option 2 (OPPO, QC)
		- A PRS resource is overlapped with MG if the minimum number of repetitions specified in the accuracy requirements are covered by the MGL excluding RF switching time.
	+ Option 3a (HW)
		- A PRS resource is considered to be fully (partially) overlapped with MG if all (some) of its instances are overlapped with an MG occasion.
		- A PRS resource instance is considered to be overlapped with an MG occasion if the minimum number of repetitions of the instance is fully covered by the MGL excluding RF switching time, where the minimum number is given in the accuracy requirements.
	+ Option 3b (Nokia)
		- Add a definition of the term ‘PRS resource instance’ in TS 38.133.
* Recommended WF
	+ It seems all 3 options are technically aligned.
	+ Based on HW R4-2114278, what is additionally considered in option 3 is the case where PRS periodicity is smaller than MGRP, and not all PRS resource occasions/instances are covered by MGL excluding RF switching time
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 2-2-2: Consideration of RSTD search window

* Proposals
	+ Option 1 (vivo)
		- If the search window defined by *nr-DL-PRS-ExpectedRSTD* and *nr-DL-PRS-ExpectedRSTD-Uncertainty* together is not covered by MGL, the UE is supposed to do PRS measurement within the entire MGL.
	+ Option 2 (HW)
		- Take into account expected RSTD and expected RSTD uncertainty in defining overlap between PRS resource and MG.
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 2-2-3: Requirements applicability for PRS resource not overlapping with MG

* Proposals
	+ Option 1a (OPPO)
		- The measurement delay and accuracy requirements do not apply for a PRS resource not overlapped with MG.
		- For the calculation of CSSF, a PFL should be excluded if none of PRS resources in this PFL are overlapped with MG.
	+ Option 1b (QC)
		- Measurement requirements apply only for PRS resources that are “fully covered by the MG”
* Recommended WF
	+ It is noted that that the following statement has been added in 9.9.1 of 38.133

|  |
| --- |
| * UE is only required to measure PRS resources that are fully or partially overlapped with measurement gaps, and the requirements in clause 9.9.2, 9.9.3 and 9.9.4 are applicable to PRS resources that are fully or partially overlapped with measurement gaps.
 |

* + Based on moderator’s understanding, this should have already covered option 1b.
	+ Further discuss if clarifications as proposed in option 1a are needed or not.

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

### Sub-topic 2-3 Other

#### Issue 2-3-1: Whether to support of per-FR gap for PRS measurement in Rel-16

* Proposals
	+ Option 1 (QC)
		- Clarify in TS 38.133 that Rel-16 PRS-based measurements are supported with per-UE measurement gaps only.
			* Tables 9.1.2-2 and 9.1.2-3 would be modified to exclude the applicability of per-FR measurement gaps for positioning measurements.
			* Applicability conditions for positioning measurements in sec 9.9.1 would explicitly mention per-UE measurement gaps.
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 2-3-2: Clarification on the start of measurement period

* Proposals
	+ Option 1 (QC)
		- The starting point for the PRS-RSTD measurement period should be as follows:
			* The time $T\_{RSTD, Total}$ starts from the first MG instance aligned with a DL PRS resource(s) in the assistance data after both the *NR-TDOA-ProvideAssistanceData* message and *NR-TDOA-RequestLocationInformation* message are delivered from LMF to the physical layer of UE via LPP [34].”
		- The starting point for the PRS-RSRP measurement period should be as follows
			* When PRS-RSRP measurements are configured for DL-AoD, the time $T\_{PRS-RSRP,total} $starts from the first MG instance aligned with DL PRS resources in the assistance data after both the *NR-DL-AoD-RequestLocationInformation* message and *NR-DL-AoD-ProvideAssistanceData* message from LMF via LPP [34] are delivered to the physical layer of UE.”
		- The starting point for the UE Rx-Tx measurement period should be as follows:
			* The time $T\_{UERxTx,Total} $starts from the first MG instance aligned with DL PRS resources in the assistance data after both the *NR-Multi-RTT-RequestLocationInformation message* and *NR-Multi-RTT-ProvideAssistanceData message from LMF* via LPP [34] are delivered to the physical layer of UE.”
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

## Companies views’ collection for 1st round

### Open issues

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2111987 (CATT) | Moderator: this CR is not for open issues listed in section 2.2, so please provide your comments to the CR directly here, if any.  |
|  |
|  |
| R4-2112569 (vivo) |  |
| R4-2114066 (Nokia) |  |
| R4-2114279 (HW) |  |
| R4-2114205 (QC) |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | *Tentative agreements:**Candidate options:**Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #3: PRS-RSRP measurement period

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc** | **Company** | **Proposals / Observations** |
| [**R4-2112541**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112541.zip) | vivo | **Proposal 1: When PRS-RSRP is configured for DL-TDOA, no application rule of measurement requirements is needed as existing requirements in clause 9.9.2 already specified/clarified measurement requirements for PRS-RSRP.****Proposal 2: When PRS-RSRP is configured for multi-RTT, no application rule of measurement requirements is needed as existing requirements in clause 9.9.4 already specified/clarified measurement requirements for PRS-RSRP.** |
| [**R4-2112565**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112565.zip) | vivo | CR |
| [**R4-2114234**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114234.zip) | Nokia, Nokia Shanghai Bell | 1. RSRP values are basic and easy-to-use to set up positioning measurements such as beam correspondence and to evaluate measurement reliability.
2. RAN1/2 define separate UE capability on PRS-RSRP measurement combined for other positioning methods.

**Proposal 1 : When PRS-RSRP measurement is required when configured for DL-TDOA or multi-RTT, the measurement period is supposed to be same as DL-TDOA or multi-RTT measurement period respectively. Accordingly, the DL-TDOA or multi-RTT measurement period requirements respectively are applied to PRS-RSRP in this case. ( option-1 )** |
| [**R4-2114272**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114272.zip) | Huawei, HiSilicon | **Proposal 1: Remove requirements related to PRS-RSRP for DL-TDOA or multi-RTT in clause 9.9.3.** |
| [**R4-2114273**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114273.zip) | Huawei, HiSilicon | CR |
| [**R4-2114452**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114452.zip) | Ericsson | * **Observation 1**: The following was agreed: When PRS-RSRP is configured for DL-TDOA, RSTD and RSRP are performed over the same measurement period.
* **Observation 2**: PRS-RSRP and RSTD are technically different measurements even if performed over the same measurement period and performed by using the same assistance data.
* **Proposal 1**: When PRS-RSRP is configured for DL-TDOA then PRS-RSRP meets requirements defined for PRS-RSRP in clause 9.9.3, TS 38.133.
 |
| [**R4-2114453**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114453.zip) | Ericsson | CR |

## Open issues summary

### Sub-topic 3-1 Applicable rrequirements for PRS-RSRP configured for DL-TDOA (multi-RTT)

#### Issue 3-1-1: Applicable requirements for PRS-RSRP configured for DL-TDOA (multi-RTT)

* Proposals
	+ Option 1 (vivo, Nokia, HW)
		- Requirements specified for RSTD (UE Rx-Tx) in clause 9.9.2 (9.9.4) apply
	+ Option 2 (Ericsson)
		- Requirements specified for PRS-RSRP in clause 9.9.3 apply
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

## Companies views’ collection for 1st round

### Open issues

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2112565 (vivo) |  |
|  |
|  |
| R4-2114273 (HW) |  |
|  |
|  |
| R4-2114453 (Ericsson) |  |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | *Tentative agreements:**Candidate options:**Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #4: UE Rx-Tx time difference measurement period

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc** | **Company** | **Proposals / Observations** |
| [**R4-2111984**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2111984.zip) | CATT | **Proposal 1: It is preferred that 160ms is used for the value of X in PRS/SRS proximity condition.** **Proposal 2: If the PRS/SRS proximity condition is not met, UE can still measure and report the UE Rx-Tx time difference within the measurement period, but the accuracy requirements is not applied due to lack of SRS resources.** **Proposal 3: UE shall continue UE Rx-Tx time difference measurement and the measurement requirements are still applicable when TA changes due to TA command.** **Proposal 4: For the case of NTA\_offset change, UE can still perform measurement and the measurement requirements are not impacted.** **Proposal 5: When cell change impacting SRS occurs during the measurement period, UE shall restart the UE Rx-Tx time difference measurement after the SRS reconfiguration on the target cell is complete.** **Proposal 6: For the case of cell change not impacting SRS, no clarification is needed in core requirements in the specification.**  |
| [**R4-2112542**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112542.zip) | vivo | **Proposal 1:****Value of X in PRS/SRS proximity condition is 160ms.****Proposal 2: UE still measures and reports UE Rx-Tx measurement if PRS/SRS proximity condition is not met.****Proposal 3: A note may be needed that positioning accuracy may be degraded when PRS/SRS proximity condition is not met.****Proposal 4: The UE shall discard the ongoing UE Rx-Tx time difference measurement and starts a new measurement if the uplink transmission timing due to network-configured TA changes during the UE Rx-Tx measurement period.****Proposal 5:****UE Rx-Tx time difference measurement requirements are not applicable if TA command is received during the measurement period.****Proposal 6: The UE shall discard the UE Rx-Tx time difference measurement and starts a new measurement if NTA-offset changes during the UE Rx-Tx measurement period.****Proposal 7:****UE Rx-Tx time difference measurement requirements are not applicable if NTA-offset changes during the measurement period.****Proposal 8: For the cell change impacting SRS configuration, UE shall continue the on-going UE Rx-Tx time difference measurement, and the current measurement period and accuracy apply.****Proposal 9: For the cell change NOT impacting SRS configuration, the UE shall continue the on-going UE Rx-Tx time difference measurement and the current measurement period and accuracy apply.****Proposal 10: For TA change due to cell change, the UE behavior should follow the conclusion of impact due to TA change.** |
| [**R4-2112567**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112567.zip) | vivo |  |
| [**R4-2113260**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2113260.zip) | OPPO | **Proposal 1: Support X=160ms for PRS/SRS proximity.** **Proposal 2: UE is still expected to measure and report UE Rx-Tx measurement if PRS/SRS proximity condition is not met.****Proposal 3: UE Rx-Tx time difference accuracy do not apply if PRS/SRS proximity condition is not met.****Proposal 4: In case of cell change impacting SRS configuration, support option 1 that the UE shall restart the UE Rx-Tx time difference measurement after the SRS reconfiguration on the target cell is complete****Proposal 5: In case of cell change not impacting SRS configuration, support option 1b that the UE shall continue the on-going UE Rx-Tx time difference measurement, and longer measurement period is expected.****Proposal 6: In case of TA change due to TA command, UE shall discard the UE Rx-Tx time difference measurement, and the UE Rx-Tx time difference measurement requirements are not applicable.****Proposal 7: If NTA\_offset changes during the measurement period, UE should discard the UE Rx-Tx time different measurement and the requirements are not applicable.**  |
| [**R4-2113261**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2113261.zip) | OPPO |  |
| [**R4-2114194**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114194.zip) | Qualcomm Incorporated | **Proposal 1: Value of X in the PRS/SRS proximity condition: X=80 ms.****Proposal 2: When the PRS/SRS proximity condition is not met, UE Rx-Tx time difference measurement requirements do not apply and UE behavior is left to implementation.****Proposal 3: UE Rx-Tx time difference measurement requirements are not applicable if TA command is received during the measurement period. UE behavior is left up to implementation.****Proposal 4: UE Rx-Tx measurement requirements are not applicable if the NTA\_offset changes during the measurement period. UE behavior is left up to implementation.****Proposal 5: If a serving cell change impacting the configuration of SRS for positioning occurs during the UE Rx-Tx time difference measurement period, the measurement period is restarted after SRS reconfiguration on the target cell is complete.****Proposal 6: If a serving cell change that does not impact the configuration of SRS for positioning occurs during the UE Rx-Tx time difference measurement period, the UE Rx-Tx shall continue the measurement and the measurement period can be longer.** |
| [**R4-2114235**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114235.zip) | Nokia, Nokia Shanghai Bell | **Observation 1 :** In certain UL transmission conditions, SRS-P scheduling and transmission may not meet the proximity condition, since SRS-P transmission has the lowest transmission priority in Rel-16.**Observation 2 :** As one concern, a UE may not complete a measurement report, if SRS-P scheduling transmission may not meet the proximity condition. 1. Regarding PRS/SRS proximity, we support X=160ms (option-2).
2. Regarding UE behavior out of the proximity, UE RX-TX time measurement and report should work within the required measurement period. (option-1)
3. Regarding requirements out of the proximity, we can agree that the current accuracy requirement may not applied (Option-1a)
4. Regarding TA change due to TA command or autonomous timing adjustment, we support option 1. A UE shall continue UE Rx-Tx time difference measurement and meet accuracy requirements.
5. Regarding TA change due to NTA\_offset change, we support option 2 in requirement, that is measurement requirements are not applicable if the NTA\_offset changes during the measurement period.
 |
| [**R4-2114275**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114275.zip) | Huawei, HiSilicon | **Proposal 1: Adopt X=160ms for the SRS/PRS proximity condition.****Proposal 2: UE should still meet the measurement period requirements if PRS/SRS proximity condition is not met, but the measurement accuracy requirements do not apply.****Proposal 3: Measurement requirements for UE Rx-Tx do not apply if there is TA change during the measurement period.** **Proposal 4: Measurement requirements for UE Rx-Tx do not apply if there is NTA\_offset change during the measurement period.** **Proposal 4: If any of the the serving cell (PCell, PSCell, or SCell) configured with the SRS for positioning changes during the measurement period, UE restarts the Rx-Tx measurement.****Proposal 5: If any of the the serving cell (PCell, PSCell, or SCell) NOT configured with the SRS for positioning changes during the measurement period, UE continues the Rx-Tx measurement** **and the current measurement period and accuracy requirements should apply.**  |
| [**R4-2114276**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114276.zip) | Huawei, HiSilicon |  |
| [**R4-2114455**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114455.zip) | Ericsson | **PRS/SRS proximity condition:*** **Observation 1**: SRS may also be used for other purposes and in some scenarios SRS overheads may have to kept low. Shorter value of in PRS/SRS proximity condition will put more restriction on network.
* **Observation 2**: When PRS/SRS proximity condition is not met then UE not meeting measurement requirement may lead to worse positioning accuracy.
* **Proposal 1**: The Value of X in PRS/SRS proximity condition is 160 ms.
* **Proposal 2**: If SRS and PRS proximity condition in proposal 1 is not met then it is up to the UE whether to transmit the UE Rx-Tx measurement results.
* **Proposal 3**: If the SRS and PRS proximity condition in proposal 1 is not met then the UE is not expected to meet the UE Rx-Tx time difference measurement requirements.

**UE Rx-Tx measurement procedure under cell TA command change:*** **Observation 3** The network configured TA command may require the UE to adjust its uplink timing in very larger adjustment step.
* **Observation 4** The network configured TA command may require the UE to adjust its uplink timing in any direction wrt the DL timing.
* **Observation 5** The UE takes multiple samples for the UE Rx-Tx time difference measurement and some may be taken before while others after the TA change inducing large positioning error if used for positioning.
* **Observation 6** Rx-Tx time difference measurement accuracy in clause 10.1.25.2, TS 38.133 does not apply under network-controlled TA change. Therefore, the UE should discard the Rx-Tx time difference measurement to prevent reporting of inaccurate measurement results.
* **Proposal 4**: The UE shall discard the UE Rx-Tx time difference measurement if the uplink transmission timing changes due to network-configured TA during the UE Rx-Tx measurement period.
* **Proposal 5**: The UE Rx-Tx time difference measurement requirements are not applicable if the uplink transmission timing changes due to network-configured TA during the UE Rx-Tx measurement period.

**UE Rx-Tx measurement procedure under NTA\_offset change*** **Observation 6**: The change in the NTA\_offset can cause very large change in the uplink transmission timing of the UE resulting in highly inaccurate measurement result.
* **Observation 7:** The UE takes multiple samples for the UE Rx-Tx time difference measurement and some may be taken before while others after the NTA\_offset change inducing large positioning error if used for positioning.
* **Proposal 6**: The UE shall discard the UE Rx-Tx measurement if the NTA\_offset changes during the UE Rx-Tx measurement period.
* **Proposal 7**: UE Rx-Tx measurement requirements (section 9.9.4 in TS 38.133) are not applicable if the NTA\_offset changes during the UE Rx-Tx measurement period.

**UE Rx-Tx measurement procedure under cell change:*** **Observation 8:** The SRS used for the UE Rx-Tx time difference measurement may not always be configured on the serving cell which is changed.
* **Observation 9:** Even when the cell change does not impact SRS configuration and the UE continues the ongoing UE Rx-Tx time difference measurement, the cell change may introduce additional delay in the UE Rx-Tx time difference measurement period.
* **Proposal 8**: When the cell change impacts the SRS, then the UE shall restart the UE Rx-Tx time difference measurement after the SRS reconfiguration on the target cell is complete.
* **Proposal 9**: When the cell change does not impact the SRS, then UE shall continue the on-going UE Rx-Tx time difference measurement and the current measurement period and accuracy apply.
* **Proposal 10**: In scenario in proposal 9, longer UE Rx-Tx time difference measurement period is expected. In this case UE Rx-Tx time difference measurement period (TUERxTx,total,HO) shall be as follows:

TUERxTx,total,HO = TUERxTx,HO + K\*Teffect + THOWhere:- K is the number of times the handover occurs during TUERxTx,total,HO;- Teffect is the largest Teffect,i among all the positioning frequency layers;- THO $T\_{HO} $is the time during which the UE Rx-Tx time difference measurement may not be possible due to handover; it can be up to Tinterrupt as defined in clause 6.1 of TS 38.133. |
| [**R4-2114456**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114456.zip) | Ericsson |  |

## Open issues summary

*It is noted that Proposal 4 from Nokia R4-2114235 mentions accuracy requirements, but it has been agreed in R4-2008664 that accuracy requirements do not apply in case of TA change.*

### Sub-topic 4-1 SRS/PRS proximity

#### Issue 4-1-1: Value for X

* Proposals
	+ Option 1 (QC)
		- 80ms
	+ Option 2 (CATT, Nokia, OPPO, vivo, Ericsson, HW)
		- 160ms
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 4-1-2: UE behaviour and requirements when proximity condition is not met

* Proposals for UE behaviour
	+ Option 1 (CATT, OPPO, vivo, Nokia, HW)
		- The UE should still measure and report UE Rx-Tx measurement even if PRS/SRS proximity condition is not met
	+ Option 2 (QC, Ericsson)
		- Up to UE implementation
* Proposals for requirements
	+ Option 1 (CATT, OPPO, Nokia, HW)
		- UE Rx-Tx measurement period requirements apply, but the UE Rx-Tx accuracy requirements may not apply
	+ Option 2 (vivo)
		- Both UE Rx-Tx measurement period and measurement accuracy requirements apply
		- A note may be needed that positioning accuracy may be degraded when PRS/SRS proximity condition is not met.
	+ Option 3 (QC, Ericsson)
		- UE Rx-Tx time difference measurement requirements do not apply.
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

### Sub-topic 4-2 Measurement period requirements with UL timing change

#### Issue 4-2-1: TA change due to TA command

* Proposals for UE behaviour
	+ Option 1 (CATT, Nokia)
		- UE shall continue UE Rx-Tx time difference measurement
	+ Option 2 (OPPO, vivo, Ericsson)
		- UE shall discard the UE Rx-Tx time difference measurement
	+ Option 3 (QC, HW)
		- Up to UE implementation
* Proposals for requirements
	+ Option 1 (CATT, Nokia)
		- UE Rx-Tx measurement period requirements are not impacted
	+ Option 2 (OPPO, QC, vivo, HW, Ericsson)
		- UE Rx-Tx measurement period requirements are not applicable
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 4-2-2: TA change due to NTA\_offset change

* Proposals for UE behaviour
	+ Option 1 (CATT)
		- UE shall continue UE Rx-Tx time difference measurement
	+ Option 2 (OPPO, vivo, Ericsson)
		- UE shall discard the UE Rx-Tx time difference measurement
	+ Option 3 (QC, HW)
		- Up to UE implementation
* Proposals for requirements
	+ Option 1 (CATT)
		- UE Rx-Tx measurement period requirements are not impacted
	+ Option 2 (OPPO, QC, vivo, Nokia, HW, Ericsson)
		- UE Rx-Tx measurement period requirements are not applicable
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

### Sub-topic 4-3 Measurement period requirements with cell change

#### Issue 4-3-1: Measurement period requirements with cell change impacting SRS

* Proposals
	+ Option 1 (CATT, OPPO, QC, HW, Ericsson)
		- UE shall restart the UE Rx-Tx time difference measurement after the SRS reconfiguration on the target cell is complete.
	+ Option 2 (vivo)
		- UE shall continue the on-going UE Rx-Tx time difference measurement, and the current measurement period and accuracy apply.
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 4-3-2: Measurement period requirements with cell change not impacting SRS

* Proposals
	+ Option 1a (CATT)
		- No clarification is needed in core requirements in the specification
	+ Option 1b (vivo, HW)
		- UE shall continue the on-going UE Rx-Tx time difference measurement and the current measurement period and accuracy apply.
	+ Option 2a (OPPO, QC)
		- UE shall continue the on-going UE Rx-Tx time difference measurement, and longer measurement period is expected.
	+ Option 2b (Ericsson)
		- UE shall continue the on-going UE Rx-Tx time difference measurement, and longer measurement period is expected.
		- In this case UE Rx-Tx time difference measurement period (TUERxTx,total,HO) shall be as follows:

TUERxTx,total,HO = TUERxTx,HO + K\*Teffect + THO

K is the number of times the handover occurs during TUERxTx,total,HO;

Teffect is the largest Teffect,i among all the positioning frequency layers;

THO $T\_{HO} $is the time during which the UE Rx-Tx time difference measurement may not be possible due to handover; it can be up to Tinterrupt as defined in clause 6.1 of TS 38.133.

* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

#### Issue 4-3-3: Measurement period requirements with cell change impacting TA

* Proposals
	+ Option 1 (vivo)
		- For TA change due to cell change, the UE behavior should follow the conclusion of impact due to TA change.
* Recommended WF
	+ Further discuss

|  |  |
| --- | --- |
| **Company** | **Comments**  |
|  |  |
|  |  |

## Companies views’ collection for 1st round

### Open issues

### CRs/TPs comments collection

*Major close to finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2112567 (vivo) |  |
|  |
|  |
| R4-2113261 (OPPO) |  |
|  |
|  |
| R4-2114276 (HW) |  |
|  |
|  |
| R4-2114456 (Ericsson) |  |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | *Tentative agreements:**Candidate options:**Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Recommendations for Tdocs

## 1st round

**New tdocs**

|  |  |  |
| --- | --- | --- |
| **Title** | **Source** | **Comments** |
| WF on … | YYY |  |
| LS on … | ZZZ | To: RAN\_X; Cc: RAN\_Y |
|  |  |  |

**Existing tdocs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Tdoc number** | **Title** | **Source** | **Recommendation**  | **Comments** |
| R4-210xxxx | CR on … | XXX | Agreeable, Revised, Merged, Postponed, Not Pursued |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Notes:

1. Please include the summary of recommendations for all tdocs across all sub-topics incl. existing and new tdocs.
2. For the Recommendation column please include one of the following:
	1. CRs/TPs: Agreeable, Revised, Merged, Postponed, Not Pursued
	2. Other documents: Agreeable, Revised, Noted
3. For new LS documents, please include information on To/Cc WGs in the comments column
4. Do not include hyper-links in the documents

## 2nd round

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Tdoc number** | **Title** | **Source** | **Recommendation**  | **Comments** |
| R4-210xxxx | CR on … | XXX | Agreeable, Revised, Merged, Postponed, Not Pursued |  |
| R4-210xxxx | WF on … | YYY | Agreeable, Revised, Noted |  |
| R4-210xxxx | LS on … | ZZZ | Agreeable, Revised, Noted |  |
|  |  |  |  |  |

Notes:

1. Please include the summary of recommendations for all tdocs across all sub-topics.
2. For the Recommendation column please include one of the following:
	1. CRs/TPs: Agreeable, Revised, Merged, Postponed, Not Pursued
	2. Other documents: Agreeable, Revised, Noted
3. Do not include hyper-links in the documents

Annex

Contact information

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email address** |
|  |  |  |

Note:

1. Please add your contact information in above table once you make comments on this email thread.
2. If multiple delegates from the same company make comments on single email thread, please add you name as suffix after company name when make comments i.e. Company A (XX, XX)