**3GPP TSG-WG RAN4 Meeting #101-e R4-211xxxx**

**Electronic meeting, November 1-12, 2021**

**Agenda Item: 8.7.1**

WF on MPR Table Placement for dual TX

Huawei, HiSilicon

# Background

In RAN4#100-e, it was agreed to use Clause 6.2G for TxD related output power requirements. In RAN4#101-e, it was agreed during the GTW session to place the MPR tables for dual TX in Clause 6.2D.

References:

[1] R4-2119723 [101-e][123] NR TxD Summary after\_1st\_Round, Moderator (Qualcomm), RAN4#101-e

[2] R4-2117200 1CC 2Tx MPR for different PAs implementations and signaling for 1CC and 2CC cases, Skyworks Solutions Inc.

[3] R4-2118550 Draft CR TS 38.101-1: Move PC1.5 MPR to Clause 6.2G, Huawei, HiSilicon, Qualcomm

# Agreements

Restructure the specification to capture the requirements of MPR in the way to align the requirement between TxD and UL-MIMO:

Option 1: Place tables for dual TX in suffix D, 6.2D.2

* Point the MPR requirement for TxD to this table.

Option 2: Merge section D and G