3GPP TSG-RAN WG4 Meeting # 101-e R4-2120008

Electronic Meeting, 1st– 12th November, 2021

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** | **DraftCR** | **rev** | **1** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR for 38.101-1 to introduce RedCap UE FR1 requirements | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_redcap-Core | | | | |  | ***Date:*** | | | 2021-11-09 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Redcap UE is introduced in Rel-17 in NR | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | To introduce requirements for RedCap UE | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No RedCap UE requirements in specificaitons. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.3, 4.3, 5.2I, 5.3I, 6.1I, 7.1I, 7.3I | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## **<<Start of Change>>**

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

ΔFGlobal Granularity of the global frequency raster

ΔFRaster Band dependent channel raster granularity

ΔfOOB Δ Frequency of Out Of Band emission

ΔFTX-RX Maximum deviation to the Tx-Rx carrier center frequency separation for asymmetric uplink/downlink channel bandwidth operation

∆MPRc Allowed Maximum Power Reduction relaxation for serving cell *c*

ΔPPowerClass Adjustment to maximum output power for a given power class

RB The starting frequency offset between the allocated RB and the measured non-allocated RB

ΔRIB,c Allowed reference sensitivity relaxation due to support for inter-band CA operation, for serving cell *c*

ΔRIB,1R Reference sensitivity adjustment due to support for 1 antenna connector for RedCap

ΔRIB,4R Reference sensitivity adjustment due to support for 4 antenna ports

ΔRIB,HD Reference sensitivity adjustment due to support for HD-FDD for RedCap

ΔShift Channel raster offset

TC Allowed operating band edge transmission power relaxation

TC,*c*Allowed operating band edge transmission power relaxation for serving cell *c*

ΔTIB,c Allowed maximum configured output power relaxation due to support for inter-band CA operation, inter-band NR-DC operation and due to support for SUL operations, for serving cell *c*

BWChannel Channel bandwidth

BWChannel,block Sub-block bandwidth, expressed in MHz. BWChannel,block= Fedge,block,high- Fedge,block,low

BWChannel\_CA Aggregated channel bandwidth, expressed in MHz

BWChannel,max Maximum channel bandwidth supported among all bands in a release

BWGB max( BWGB,Channel(*k*) )

BWGB,Channel(k) Minimum guard band defined in clause 5.3A.1 of carrier *k*

BWDL Channel bandwidth for DL

BWUL Channel bandwidth for UL

BWinterferer Bandwidth of the interferer

Ceil(x) Rounding upwards; ceil(x) is the smallest integer such that ceil(x) ≥ x

Floor(x) Rounding downwards; floor(x) is the greatest integer such that floor(x) ≤ x

FC *RF reference frequency* on the channel raster, given in table 5.4.2.2-1

FC,block, high Fc of the highest transmitted/received carrier in a *sub-block*

FC,block, low Fc of the lowest transmitted/received carrier in a *sub-block*

FC,low The Fc of the lowest carrier, expressed in MHz

FC,high The Fc of the highest carrier, expressed in MHz

FDL\_low The lowest frequency of the downlink *operating band*

FDL\_high The highest frequency of the downlink *operating band*

FUL\_low The lowest frequency of the uplink *operating band*

FUL\_high The highest frequency of the uplink *operating band*

Fedge,block,low The lower *sub-block* edge, where Fedge,block,low = FC,block,low - Foffset, low.

Fedge,block,high The upper *sub-block* edge, where Fedge,block,high = FC,block,high + Foffset, high.

Fedge , low The *lower edge* of *aggregated channel bandwidth*, expressed in MHz. Fedge,low = FC,low - Foffset,low.

Fedge, high The *higher edge* of *aggregated channel bandwidth*, expressed in MHz. Fedge,high = FC,high + Foffset,high.

FInterferer (offset) Frequency offset of the interferer (between the center frequency of the interferer and the carrier frequency of the carrier measured)

FInterferer Frequency of the interferer

FIoffset Frequency offset of the interferer (between the center frequency of the interferer and the closest edge of the carrier measured)

Foffset Frequency offset from FC\_high to the *higher edge* or FC\_low to the *lower edge.*

Foffset,high Frequency offset from FC,high to the upper *UE RF Bandwidth edge*, or from FC,block, high to the upper sub-block edge

Foffset,low Frequency offset from FC,low to the lower *UE RF Bandwidth edge*, or from FC,block, low to the lower sub-block edge

FOOB The boundary between the NR out of band emission and spurious emission domains

FREF RF reference frequency

FREF-Offs Offset used for calculating FREF

FREF, shift RF reference frequency for Supplementary Uplink (SUL) bands, the uplink of all FDD bands, and TDD bands

Fuw (offset) The frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer

GBChannel Minimum guard band defined in clause 5.3.3

LCRB Transmission bandwidth which represents the length of a contiguous resource block allocation expressed in units of resources blocks

Max() The largest of given numbers

Min() The smallest of given numbers

 Physical resource block number

NRACLR NR ACLR

NRB Transmission bandwidth configuration, expressed in units of resource blocks

NRB\_agg The number of the aggregated RBs within the fully allocated aggregated channel bandwidth

for carrier 1 to j, where *μ* is defined in TS 38.211 [6]

NRB,c The transmission bandwidth configuration of component carrier c, expressed in units of resource blocks

for carrier j, where *μ* is defined in TS 38.211 [6]

NRB,largest BW The largest transmission bandwidth configuration of the component carriers in the bandwidth combination, expressed in units of resource blocks

NRB,low The transmission bandwidth configurations according to Table 5.3.2-1 for the lowest assigned component carrier in clause 5.3A.1

NRB,high The transmission bandwidth configurations according to Table 5.3.2-1 for the highest assigned component carrier in clause 5.3A.1

NREF NR Absolute Radio Frequency Channel Number (NR-ARFCN)

NREF-Offs Offset used for calculating NREF

PCMAX The configured maximum UE output power

PCMAX, *c* The configured maximum UE output power for serving cell *c*

PCMAX, *f*, *c* The configured maximum UE output power for carrier *f* of serving cell *c* in each slot

PEMAX Maximum allowed UE output power signalled by higher layers

PEMAX, *c* Maximum allowed UE output power signalled by higher layers for serving cell *c*

PInterferer Modulated mean power of the interferer

Plargest BW Power of the largest transmission bandwidth configuration of the component carriers in the bandwidth combination

PPowerClass The nominal UE power (i.e., no tolerance)

P-MPR*c* Power Management Maximum Power Reduction for serving cell *c*

PRB The transmitted power per allocated RB, measured in dBm

PUMAX The measured configured maximum UE output power

Puw Power of an unwanted DL signal

Pw Power of a wanted DL signal

RBstart The lowest RB index of transmitted resource blocks

RBstart\_CA The lowest RB index of transmitted resource blocks for intra-band contiguous CA

SCSc SCS for the component carrier c

SCSlargest BW SCS for the largest transmission bandwidth configuration of the component carriers in the bandwidth combination

SCSlow SCS for the lowest assigned component carrier in clause 5.3A.1

SCShigh SCS for the highest assigned component carrier in clause 5.3A.1

*tp* Transient Period value signalled by the UE

*tpstart* Start position of transient period relative to the symbol boundary

T(PCMAX, *f*, *c*) Tolerance for applicable values of PCMAX, *f*, *c* for configured maximum UE output power for carrier *f* of serving cell *c*

TL,c Absolute value of the lower tolerance for the applicable *operating band* as specified in clause 6.2.1

SSREF SS block reference frequency position

UTRAACLR UTRA ACLR

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

ACLR Adjacent Channel Leakage Ratio

ACS Adjacent Channel Selectivity

A-MPR Additional Maximum Power Reduction

BS Base Station

BW Bandwidth

BWP Bandwidth Part

CA Carrier Aggregation

CA\_nX-nY Inter-band CA of component carrier(s) in one sub-block within Band nX and component carrier(s) in one sub-block within Band nY where nX and nY are the applicable NR *operating bands*

CC Component Carriers

CG Carrier Group

CP-OFDM Cyclic Prefix-OFDM

CW Continuous Wave

DC Dual Connectivity

DFT-s-OFDM Discrete Fourier Transform-spread-OFDM

DM-RS Demodulation Reference Signal

DTX Discontinuous Transmission

E-UTRA Evolved UTRA

EIRP Equivalent Isotropically Radiated Power

EVM Error Vector Magnitude

FR Frequency Range

FRC Fixed Reference Channel

FWA Fixed Wireless Access

GSCN Global Synchronization Channel Number

IBB In-band Blocking

IDFT Inverse Discrete Fourier Transformation

ITS Intelligent Transportation System

ITU‑R Radiocommunication Sector of the International Telecommunication Union

MBW Measurement bandwidth defined for the protected band

MCG Master Cell Group

MOP Maximum Output Power

MPR Allowed maximum power reduction

MSD Maximum Sensitivity Degradation

NR New Radio

NR-ARFCN NR Absolute Radio Frequency Channel Number

NS Network Signalling

OCNG OFDMA Channel Noise Generator

OOB Out-of-band

P-MPR Power Management Maximum Power Reduction

PRB Physical Resource Block

PSCCH Physical Sidelink Control CHannel

PSSCH Physical Sidelink Shared CHannel

QAM Quadrature Amplitude Modulation

RE Resource Element

REFSENS Reference Sensitivity

RedCap Reduced Capability

RF Radio Frequency

RMS Root Mean Square (value)

RSRP Reference Signal Receiving PowerRx Receiver

Rx Receiver

SC Single Carrier

SCG Secondary Cell Group

SCS Subcarrier spacing

SDL Supplementary Downlink

SEM Spectrum Emission Mask

SL Sidelink

SL-MIMO Sidelink-Multiple Antenna transmission

SNR Signal-to-Noise Ratio

SRS Sounding Reference Symbol

SS Synchronization Symbol

SUL Supplementary uplink

TAE Time Alignment Error

TAG Timing Advance Group

Tx Transmitter

TxD Tx Diversity

UL MIMO Uplink Multiple Antenna transmission

ULFPTx Uplink Full Power Transmission

V2X Vehicle to Everything

## **<<Next of Change>>**

## 4.3 Specification suffix information

Unless stated otherwise the following suffixes are used for indicating at 2nd level clause, shown in Table 4.3-1.

Table 4.3-1: Definition of suffixes

|  |  |
| --- | --- |
| Clause suffix | Variant |
| None | Single Carrier |
| A | Carrier Aggregation (CA) |
| B | Dual-Connectivity (DC) |
| C | Supplement Uplink (SUL) |
| D | UL MIMO |
| E | V2X |
| F | Shared spectrum channel access |
| G | Tx Diversity (TxD) |
| H | Carrier Aggregation(CA) for UL MIMO |
| I | RedCap |

A terminal which supports the above features needs to meet both the general requirements and the additional requirement applicable to the additional clause (suffixes A to F) in clauses 5, 6 and 7. Where there is a difference in requirement between the general requirements and the additional clause requirements (suffixes A to F) in clauses 5, 6 and 7, the tighter requirements are applicable unless stated otherwise in the additional clause.

A terminal which supports more than one feature in clauses 5, 6 and 7 shall meet all of the separate corresponding requirements.

For a terminal that supports SUL for the band combination specified in Table 5.2C-1, the current version of the specification assumes the terminal is configured with active transmission either on UL carrier or SUL carrier at any time in one serving cell and the UE requirements for single carrier shall apply for the active UL or SUL carrier accordingly. For a terminal that supports SUL, the current version of the specification assumes the terminal is not configured with UL MIMO on SUL carrier.

For a terminal that supports operation in shared spectrum, the current version of this specification assumes in the uplink sub-bands within a wideband channel shall be contiguously allocated to the UE. The uplink requirements for one or more non-transmitted sub-bands between two transmitted sub-bands does not form a part of the current version of this specification.

For a terminal that is declared as RedCap UE, carrier aggregation, dual connectivity and wider bandwidths are not applicable.

## **<<Next of Change>>**

## 5.2I Operating band for RedCap

The operating bands defined in Table 5.2-1 are applicable for RedCap UE.

## **<<Next of Change>>**

## 5.3I Channel bandwidth for RedCap

The UE channel bandwidth specified in clause 5.3 is applicable for RedCap UE, but the maximum channel bandwidth for RedCap UE in the operating band is 20MHz.

## **<<Next of Change>>**

## 6.1I General for RedCap

Unless otherwise stated, the transmitter characteristics are applicable for RedCap UE. However, only power class 2 and power class 3 are supported by RedCap UE.

## **<<Next of Change>>**

## 7.1I General for RedCap

Unless otherwise stated, the receiver characteristics are applicable for RedCap UE. The RedCap UE is required to be equipped with one or two Rx antenna connectors in the operating band.

## **<<Next of Change>>**

## 7.3I Reference sensitivity for RedCap

For RedCap UE equipped with two Rx antenna connectors, reference sensitivity specified in clause 7.3.2 for each band are applied.

For RedCap UE equipped with one Rx antenna connector, reference sensitivity for 2Rx antenna ports in Table 7.3.2-1 shall be modified by the amount given in ΔRIB,1R = 2.5 dB for all the operating bands. The excetptions with ΔRIB,1R = 3dB are allowed for all the FDD bands under 10MHz/15MHz/20MHz channel bandwidths.

For RedCap UE supporting HD-FDD in the FDD operating bands, reference sensitivity for full duplex in the FDD operating bands shall be additionally modified by the amount given in ΔRIB,HD = -0.8dB for the FDD operating bands. The exceptions for ΔRIB,HD are allowed in accordance with table 7.3I-1 for some FDD operating bands.

Table 7.3I-1: ΔRIB,HD exceptions

|  |  |
| --- | --- |
| Operating band | ΔRIB,HD value |
| TBD | TBD |

## **<<End of Change>>**