**3GPP TSG-RAN WG4 Meeting #101-e R4-2118488**

**Electronic Meeting, 1 November – 11 November 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **-1** | **CR** | **0959** | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to add NR intra-band FR1 in TS 38.101-1 |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_CA\_R17\_Intra |  | ***Date:*** | 2021-11-16 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Adding approved NR Intra-band FR1 combinations |
|  |  |
| ***Summary of change:*** | Adding the following intra-band contiguous combinaitons:CA\_n2BCA\_n5BCA\_n25BCA\_n77BCA\_n96BCA\_n96CCA\_n96DCA\_n96EAdding the following intra-band non-contiguous combinations:CA\_n1(2A)CA\_n12(2A)CA\_n25(2A)CA\_n25(3A)CA\_n41(2A)CA\_n41(3A)CA\_n41(4A)CA\_n96(2A)CA\_n96(3A)CA\_n96(4A) |
|  |  |
| ***Consequences if not approved:*** | Approved NR Intra-band FR1 combinations are not added |
|  |  |
| ***Clauses affected:*** | 5.2, 7.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-3 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

---Start of changes---

Table 5.2A.1-1: Intra-band contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band(Table 5.2-1) |
| CA\_n1 | n1 |
| CA\_n2 | n2 |
| CA\_n5 | n5 |
| CA\_n7 | n7 |
| CA\_n25 | n25 |
| CA\_n40 | n40 |
| CA\_n41 | n41 |
| CA\_n46 | n46 |
| CA\_n48 | n48 |
| CA\_n66 | n66 |
| CA\_n71 | n71 |
| CA\_n77 | n77 |
| CA\_n78 | n78 |
| CA\_n79 | n79 |
| CA\_n96 | n96 |
| NOTE 1: The minimum requirements only apply for non simultaneous Tx/Rx between all carriers for TDD combinations. |

Table 5.2A.1-2: Intra-band non-contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band(Table 5.2-1) |
| CA\_n1(\*) | n1 |
| CA\_n3(\*) | n3 |
| CA\_n7(\*) | n7 |
| CA\_n12(\*) | n12 |
| CA\_n25(\*) | n25 |
| CA\_n41(\*) | n41 |
| CA\_n48(\*) | n48 |
| CA\_n66(\*) | n66 |
| CA\_n71(\*) | n71 |
| CA\_n77(\*) | n77 |
| CA\_n78(\*) | n78 |
| CA\_n96(\*) | n96 |
| NOTE 1: The minimum requirements only apply for non simultaneous Tx/Rx between all carriers for TDD combinations.NOTE 2: The notation CA\_nX(\*) in this table indicates intra-band non-contiguous CA for band nX. The configurations for each band are in 5.5A.2.  |

### ---Text omitted---

Table 5.5A.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |
| --- |
| NR CA configuration / Bandwidth combination set |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated bandwidth (MHz) | Bandwidth combination set |
| CA\_n1B | - | 10 | 10,15 |  |  |  | 40 | 0 |
|  |  | 15 | 15,20 |  |  |  |  |  |
|  |  | 20 | 20 |  |  |  |  |  |
| CA\_n2B | - | 5 | 15 |  |  |  | 20 | 0 |
|  |  | 10 | 10 |  |  |  |  |  |
| CA\_n5B | CA\_n5B | 5, 10, 15 | 5, 10, 15 |  |  |  | 20 | 0 |
| CA\_n7B | CA\_n7B | 10 | 10, 15, 20, 30, 40 |  |  |  | 50 | 0 |
|  |  | 15 | 15, 20, 30 |  |  |  |  |  |
|  |  | 20 | 20, 30 |  |  |  |  |  |
| CA\_n25B | - | 5 | 15 |  |  |  | 20 | 0 |
|  |  | 10 | 10 |  |  |  |  |  |
| CA\_n40B | - | 20 | 80 |  |  |  | 100 | 0 |
|  |  | 50 | 50 |  |  |  |  |  |
| CA\_n41B | CA\_n41B | 10, 20, 30, 40, 50 | 10, 20, 30, 40, 50 |  |  |  | 100 | 0 |
| CA\_n41C | CA\_n41C | 40 | 80, 100 |  |  |  | 180 | 0 |
| 50, 60, 80 | 60, 80, 100 |  |  |  |  |  |
| 10 | 100 |  |  |  | 190 | 1 |
| 15, 20 | 90, 100 |  |  |  |  |  |
| 40 | 80, 90, 100 |  |  |  |  |  |
| 50, 60, 80, 90 | 60, 80, 90, 100 |  |  |  |  |  |
| 10 | 100 |  |  |  | 190 | 2 |
| 15, 20 | 90, 100 |  |  |  |  |  |
| 30, 40 | 80, 90, 100 |  |  |  |  |  |
| 50, 60, 80, 90 | 60, 80, 90, 100 |  |  |  |  |  |
|  |  | See n41 channel bandwidths in Table 5.3.5-1 for each carrier2 |  |  |  | 190 | 4 and 5 |
| CA\_n46B | - | 20, 40, 60 | 20, 40 |  |  |  | 100 | 0 |
| CA\_n46C | - | 60, 80 | 60, 80 |  |  |  | 160 | 0 |
| CA\_n46D | - | 60, 80 | 80 | 80 |  |  | 240 | 0 |
| CA\_n46M | - | 20, 40, 60 | 20, 40 | 20, 40 |  |  | 140 | 0 |
| CA\_n46N | - | 20, 40, 80 | 20, 40 | 20, 40 | 20, 40 |  | 200 | 0 |
| CA\_n46O | - | 20, 60 | 20, 40 | 20, 40 | 20, 40 | 20, 40 | 220 | 0 |
| CA\_n48B | CA\_n48B | 5 | 15, 20 |  |  |  | 40 | 0 |
|  |  | 10, 15, 20 | 10, 15, 20 |  |  |  |  |  |
|  |  | 15, 20 | 15, 20 |  |  |  |  |  |
|  | - | 10 | 50, 60, 80, 90 |  |  |  | 100 | 1 |
|  |  | 15, 20 | 40, 50, 60, 80 |  |  |  |  |  |
|  |  | 40 | 40, 50, 60 |  |  |  |  |  |
|  | - | 10, 15, 20, 30, 40 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90 |  |  |  | 100 | 2 |
| CA\_n48C | - | 10 | 100 |  |  |  | 140 | 0 |
|  |  | 15 | 90,100 |  |  |  |  |  |
|  |  | 20 | 90, 100 |  |  |  |  |  |
|  |  | 40 | 80, 90, 100 |  |  |  |  |  |
|  | - | 10, 15, 20, 30, 40 | 70, 80, 90, 100 |  |  |  | 140 | 1 |
| CA\_n66B | - | 5 1 | 20, 40 |  |  |  | 50 | 0 |
|  |  | 10 | 15, 20, 40 |  |  |  |  |  |
|  |  | 15 | 15, 20 |  |  |  |  |  |
| CA\_n71B | - | 5 | 20 |  |  |  | 25 | 0 |
|  |  | 10 | 15 |  |  |  |  |  |
|  |  | 10 | 20 |  |  |  | 35 | 1 |
|  |  | 15 | 15, 20 |  |  |  |  |  |
|  |  | 5, 10, 15 | 15, 20 |  |  |  | 35 | 2 |
| CA\_n77B | - | 20 | 25, 30, 40 |  |  |  | 60 | 0 |
|  |  | 25 | 30 |  |  |  |  |  |
| CA\_n77C | CA\_n77C | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
|  |  | 60 | 60, 80, 100 |  |  |  |  |  |
|  |  | 80 | 80, 100 |  |  |  |  |  |
|  |  | 100 | 100 |  |  |  |  |  |
|  |  | 10 | 100 |  |  |  | 200 | 1 |
|  |  | 15, 20 | 90, 100 |  |  |  |  |  |
|  |  | 25, 30 | 80, 90, 100 |  |  |  |  |  |
|  |  | 40 | 70, 80, 90, 100 |  |  |  |  |  |
|  |  | 50, 60, 70, 80, 90, 100 | 60, 70, 80, 90, 100 |  |  |  |  |  |
| CA\_n77D | - | 100 | 100 | 100 |  |  | 300 | 0 |
| CA\_n78B | - | 20 | 50 |  |  |  | 70 | 0 |
| CA\_n78C | CA\_n78C | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
|  |  | 60 | 60, 80, 100 |  |  |  |  |  |
|  |  | 80 | 80, 100 |  |  |  |  |  |
|  |  | 100 | 100 |  |  |  |  |  |
|  |  | 10 | 100 |  |  |  | 200 | 1 |
|  |  | 15, 20 | 90, 100 |  |  |  |  |  |
|  |  | 25, 30 | 80, 90, 100 |  |  |  |  |  |
|  |  | 40 | 70, 80, 90, 100 |  |  |  |  |  |
|  |  | 50, 60, 70, 80, 90, 100 | 60, 70, 80, 90, 100 |  |  |  |  |  |
| CA\_n78D | - | 100 | 100 | 100 |  |  | 300 | 0 |
| CA\_n79C | CA\_n79C | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
|  |  | 60 | 60, 80, 100 |  |  |  |  |  |
|  |  | 80 | 80, 100 |  |  |  |  |  |
|  |  | 100 | 100 |  |  |  |  |  |
| CA\_n79D | - | 100 | 100 | 100 |  |  | 300 | 0 |
| CA\_n96B | CA\_n96B | 20, 40 | 20, 40, 60, 80 |  |  |  | 100 | 0 |
| CA\_n96C | CA\_n96C | 80 | 40, 60, 80 |  |  |  | 160 | 0 |
| CA\_n96D |  | 80 | 80 | 60, 80 |  |  | 240 | 0 |
| CA\_n96E |  | 80 | 80 | 80 | 80 |  | 320 | 0 |
| NOTE 1: 5 MHz is not applicable for 30/60 kHz SCS.NOTE 2: The aggregated bandwidth must be greater than or equal to the minimum for the bandwidth class defined in Table 5.3A.5-1, and smaller than or equal to the maximum aggregated bandwidth |

Table 5.5A.1-2: Void

### 5.5A.2 Configurations for intra-band non-contiguous CA

Table 5.5A.2-1: NR CA configurations and bandwidth combination sets defined for intra-band non-contiguous CA

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | MaximumAggregated bandwidth(MHz) | Bandwidth combination set |
| CA\_n1(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n2(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n3(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n5(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 25 | 0 |
| CA\_n7(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n12(2A) | - | 5 | 5 |  |  | 10 | 0 |
| CA\_n25(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
|  |  | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  |  | 60 | 1 |
| CA\_n25(3A) | - | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  | 55 | 0 |
| CA\_n41(2A) | CA\_n41(2A) | 40, 50, 60, 80, 100 | 40, 50, 60, 80, 100 |  |  | 180 | 0 |
|  | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 190 | 1 |
| - | 10, 15, 20, 30, 40, 50, 60, 80, 90 | 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |  | 190 | 2 |
|  |  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 190 | 3 |
|  |  | See n41 channel bandwidths in Table 5.3.5-1 for each carrier |  |  | 190 | 4 and 5 |
| CA\_n41(3A) | - | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  | 190 | 0 |
| CA\_n48(2A) |  | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 1402 | 0 |
|  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 1402 | 1 |
| CA\_n48(3A) | - | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 |  | 1402 | 0 |
|  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  | 1402 | 1 |
| CA\_n48(4A) | - | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 1352 | 0 |
|  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1352 | 1 |
| CA\_n66(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20, 40 |  |  | 60 | 0 |
| 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  |  | 80 | 1 |
| 5, 10, 15, 20, 40 | 5, 10, 15, 20, 40 |  |  | 80 | 2 |
| CA\_n66(3A) | - | 5, 10, 15, 20, 40 | 5, 10, 15, 20, 40 | 5, 10, 15, 20, 40 |  | 80 | 0 |
| CA\_n71(2A) | - | 5,10, 15, 20 | 5,10,15, 20 |  |  | 30 | 0 |
| CA\_n77(2A) | CA\_n77(2A) | 20, 40, 80, 100 | 20, 40, 80, 100 |  |  | 200 | 0 |
|  |  | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 200 | 1 |
| CA\_n77(3A) | - | 20, 40, 80, 100 | 20, 40, 80, 100 | 20, 40, 80, 100 |  | 300 | 0 |
| 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  | 300 | 1 |
| CA\_n78(2A) | CA\_n78(2A) | 10, 20, 40, 50, 60, 80, 90, 100 | 10, 20, 40, 50, 60, 80, 90, 100 |  |  | 200 | 0 |
|  |  | 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |  | 200 | 1 |
|  |  | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 200 | 2 |
| CA\_n96(2A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 |  |  | 160 | 0 |
| CA\_n96(3A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 |  | 240 | 0 |
| CA\_n96(4A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 | 320 | 0 |
| NOTE 1: Void.NOTE 2: Parameter value accounts for both, the maximum frequency range of band n48 (150 MHz), and the minimum frequency gaps in between NR non-contiguous component carriers. |

Table 5.5A.2-2: NR CA configurations and bandwidth combination sets defined for mixed intra-band contiguous and non-contiguous CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration | NR Band | Channel bandwidth (MHz) | Bandwidth combination set |
|  |  |  | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n41(A-C) | - | n41 |  | 10 | 15 | 20 |  | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 0 |
|  | n41 | See CA\_n41C Bandwidth Combination Set 2 in Table 5.5A.1-1 |  |
| CA\_n48(A-B) | CA\_n48B | n48 | 5 | 10 | 15 | 20 |  |  | 40 | 501 | 601 |  | 801 | 901 | 1001 | 0 |
|  | n48 | See CA\_n48B Bandwidth Combination Set 0 in Table 5.5A.1-1 |  |
| CA\_n48B | n48 | 5 | 10 | 15 | 20 |  | 30 | 40 | 501 | 601 | 701 | 801 | 901 | 1001 | 1 |
|  | n48 | See CA\_n48B Bandwidth Combination Set 2 in Table 5.5A.1-1 |  |
| CA\_n48(A-C) | - | n48 | 5 | 10 | 15 | 20 |  |  | 40 | 501 | 601 |  | 801 | 901 | 1001 | 0 |
|  | n48 | See CA\_n48C Bandwidth Combination Set 0 in Table 5.5A.1-1 |  |
| - | n48 | 5 | 10 | 15 | 20 |  | 30 | 40 | 501 | 601 | 701 | 801 | 901 | 1001 | 1 |
|  | n48 | See CA\_n48C Bandwidth Combination Set 1 in Table 5.5A.1-1 |  |
| NOTE 1: This UE channel bandwidth is applicable only to downlink |

### ---Text omitted---

Table 7.3A.2.1-1: Intra-band contiguous CA uplink configuration for reference sensitivity

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| CA configuration | SCS(PCC/SCC)(kHz) | Aggregated channel bandwidth (PCC+SCC) | UL PCC allocation(LCRB) | UL SCC allocation(LCRB) | PCC ΔRIBNC (dB) | SCC ΔRIBNC (dB) | Duplex mode |
| CA\_n5B | 15/15 | 15MHz + 5MHz | 15 (RBstart = 64) | 5 (RBstart = 0) | 29.7 | 23.6 | FDD |
| 10MHz + 10MHz | 10 (RBstart = 42) | 10 (RBstart = 0) | 26.1 | 30.8 |
| CA\_n7B | 15/15 | 40MHz + 10MHz | 25 (RBstart = 191)  | 20 (RBstart = 32)  | 25 | 34 | FDD |
| 40MHz + 10MHz | 64 (RBstart = 152)  | 0 | 5.5 | 8.5 |
| 30MHz + 20MHz | 64 (RBstart = 96)  | 0 | 4 | 8.5 |
| 30MHz + 15MHz | 64 (RBstart = 96)  | 0 | 0 | 8 |
| NOTE 1: All combinations of channel bandwidths defined in Table 5.5A.1-1.NOTE 2: The carrier centre frequency of PCC in the UL operating band is configured closer to the DL operating band.NOTE 3: The transmitted power over both PCC and SCC shall be set to PUMAX as defined in subclause 6.2A.4.NOTE 4: The PCC allocation is same as Transmission bandwidth configuration NRB as defined in Table 5.3.2-1.  |

### ---Text omitted---

Table 7.3A.2.2-1: Intra-band non-contiguous CA with one uplink configuration for reference sensitivity in FDD bands.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CA configuration | SCS(PCC/SCC)(kHz) | Aggregated channel bandwidth (PCC+SCC) | Wgap / [MHz] | UL PCC allocation(LCRB) | ΔRIBNC (dB) | Duplex mode |
| CA\_n1(2A) | 15/15 | 5MHz + 5MHz | 0.0 < Wgap ≤ 50.0 | 25 | 0.5 | FDD |
| CA\_n2(2A) | 15/15 | 5MHz + 5MHz | Wgap = 55.0 | 105 | 5.0 | FDD |
|  |  |  | Wgap = 30.0 | 25 | 0.0 |  |
| CA\_n3(2A) | 15/15 | 5MHz + 5MHz | Wgap = 65.0 | 125 | 4.7 | FDD |
|  |  |  | Wgap = 45.0 | 255 | 0.0 |  |
| CA\_n5(2A) | 15/15 | 15MHz + 5MHz | Wgap = 5.0 | 55 | 6.3 | FDD |
| CA\_n7(2A) | 15/15 | 10MHz + 5MHz | Wgap = 55 | 325 | 0.0 | FDD |
|  |  |  | Wgap = 30 | 505 | 0.0 |  |
| CA\_n12(2A) | 15/15 | 5MHz + 5MHz | 0.0 < Wgap ≤ 7.0 | 5(RBstart=12) | 3 | FDD |
| CA\_n25(2A) 9 | 15/15 | 5MHz + 5MHz | Wgap = 55.0 | 105 | 5.0 | FDD |
|  |  |  | Wgap = 30.0 | 25 | 0.0 |  |
| CA\_n25(2A) 10CA\_n25(3A) | 15/15 | 40MHz + 5MHz | Wgap = 20.0 | 40 (RBstart = 176) | [24.6] 8 | FDD |
| CA\_n66(2A)CA\_n66(3A) | N/A | NOTE 1 | NOTE 2 | NOTE 3, NOTE 4 | 0.0 | FDD |
| CA\_n71(2A) | 15/15 | 5MHz + 5MHz | Wgap = 25.0 | 5 | 4.0 | FDD |
|  |  |  | Wgap = 5.0 | 20 | 0.0 |  |
|  |  | 10MHz + 5MHz | Wgap = 20.0 | 5 (RBstart = 9) | 4.6 |  |
|  |  |  | Wgap = 5.0 | 20 (RBstart = 9) | 2.3 |  |
|  |  | 15MHz + 10MHz | Wgap = 10.0 | 5 (RBstart = 2) | 22.2 |  |
|  |  |  | Wgap = 5.0 | 20 (RBstart = 19) | 5.2 |  |
| NOTE 1: All combinations of channel bandwidths defined in Table 5.5A.2-1.NOTE 2: All applicable sub-block gap sizes.NOTE 3: The PCC allocation is same as Transmission bandwidth configuration NRB as defined in Table 5.3.2-1. NOTE 4: The carrier center frequency of PCC in the DL operating band is configured closer to the UL operating band.NOTE 5: Refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission.NOTE 6: Wgap is the sub-block gap between the two sub-blocks.NOTE 7: The carrier centre frequency of SCC in the DL operating band is configured closer to the UL operating band.NOTE 8: For operation with three or more non-contiguous component carriers, ΔRIBNC applies to all secondary component carriers.NOTE 9: Bandwidth Combination Set 0.NOTE 10: Bandwidth Combination Set 1 |

### ---Text omitted---

##### 7.3A.3.2.5 ΔRIB,c for five bands

Table 7.3A.3.2.5-1: ΔRIB,c due to CA (five bands)

|  |  |  |
| --- | --- | --- |
| Inter-band CA combination | NR Band | ΔRIB,c (dB) |
| CA\_n1-n3-n7-n28-n78 | n1 | 0.2 |
|  | n3 | 0.2 |
|  | n7 | 0.2 |
|  | n28 | 0.2 |
|  | n78 | 0.5 |

#### 7.3A.3.3 ΔRIB,c for Intra-band CA

Table 7.3A.3.3-1: ΔRIB,c due to Intra-band contiguous CA

|  |  |  |
| --- | --- | --- |
| Inter-band CA combination | Operating Band | ΔRIB,c (dB) |
| CA\_n96E | n96 | 0.5 |

Table 7.3A.3.3-2: ΔRIB,c due to Intra-band non-contiguous CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CA configuration | SCS(PCC/SCC)(kHz) | Aggregated channel bandwidth (PCC+SCC) | ΔRIBNC (dB) | Duplex mode |
| CA\_n96(4A) | 15/30/60 | 320MHz | 0.5 | TDD |

### 7.3A.4 Reference sensitivity exceptions due to UL harmonic interference for CA

### ---Text omitted---

Table 7.6A.2.1-2a: In-band blocking for intra-band contiguous CA with FDL\_low < 2700 MHz and FUL\_low < 2700 MHz

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Case 1 | Case 2 | Case 3 |
|  | Pinterferer | dBm | -56 | -44 |  |
| n2, n25, n41, n66, n484, n40 | Finterferer (offset) | MHz | -BWchannel CA/2 –FIoffset, case 1andBWchannel CA/2 +FIoffset, case 1 | ≤ -BWchannel CA/2 –FIoffset, case 2and≥ BWchannel CA/2 +FIoffset, case 2 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 15toFDL\_high + 15 |  |
| n71 | Finterferer | MHz | NOTE 2 | FDL\_low – 12toFDL\_high + 15 | FDL\_low – 12 |
| NOTE 1: The absolute value of the interferer offset Finterferer (offset) shall be further adjusted to MHz with SCS the sub-carrier spacing of the carrier closest to the interferer in MHz. The interferer is an NR signal with 15 kHz SCS.NOTE 2: For each carrier frequency, the requirement applies for two interferer carrier frequencies: a: -BWchannel CA/2 – FIoffset, case 1; b: BWchannel CA/2 + FIoffset, case 1NOTE 3: BWchannel CA denotes the aggregated channel bandwidth of the wanted signalNOTE 4: n48 follows the requirement in this frequency range according to the general requirement defined in Clause 7.1A. |

### ---Text omitted---

Table 7.6A.3-2: Out of-band blocking for intra-band contiguous CA

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Range1 | Range 2 | Range 3 |
|  | Pinterferer | dBm | -45 | -30 | -15 |
| n2, n25, n41, n66, n71, n485, n40 | Finterferer (CW) | MHz | -60 < f – FDL\_low < -15or15 < f – FDL\_high < 60 | -85 < f – FDL\_low ≤ -60or60 ≤ f – FDL\_high < 85 | 1 ≤ f ≤ FDL\_low – 85orFDL\_high + 85 ≤ f≤ 12750 |
| n77, n78(NOTE 3) | Finterferer (CW) | MHz | N/A | N/A | 1 ≤ f ≤ FDL\_low – MAX(200,3\*BWChannel\_CA)orFDL\_high+ MAX(200,3\*BWChannel\_CA)≤ f ≤ 12750 |
| n79(NOTE 4) | Finterferer (CW) | MHz | N/A | N/A | 1 ≤ f ≤ FDL\_low – MAX(150,3\*BWChannel\_CA)orFDL\_high + MAX(150,3\*BWChannel\_CA)≤ f ≤ 12750 |
| NOTE 1: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 6000 MHz.NOTE 2: BWChannel\_CA denotes the aggregated channel bandwidth of the wanted signalNOTE 3: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 2700 MHz and FInterferer < 4800 MHz. For BWChannel\_CA > 15 MHz, the requirement for Range 1 is not applicable and Range 2 applies from the frequency offset of 3\*BWChannel\_CA from the band edge. For BWChannel\_CA larger than 60 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.NOTE 4: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 3650 MHz and FInterferer < 5750 MHz. For BWChannel\_CA≥ 40 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.NOTE 5: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 2700 MHz and FInterferer < 4800 MHz |

### ---Text omitted---

Table 7.6A.4.1-1: Narrow-band blocking for intra-band contiguous CA

|  |  |  |  |
| --- | --- | --- | --- |
| NR band | Parameter | Unit | NR CA bandwidth class |
|  |  |  | B | C |
| n1, n2, n25, n41, n66, n71, n48, n40 | Pw in Transmission Bandwidth Configuration, per CC | dBm | REFSENS + NR CA Bandwidth Class specific value below |
|  |  |  | 16 | 16 |
|  | Puw (CW) | dBm | -55 | -55 |
|  | Fuw (offset for*f* = 15 kHz, 30 kHz) | MHz | - Foffset – 0.2/+ Foffset + 0.2 | - Foffset – 0.2/+ Foffset + 0.2 |
|  |  |  |  |  |
| NOTE 1: The transmitter shall be set a 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in Table 7.3.2-3 with PCMAX\_L,f,c defined in clause 6.2.4.NOTE 2: Reference measurement channel is specified in Annexes A.3.2 and A3.2 with one sided dynamic OCNG Pattern OP.1 FDD/TDD as described in Annex A.5.1.1/A.5.2.1.NOTE 3: The PREFSENS power level is specified in Table 7.3.2-1 and Table 7.3.2-2 for two and four antenna ports, respectively.NOTE 4: The Fuw (offset) is the frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer and shall be further adjusted to MHz to be offset from the sub-carrier raster. |

### ---End of changes---