**3GPP TSG-RAN WG4 Meeting #101-e *R4-2120433***

**Electronic meeting, November 1-12, 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.133** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Big CR to TS 38.133: Rel-16 WIs RRM maintenance Part 2 (Rel-17) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | MCC, Intel Corporation | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_pos | | | | |  | ***Date:*** | | | 2021-11-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This big CR is the mirror CR for R4-2120432. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | This big CR is the mirror CR for R4-2120432. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | This big CR is the mirror CR for R4-2120432. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | R4-2119401 Correction to Ês and Iot symbol definitions for gNB measurements  3.2, 3.3  R4-2117345 Draft CR on UE positioning measurement requirements  9.1.2  R4-2119331 CR to update positioning measurement requirements  9.9.1, 9.9.2, 9.9.3, 9.9.4  R4-2117757 Draft CR to 38.133 correction to NR positioning measurement requirements  9.9.2, 9.9.3, 9.9.4  R4-2119334 CR on accuracy requirements for positioning measurement  10.1.23.2  R4-2117759 Draft CR to 38.133 correction to NR positioning accuracy requirements  10.1.24, B.2.1.6  R4-2119336 CR to update TCs for PRS measurement requirements  A.6.6.12, A.7.6.9  R4-2117350 DraftCR on RSTD and UE Rx-Tx test cases  A.6.6.14, A.7.6.11  R4-2119338 CR to update TC for PRS measurement accuracy  A.6.7.15.1, A.7.7.12.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.533 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*<Start of change1>*

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

[…] Values included in square bracket must be considered for further studies, because it means that a decision about that value was not taken.

BWChannel Channel bandwidth, defined in TS 38.101-1, 38.101-2 and 38.101-3 subclause 3.2

Ês Received energy per RE (power normalized to the subcarrier spacing) during the useful part of the symbol, i.e. excluding the cyclic prefix, at the UE antenna connector or at the gNB reference point as defined in TS 38.215, subclause 5.2 for the respective measurement type

FC *RF reference frequency* on the channel raster, given in table 5.4.2.2-1 in TS 38.101-1 and 38.101-2

FC,low The Fc of the lowest carrier, expressed in MHz

Io The total received power density, including signal and interference, as measured at the UE antenna connector.

Ioc The power spectral density (integrated in a noise bandwidth equal to the chip rate and normalized to the chip rate) of a band limited noise source (simulating interference from cells, which are not defined in a test procedure) as measured at the UE antenna connector.

Iot The received power spectral density of the total noise and interference for a certain RE (power integrated over the RE and normalized to the subcarrier spacing) as measured at the UE antenna connector or at the gNB reference point as defined in TS 38.215, subclause 5.2 for the respective measurement type

 The power spectral density of a white noise source (average power per RE normalised to the subcarrier spacing), simulating interference from cells that are not defined in a test procedure, as measured at the UE antenna connector

 Physical Resource Block number as defined in clause 3.2 in TS 38.211.

 Timing offset between uplink and downlink radio frames at the UE, as defined in clause 4.2 in TS 38.213.

 Fixed timing advance offset, as defined in clause 7.1.2.2 in TS 38.133.

   Configured UE transmitted power as defined in clause 6.2.4 in TS 38.101-1, 38-101-2 and 38.101-3.

PCMAX,c Configured UE transmitted power on a serving cell *c* as defined in clause 6.2.4 in TS 38.101-1, 38-101-2 and 38.101-3

S Cell Selection Criterion defined in TS 38.304, subclause 5.2.3.2 for NR

SSB\_RP Received (linear) average power of the resource elements that carry NR synchronisation burst, measured at the UE antenna connector

Srxlev Cell selection RX level, defined in TS 38.304, subclause 5.2.3.2

Squal Cell selection quality, defined in TS 38.304, subclause 5.2.3.2

Sintrasearch Defined in TS 38.304 , subclause 5.2.4.7 for E-UTRAN amd 38.304 subclause 5.2.4.7 for NR

Snonintrasearch Defined in TS 38.304 , subclause 5.2.4.7

Threshx, high Defined in TS 38.304 , subclause 5.2.4.7

Threshx, low Defined in TS 38.304 , subclause 5.2.4.7

Threshserving, low Defined in TS 38.304 , subclause 5.2.4.7

TRE-ESTABLISH-REQ The RRC Re-establishment delay requirement, the time between the moment when erroneous CRCs are applied, to when the UE starts to send preambles on the PRACH.

Tc Basic time unit, defined in clause 4.1 of TS 38.211 [6].

Ts Reference time unit, defined in clause 4.1 of TS 38.211 [6].

Treselection Defined in TS 25.304, subclause 5.2.6.1.5

TreselectionRAT Defined in TS 36.304 , subclause 5.2.4.7

TreselectionEUTRA Defined in TS 36.304 , subclause 5.2.4.7

TreselectionUTRA Defined in TS 36.304 , subclause 5.2.4.7

TreselectionGERANDefined in TS 36.304 , subclause 5.2.4.

Threshx, high Defined in TS 38.304 , subclause 5.2.4.7

Threshx, low Defined in TS 38.304 , subclause 5.2.4.7

Threshserving, low Defined in TS 38.304 , subclause 5.2.4.7

TUE\_re-establish\_delay Time between the moments when any of the conditions requiring RRC re-establishment as defined in clause 5.3.7 in TS 38.331 [2] is detected by the UE and when the UE sends PRACH to the target PCell.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [11] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [11].

AoA Angle of Arrival

AoD Angle of Departure

BFD Beam Failure Detection

BFD-RS BFD Reference Signal

BLER Block Error Rate

BM-RS Beam Management Reference Signal

BWP Bandwidth Part

CA Carrier Aggregation

CBD Candidate Beam Detection

CBW Channel Bandwidth

CC Component Carrier

CCA Clear Channel Assessment

CLI Cross Link Interference

CMR Channel Measurement Resource

CORESET Control Resource Set

CP Cyclic Prefix

CSI Channel-State Information

CSI-RS CSI Reference Signal

CSI-RSRP CSI Reference Signal based Reference Signal Received Power

CSI-RSRQ CSI Reference Signal based Reference Signal Received Quality

CSI-SINR CSI Reference Signal based Signal to Noise and Interference Ratio

CSI\_RP Received (linear) average power of the resource elements that carry NR CSI-RS signals and channels, measured at the UE antenna connector

DBT Discovery Burst Transmission

DC Dual Connectivity

DCI Downlink Control Information

DL Downlink

DL-AoD Downlink Angle-of-Departure

DL-TDOA Downlink Time Difference Of Arrival

DMRS Demodulation Reference Signal

DRX Discontinuous Reception

E-CID Enhanced Cell ID

E-UTRA Evolved UTRA

E-UTRAN Evolved UTRAN

EN-DC E-UTRA-NR Dual Connectivity

FDD Frequency Division Duplex

FR Frequency Range

HARQ Hybrid Automatic Repeat Request

HO Handover

IMR Interference Measurement Resource

L1-RSRP Layer 1 RSRP

L1 SL-RSRP Layer 1 Sidelink RSRP which corresponds to PSCCH-RSRP and/or PSSCH-RSRP

LMF Location Management Function

LPP LTE Positioning Protocol

MAC Medium Access Control

MCG Master Cell Group

MDT Minimization of Drive Tests

MG Measurement Gap

MGL Measurement Gap Length

MGRP Measurement Gap Repetition Period

MIB Master Information Block

MN Master Node

MR-DC Multi-Radio Dual Connectivity

NE-DC NR-E-UTRA Dual Connectivity

NGEN-DC NG-RAN E-UTRA-NR Dual Connectivity

NR New Radio

NR-DC NR-NR Dual Connectivity

OFDM Orthogonal Frequency Division Multiplexing

OFDMA Orthogonal Frequency Division Multiple Access

OTDOA Observed Time Difference Of Arrival

PBCH Physical Broadcast Channel

PCC Primary Component Carrier

PCell Primary Cell

PDCCH Physical Downlink Control Channel

PDSCH Physical Downlink Shared Channel

PLMN Public Land Mobile Network

PRACH Physical RACH

PRP PRS Received Power

PRS Positioning Reference Signal

PRS-RSRP Positioning Reference Signal based Reference Signal Received Power

PSBCH Physical Sidelink Broadcast Channel

PSBCH-RSRP Physical Sidelink Broadcast Channel DMRS based Reference Signal Received Power

PSCCH Physical Sidelink Control Channel

PSCCH-RSRP Physical Sidelink Control Channel DMRS based Reference Signal Received Power

PSCell Primary SCell

PSS Primary Synchronization Signal

PSSCH Physical Sidelink Shared Channel

PSSCH-RSRP Physical Sidelink Shared Channel DMRS based Reference Signal Received Power

pTAG Primary Timing Advance Group

PUCCH Physical Uplink Control Channel

PUSCH Physical Uplink Shared Channel

QCL Quasi Co-Location

RACH Random Access Channel

RAT Radio Access Technology

RLM Radio Link Monitoring

RLM-RS Reference Signal for RLM

RMSI Remaining Minimum System Information

RRC Radio Resource Control

RRM Radio Resource Management

RSSI Received Signal Strength Indicator

RSRP Reference Signal Received Power

RSRQ Reference Signal Received Quality

RSTD Reference Signal Time Difference

RTT Round Trip Time

S-SSB Sidelink Synchronization Signal Block

S-SSB\_RP Received (linear) average power of the resource elements that carry NR S-SSB signals and channels, measured at the UE antenna connector

SA Standalone operation mode

SCC Secondary Component Carrier

SCell Secondary Cell

SCG Secondary Cell Group

SCS Subcarrier Spacing

SCSSSB SSB subcarrier spacing

SDL Supplementary Downlink

SFN System Frame Number

SFTD SFN and Frame Timing DifferenceSI System Information

SIB System Information Block

SL-RSSI Sidelink Received Signal Strength Indicator

SLSS Sidelink Synchronization Signal

SMTC SSB-based Measurement Timing configuration

SpCell Special Cell

SRS Sounding Reference Signal

SRS-RSRP Sounding Reference Signal based Reference Signal Received Power

SS-RSRP Synchronization Signal based Reference Signal Received Power

SS-RSRQ Synchronization Signal based Reference Signal Received Quality

SS-SINR Synchronization Signal based Signal to Noise and Interference Ratio

SSB Synchronization Signal Block

SSB\_RP Received (linear) average power of the resource elements that carry NR SSB signals and channels, measured at the UE antenna connector.

SSS Secondary Synchronization Signal

sTAG Secondary Timing Advance Group

SUL Supplementary Uplink

TA Timing Advance

TAG Timing Advance Group

TCI Transmission Configuration Indicator

TDD Time Division Duplex

TDOA Time Difference Of Arrival

TRP Transmission-Reception Point

TTI Transmission Time Interval

UE User Equipment

UL Uplink

*<End of change1>*

*<Start of change2>*

### 9.1.2 Measurement gap

If the UE requires measurement gaps to identify and measure intra-frequency cells and/or inter-frequency cells and/or inter-RAT E-UTRAN cells, and the UE does not support independent measurement gap patterns for different frequency ranges as specified in Table 5.1-1 in [18, 19, 20], in order for the requirements in the following clauses to apply the network must provide a single per-UE measurement gap pattern for concurrent monitoring of all frequency layers.

If the UE requires measurement gaps to identify and measure intra-frequency cells and/or inter-frequency cells and/or inter-RAT E-UTRAN cells, and the UE supports independent measurement gap patterns for different frequency ranges as specified in Table 5.1-1 in [18, 19, 20], in order for the requirements in the following clauses to apply the network must provide either per-FR measurement gap patterns for frequency range where UE requires per-FR measurement gap for concurrent monitoring of all frequency layers of each frequency range independently, or a single per-UE measurement gap pattern for concurrent monitoring of all frequency layers of all frequency ranges.

If the UE is configured via LPP [34] to measure PRS for any RSTD, PRS-RSRP, and UE Rx-Tx time difference measurement defined in TS 38.215 [4], in order for the requirements in clauses 9.9.2, 9.9.3, and 9.9.4 to apply, the network must provide

- a single per-UE measurement gap pattern for concurrent monitoring of all positioning frequency layers and intra-frequency, inter-frequency and/or inter-RAT frequency layers of all frequency ranges, or

During the per-UE measurement gaps the UE:

- is not required to conduct reception/transmission from/to the corresponding E-UTRAN PCell, E-UTRAN SCell(s) and NR serving cells for E-UTRA-NR dual connectivity except the reception of signals used for RRM measurement(s) and the signals used for random access procedure according to TS38.321 [7].

- is not required to conduct reception/transmission from/to the corresponding NR serving cells for SA (with single carrier or CA configured) except the reception of signals used for RRM measurement(s), PRS measurement(s) and the signals used for random access procedure according to [7].

- is not required to conduct reception/transmission from/to the corresponding PCell, SCell(s) and E-UTRAN serving cells for NR-E-UTRA dual connectivity except the reception of signals used for RRM measurement(s), PRS measurement(s) and the signals used for random access procedure according to [7].

- is not required to conduct reception/transmission from/to the corresponding NR serving cells for NR-DC except the reception of signals used for RRM measurement(s) , PRS measurement(s) and the signals used for random access procedure according to [7].

During the per-FR measurement gaps the UE:

- is not required to conduct reception/transmission from/to the corresponding E-UTRAN PCell, E-UTRAN SCell(s) and NR serving cells in the corresponding frequency range for E-UTRA-NR dual connectivity except the reception of signals used for RRM measurement(s) and the signals used for random access procedure according to TS38.321 [7].

- is not required to conduct reception/transmission from/to the corresponding NR serving cells in the corresponding frequency range for SA (with single carrier or CA configured) except the reception of signals used for RRM measurement(s) and the signals used for random access procedure according to TS38.321 [7].

- is not required to conduct reception/transmission from/to the corresponding PCell, SCell(s) and E-UTRAN serving cells in the corresponding frequency range for NR-E-UTRA dual connectivity except the reception of signals used for RRM measurement(s) and the signals used for random access procedure according to TS38.321 [7].

- is not required to conduct reception/transmission from/to the corresponding NR serving cells in the corresponding frequency range for NR-DC except the reception of signals used for RRM measurement(s) and the signals used for random access procedure according to TS38.321 [7].

*<End of change2>*

*<Start of change3>*

### 9.9.1 Introduction

This clause contains requirements for UE capable of performing NR positioning measurements defined in TS 38.215 [4], including RSTD, PRS-RSRP, UE Rx-Tx time difference, and NR E-CID measurements.

For RSTD, PRS-RSRP and UE Rx-Tx time difference measurements, the requirements in clauses 9.9.2, 9.9.3 and 9.9.4 apply provided:

- UE is configured with per-UE measurement gaps

- No active BWP switching occurs during the measurement gaps for PRS measurement, and

All measurement requirements specified in clause 9.9.2, 9.9.3 and 9.9.4 shall apply without DRX as well as for any DRX configuration specified in TS 38.331 [2].

UE is not required to perform additional SSB measurement for the SSB configured as QCL source of PRS resources.

UE is only required to measure PRS resources that are fully or partially overlapped with measurement gaps, and the requirements in clause 9.9.2, 9.9.3 and 9.9.4 are applicable to PRS resources that are fully or partially overlapped with measurement gaps.

A PRS resource is considered to be fully (partially) overlapped with measurement gaps if all (some) of its instances are overlapped with a measurement gap occasion. A PRS resource instance is considered to be overlapped with measurement gap occasion if the minimum number of unmuted repetitions of the instance taking into account *nr-DL-PRS-ExpectedRSTD-Uncertainty* and *nr-DL-PRS-ExpectedRSTD* is fully covered by the MGL excluding RF switching time, where the minimum number is given in the accuracy requirements in clause 10.1.23, 10.1.24 and 10.1.25 for RSTD, PRS-RSRP and UE Rx-Tx time difference, respectively.

When UE is configured with measurement for more than one positioning requests, the measurement period for each request may be longer than measurement period when UE is configured with measurement for single positioning request.

### 9.9.2 RSTD measurements

#### 9.9.2.1 Introduction

The requirements in clause 9.9.2 shall apply provided the UE has received *NR-DL-TDOA-RequestLocationInformation* message from LMF via LPP [34] requesting the UE to measure and report DL RSTD measurements defined in TS 38.215 [4].

#### 9.9.2.2 Requirements Applicability

The requirements in clause 9.9.2 apply for periodic and triggered RSTD measurements, provided:

- PRS-RSTD related side conditions given in clause 10.1.23 for FR1 and FR2 are fulfilled, for a corresponding Band.

#### 9.9.2.3 Measurement Capability

UE PRS RSTD measurement capability is as indicated by the UE in *NR-DL-TDOA-ProvideCapabilities*, according to TS 37.355[34].

#### 9.9.2.4 Measurement Reporting Requirements

The measurement reporting delay is defined as the time between the moment when the periodic measurement report is triggered and the moment when the UE starts to transmit the measurement report over the air interface. This requirement assumes that the measurement report is not delayed by other LPP signalling on the DCCH. This measurement reporting delay excludes a delay uncertainty resulted when inserting the measurement report to the TTI of the uplink DCCH. The delay uncertainty is: 2 x TTIDCCH where TTIDCCH is the duration of subframe or slot or subslot when the measurement report is transmitted on the PUSCH with subframe or slot or subslot duration. This measurement reporting delay excludes any delay caused by no UL resources for UE to send the measurement report.

The reported RSTD measurement values contained in measurement reports shall be based on the measurement report mapping requirements specified in clauses 10.1.23.3.

The RSTD measurements performed and reported according to this section shall meet the RSTD measurement accuracy requirements in clause 10.1.23, for each measured DL PRS resource.

##### 9.9.2.4.1 Void

##### 9.9.2.4.2 Void

##### 9.9.2.4.3 Void

#### 9.9.2.5 Measurements Period Requirements

When physical layer receives last of *NR-TDOA-ProvideAssistanceData* message and *NR-TDOA-RequestLocationInformation* message from LMF via LPP [34]*,* the UE shall be able to measure multiple (up to the UE capability specified in Clause 9.9.2.3) DL RSTD measurements, defined in TS 38.215 [4], during the measurement period defined as:

Where ,

is the index of positioning frequency layer,

is total number of positioning frequency layers, and

is the periodicity of the PRS RSTD measurement in positioning frequency layer i

is the measurement period for PRS RSTD measurement in positioning frequency layer *i* as specified below:

,

where:

is the UE Rx beam sweeping factor. In FR1, = 1; and in FR2, = 8.

is the carrier-specific scaling factor for NR PRS-based positioning measurements in positioning frequency layer *i* as defined in clause 9.1.5.2.

is the maximum number of DL PRS resources in positioning frequency layer *i* configured in a slot.

is the time duration of available PRS in the positioning frequency layer i to be measured during , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only the PRS resources unmuted and fully or partially overlapped with MG are considered.

is the number of PRS RSTD samples and = 4.

is the measurement duration for the last PRS RSTD sample in positioning frequency layer *i*, including the sampling time and processing time, = + ,

is the periodicity of the PRS RSTD measurement in positioning frequency layer i defined as:

*=*

Where,

corresponds to *durationOfPRS-ProcessingSymbolsInEveryTms* in TS 37.355 [34],

*,* the least common multiple between and .

is the repetition periodicity of the measurement gap applicable for measurement in the PRS frequency layer i.

is the periodicity of DL PRS resource with muting on positioning frequency layer *i*.

If more than one PRS periodicities are configured in positioning frequency layer *i*, the least common multiple of PRS periodicities among all DL PRS resource sets in the positioning frequency layer is used to derive , where,

, is the PRS periodicity with muting per PRS resource,

is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

is the scaling factor considering PRS resource muting. , where

is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and is the size of the bitmap .

* Note: For the purpose of calculating TPRS,i, only the PRS resources fully or partially covered by the MG are considered.

is UE capability combination per band where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSysmbols* in TS 37.355 [34] processed every T ms corresponding to *durationOfPRS-ProcessingSymbolsInEveryTms* in TS 37.355 [34] for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in TS 37.355 [34].

is UE capability for number of DL PRS resources that it can process in a slot as indicated by *maxNumOfDL-PRS-ResProcessedPerSlot* specified in TS 37.355 [34].

The time *s*tarts from the first MG instance aligned with a DL PRS resource(s) in the assistance data after both the *NR-TDOA-ProvideAssistanceData* message and *NR-TDOA-RequestLocationInformation* message are delivered from LMF to the physical layer of UE via LPP [34].

Note: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

If during the measurement period of one or more positioning frequency layers, the MG pattern is reconfigured, the measurement period can be longer. When PRS-RSRP is configured for DL-TDOA, RSTD and RSRP are performed over the same measurement period.

The measurement requirements in this clause apply, provided no PRS symbols are dropped during the measurement period TRSTD,Total within measurement gaps due to collisions with other signals; otherwise, the measurement period can be longer.

The measurement requirements do not apply for a PRS resource, if the PRS resource is across two sampling duration of N within duration .

The measurement requirements do not apply for a PRS resource, if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

The requirements in clause 9.9.2 do not apply if the PRS configuration given by higher layer paramters *NR-DL-PRS-AssistanceData* exceeds any of the UE measurement capabilities given by *NR-DL-PRS-ResourcesCapability* in *NR-DL-TDOA-ProvideCapabilities*, and it is up to UE implementation which PRS resources are measured, subject to UE measurement capabilities*.*

If handover occurs while RSTD measurements are being performed, then the UE shall continue and complete the on-going RSTD measurements. The UE shall also meet the RSTD measurement requirements in this clause and measurement accuracy requirements in clause 10.1.23. However, in this case the RSTD measurement period shall be as follows:

Where,

- is the number of times handover occurs during ;

- is the largest among all positioning frequency layers;

- is the time during which the RSTD measurement may not be possible due to handover; it can be up to Tinterrupt as defined in clause 6.1.

#### 9.9.2.6 Void

### 9.9.3 PRS-RSRP measurements

#### 9.9.3.1 Introduction

The requirements in clause 9.9.3.5 shall apply provided the UE has received a message from LMF via LPP [34] requesting the UE to measure and report PRS-RSRP measurements defined in TS 38.215 [4].

#### 9.9.3.2 Requirements applicability

The requirements in clause 9.9.3 apply for periodic and triggered PRS-RSRP measurements, provided:

- PRS-RSRP related side conditions given in clause 10.1.24 are met for a corresponding Band.

#### 9.9.3.3 Measurement Capability

UE PRS-RSRP measurement capability is as indicated by the UE in *NR-DL-AoD-ProvideCapabilities* according to TS 37.355 [34].

#### 9.9.3.4 Measurement Reporting Requirements

This requirement assumes that the measurement report is not delayed by other LPP signalling on the DCCH. This measurement reporting delay excludes a delay uncertainty resulted when inserting the measurement report to the TTI of the uplink DCCH. The delay uncertainty is: 2 x TTIDCCH where TTIDCCH is the duration of subframe or slot or subslot when the measurement report is transmitted on the PUSCH with subframe or slot or subslot duration. This measurement reporting delay excludes any delay caused by no UL resources for UE to send the measurement report.

The reported PRS-RSRP measurement values contained in measurement reports shall be based on the measurement report mapping requirements specified in clauses 10.1.24.3.

The PRS-RSRP measurement accuracy for all measured PRS resources shall be fulfilled according to the accuracy requriements specified in the clauses 10.1.24.

#### 9.9.3.5 Measurement Period Requirements

When the physical layer receives *NR-DL-AoD-ProvideAssistanceData* message and *NR-DL-AoD-RequestLocationInformation* message from LMF via LPP [34], the UE shall be able to measure multiple (up to the UE capability specified in Clause 9.9.3.3) PRS-RSRP measurements, defined in TS 38.215 [4], from configured PRS resources for configured TRPs on configured positioning frequency layers, within ms.

where

*i* is the index of positioning frequency layer,

L is total number of positioning frequency layers,

is the periodicity of the PRS-RSRP measurement in positioning frequency layer *i*.

where

is the carrier specific scaling factor for PRS-RSRP measurements specified in clause 9.1.5.2,

is the scaling factor for Rx beam sweeping, and =1 if positioning frequency layer *i* is in FR1 and =8 if positioning frequency layer *i* is in FR2,

is the time duration of available PRS to be measured in the positioning frequency layer i to be measured during , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only the PRS resources unmuted and fully or partially overlapped with MG are considered.

is the maximum number of DL PRS resources of positioning frequency layer i configured in a slot,

is UE capability combination per band where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSysmbols* in TS 37.355 [34] processed every T ms corresponding to *durationOfPRS-ProcessingSymbolsInEveryTms* in TS 37.355 [34] for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in TS 37.355 [34],

is UE capability for number of DL PRS resources that it can process in a slot as indicated by *maxNumOfDL-PRS-ResProcessedPerSlot* in clause 6.4.3 of TS 37.355 [34],

is the number of PRS-RSRP measurement samples and = 4,

*= +* is the measurement duration for the last PRS-RSRP sample, including the sampling time and processing time,

is the periodicity of PRS-RSRP measurement in positioning frequency layer *i*,

corresponds to durationOfPRS-ProcessingSymbolsInEveryTms in TS 37.355 [34],

the least common multiple between and ,

is the maximum PRS resource periodicity among all PRS resources in positioning frequency layer i,

is the measurement gap repetition period in positioning frequency layer i.

If positioning frequency layer *i* has more than one DL PRS resource set with different PRS periodicities with muting, , the least common multiple of among the DL PRS resource sets is used to derive , where:

is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

is the scaling factor considering PRS resource muting. , where is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and is the size of the bitmap .

Note: For the purpose of calculating TPRS,i, only the PRS resources fully or partially covered by the MG are considered.

When PRS-RSRP measurements are configured for DL-AoD, the time starts from the first MG instance aligned with DL PRS resources in the assistance data after both the *NR-DL-AoD-RequestLocationInformation* message and *NR-DL-AoD-ProvideAssistanceData* message from LMF via LPP [34] are delivered to the physical layer of UE.

Note: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

When the PRS-RSRP measurement is configured together with RSTD measurement then the PRS-RSRP measurement shall meet the RSTD measurement requirements defined in clause 9.9.2.

When the PRS-RSRP measurement is configured together with UE Rx-Tx time difference measurement then the PRS-RSRP measurement shall meet the UE Rx-Tx time difference measurement requirements defined in clause 9.9.4.

The measurement requirements do not apply for a PRS resource:

- if the PRS resource is across two sampling duration of N within duration or

- if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

If during the measurement period of one or more positioning frequency layers, the MG pattern is reconfigured either per UE request or not per UE request, the measurement period can be longer.

The requirements in this section apply, provided no PRS symbols are dropped during the measurement period within measurement gaps due to collisions with other signals; otherwise, a longer measurement period may be used.

The requirements in clause 9.9.3 do not apply if the PRS configuration given by higher layer paramters *NR-DL-PRS-AssistanceData* exceeds any of the UE measurement capabilities given by *NR-DL-PRS-ResourcesCapability* in *NR-DL-AoD-ProvideCapabilities*, and it is up to UE implementation which PRS resources are measured, subject to UE measurement capabilities*.*

If handover occurs while PRS-RSRP measurements are being performed then the UE shall complete the ongoing PRS-RSRP measurements session. The UE shall also meet the PRS-RSRP measurement requirements in this clause and measurement accuracy requirements in clause 10.1.24. However, in this case the PRS-RSRP measurement period shall be as follows:

where

is the number of times handover occurs during ;

is the largest among all positioning frequency layers;

is the time during which the PRS-RSRP measurement may not be possible due to handover; it can be up to Tinterrupt as defined in clause 6.1.

### 9.9.4 UE Rx-Tx time difference measurements

#### 9.9.4.1 Introduction

The requirements in this clause shall apply, provided the UE has received *nr-Multi-RTT-RequestLocationInformation* message from LMF via LPP [34] requesting the UE to measure and report one or more UE Rx-Tx time difference measurements defined in TS 38.215 [4].

#### 9.9.4.2 Requirements Applicability

The requirements in clause 9.9.4 apply for periodic and triggered UE Rx-Tx time difference measurements, provided:

- UE Rx-Tx time difference measurement related side conditions given in clause 10.1.25 are met for a corresponding band.

- SRS is configured on at least one of the PCell, PSCell and SCell.

#### 9.9.4.3 Measurement Capability

UE Rx-Tx time difference measurement capability is as indicated by the UE in *NR-Multi-RTT-ProvideCapabilities,* according to TS 37.355 [34].

#### 9.9.4.4 Measurement Reporting Requirements

This requirement assumes that the measurement report is not delayed by other LPP signalling on the DCCH. This measurement reporting delay excludes a delay uncertainty resulted when inserting the measurement report to the TTI of the uplink DCCH. The delay uncertainty is: 2 x TTIDCCH where TTIDCCH is the duration of subframe or slot or subslot when the measurement report is transmitted on the PUSCH with subframe or slot or subslot duration. This measurement reporting delay excludes any delay caused by no UL resources for UE to send the measurement report.

The UE Rx-Tx time difference measurement values contained in measurement reports shall be based on the measurement report mapping requirements specified in clause 10.1.25.

The UE Rx-Tx time difference measurement accuracy for all measured DL PRS resourcesshall be fulfilled according to the accuracy requirements specified in clause 10.1.25.

#### 9.9.4.5 Measurement Period Requirements

When physical layer receives last of *NR-Multi-RTT-ProvideAssistanceData* message and *NR-Multi-RTT-RequestLocationInformation* message from LMF via LPP [34]*,* UE shall be able to measure multiple (up to the UE capability specified in clause 9.9.4.3) UE Rx-Tx time difference measurements as defined in TS 38.215 [4] in configured positioning frequency layers within the measurement period ms.

*.*

where is the index of positioning frequency layer,

is the measurement period for UE Rx-Tx time difference measurements in positioning frequency layer *i* as further defined in this clause,

L is total number of positioning frequency layers, and

is the periodicity of the UE Rx-Tx time difference measurement in positioning frequency layer *i* as defined further in this clause.

Where

is the carrier-specific scaling factor for NR PRS-based measurement in the positioning frequency layer *i* as defined in clause 9.1.5.2,

is the scaling factor for Rx beam sweeping, and =1 if positioning frequency layer *i* is in FR1 and =8 if positioning frequency layer *i* is in FR2,

is the time duration of available PRS resources in the positioning frequency layer *i*, to be measured during , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only the PRS resources unmuted and fully or partially overlapped with MG are considered.

is the maximum number of DL PRS resources of positioning frequency layer i configured in a slot,

is UE capability combination per band where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSysmbols* in TS 37.355 [34] processed every T ms corresponding to *durationOfPRS-ProcessingSymbolsInEveryTms* in TS 37.355 [34] for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in clause 4.2.7.2 of TS 37.355 [34],

is UE capability for number of DL PRS resources that it can process in a slot corresponding to *maxNumOfDL-PRS-ResProcessedPerSlot* as specified in clause 6.4.3 of TS 37.355 [34],

is the number of UE Rx-Tx time difference measurement samples and = 4,

is the measurement duration for the last UE Rx-Tx time difference measurement sample in the positioning layer i, including the sampling time and processing time,  *= +*  ,

is periodicity of UE Rx-Tx time difference measurement in positioning frequency layer *i*:

where

corresponds to durationOfPRS-ProcessingSymbolsInEveryTms in TS 37.355 [34],

, the least common multiple between and

is the measurement gap repetition periodicity in positioning frequency layer i.

is the PRS resource periodicity in positioning frequency layer *i*. If the positioning frequency layer *i* has more than one DL PRS resource sets with different PRS periodicities with muting, , the least common multiple of among DL PRS resource sets is used to derive , where

is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

is the scaling factor considering PRS resource muting. , where is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and is the size of the bitmap .

Note: For the purpose of calculating TPRS,i, only the PRS resources fully or partially covered by the MG are considered.

The time starts from the first MG instance aligned with DL PRS resources in the assistance data after both the *NR-Multi-RTT-RequestLocationInformation* message and *NR-Multi-RTT-ProvideAssistanceData* message from LMF via LPP [34] are delivered to the physical layer of UE.

Note: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

The UE Rx-Tx time difference measurement period is restarted if HO occurs during the measurement period and after SRS reconfiguration on the target cell is complete.

The measurement requirements do not apply for a PRS resource:

- if the PRS resource is across two sampling duration of N within duration or

- if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

If during the measurement period of one or more positioning frequency layers, the MG pattern is reconfigured either per UE request or not per UE request, the measurement period can be longer.

The requirements in this section apply, provided no PRS symbols are dropped during the measurement period TUERxTx,Total within measurement gaps due to collisions with other signals; otherwise, a longer measurement period may be used.

When PRS-RSRP is configured for multi-RTT, the UE Rx-Tx time difference measurements and PRS-RSRP measurements are performed over the same measurement period.

The requirements in clause 9.9.4 do not apply if the PRS configuration given by higher layer paramters *NR-DL-PRS-AssistanceData* exceeds any of the UE measurement capabilities given by *NR-DL-PRS-ResourcesCapability* in *NR-Multi-RTT-ProvideCapabilities*, and it is up to UE implementation which PRS resources are measured, subject to UE measurement capabilities*.*

*Editor’s note: FFS: Measurement period requirements when cell change does not impact SRS configuration*

*Editor’s note: FFS: Measurement period requirements when cell change does impact SRS configuration*

If UE uplink transmission timing changes due to the network-configured Timing Advance command during the UE Rx-Tx measurement period, then the UE Rx-Tx time difference measurement period is restarted after uplink transmission timing changes, and the UE Rx-Tx time difference measurement period requirements in this clause shall not apply.

If UE uplink transmission timing changes due to the change in the NTA\_offset defined in Table 7.1.2-2 during the UE Rx-Tx measurement period, then the UE Rx-Tx time difference measurement period is restarted after uplink transmission timing changes, and the UE Rx-Tx time difference measurement period requirements in this clause shall not apply.

*<End of change3>*

*<Start of change4>*

9.9.2 RSTD measurements

9.9.2.1 Introduction

The requirements in clause 9.9.2 shall apply provided the UE has received *NR-DL-TDOA-RequestLocationInformation* message from LMF via LPP [34] requesting the UE to measure and report DL RSTD measurements defined in TS 38.215 [4].

9.9.2.2 Requirements Applicability

The requirements in clause 9.9.2 apply for periodic and triggered RSTD measurements, provided:

- PRS-RSTD related side conditions given in clause 10.1.23 for FR1 and FR2 are fulfilled, for a corresponding Band.

9.9.2.3 Measurement Capability

UE PRS RSTD measurement capability is as indicated by the UE in *NR-DL-TDOA-ProvideCapabilities*, according to TS 37.355[34].

9.9.2.4 Measurement Reporting Requirements

The measurement reporting delay is defined as the time between the moment when the periodic measurement report is triggered and the moment when the UE starts to transmit the measurement report over the air interface. This requirement assumes that the measurement report is not delayed by other LPP signalling on the DCCH. This measurement reporting delay excludes a delay uncertainty resulted when inserting the measurement report to the TTI of the uplink DCCH. The delay uncertainty is: 2 x TTIDCCH where TTIDCCH is the duration of subframe or slot or subslot when the measurement report is transmitted on the PUSCH with subframe or slot or subslot duration. This measurement reporting delay excludes any delay caused by no UL resources for UE to send the measurement report.

The reported RSTD measurement values contained in measurement reports shall be based on the measurement report mapping requirements specified in clauses 10.1.23.3.

The RSTD measurements performed and reported according to this section shall meet the RSTD measurement accuracy requirements in clause 10.1.23, for each measured DL PRS resource.

9.9.2.4.1 Void

9.9.2.4.2 Void

9.9.2.4.3 Void

9.9.2.5 Measurements Period Requirements

When physical layer receives last of *NR-TDOA-ProvideAssistanceData* message and *NR-TDOA-RequestLocationInformation* message from LMF via LPP [34]*,* the UE shall be able to measure multiple (up to the UE capability specified in Clause 9.9.2.3) DL RSTD measurements, defined in TS 38.215 [4], during the measurement period defined as:

Where ,

is the index of positioning frequency layer,

is total number of positioning frequency layers, and

is the periodicity of the PRS RSTD measurement in positioning frequency layer i

is the measurement period for PRS RSTD measurement in positioning frequency layer *i* as specified below:

,

where:

is the UE Rx beam sweeping factor. In FR1, = 1; and in FR2, = 8.

is the carrier-specific scaling factor for NR PRS-based positioning measurements in positioning frequency layer *i* as defined in clause 9.1.5.2.

is the maximum number of DL PRS resources in positioning frequency layer *i* configured in a slot.

is the time duration of available PRS in the positioning frequency layer i to be measured during , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only the PRS resources unmuted and fully or partially overlapped with MG are considered.

is the number of PRS RSTD samples and = 4.

is the measurement duration for the last PRS RSTD sample in positioning frequency layer *i*, including the sampling time and processing time, = + ,

is the periodicity of the PRS RSTD measurement in positioning frequency layer i defined as:

*=*

Where,

corresponds to *durationOfPRS-ProcessingSymbolsInEveryTms* in TS 37.355 [34],

*,* the least common multiple between and .

is the repetition periodicity of the measurement gap applicable for measurement in the PRS frequency layer i.

is the periodicity of DL PRS resource with muting on positioning frequency layer *i*.

If more than one PRS periodicities are configured in positioning frequency layer *i*, the least common multiple of PRS periodicities among all DL PRS resource sets in the positioning frequency layer is used to derive the measurement period of that positioning frequency layer *i*. Where,

, is the PRS periodicity with muting per PRS resource,

is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

is the scaling factor considering PRS resource muting. If bitmap for higher-layer parameter *DL-PRS-MutingPattern* is provided, and , then ; otherwise, if bitmap is not provided or , then .

is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and L is the size of the bitmap .

* Note: For the purpose of calculating TPRS,i, only the PRS resources fully or partially covered by the MG are considered.

is UE capability combination per band where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSysmbols* in TS 37.355 [34] processed every T ms corresponding to *durationOfPRS-ProcessingSymbolsInEveryTms* in TS 37.355 [34] for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in TS 37.355 [34].

is UE capability for number of DL PRS resources that it can process in a slot as indicated by *maxNumOfDL-PRS-ResProcessedPerSlot* specified in TS 37.355 [34].

The time *s*tarts from the first MG instance aligned with a DL PRS resource(s) in the assistance data after both the *NR-TDOA-ProvideAssistanceData* message and *NR-TDOA-RequestLocationInformation* message are delivered from LMF to the physical layer of UE via LPP [34].

Note: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

If during the measurement period of one or more positioning frequency layers, the MG pattern is reconfigured, the measurement period can be longer. When PRS-RSRP is configured for DL-TDOA, RSTD and RSRP are performed over the same measurement period.

The measurement requirements in this clause apply, provided no PRS symbols are dropped during the measurement period TRSTD,Total within measurement gaps due to collisions with other signals; otherwise, the measurement period can be longer.

If CSSF changes during the measurement period, the measurement period could be longer.

The measurement requirements do not apply for a PRS resource, if the PRS resource is across two sampling duration of N within duration LPRS.

The measurement requirements do not apply for a PRS resource, if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

If handover occurs while RSTD measurements are being performed, then the UE shall continue and complete the on-going RSTD measurements. The RSTD measurement period can be longer. The UE shall meet the RSTD measurement accuracy requirements in clause 10.1.23.

9.9.2.6 Void

9.9.3 PRS-RSRP measurements

9.9.3.1 Introduction

The requirements in clause 9.9.3.5 shall apply provided the UE has received a message from LMF via LPP [34] requesting the UE to measure and report PRS-RSRP measurements defined in TS 38.215 [4].

9.9.3.2 Requirements applicability

The requirements in clause 9.9.3 apply for periodic and triggered PRS-RSRP measurements, provided:

- PRS-RSRP related side conditions given in clause 10.1.24 are met for a corresponding Band.

9.9.3.3 Measurement Capability

UE PRS-RSRP measurement capability is as indicated by the UE in *NR-DL-AoD-ProvideCapabilities* according to TS 37.355 [34].

9.9.3.4 Measurement Reporting Requirements

This requirement assumes that the measurement report is not delayed by other LPP signalling on the DCCH. This measurement reporting delay excludes a delay uncertainty resulted when inserting the measurement report to the TTI of the uplink DCCH. The delay uncertainty is: 2 x TTIDCCH where TTIDCCH is the duration of subframe or slot or subslot when the measurement report is transmitted on the PUSCH with subframe or slot or subslot duration. This measurement reporting delay excludes any delay caused by no UL resources for UE to send the measurement report.

The reported PRS-RSRP measurement values contained in measurement reports shall be based on the measurement report mapping requirements specified in clauses 10.1.24.3.

The PRS-RSRP measurement accuracy for all measured PRS resources shall be fulfilled according to the accuracy requriements specified in the clauses 10.1.24.

9.9.3.5 Measurement Period Requirements

When the physical layer receives *NR-DL-AoD-ProvideAssistanceData* message and *NR-DL-AoD-RequestLocationInformation* message from LMF via LPP [34], the UE shall be able to measure multiple (up to the UE capability specified in Clause 9.9.3.3) PRS-RSRP measurements, defined in TS 38.215 [4], from configured PRS resources for configured TRPs on configured positioning frequency layers, within ms.

where

*i* is the index of positioning frequency layer,

L is total number of positioning frequency layers,

is the periodicity of the PRS-RSRP measurement in positioning frequency layer *i*.

where

is the carrier specific scaling factor for PRS-RSRP measurements specified in clause 9.1.5.2,

is the scaling factor for Rx beam sweeping, and =1 if positioning frequency layer *i* is in FR1 and =8 if positioning frequency layer *i* is in FR2,

is the time duration of available PRS to be measured in the positioning frequency layer i to be measured during , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only the PRS resources unmuted and fully or partially overlapped with MG are considered.

is the maximum number of DL PRS resources of positioning frequency layer i configured in a slot,

is UE capability combination per band where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSysmbols* in TS 37.355 [34] processed every T ms corresponding to *durationOfPRS-ProcessingSymbolsInEveryTms* in TS 37.355 [34] for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in TS 37.355 [34],

is UE capability for number of DL PRS resources that it can process in a slot as indicated by *maxNumOfDL-PRS-ResProcessedPerSlot* in clause 6.4.3 of TS 37.355 [34],

is the number of PRS-RSRP measurement samples and = 4,

*= +* is the measurement duration for the last PRS-RSRP sample, including the sampling time and processing time,

is the periodicity of PRS-RSRP measurement in positioning frequency layer *i*,

corresponds to durationOfPRS-ProcessingSymbolsInEveryTms in TS 37.355 [34],

the least common multiple between and ,

is the maximum PRS resource periodicity among all PRS resources in positioning frequency layer i,

is the measurement gap repetition period in positioning frequency layer i.

If positioning frequency layer *i* has more than one DL PRS resource set with different PRS periodicities with muting, , the least common multiple of among the DL PRS resource sets is used to derive the measurement period of that positioning frequency layer. Where:

is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

is the scaling factor considering PRS resource muting. If bitmap for higher-layer parameter *DL-PRS-MutingPattern* is provided, and , then ; otherwise, if bitmap is not provided or , then . is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and L is the size of the bitmap .

Note: For the purpose of calculating TPRS,i, only the PRS resources fully or partially covered by the MG are considered.

When PRS-RSRP measurements are configured for DL-AoD, the time starts from the first MG instance aligned with DL PRS resources in the assistance data after both the *NR-DL-AoD-RequestLocationInformation* message and *NR-DL-AoD-ProvideAssistanceData* message from LMF via LPP [34] are delivered to the physical layer of UE.

Note: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

When the PRS-RSRP measurement is configured together with RSTD measurement then the PRS-RSRP measurement shall meet the RSTD measurement requirements defined in clause 9.9.2.

When the PRS-RSRP measurement is configured together with UE Rx-Tx time difference measurement then the PRS-RSRP measurement shall meet the UE Rx-Tx time difference measurement requirements defined in clause 9.9.4.

If CSSF changes during the measurement period, the measurement period could be longer.

The requirements in this section apply, provided no PRS symbols are dropped during the measurement period TPRS-RSRP,Total within measurement gaps due to collisions with other signals; otherwise, a longer measurement period may be used.

The measurement requirements do not apply for a PRS resource:

- if the PRS resource is across two sampling duration of N within duration or

- if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

If during the measurement period of one or more positioning frequency layers, the MG pattern is reconfigured either per UE request or not per UE request, the measurement period can be longer.

The requirements in this section apply, provided no PRS symbols are dropped during the measurement period within measurement gaps due to collisions with other signals; otherwise, a longer measurement period may be used.

If handover occurs while PRS-RSRP measurements are being performed then the UE shall complete the ongoing PRS-RSRP measurements session. The PRS-RSRP measurement period can be longer. The UE shall meet the PRS-RSRP measurement accuracy requirements in clause 10.1.24.

*<End of change4>*

*<Start of change5>*

### 9.9.4 UE Rx-Tx time difference measurements

#### 9.9.4.1 Introduction

The requirements in this clause shall apply, provided the UE has received *nr-Multi-RTT-RequestLocationInformation* message from LMF via LPP [34] requesting the UE to measure and report one or more UE Rx-Tx time difference measurements defined in TS 38.215 [4].

#### 9.9.4.2 Requirements Applicability

The requirements in clause 9.9.4 apply for periodic and triggered UE Rx-Tx time difference measurements, provided:

- UE Rx-Tx time difference measurement related side conditions given in clause 10.1.25 are met for a corresponding band.

- SRS is configured on at least one of the PCell, PSCell and SCell.

#### 9.9.4.3 Measurement Capability

UE Rx-Tx time difference measurement capability is as indicated by the UE in *NR-Multi-RTT-ProvideCapabilities,* according to TS 37.355 [34].

#### 9.9.4.4 Measurement Reporting Requirements

This requirement assumes that the measurement report is not delayed by other LPP signalling on the DCCH. This measurement reporting delay excludes a delay uncertainty resulted when inserting the measurement report to the TTI of the uplink DCCH. The delay uncertainty is: 2 x TTIDCCH where TTIDCCH is the duration of subframe or slot or subslot when the measurement report is transmitted on the PUSCH with subframe or slot or subslot duration. This measurement reporting delay excludes any delay caused by no UL resources for UE to send the measurement report.

The UE Rx-Tx time difference measurement values contained in measurement reports shall be based on the measurement report mapping requirements specified in clause 10.1.25.

The UE Rx-Tx time difference measurement accuracy for all measured DL PRS resourcesshall be fulfilled according to the accuracy requirements specified in clause 10.1.25.

#### 9.9.4.5 Measurement Period Requirements

When physical layer receives last of *NR-Multi-RTT-ProvideAssistanceData* message and *NR-Multi-RTT-RequestLocationInformation* message from LMF via LPP [34]*,* UE shall be able to measure multiple (up to the UE capability specified in clause 9.9.4.3) UE Rx-Tx time difference measurements as defined in TS 38.215 [4] in configured positioning frequency layers within the measurement period ms.

*.*

where is the index of positioning frequency layer,

is the measurement period for UE Rx-Tx time difference measurements in positioning frequency layer *i* as further defined in this clause,

L is total number of positioning frequency layers, and

is the periodicity of the UE Rx-Tx time difference measurement in positioning frequency layer *i* as defined further in this clause.

Where

is the carrier-specific scaling factor for NR PRS-based measurement in the positioning frequency layer *i* as defined in clause 9.1.5.2,

is the scaling factor for Rx beam sweeping, and =1 if positioning frequency layer *i* is in FR1 and =8 if positioning frequency layer *i* is in FR2,

is the time duration of available PRS resources in the positioning frequency layer *i*, to be measured during , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only the PRS resources unmuted and fully or partially overlapped with MG are considered.

is the maximum number of DL PRS resources of positioning frequency layer i configured in a slot,

is UE capability combination per band where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSysmbols* in TS 37.355 [34] processed every T ms corresponding to *durationOfPRS-ProcessingSymbolsInEveryTms* in TS 37.355 [34] for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in clause 4.2.7.2 of TS 37.355 [34],

is UE capability for number of DL PRS resources that it can process in a slot corresponding to *maxNumOfDL-PRS-ResProcessedPerSlot* as specified in clause 6.4.3 of TS 37.355 [34],

is the number of UE Rx-Tx time difference measurement samples and = 4,

is the measurement duration for the last UE Rx-Tx time difference measurement sample in the positioning layer i, including the sampling time and processing time,  *= +*  ,

is periodicity of UE Rx-Tx time difference measurement in positioning frequency layer *i*:

where

corresponds to durationOfPRS-ProcessingSymbolsInEveryTms in TS 37.355 [34],

, the least common multiple between and

is the measurement gap repetition periodicity in positioning frequency layer i.

is the PRS resource periodicity in positioning frequency layer *i*. If the positioning frequency layer *i* has more than one DL PRS resource sets with different PRS periodicities with muting, , the least common multiple of among DL PRS resource sets is used to derive the measurement period of that positioning frequency layer.

is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

is the scaling factor considering PRS resource muting. If bitmap for higher-layer parameter *DL-PRS-MutingPattern* is provided, and , then ; otherwise, if bitmap is not provided or , then . is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and L is the size of the bitmap .

Note: For the purpose of calculating TPRS,i, only the PRS resources fully or partially covered by the MG are considered.

The time starts from the first MG instance aligned with DL PRS resources in the assistance data after both the *NR-Multi-RTT-RequestLocationInformation* message and *NR-Multi-RTT-ProvideAssistanceData* message from LMF via LPP [34] are delivered to the physical layer of UE.

Note: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

The UE Rx-Tx time difference measurement period is restarted if HO occurs during the measurement period and after SRS reconfiguration on the target cell is complete.

The measurement requirements do not apply for a PRS resource:

- if the PRS resource is across two sampling duration of N within duration or

- if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

If during the measurement period of one or more positioning frequency layers, the MG pattern is reconfigured either per UE request or not per UE request, the measurement period can be longer.

The requirements in this section apply, provided no PRS symbols are dropped during the measurement period TUERxTx,Total within measurement gaps due to collisions with other signals; otherwise, a longer measurement period may be used.

When PRS-RSRP is configured for multi-RTT, the UE Rx-Tx time difference measurements and PRS-RSRP measurements are performed over the same measurement period.

When PSCell or SCell addition or release does not cause SRS reconfiguration during the measurement period, UE continues the UE Rx-Tx time difference measurement, and the measurement period requirements apply.

When PSCell or SCell addition or release causes SRS reconfiguration during the measurement period, UE shall restart the UE Rx-Tx time difference measurement after the SRS reconfiguration on the target cell is complete.

*Editor’s note:* FFS when SRS is reconfigured without cell change during the measurement period, UE shall restart the UE Rx-Tx time difference measurement after the SRS reconfiguration on the target cell is complete.

If UE uplink transmission timing changes due to the network-configured Timing Advance command during the UE Rx-Tx measurement period, then the UE Rx-Tx time difference measurement period is restarted after uplink transmission timing changes, and the UE Rx-Tx time difference measurement period requirements in this clause shall not apply.

If UE uplink transmission timing changes due to the change in the NTA\_offset defined in Table 7.1.2-2 during the UE Rx-Tx measurement period, then the UE Rx-Tx time difference measurement period is restarted after uplink transmission timing changes, and the UE Rx-Tx time difference measurement period requirements in this clause shall not apply.

*<End of change5>*

*<Start of change6>*

#### 10.1.23.2 Measurement Accuracy Requirements

The RSTD measurement reported by the UE shall fulfil the accuracy requirements defined in Table 10.1.23.2-1 for AWGN channel and Table 10.1.23.2-3 for fading channel for FR1, provided that the following conditions are met.

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for RSTD measurements are fulfilled according to Annex B.2.14 for a corresponding Band for each relevant PRS resource configured for measurement.

The RSTD measurement reported by the UE shall fulfil the accuracy requirements defined in Table 10.1.23.2-2 for AWGN channel and Table 10.1.23.2-4 for fading channel for FR2, provided that the following conditions are met.

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for RSTD measurements are fulfilled according to Annex B.2.14 for a corresponding Band for each relevant PRS resource configured for measurement.

Note: The requriements for fading channel in this clause are derived based on TDL-A (30 ns delay spread, 5Hz) and TDL-C (60 ns delay spread, 300 Hz) channel models for FR1 and FR2 respectively.

When UE measures RSTD on PRS resources belonging to different PFLs, then the RSTD accuracy is defined as the accuracy corresponding to the largest accuracy value among different PFLs.

The requirements in this clause apply provided that the time offset between the two PRS resource instances from the reference cell and the neighbor cell, which are used for a single RSTD estimate, is no greater than TBD ms.

[*Editor notes: The margins for measurements on different PFLs shall be considered in the group delay margin]*

Table 10.1.23.2-1: RSTD absolute accuracy in FR1 for AWGN channel

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | Conditions | | | | | | |
| PRS Ês/Iot | PRS SCS | PRS bandwidth  Note 1 | PRS resource repetition ()  Note 2 | Io Note 3 range | | |
| NR operating band groups Note 4 | Minimum Io | Maximum Io |
| Tc Note 5 | dB | kHz | RB |  |  | dBm/SCS | dBm/BWChannel |
| [132] +ΔNote 7 | (PRS Ês/Iot)ref ≥-6dB  (PRS Ês/Iot)*i* ≥-13dB | 15 | ≥ [24] | ≥ [4] | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,  NR\_SDL\_FR1\_A | -121 | -50 |
| NR\_FDD\_FR1\_B | -120.5 | -50 |
| NR\_TDD\_FR1\_C | -120 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -50 |
| NR\_FDD\_FR1\_F | -118.5 | -50 |
| NR\_FDD\_FR1\_G | -118 | -50 |
| NR\_FDD\_FR1\_H | -117.5 | -50 |
| [98] +Δ | ≥ [52] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [42] +Δ | ≥ [104] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [75] +Δ | 30 | ≥ [24] | ≥ [4] | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,  NR\_SDL\_FR1\_A | -118 | -50 |
| NR\_FDD\_FR1\_B | -117.5 | -50 |
| NR\_TDD\_FR1\_C | -117 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -116.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -116 | -50 |
| NR\_FDD\_FR1\_F | -115.5 | -50 |
| NR\_FDD\_FR1\_G | -115 | -50 |
| NR\_FDD\_FR1\_H | -114.5 | -50 |
| [48] +Δ | ≥ [48] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [24] +Δ | ≥ [132] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [50] +Δ | 60 | ≥ [24] | ≥ [4] | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,  NR\_SDL\_FR1\_A | -115 | -50 |
| NR\_FDD\_FR1\_B | -114.5 | -50 |
| NR\_TDD\_FR1\_C | -114 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -113.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -113 | -50 |
| NR\_FDD\_FR1\_F | -113.5 | -50 |
| NR\_FDD\_FR1\_G | -113 | -50 |
| NR\_FDD\_FR1\_H | -111.5 | -50 |
| [24] +Δ | ≥ [64] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [10] +Δ | ≥ [132] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| NOTE 1: Minimum PRS bandwidth, which is minimum of the PRS bandwidths of the reference resource and the measured neighbour resource i.  NOTE 2: Minimum number of PRS resource repetitions among the reference resource and the measured neighbour resource i. are configured by higher layer parameter *dl-PRS-ResourceRepetitionFactor, dl-PRS-NumSymbols and dl-PRS-CombSizeN*defined in TS 37.355 [34], respectively.  NOTE 3: Io is assumed to have constant EPRE across the bandwidth.  NOTE 4: NR operating band groups in FR1 are as defined in clause 3.5.2.  NOTE 5: Tc is the basic timing unit defined in TS 38.211 [6].  NOTE 6: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth of the smallest RB number for the corresponding SCS.  NOTE 7: Δ=TBD. | | | | | | | |

Table 10.1.23.2-2: RSTD absolute accuracy in FR2 for AWGN channel

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Accuracy | Conditions | | | | | |
| PRS Ês/Iot | PRS SCS | PRS bandwidth  Note 1 | PRS resource repetition  () Note 2 | Io Note 3 range | |
| Minimum Io | Maximum Io |
| Tc Note 4 | dB | kHz | RB |  | dBm/SCS | dBm/BWChannel |
| [35] +ΔNote 6 | (PRS Ês/Iot)ref ≥-6dB  (PRS Ês/Iot)*i* ≥-13dB | 60 | ≥ [24] | ≥ [1] | Same value as PRS\_RP in Table B.2.z-2, according to UE Power class, operating band and angle of arrival | -50 |
| [24] +Δ | ≥ [64] | ≥ [1] | Note 5 | Note 5 |
| [11] +Δ | ≥ [132] | ≥ [1] | Note 5 | Note 5 |
| [24] +Δ | 120 | ≥ [32] | ≥ [1] | Same value as PRS\_RP in Table B.2.z-2, according to UE Power class, operating band and angle of arrival | -50 |
| [13] +Δ | ≥ [64] | ≥ [1] | Note 5 | Note 5 |
| [6] +Δ | ≥ [128] | ≥ [1] | Note 5 | Note 5 |
| NOTE 1: Minimum PRS bandwidth, which is minimum of the PRS bandwidths of the reference resource and the measured neighbour resource i.  NOTE 2: Minimum number of PRS resource repetitions among the reference resource and the measured neighbour resource i. are configured by higher layer parameter *dl-PRS-ResourceRepetitionFactor, dl-PRS-NumSymbols and dl-PRS-CombSizeN*defined in TS 37.355 [34], respectively.  NOTE 3: Io is assumed to have constant EPRE across the bandwidth.  NOTE 4: Tc is the basic timing unit defined in TS 38.211 [6].  NOTE 5: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth of the smallest RB number for the corresponding SCS.  NOTE 6: Δ=TBD. | | | | | | |

Table 10.1.23.2-3: RSTD absolute accuracy in FR1 for fading channel

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | Conditions | | | | | | |
| PRS Ês/Iot | PRS SCS | PRS bandwidth  Note 1 | PRS resource repetition ()  Note 2 | Io Note 3 range | | |
| NR operating band groups Note 4 | Minimum Io | Maximum Io |
| Tc Note 5 | dB | kHz | RB |  |  | dBm/SCS | dBm/BWChannel |
| [247] +ΔNote 7 | (PRS Ês/Iot)ref ≥-6dB  (PRS Ês/Iot)*i* ≥-13dB | 15 | ≥ [24] | ≥ [4] | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,  NR\_SDL\_FR1\_A | -121 | -50 |
| NR\_FDD\_FR1\_B | -120.5 | -50 |
| NR\_TDD\_FR1\_C | -120 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -50 |
| NR\_FDD\_FR1\_F | -118.5 | -50 |
| NR\_FDD\_FR1\_G | -118 | -50 |
| NR\_FDD\_FR1\_H | -117.5 | -50 |
| [140] +Δ | ≥ [52] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [86] +Δ | ≥ [104] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [118] +Δ | 30 | ≥ [24] | ≥ [4] | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,  NR\_SDL\_FR1\_A | -118 | -50 |
| NR\_FDD\_FR1\_B | -117.5 | -50 |
| NR\_TDD\_FR1\_C | -117 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -116.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -116 | -50 |
| NR\_FDD\_FR1\_F | -115.5 | -50 |
| NR\_FDD\_FR1\_G | -115 | -50 |
| NR\_FDD\_FR1\_H | -114.5 | -50 |
| [109] +Δ | ≥ [48] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [28] +Δ | ≥ [132] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [147] +Δ | 60 | ≥ [24] | ≥ [4] | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,  NR\_SDL\_FR1\_A | -115 | -50 |
| NR\_FDD\_FR1\_B | -114.5 | -50 |
| NR\_TDD\_FR1\_C | -114 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -113.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -113 | -50 |
| NR\_FDD\_FR1\_F | -113.5 | -50 |
| NR\_FDD\_FR1\_G | -113 | -50 |
| NR\_FDD\_FR1\_H | -111.5 | -50 |
| [27] +Δ | ≥ [64] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| [21] +Δ | ≥ [132] | ≥ [1] | Note 6 | Note 6 | Note 6 |
| NOTE 1: Minimum PRS bandwidth, which is minimum of the PRS bandwidths of the reference resource and the measured neighbour resource i.  NOTE 2: Minimum number of PRS resource repetitions among the reference resource and the measured neighbour resource i. are configured by higher layer parameter *dl-PRS-ResourceRepetitionFactor, dl-PRS-NumSymbols and dl-PRS-CombSizeN*defined in TS 37.355 [34], respectively.  NOTE 3: Io is assumed to have constant EPRE across the bandwidth.  NOTE 4: NR operating band groups in FR1 are as defined in clause 3.5.2.  NOTE 5: Tc is the basic timing unit defined in TS 38.211 [6].  NOTE 6: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth of the smallest RB number for the corresponding SCS.  NOTE 7: Δ=TBD. | | | | | | | |

Table 10.1.23.2-4: RSTD absolute accuracy in FR2 for fading channel

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Accuracy | Conditions | | | | | |
| PRS Ês/Iot | PRS SCS | PRS bandwidth  Note 1 | PRS resource repetition  () Note 2 | Io Note 3 range | |
| Minimum Io | Maximum Io |
| Tc Note 4 | dB | kHz | RB |  | dBm/SCS | dBm/BWChannel |
| [83] +ΔNote 6 | (PRS Ês/Iot)ref ≥-6dB  (PRS Ês/Iot)*i* ≥-13dB | 60 | ≥ [24] | ≥ [4] | Same value as PRS\_RP in Table B.2.z-2, according to UE Power class, operating band and angle of arrival | -50 |
| [64] +Δ | ≥ [64] | ≥ [1] | Note 5 | Note 5 |
| [46] +Δ | ≥ [132] | ≥ [1] | Note 5 | Note 5 |
| [48] +Δ | 120 | ≥ [32] | ≥ [4] | Same value as PRS\_RP in Table B.2.z-2, according to UE Power class, operating band and angle of arrival | -50 |
| [54] +Δ | ≥ [64] | ≥ [1] | Note 5 | Note 5 |
| [36] +Δ | ≥ [128] | ≥ [1] | Note 5 | Note 5 |
| NOTE 1: Minimum PRS bandwidth, which is minimum of the PRS bandwidths of the reference resource and the measured neighbour resource i.  NOTE 2: Minimum number of PRS resource repetitions among the reference resource and the measured neighbour resource i. are configured by higher layer parameter *dl-PRS-ResourceRepetitionFactor, dl-PRS-NumSymbols and dl-PRS-CombSizeN*defined in TS 37.355 [34], respectively.  NOTE 3: Io is assumed to have constant EPRE across the bandwidth.  NOTE 4: Tc is the basic timing unit defined in TS 38.211 [6].  NOTE 5: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth of the smallest RB number for the corresponding SCS.  NOTE 6: Δ=TBD. | | | | | | |

*<End of change6>*

*<Start of change7>*

### 10.1.24 PRS-RSRP Measurements

#### 10.1.24.1 Introduction

The requirements in Clause 10.1.24 shall apply, provided the UE has received *nr-DL-TDOA-RequestLocationInformation* or *nr-Multi-RTT-RequestLocationInformation* or *nr-DL-AoD-RequestLocationInformation* message from LMF via LPP [34] requesting the UE to report one or more DL PRS-RSRP measurements defined in TS 38.215 [4].

#### 10.1.24.2 Measurement Accuracy Requirements

##### 10.1.24.2.1 Absolute PRS RSRP accuracy

The absolute accuracy requirements for PRS-RSRP measurement for FR1 defined in Table 10.1.24.2.1-1 are valid under the following conditions:

Conditions defined in 38.101-1 Clause 7.3 for reference sensitivity are fulfilled.

PRP 1,2|dBm according to Annex B.2.14 for a corresponding Band

The absolute accuracy requirements for PRS-RSRP measurement for FR2 defined in Table 10.1.24.2.1-2 are valid under the following conditions:

Conditions defined in 38.101-2 Clause 7.3 for reference sensitivity are fulfilled.

PRP 1,2|dBm according to Annex B.2.14 for a corresponding Band

Table 10.1.24.2.1-1: PRS-RSRP absolute accuracy for FR1

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | | | |
| Normal condition | Extreme condition | PRS Ês/Iot | PRS BW | **Repetition factor**  ( | Io Note 7 range | | | | |
| NR operating band groups Note 8 | **Minimum Io Note 1**  dBm / SCSPRS | | | Maximum Io |
| dB | dB | dB | PRB | - |  | dBm / SCSPRS | | | dBm/BWChannel |
| **dBm/15kHz** Note 6 | **dBm/30kHz** Note 6 | **dBm/60kHz** Note 6 |
| ±3.5 | [TBD] | ≥-3dB | ≥24 | All | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A | -127 | -124 | -121 | -50 |
| NR\_FDD\_FR1\_B | -126.5 | -123.5 | -120.5 | -50 |
| NR\_TDD\_FR1\_C | -126 | -123 | -120 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -125.5 | -122.5 | -119.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -125 | -122 | -119 | -50 |
| NR\_FDD\_FR1\_F | -124.5 | -121.5 | -118.5 | -50 |
| NR\_FDD\_FR1\_G | -124 | -121 | -118 | -50 |
| NR\_FDD\_FR1\_H | -123.5 | -120.5 | -117.5 | -50 |
| Note 4 | | | | |
| Note 4 | | | | |
| ±8.5 | [TBD] | ≥-13dB | 24 ≤ BW ≤ 52 | All | Note 4 | | | | |
| ±6 |  | 52< BW≤ 104 | All | Note 4 | | | | |
| ±4.5 |  | BW >104 | All | Note 4 | | | | |
| NOTE 1: This minimum Io condition is expressed as the average Io per RE over all REs in an OFDM symbol.  NOTE 2: Void.  NOTE 3: PRS bandwidth is as indicated in *prs-Bandwidth* in the OTDOA or DL-AoD assistance data defined in [34].  NOTE 4: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth ≥ [24] RB.  NOTE 5: The serving cell, the reference cell, and the measured neighbour cell i are on the same carrier frequency.  NOTE 6: The condition level is increased by ∆>0, when applicable, as described in Sections B.3.2 and B.3.3.  NOTE 7: The Io is defined in PRS positioning subframes. The same Io range applies to PRS and non-PRS symbols. Io levels are different in PRS and non-PRS symbols within the same subframe.  NOTE 8: NR operating band groups are as defined in Section 3.5.2. | | | | | | | | | |

Table 10.1.24.2.1-2: PRS-RSRP absolute accuracy for FR2

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | |
| Normal condition | Extreme condition | PRS Ês/Iot | PRS BW | **Repetition factor**  ( | Io Note 7 range | | |
| Minimum Io Note 1  dBm / SCSPRS | | Maximum Io |
| dB | dB | dB | PRB | - | dBm / SCSPRS | | dBm/BWChannel |
| **dBm/120kHz** Note 6 | **dBm/60kHz** Note 6 |
| ±5 | [TBD] | ≥-3dB | ≥24 | All | Same value as PRP in Table B.2.14 -2, according to UE Power class, operating band and angle of arrival | | -50 |
| Note 4 | | |
| Note 4 | | |
| ±8.5 | [TBD] | ≥-13dB | 24 ≤ BW ≤ 64 | All | Note 4 | | |
| ±6 |  | BW >64 | All | Note 4 | | |
| NOTE 1: This minimum Io condition is expressed as the average Io per RE over all REs in an OFDM symbol.  NOTE 2: Void.  NOTE 3: PRS bandwidth is as indicated in *prs-Bandwidth* in the OTDOA or DL-AoD assistance data defined in [34].  NOTE 4: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth ≥ [24] RB.  NOTE 5: The serving cell, the reference cell, and the measured neighbour cell i are on the same carrier frequency.  NOTE 6: The condition level is increased by ∆>0, when applicable, as described in Sections B.3.2 and B.3.3.  NOTE 7: The Io is defined in PRS positioning subframes. The same Io range applies to PRS and non-PRS symbols. Io levels are different in PRS and non-PRS symbols within the same subframe.  NOTE 8: NR operating band groups are as defined in Section 3.5.2. | | | | | | | |

10.1.24.2.2 Relative PRS RSRP accuracy

The relative accuracy of PRS-RSRP is defined as accuracy of the difference between two PRS-RSRP measurements.

The relative PRS-RSRP accuracy requirements apply for the cases when PRS-RSRP is measured from PRS resources in the same PRS resource set in FR1 or FR2, and measured with same Rx beam in case of FR2.

The accuracy requirements for PRS-RSRP measurement for FR1 defined in Table 10.1.24.2.2-1 are valid under the following conditions:

Conditions defined in 38.101-1 Clause 7.3 for reference sensitivity are fulfilled.

PRP 1,2|dBm according to Annex B.2.14 for a corresponding Band

The accuracy requirements for PRS-RSRP measurement for FR2 defined in Table 10.1.24.2.2-2 are valid under the following conditions:

Conditions defined in 38.101-2 Clause 7.3 for reference sensitivity are fulfilled.

PRP 1,2|dBm according to Annex B.2.14 for a corresponding Band

Table 10.1.24.2.2-1: PRS-RSRP relative accuracy for FR1

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | | | |
| Normal condition | Extreme condition | PRS Ês/Iot | PRS BW | **Repetition factor**  ( | Io Note 7 range | | | | |
| NR operating band groups Note 8 | Minimum Io Note 1  dBm / SCSPRS | | | Maximum Io |
| dB | dB | dB | PRB | - |  | dBm / SCSPRS | | | dBm/BWChannel |
| **dBm/15kHz** Note 6 | **dBm/30kHz** Note 6 | **dBm/60kHz** Note 6 |
| ±3.5 | [TBD] | ≥-3dB | ≥24 | All | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A | -127 | -124 | -121 | -50 |
| NR\_FDD\_FR1\_B | -126.5 | -123.5 | -120.5 | -50 |
| NR\_TDD\_FR1\_C | -126 | -123 | -120 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -125.5 | -122.5 | -119.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -125 | -122 | -119 | -50 |
| NR\_FDD\_FR1\_F | -124.5 | -121.5 | -118.5 | -50 |
| NR\_FDD\_FR1\_G | -124 | -121 | -118 | -50 |
| NR\_FDD\_FR1\_H | -123.5 | -120.5 | -117.5 | -50 |
| Note 4 | | | | |
| Note 4 | | | | |
| ±9.5 | [TBD] | ≥-13dB | 24 ≤ BW ≤ 52 | All | Note 4 | | | | |
| ±6.5 |  | 52< BW≤ 104 | All | Note 4 | | | | |
| ±5.0 |  | BW >104 | All | Note 4 | | | | |
| NOTE 1: This minimum Io condition is expressed as the average Io per RE over all REs in an OFDM symbol.  NOTE 2: Void.  NOTE 3: PRS bandwidth is as indicated in *prs-Bandwidth* in the OTDOA or DL-AoD assistance data defined in [34].  NOTE 4: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth ≥ [24] RB.  NOTE 5: The serving cell, the reference cell, and the measured neighbour cell i are on the same carrier frequency.  NOTE 6: The condition level is increased by ∆>0, when applicable, as described in Sections B.3.2 and B.3.3.  NOTE 7: The Io is defined in PRS positioning subframes. The same Io range applies to PRS and non-PRS symbols. Io levels are different in PRS and non-PRS symbols within the same subframe.  NOTE 8: NR operating band groups are as defined in Section 3.5.2. | | | | | | | | | |

Table 10.1.24.2.2-2: PRS-RSRP relative accuracy for FR2

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | |
| Normal condition | Extreme condition | PRS Ês/Iot | PRS BW | **Repetition factor**  ( | Io Note 7 range | | |
| Minimum Io Note 1  dBm / SCSPRS | | Maximum Io |
| dB | dB | dB | PRB | - | dBm / SCSPRS | | dBm/BWChannel |
| **dBm/120kHz** Note 6 | **dBm/60kHz** Note 6 |
| ±5.0 | [TBD] | ≥-3dB | ≥[24] | All | Same value as PRP in Table B.2.14-2, according to UE Power class, operating band and angle of arrival | | -50 |
| Note 4 | | |
| Note 4 | | |
| ±10 | [TBD] | ≥-13dB | 24 ≤ BW ≤ 64 | All | Note 4 | | |
| ±7.5 |  | BW >64 | All | Note 4 | | |
| NOTE 1: This minimum Io condition is expressed as the average Io per RE over all REs in an OFDM symbol.  NOTE 2: Void.  NOTE 3: PRS bandwidth is as indicated in *prs-Bandwidth* in the OTDOA or DL-AoD assistance data defined in [34].  NOTE 4: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth ≥ [24] RB.  NOTE 5: The serving cell, the reference cell, and the measured neighbour cell i are on the same carrier frequency.  NOTE 6: The condition level is increased by ∆>0, when applicable, as described in Sections B.3.2 and B.3.3.  NOTE 7: The Io is defined in PRS positioning subframes. The same Io range applies to PRS and non-PRS symbols. Io levels are different in PRS and non-PRS symbols within the same subframe.  NOTE 8: NR operating band groups are as defined in Section 3.5.2. | | | | | | | |

*<End of change7>*

*<Start of change8>*

### A.6.6.12 RSTD measurements

#### A. 6.6.12.1 NR RSTD measurement reporting delay test case for single positioning frequency layer in FR1 SA

##### A. 6.6.12.1.1 Test Purpose and Environment

The purpose of the test is to verify that the RSTD measurement meets the requirements specified in Clause 9.9.2 in an environment with AWGN propagation conditions in FR1 in standalone scenario when single positioning frequency layer is configured.

The supported test configurations are specified in Table A.6.6.12.1.1-1.

Table A.6.6.12.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. | |

In the test there are three synchronous cells: Cell 1, Cell 2 and Cell 3. Cell 1 is the reference as well as the PCell. Cell 2 and Cell 3 are the neighbour cells. All 3 cells are on the same RF channel in FR1.

The test consists of two consecutive time intervals, with duration of T1 and T2. During time duration T1, the UE shall not have any timing information of Cell 2 and Cell 3. All three cells transmit PRS during T2.

Note: The information on when PRS is muted is conveyed to the UE using PRS muting information.

The *NR-DL-TDOA-ProvideAssistanceData* and *nr-DL-TDOA-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE during T1. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the *DL-TDOA assistance* data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources.

The UE is configured with measurement gap pattern ID # 24 or #0 before T2.

The general test parameters are listed in Table A.6.6.12.1.1-2, and cell specific test parameters are listed in Table A.6.6.12.1.1-3.

Table A.6.6.12.1.1-2: General test parameters for RSTD measurement reporting delay

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | Unit | Value | Comment |
| Reference cell | |  | Cell 1 | Reference cell is the cell in the DL-TDOA assistance data with respect to which the RSTD measurement is defined, as specified in TS 38.215 [4] and TS 37.355[34]. The reference cell is the PCell in this test case. |
| Neighbor cells | |  | Cell 2 and Cell 3 | Cell 2 and Cell 3 appear at the first and second places in the neighbour cell list in the DL-TDOA assistance data. |
| SSB configuration | Config 1 |  | SSB.1 FR1 |  |
| Config 2 |  | SSB.1 FR1 |
| Config 3 |  | SSB.2 FR1 |
| SMTC configuration | Config 1 |  | SMTC.2 |  |
| Config 2 |  | SMTC.1 |
| Config 3 |  | SMTC.1 |
| PDSCH RMC configuration | Config 1 |  | SR.1.1 FDD |  |
| Config 2 |  | SR.1.1 TDD |  |
| Config 3 |  | SR.2.1 TDD |  |
| RMSI CORESET RMC configuration | Config 1 |  | CR.1.1 FDD | As specified in clause A.3.1.2.1 |
| Config 2 |  | CR.1.1 TDD |  |
| Config 3 |  | CR.2.1 TDD |  |
| Dedicated CORESET RMC configuration | Config 1 |  | CR.1.1 FDD |  |
| Config 2 |  | CR.1.1 TDD |  |
| Config 3 |  | CR.2.1 TDD |  |
| Initial BWP configuration | Config 1,2,3 |  | DLBWP.0.1  ULBWP.0.1 |  |
| Active DL BWP configuration | Config 1,2,3 |  | DLBWP.1.1 |  |
| Active UL BWP configuration | Config 1,2,3 |  | ULBWP.1.1 |  |
| PRS Configuration | Config 1 |  | PRS.1.1 FR1 | As specified in clause A.3.31 |
| Config 2 |  | PRS.1.2 FR1 |
| Config 3 |  | PRS.2.1 FR1 |
| Physical cell ID PCI | |  | (PCI of Cell 1 – PCI of Cell 2)mod6=0  and  (PCI of Cell 1 – PCI of Cell 3)mod6=0 | The cell PCIs are selected such that the relative shifts of PRS patterns among cells are as given by the test parameters |
| CP length | |  | Normal |  |
| DRX | |  | OFF |  |
| Measurement gap | |  | GP#24 or GP#0 | GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured |
| Radio frame receive time offset between the cells at the UE antenna connector | | μs | Cell 2 to Cell 1: 0  Cell 3 to Cell 1: 3 | PRS are transmitted from synchronous cells |
| Expected RSTD | | μs | Cell 2: 3  Cell 3: 3  Other neighbour cells: randomly between -3 and 3 | The expected RSTD is what is expected at the receiver. The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355[34] is the expectedRSTD indicator |
| Expected RSTD uncertainty for all neighbour cells | | μs | 5 | The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355[34] is the expectedRSTD-Uncertainty index |
| Number of cells provided in DL-TDOA assistance data | |  | 16 | Including the reference cell |
| PRS muting info | |  | Cell 1: ‘10’  Cell 2: ‘01’  Cell 3: ‘10’ | Correponds to prs-MutingInfo defined in TS 37.355 [34] |
| PRS resource RE offset | |  | Cell 1: 0  Cell 2: 0  Cell 3: 1 | Cell 1 and Cell 3 are configured with different resource offsets |
| T1 | | s | 3 | The length of the time interval from the beginning of each test |
| T2 | | s | [1.28] | The length of the time interval that follows immediately after time interval T1 |

Table A.6.6.12.1.1-3: Cell-specific test parameters for RSTD measurement reporting delay during T1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | | Unit | Cell 1 | Cell 2 | Cell 3 |
| NR RF Channel Number | |  | 1 | 1 | 1 |
| Positiong frequency layer | |  | 1 | 1 | 1 |
| Correlation Matrix and Antenna Configuration | |  | 1x2 Low | 1x2 Low | 1x2 Low |
| OCNG patterns defined in A.3.2.1 | |  | OP.1 | N/A | N/A |
| Note 3 | Config 1 | dBm/SCS | -98 | | |
| Config 2 | dBm/SCS | -98 | | |
| Config 3 | dBm/SCS | -95 | | |
| PRS | | dB | -Infinity | -Infinity | -Infinity |
| SSB | | dB | 10 | -Infinity | -Infinity |
| Io Note 4 | Config 1 | dBm/  9.36MHz | -68.63 | -70.05 | -70.05 |
| Config 2 | dBm/  9.36MHz | -68.63 | -70.05 | -70.05 |
| Config 3 | dBm/  38.16MHz | -63.20 | -63.96 | -63.96 |
| SSB RP Note4 | Config 1 | dBm/SCS | -88 | -Infinity | -Infinity |
| Config 2 | dBm/SCS | -88 | -Infinity | -Infinity |
| Config 3 | dBm/SCS | -88 | -Infinity | -Infinity |
| Propagation Condition | |  | AWGN | | |
| Note 1: OCNG shall be used such that active cell (Cell 1) is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.  Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 4: SSB RP and Io levels have been derived from other parameters and are given for information purpose. These are not settable test parameters. | | | | | |

**Table A.6.6.12.1.1-4: Cell-specific test parameters for RSTD measurement reporting delay during T2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Cell 1** | **Cell 2** | **Cell 3** |
| **T2** | **T2** | **T2** |
| NR RF Channel Number | |  | 1 | 1 | 1 |
| Correlation Matrix and Antenna Configuration | |  | 1x2 Low | 1x2 Low | 1x2 Low |
| OCNG patterns defined in A.3.2.1 | |  | OP.1 | OP.1 | OP.1 |
| PRACH configuration | |  | FR1 PRACH configuration 1 | FR1 PRACH configuration 1 | FR1 PRACH configuration 1 |
| Note 3 | Config 1 | dBm/SCS | -98 | -98 | -98 |
| Config 2 | dBm/SCS | -98 | -98 | -98 |
| Config 3 | dBm/SCS | -95 | -95 | -95 |
| PRS | Config 1 | dB | -5.45 | -11.67 | -11.67 |
| Config 2 | dB | -5.45 | -11.67 | -11.67 |
| Config 3 | dB | -5.45 | -11.67 | -11.67 |
| Io Note 4 | Config 1 | dBm/  9.36MHz | -69.59 | -69.93 | -69.93 |
| Config 2 | dBm/  96.48MHz | -69.59 | -69.93 | -69.93 |
| Config 3 | dBm/  38.16MHz | -63.72 | -63.89 | -63.89 |
| PRS | | dB | -6 | 13 | -13 |
| Propagation Condition | |  | AWGN | | |
| Note 1: OCNG shall be used such that active cells (all, except Cell 3 in T3) are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols other than those in the subframes with transmitted PRS.  Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled. | | | | | |

##### A.6.6.12.1.2 Test Requirements

The RSTD measurement time fulfils the requirements specified in Clause 9.9.2.5.

The UE shall perform and report the RSTD measurements for Cell 2 and Cell 3 with respect to the reference cell in the DL-TDOA assistance data, Cell 1, within the time duration specified in section 9.9.1.5 starting from the beginning of time interval T2.

The rate of the correct events for each neighbour cell observed during repeated tests shall be at least 90%, where the reported RSTD measurement for each correct event shall be within the RSTD reporting range specified in Clause 10.1.23.3, i.e., between RSTD\_0000000 and RSTD1970049

#### A. 6.6.12.2 NR RSTD measurement reporting delay test case for dual positioning frequency layers in FR1 SA

##### A. 6.6.12.2.1 Test Purpose and Environment

The purpose of the test is to verify that the RSTD measurement meets the requirements specified in Clause 9.9.2 in an environment with AWGN propagation conditions in FR1 in standalone scenario when dual positioning frequency layers are configured.

The supported test configurations are specified in Table A.6.6.12.2.1-1.

Table A.6.6.12.2.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. | |

In the test there are three synchronous cells: Cell 1, Cell 2 and Cell 3. Cell 1 is the reference as well as the PCell. Cell 2 and Cell 3 are the neighbour cells. Cell 3 is on a different RF channel with Cell 1 and Cell 2.

The test consists of two consecutive time intervals, with duration of T1 and T2. During time duration T1, the UE shall not have any timing information of Cell 2 and Cell 3. All three cells transmit PRS during T2.

Note: The information on when PRS is muted is conveyed to the UE using PRS muting information.

The *NR-DL-TDOA-ProvideAssistanceData* and *nr-DL-TDOA-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE during T1. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the *DL-TDOA assistance* data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources.

The UE is configured with measurement gap pattern ID # 24 or #0 before T2.

The general test parameters are listed in Table A.6.6.12.2.1-2, and cell specific test parameters are listed in Table A.6.6.12.2.1-3.

Table A.6.6.12.2.1-2: General test parameters for RSTD measurement reporting delay

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | Unit | Value | Comment |
| Reference cell | |  | Cell 1 | Reference cell is the cell in the DL-TDOA assistance data with respect to which the RSTD measurement is defined, as specified in TS 38.215 [4] and TS 37.355[34]. The reference cell is the PCell in this test case. |
| Neighbor cells | |  | Cell 2 and Cell 3 | Cell 2 and Cell 3 appear at the first and second places in the neighbour cell list in the DL-TDOA assistance data. |
| SSB configuration | Config 1 |  | SSB.1 FR1 |  |
| Config 2 |  | SSB.1 FR1 |
| Config 3 |  | SSB.2 FR1 |
| SMTC configuration | Config 1 |  | SMTC.2 |  |
| Config 2 |  | SMTC.1 |
| Config 3 |  | SMTC.1 |
| PDSCH RMC configuration | Config 1 |  | SR.1.1 FDD |  |
| Config 2 |  | SR.1.1 TDD |  |
| Config 3 |  | SR.2.1 TDD |  |
| RMSI CORESET RMC configuration | Config 1 |  | CR.1.1 FDD | As specified in clause A.3.1.2.1 |
| Config 2 |  | CR.1.1 TDD |  |
| Config 3 |  | CR.2.1 TDD |  |
| Dedicated CORESET RMC configuration | Config 1 |  | CR.1.1 FDD |  |
| Config 2 |  | CR.1.1 TDD |  |
| Config 3 |  | CR.2.1 TDD |  |
| Initial BWP configuration | Config 1,2,3 |  | DLBWP.0.1  ULBWP.0.1 |  |
| Active DL BWP configuration | Config 1,2,3 |  | DLBWP.1.1 |  |
| Active UL BWP configuration | Config 1,2,3 |  | ULBWP.1.1 |  |
| PRS Configuration | Config 1 |  | PRS.1.1 FR1 | As specified in clause A.3.xx |
| Config 2 |  | PRS.1.2 FR1 |
| Config 3 |  | PRS.2.1 FR1 |
| Physical cell ID PCI | |  | (PCI of Cell 1 – PCI of Cell 2)mod6=0  and  (PCI of Cell 1 – PCI of Cell 3)mod6=0 | The cell PCIs are selected such that the relative shifts of PRS patterns among cells are as given by the test parameters |
| CP length | |  | Normal |  |
| DRX | |  | OFF |  |
| Measurement gap | |  | GP#24 or GP#0 | GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured |
| Radio frame receive time offset between the cells at the UE antenna connector | | μs | Cell 2 to Cell 1: 0  Cell 3 to Cell 1: 3 | PRS are transmitted from synchronous cells |
| Expected RSTD | | μs | Cell 2: 3  Cell 3: 3  Other neighbour cells: randomly between -3 and 3 | The expected RSTD is what is expected at the receiver. The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355[34] is the expectedRSTD indicator |
| Expected RSTD uncertainty for all neighbour cells | | μs | 500 | The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355[34] is the expectedRSTD-Uncertainty index |
| Number of cells provided in DL-TDOA assistance data | |  | 16 | Including the reference cell |
| PRS muting info | |  | Cell 1: ‘10’  Cell 2: ‘01’  Cell 3: ‘10’ | Correponds to prs-MutingInfo defined in TS 37.355 [34] |
| PRS resource RE offset | |  | Cell 1: 0  Cell 2: 0  Cell 3: 1 | Cell 1 and Cell 3 are configured with different resource offsets |
| T1 | | s | 3 | The length of the time interval from the beginning of each test |
| T2 | | s | [1.28] | The length of the time interval that follows immediately after time interval T1 |

Table A.6.6.12.2.1-3: Cell-specific test parameters for RSTD measurement reporting delay during T1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | | Unit | Cell 1 | Cell 2 | Cell 3 |
| NR RF Channel Number | |  | 1 | 1 | 2 |
| Positiong frequency layer | |  | 1 | 1 | 2 |
| Correlation Matrix and Antenna Configuration | |  | 1x2 Low | 1x2 Low | 1x2 Low |
| OCNG patterns defined in A.3.2.1 | |  | OP.1 | N/A | N/A |
| Note 3 | Config 1 | dBm/SCS | -98 | | |
| Config 2 | dBm/SCS | -98 | | |
| Config 3 | dBm/SCS | -95 | | |
| PRS | | dB | -Infinity | -Infinity | -Infinity |
| Io Note 4 | Config 1 | dBm/  9.36MHz | -68.63 | -70.05 | -70.05 |
| Config 2 | dBm/  9.36MHz | -68.63 | -70.05 | -70.05 |
| Config 3 | dBm/  38.16MHz | -63.20 | -63.96 | -63.96 |
| SSB RP Note4 | Config 1 | dBm/SCS | -88 | -Infinity | -Infinity |
| Config 2 | dBm/SCS | -88 | -Infinity | -Infinity |
| Config 3 | dBm/SCS | -88 | -Infinity | -Infinity |
| Propagation Condition | |  | AWGN | | |
| Note 1: OCNG shall be used such that active cell (Cell 1) is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.  Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 4: SSB RP and Io levels have been derived from other parameters and are given for information purpose. These are not settable test parameters. | | | | | |

**Table A.6.6.12.2.1-4: Cell-specific test parameters for RSTD measurement reporting delay during T2 and T3**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Cell 1** | **Cell 2** | **Cell 3** |
| **T2** | **T2** | **T2** |
| NR RF Channel Number | |  | 1 | 1 | 2 |
| Positiong frequency layer | |  | 1 | 1 | 2 |
| Correlation Matrix and Antenna Configuration | |  | 1x2 Low | 1x2 Low | 1x2 Low |
| OCNG patterns defined in A.3.2.1 | |  | OP.1 | OP.1 | OP.1 |
| PRACH configuration | |  | FR1 PRACH configuration 1 | FR1 PRACH configuration 1 | FR1 PRACH configuration 1 |
| Note 3 | Config 1 | dBm/SCS | -98 | -98 | -98 |
| Config 2 | dBm/SCS | -98 | -98 | -98 |
| Config 3 | dBm/SCS | -95 | -95 | -95 |
| PRS | Config 1 | dB | -5.45 | -11.67 | -11.67 |
| Config 2 | dB | -5.45 | -11.67 | -11.67 |
| Config 3 | dB | -5.45 | -11.67 | -11.67 |
| Io Note 4 | Config 1 | dBm/  9.36MHz | -69.59 | -69.93 | -69.93 |
| Config 2 | dBm/  96.48MHz | -69.59 | -69.93 | -69.93 |
| Config 3 | dBm/  38.16MHz | -63.72 | -63.89 | -63.89 |
| PRS | | dB | -6 | -13 | -13 |
| Propagation Condition | |  | AWGN | | |
| Note 1: OCNG shall be used such that active cells (all, except Cell 3 in T3) are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols other than those in the subframes with transmitted PRS.  Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled. | | | | | |

##### A.6.6.12.2.2 Test Requirements

The RSTD measurement time fulfils the requirements specified in Clause 9.9.2.5.

The UE shall perform and report the RSTD measurements for Cell 2 and Cell 3 with respect to the reference cell in the DL-TDOA assistance data, Cell 1, within the time duration specified in section 9.9.1.5 starting from the beginning of time interval T2.

The rate of the correct events for each neighbour cell observed during repeated tests shall be at least 90%, where the reported RSTD measurement for each correct event shall be within the RSTD reporting range specified in Clause 10.1.23.3, i.e., between RSTD\_0000000 and RSTD\_1970049.

*<End of change8>*

*<Start of change9>*

### A.6.6.14 UE Rx-Tx time difference measurements

#### A.6.6.14.1 UE Rx-Tx time difference measurement for single positioning frequency layer in FR1 SA

##### A.6.6.14.1.1 Test purpose and environment

The purpose of the test is to verify that the UE Rx-Tx measurement meets the requirements specified in clause 9.9.4.5 in AWGN propagation condition in FR1 in standalone scenario when single positioning frequency layer is configured.

The supported test configurations in listed in Table A.6.6.14.1.1-1.

Table A.6.6.14.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. | |

There are two cells in the test: PCell (Cell 1) and a neighbour cell (Cell 2). All cells are on the same RF channel in FR1.

The test consists of two consecutive time intervals, with duration of T1 and T2. Cell 1 and Cell 2 mute PRS transmission during T1 and transmit PRS during T2.

The *NR-Multi-RTT-ProvideAssistanceData* and *nr-Multi-RTT-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE during T1. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the multi-RTT assistance data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources.

The UE is configured with measurement gap pattern ID #0 or ID #24 before T2.

The UE is configured to transmit SRS during T2.

The general test parameters and cell specific test parameters are as given in Table A.6.6.14.1.1-2 and Table A.6.6.14.1.1-3 respectively.

Table A.6.6.14.1.1-2: General test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Active cell |  | 1, 2, 3 | Cell 1 | Cell 1 is the PCell in *NR-Multi-RTT-ProvideAssistanceData* [34]. |
| Neighbour cell |  | 1, 2, 3 | Cell 2 | Cell 2 is a neighbour cell in *NR-Multi-RTT-ProvideAssistanceData* [34]. |
| RF Channel Number |  | 1, 2, 3 | 1 | For both Cell 1 and Cell 2 |
| BWchannel | MHz | 1 | 10: NRB,c = 52 |  |
| 2 | 10: NRB,c = 52 |  |
| 3 | 40: NRB,c = 106 |  |
| SSB configuration |  | 1 | SSB.1 FR1 |  |
|  |  | 2 | SSB.1 FR1 |  |
|  |  | 3 | SSB.2 FR1 |  |
| SMTC configuration |  | 1 | SMTC.2 |  |
|  |  | 2 | SMTC.1 |  |
|  |  | 3 | SMTC.1 |  |
| Measurement gap |  | 1, 2, 3 | GP#24 or GP#0 Note 1 |  |
| CP length |  | 1, 2, 3 | Normal |  |
| DRX |  | 1, 2, 3 | OFF |  |
| Time offset between serving and neighbour cells | μs | 1, 2, 3 | 3 | Synchronous cells |
| T1 | s | 1, 2, 3 | 5 |  |
| T2 | s | 1, 2, 3 | 10 |  |
| Note 1: GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured. | | | | |

Table A.6.6.14.1.1-3: Cell specific test parameters

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | | Cell 2 | |
|  |  | T1 | T2 | T1 | T2 |
| TDD configuration |  | 1 | N/A | | N/A | |
|  | 2 | TDDConf.1.1 | | TDDConf.1.1 | |
|  |  | 3 | TDDConf.2.1 | | TDDConf.2.1 | |
| PDSCH RMC configuration |  | 1 | SR.1.1 FDD | | N/A | |
|  | 2 | SR.1.1 TDD | |  | |
|  | 3 | SR.2.1 TDD | |  | |
| RMSI CORESET RMC configuration |  | 1 | CR.1.1 FDD | | N/A | |
|  | 2 | CR.1.1 TDD | |
|  |  | 3 | CR.2.1 TDD | |
| Dedicated CORESET RMC configuration |  | 1 | CCR.1.1 FDD | | N/A | |
|  | 2 | CCR.1.1 TDD | |
|  | 3 | CCR.2.1 TDD | |
| OCNG Patterns |  | 1, 2, 3 | OP.1 | | OP.1 | |
| TRS Configuration |  | 1 | TRS.1.1 FDD | | N/A | |
|  | 2 | TRS.1.1 TDD | |
|  |  | 3 | TRS.1.2 TDD | |
| Initial BWP configuration |  | 1, 2, 3 | DLBWP.0.1 ULBWP.0.1 | | N/A | |
| Active DL BWP configuration |  | 1, 2, 3 | DLBWP.1.1 | | N/A | |
| Active UL BWP configuration |  | 1, 2, 3 | ULBWP.1.1 | | N/A | |
| PRS configuration |  | 1 | PRS.1.2 FR1 | | PRS.1.2 FR1 | |
|  | 2 | PRS.1.2 FR1 | | PRS.1.2 FR1 | |
|  | 3 | PRS.2.2 FR1 | | PRS.2.2 FR1 | |
| PRS muting info |  | 1, 2, 3 | ‘10’ | | ‘01’ | |
| SRS configuration |  | 1 | POS-SRS.1 | | N/A | |
|  | 2 | POS-SRS.1 | | N/A | |
|  | 3 | POS-SRS.2 | | N/A | |
| Note 2 | dBm/SCS | 1 | -98 | | | |
|  | 2 | -98 | | | |
|  | 3 | -95 | | | |
| Note 2 | dBm/15 kHz | 1 | -98 | | | |
|  | 2 |  | | | |
|  | 3 |  | | | |
| PRS | dB | 1 | -Infinity | -2.41 | -Infinity | -12.12 |
|  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS | dB | 1 | -Infinity | -2 | -Infinity | -10 |
|  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS-RSRP Note 3 | dBm/SCS kHz | 1 | -Infinity | -100 | -Infinity | -108 |
|  | 2 | -Infinity | -100 | -Infinity | -108 |
|  | 3 | -Infinity | -97 | -Infinity | -105 |
| Io | dBm/9.36 MHz | 1 | N/A | -67.67 | N/A | -67.67 |
| dBm/9.36 MHz | 2 | -67.67 | -67.67 |
| dBm/38.16 MHz | 3 | -61.57 | -61.57 |
| Propagation Condition |  | 1, 2, 3 | AWGN | | | |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 3: PRS-RSRP levels have been derived from other parameters for information purposes. They are not settable parameters themselves. | | | | | | |

Table A.6.6.14.1.1-4: Void



##### A.6.6.14.1.2 Test requirements

The UE Rx-Tx time difference measurement time fulfils the requirements specified in clause 9.9.4.5.

The UE shall perform and report the UE Rx-Tx time difference measurements for Cell 1 and Cell 2 within the specified UE Rx-Tx time difference measurement time starting from the beginning of time interval T2.

The rate of the correct events for each neighbour cell observed during repeated tests shall be at least 90%, where the reported UE Rx-Tx measurement for each correct event shall be within the UE Rx-Tx reporting range specified in clause 10.1.25.3.1.

#### A.6.6.14.2 UE Rx-Tx time difference measurement for dual positioning frequency layers in FR1 SA

##### A.6.6.14.2.1 Test purpose and environment

The purpose of the test is to verify that the UE Rx-Tx measurement meets the requirements specified in clause 9.9.4.5 in AWGN propagation condition in FR1 in standalone scenario when dual positioning frequency layers are configured.

The supported test configurations in listed in Table A.6.6.14.2.1-1.

Table A.6.6.14.2.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. | |

There are two cells in the test: PCell (Cell 1) and a neighbour cell (Cell 2). Cell 1 and Cell2 are on different RF channels in FR1.

The test consists of two consecutive time intervals, with duration of T1 and T2. Cell 1 and Cell 2 mute PRS transmission during T1 and transmit PRS during T2.

The *NR-Multi-RTT-ProvideAssistanceData* and *nr-Multi-RTT-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE during T1. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the multi-RTT assistance data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources.

The UE is configured with measurement gap pattern ID #0 or ID #24 before T2.

The UE is configured to transmit SRS during T2.

The general test parameters and cell specific test parameters are as given in Table A.6.6.14.2.1-2 and Table A.6.6.14.2.1-3 respectively.

Table A.6.6.14.2.1-2: General test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Active cell |  | 1, 2, 3 | Cell 1 | Cell 1 is the PCell in *NR-Multi-RTT-ProvideAssistanceData* [34]. |
| Neighbour cell |  | 1, 2, 3 | Cell 2 | Cell 2 is a neighbour cell in *NR-Multi-RTT-ProvideAssistanceData* [34]. |
| RF Channel Number |  | 1, 2, 3 | 1 | For Cell 1 |
| RF Channel Number |  | 1, 2, 3 | 2 | For Cell 2 |
| BWchannel | MHz | 1 | 10: NRB,c = 52 |  |
| 2 | 10: NRB,c = 52 |  |
| 3 | 40: NRB,c = 106 |  |
| SSB configuration |  | 1 | SSB.1 FR1 |  |
|  |  | 2 | SSB.1 FR1 |  |
|  |  | 3 | SSB.2 FR1 |  |
| SMTC configuration |  | 1 | SMTC.2 |  |
|  |  | 2 | SMTC.1 |  |
|  |  | 3 | SMTC.1 |  |
| Measurement gap |  | 1, 2, 3 | GP#24 or GP#0 Note 1 |  |
| CP length |  | 1, 2, 3 | Normal |  |
| DRX |  | 1, 2, 3 | OFF |  |
| Time offset between serving and neighbour cells | μs | 1, 2, 3 | 3 | Synchronous cells |
| T1 | s | 1, 2, 3 | 5 |  |
| T2 | s | 1, 2, 3 | 10 |  |
| Note 1: GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured. | | | | |

Table A.6.6.14.2.1-3: Cell specific test parameters

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | | Cell 2 | |
|  |  | T1 | T2 | T1 | T2 |
| TDD configuration |  | 1 | N/A | | N/A | |
|  | 2 | TDDConf.1.1 | | TDDConf.1.1 | |
|  |  | 3 | TDDConf.2.1 | | TDDConf.2.1 | |
| PDSCH RMC configuration |  | 1 | SR.1.1 FDD | | N/A | |
|  | 2 | SR.1.1 TDD | |  | |
|  | 3 | SR.2.1 TDD | |  | |
| RMSI CORESET RMC configuration |  | 1 | CR.1.1 FDD | | N/A | |
|  | 2 | CR.1.1 TDD | |
|  |  | 3 | CR.2.1 TDD | |
| Dedicated CORESET RMC configuration |  | 1 | CCR.1.1 FDD | | N/A | |
|  | 2 | CCR.1.1 TDD | |
|  | 3 | CCR.2.1 TDD | |
| OCNG Patterns |  | 1, 2, 3 | OP.1 | | OP.1 | |
| TRS Configuration |  | 1 | TRS.1.1 FDD | | N/A | |
|  | 2 | TRS.1.1 TDD | |
|  |  | 3 | TRS.1.2 TDD | |
| Initial BWP configuration |  | 1, 2, 3 | DLBWP.0.1 ULBWP.0.1 | | N/A | |
| Active DL BWP configuration |  | 1, 2, 3 | DLBWP.1.1 | | N/A | |
| Active UL BWP configuration |  | 1, 2, 3 | ULBWP.1.1 | | N/A | |
| PRS configuration |  | 1 | PRS.1.2 FR1 | | PRS.1.2 FR1 | |
|  | 2 | PRS.1.2 FR1 | | PRS.1.2 FR1 | |
|  | 3 | PRS.2.2 FR1 | | PRS.2.2 FR1 | |
| PRS muting info |  | 1, 2, 3 | ‘10’ | | ‘01’ | |
| SRS configuration |  | 1 | POS-SRS.1 | | N/A | |
|  | 2 | POS-SRS.1 | | N/A | |
|  | 3 | POS-SRS.2 | | N/A | |
| Note 2 | dBm/SCS | 1 | -98 | | | |
|  | 2 | -98 | | | |
|  | 3 | -95 | | | |
| Note 2 | dBm/15 kHz | 1 | -98 | | | |
|  | 2 |  | | | |
|  | 3 |  | | | |
| PRS | dB | 1 | -Infinity | -3 | -Infinity | -13 |
|  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS | dB | 1 | -Infinity | -3 | -Infinity | -13 |
|  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS-RSRP Note 3 | dBm/SCS kHz | 1 | -Infinity | -101 | -Infinity | -111 |
|  | 2 | -Infinity | -101 | -Infinity | -111 |
|  | 3 | -Infinity | -98 | -Infinity | -108 |
| Io | dBm/9.36 MHz | 1 | N/A | -68.28 | N/A | -69.63 |
| dBm/9.36 MHz | 2 | -68.28 | -69.63 |
| dBm/38.16 MHz | 3 | -62.19 | -63.54 |
| Propagation Condition |  | 1, 2, 3 | AWGN | | | |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 3: PRS-RSRP levels have been derived from other parameters for information purposes. They are not settable parameters themselves. | | | | | | |

Table A.6.6.14.2.1-4: Void



##### A.6.6.14.2.2 Test requirements

The UE Rx-Tx time difference measurement time fulfils the requirements specified in clause 9.9.4.5.

The UE shall perform and report the UE Rx-Tx time difference measurements for Cell 1 and Cell 2 within the specified UE Rx-Tx time difference measurement time starting from the beginning of time interval T2.

The rate of the correct events for each neighbour cell observed during repeated tests shall be at least 90%, where the reported UE Rx-Tx measurement for each correct event shall be within the UE Rx-Tx reporting range specified in clause 10.1.25.3.1.

*<End of change9>*

*<Start of change10>*

#### A.6.7.15.1 UE Rx-Tx time difference measurement accuracy for single positioning frequency layer in FR1 SA

##### A.6.7.15.1.1 Test purpose and environment

The purpose of the test is to verify that the UE Rx-Tx time difference measurement accuracy is within the specified limits. This test will verify the requirements in clause 10.1.25.2. The test is conducted in AWGN propagation condition in FR1 in standalone scenario when single positioning frequency layer is configured.

The supported test configurations in listed in Table A.6.7.15.1.1-1.

Table A.6.7.15.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| **Configuration** | **Description** |
| 1 | 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. | |

There are two cells in the test: PCell (Cell 1) and a neighbour cell (Cell 2). All cells are on the same RF channel in FR1.

The *NR-Multi-RTT-ProvideAssistanceData* and *nr-Multi-RTT-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE before the start of the test.

The UE is configured with measurement gap pattern ID #0 or ID #24 before the test.

The UE is configured to transmit SRS on Cell 1 during the test.

The test equipment measures the transmit timing of the UE using the transmitted SRS and measures the receive timing using the PRS. The test equipment then compares the difference of these two timings to the UE Rx-Tx measurement reported by the UE for each cell.

##### A.6.7.15.1.2 Test parameters

The UE Rx-Tx time difference accuracy test parameters are given in Table A.6.7.15.1.2-1.

Table A.6.7.15.1.2-2: SRS configuration for UE Rx-Tx time difference measurement accuracy test

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | | Cell 2 | |
|  |  |
| RF Channel Number |  | 1,2,3 | 1 | | 1 | |
| Measurement gap |  | 1,2,3 | GP#24 or GP#0 Note 4 | | | |
| DRX |  | 1,2,3 | OFF | | | |
| Time offset with Cell 1 | μs | 1, 2, 3 | N/A | | 3 | |
| TDD configuration |  | 1 | N/A | | N/A | |
|  | 2 | TDDConf.1.1 | | TDDConf.1.1 | |
|  |  | 3 | TDDConf.2.1 | | TDDConf.2.1 | |
| PDSCH RMC configuration |  | 1 | SR.1.1 FDD | | N/A | |
|  | 2 | SR.1.1 TDD | |  | |
|  | 3 | SR.2.1 TDD | |  | |
| RMSI CORESET RMC configuration |  | 1 | CR.1.1 FDD | | N/A | |
|  | 2 | CR.1.1 TDD | |
|  |  | 3 | CR.2.1 TDD | |
| Dedicated CORESET RMC configuration |  | 1 | CCR.1.1 FDD | | N/A | |
|  | 2 | CCR.1.1 TDD | |
|  | 3 | CCR.2.1 TDD | |
| OCNG Patterns |  | 1, 2, 3 | OP.1 | | OP.1 | |
| TRS Configuration |  | 1 | TRS.1.1 FDD | | N/A | |
|  | 2 | TRS.1.1 TDD | |
|  | 3 | TRS.1.2 TDD | |
| Initial BWP configuration |  | 1, 2, 3 | DLBWP.0.1 ULBWP.0.1 | | N/A | |
| Active DL BWP configuration |  | 1, 2, 3 | DLBWP.1.1 | | N/A | |
| Active UL BWP configuration |  | 1, 2, 3 | ULBWP.1.1 | | N/A | |
| PRS configuration |  | 1 | PRS.1.2 FR1 | | PRS.1.2 FR1 | |
|  | 2 | PRS.1.2 FR1 | | PRS.1.2 FR1 | |
|  | 3 | PRS.2.2 FR1 | | PRS.2.2 FR1 | |
| SRS configuration |  | 1 | POS-SRS.1 | | N/A | |
|  | 2 | POS-SRS.1 | | N/A | |
|  | 3 | POS-SRS.2 | | N/A | |
| Note 2 | dBm/SCS | 1 | -98 | | | |
|  | 2 | -98 | | | |
|  | 3 | -95 | | | |
| Note 2 | dBm/15 kHz | 1 | -98 | | | |
|  | 2 |  | | | |
|  | 3 |  | | | |
| PRS | dB | 1 | -Infinity | -2.41 | -Infinity | -12.12 |
|  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS | dB | 1 | -Infinity | -2 | -Infinity | -10 |
|  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS-RSRP Note 3 | dBm/SCS kHz | 1 | -Infinity | -100 | -Infinity | -108 |
|  | 2 | -Infinity | -100 | -Infinity | -108 |
|  | 3 | -Infinity | -97 | -Infinity | -105 |
| Io | dBm/9.36 MHz | 1 | N/A | -67.67 | N/A | -67.67 |
| dBm/9.36 MHz | 2 | -67.67 | -67.67 |
| dBm/38.16 MHz | 3 | -61.57 | -61.57 |
| Propagation Condition |  | 1, 2, 3 | AWGN | | | |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 3: PRS-RSRP levels have been derived from other parameters for information purposes. They are not settable parameters themselves.  Note 4: GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured. | | | | | | |

Table A.6.7.15.1.2-2: Void



##### A.6.7.15.1.3 Test requirements

The UE Rx-Tx time difference measurement time fulfils the UE Rx-Tx measurement accuracy requirements specified in clause 10.1.25.2 for both Cell 1 and Cell 2.

*<End of change10>*

*<Start of change11>*

### A.7.6.9 RSTD measurements

#### A.7.6.9.1 NR RSTD measurement reporting delay test case for single positioning frequency layer in FR2 SA

##### A.7.6.9.1.1 Test Purpose and Environment

The purpose of the test is to verify that the RSTD measurement meets the requirements specified in Clause 9.9.2 in an environment with AWGN propagation conditions in FR2 in standalone scenario when single positioning frequency layer is configured.

Supported test configurations are shown in table A.7.7.1.1-1. The test parameters are as given in Table 7.6.7.1.1-2, Table A.7.6.9.1.1-3 and Table A.7.6.9.1.1-4.

Table A.7.6.9.1.1-1: Supported test configurations for NR RSTD

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |

In the test there are three synchronous cells: Cell 1, Cell 2 and Cell 3. Cell 1 is the reference as well as the PCell. Cell 2 and Cell 3 are the neighbour cells. All cells are on the same RF channel distributed in single positioning frequency layers.

The test consists of two consecutive time intervals, with duration of T1 and T2. During time duration T1, the UE shall not have any timing information of Cell 2 and Cell 3. All three cells transmit PRS during T2.

Note: The information on when PRS is muted is conveyed to the UE using PRS muting information.

The *NR-DL-TDOA-ProvideAssistanceData* and *nr-DL-TDOA-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE during T1. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the *DL-TDOA assistance* data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources.

The UE is configured with measurement gap pattern ID # 24 or #13 before T2.

Table A.7.6.9.1.1-2: General test parameters for RSTD measurement reporting delay

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | Unit | Value | Comment |
| Reference cell | |  | Cell 1 | Reference cell is the cell in the DL-TDOA assistance data with respect to which the RSTD measurement is defined, as specified in TS 38.215 [4] and TS 37.355[34]. The reference cell is the PCell in this test case. |
| Neighbor cells | |  | Cell 2 and Cell 3 | Cell 2 and Cell 3 appear at the first and second places in the neighbour cell list in the DL-TDOA assistance data. |
| SSB configuration | Config 1 |  | SSB.2 FR2 |  |
| SMTC configuration | Config 1 |  | SMTC.1 |  |
| PDSCH RMC configuration | Config 1 |  | SR.1.1 FDD |  |
| RMSI CORESET RMC configuration | Config 1 |  | CR.3.1 TDD | As specified in clause A.3.1.2.1 |
| Dedicated CORESET RMC configuration | Config 1 |  | CR.1.1 FDD |  |
| PRS Configuration | Config 1 |  | PRS.1.1. FR2 | As specified in clause A.3.31 |
| Physical cell ID PCI | |  | (PCI of Cell 1 – PCI of Cell 2)mod6=0  and  (PCI of Cell 1 – PCI of Cell 3)mod6=0 | The cell PCIs are selected such that the relative shifts of PRS patterns among cells are as given by the test parameters |
| CP length | |  | Normal |  |
| DRX | |  | OFF |  |
| Measurement gap | |  | GP#24 or GP#[13] | GP#24 is configured if UE supports MG#24, otherwise GP#13 is configured |
| Radio frame receive time offset between the cells at the UE antenna connector | | μs | Cell 2 to Cell 1: 0  Cell 3 to Cell 1: 3 | PRS are transmitted from synchronous cells |
| Expected RSTD | | μs | Cell 2: 3  Cell 3: 3  Other neighbour cells: randomly between -3 and 3 | The expected RSTD is what is expected at the receiver. The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355[34] is the expectedRSTD indicator |
| Expected RSTD uncertainty for all neighbour cells | | μs | 500 | The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355[34] is the expectedRSTD-Uncertainty index |
| Number of cells provided in DL-TDOA assistance data | |  | 16 | Including the reference cell |
| PRS muting info | |  | Cell 1: ‘10’  Cell 2: ‘01’  Cell 3: ‘10’ | Correponds to prs-MutingInfo defined in TS 37.355 [24] |
| PRS resource RE offset | |  | Cell 1: 0  Cell 2: 0  Cell 3: 1 | Cell 1 and Cell 3 are configured with different resource offsets |
| T1 | | s | 3 | The length of the time interval from the beginning of each test |
| T2 | | s | [1.28] | The length of the time interval that follows immediately after time interval T1 |
| AoA setup | |  | Setup 1 | As defined in A.3.15.1 |
| Beam assumption | |  | Rough | Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation |

Table A.7.6.9.1.1-3: Cell-specific test parameters for RSTD measurement reporting delay during T1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | | Unit | Cell 1 | Cell 2 | Cell 3 |
| NR RF Channel Number | |  | 1 | 1 | 1 |
| Positiong frequency layer | |  | 1 | 1 | 1 |
| Correlation Matrix and Antenna Configuration | |  | 1x2 Low | 1x2 Low | 1x2 Low |
| OCNG patterns defined in A.3.2.1 | |  | OP.5 FDD | N/A | N/A |
| Note 3 | Config 1 | dBm/SCS | -89 | | |
| PRS | | dB | -Infinity | -Infinity | -Infinity |
| Io Note 4 | Config 1 | dBm/  95.04MHz | -58.86 | -60.01 | -60.01 |
| SSB RP Note4 | Config 1 | dBm/SCS | -89 | -Infinity | -Infinity |
|  |  | dB | 0 | -Infinity | -Infinity |
| Propagation Condition | |  | AWGN | | |
| Note 1: OCNG shall be used such that active cell (Cell 1) is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.  Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 4: SSB RP and Io levels have been derived from other parameters and are given for information purpose. These are not settable test parameters. | | | | | |

**Table A.7.6.9.1.1-4: Cell-specific test parameters for RSTD measurement reporting delay during T2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Cell 1** | **Cell 2** | **Cell 3** |
| **T2** | **T2** | **T2** |
| RF Channel Number | |  | 1 | 1 | 1 |
| Positiong frequency layer | |  | 1 | 1 | 1 |
| Correlation Matrix and Antenna Configuration | |  | 1x2 Low | 1x2 Low | 1x2 Low |
| OCNG patterns defined in A.3.2.1 | |  | OP.1 | OP.1 | OP.1 |
| PRACH configuration | |  | FR2 PRACH configuration 1 | FR2 PRACH configuration 1 | FR2 PRACH configuration 1 |
| Note 3 | Config 1 | dBm/SCS | -89 | -89 | -89 |
| PRS | Config 1 | dB | -5.44 | -11.67 | -11.67 |
| Io | Config 1 | dBm/  9.36MHz | -59.65 | -59.92 | -59.92 |
| PRS | | dB | -6 | -13 | -13 |
| Propagation Condition | |  | AWGN | | |
| Note 1: OCNG shall be used such that active cells (all, except Cell 3 in T3) are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols other than those in the subframes with transmitted PRS.  Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled. | | | | | |

**Table A.7.6.9.1.-5: Void**



##### A.7.6.9.1.2 Test Requirements

The RSTD measurement time fulfils the requirements specified in Clause 9.9.2.5.

The UE shall perform and report the RSTD measurements for Cell 2 and Cell 3 with respect to the reference cell in the DL-TDOA assistance data, Cell 1, within the time duration specified in section 9.9.1.5 starting from the beginning of time interval T2.

The rate of the correct events for each neighbour cell observed during repeated tests shall be at least 90%, where the reported RSTD measurement for each correct event shall be within the RSTD reporting range specified in Clause 10.1.23.3, i.e., between RSTD\_0000000 and RSTD\_1970049.

#### A.7.6.9.2 NR RSTD measurement reporting delay test case for dual positioning frequency layers in FR2 SA

##### A.7.6.9.2.1 Test Purpose and Environment

The purpose of the test is to verify that the RSTD measurement meets the requirements specified in Clause 9.9.2 in an environment with AWGN propagation conditions in FR2 in standalone scenario when dual positioning frequency layer is configured.

Supported test configurations are shown in table A.7.6.9.2.1-1. The test parameters are as given in Table 7.6.7.2.1-2, Table A.7.6.9.2.1-3 and , Table A.7.6.9.2.1-4.

Table A.7.6.9.2.1-1: Supported test configurations for NR RSTD

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |

In the test there are three synchronous cells: Cell 1, Cell 2 and Cell 3. Cell 1 is the reference as well as the PCell. Cell 2 and Cell 3 are the neighbour cells. All cells are on the 2 RF channels distributed in dual positioning frequency layers.

The test consists of two consecutive time intervals, with duration of T1 and T2. During time duration T1, the UE shall not have any timing information of Cell 2 and Cell 3. All three cells transmit PRS during T2.Note: The information on when PRS is muted is conveyed to the UE using PRS muting information.

The *NR-DL-TDOA-ProvideAssistanceData* and *nr-DL-TDOA-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE during T1. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the *DL-TDOA assistance* data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources.

The UE is configured with measurement gap pattern ID # 24 or #13 before T2.

Table A.7.6.9.2.1-2: General test parameters for RSTD measurement reporting delay

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | Unit | Value | Comment |
| Reference cell | |  | Cell 1 | Reference cell is the cell in the DL-TDOA assistance data with respect to which the RSTD measurement is defined, as specified in TS 36.214 [4] and TS 37.355[34]. The reference cell is the PCell in this test case. |
| Neighbor cells | |  | Cell 2 and Cell 3 | Cell 2 and Cell 3 appear at the first and second places in the neighbour cell list in the DL-TDOA assistance data. |
| SSB configuration | Config 1 |  | SSB.2 FR2 |  |
| SMTC configuration | Config 1 |  | SMTC.1 |  |
| PDSCH RMC configuration | Config 1 |  | SR.1.1 FDD |  |
| RMSI CORESET RMC configuration | Config 1 |  | CR.3.1 TDD | As specified in clause A.3.1.2.1 |
| Dedicated CORESET RMC configuration | Config 1 |  | CR.1.1 FDD |  |
| PRS Configuration | Config 1 |  | PRS.1.1. FR2 | As specified in clause A.3.31 |
| Physical cell ID PCI | |  | (PCI of Cell 1 – PCI of Cell 2)mod6=0  and  (PCI of Cell 1 – PCI of Cell 3)mod6=0 | The cell PCIs are selected such that the relative shifts of PRS patterns among cells are as given by the test parameters |
| CP length | |  | Normal |  |
| DRX | |  | OFF |  |
| Measurement gap | |  | GP#24 or GP#13 | GP#24 is configured if UE supports MG#24, otherwise GP#13 is configured |
| Radio frame receive time offset between the cells at the UE antenna connector | | μs | Cell 2 to Cell 1: 0  Cell 3 to Cell 1: 3 | PRS are transmitted from synchronous cells |
| Expected RSTD | | μs | Cell 2: 3  Cell 3: 3  Other neighbour cells: randomly between -3 and 3 | The expected RSTD is what is expected at the receiver. The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355[34] is the expectedRSTD indicator |
| Expected RSTD uncertainty for all neighbour cells | | μs | 5 | The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355[34] is the expectedRSTD-Uncertainty index |
| Number of cells provided in DL-TDOA assistance data | |  | 16 | Including the reference cell |
| PRS muting info | |  | Cell 1: ‘10’  Cell 2: ‘01’  Cell 3: ‘10’ | Correponds to prs-MutingInfo defined in TS 37.355 [24] |
| PRS resource RE offset | |  | Cell 1: 0  Cell 2: 0  Cell 3: 1 | Cell 1 and Cell 3 are configured with different resource offsets |
| T1 | | s | 3 | The length of the time interval from the beginning of each test |
| T2 | | s | 1.28 | The length of the time interval that follows immediately after time interval T1 |
| AoA setup | |  | Setup 1 | As defined in A.3.15.1 |
| Beam assumption | |  | Rough | Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation |

Table A.7.6.9.2.1-3: Cell-specific test parameters for RSTD measurement reporting delay during T1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | | Unit | Cell 1 | Cell 2 | Cell 3 |
| NR RF Channel Number | |  | 1 | 1 | 2 |
| Positiong frequency layer | |  | 1 | 1 | 2 |
| Correlation Matrix and Antenna Configuration | |  | 1x2 Low | 1x2 Low | 1x2 Low |
| OCNG patterns defined in A.3.2.1 | |  | OP.1 | N/A | N/A |
| EPRE ratio of PBCH DMRS to SSS | |  |  |  |  |
| EPRE ratio of PBCH to PBCH DMRS | |
| EPRE ratio of PDCCH DMRS to SSS | |
| EPRE ratio of PDCCH to PDCCH DMRS | |
| EPRE ratio of PDSCH DMRS to SSS | |
| EPRE ratio of PDSCH to PDSCH | |
| EPRE ratio of OCNG DMRS to SSS(Note 1) | |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) | |
| Note 3 | Config 1 | dBm/SCS | -89 | | |
| PRS | | dB | -Infinity | -Infinity | -Infinity |
| Io Note 4 | Config 1 | dBm/95.04MHz | -58.86 | -60.01 | -60.01 |
| SSB RP Note4 | Config 1 | dBm/SCS | -89 | -Infinity | -Infinity |
|  |  | dB | 0 | -Infinity | -Infinity |
| Propagation Condition | |  | AWGN | | |
| Note 1: OCNG shall be used such that active cell (Cell 1) is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.  Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 4: SSB RP and Io levels have been derived from other parameters and are given for information purpose. These are not settable test parameters. | | | | | |

**Table A.7.6.9.2.1-4: Cell-specific test parameters for RSTD measurement reporting delay during T2 and T3**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Cell 1** | **Cell 2** | **Cell 3** |
| **T2** | **T2** | **T2** |
| RF Channel Number | |  | 1 | 1 | 2 |
| Positiong frequency layer | |  | 1 | 1 | 2 |
| Correlation Matrix and Antenna Configuration | |  | 1x2 Low | 1x2 Low | 1x2 Low |
| OCNG patterns defined in A.3.2.1 | |  | OP.1 | OP.1 | OP.1 |
| PRACH configuration | |  | FR2 PRACH configuration 1 | FR2 PRACH configuration 1 | FR2 PRACH configuration 1 |
| Note 3 | Config 1 | dBm/SCS | -89 | -89 | -89 |
| PRS | Config 1 | dB | -5.44 | -11.67 | -11.67 |
| Io | Config 1 | dBm/  9.36MHz | -59.65 | -59.92 | -59.92 |
| PRS | | dB | -6 | -13 | -13 |
| Propagation Condition | |  | AWGN | | |
| Note 1: OCNG shall be used such that active cells (all, except Cell 3 in T3) are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols other than those in the subframes with transmitted PRS.  Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled. | | | | | |

**Table A.7.6.9.2.1-5: Void**



##### A.7.6.9.2.2 Test Requirements

The RSTD measurement time fulfils the requirements specified in Clause 9.9.2.5.

The UE shall perform and report the RSTD measurements for Cell 2 and Cell 3 with respect to the reference cell in the DL-TDOA assistance data, Cell 1, within the time duration specified in section 9.9.1.5 starting from the beginning of time interval T2.

The rate of the correct events for each neighbour cell observed during repeated tests shall be at least 90%, where the reported RSTD measurement for each correct event shall be within the RSTD reporting range specified in Clause 10.1.23.3, i.e., between RSTD\_0000000 and RSTD\_1970049.

*<End of change11>*

*<Start of change12>*

### A.7.6.11 UE Rx-Tx time difference measurements

#### A.7.6.11.1 UE Rx-Tx time difference measurements for single positioning frequency layer in FR2 SA

##### A.7.6.11.1.1 Test purpose and environment

The purpose of the test is to verify that the UE Rx-Tx measurement meets the requirements specified in clause 9.9.4.5 in AWGN propagation condition in FR2 in standalone scenario when single positioning frequency layer is configured.

The supported test configurations in listed in Table A.7.6.11.1.1-1.

Table A.7.6.11.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| **Config** | **Description** |
| 1 | 120 kHz SSB and PRS SCS, 100 MHz bandwidth, TDD duplex mode |

There are two cells in the test: PCell (Cell 1) and a neighbour cell (Cell 2). All cells are on the same RF channel in FR2.

The test consists of two consecutive time intervals, with duration of T1 and T2. Cell 1 and Cell 2 mute PRS transmission during T1 and transmit PRS during T2.

The *NR-Multi-RTT-ProvideAssistanceData* and *nr-Multi-RTT-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE during T1. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the multi-RTT assistance data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources.

The UE is configured with measurement gap pattern ID #13 or ID #24 before T2.

The UE is configured to transmit SRS during T2.

The general test parameters and cell specific test parameters are as given in Table A.7.6.11.1.1-2 and Table A.7.6.11.1.1-3 respectively.

Table A.7.6.11.1.1-2: General test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Active cell |  | 1 | Cell 1 | Cell 1 is the PCell in *NR-Multi-RTT-ProvideAssistanceData* [34]. |
| Neighbour cell |  | 1 | Cell 2 | Cell 2 is a neighbour cell in *NR-Multi-RTT-ProvideAssistanceData* [34]. |
| RF Channel Number |  | 1 | 1 | For both Cell 1 and Cell 2 |
| BWchannel | MHz | 1 | 100: NRB,c = 66 |  |
| SSB configuration |  | 1 | SSB.2 FR2 |  |
| SMTC configuration |  | 1 | SMTC.1 |  |
| Measurement gap |  | 1 | GP#24 or GP#13 Note 1 |  |
| CP length |  | 1 | Normal |  |
| DRX |  | 1 | OFF |  |
| Time offset between serving and neighbour cells | μs | 1 | 3 | Synchronous cells |
| T1 | s | 1 | 5 |  |
| T2 | s | 1 | 20 |  |
| NOTE 1: GP#24 is configured if UE supports MG#24, otherwise GP#13 is configured. | | | | |

Table A.7.6.11.1.1-3: Cell specific test parameters

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | | Cell 2 | |
|  |  | T1 | T2 | T1 | T2 |
| AoA setup |  | 1 | Setup 1 as specified in clause A.3.15 | | | |
| Beam AssumptionNote 7 |  | 1 | Rough | | Rough | |
| TDD configuration |  | 1 | TDDConf.3.1 | | TDDConf.3.1 | |
| PDSCH RMC configuration |  | 1 | SR.3.1 TDD | | N/A | |
| RMSI CORESET RMC configuration |  | 1 | CR.3.1 TDD | | N/A | |
| Dedicated CORESET RMC configuration |  | 1 | CCR.3.1 TDD | | N/A | |
| OCNG Patterns |  | 1 | OP.1 | | OP.1 | |
| TRS Configuration |  | 1 | TRS.2.1 TDD | | N/A | |
| Initial BWP configuration |  | 1 | DLBWP.0.1 ULBWP.0.1 | | N/A | |
| Active DL BWP configuration |  | 1 | DLBWP.1.1 | | N/A | |
| Active UL BWP configuration |  | 1 | ULBWP.1.1 | | N/A | |
| PRS configuration |  | 1 | PRS.1.1 FR2 | | PRS.1.1 FR2 | |
| PRS muting info |  | 1 | ‘10’ | | ‘01’ | |
| SRS configuration |  | 1 | POS-SRS.3 | | N/A | |
| Note 2 | dBm/SCS | 1 | -89 | | | |
| Note 2 | dBm/15 kHz | 1 | -98 | | | |
| PRS | dB | 1 | -Infinity | -2.41 | -Infinity | -12.12 |
| PRS | dB | 1 | -Infinity | -2 | -Infinity | -10 |
| PRS-RSRP Note 3 | dBm/SCS kHz | 1 | -Infinity | -91 | -Infinity | -99 |
| Io | dBm/95.04 MHz | 1 | N/A | -57.63 | N/A | -57.63 |
| Propagation Condition |  | 1 | AWGN | | | |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 3: PRS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.  Note 4: PRS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port.  Note 5: Equivalent power received by an antenna with 0 dBi gain at the centre of the quiet zone  Note 6: As observed with 0 dBi gain antenna at the centre of the quiet zone  Note 7: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation | | | | | | |

Table Table A.7.6.11.1.1-4: Void



##### A.7.6.11.1.2 Test requirements

The UE Rx-Tx time difference measurement time fulfils the requirements specified in clause 9.9.4.5.

The UE shall perform and report the UE Rx-Tx time difference measurements for Cell 1 and Cell 2 within the specified UE Rx-Tx time difference measurement time starting from the beginning of time interval T2.

The rate of the correct events for each neighbour cell observed during repeated tests shall be at least 90%, where the reported UE Rx-Tx measurement for each correct event shall be within the UE Rx-Tx reporting range specified in clause 10.1.25.3.1.

#### A.7.6.11.2 UE Rx-Tx time difference measurement period for dual positioning frequency layers in FR2 SA

##### A.7.6.11.2.1 Test purpose and environment

The purpose of the test is to verify that the UE Rx-Tx measurement meets the requirements specified in clause 9.9.4.5 in AWGN propagation condition in FR2 in standalone scenario when dual positioning frequency layers are cnfigured.

The supported test configurations in listed in Table A.7.6.11.2.1-1.

Table A.7.6.11.2.1-1: Supported test configurations

|  |  |
| --- | --- |
| **Config** | **Description** |
| 1 | 120 kHz SSB and PRS SCS, 100 MHz bandwidth, TDD duplex mode |

There are two cells in the test: PCell (Cell 1) and a neighbour cell (Cell 2). All cells are on different RF channels in FR2.

The test consists of two consecutive time intervals, with duration of T1 and T2. Cell 1 and Cell 2 mute PRS transmission during T1 and transmit PRS during T2.

The *NR-Multi-RTT-ProvideAssistanceData* and *nr-Multi-RTT-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE during T1. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the multi-RTT assistance data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources.

The UE is configured with measurement gap pattern ID #13 or ID #24 before T2.

The UE is configured to transmit SRS during T2.

The general test parameters and cell specific test parameters are as given in Table A.7.6.11.2.1-2 and Table A.7.6.11.2.1-3 respectively.

Table A.7.6.11.2.1-2: General test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Active cell |  | 1 | Cell 1 | Cell 1 is the PCell in *NR-Multi-RTT-ProvideAssistanceData* [34]. |
| Neighbour cell |  | 1 | Cell 2 | Cell 2 is a neighbour cell in *NR-Multi-RTT-ProvideAssistanceData* [34]. |
| RF Channel Number |  | 1 | 1 | For Cell 1 |
| RF Channel Number |  | 1 | 2 | For Cell 2 |
| BWchannel | MHz | 1 | 100: NRB,c = 66 |  |
| SSB configuration |  | 1 | SSB.2 FR2 |  |
| SMTC configuration |  | 1 | SMTC.1 |  |
| Measurement gap |  | 1 | GP#24 or GP#13 Note 1 |  |
| CP length |  | 1 | Normal |  |
| DRX |  | 1 | OFF |  |
| Time offset between serving and neighbour cells | μs | 1 | 3 | Synchronous cells |
| T1 | s | 1 | 5 |  |
| T2 | s | 1 | 20 |  |
| Note 1: GP#24 is configured if UE supports MG#24, otherwise GP#13 is configured. | | | | |

Table A.7.6.11.2.1-3: Cell specific test parameters

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | | Cell 2 | |
|  |  | T1 | T2 | T1 | T2 |
| AoA setup |  | 1 | Setup 1 as specified in clause A.3.15 | | | |
| Beam AssumptionNote 7 |  | 1 | Rough | | Rough | |
| TDD configuration |  | 1 | TDDConf.3.1 | | TDDConf.3.1 | |
| PDSCH RMC configuration |  | 1 | SR.3.1 TDD | | N/A | |
| RMSI CORESET RMC configuration |  | 1 | CR.3.1 TDD | | N/A | |
| Dedicated CORESET RMC configuration |  | 1 | CCR.3.1 TDD | | N/A | |
| OCNG Patterns |  | 1 | OP.1 | | OP.1 | |
| TRS Configuration |  | 1 | TRS.2.1 TDD | | N/A | |
| Initial BWP configuration |  | 1 | DLBWP.0.1 ULBWP.0.1 | | N/A | |
| Active DL BWP configuration |  | 1 | DLBWP.1.1 | | N/A | |
| Active UL BWP configuration |  | 1 | ULBWP.1.1 | | N/A | |
| PRS configuration |  | 1 | PRS.1.1 FR2 | | PRS.1.1 FR2 | |
| PRS muting info |  | 1 | ‘10’ | | ‘01’ | |
| SRS configuration |  | 1 | POS-SRS.3 | | N/A | |
| Note 2 | dBm/SCS | 1 | -89 | | | |
| Note 2 | dBm/15 kHz | 1 | -98 | | | |
| PRS | dB | 1 | -Infinity | -2.41 | -Infinity | -12.12 |
| PRS | dB | 1 | -Infinity | -2 | -Infinity | -10 |
| PRS-RSRP Note 3 | dBm/SCS kHz | 1 | -Infinity | -91 | -Infinity | -99 |
| Io | dBm/95.04 MHz | 1 | N/A | -57.89 | N/A | -59.60 |
| Propagation Condition |  | 1 | AWGN | | | |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 3: PRS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.  Note 4: PRS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port.  Note 5: Equivalent power received by an antenna with 0 dBi gain at the centre of the quiet zone  Note 6: As observed with 0 dBi gain antenna at the centre of the quiet zone  Note 7: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation | | | | | | |

Table Table A.7.6.11.1.1-4: Void



##### A.7.6.11.2.2 Test requirements

The UE Rx-Tx time difference measurement time fulfils the requirements specified in clause 9.9.4.5.

The UE shall perform and report the UE Rx-Tx time difference measurements for Cell 1 and Cell 2 within the specified UE Rx-Tx time difference measurement time starting from the beginning of time interval T2.

The rate of the correct events for each neighbour cell observed during repeated tests shall be at least 90%, where the reported UE Rx-Tx measurement for each correct event shall be within the UE Rx-Tx reporting range specified in clause 10.1.25.3.1.

*<End of change12>*

*<Start of change13>*

#### A.7.7.12.1 UE Rx-Tx time difference measurement period for single positioning frequency layer in FR2 SA

##### A.7.7.12.1.1 Test purpose and environment

The purpose of the test is to verify that the UE Rx-Tx time difference measurement accuracy is within the specified limits. This test will verify the requirements in clause 10.1.25.2. The test is conducted in AWGN propagation condition in FR2 in standalone scenario when single positioning frequency layer is configured.

The supported test configurations in listed in Table A.7.7.12.1.1-1.

Table A.7.7.12.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| **Config** | **Description** |
| 1 | 120 kHz SSB and PRS SCS, 100 MHz bandwidth, TDD duplex mode |

There are two cells in the test: PCell (Cell 1) and a neighbour cell (Cell 2). All cells are on the same RF channel in FR2.

The *NR-Multi-RTT-ProvideAssistanceData* and *nr-Multi-RTT-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.12.1], shall be provided to the UE before the start of the test.

The UE is configured with measurement gap pattern ID #0 or ID #24 before the test.

The UE is configured to transmit SRS on Cell 1 during the test.

The test equipment measures the transmit timing of the UE using the transmitted SRS and measures the receive timing using the PRS. The test equipment then compares the difference of these two timings to the UE Rx-Tx measurement reported by the UE for each cell.

##### A.7.7.12.1.2 Test parameters

The UE Rx-Tx time difference accuracy test parameters are given in Table A.7.7.12.1.2-1.

Table A.7.7.12.1.2-1: SRS configuration for UE Rx-Tx time difference measurement accuracy test

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | | Cell 2 | |
|  |
| AoA setup |  | 1 | Setup 1 as specified in clause A.3.15 | | | |
| Beam AssumptionNote 7 |  | 1 | Rough | | Rough | |
| Measurement gap |  | 1 | GP#24 or GP#0 Note 8 | | | |
| DRX |  | 1 | OFF | | | |
| Time offset with Cell 1 | μs | 1 | N/A | | 3 | |
| TDD configuration |  | 1 | TDDConf.3.1 | | TDDConf.3.1 | |
| PDSCH RMC configuration |  | 1 | SR.3.1 TDD | | N/A | |
| RMSI CORESET RMC configuration |  | 1 | CR.3.1 TDD | | N/A | |
| Dedicated CORESET RMC configuration |  | 1 | CCR.3.1 TDD | | N/A | |
| OCNG Patterns |  | 1 | OP.1 | | OP.1 | |
| TRS Configuration |  | 1 | TRS.2.1 TDD | | N/A | |
| Initial BWP configuration |  | 1 | DLBWP.0.1 ULBWP.0.1 | | N/A | |
| Active DL BWP configuration |  | 1 | DLBWP.1.1 | | N/A | |
| Active UL BWP configuration |  | 1 | ULBWP.1.1 | | N/A | |
| PRS configuration |  | 1 | PRS.1.1 FR2 | | PRS.1.1 FR2 | |
| SRS configuration |  | 1 | POS-SRS.3 | | N/A | |
| Note 2 | dBm/SCS | 1 | -89 | | | |
| Note 2 | dBm/15 kHz | 1 | -98 | | | |
| PRS | dB | 1 | -Infinity | -2.41 | -Infinity | -12.12 |
| PRS | dB | 1 | -Infinity | -2 | -Infinity | -10 |
| PRS-RSRP Note 3 | dBm/SCS kHz | 1 | -Infinity | -91 | -Infinity | -99 |
| Io | dBm/95.04 MHz | 1 | N/A | -57.63 | N/A | -57.63 |
| Propagation Condition |  | 1 | AWGN | | | |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.  Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 3: PRS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.  Note 4: PRS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port.  Note 5: Equivalent power received by an antenna with 0 dBi gain at the centre of the quiet zone  Note 6: As observed with 0 dBi gain antenna at the centre of the quiet zone  Note 7: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation  Note 8: GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured. | | | | | | |

Table A.7.7.12.1.2-2: Void



##### A.7.7.12.1.3 Test requirements

The UE Rx-Tx time difference measurement time fulfils the UE Rx-Tx measurement accuracy requirements specified in clause 10.1.25.2 for both Cell 1 and Cell 2.

*<End of change13>*

*<Start of change14>*

### B.2.1.6 Gain to PRS-RSRP measurement point for FR2

#### B.2.1.6.1 Gain to PRS-RSRP measurement point for Rx Beam Peak angle of arrival

In clause 5.1.28 of TS 38.215 [4] PRS-RSRP is defined to be measured based on the combined signal from antenna elements corresponding to a given receiver branch. The reference point for requirement parameters from the UE perspective is the input of the UE antenna array. The gain “G” relates the combined signal from antenna elements corresponding to a given receiver branch to the reference point for requirement parameters.

The gain “G” affects absolute signal level values reported by the UE.




Figure B.2.1.6.1-1: Gain and Reference point for requirement parameters

The gain range for each power class is specified in Table B.2.1.61-1.

Table B.2.1.6.1-1: UE gain G, Rx beam peak direction

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | UE Power class | | | |
|  | 1 | 2 | 3 | 4 |
| Minimum, dBi | FFS | FFS | -10 | FFS |
| Maximum, dBi | FFS | FFS | +20 | FFS |

Gain range in spherical coverage directions may be lower than in Rx beam peak direction, according to the difference between the EIS spherical coverage value specified in TS 38.101-2 [19] clause 7.3.4 and the Reference sensitivity level specified in TS 38.101-2 [19] clause 7.3.2.

*<End of change14>*