**3GPP TSG- RAN WG4 Meeting # 104-eR4-2213681**

**Electronic meeting, Aug 15 - Aug 26, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.104** | **CR** |  | **rev** |  | **Current version:** | **17.6.0** |  |
|  | | | | | | | | |
| *For* ***[HELP](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)*** *on using this form: comprehensive instructions can be found at  <http://www.3gpp.org/Change-Requests>.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draft CR to TS38.104 the introduction of APT600MHz | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | APT\_NR600-Core | | | | |  | ***Date:*** | | | 2022-8-8 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | APT600MHz is agreed to be introduced in Rel-18, currently the BS RF requirements for APT600MHz is still missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | To introduce the BS RF requirements of APT600MHz into the spec. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | BS RF requirements for APT600MHz is missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2, 5.3.5, 5.4.2.3, 5.4.3.3, 6.6.5.2.3 and 6.6.5.2.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | 37.104, 36.104, 38.133. | | |
| ***affected:*** | | **X** |  | Test specifications | | | | 38.141-1, 38.141-2 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

#### < START OF CHANGE>

## 5.2 *Operating bands*

NR is designed to operate in the *operating bands* defined in table 5.2-1 and 5.2-2.

NR operating band n1, which is defined in Table 5.2-1, can be applied for HAPS operation.

NB-IoT is designed to operate in the NR operating bands n1, n2, n3, n5, n7, n8, n12, n13, n14, n18, n20, n25, n26, n28, n41, n65, n66, n70, n71, n74, n85, n90 which are defined in Table 5.2-1.

Table 5.2-1: NR *operating bands* in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | Uplink (UL) *operating band* BS receive / UE transmit  FUL,low – FUL,high | Downlink (DL) *operating band* BS transmit / UE receive  FDL,low – FDL,high | Duplex mode |
| n1 | 1920 MHz – 1980 MHz | 2110 MHz – 2170 MHz | FDD |
| n2 | 1850 MHz – 1910 MHz | 1930 MHz – 1990 MHz | FDD |
| n3 | 1710 MHz – 1785 MHz | 1805 MHz – 1880 MHz | FDD |
| n5 | 824 MHz – 849 MHz | 869 MHz – 894 MHz | FDD |
| n7 | 2500 MHz – 2570 MHz | 2620 MHz – 2690 MHz | FDD |
| n8 | 880 MHz – 915 MHz | 925 MHz – 960 MHz | FDD |
| n12 | 699 MHz – 716 MHz | 729 MHz – 746 MHz | FDD |
| n13 | 777 MHz – 787 MHz | 746 MHz – 756 MHz | FDD |
| n14 | 788 MHz – 798 MHz | 758 MHz – 768 MHz | FDD |
| n18 | 815 MHz – 830 MHz | 860 MHz – 875 MHz | FDD |
| n20 | 832 MHz – 862 MHz | 791 MHz – 821 MHz | FDD |
| n247 | 1626.5 MHz – 1660.5 MHz | 1525 MHz – 1559 MHz | FDD |
| n25 | 1850 MHz – 1915 MHz | 1930 MHz – 1995 MHz | FDD |
| n26 | 814 MHz – 849 MHz | 859 MHz – 894 MHz | FDD |
| n28 | 703 MHz – 748 MHz | 758 MHz – 803 MHz | FDD |
| n29 | N/A | 717 MHz – 728 MHz | SDL |
| n30 | 2305 MHz – 2315 MHz | 2350 MHz – 2360 MHz | FDD |
| n34 | 2010 MHz – 2025 MHz | 2010 MHz – 2025 MHz | TDD |
| n38 | 2570 MHz – 2620 MHz | 2570 MHz – 2620 MHz | TDD |
| n39 | 1880 MHz – 1920 MHz | 1880 MHz – 1920 MHz | TDD |
| n40 | 2300 MHz – 2400 MHz | 2300 MHz – 2400 MHz | TDD |
| n41 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n46 | 5150 MHz – 5925 MHz | 5150 MHz – 5925 MHz | TDD(NOTE 3) |
| n48 | 3550 MHz – 3700 MHz | 3550 MHz – 3700 MHz | TDD |
| n50 | 1432 MHz – 1517 MHz | 1432 MHz – 1517 MHz | TDD |
| n51 | 1427 MHz – 1432 MHz | 1427 MHz – 1432 MHz | TDD |
| n53 | 2483.5 MHz – 2495 MHz | 2483.5 MHz – 2495 MHz | TDD |
| n65 | 1920 MHz – 2010 MHz | 2110 MHz – 2200 MHz | FDD |
| n66 | 1710 MHz – 1780 MHz | 2110 MHz – 2200 MHz | FDD |
| n67 | N/A | 738 MHz – 758 MHz | SDL |
| n70 | 1695 MHz – 1710 MHz | 1995 MHz – 2020 MHz | FDD |
| n71 | 663 MHz – 698 MHz | 617 MHz – 652 MHz | FDD |
| n74 | 1427 MHz – 1470 MHz | 1475 MHz – 1518 MHz | FDD |
| n75 | N/A | 1432 MHz – 1517 MHz | SDL |
| n76 | N/A | 1427 MHz – 1432 MHz | SDL |
| n77 | 3300 MHz – 4200 MHz | 3300 MHz – 4200 MHz | TDD |
| n78 | 3300 MHz – 3800 MHz | 3300 MHz – 3800 MHz | TDD |
| n79 | 4400 MHz – 5000 MHz | 4400 MHz – 5000 MHz | TDD |
| n80 | 1710 MHz – 1785 MHz | N/A | SUL |
| n81 | 880 MHz – 915 MHz | N/A | SUL |
| n82 | 832 MHz – 862 MHz | N/A | SUL |
| n83 | 703 MHz – 748 MHz | N/A | SUL |
| n84 | 1920 MHz – 1980 MHz | N/A | SUL |
| n85 | 698 MHz – 716 MHz | 728 MHz – 746 MHz | FDD |
| n86 | 1710 MHz – 1780 MHz | N/A | SUL |
| n89 | 824 MHz – 849 MHz | N/A | SUL |
| n90 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n91 | 832 MHz – 862 MHz | 1427 MHz – 1432 MHz | FDD(NOTE 2) |
| n92 | 832 MHz – 862 MHz | 1432 MHz – 1517 MHz | FDD (NOTE 2) |
| n93 | 880 MHz – 915 MHz | 1427 MHz – 1432 MHz | FDD(NOTE 2) |
| n94 | 880 MHz – 915 MHz | 1432 MHz – 1517 MHz | FDD(NOTE 2) |
| n95 (NOTE 1) | 2010 MHz – 2025 MHz | N/A | SUL |
| n96 (NOTE 4) | 5925 MHz – 7125 MHz | 5925 MHz – 7125 MHz | TDD(NOTE 3) |
| n975 | 2300 MHz – 2400 MHz | N/A | SUL |
| n985 | 1880 MHz – 1920 MHz | N/A | SUL |
| n996 | 1626.5 MHz -1660.5 MHz | N/A | SUL |
| n100 | 874.4 MHz – 880 MHz | 919.4 MHz – 925 MHz | FDD |
| n101 | 1900 MHz – 1910 MHz | 1900 MHz – 1910 MHz | TDD |
| n1024 | 5925 MHz – 6425 MHz | 5925 MHz – 6425 MHz | TDD3 |
| n1048 | 6425 MHz – 7125 MHz | 6425 MHz – 7125 MHz | TDD |
| [n105] | 663 MHz – 703 MHz | 612 MHz – 652 MHz | FDD |
| NOTE 1: This band is applicable in China only.  NOTE 2: Variable duplex operation does not enable dynamic variable duplex configuration by the network, and is used such that DL and UL frequency ranges are supported independently in any valid frequency range for the band.  NOTE 3: This band is restricted to operation with shared spectrum channel access as defined in TS 37.213 [20].  NOTE 4: This band is applicable only in countries/regions designating this band for shared-spectrum access use subject to country-specific conditions.  NOTE 5: The requirements for this band are applicable only where no other NR or E-UTRA TDD operating band(s) are used within the frequency range of this band in the same geographical area. For scenarios where other NR or E-UTRA TDD operating band(s) are used within the frequency range of this band in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications.  NOTE 6: UL operation is restricted to 1627.5 – 1637.5 MHz and 1646.5 – 1656.5 MHz per FCC Order DA 20-48.  NOTE 7: DL operation is restricted to 1526-1536 MHz frequency range. UL operation is restricted to 1627.5 – 1637.5 MHz and 1646.5 – 1656.5 MHz per FCC Order 20-51 [24]  NOTE 8: [This band is applicable only in countries/regions designating this band for IMT licensed operation in accordance with RCC Recommendation 1/21.] | | | |

Table 5.2-2: NR *operating bands* in FR2

|  |  |  |
| --- | --- | --- |
| NR *operating band* | Uplink (UL) and Downlink (DL) *operating band* BS transmit/receive UE transmit/receive  FUL,low – FUL,high  FDL,low – FDL,high | Duplex mode |
| n257 | 26500 MHz – 29500 MHz | TDD |
| n258 | 24250 MHz – 27500 MHz | TDD |
| n259 | 39500 MHz – 43500 MHz | TDD |
| n260 | 37000 MHz – 40000 MHz | TDD |
| n261 | 27500 MHz – 28350 MHz | TDD |
| n262 | 47200 MHz – 48200 MHz | TDD |
| n263 | 57000 MHz – 71000 MHz | TDD |

#### < Next OF CHANGE>

### 5.3.5 *BS channel bandwidth* per *operating band*

The requirements in this specification apply to the combination of *BS channel bandwidths*, SCS and *operating bands* shown in table 5.3.5-1 for FR1 and in table 5.3.5-2 and 5.3.5-3 for FR2. The *transmission bandwidth configuration* in table 5.3.2-1, table 5.3.2-2 and table 5.3.2-3 shall be supported for each of the *BS channel bandwidths* within the BS capability. The *BS channel bandwidths* are specified for both the Tx and Rx path.

Table 5.3.5-1: *BS channel bandwidths* and SCS per *operating band* in FR2-1

| NR Band | SCS (kHz) | *BS channel bandwidth* (MHz) | | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 5 | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 | 45 | 50 |  |  |  |  |  |
| n1 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 | 45 | 50 |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 | 45 | 50 |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 | 35 | 40 |  |  |  |  |  |  |  |
| n2 | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 |  |  |  |  |  |
| n3 | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 257 |  |  |  |  |  |  |  |  |  |  |
| n5 | 30 |  | 10 | 15 | 20 | 257 |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 | 35 | 40 |  | 50 |  |  |  |  |  |
| n7 | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 |  | 50 |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 |  | 50 |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  | 35 |  |  |  |  |  |  |  |  |
| n8 | 30 |  | 10 | 15 | 20 |  |  | 35 |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | 30 |  | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n13 | 15 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | 30 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | 30 |  | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
| n20 | 30 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n24 | 30 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 |  |  |  |  |  |  |
| n25 | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 |  |  |  |  |  |  |
| n26 | 15 | 5 | 10 | 15 | 20 | 257 | 307 |  |  |  |  |  |  |  |  |  |
|  | 30 |  | 10 | 15 | 20 | 257 | 307 |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
| n28 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n29 | 30 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | 30 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | 30 |  | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
| n38 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
| n39 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
|  | 15 | 54 | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
| n40 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 15 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 |  |  |  |  |  |
| n41 | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 15 |  | 106 |  | 20 |  |  |  | 40 |  |  |  |  |  |  |  |
| n46 | 30 |  | 106 |  | 20 |  |  |  | 40 |  |  | 60 |  | 80 |  |  |
|  | 60 |  | 106 |  | 20 |  |  |  | 40 |  |  | 60 |  | 80 |  |  |
|  | 15 | 52 | 10 | 15 | 20 |  | 30 |  | 40 |  | 501 |  |  |  |  |  |
| n48 | 30 |  | 10 | 15 | 20 |  | 30 |  | 40 |  | 501 | 601 | 701 | 801 | 901 | 1001 |
|  | 60 |  | 10 | 15 | 20 |  | 30 |  | 40 |  | 501 | 601 | 701 | 801 | 901 | 1001 |
|  | 15 | 52 | 10 | 15 | 20 |  | 30 |  | 40 |  | 50 |  |  |  |  |  |
| n50 | 30 |  | 10 | 15 | 20 |  | 30 |  | 40 |  | 50 | 60 |  | 80 |  |  |
|  | 60 |  | 10 | 15 | 20 |  | 30 |  | 40 |  | 50 | 60 |  | 80 |  |  |
|  | 15 | 5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n51 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n53 | 30 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  | 50 |  |  |  |  |  |
| n65 | 30 |  | 10 | 15 | 20 |  |  |  |  |  | 50 |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 |  |  |  |  |  | 50 |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 |  |  |  |  |  |  |
| n66 | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
| n67 | 30 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 |  |  |  |  |  |  |  |  |  |  |
| n70 | 30 |  | 10 | 15 | 20 | 25 |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 | 35 |  |  |  |  |  |  |  |  |
| n71 | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
| n74 | 30 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
| n75 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
|  | 15 | 5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n76 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
| n77 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 15 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
| n78 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 15 |  | 10 |  | 20 |  | 30 |  | 40 |  | 50 |  |  |  |  |  |
| n79 | 30 |  | 10 |  | 20 |  | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 60 |  | 10 |  | 20 |  | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
| n80 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
| n81 | 30 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
| n82 | 30 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
| n83 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
| n84 | 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
| n85 | 30 |  | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  | 40 |  |  |  |  |  |  |  |
| n86 | 30 |  | 10 | 15 | 20 |  |  |  | 40 |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 | 20 |  |  |  | 40 |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
| n89 | 30 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 |  |  |  |  |  |
| n90 | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 60 |  | 10 | 15 | 20 | 25 | 30 | 35 | 40 | 45 | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 15 | 5 | 103 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n91 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
| n92 | 30 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 103 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
| n94 | 30 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
| n95 | 30 |  | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | 10 | 15 |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 |  |  |  | 20 |  |  |  | 40 |  |  |  |  |  |  |  |
| n96 | 30 |  |  |  | 20 |  |  |  | 40 |  |  | 60 |  | 80 |  |  |
|  | 60 |  |  |  | 20 |  |  |  | 40 |  |  | 60 |  | 80 |  |  |
| n97 | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 |  |  |  |  |  |
| 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
| 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
| n98 | 15 | 5 | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
| 30 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
| 60 |  | 10 | 15 | 20 | 25 | 30 |  | 40 |  |  |  |  |  |  |  |
| n99 | 15 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | 5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n100 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n101 | 15 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 |  |  |  | 20 |  |  |  | 40 |  |  |  |  |  |  |  |
| n102 | 30 |  |  |  | 20 |  |  |  | 40 |  |  | 60 |  | 80 |  |  |
|  | 60 |  |  |  | 20 |  |  |  | 40 |  |  | 60 |  | 80 |  |  |
|  | 15 |  |  |  | 20 |  | 30 |  | 40 |  | 50 |  |  |  |  |  |
| n104 | 30 |  |  |  | 20 |  | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 60 |  |  |  | 20 |  | 30 |  | 40 |  | 50 | 60 | 70 | 80 | 90 | 100 |
|  | 15 | 5 | 10 | 15 | 20 | 25 | 30 | 35 |  |  |  |  |  |  |  |  |
| [n105] | 30 |  | 10 | 15 | 20 | 25 | 30 | 35 |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an downlink SCell part of CA configuration.  NOTE 2: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.  NOTE 3: For this bandwidth, it only applies for UL transmission.  NOTE 4: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.  NOTE 5: Void.  NOTE 6: This bandwidth can only be applied in certain regions where the absence of non 3GPP technologies can be guaranteed on a long term basis in this version of specification.  NOTE 7: For this bandwidth, it only applies for DL transmission. | | | | | | | | | | | | | | | | |

Table 5.3.5-2: *BS channel bandwidths* and SCS per *operating band* in FR2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR Band | SCS (kHz) | *BS channel bandwidth* (MHz) | | | |
| 50 | 100 | 200 | 400 |
| n257 | 60 | 50 | 100 | 200 |  |
|  | 120 | 50 | 100 | 200 | 400 |
| n258 | 60 | 50 | 100 | 200 |  |
|  | 120 | 50 | 100 | 200 | 400 |
| n259 | 60 | 50 | 100 | 200 |  |
|  | 120 | 50 | 100 | 200 | 400 |
| n260 | 60 | 50 | 100 | 200 |  |
|  | 120 | 50 | 100 | 200 | 400 |
| n261 | 60 | 50 | 100 | 200 |  |
|  | 120 | 50 | 100 | 200 | 400 |
| n262 | 60 | 50 | 100 | 200 |  |
|  | 120 | 50 | 100 | 200 | 400 |

Table 5.3.5-3: *BS channel bandwidths* and SCS per *operating band* in FR2-2

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | *BS channel bandwidth* (MHz) | | | | | |
| NR Band | SCS (kHz) | 100 | 400 | 800 | 1600 | 2000 |
| n263 | 120 | 100 | 400 |  |  |  |
|  | 480 |  | 400 | 800 | 1600 |  |
|  | 960 |  | 400 | 800 | 1600 | 2000 |

#### < Next OF CHANGE>

#### 5.4.2.3 Channel raster entries for each *operating band*

The RF channel positions on the channel raster in each NR *operating band* are given through the applicable NR-ARFCN in table 5.4.2.3-1 for FR1 and table 5.4.2.3-2 for FR2, using the channel raster to resource element mapping in clause 5.4.2.2.

- For NR *operating bands* with 100 kHz channel raster, ΔFRaster = 20 × ΔFGlobal. In this case, every 20th NR-ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 is given as <20>.

- For NR *operating bands* with 15 kHz channel raster below 3 GHz, ΔFRaster = *I* × ΔFGlobal, where *I* ϵ {3,6}. In this case, every *Ith* NR‑ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 is given as <*I*>.

- For NR *operating bands* with 15 kHz and 60 kHz channel raster above 3 GHz, ΔFRaster = *I* ×ΔFGlobal, where *I* ϵ {1, 2}. In this case, every *Ith* NR‑ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 and table 5.4.2.3-2 is given as <*I*>.

- For frequency bands with two ΔFRaster in FR1, the higher ΔFRaster applies to channels using only the SCS that is equal to or larger than the higher ΔFRaster and SSB SCS is equal to the higher ΔFRaster.

- For frequency bands with two ΔFRaster in FR2, the higher ΔFRaster applies to channels using only the SCS that is equal to the higher ΔFRaster and the SSB SCS that is equal to or larger than the higher ΔFRaster.

Table 5.4.2.3-1: Applicable NR-ARFCN per *operating band* in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | ΔFRaster  (kHz) | Uplink  range of NREF  (First – <Step size> – Last) | Downlink  range of NREF  (First – <Step size> – Last) |
| n1 | 100 | 384000 – <20> – 396000 | 422000 – <20> – 434000 |
| n2 | 100 | 370000 – <20> – 382000 | 386000 – <20> – 398000 |
| n3 | 100 | 342000 – <20> – 357000 | 361000 – <20> – 376000 |
| n5 | 100 | 164800 – <20> – 169800 | 173800 – <20> – 178800 |
| n7 | 100 | 500000 – <20> – 514000 | 524000 – <20> – 538000 |
| n8 | 100 | 176000 – <20> – 183000 | 185000 – <20> – 192000 |
| n12 | 100 | 139800 – <20> – 143200 | 145800 – <20> – 149200 |
| n13 | 100 | 155400 – <20> – 157400 | 149200 – <20> – 151200 |
| n14 | 100 | 157600 – <20> –159600 | 151600 – <20> – 153600 |
| n18 | 100 | 163000 – <20> – 166000 | 172000 – <20> – 175000 |
| n20 | 100 | 166400 – <20> – 172400 | 158200 – <20> – 164200 |
| n25 | 100 | 370000 – <20> – 383000 | 386000 – <20> – 399000 |
| n24 | 100 | 325300 – <20> – 332100 | 305000 – <20> – 311800 |
| n26 | 100 | 162800 – <20> – 169800 | 171800 – <20> – 178800 |
| n28 | 100 | 140600 – <20> – 149600 | 151600 – <20> – 160600 |
| n29 | 100 | N/A | 143400 – <20> – 145600 |
| n30 | 100 | 461000 – <20> – 463000 | 470000 – <20> – 472000 |
| n34 | 100 | 402000 – <20> – 405000 | 402000 – <20> – 405000 |
| n38 | 100 | 514000 – <20> – 524000 | 514000 – <20> – 524000 |
| n39 | 100 | 376000 – <20> – 384000 | 376000 – <20> – 384000 |
| n40 | 100 | 460000 – <20> – 480000 | 460000 – <20> – 480000 |
| n41 | 15 | 499200 – <3> – 537999 | 499200 – <3> – 537999 |
|  | 30 | 499200 – <6> – 537996 | 499200 – <6> – 537996 |
| n461 | 15 | 743334 – <1> – 795000 | 743334 – <1> – 795000 |
| n48 | 15 | 636667 – <1> – 646666 | 636667 – <1> – 646666 |
|  | 30 | 636668 – <2> – 646666 | 636668 – <2> – 646666 |
| n50 | 100 | 286400 – <20> – 303400 | 286400 – <20> – 303400 |
| n51 | 100 | 285400 – <20> – 286400 | 285400 – <20> – 286400 |
| n53 | 100 | 496700 – <20> – 499000 | 496700 – <20> – 499000 |
| n65 | 100 | 384000 – <20> – 402000 | 422000 – <20> – 440000 |
| n66 | 100 | 342000 – <20> – 356000 | 422000 – <20> – 440000 |
| n67 | 100 | N/A | 147600 – <20> – 151600 |
| n70 | 100 | 339000 – <20> – 342000 | 399000 – <20> – 404000 |
| n71 | 100 | 132600 – <20> – 139600 | 123400 – <20> – 130400 |
| n74 | 100 | 285400 – <20> – 294000 | 295000 – <20> – 303600 |
| n75 | 100 | N/A | 286400 – <20> – 303400 |
| n76 | 100 | N/A | 285400 – <20> – 286400 |
| n77 | 15 | 620000 – <1> – 680000 | 620000 – <1> – 680000 |
|  | 30 | 620000 – <2> – 680000 | 620000 – <2> – 680000 |
| n78 | 15 | 620000 – <1> – 653333 | 620000 – <1> – 653333 |
|  | 30 | 620000 – <2> – 653332 | 620000 – <2> – 653332 |
| n79 | 15 | 693334 – <1> – 733333 | 693334 – <1> – 733333 |
|  | 30 | 693334 – <2> – 733332 | 693334 – <2> – 733332 |
| n80 | 100 | 342000 – <20> – 357000 | N/A |
| n81 | 100 | 176000 – <20> – 183000 | N/A |
| n82 | 100 | 166400 – <20> – 172400 | N/A |
| n83 | 100 | 140600 – <20> –149600 | N/A |
| n84 | 100 | 384000 – <20> – 396000 | N/A |
| n85 | 100 | 139600 – <20> – 143200 | 145600 – <20> – 149200 |
| n86 | 100 | 342000 – <20> – 356000 | N/A |
| n89 | 100 | 164800 – <20> – 169800 | N/A |
|  | 15 | 499200 – <3> – 537999 | 499200 – <3> – 537999 |
| n90 | 30 | 499200 – <6> – 537996 | 499200 – <6> – 537996 |
|  | 100 | 499200 – <20> – 538000 | 499200 – <20> – 538000 |
| n91 | 100 | 166400 – <20> – 172400 | 285400 – <20> – 286400 |
| n92 | 100 | 166400 – <20> – 172400 | 286400 – <20> – 303400 |
| n93 | 100 | 176000 – <20> – 183000 | 285400 – <20> – 286400 |
| n94 | 100 | 176000 – <20> – 183000 | 286400 – <20> – 303400 |
| n95 | 100 | 402000 – <20> – 405000 | N/A |
| n962 | 15 | 795000 – <1> – 875000 | 795000 – <1> – 875000 |
| n97 | 100 | 460000 – <20> – 480000 | N/A |
| n98 | 100 | 376000 – <20> – 384000 | N/A |
| n99 | 100 | 325300 -- <20> – 332100 | N/A |
| n100 | 100 | 174880 – <20> – 176000 | 183880 – <20> – 185000 |
| n101 | 100 | 380000 – <20> – 382000 | 380000 – <20> – 382000 |
| n1023 | 15 | 796334 – <1> – 828333 | 796334 – <1> – 828333 |
| n104 | 15 | 828334 – <1> – 875000 | 828334 – <1> – 875000 |
|  | 30 | 828334 – <2> – 875000 | 828334 – <2> – 875000 |
| [n105] | 100 | 132600 – <20> – 140600 | 122400 – <20> – 130400 |
| NOTE 1: Applicable NR-ARFCN for band n46  for 10 MHz channel bandwidth, NREF = {782000, 788668}  for 20 MHz channel bandwidth, NREF = {744000, 745332, 746668, 748000, 749332, 750668, 752000, 753332, 754668, 756000, 765332, 766668, 768000, 769332, 770668, 772000, 773332, 774668, 776000, 777332, 778668, 780000, 781332, 783000, 784332, 785668, 787000, 788332, 789668, 791000, 792332, 793668};  for 40 MHz channel bandwidth, NREF = {744668, 746000, 748668, 751332, 754000, 755332, 766000, 767332, 770000, 772668, 775332, 778000, 780668, 783668, 786332, 787668, 790332, 793000};  for 60 MHz channel bandwidth, NREF = {745332, 746668, 748000, 752000, 753332, 754668, 766668, 768000, 769332, 773332, 774668, 778668, 780000, 784332, 785668, 791000, 792332};  for 80 MHz channel bandwidth, NREF = {746000, 747332, 752668, 754000, 767332, 768668, 774000, 779332, 785000, 791668}  for 100 MHz channel bandwidth, NREF = {746668, 753332, 768000, 791000}  NOTE 2: Applicable NR-ARFCN for band n96  for 20 MHz channel bandwidth, NREF = {797000, 798332, 799668, 801000, 802332, 803668, 805000, 806332, 807668, 809000, 810332, 811668, 813000, 814332, 815668, 817000, 818332, 819668, 821000, 822332, 823668, 825000, 826332, 827668, 829000, 830332, 831668, 833000, 834332, 835668, 837000, 838332, 839668, 841000, 842332, 843668, 845000, 846332, 847668, 849000, 850332, 851668, 853000, 854332, 855668, 857000, 858332, 859668, 861000, 862332, 863668, 865000, 866332, 867668, 869000, 870332, 871668, 873000, 874332}  for 40 MHz channel bandwidth, NREF = {797668, 800332, 803000, 805668, 808332, 811000, 813668, 816332, 819000, 821668, 824332, 827000, 829668, 832332, 835000, 837668, 840332, 843000, 845668, 848332, 851000, 853668, 856332, 859000, 861668, 864332, 867000, 869668, 872332}  for 60 MHz channel bandwidth, NREF = {798332, 799668, 803668, 805000, 809000, 810332, 814332, 815668, 819668, 821000, 825000, 826332, 830332, 831668, 835668, 837000, 841000, 842332, 846332, 847668, 851668, 853000, 857000, 858332, 862332, 863668, 867668, 869000, 873000}  for 80 MHz channel bandwidth, NREF = {799000, 804332, 809668, 815000, 820332, 825668, 831000, 836332, 841668, 847000, 852332, 857668, 863000, 868332}  for 100 MHz channel bandwidth, NREF = {799668, 803668, 810332, 814332, 821000, 825000, 831668, 835668, 842332, 846332, 853000, 857000, 863668, 867668, 869000, 870332, 871668}  NOTE 3: Applicable NR-ARFCN for band n102  for 20 MHz channel bandwidth, NREF = {795668, 797000, 798332, 799668, 801000, 802332, 803668, 805000, 806332, 807668, 809000, 810332, 811668, 813000, 814332, 815668, 817000, 818332, 819668, 821000, 822332, 823668, 825000, 826332, 827668}  for 40 MHz channel bandwidth, NREF = {797668, 800332, 803000, 805668, 808332, 811000, 813668, 816332, 819000, 821668, 824332, 827000}  for 60 MHz channel bandwidth, NREF = {798332, 799668, 803668, 805000, 809000, 810332, 814332, 815668, 819668, 821000, 825000, 826332}  for 80 MHz channel bandwidth, NREF = {799000, 804332, 809668, 815000, 820332, 825668}  for 100 MHz channel bandwidth, NREF = {799668, 803668, 810332, 814332, 821000, 825000} | | | |

Table 5.4.2.3-2: Applicable NR-ARFCN per *operating band* in FR2

|  |  |  |
| --- | --- | --- |
| NR *operating band* | ΔFRaster  (kHz) | Uplink and Downlink  range of NREF  (First – <Step size> – Last) |
| n257 | 60 | 2054166 – <1> – 2104165 |
|  | 120 | 2054167 – <2> – 2104165 |
| n258 | 60 | 2016667 – <1> – 2070832 |
|  | 120 | 2016667 – <2> – 2070831 |
| n259 | 60 | 2270833 – <1> – 2337499 |
|  | 120 | 2270833 – <2> – 2337499 |
| n260 | 60 | 2229166 – <1> – 2279165 |
|  | 120 | 2229167 – <2> – 2279165 |
| n261 | 60 | 2070833 – <1> – 2084999 |
|  | 120 | 2070833 – <2> – 2084999 |
| n262 | 60 | 2399166 – <1> – 2415832 |
|  | 120 | 2399167 – <2> – 2415831 |
| n263 | 120 | See Table 5.4.2.3-2 |
|  | 480 |  |
|  | 960 |  |

Table 5.4.2.3-3: Applicable NR-ARFCN for operation in band n263

|  |  |
| --- | --- |
| Channel Bandwidth | Applicable NR-ARFCN |
| 100 MHz | 2564083 + 1680 \* N, N = 0:137 |
| 400 MHz | 2566603 + 6720 \* N, N = 0:33 |
| 800 MHz | 2569963 + 6720 \* N, N = 0:32 |
| 1600 MHz | 2576683 + 6720 \* N, N =0:30 |
| 2000 MHz | 2580043 + 6720 \* N, N=0:29,  2585083, 2655643, 2692603, 2764843 |

#### < Next OF CHANGE>

#### 5.4.3.3 Synchronization raster entries for each operating band

The synchronization raster for each band is give in table 5.4.3.3-1. The distance between applicable GSCN entries is given by the <Step size> indicated in table 5.4.3.3-1 for FR1 and table 5.4.3.3-2 for FR2.

Table 5.4.3.3-1: Applicable SS raster entries per *operating band* (FR1)

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | SS Block SCS | SS Block pattern (NOTE 1) | Range of GSCN  (First – <Step size> – Last) |
| n1 | 15 kHz | Case A | 5279 – <1> – 5419 |
| n2 | 15 kHz | Case A | 4829 – <1> – 4969 |
| n3 | 15 kHz | Case A | 4517 – <1> – 4693 |
| n5 | 15 kHz | Case A | 2177 – <1> – 2230 |
|  | 30 kHz | Case B | 2183 – <1> – 2224 |
| n7 | 15 kHz | Case A | 6554 – <1> – 6718 |
| n8 | 15 kHz | Case A | 2318 – <1> – 2395 |
| n12 | 15 kHz | Case A | 1828 – <1> – 1858 |
| n13 | 15 kHz | Case A | 1871 – <1> – 1885 |
| n14 | 15 kHz | Case A | 1901 – <1> – 1915 |
| n18 | 15kHz | CaseA | 2156 – <1> – 2182 |
| n20 | 15 kHz | Case A | 1982 – <1> – 2047 |
| n24 | 15 kHz | Case A | 3818 – <1> – 3892 |
| 30 kHz | Case B | 3824 – <1> – 3886 |
| n25 | 15 kHz | Case A | 4829 – <1> – 4981 |
| n26 | 15 kHz | Case A | 2153 – <1> – 2230 |
| n28 | 15 kHz | Case A | 1901 – <1> – 2002 |
| n29 | 15 kHz | Case A | 1798 – <1> – 1813 |
| n30 | 15 kHz | Case A | 5879 – <1> – 5893 |
| n34 | 15 kHz | Case A | NOTE 3 |
|  | 30 kHz | Case C | 5036 – <1> – 5050 |
| n38 | 15 kHz | Case A | NOTE 2 |
|  | 30 kHz | Case C | 6437 – <1> – 6538 |
| n39 | 15 kHz | Case A | NOTE 4 |
|  | 30 kHz | Case C | 4712 – <1> – 4789 |
| n40 | 30 kHz | Case C | 5762 – <1> – 5989 |
| n41 | 15 kHz | Case A | 6246 – <3> – 6717 |
|  | 30 kHz | Case C | 6252 – <3> – 6714 |
| n465 | 30 kHz | Case C | 8993 – <1> – 9530 |
| n48 | 30 kHz | Case C | 7884 – <1> – 7982 |
| n50 | 30 kHz | Case C | 3590 – <1> – 3781 |
| n51 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n53 | 15 kHz | Case A | 6215 – <1> – 6232 |
| n65 | 15 kHz | Case A | 5279 – <1> – 5494 |
| n66 | 15 kHz | Case A | 5279 – <1> – 5494 |
|  | 30 kHz | Case B | 5285 – <1> – 5488 |
| n67 | 15 kHz | Case A | 1850 – <1> – 1888 |
| n70 | 15 kHz | Case A | 4993 – <1> – 5044 |
| n71 | 15 kHz | Case A | 1547 – <1> – 1624 |
| n74 | 15 kHz | Case A | 3692 – <1> – 3790 |
| n75 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n76 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n77 | 30 kHz | Case C | 7711 – <1> – 8329 |
| n78 | 30 kHz | Case C | 7711 – <1> – 8051 |
| n79 | 30 kHz | Case C | 8480 – <16> – 88807 |
|  |  |  | 8475 – <1> – 88848 |
| n85 | 15 kHz | Case A | 1826 – <1> – 1858 |
| n90 | 15 kHz | Case A | 6246 – <1> – 671710 |
|  | 15 kHz | Case A | 6245 – <1> – 671811 |
|  | 30 kHz | Case C | 6252 – <1> – 6714 |
| n91 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n92 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n93 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n94 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n96**6** | 30 kHz | Case C | 9531 – <1> – 10363 |
| n100 | 15 kHz | Case A | 2303 – <1> – 2307 |
| n101 | 15 kHz | Case A | 4754 – <1> – 4768 |
| 30kHz | Case C | 4760 – <1> – 4764 |
| n102**9** | 30 kHz | Case C | 9531 – <1> – 9877 |
| n104 | 30 kHz | Case C | 9882 – <7> – 10358 |
| [n105] | 15 kHz | Case A | 1535 – <1> – 1624 |
| NOTE 1: SS Block pattern is defined in clause 4.1 in TS 38.213 [10].  NOTE 2: The applicable SS raster entries are GSCN = {6432, 6443, 6457, 6468, 6479, 6493, 6507, 6518, 6532, 6543}  NOTE 3: The applicable SS raster entries are GSCN = {5032, 5043, 5054}  NOTE 4: The applicable SS raster entries are GSCN = {4707, 4715, 4718, 4729, 4732, 4743, 4747, 4754, 4761, 4768, 4772, 4782, 4786, 4793}  NOTE 5: The following GSCN are allowed for operation in band n46:  GSCN = {8996, 9010, 9024, 9038, 9051, 9065, 9079, 9093, 9107, 9121, 9218, 9232, 9246, 9260, 9274, 9288, 9301, 9315, 9329, 9343, 9357, 9371, 9385, 9402, 9416, 9430, 9444, 9458, 9472, 9485, 9499, 9513}.  NOTE 6: The following GSCN are allowed for operation in band n96:  GSCN = { 9548, 9562, 9576, 9590, 9603, 9617, 9631, 9645, 9659, 9673, 9687, 9701, 9714, 9728, 9742, 9756, 9770, 9784, 9798, 9812, 9826, 9840, 9853, 9867, 9881, 9895, 9909, 9923, 9937, 9951, 9964, 9978, 9992, 10006, 10020, 10034, 10048, 10062, 10076, 10090, 10103, 10117, 10131, 10145, 10159, 10173, 10187, 10201, 10214, 10228, 10242, 10256, 10270, 10284, 10298, 10312, 10325, 10339, 10353}.  NOTE 7: The SS raster entries apply for channel bandwidths larger than or equal to 40 MHz.  NOTE 8: The SS raster entries apply for channel bandwidths smaller than 40 MHz.  NOTE 9: The following GSCN are allowed for operation in band n102:  GSCN = {9535, 9548, 9562, 9576, 9590, 9603, 9617, 9631, 9645, 9659, 9673, 9687, 9701, 9714, 9728, 9742, 9756, 9770, 9784, 9798, 9812, 9826, 9840, 9853, 9867}  NOTE 10: The SS raster entries apply for channel bandwidths larger than or equal to 10 MHz.  NOTE 11: The SS raster entries apply for channel bandwidth equal to 5 MHz. | | | |

Table 5.4.3.3-2: Applicable SS raster entries per *operating band* (FR2)

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | SS Block SCS | SS Block pattern (note 1) | Range of GSCN  (First – <Step size> – Last) |
| n257 | 120 kHz | Case D | 22388 – <1> – 22558 |
|  | 240 kHz | Case E | 22390 – <2> – 22556 |
| n258 | 120 kHz | Case D | 22257 – <1> – 22443 |
|  | 240 kHz | Case E | 22258 – <2> – 22442 |
| n259 | 120 kHz | Case D | 23140 – <1> – 23369 |
|  | 240 kHz | Case E | 23142 – <2> – 23368 |
| n260 | 120 kHz | Case D | 22995 – <1> – 23166 |
|  | 240 kHz | Case E | 22996 – <2> – 23164 |
| n261 | 120 kHz | Case D | 22446 – <1> – 22492 |
|  | 240 kHz | Case E | 22446 – <2> – 22490 |
| n262 | 120 kHz | Case D | 23586 – <1> – 23641 |
|  | 240 kHz | Case E | 23588 – <2> – 23640 |
| n263 | 120 kHz | Case D | Table 5.4.3.3-2 |
|  | 480 kHz | Case F |  |
|  | 960 kHz2 | Case G | 24162 – <6> – 24954 |
| NOTE 1: SS Block pattern is defined in section 4.1 in TS 38.213 [10].  NOTE 2: SS Block SCS of 960 kHz is not used for initial access. | | | |

Table 5.4.3.3-3: Allowed GSCN for operation in band n263 for 120 kHz and 480 kHz

|  |  |
| --- | --- |
| SS Block SCS | Range of GSCN |
| 120 kHz | 24156 + 6 \* N – 3 \* floor((N+5)/18), N=0:137 |
| 480 kHz | 24162 + 24 \* N – 12 \* floor((N+4)/18), N=0:33 |

#### < Next OF CHANGE>

6.6.4.2.2.1 Category B requirements (Option 1)

For BS operating in Bands n5, n8, n12, n20, n26, n28, n29, n67, n71, n85,[n105], the *basic limits* are specified in table 6.6.4.2.2.1-1:

Table 6.6.4.2.2.1-1: Wide Area BS operating band unwanted emission limits   
(NR bands below 1 GHz) for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limits* (Note 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz |
| 5 MHz ≤ Δf <  min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <  min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz |
| 10 MHz ≤ Δf ≤ Δfmax | 10.05 MHz ≤ f\_offset < f\_offsetmax | -16 dBm (Note 3) | 100 kHz |
| NOTE 1: For a BS supporting *non-contiguous spectrum* operation within any *operating band*, the emission limits within *sub-block gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *sub-block gap*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *sub-block gap*, where the emission limits within *sub-block gaps* shall be ‑16 dBm/100 kHz.  NOTE 2: For a *multi-band connector* with *Inter RF Bandwidth gap* < 2\*ΔfOBUE the emission limits within the *Inter RF Bandwidth gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or RF Bandwidth on each side of the *Inter RF Bandwidth gap*, where the contribution from the far-end *sub-block* or RF Bandwidth shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or RF Bandwidth.  NOTE 3: The requirement is not applicable when Δfmax < 10 MHz. | | | |

For BS operating in Bands n1, n2, n3, n7, n25, n34, n38, n39, n40, n41, n48, n50, n65, n66, n70, n75, n77, n78, n79, n90, n92, n94, *basic limits* are specified in tables 6.6.4.2.2.1-2:

Table 6.6.4.2.2.1-2: Wide Area BS operating band unwanted emission limits   
(NR bands above 1 GHz) for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limits* (Note 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz |
| 5 MHz ≤ Δf <  min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <  min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz |
| 10 MHz ≤ Δf ≤ Δfmax | 10.5 MHz ≤ f\_offset < f\_offsetmax | -15 dBm (Note 3) | 1MHz |
| NOTE 1: For a BS supporting *non-contiguous spectrum* operation within any *operating band*, the emission limits within *sub-block gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *sub-block gap*, where the contribution from the far-end *sub-block* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *sub-block gap*, where the emission limits within *sub-block gaps* shall be ‑15 dBm/1 MHz.  NOTE 2: For a *multi-band connector* with *Inter RF Bandwidth gap* < 2\*ΔfOBUE the emission limits within the *Inter RF Bandwidth gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or RF Bandwidth on each side of the *Inter RF Bandwidth gap*, where the contribution from the far-end *sub-block* or RF Bandwidth shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or RF Bandwidth.  NOTE 3: The requirement is not applicable when Δfmax < 10 MHz. | | | |

For *BS type 1-C* operating in Band n104, thelimits are specified in tables 6.6.4.2.2.1-2a:

Table 6.6.4.2.2.1-2a: Wide Area *BS type 1-C* operating band unwanted emission limits for band n104 for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | Basic limits | Measurement bandwidth |
| 0 MHz ≤ Δf < 20 MHz | 0.05 MHz ≤ f\_offset < 20.05 MHz |  | 100 kHz |
| 20 MHz ≤ Δf <  min(40 MHz, Δfmax) | 20.05 MHz ≤ f\_offset <  min(40.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz |
| 40 MHz ≤ Δf ≤ Δfmax | 40.5 MHz ≤ f\_offset < f\_offsetmax | -15 dBm (Note 3) | 1MHz |
| NOTE 1: For a BS supporting *non-contiguous spectrum* operation within any *operating band* the emission limits within *sub-block gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *sub-block gap*. Exception is f ≥ 100MHz from both adjacent *sub-blocks* on each side of the *sub-block gap*, where the emission limits within *sub-block gaps* shall be ‑15 dBm/1 MHz.  NOTE 2: For a *multi-band connector* with *Inter RF Bandwidth gap* < 2\*ΔfOBUE the emission limits within the *Inter RF Bandwidth gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or RF Bandwidth on each side of the *Inter RF Bandwidth gap*.  NOTE 3: The requirement is not applicable when Δfmax <40 MHz. | | | |

For *BS type 1-H* operating in Band n104, *basic limits* are specified in tables 6.6.4.2.2.1-2b:

Table 6.6.4.2.2.1-2b: Wide Area *BS type 1-H* operating band unwanted emission limits for band n104 for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | Basic limits | Measurement bandwidth |
| 0 MHz ≤ Δf < 50 MHz | 0.05 MHz ≤ f\_offset < 50.05 MHz |  | 100 kHz |
| 50 MHz ≤ Δf <  min(100 MHz, Δfmax) | 50.05 MHz ≤ f\_offset <  min(100.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz |
| 100 MHz ≤ Δf ≤ Δfmax | 100.5 MHz ≤ f\_offset < f\_offsetmax | -15 dBm (Note 3) | 1MHz |
| NOTE 1: For a BS supporting *non-contiguous spectrum* operation within any *operating band* the emission limits within *sub-block gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *sub-block gap*. Exception is f ≥ 100MHz from both adjacent *sub-blocks* on each side of the *sub-block gap*, where the emission limits within *sub-block gaps* shall be ‑15 dBm/1 MHz.  NOTE 2: For a *multi-band connector* with *Inter RF Bandwidth gap* < 2\*ΔfOBUE the emission limits within the *Inter RF Bandwidth gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or RF Bandwidth on each side of the *Inter RF Bandwidth gap*.  NOTE 3: The requirement is not applicable when Δfmax < 100 MHz. | | | |

#### < Next OF CHANGE>

##### 6.6.5.2.3 Additional spurious emissions requirements

These requirements may be applied for the protection of system operating in frequency ranges other than the BS downlink *operating band*. The limits may apply as an optional protection of such systems that are deployed in the same geographical area as the BS, or they may be set by local or regional regulation as a mandatory requirement for an NR *operating band*. It is in some cases not stated in the present document whether a requirement is mandatory or under what exact circumstances that a limit applies, since this is set by local or regional regulation. An overview of regional requirements in the present document is given in clause 4.5.

Some requirements may apply for the protection of specific equipment (UE, MS and/or BS) or equipment operating in specific systems (GSM, CDMA, UTRA, E-UTRA, NR, etc.) as listed below.

The spurious emission *basic limits* are provided in table 6.6.5.2.3 -1 for a BS where requirements for co-existence with the system listed in the first column apply. For a *multi-band connector*, the exclusions and conditions in the Note column of table 6.6.5.2.3 -1 apply for each supported *operating band*.

Table 6.6.5.2.3-1: BS spurious emissions *basic* *limits* for BS for co-existence with systems operating in other frequency bands

| System type for NR to co-exist with | Frequency range for co-existence requirement | *Basic limits* | *Measurement bandwidth* | Note |
| --- | --- | --- | --- | --- |
|  | 921 – 960 MHz | -57 dBm | 100 kHz | This requirement does not apply to BS operating in band n8 |
| GSM900 | 876 – 915 MHz | -61 dBm | 100 kHz | For the frequency range 880-915 MHz, this requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 1805 – 1880 MHz | -47 dBm | 100 kHz | This requirement does not apply to BS operating in band n3. |
| DCS1800 | 1710 – 1785 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 1930 – 1990 MHz | -47 dBm | 100 kHz | This requirement does not apply to BS operating in band n2, n25 or band n70. |
| PCS1900 | 1850 – 1910 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n2 or n25 since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 869 – 894 MHz | -57 dBm | 100 kHz | This requirement does not apply to BS operating in band n5 or n26. |
| GSM850 or CDMA850 | 824 – 849 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n5 or n26, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band I or | 2110 – 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65 |
| E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band II or | 1930 – 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2 or n70. |
| E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band III or | 1805 – 1880 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n3. |
| E-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band IV or | 2110 – 2155 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66 |
| E-UTRA Band 4 | 1710 – 1755 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band V or | 869 – 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26. |
| E-UTRA Band 5 or NR Band n5 | 824 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band VI, XIX or | 860 – 890 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n18. |
| E-UTRA Band 6, 18, 19 or NR Band n18 | 815 – 830 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n18, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 830 – 845 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD Band VII or | 2620 – 2690 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n7. |
| E-UTRA Band 7 or NR Band n7 | 2500 – 2570 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n7, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band VIII or | 925 – 960 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n8 or n100. |
| E-UTRA Band 8 or NR Band n8 | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band IX or | 1844.9 – 1879.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n3. |
| E-UTRA Band 9 | 1749.9 – 1784.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band X or | 2110 – 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66 |
| E-UTRA Band 10 | 1710 – 1770 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XI or XXI or | 1475.9 – 1510.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92 or n94. |
| E-UTRA Band 11 or 21 | 1427.9 – 1447.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
|  | 1447.9 – 1462.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92 or n94. |
| UTRA FDD Band XII or | 729 – 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n12 or n85. |
| E-UTRA Band 12 or NR Band n12 | 699 – 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n12 or n85, since it is already covered by the requirement in clause 6.6.5.2.2.  For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XIII or | 746 – 756 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n13. |
| E-UTRA Band 13 or NR Band n13 | 777 – 787 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n13, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XIV or | 758 – 768 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n14. |
| E-UTRA Band 14 or NR band n14 | 788 – 798 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n14, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 734 – 746 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 17 | 704 – 716 MHz | -49 dBm | 1 MHz | For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XX or | 791 – 821 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n20 or n28. |
| E-UTRA Band 20 or NR Band n2 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XXII | 3510 – 3590 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n48, n77 or n78. |
| or E-UTRA Band 22 | 3410 – 3490 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n77 or n78. |
|  | 1525 – 1559 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n24. |
| E-UTRA Band 24 or NR Band n24 | 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n24, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XXV or | 1930 – 1995 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, n25 or n70. |
| E-UTRA Band 25 or NR band n25 | 1850 – 1915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n25 since it is already covered by the requirement in clause 6.6.5.2.2. For BS operating in Band n2, it applies for 1910 MHz to 1915 MHz, while the rest is covered in clause 6.6.5.2.2. |
| UTRA FDD Band XXVI or | 859 – 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26. |
| E-UTRA Band 26 or NR Band n26 | 814 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n26 since it is already covered by the requirement in clause 6.6.5.2.2. For BS operating in Band n5, it applies for 814 MHz to 824 MHz, while the rest is covered in clause 6.6.5.2.2. |
|  | 852 – 869 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n5. |
| E-UTRA Band 27 | 807 – 824 MHz | -49 dBm | 1 MHz | This requirement also applies to BS operating in Band n28, starting 4 MHz above the Band n28 downlink *operating band* (Note 5). |
| E-UTRA Band 28 or | 758 – 803 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, n67 or n28. |
| NR Band n28 | 703 – 748 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n28, since it is already covered by the requirement in clause 6.6.5.2.2.  For BS operating in band n67, it applies for 703 MHz to 736 MHz. |
| E-UTRA Band 29 or NR Band n29 | 717 – 728 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n29 or n85 |
| E-UTRA Band 30 or | 2350 – 2360 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n30 |
| NR Band n30 | 2305 – 2315 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n30, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 462.5 – 467.5 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 31 | 452.5 – 457.5 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD band XXXII or E-UTRA band 32 | 1452 – 1496 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92 or n94. |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n34. |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n2 or n25. |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n38. |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n39. |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n41, n53 or [n90]. |
| E-UTRA Band 42 | 3400 – 3600 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 44 | 703 – 803 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n28. |
| E-UTRA Band 45 | 1447 – 1467 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 46 or NR Band n46 | 5150 – 5925 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n46, n96 or n102. |
| E-UTRA Band 47 | 5855 – 5925 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 50 or NR band n50 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 53 or NR Band n53 | 2483.5 - 2495 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n41, n53 or n90. |
| E-UTRA Band 65 or | 2110 – 2200 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65. |
| NR Band n65 | 1920 – 2010 MHz | -49 dBm | 1 MHz | For BS operating in Band n1, it applies for 1980 MHz to 2010 MHz, while the rest is covered in clause 6.6.5.2.2.  This requirement does not apply to BS operating in band n65, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 66 or | 2110 – 2200 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66. |
| NR Band n66 | 1710 – 1780 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 67 or NR Band n67 | 738 – 758 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n28 or n67. |
| E-UTRA Band 68 | 753 -783 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n28. |
|  | 698-728 MHz | -49 dBm | 1 MHz | For BS operating in Band n28, this requirement applies between 698 MHz and 703 MHz, while the rest is covered in clause 6.6.5.2.2. |
| E-UTRA Band 69 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n38. |
| E-UTRA Band 70 or | 1995 – 2020 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, n25 or n70 |
| NR Band n70 | 1695 – 1710 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n70, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 71 or | 617 – 652 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n71 or [n105] |
| NR Band n71 | 663 – 698 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n71 or [n105], since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 461 – 466 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 72 | 451 – 456 MHz | -49 dBm | 1 MHz |  |
| E-UTRA Band 74 | 1475 – 1518 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92 or n94. |
| or NR Band n74 | 1427 – 1470 MHz | -49 dBm | 1MHz | This requirement does not apply to BS operating in band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 75 or NR Band n75 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 76 or NR Band n76 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75, n76, n91, n92, n93 or n94. |
| NR Band n77 | 3.3 – 4.2 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n79 |
| NR Band n80 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n81 | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n82 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n83 | 703 – 748 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n28, since it is already covered by the requirement in clause 6.6.5.2.2.  For BS operating in Band n67, it applies for 703 MHz to 736 MHz. |
| NR Band n84 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n1, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 85 or NR Band n85 | 728 – 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n12 or n85.  For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
|  | 698 – 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n12 or n85, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n86 | 1710 – 1780 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n89 | 824 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n5, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75 or n76. |
| NR Band n91 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75 or n76. |
| NR Band n92 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75 or n76. |
| NR Band n93 | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75 or n76. |
| NR Band n94 | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n95 | 2010 – 2025 MHz | -52 dBm | 1 MHz |  |
| NR Band n96 | 5925 – 7125 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n46, n96, n102 or n104. |
| NR Band n97 | 2300 – 2400MHz | -52 dBm | 1 MHz |  |
| NR Band n98 | 1880 – 1920MHz | -52 dBm | 1 MHz |  |
| NR Band n99 | 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n24, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR band n100 | 919.4 – 925 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n8 or n100. |
|  | 874.4 – 880 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n100, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR band n101 | 1900 – 1910 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n101. |
| NR Band n102 | 5925 – 6425 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n46, n96, n102 or n104. |
| E-UTRA Band 103 | 757 – 758 MHz | -52 dBm | 1 MHz |  |
|  | 787 – 788 MHz | -49 dBm | 1 MHz |  |
| NR Band n104 | 6425 – 7125 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n96, n102 or n104 |
| NR Band [n105] | 612 – 652 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n71 or [n105] |
|  | 663 – 703 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n71 or [n105], since it is already covered by the requirement in clause 6.6.5.2.2. |

##### 6.6.5.2.4 Co-location with other base stations

These requirements may be applied for the protection of other BS receivers when GSM900, DCS1800, PCS1900, GSM850, CDMA850, UTRA FDD, UTRA TDD, E-UTRA and/or NR BS are co-located with a BS.

The requirements assume a 30 dB coupling loss between transmitter and receiver and are based on co-location with base stations of the same class.

The *basic limits* are in table 6.6.5.2.4-1 for a BS where requirements for co-location with a BS type listed in the first column apply, depending on the declared Base Station class. For a *multi-band connector*, the exclusions and conditions in the Note column of table 6.6.5.2.4-1 shall apply for each supported *operating band*.

Table 6.6.5.2.4-1: BS spurious emissions *basic* limits for BS co-located with another BS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Type of co-located BS | Frequency range for | *Basic limits* | | | Measurement | Note |
|  | co-location requirement | WA BS | MR BS | LA BS | bandwidth |  |
| GSM900 | 876 – 915 MHz | -98 dBm | -91 dBm | -70 dBm | 100 kHz |  |
| DCS1800 | 1710 – 1785 MHz | -98 dBm | -91 dBm | -80 dBm | 100 kHz |  |
| PCS1900 | 1850 – 1910 MHz | -98 dBm | -91 dBm | -80 dBm | 100 kHz |  |
| GSM850 or CDMA850 | 824 – 849 MHz | -98 dBm | -91 dBm | -70 dBm | 100 kHz |  |
| UTRA FDD Band I or E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band II or E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band III or E-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band IV or E-UTRA Band 4 | 1710 – 1755 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band V or E-UTRA Band 5 or NR Band n5 | 824 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VI, XIX or E-UTRA Band 6, 19 | 830 – 845 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VII or E-UTRA Band 7 or NR Band n7 | 2500 – 2570 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VIII or E-UTRA Band 8 or NR Band n8 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band IX or E-UTRA Band 9 | 1749.9 – 1784.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band X or E-UTRA Band 10 | 1710 – 1770 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XI or E-UTRA Band 11 | 1427.9 –1447.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n75, n91, n92, n93 or n94 |
| UTRA FDD Band XII or  E-UTRA Band 12 or NR Band n12 | 699 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XIII or  E-UTRA Band 13 or NR Band n13 | 777 – 787 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XIV or  E-UTRA Band 14 or NR Band n14 | 788 – 798 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 17 | 704 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 18 or NR Band n18 | 815 – 830 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XX or E-UTRA Band 20 or NR Band n20 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXI or E-UTRA Band 21 | 1447.9 – 1462.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n75, n92 or n94 |
| UTRA FDD Band XXII or E-UTRA Band 22 | 3410 – 3490 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 24 or NR Band n24 | 1626.5 – 1660.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXV or  E-UTRA Band 25 or NR Band n25 | 1850 – 1915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXVI or  E-UTRA Band 26 or NR Band n26 | 814 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 27 | 807 – 824 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 28 or NR Band n28 | 703 – 748 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 30 or NR Band n30 | 2305 – 2315 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 31 | 452.5 – 457.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n34 |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n2 or band n25 |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n38. |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n39 |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n41, n53 or [n90] |
| E-UTRA Band 42 | 3400 – 3600 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 43 | 3600 – 3800 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 44 | 703 – 803 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n28 |
| E-UTRA Band 45 | 1447 – 1467 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 46 or NR Band n46 | 5150 – 5925 MHz | N/A | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n46, n96 or n102 |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 50 or NR Band n50 | 1432 – 1517 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n51, n74, n75, n91, n92, n93 or n94 |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | N/A | N/A | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n74, n75, n76, n91, n92, n93 or n94 |
| E-UTRA Band 53 or NR Band n53 | 2483.5 – 2495 MHz | N/A | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n41, n53 or n90 |
| E-UTRA Band 65 or NR Band n65 | 1920 – 2010 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 66 or NR Band n66 | 1710 – 1780 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 68 | 698 – 728 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 70 or NR Band n70 | 1695 – 1710 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 71 or NR Band n71 | 663 – 698 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This requirement does not apply to BS operating in Band n71 or [n105]. |
| E-UTRA Band 72 | 451 – 456 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 74 or NR Band n74 | 1427 – 1470 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n51, n91, n92, n93 or n94 |
| NR Band n77 | 3.3 – 4.2 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n80 | 1710 – 1785 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n81 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n82 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n83 | 703 – 748 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n84 | 1920 – 1980 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 85 or NR Band 85 | 698 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n86 | 1710 – 1780 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n89 | 824 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n91 | 832 – 862 MHz | N/A | N/A | -88 dBm | 100 kHz |  |
| NR Band n92 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n93 | 880 – 915 MHz | N/A | N/A | -88 dBm | 100 kHz |  |
| NR Band n94 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n95 | 2010 – 2025 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n96 | 5925 – 7125 MHz | N/A | -90 dBm | -87 dBm | 100 kHz | This is not applicable to BS operating in Band n46,  n96, n102 or n104 |
| NR Band n97 | 2300 – 2400MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n98 | 1880 – 1920MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n99 | 1626.5 – 1660.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n100 | 874.4 – 880 MHz | -96 dBm | NA | NA | 100 kHz |  |
| NR Band n101 | 1900 – 1910 MHz | -96 dBm | NA | NA | 100 kHz |  |
| NR Band n102 | 5925 – 6425 MHz | N/A | -90 dBm | -87 dBm | 100 kHz | This is not applicable to BS operating in Band n46, n96, n102 or n104 |
| E-UTRA Band 103 | 787 – 788 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n104 | 6425 – 7125 MHz | -95 dBm | -90 dBm | -87 dBm | 100 kHz | This requirement does not apply to BS operating in Band n96, n102 or n104. |
| NR Band [n105] | 663 – 703 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This requirement does not apply to BS operating in Band n71 or [n105]. |

NOTE 1: As defined in the scope for spurious emissions in this clause, the co-location requirements in table 6.6.5.2.4-1 do not apply for the frequency range extending ΔfOBUE immediately outside the BS transmit frequency range of a downlink *operating band* (see table 5.2-1). The current state-of-the-art technology does not allow a single generic solution for co-location with other system on adjacent frequencies for 30dB BS-BS minimum coupling loss. However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [4].

NOTE 2: Table 6.6.5.2.4-1 assumes that two *operating bands*, where the corresponding BS transmit and receive frequency ranges in table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-location requirements may apply that are not covered by the 3GPP specifications.

NOTE 3: Co-located TDD base stations that are synchronized and using the same or adjacent *operating band* can transmit without special co-locations requirements. For unsynchronized base stations, special co-location requirements may apply that are not covered by the 3GPP specifications.

#### < End OF CHANGE>