**3GPP TSG-RAN WG4 Meeting #104-e *R4-220xxxx***

**E-Meeting, 15 Aug. – 26 Aug., 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **36.133** | **CR** |  | **rev** |  | **Current version:** | **15.17.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | R4-22xxxxx Big CR for 36.133 maintenance (Rel-15) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | MCC, Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI 14, NR\_newRAT-Core | | | | |  | ***Date:*** | | | 2022-08-30 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Big CR to merge the multiple endorsed draft CRs in RAN4#104-e. List of draft CRs merged are   * R4- 2211602 CR: Corrections on LTE V2X Synchronization Reference Selection/Reselection Tests   + The syncOffsetIndicators of SyncRef UE 1 and SyncRef UE 2 are different and therefore they can’t be the interference of each other as they are not overlapping in time domain. Without interference, Es/Noc and Es/Iot are the same. * R4-2214702 Correction to NR SCell interruption requirements 36.133\_r15   + During last 2 RAN4 meetings, interruption length for SSB-less SCell and SCell without SMTC configuration were discussed. For a SCell which actually transmits SSB but has no SMTC configuration, it’s agreed that the SMTC duration for this SCell shall be assumed as [X] ms, where X is TBD.   During discussion we received comments that X may be less than 5ms. The main reason is that for a SCell transmitting SSB, its SSB time domain pattern can be explicitly obtained from ssb-PositionsInBurst. Then the length of assumed SMTC duration can be reduced.  We suggest x = number of consecutive subframes which contains all SSBs indicated by ssb-PositionsInBurst. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The summary of change in each endorsed draft CRs are copied below.   * R4- 2211602 CR: Corrections on LTE V2X Synchronization Reference Selection/Reselection Tests   In T3, for SyncRef UE 1:  Es/Iot = Es/Noc = 0dB  and for SyncRef UE 2:  Es/Iot = Es/Noc = 3dB   * R4-2214702 Correction to NR SCell interruption requirements 36.133\_r15   + Interruption requirements for SCell addition/ activation are updated | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | * R4- 2211602 CR: Corrections on LTE V2X Synchronization Reference Selection/Reselection Tests   + Es/Iot specified in the test configuration is incorrect. * R4-2214702 Correction to NR SCell interruption requirements 36.133\_r15   + Requirements are not clear | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | * R4- 2211602 CR: Corrections on LTE V2X Synchronization Reference Selection/Reselection Tests   + A.12.3 * R4-2214702 Correction to NR SCell interruption requirements 36.133\_r15   + 7.32.2.4, 7.32.2.5, 7.36.2.3, 7.36.2.4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 36.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
|  |

<Start of Change 1>

## A.12.3 V2X Synchronization Reference Selection/Reselection Tests

### A.12.3.1 V2X Synchronization Reference Selection/Reselection Tests for GNSS configured as the highest priority

#### A.12.3.1.1 Test Purpose and Environment

The purpose of this test is to verify the requirements related to SyncRef UE selection / reselection defined in clause 13.4, when GNSS is configured as the highest priority. For this test, the UE is triggered by the test loop function or the upper layers to transmit for V2X Sidelink Communication.

The test parameters are given in Table A.12.3.1.1-1and A.12.3.1.1-2 below. There are no GNSS signals in this test. There are one active cell (PCell) and two active SyncRef UEs (SyncRef UE 1 and SyncRef UE 2) in this test. The test system shall emulate SyncRef UE 1 and SyncRef UE 2 to transmit SLSS and MIB-SL every SLSS period.

The test system can verify the selection / reselection of SyncRef UE by monitoring the SLSS ID used by the V2X UE for its SLSS+MIB-SL transmissions. When the V2X UE is not synchronized to any SyncRef UE, then the V2X UE shall use the SLSS ID pre-configured in the V2X UE. When the V2X UE is synchronized to a SyncRef UE, the V2X UE shall derive its SLSS ID from the SLSS ID of the SyncRef UE as per clause 5.10.7.3 of TS 36.331.

The test consists of three successive time periods, with time duration of T1, T2 and T3 respectively. During T1, both SyncRef UE 1 and SyncRef UE 2 are powered off and the V2X UE will select PCell as synchronization source. During T2, SyncRef UE 1 is powered ON and the V2X UE will select SyncRef UE 1 as the synchronization source. During T3, a higher priority SyncRef UE 2 is additionally powered ON and the V2X UE will reselect to the higher priority SyncRef UE 2 as the synchronization source.

Table A.12.3.1.1-1: Test Parameters for V2X Synchronization Reference Selection/Reselection Tests for GNSS configured as the highest priority

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | Unit | Value | Comment |
| Initial condition | Active synchronization source |  | Cell 1 | UE transmits for V2X Sidelink Communication and SLSS+MIB-SL with SLSS ID = 30 and in-coverage set as TRUE in MIB-SL. |
| T2 end condition | Active synchronization source |  | Sync Ref UE 1 | UE transmits for V2X Sidelink Communication and SLSS+MIB-SL with SLSS ID = 168 and in-coverage set as FALSE in MIB-SL. |
| Final condition | Active synchronization source |  | Sync Ref UE 2 | UE transmits for V2X Sidelink Communication and SLSS+MIB-SL with SLSS ID = 0 and in-coverage set as FALSE in MIB-SL. |
| Active SyncRef UEs | |  | SyncRef UE 1  SyncRef UE 2 | Transmitting SLSS+MIB-SL on RF channel number 1 (TDD carrier in Band 47) |
| Active cell | |  | Cell 1 | E-UTRA FDD Cell 1 on RF channel number 2 |
| Timing offset between SyncRef UE 1 and SyncRef UE 2 | | μs | 3 | Synchronous |
| Frequency offset of SyncRef UE 1 | | ppm | 0 |  |
| Frequency offset of SyncRef UE 2 | | ppm | 0 |  |
| V2X sidelink Communication configuration | |  | As specified in Table A.3.24.2-2  (Configuration #2) | IE values unless specified otherwise in this test. |
| typeTxSync | |  | *gnss* |  |
| slssid | |  | *30* |  |
| syncTxThreshIC | |  | +infinity |  |
| T1 | | s | 24 |  |
| T2 | | s | 16 |  |
| T3 | | s | 3.2 |  |

Table A.12.3.1.1-2: SyncRef UE Specific Test Parameters for V2X Synchronization Reference Selection/Reselection Tests for GNSS configured as the highest priority

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | SyncRef UE 1 | | | SyncRef UE 2 | | |
| T1 | T2 | T3 | T1 | T2 | T3 |
| E-UTRA RF Channel Number |  | 1 | | | | | |
| BWchannel Note 4 | MHz | 5 or 10 | | | | | |
| V2X Sidelink Communication resource pool configuration |  | As specified in Table A.3.24.2-1  (Configuration #1) | | | As specified in Table A.3.24.2-2  (Configuration #2) | | |
| networkControlledSyncTx |  | N/A | | | ON | | |
| syncTxThreshOoC | dBm/15 kHz | +infinity | | | N/A | | |
| slssid |  | 0 | | | 0 | | |
| inCoverage (in MIB-SL) |  | FALSE | | | TRUE | | |
| syncOffsetIndicator |  | syncOffsetIndicator2 | | | syncOffsetIndicator1 | | |
| Note1 | dBm/15 kHz | -95 | | | | | |
|  | dB | -infinity | 0 | 0 | -infinity | -infinity | 3 |
|  | dB | -infinity | 0 | 0 | -infinity | -infinity | 3 |
| S-RSRP Note2, Note 3 | dBm/15 kHz | -infinity | -95 | -95 | -infinity | -infinity | -92 |
| Propagation Condition |  | AWGN | | | | | |
| Note 1: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 2: S-RSRP levels have been derived from other parameters for information purposes. They are not settable parameters themselves.  Note 3: SSSS Es/Iot is set the same as PSSS/PSBCH Es/Iot. | | | | | | | |

Table A.12.3.1.1-3: Cell Test Parameters for V2X Synchronization Reference Selection/Reselection Tests for GNSS configured as the highest priority

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Cell 1 | | |
| T1 | T2 | T3 |
| E-UTRA RF Channel Number |  | 2 | | |
| BWchannel | MHz | 10 | | |
| PDCCH/PCFICH/PHICH Reference measurement channel defined in A.3.1.2.1 |  | R.6 FDD | | |
| OCNG Patterns defined in A.3.2.1.2 |  | OP.2 FDD | | |
| PBCH\_RA | dB | 0 | | |
| PBCH\_RB |
| PSS\_RA |
| SSS\_RA |
| PCFICH\_RB |
| PHICH\_RA |
| PHICH\_RB |
| PDCCH\_RA |
| PDCCH\_RB |
| PDSCH\_RA |
| PDSCH\_RB |
| OCNG\_RANote 1 |
| OCNG\_RBNote 1 |
| Note2 | dBm/15 kHz | -95 | | |
|  | dB | 4.5 | 4.5 | 4.5 |
| RSRP Note3 | dBm/15 kHz | -90.5 | -90.5 | -90.5 |
| SCH\_RP Note 3 | dBm/15 kHz | -90.5 | -90.5 | -90.5 |
| Propagation Condition |  | AWGN | | |
| Note 1: OCNG shall be used such that cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.  Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 3: RSRP and SCH\_RP levels have been derived from other parameters for information purposes. They are not settable parameters themselves. | | | | |

#### A.12.3.1.2 Test Requirements

1) During T2, SyncRef UE selection delay is defined as the time from the beginning of T2 to the time UE is synchronized to SyncRef UE 1 and changes its SLSS transmissions timing and SLSS ID to follow SyncRef UE 1 as the synchronization source. For the test configuration, the SLSS ID will be changed to 168 (with in-coverage IE in MIB-SL set to FALSE) after SyncRef UE selection delay from start of T2.

The SyncRef UE selection delay shall be less than 8.8sec. The SyncRef UE selection/reselection delay can be expressed as:

SyncRef UE selection/reselection delay = Tdetect,SyncRef UE + Tevaluate,SLSS + SLSS period

Where

- Tdetect,SyncRef UE = 8sec (as specified in sub-clause 13.4)

- Tevaluate,SLSS = 0.64 (as specified in sub-clause 13.3.1.3)

- SLSS period = 160ms

This gives a total of 8.8seconds.

2) During T3, SyncRef UE reselection delay is defined as the time from the beginning of T3 to the time UE changes its synchronization source from SyncRef UE 1 to SyncRef UE 2, and changes its SLSS transmissions timing and SLSS ID to follow SyncRef UE 2 as the synchronization source. For the test configuration, the SLSS ID will still be 0 (with in-coverage IE in MIB-SL set to FALSE) after SyncRef UE selection delay from start of T3.

The SyncRef UE reselection delay shall be less than 2.4sec. The SyncRef UE selection/reselection delay can be expressed as:

SyncRef UE selection/reselection delay = Tdetect,SyncRef UE + Tevaluate,SLSS + SLSS period

Where

- Tdetect,SyncRef UE = 1.6sec (as specified in sub-clause 13.4)

- Tevaluate,SLSS = 0.64 (as specified in sub-clause 13.3.1.3)

- SLSS period = 160ms

This gives a total of 2.4seconds.

The test system will verify that the V2X UE does not drop or delay more than 6% of its V2X data and SLSS transmissions during the duration of T2, and does not drop or delay more than 30% of its SLSS transmissions during the duration of T3.

The rate of correct SyncRef UE selection / reselection observed during repeated tests shall be at least 90%.

### A.12.3.2 V2X Synchronization Reference Selection/Reselection Tests for eNB configured as the highest priority

#### A.12.3.2.1 Test Purpose and Environment

The purpose of this test is to verify the requirements related to SyncRef UE selection / reselection defined in clause 13.4, when eNB is configured as the highest priority. For this test, the UE is triggered by the test loop function or the upper layers to transmit for V2X Sidelink Communication.

The test parameters are given in Table A.12.3.2.1-1and A.12.3.2.1-2 below. There are no active cells and GNSS is reliable during the whole test. The test system can emulate and send the GNSS signal to the test UE. The test parameters for GNSS signals are defined in B.6.1. There are two active SyncRef UEs (SyncRef UE 1 and SyncRef UE 2) in this test. The test system shall emulate SyncRef UE 1 and SyncRef UE 2 to transmit SLSS and MIB-SL every SLSS period.

The test system can verify the selection / reselection of SyncRef UE by monitoring the SLSS ID used by the V2X UE for its SLSS+MIB-SL transmissions. When the V2X UE is not synchronized to any SyncRef UE, then the V2X UE shall use the SLSS ID pre-configured in the V2X UE. When the V2X UE is synchronized to a SyncRef UE, the V2X UE shall derive its SLSS ID from the SLSS ID of the SyncRef UE as per clause 5.10.7.3 of TS 36.331.

The test consists of three successive time periods, with time duration of T1, T2 and T3 respectively. During T1, both SyncRef UE 1 and SyncRef UE 2 are powered off and the V2X UE will select GNSS as synchronization source. During T2, SyncRef UE 1 is powered ON and the V2X UE will select SyncRef UE 1 as the synchronization source. During T3, a higher priority SyncRef UE 2 is additionally powered ON and the V2X UE will reselect to the higher priority SyncRef UE 2 as the synchronization source.

Table A.12.3.2.1-1: Test Parameters for V2X Synchronization Reference Selection/Reselection Tests for eNB configured as the highest priority

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | Unit | Value | Comment |
| Initial condition | Active synchronization source |  | GNSS | UE transmits for V2X Sidelink Communication and SLSS+MIB-SL with SLSS ID = 0 and in-coverage set as TRUE in MIB-SL. |
| T2 end condition | Active synchronization source |  | Sync Ref UE 1 | UE transmits for V2X Sidelink Communication and SLSS+MIB-SL with SLSS ID = 168+59 and in-coverage set as FALSE in MIB-SL. |
| Final condition | Active synchronization source |  | Sync Ref UE 2 | UE transmits for V2X Sidelink Communication and SLSS+MIB-SL with SLSS ID = 30 and in-coverage set as FALSE in MIB-SL. |
| Active cell | |  | None |  |
| Active SyncRef UEs | |  | SyncRef UE 1  SyncRef UE 2 | Transmitting SLSS+MIB-SL on RF channel number 1 |
| Timing offset between SyncRef UE 1 and SyncRef UE 2 | | ms | 3 | Asynchronous |
| Frequency offset of SyncRef UE 1 | | ppm | 0 |  |
| Frequency offset of SyncRef UE 2 | | ppm | 5 |  |
| V2X sidelink Communication preconfiguration | |  | As specified in Table A.3.24.2-1  (Configuration #1) | IE values unless specified otherwise in this test. |
| syncPriority | |  | *enb* |  |
| syncTxThreshOoC | |  | 11 (+infinity) |  |
| T1 | | s | 24 |  |
| T2 | | s | 16 |  |
| T3 | | s | 16 |  |

Table A.12.3.2.1-2: SyncRef UE Specific Test Parameters for V2X Synchronization Reference Selection/Reselection Tests for eNB configured as the highest priority

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Unit | SyncRef UE 1 | | | SyncRef UE 2 | | |
| T1 | T2 | T3 | T1 | T2 | T3 |
| E-UTRA RF Channel Number |  | 1 | | | | | |
| BWchannel | MHz | 5 or 10 | | | | | |
| V2X Sidelink Communication resource pool configuration |  | As specified in Table A.3.24.2-1  (Configuration #1) | | | As specified in Table A.3.24.2-2  (Configuration #2) | | |
| networkControlledSyncTx |  | N/A | | | ON | | |
| syncTxThreshOoC | dBm/15 kHz | +infinity | | | N/A | | |
| slssid |  | 59 | | | 30 | | |
| inCoverage (in MIB-SL) |  | FALSE | | | TRUE | | |
| syncOffsetIndicator |  | syncOffsetIndicator2 | | | syncOffsetIndicator1 | | |
| Note1 | dBm/15 kHz | -95 | | | | | |
|  | dB | -infinity | 0 | 0 | -infinity | -infinity | 3 |
|  | dB | -infinity | 0 | 0 | -infinity | -infinity | 3 |
| S-RSRP Note2, Note 3 | dBm/15 kHz | -infinity | -95 | -95 | -infinity | -infinity | -92 |
| Propagation Condition |  | AWGN | | | | | |
| Note 1: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.  Note 2: S-RSRP levels have been derived from other parameters for information purposes. They are not settable parameters themselves.  Note 3: SSSS Es/Iot is set the same as PSSS/PSBCH Es/Iot. | | | | | | | |

#### A.12.3.1.2 Test Requirements

1) During T2, SyncRef UE selection delay is defined as the time from the beginning of T2 to the time UE is synchronized to SyncRef UE 1 and changes its SLSS transmissions timing and SLSS ID to follow SyncRef UE 1 as the synchronization source. For the test configuration, the SLSS ID will be changed to 168+59 (with in-coverage IE in MIB-SL set to FALSE) after SyncRef UE selection delay from start of T2.

The SyncRef UE selection delay shall be less than 8.8sec. The SyncRef UE selection/reselection delay can be expressed as:

SyncRef UE selection/reselection delay = Tdetect,SyncRef UE + Tevaluate,SLSS + SLSS period

Where

- Tdetect,SyncRef UE = 8sec (as specified in sub-clause 11.4)

- Tevaluate,SLSS = 0.64 (as specified in sub-clause 13.3.1.3)

- SLSS period = 160ms

This gives a total of 8.8 seconds.

2) During T3, SyncRef UE reselection delay is defined as the time from the beginning of T3 to the time UE changes its synchronization source from SyncRef UE 1 to SyncRef UE 2, and changes its SLSS transmissions timing and SLSS ID to follow SyncRef UE 2 as the synchronization source. For the test configuration, the SLSS ID will be changed o 30 (with in-coverage IE in MIB-SL set to FALSE) after SyncRef UE selection delay from start of T3.

The SyncRef UE reselection delay shall be less than 8.8sec. The SyncRef UE selection/reselection delay can be expressed as:

SyncRef UE selection/reselection delay = Tdetect,SyncRef UE + Tevaluate,SLSS + SLSS period

Where

- Tdetect,SyncRef UE = 8sec (as specified in sub-clause 11.4)

- Tevaluate,SLSS = 0.64 (as specified in sub-clause 13.3.1.3)

- SLSS period = 160ms

This gives a total of 8.8 seconds.

The test system will verify that the V2X UE does not drop or delay more than 6% of its V2X data and SLSS transmissions during the duration of T2 and T3.

The rate of correct SyncRef UE selection / reselection observed during repeated tests shall be at least 90%.

<End of Change 1>

<Start of Change 2>

### 7.32.2.4 Interruptions at SCell addition/release

When one SCell belonging to MCG is added or released:

- the requirements in clause 7.8.2.7 shall apply.

When one NR SCell belonging to SCG is added or released:

- an interruption on PCell or activated SCell in MCG shall not exceed X1 subframes for synchronous intraband EN-DC, X1+1 subframes for asynchronous intraband EN-DC, 1 subframe for synchronous interband EN-DC or 2 subframes for asynchronous interband EN-DC. For SCell addition X1 is equal to the duration of the SMTC of the SCell being added + 1 ms. If SSB configuration (*absoluteFrequencySSB*) but no SMTC configuration is provided for the SCell being added, the SSB transmission periodicity is assumed to be 5ms and TSMTC duration for the SCell being added is x ms, where x = the number of consecutive subframes containing all SSBs in one SSB burst transmitted by the SCell being added. If no SSB configuration (*absoluteFrequencySSB*) nor SMTC configuration is provided for the SCell being added, TSMTC duration for the SCell being added is 0ms.

- The interruption is based on assumption that the cell specific reference signals from both cells are available in the same slot. For SCell release X1 is equal to 1ms.

### 7.32.2.5 Interruptions at SCell activation/deactivation

When one SCell belonging to MCG is activated or deactivated:

- the requirements in clause 7.8.2.8 shall apply.

When one NR SCell belonging to SCG is activated or deactivated

- an interruption on PCell or activated SCell in MCG shall not exceed X1 subframes for synchronous intraband EN-DC, X1+1 subframes for asynchronous intraband EN-DC, 1 subframe for synchronous interband EN-DC or 2 subframes for asynchronous interband EN-DC. For SCell activation X1 is equal to the duration of the SMTC of the SCell being activated + 1 ms. If SSB configuration (*absoluteFrequencySSB*) but no SMTC configuration is provided for the SCell being activated, the SSB transmission periodicity is assumed to be 5ms and TSMTC duration for the SCell being activated is x ms, where x = the number of consecutive subframes containing all SSBs in one SSB burst transmitted by the SCell being activated. If no SSB configuration (*absoluteFrequencySSB*) nor SMTC configuration is provided for the SCell being activated, TSMTC duration for the SCell being activated is 0ms.

- The interruption is based on assumption that the cell specific reference signals from both cells are available in the same slot. For SCell deactivation X1 is equal to 1ms.

<End of Change 2>

<Start of Change 3>

### 7.36.2.3 Interruptions at SCell addition/release

When one SCell belonging to SCG is added or released:

- the requirements in clause 7.8.2.7 shall apply.

When one NR SCell belonging to MCG is added or released:

- an interruption on PSCell or activated SCell in SCG shall not exceed X1 subframes for synchronous intraband NE-DC, X1+1 subframes for asynchronous intraband NE-DC, 1 subframe for synchronous interband NE-DC or 2 subframes for asynchronous interband NE-DC. For SCell addition X1 is equal to the duration of the SMTC of the SCell being added + 1 ms. If SSB configuration (*absoluteFrequencySSB*) but no SMTC configuration is provided for the SCell being added, the SSB transmission periodicity is assumed to be 5ms and TSMTC duration for the SCell being added is x ms, where x = the number of consecutive subframes containing all SSBs in one SSB burst transmitted by the SCell being added. If no SSB configuration (*absoluteFrequencySSB*) nor SMTC configuration is provided for the SCell being added, TSMTC duration for the SCell being added is 0ms.

- The interruption is based on assumption that the cell specific reference signals from both cells are available in the same slot. For SCell release X1 is equal to 1 ms.

### 7.36.2.4 Interruptions at SCell activation/deactivation

When one SCell belonging to SCG is activated or deactivated:

- the requirements in clause 7.8.2.8 shall apply.

When one NR SCell belonging to MCG is activated or deactivated

- an interruption on PSCell or activated SCell in SCG shall not exceed X1 subframes for synchronous intraband NE-DC, X1+1 subframes for asynchronous intraband NE-DC, 1 subframe for synchronous interband NE-DC or 2 subframes for asynchronous interband NE-DC. For SCell activation X1 is equal to the duration of the SMTC of the NR SCell being activated + 1 ms. If SSB configuration (*absoluteFrequencySSB*) but no SMTC configuration is provided for the SCell being activated, the SSB transmission periodicity is assumed to be 5ms and TSMTC duration for the SCell being activated is x ms, where x = the number of consecutive subframes containing all SSBs in one SSB burst transmitted by the SCell being activated. If no SSB configuration (*absoluteFrequencySSB*) nor SMTC configuration is provided for the SCell being activated, TSMTC duration for the SCell being activated is 0ms.

- The interruption is based on assumption that the cell specific reference signals from both cells are available in the same slot. For SCell deactivation X1 is equal to 1 ms.

<End of Change 3>