**3GPP TSG- Meeting #104-e**

**, - , 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Big CR for TS 38.101-4 Maintenance (Rel-15, CAT F) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This big CR merges endorsed draft CR to 38.101-4 in RAN4#104-e. The reason for change in endorsed draft CR is copied below   * R4-2211571   As per the agreement from last meeting, SIB1 shall only be scheduled during call setup to prevent collisions between SIB1 and PDSCH. This now needs to captured in the specification   * R4-2211582   In Table 6.2.3.2.2.2.3-1 aperiodic TriggeringOffeset is set to 0 although NZP CSI-RS is set to periodic. According to TS 38.331 aperiodicTriggeringOffset is the "offset X between the slot containing the DCI that triggers a set of aperiodic NZP CSI-RS resources". Hence, for periodic CSI-RS, aperiodicTriggeringOffset should be "not present.   * R4-2213077   The table headers for PBCH TDD demodulation requirements are wrong, as the referred channel name BPCH is wrong. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The summary of change in endorsed draft CR is copied as below:   * R4-2211571   Add statement on SIB1 scheduling to the Annex.   * R4-2211582:   aperiodicTriggeringOffset has been set to “Not Configured” in Table 6.2.3.2.2.2.3-1.  Editorial correction of incorrect table number.   * R4-2213077   The table headers for PBCH TDD demodulation requirements are corrected for 2 Rx (subclause 5.4.2.2) and for 4 Rx (subclause 5.4.3.2) to refer to SS/PBCH block index. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The consequences if not approved for endorsed draft CR are coppied as below.   * R4-2211571   SIB1 scheduling remains ambiguous.   * R4-2211582   The specification will remain incorrect   * R4-2213077   Incorrect table headers with a wrong channel name remain in specification for PBCH TDD performance requirements. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.4.2.2, 5.4.3.2, 6.2.3.2.2.2, Annex A.3.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **x** |  | Test specifications | | | | TS 38.521-4 | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

<Start Of Change R4-2213077>

## 5.4 PBCH demodulation requirements

#### **<< Unchanged sections omitted >>**

#### 5.4.2.2 TDD

Table 5.4.2.2-1: Test parameters for PBCH

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Single antenna port** |
| Physical Cell ID |  | 0 |
| Cyclic prefix |  | Normal |
| Number of SS/PBCH blocks within an SS burst set periodicity |  | 1 |
| SS/PBCH block index Note1 |  | 0 |
| SS/PBCH block periodicity | ms | 20 |
| TDD UL-DL pattern |  | FR1.30-1 |
| Note 1: as specified in clause 4.1 of TS 38.213 [11]  Note 2: as specified in clause 11.1 of TS 38.213 [11] | | |

For the parameters specified in Table 5.4.2.2-1 the average probability of a miss-detected PBCH (Pm-bch) shall be below the specified values in Table 5.4.2.2-2 in case SS/PBCH block index is not known and below the specified values in Table.5.4.2.2-3 in case SS/PBCH block index is known. The downlink physical setup is in accordance with Annex C.3.1.

Table 5.4.2.2-2: Minimum performance PBCH in case SS/PBCH block index is not known

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Test number** | **Bandwidth (MHz) / Subcarrier spacing (kHz)** | **Reference channel** | **Propagation condition** | **Antenna configuration and correlation matrix** | **Reference value** | |
| **Pm-bch (%)** | **SNR (dB)** |
| 1 | 40 / 30 | R.PBCH.2 | TDLA30-10 | 1 x 2 Low | 1 | -5.3 |

Table 5.4.2.2-3 Minimum performance PBCH in case SS/PBCH block index is known

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth (MHz) / Subcarrier spacing (kHz) | Reference channel | Propagation condition | Antenna configuration and correlation matrix | Reference value | |
| Pm-bch (%) | SNR (dB) |
| 1 | 40 / 30 | R.PBCH.2 | TDLA30-10 | 1 x 2 Low | 1 | -6.5 |

#### **<< Unchanged sections omitted >>**

#### 5.4.3.2 TDD

Table 5.4.3.2-1: Test parameters for PBCH

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Single antenna port |
| Physical Cell ID |  | 0 |
| Cyclic prefix |  | Normal |
| Number of SS/PBCH blocks within an SS burst set periodicity |  | 1 |
| SS/PBCH block index Note1 |  | 0 |
| SS/PBCH block periodicity | ms | 20 |
| TDD UL-DL pattern |  | FR1.30-1 |
| Note 1: as specified in clause 4.1 of TS 38.213 [11]  Note 2: as specified in clause 11.1 of TS 38.213 [11] | | |

For the parameters specified in Table 5.4.3.2-1 the average probability of a miss-detected PBCH (Pm-bch) shall be below the specified values in Table 5.4.3.2-2 in case SS/PBCH block index is not known and below the specified values in Table.5.4.3.2-3 in case SS/PBCH block index is known. The downlink physical setup is in accordance with Annex C.3.1.

Table 5.4.3.2-2: Minimum performance PBCH in case SS/PBCH block index is not known

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth (MHz) / Subcarrier spacing (kHz) | Reference channel | Propagation condition | Antenna configuration and correlation matrix | Reference value | |
| Pm-bch (%) | SNR (dB) |
| 1 | 40 / 30 | R.PBCH.2 | TDLA30-10 | 1 x 4 Low | 1 | -8.6 |

Table 5.4.3.2-3: Minimum performance PBCH in case SS/PBCH block index is known

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth (MHz) / Subcarrier spacing (kHz) | Reference channel | Propagation condition | Antenna configuration and correlation matrix | Reference value | |
| Pm-bch (%) | SNR (dB) |
| 1 | 40 / 30 | R.PBCH.2 | TDLA30-10 | 1 x 4 Low | 1 | -9.6 |

<End of Change R4-2213077>

<Start Of Change R4-2211582>

6.2.3.2.2.2 Minimum requirement for sub-band CQI reporting

The purpose of the requirements is to verify that the preferred sub-bands can be used for frequency-selective scheduling under the frequency-selective fading conditions.

The accuracy of sub-band channel CQI reporting under the frequency-selective fading conditions is determined by a double-sided percentile of the reported differential CQI offset level 0 per sub-band, and the relative increase of the throughput obtained when transmitting the transport format indicated by the corresponding reported sub-band CQI on a randomly selected sub-band among the sub-bands with the highest reported differential CQI offset level compared to the throughput when transmitting a fixed transport format according to the wideband CQI median on a randomly selected sub-band among all the sub-bands. To account for sensitivity of the input SNR the sub-band CQI reporting under frequency selective fading conditions is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.3.2.2.2-1 and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) A sub-band differential CQI offset level of 0 shall be reported at least α% of the time but less than β% of the time for each sub-band, where α and β are specified in Table 6.2.3.2.2.2-2;

b) The ratio of the throughput obtained when transmitting the corresponding transport format on a randomly selected sub-band among the sub-bands with the highest differential CQI offset level and that obtained when transmitting the transport format indicated by the reported wideband CQI median on a randomly selected sub-band among all the sub-bands shall be ≥ *γ*, where *γ* is specified in Table 6.2.3.2.2.2-2;

c) When transmitting the corresponding transport format on a randomly selected sub-band among the sub-bands with the highest differential CQI offset level, the average BLER for the indicated transport format shall be greater than or equal to 0.02.

The requirements only apply for sub-bands of full size and the random scheduling across the sub-bands is done by selecting a new sub-band in each available downlink transmission instance for TDD.

Table 6.2.3.2.2.2-1: Sub-band CQI reporting test under frequency-selective fading conditions

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Parameter** | | | **Unit** | **Test 1** | | **Test 2** | |
| Bandwidth | | | MHz | 40 | | | |
| Subcarrier spacing | | | kHz | 30 | | | |
| Duplex Mode | | |  | TDD | | | |
| TDD UL-DL pattern | | |  | FR1.30-1 | | | |
| SNR | | | dB | 5 | 6 | 11 | 12 |
| Propagation channel | | |  | Two tap model specified in Annex B.2.4 with *a*=1, *f*D = 5Hz, and τd=0.1125μs | | | |
| Antenna configuration | | |  | 2×4 | | | |
| Correlation configuration | | |  | As per Annex B.1 | | | |
| Beamforming Model | | |  | As specified in Annex B.4.1 | | | |
| ZP CSI-RS configuration | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 4 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 5, (4) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | 9 | | | |
| CSI-RS  periodicity and offset | | slot | 10/1 | | | |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 2 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 3,(6) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | 13 | | | |
| NZP CSI-RS-timeConfig  periodicity and offset | | slot | 10/1 | | | |
| CSI-IM configuration | CSI-IM resource Type | |  | Periodic | | | |
| CSI-IM RE pattern | |  | 0 | | | |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) | |  | (4, 9) | | | |
| CSI-IM timeConfig  periodicity and offset | | slot | 10/1 | | | |
| ReportConfigType | | |  | Aperiodic | | | |
| CQI-table | | |  | Table 2 | | | |
| reportQuantity | | |  | cri-RI-PMI-CQI | | | |
| timeRestrictionForChannelMeasurements | | |  | Not configured | | | |
| timeRestrictionForInterferenceMeasurements | | |  | Not configured | | | |
| cqi-FormatIndicator | | |  | Subband | | | |
| pmi-FormatIndicator | | |  | Wideband | | | |
| Sub-band Size | | | RB | 16 | | | |
| csi-ReportingBand | | |  | 1111111 | | | |
| CSI-Report periodicity and offset | | | slot | Not configured | | | |
| Aperiodic Report Slot Offset | | |  | 8 | | | |
| CSI request | | |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 | | | |
| reportTriggerSize | | |  | 1 | | | |
| CSI-AperiodicTriggerStateList | | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM | | | |
| aperiodicTriggeringOffset | | |  | Not configured | | | |
| Codebook configuration | | Codebook Type |  | typeI-SinglePanel | | | |
| Codebook Mode |  | 1 | | | |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured | | | |
| CodebookSubsetRestriction |  | 000001 | | | |
| RI Restriction |  | N/A | | | |
| Physical channel for CSI report | | |  | PUSCH | | | |
| CQI/RI/PMI delay | | | ms | 9.5 | | | |
| Maximum number of HARQ transmission | | |  | 1 | | | |
| Measurement channel | | |  | As specified in Table A.4-2, TBS.2-6 | | | |

Table 6.2.3.2.2.2-2: Minimum requirements

|  |  |  |
| --- | --- | --- |
| **Parameters** | **Test 1** | **Test 2** |
| *α* [%] | 2 | 2 |
| *β* [%] | 55 | 55 |
| ** | 1.05 | 1.05 |

<End of Change R4-2211582>

<Start Of Change R4-2211571>

# A.3 DL reference measurement channels

## A.3.1 General

The transport block size (TBS) determination procedure is described in clause 5.1.3.2 of TS 38.214 [12].

Unless otherwise stated, no user data is scheduled on slot #0 within 20 ms in order to avoid SSB and PDSCH transmissions in one slot and simplify test configuration.

Unless otherwise stated, SIB1 transmission shall only be scheduled during call setup to avoid SIB1 and PDSCH transmissions in the same slot.

<End of Change R4-2211571>