**3GPP TSG-RAN WG4 Meeting #108 R4-2313339**

**Toulouse, France, 21st August – 25th August 2023**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** |  | **rev** |  | **Current version:** | **18.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draft CR adding 3 bands CA configuration | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson, Telstra | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R18\_3BDL\_xBUL | | | | |  | ***Date:*** | | | 2023-08-11 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Adding new configuration | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding  CA\_n1A-n3B-n28A  CA\_n3B-n7A-n28A  CA\_n3B-n7B-n28A  CA\_n3B-n28A-n78A  CA\_n3B-n28A-n78(2A)  CA\_n7B-n28A-n78(2A) | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | New configuration are not added | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

Table 5.5A.3.2-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (three bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration  or single uplink carrier6 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n1A-n3A-n5A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n3A-n5A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7B | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3(2A)-n7A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3A-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3B-n7A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3B-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3(2A)-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3B-n7B | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3A-n8A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n18A | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n3A-n8A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n18 | 5, 10, 15 |  |
| CA\_n1A-n3A-n20A | CA\_n1A-n3A CA\_n1A-n20A CA\_n3A-n20A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n20 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n26A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n26(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3B-n26A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n1A-n3B-n26(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3A-n28A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 201, 301 |  |
| CA\_n1A-n3B-n28A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3B-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3A-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3B-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3(2A)-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3(2A)-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3A-n40A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n3A-n40A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n41A | n417  CA\_n1A-n3A  CA\_n1A-n41A  CA\_n3A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n67A | CA\_n1A-n3A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n75A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n77A | n777  CA\_n1A-n3A  CA\_n1A-n77A  CA\_n3A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n77(2A) | n777  CA\_n1A-n3A  CA\_n1A-n77A  CA\_n3A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n3A-n77(3A) | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n3A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n1A-n3A-n78A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n78A | CA\_n1A-n3A  CA\_n1A-n78A7  CA\_n3A-n78A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n78(2A) | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n78C | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3B-n78A | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n78(2A) | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n79A | CA\_n1A-n3A  CA\_n1A-n79A  CA\_n3A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3B-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3B-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3B-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3B-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3(2A)-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3(2A)-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3(2A)-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3(2A)-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3A-n105A | CA\_n1A-n3A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n5A-n7A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n5A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n5A-n7B | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n5A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n5A-n28A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n1A-n5A-n78A | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n1A-n7A-n8A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n26A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n26(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n7B-n26A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n7B-n26(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n7A-n38A10 | n1A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n7A-n38A10 | n1A | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n7A-n40A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n7A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n7A-n67A | CA\_n1A-n7A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n75A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n8A-n28A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n28 | 10, 15, 20 |  |
| CA\_n1A-n8A-n40A | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n8A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n8A-n77A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n8A-n77(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n7A-n28A | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n7B-n28A | CA\_n1A-n28A  CA\_n1A-n7A  CA\_n7A-n28A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n78A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901,100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 901, 100 |  |
|  | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7B-n78A | CA\_n1A-n78A  CA\_n1A-n7A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n1A-n7B-n78(2A) | CA\_n1A-n78A  CA\_n1A-n7A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n7A-n78(2A) | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A)  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n7A-n78C | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n8A-n78A | CA\_n1A-n8A  CA\_n1A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | - | n1 | 5, 10, 15, 20 | 1 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n8A-n78(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
| CA\_n1A-n8A-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n18A-n28A | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n18A-n28A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
| CA\_n1A-n18A-n41A | CA\_n1A-n18A  CA\_n1A-n41A  CA\_n18A-n41A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n77A | CA\_n1A-n18A  CA\_n1A-n77A  CA\_n18A-n77A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n77(2A) | CA\_n1A-n18A  CA\_n1A-n77A  CA\_n18A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n20A-n67A | CA\_n1A-n20A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n20A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n26A-n78A | CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n26(2A)-n78A | CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n26A-n78(2A) | CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n26(2A)-n78(2A) | CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n28A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n28A-n40A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40B | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | CA\_n40B\_BCS0 |  |
| CA\_n1A-n28A-n41A | n417  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n28A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n28A-n46A | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | 10, 20, 40, 60, 80 |  |
| CA\_n1A-n28A-n46C | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46C\_BCS0 |  |
| CA\_n1A-n28A-n46D | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46D\_BCS0 |  |
| CA\_n1A-n28A-n46(2A) | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
| CA\_n1A-n28A-n75A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n28A-n77A | n777  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n77(2A) | n777  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n28A-n77(3A) | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n1A-n28A-n78A | CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n78(2A) | CA\_n78(2A)  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n28A-n78C | CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n28A-n79A | CA\_n1A-n28A  CA\_n1A-n79A  CA\_n28A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n28A-n102A | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n28A-n102B | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n28A-n102C | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n28A-n102D | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n28A-n102E | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n28A-n102(2A) | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102 | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40A-n77A | CA\_n1A-n40A  CA\_n1A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40A-n77(2A) | CA\_n1A-n40A  CA\_n1A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n40A-n78A | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 2 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40B-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n40A-n105A | CA\_n1A-n40A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n41A-n77A | n417  n777  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n41A-n77(2A) | n417  n777  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n41A-n77(3A) | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n1A-n41A-n79A | CA\_n1A-n41A  CA\_n1A-n79A  CA\_n41A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n46A-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 10, 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46C-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46D-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46(2A)-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46A-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78(2A) | n46 | 10, 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46C-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78(2A) | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46D-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78(2A) | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46(2A)-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n67A-n78A | CA\_n1A-n78A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n67A-n78(2A) | CA\_n1A-n78A CA\_n78(2A) | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n75A-n78A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n77A-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n77(2A)-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n77(3A)-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n78A-n79A5 | CA\_n1A-n78A  CA\_n1A-n79A  CA\_n78A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n78(2A)-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n78A-n102A | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n78A-n102B | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n78A-n102C | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n78A-n102D | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n78A-n102E | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n78A-n102(2A) | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n78(2A)-n102A | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n78(2A)-n102B | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n78(2A)-n102C | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n78(2A)-n102D | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n78(2A)-n102E | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n78(2A)-n102(2A) | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n78A-n105A | CA\_n1A-n78A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n2A-n5A-n30A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n5A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n5A-n41A | CA\_n2A\_n5A  CA\_n2A\_n41A  CA\_n5A\_n41A | n2 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n2A-n5A-n48A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48B | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A  CA\_n48B | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n2A-n5A-n48(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
| CA\_n2A-n5A-n48(A-B) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
| CA\_n2(2A)-n5A-n30A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n5A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n5A-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n5A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n2A-n5A-n66(3A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n5A-n77A | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n77C | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7  CA\_n77C | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n5A-n77(2A) | n777  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n5A-n77A | n777  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n5A-n77(2A) | n777  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n7A-n12A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n12 | 5, 10, 15 |  |
| CA\_n2A-n7A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n12A-n30A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n12A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n12A-n30A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n12A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n12A-n41A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n2A-n12A-n66A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n12A-n66A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n12A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66(3A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n12A-n77A | n777  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n77A | n777  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n77(2A) | n777  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n77(2A) | n777  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n30A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n14A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n14A-n30A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n14A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n14A-n66A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n66A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66(3A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n14A-n77A | n777  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n77(2A) | n777  CA\_n2A-n14A CA\_n2A-n77A7 CA\_n14A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n14A-n77A | n777  CA\_n2A-n14A CA\_n2A-n77A7 CA\_n14A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n14A-n77(2A) | n777  CA\_n2A-n14A CA\_n2A-n77A7 CA\_n14A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A | CA\_n2A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n29A-n30A | CA\_n2A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n29A-n66A | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n29A-n66A | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n29A-n66(2A) | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n66(2A) | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n29A-n77A | n777  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n29A-n77A | n777  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n77(2A) | n777  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n77(2A) | n777  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2(2A)-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2(2A)-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n2A-n30A-n66(3A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n30A-n77A | n777  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n30A-n77(2A) | n777  CA\_n2A-n30A CA\_n2A-n77A7 CA\_n30A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n30A-n77A | n777  CA\_n2A-n30A CA\_n2A-n77A7 CA\_n30A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n30A-n77(2A) | n777  CA\_n2A-n30A CA\_n2A-n77A7 CA\_n30A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n48A-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48(A-B)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48B-n66A | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48(2A)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48A-n77A | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48A-n77C | n777,9  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n77C | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n48(2A)-n77C | CA\_n2A-n48A  CA\_n2A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n48B-n77C | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n48B-n77A | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48(2A)-n77A | CA\_n2A-n48A  CA\_n2A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n66A-n77A | n777, 9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n66A-n77A | n777  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66(2A)-n77A | n777  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n77C | n777, 9  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n66A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n66A-n77(2A) | n777  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n66(2A)-n77A | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n66(2A)-n77(2A) | n777  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n66A-n77(2A) | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66(2A)-n77(2A) | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66(3A)-n77A | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66(3A)-n77(2A) | n777  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66A-n78A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n78(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n2A-n71A-n78A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n71A-n78(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n5A-n7A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n3A-n5A-n7B | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n3A-n5A-n28A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n5A-n78A | CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n8A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20, 35 |  |
| CA\_n3A-n7A-n26A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n3A-n7A-n26(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3A-n7B-n26A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n3A-n7B-n26(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3B-n7A-n26A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n3B-n7A-n26(2A) | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3B-n7B-n26A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n3B-n7B-n26(2A) | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3A-n7A-n28A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3A-n7B-n28A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3B-n7A-n28A | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3B-n7B-n28A | CA\_n7B  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3A-n7A-n38A10 | n3A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3B-n7A-n38A10 | n3A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3(2A)-n7A-n38A10 | n3A | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3A-n7A-n67A | CA\_n3A-n7A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n3A-n7A-n75A | - | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n78A | - | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n3A-n7A-n78C | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n7B-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n3A-n7B-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7A-n78(2A) | CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n7A-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n7B-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7A-n79A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n79A | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3(2A)-n7A-n79A | - | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n8A-n28A | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20, 35 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n8A-n41A | CA\_n3A-n8A  CA\_n3A-n41A  CA\_n8A-n41A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n77A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n77(2A) | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n8A-n78A | CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n18A-n28A | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n18A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n28 | 5, 10 |
| CA\_n3A-n18A-n41A | CA\_n3A-n41A  CA\_n3A-n18A  CA\_n18A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |
| CA\_n3A-n18A-n77A | CA\_n3A-n18A  CA\_n3A-n77A  CA\_n18A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |
| CA\_n3A-n18A-n77(2A) | CA\_n3A-n18A  CA\_n3A-n77A  CA\_n18A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n20A-n67A | CA\_n3A-n20A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
| n20 | 5, 10, 15, 20 |
| n67 | 5, 10, 15, 20 |
| CA\_n3A-n20A-n28A | CA\_n3A-n20A  CA\_n3A-n28A  CA\_n20A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n20A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | n20 | 5, 10, 15, 20 |
|  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
| CA\_n3A-n26A-n78A | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n26A-n78A | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n28A-n38A | - | n3 | 5, 10, 15, 20, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n38 | 5, 10, 15, 20, 30, 40 |  |
| CA\_n3A-n28A-n40A | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n28A-n40A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n40 | 20, 40 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A | n417  CA\_n3A-n28A  CA\_n3A-n41A7  CA\_n28A-n41A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n28A-n41B | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n28A-n41A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | CA\_n41B\_BCS0 |  |
| CA\_n3A-n28A-n77A | n777  CA\_n3A-n28A  CA\_n3A-n77A7  CA\_n28A-n77A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 | 2 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n77(2A) | n777  CA\_n3A-n28A  CA\_n3A-n77A7  CA\_n28A-n77A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  | CA\_n77(2A) | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n3A-n28A-n77(3A) | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n3A-n28A-n78A | CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n28 | 5, 10 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n28A-n78C | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n28A-n78(2A) | CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A)  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n28A-n78A | CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n28A-n78(2A) | CA\_n78(2A)  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n28A-n79A | CA\_n3A-n28A  CA\_n3A-n79A  CA\_n28A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
| CA\_n3A-n38A-n40A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n40A-n105A | CA\_n3A-n40A  CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n77A-n79A4 | CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n77(2A)-n79A4 | CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n77(3A)-n79A4 | CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n40A-n41A | CA\_n3A-n40A  CA\_n3A-n41A  CA\_n40A-n41A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n40A-n77A | CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n40A-n77(2A) | CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n41A-n77A | n417  n777  CA\_n3A-n41A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A7 | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41B-n77A | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41A-n77(2A) | n417  n777  CA\_n3A-n41A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n3A-n41A-n77(3A) | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n3A-n41A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  | CA\_n3A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n78A | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n41A-n78(2A) | CA\_n3A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n78A | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n41A-n79A | CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30 | 2 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n67A-n78A | CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n67A-n78(2A) | CA\_n78(2A)  CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n75A-n78A | - | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n78A-n79A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n78A-n79C | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3B-n78A-n79A | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3B-n78A-n79C | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3(2A)-n78A-n79A | - | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3(2A)-n78A-n79C | - | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3A-n78A-n105A | CA\_n3A-n78A  CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n7A-n28A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n5A-n7A-n77A | CA\_n5A-n7A  CA\_n5A-n77A  CA\_n7A-n77A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n7A-n77(2A) | CA\_n77(2A)  CA\_n5A-n7A  CA\_n5A-n77A  CA\_n7A-n77A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n5A-n7A-n77(3A) | CA\_n77(2A)  CA\_n5A-n7A  CA\_n5A-n77A  CA\_n7A-n77A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n5A-n7A-n78A | CA\_n5A-n78A7  CA\_n7A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n5 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n5A-n7B-n78A | CA\_n5A-n78A7  CA\_n7A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n5 | 5, 10, 15, 20 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n5A-n12A-n77A | n777  CA\_n5A-n12A  CA\_n5A-n77A7  CA\_n12A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n12A-n77(2A) | n777  CA\_n5A-n12A CA\_n5A-n77A7 CA\_n12A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n14A-n77A | n777  CA\_n5A-n14A  CA\_n5A-n77A7  CA\_n14A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n14A-n77(2A) | n777  CA\_n5A-n14A CA\_n5A-n77A7 CA\_n14A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n25(2A)-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n25A-n66(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n66(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n5A-n25A-n77A | CA\_n5A-n25A | n5 | 5, 10, 15, 20 | 0 |
|  | CA\_n5A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n25A-n77A | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n77A | CA\_n5A-n25A  CA\_n5A-n77A  CA\_n25A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n77(2A) | CA\_n5A-n25A  CA\_n5A-n77A  CA\_n25A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n77(3A) | CA\_n77(2A)  CA\_n5A-n25A  CA\_n5A-n77A  CA\_n25A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n77(2A) | CA\_n5A-n25A  CA\_n5A-n77A  CA\_n25A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n78A | CA\_n5A-n25A  CA\_n5A-n78A  CA\_n25A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n78A | CA\_n5A-n25A  CA\_n5A-n78A  CA\_n25A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n78(2A) | CA\_n5A-n25A  CA\_n5A-n78A  CA\_n25A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25(2A)-n78(2A) | CA\_n5A-n25A  CA\_n5A-n78A  CA\_n25A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n29A-n77A | n777  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n29A-n77(2A) | n777  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n30A-n66A | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n5A-n30A-n66(2A) | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n5A-n30A-n66(3A) | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n5A-n30A-n77A | n777  CA\_n5A-n30A  CA\_n5A-n77A7  CA\_n30A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n30A-n77(2A) | n777  CA\_n5A-n30A CA\_n5A-n77A7 CA\_n30A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n40A-n78A | CA\_n5A-n40A  CA\_n5A-n78A  CA\_n40A-n78A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n40 | 58, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90,100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90,100 |  |
| CA\_n5A-n41A-n66A | CA\_n5A-n41A CA\_n5A-n66A CA\_n41A-n66A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
| CA\_n5A-n48A-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48(A-B)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48B-n66A | CA\_n48B  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48(2A)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48A-n77A | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48A-n77C | n777,9  CA\_n5A-n48A  CA\_n5A-n77A  CA\_n77C | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n48B-n77A | CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48B-n77C | CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | CA\_n77C BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | CA\_n77C BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 3 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | CA\_n77C BCS1 |  |
| CA\_n5A-n48(2A)-n77A | CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48(2A)-n77C | CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 3 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n66A-n77A | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n77A | n777  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n77(2A) | n777  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n66(3A)-n77A | n777  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(3A)-n77(2A) | n777  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n66A-n77C | CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n66A-n77(2A) | n777  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n66A-n77(3A) | CA\_n77(2A)  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n5A-n66A-n78A | CA\_n5A-n66A  CA\_n5A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n78A | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66A-n78(2A) | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n66(2A)-n78(2A) | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n8A-n28A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n7A-n8A-n40A | CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n7A-n8A-n78A | CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n12A-n25A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n12A-n66A | - | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
| CA\_n7A-n12A-n77A | - | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n25(2A)-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n25(2A)-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7(2A)-n25A-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7(2A)-n25(2A)-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7(2A)-n25A-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7A-n25A-n71A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n7A-n25A-n77A | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n77A | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n77(2A) | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n77(3A) | CA\_n77(2A)  CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n7A-n25(2A)-n77(2A) | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25A-n77A | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25(2A)-n77A | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n77(2A) | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n77(2A) | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n78A | CA\_n7A-n25A  CA\_n7A-n78A  CA\_n25A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7(2A)-n25A-n78A | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7A-n25(2A)-n78A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7(2A)-n25(2A)-n78A | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7A-n25A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n78A  CA\_n25A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25A-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n25(2A)-n78(2A) | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7(2A)-n25(2A)-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n26A-n78A | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n26A-n78(2A) | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n26(2A)-n78A | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n26(2A)-n78(2A) | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7B-n26A-n78A | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n7B | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7B-n26A-n78(2A) | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n7B  CA\_n26A-n78A | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7B-n26(2A)-n78A | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7B-n26(2A)-n78(2A) | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n28A-n38A11 | n28 | n7 | 5, 10, 15, 20, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n38 | 5, 10, 15, 20, 30, 40 |  |
| CA\_n7A-n28A-n78(2A) | CA\_n78(2A)  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n28A-n78A | CA\_n7A-n78A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n28A-n78A7 | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n7A-n28A-n78C | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n7B-n28A-n78A | CA\_n7A-n78A7  CA\_n28A-n78A7 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A  CA\_n7B | n7 | CA\_n7B\_BCS0 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n7B-n28A-n78(2A) | CA\_n7B  CA\_n78(2A)  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n40A-n78A | CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46A-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46C-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46D-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46(2A)-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46(2A)-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46A-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46C-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46D-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n66A-n71A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n7A-n66A-n77A | CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n77A | CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n77(2A) | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n66A-n77(3A) | CA\_n77(2A)  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n7A-n66(2A)-n77(2A) | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n66A-n77A | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66(2A)-n77A | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66A-n77(2A) | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n66(2A)-n77(2A) | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n66A-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66A-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66(2A)-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n78(2A) | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66A-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66(2A)-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n67A-n78A | CA\_n7A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n67A-n78(2A) | CA\_n7A-n78A CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n71A-n77A | CA\_n7A-n71A  CA\_n7A-n77A  CA\_n71A-n77A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n71A-n77(2A) | CA\_n77(2A)  CA\_n7A-n71A  CA\_n7A-n77A  CA\_n71A-n77A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n7A-n71A-n77(3A) | CA\_n77(2A)  CA\_n7A-n71A  CA\_n7A-n77A  CA\_n71A-n77A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n7A-n75A-n78A | - | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n78A-n102A | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n7A-n78A-n102B | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n7A-n78A-n102C | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n7A-n78A-n102D | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n7A-n78A-n102E | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n7A-n78A-n102(2A) | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n7A-n78(2A)-n102A | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n7A-n78(2A)-n102B | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n7A-n78(2A)-n102C | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n7A-n78(2A)-n102D | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n7A-n78(2A)-n102E | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n7A-n78(2A)-n102(2A) | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n8A-n20A-n75A |  | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n28A-n75A |  | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n28A-n78A | - | n8 | 5, 10, 15, 20 | 0 |
|  | n28 | 5, 10, 15, 20 |
|  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
| CA\_n8A-n38A-n40A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n39A-n41A | CA\_n8A-n39A  CA\_n8A-n41A  CA\_n39A-n41A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  | - | n8 | 5, 10, 15, 20 | 1 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
| CA\_n8A-n39A-n79A | CA\_n8A-n39A  CA\_n8A-n79A  CA\_n39A-n79A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n40A-n41A | CA\_n8A-n40A  CA\_n8A-n41A  CA\_n40A-n41A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n8A-n40A-n78A | CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n41A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n8 | 5, 10, 15, 20 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n78A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n78(2A)-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n12A-n25A-n41A | - | n12 | 5, 10, 15 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n12A-n30A-n66A | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n12A-n30A-n66(2A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n12A-n30A-n66(3A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n12A-n30A-n77A | n777  CA\_n12A-n30A,  CA\_n12A-n77A7  CA\_n30A-n77A7 | n12 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n30A-n77(2A) | n777  CA\_n12A-n30A CA\_n12A-n77A7 CA\_n30A-n77A7 | n12 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n41A-n66A | - | n12 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n12A-n41A-n77A | - | n12 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66A-n77A | n777  CA\_n12A-n66A  CA\_n12A-n77A7 CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66(2A)-n77A | n777  CA\_n12A-n66A CA\_n12A-n77A7 CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66A-n77(2A) | n777  CA\_n12A-n66A CA\_n12A-n77A7 CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n66(2A)-n77(2A) | n777  CA\_n12A-n66A CA\_n12A-n77A7 CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n66(3A)-n77A | n777  CA\_n12A-n66A CA\_n12A-n77A7 CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66(3A)-n77(2A) | n777  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n25A-n66A | CA\_n13A-n25A  CA\_n13A-n66A  CA\_n25A-n66A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n13A-n25A-n77A | CA\_n13A-n25A  CA\_n13A-n77A  CA\_n25A-n77A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n25A-n77(2A) | CA\_n77(2A)  CA\_n13A-n25A  CA\_n13A-n77A  CA\_n25A-n77A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n66A-n77A | n777, 9  CA\_n13A-n66A  CA\_n13A-n77A  CA\_n66A-n77A | n13 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n66A-n77(2A) | CA\_n77(2A)  CA\_n13A-n66A  CA\_n13A-n77A  CA\_n66A-n77A | n13 | 5, 10 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n30A-n66A | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n14A-n30A-n66(2A) | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n14A-n30A-n66(3A) | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n14A-n30A-n77A | n777  CA\_n14A-n30A  CA\_n14A-n77A7  CA\_n30A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n77(2A) | n777  CA\_n14A-n30A  CA\_n14A-n77A7 CA\_n30A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66A-n77A | n777  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66(2A)-n77A | n777  CA\_n14A-n66A CA\_n14A-n77A7 CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66A-n77(2A) | n777  CA\_n14A-n66A CA\_n14A-n77A7 CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66(2A)-n77(2A) | n777  CA\_n14A-n66A CA\_n14A-n77A7 CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66(3A)-n77A | n777  CA\_n14A-n66A CA\_n14A-n77A7 CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66(3A)-n77(2A) | n777  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n28A-n41A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n28A-n77A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n28A-n77(2A) | CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n41A-n77A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n41A-n77(2A) | CA\_n18A-n41A  CA\_n18A-n77A  CA\_n41A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n20A-n28A-n75A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20 |  |
| CA\_n20A-n28A-n78A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n20A-n28A-n78C | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n24A-n41A-n48A | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41(2A)-n48A | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41A-n48(2A) | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
| CA\_n24A-n41(2A)-n48(2A) | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
| CA\_n24A-n41A-n77A | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41(2A)-n77A | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41A-n77(2A) | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n41(2A)-n77(2A) | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n48A-n77A |  | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n48(2A)-n77A |  | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n48A-n77(2A) |  | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n48(2A)-n77(2A) |  | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n25A-n29A-n66A | CA\_n25A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n38A-n66A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A-n66A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A-n66(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n25A-n38A-n66(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n25A-n38A-n78A | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n38A-n78A | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n38A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41C-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n66A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n66A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | 5, 10, 15, 20, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41A-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41C-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n71A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n71A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(3A)-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77(2A) | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n77(2A) | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n77A | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n77(2A) | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n77(2A) | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n41A-n78A | CA\_n25A-n41A  CA\_n25A-n78A  CA\_n41A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n41A-n78(2A) | CA\_n25A-n41A  CA\_n25A-n78A  CA\_n41A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n48A-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n48(2A)-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n48C-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n66A-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A)-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n77A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n77(2A) | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n66A-n77(3A) | CA\_n77(2A)  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n25A-n66(2A)-n77(2A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n77A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A)-n77A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n77(2A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n66(2A)-n77(2A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n25A-n66A-n78A | CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66(2A)-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66A-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n66(2A)-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66(2A)-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n66(2A)-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66A-n85A | CA\_n25A-n66A  CA\_n25A-n85A  CA\_n66A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71A-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71A-n77(2A) | n777,9  CA\_n77(2A)  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A) BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71A-n77(3A) | CA\_n77(2A)  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A) BCS1 |  |
| CA\_n25A-n71B-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71B-n77(2A) | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71(2A)-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71(2A)-n77(2A) | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n71A-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71B-n77A | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71(2A)-n77A | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71A-n77(2A) | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71A-n78A | CA\_n25A-n71A  CA\_n25A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n71A-n78(2A) | CA\_n25A-n71A  CA\_n25A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n77A-n85A | CA\_n25A-n77A  CA\_n25A-n85A  CA\_n77A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n26A-n66A-n70A | CA\_n26A-n66A  CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n66(2A)-n70A | CA\_n26A-n66A  CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n28A-n38A-n78A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n39A-n40A | CA\_n28A-n39A  CA\_n28A-n40A  CA\_n39A-n40A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
| CA\_n28A-n39A-n41A | CA\_n28A-n39A  CA\_n28A-n41A  CA\_n39A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n39A-n41C | CA\_n28A-n39A  CA\_n28A-n41A  CA\_n39A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | CA\_n41C\_BCS1 |  |
| CA\_n28A-n39A-n79A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n40A-n41A | CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n40A-n41C | CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C\_BCS0 |  |
| CA\_n28A-n40A-n78A | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n28 | 5, 10, 15, 20 | 1 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n40A-n77A | CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n40A-n77(2A) | CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n28A-n40B-n78A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n40A-n79A | CA\_n28A-n40A  CA\_n28A-n79A  CA\_n40A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n41A-n77A | n417  n777  CA\_n28A-n41A7 | n28 | 5, 10, 15, 20, 30 | 0 |
|  | CA\_n28A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n41B-n77A | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n28 | 5, 10 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n41A-n77(2A) | n417  n777  CA\_n28A-n41A7 | n28 | 5, 10, 15, 20, 30 | 0 |
|  | CA\_n28A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n28A-n41A-n77(3A) | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n28 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n28A-n41A-n78A | CA\_n28A-n41A  CA\_n41A-n78A  CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n41A-n78(2A) | CA\_n78(2A) | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n41A-n79A | CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n41A-n79C | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n28A-n41C-n79A | CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n41C-n79C | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n28A-n46A-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46C-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46D-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46(2A)-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46(2A)-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46A-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46C-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46D-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n75A-n78A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n77A-n79A4 | CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n77(2A)-n79A4 | CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n77(3A)-n79A4 | CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n78A-n79A | CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n78A-n102A | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n28A-n78A-n102B | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n28A-n78A-n102C | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n28A-n78A-n102D | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n28A-n78A-n102E | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n28A-n78A-n102(2A) | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n28A-n78(2A)-n102A | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n28A-n78(2A)-n102B | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n28A-n78(2A)-n102C | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n28A-n78(2A)-n102D | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n28A-n78(2A)-n102E | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n28A-n78(2A)-n102(2A) | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n29A-n30A-n66A | CA\_n30A-n66A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n29A-n30A-n66(2A) | CA\_n30A-n66A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n29A-n30A-n77A | n777  CA\_n30A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n30A-n77(2A) | n777  CA\_n30A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66A-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66B-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66(2A)-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66A-n77A | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66(2A)-n77A | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66A-n77(2A) | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66(3A)-n77A | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66(2A)-n77(2A) | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66(3A)-n77(2A) | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n70A-n71A | CA\_n70A-n71A | n29 | 5, 10 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n30A-n66A-n77A | n777  CA\_n30A-n66A  CA\_n30A-n77A7  CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66(2A)-n77A | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66A-n77(2A) | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n30A-n66(2A)-n77(2A) | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n30A-n66(3A)-n77A | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66(3A)-n77(2A) | n777  CA\_n30A-n66A  CA\_n30A-n77A7  CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n38A-n66A-n78A | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66A-n78(2A) | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n38A-n66(2A)-n78A | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66(2A)-n78(2A) | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n39A-n40A-n41A | CA\_n39A-n40A  CA\_n39A-n41A  CA\_n40A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n39A-n40A-n79A | CA\_n39A-n40A  CA\_n40A-n79A  CA\_n39A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n39A-n41A-n79A | CA\_n39A-n41A  CA\_n39A-n79A  CA\_n41A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n40A-n41A-n79A | CA\_n40A-n41A  CA\_n40A-n79A  CA\_n41A-n79A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | , 40, 50, 60, 80, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | , 40, 50, 60, 80, 100 |  |
| CA\_n40A-n78A-n105A | CA\_n40A-n78A  CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n41A-n66A-n70A | CA\_n41A-n66A  CA\_n41A-n70A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n41A-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71B | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41A-n66A-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n71A | n417,9  CA\_n41A-n66A7  CA\_n66A-n71A  CA\_n41A-n71A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n71B | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n41A-n71A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n71(2A) | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n41A-n71A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n66A-n71A | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71B | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n71(2A) | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A)-n71A | CA\_n41A-n71A  CA\_n41A-n66A CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7 CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71B | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41C  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41C-n66A-n71(2A) | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41C  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41C-n66(2A)-n71A | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n41C  CA\_n66A-n71A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7 CA\_n41C7  CA\_n66A-n71A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n41A-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n77(2A) | n417,9  n777,9  CA\_n41A-n77A7  CA\_n41A-n66A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n77(2A) | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n77(2A) | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(3A)-n66A-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n77(2A) | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n41C  CA\_n66A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n41C  CA\_n66A-n77A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n78A | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n78(2A) | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66(2A)-n78A | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66(2A)-n78(2A) | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66A-n85A | CA\_n41A-n66A  CA\_n41A-n85A  CA\_n66A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n70A-n78A | CA\_n41A-n70A  CA\_n41A-n78A  CA\_n70A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71A-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71A-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(3A)-n71A-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71(2A)-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71A-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(A-C)-n71A-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71A-n78A | CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n71A-n78(2A) | CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n77A-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77(2A)-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77(3A)-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77A-n85A | CA\_n41A-n77A  CA\_n41A-n85A  CA\_n77A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n46A-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48A-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48B-n96A |  | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48C-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48A-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48A-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48A-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48A-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48A-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48A-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48A-n96C | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48B-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48C-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48C-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48C-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48C-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48C-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48C-n96C | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48A-n96D | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48A-n96D | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48A-n96D | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48A-n96D | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48A-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48A-n96D | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48C-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48A-n96E | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48A-n96E | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48A-n96E | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48A-n96E | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48A-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48A-n96E | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48C-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(2A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(2A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(2A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(2A)-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(2A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(3A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(3A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(3A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(3A)-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(3A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(4A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(4A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(4A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(4A)-n96D |  | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(4A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n48A-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n66(2A)-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48(2A)-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48B-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66(2A)-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66A-n71(2A) | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48A-n66A-n77A | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66(2A)-n77A | CA\_n48A-n66A  CA\_n66A-n77A | n48 | 5, 10, 15, 20, 30, 40, 501, 601, 701 , 801, 901, 1001 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66A-n77C | n777,9  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n77C | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48B-n66A-n77C | CA\_n48A-n66A  CA\_n66A-n77A  CA\_n77C | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48B-n66A-n77A | CA\_n48A-n66A  CA\_n66A-n77A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n77A | CA\_n48A-n66A  CA\_n66A-n77A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n77C | CA\_n48A-n66A  CA\_n66A-n77A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 3 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48A-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n70A-n71(2A) | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48A-n70A-n77A | CA\_n48A-n70A  CA\_n70A-n77A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n70A-n77A | CA\_n48A-n70A  CA\_n70A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n71A-n77A | CA\_n48A-n71A  CA\_n71A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n71A-n77A | CA\_n48A-n71A  CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n70A-n78A | CA\_n66A-n78A CA\_n70A-n78A | n66 | 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n70A-n71(2A) | CA\_n66A-n71A  CA\_n70A-n71A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n66B-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201,251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66(2A)-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n70A-n77A | CA\_n66A-n77A  CA\_n70A-n77A | n66 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66(2A)-n70A-n77A | CA\_n66A-n77A  CA\_n70A-n77A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n71A-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B-n77A | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71(2A)-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71(2A)-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66(2A)-n71A-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71A-n77(2A) | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71A-n77(3A) | CA\_n77(2A)  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n66(2A)-n71B-n77A | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71(2A)-n77A | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71A-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71A-n78A | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n71A-n78(2A) | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n66(2A)-n71A-n78A | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66(2A)-n71A-n78(2A) | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n66A-n77A-n85A | CA\_n66A-n77A  CA\_n66A-n85A  CA\_n77A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n70A-n71A-n77A | CA\_n70A-n71A  CA\_n70A-n77A  CA\_n71A-n77A | n70 | 5, 10, 15, 20, 25 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| NOTE 1: This UE channel bandwidth is applicable only to downlink  NOTE 2: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz.  NOTE 3: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1.  NOTE 4: The minimum requirements only apply for non-simultaneous Tx/Rx between all carriers for TDD combinations.  NOTE 5: Simultaneous Rx/Tx capability for TDD combinations does not apply for UEs supporting band n78 with an n77 implementation.  NOTE 6: Only single uplink carriers with power class other than PC3 are listed.  NOTE 7: Power Class 2 is allowed for this uplink combination or single uplink carrier in this downlink/uplink combination  NOTE 8: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.  NOTE 9: Power Class 1.5 is allowed for single uplink carrier in this downlink/uplink combination  NOTE 10: For a band combination which include band n7 and n38 simultaneously, carriers in band n7 and n38 can only be configured as downlink carriers. Power imbalance between downlink carriers on Band n7 and Band n38 is assumed to be within 6dB.  NOTE 11: UL carrier shall be supported in Band n28 only. Power imbalance between downlink carriers on Band 7 and Band 38 is assumed to be within 6dB. | | | | |

---End of changes---