**3GPP TSG-RAN WG4 Meeting #108 R4-2313222**

**Toulouse, France, 21st August – 25th August 2023**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **-1** | **CR** | 1775 | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Big CR on TS38.101-1: Addition of intra-band CA Combinations | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | HPUE\_NR\_FR1\_TDD\_intra\_CA\_R18 | | | | |  | ***Date:*** | | | 2023-08-22 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Adding new HPUE UL configurations | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Capture endorsed R4-2311113   * Adding PC2 UL n77(2A) to DL CA\_n77(2A) (included in big CR R4-2219390 but not implemented in spec) * Adding PC2 UL n77(2A) to DL CA\_n77(3A) (with PC3 UL n77(2A) to DL n77(3A) being added in R4-2311108) * Adding PC2 UL n78 to DL CA\_n78(2A) (included in big CR R4-2219390 but not implemented in spec) * Adding PC1.5 UL n78 to DL CA\_n78(2A) (included in big CR R4-2219390 but not implemented in spec) * Adding PC2 UL n78(2A) to DL CA\_n78(2A) | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | HPUE UL configurationa are not added | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

Table 5.5A.2-1: NR CA configurations and bandwidth combination sets defined for intra-band non-contiguous CA

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink CA Configurations or single uplink carrier5 | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Maximum  Aggregated bandwidth  (MHz) | Bandwidth combination set |
| CA\_n1(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n2(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
|  |  | See n2 channel bandwidths in Table 5.3.5-1 for each carrier | |  |  | 40 | 4 and 5 |
| CA\_n3(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
|  | - | 5, 10, 15, 20, 25, 30 | 5, 10, 15, 20, 25, 30 |  |  | 60 | 1 |
| CA\_n5(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 25 | 0 |
| CA\_n7(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n12(2A) | - | 5 | 5 |  |  | 10 | 0 |
| CA\_n25(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
|  |  | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  |  | 60 | 1 |
|  |  | See n25 channel bandwidths in Table 5.3.5-1 for each carrier | |  |  | 60 | 4 and 5 |
| CA\_n25(3A) | - | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  | 55 | 0 |
|  |  | See n25 channel bandwidths in Table 5.3.5-1 for each carrier | |  |  | 55 | 4 and 5 |
| CA\_n26(2A) | - | 5, 10, 15 | 5, 10, 15 |  |  | 30 | 0 |
| CA\_n41(2A) | n413,4 CA\_n41(2A) | 40, 50, 60, 80, 100 | 40, 50, 60, 80, 100 |  |  | 180 | 0 |
|  |  | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 190 | 1 |
|  |  | 10, 15, 20, 30, 40, 50, 60, 80, 90 | 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |  | 190 | 2 |
|  |  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 190 | 3 |
|  |  | See n41 channel bandwidths in Table 5.3.5-1 for each carrier | |  |  | 190 | 4 and 5 |
| CA\_n41(3A) | n413,4 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  | 190 | 0 |
|  |  | See n41 channel bandwidths in Table 5.3.5-1 for each carrier | | |  | 190 | 4 and 5 |
| CA\_n41(4A) | n413 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 190 | 0 |
|  |  | See n41 channel bandwidths in Table 5.3.5-1 for each carrier | | | | 190 | 4 and 5 |
| CA\_n46(2A) | - | 10, 20, 40, 60, 80 | 10, 20, 40, 60, 80 |  |  | 160 | 0 |
| CA\_n48(2A) | - | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 1402 | 0 |
|  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 1402 | 1 |
|  |  | See n48 channel bandwidths in Table 5.3.5-1 for each carrier | |  |  | 1402 | 4 and 5 |
| CA\_n48(3A) | - | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 |  | 1402 | 0 |
|  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  | 1402 | 1 |
| CA\_n48(4A) | - | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 1352 | 0 |
|  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1352 | 1 |
| CA\_n66(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20, 40 |  |  | 60 | 0 |
| 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  |  | 80 | 1 |
| 5, 10, 15, 20, 40 | 5, 10, 15, 20, 40 |  |  | 80 | 2 |
|  |  | See n66 channel bandwidths in Table 5.3.5-1 for each carrier | |  |  | 85 | 4 and 5 |
| CA\_n66(3A) | - | 5, 10, 15, 20, 40 | 5, 10, 15, 20, 40 | 5, 10, 15, 20, 40 |  | 80 | 0 |
| CA\_n71(2A) | - | 5, 10, 15, 20 | 5,10,15, 20 |  |  | 30 | 0 |
|  |  | See n71 channel bandwidths in Table 5.3.5-1 for each carrier up to 25 MHz per carrier | |  |  | 30 | 4 and 5 |
| CA\_n77(2A)6 | n773,4  CA\_n77(2A)3 | 20, 40, 80, 100 | 20, 40, 80, 100 |  |  | 200 | 0 |
|  |  | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 200 | 1 |
|  |  | See n77 channel bandwidths in Table 5.3.5-1 for each carrier | |  |  | 200 | 4 and 5 |
| CA\_n77(3A) | n773,4  CA\_n77(2A)3 | 20, 40, 80, 100 | 20, 40, 80, 100 | 20, 40, 80, 100 |  | 300 | 0 |
| 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  | 300 | 1 |
|  |  | See n77 channel bandwidths in Table 5.3.5-1 for each carrier | | |  | 300 | 4 and 5 |
| CA\_n78(2A)6 | n783,4  CA\_n78(2A)3 | 10, 20, 40, 50, 60, 80, 90, 100 | 10, 20, 40, 50, 60, 80, 90, 100 |  |  | 200 | 0 |
|  |  | 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |  | 200 | 1 |
|  |  | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 200 | 2 |
|  |  | See n78 channel bandwidths in Table 5.3.5-1 for each carrier | |  |  | 200 | 4 and 5 |
| CA\_n96(2A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 |  |  | 160 | 0 |
| CA\_n96(3A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 |  | 240 | 0 |
| CA\_n96(4A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 | 320 | 0 |
| CA\_n102(2A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 |  |  | 160 | 0 |
| CA\_n102(3A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 |  | 240 | 0 |
| CA\_n102(4A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 | 320 | 0 |
| NOTE 1: Void.  NOTE 2: Parameter value accounts for both, the maximum frequency range of band n48 (150 MHz), and the minimum frequency gaps in between NR non-contiguous component carriers.  NOTE 3: Power Class 2 is allowed for this uplink combination or single uplink carrier in this downlink/uplink combination  NOTE 4: Power Class 1.5 is allowed for this uplink combination or single uplink carrier in this downlink/uplink combination  NOTE 5: Only single uplink carriers with power class other than PC3 are listed.  NOTE 6: For a UE not indicating *[intraBandNonColocatedCA-r18]*, the minimum requirements for intra-band non-contiguous CA apply when the maximum power spectral density imbalance between downlink carriers is within 6 dB. For a UE indicating *[intraBandNonColocatedCA-r18]*, the power imbalance requirement defined in subclause 7.10A apply. For these UEs, the power spectral density imbalance condition also applies for these carriers when applicable intra-band non-contiguous NR CA configuration is a subset of a higher order NR CA configuration. | | | | | | | |

---End of changes---