**3GPP TSG-RAN WG4 Meeting #95-e *R4-2008914***

Electronic meeting, -

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** | **0359** | **rev** | 1 | **Current version:** | **16.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_n65\_BW | | | | |  | ***Date:*** | | | 2020-05-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Add channel BW support in band n65 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Consider new CBW in the list of supported CBW for n65  Add A-MPR requirements for n65 and 50 MHz CBW.  Update REFSENS requirements  Fixing also an error on refrenced tables for NS\_48 and NS\_49 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The new CBW won’t be supported in band n65 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.3.5, 6.2.3, 6.5.3.3.22, 6.5.3.3.23, 7.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS | | |
| ***affected:*** | | **x** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |

|  |  |
| --- | --- |
| ***This CR's revision history:*** |  |

*<Start of the change>*

### 5.3.5 UE channel bandwidth per operating band

The requirements in this specification apply to the combination of channel bandwidths, SCS and operating bands shown in Table 5.3.5-1. The transmission bandwidth configuration in Table 5.3.2-1 shall be supported for each of the specified channel bandwidths. The channel bandwidths are specified for both the TX and RX path.

Table 5.3.5-1 Channel bandwidths for each NR band

|  |  | | NR band / SCS / UE Channel bandwidth | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR Band | SCS  kHz | 5 MHz | | 10 MHz | 15 MHz | 20MHz | 25 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 70 MHz | 80 MHz | 90 MHz | 100 MHz |
| n1 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n2 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n3 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| n5 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n7 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n8 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | 15 | Yes | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | 15 | Yes | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | 15 | Yes | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n20 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n25 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n26 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n28 | 15 | Yes | | Yes | Yes | Yes7 |  | Yes7 |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes7 |  | Yes7 |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n29 | 15 | Yes | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | 15 | Yes | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | 15 | Yes | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| n38 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n39 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n40 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  |  |
| n41 | 15 |  | | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| 60 |  | | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| n48 | 15 | Yes5 | | Yes | Yes | Yes |  |  | Yes | Yes6 |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  | Yes | Yes6 | Yes6 |  | Yes6 | Yes6,4 | Yes6 |
| 60 |  | | Yes | Yes | Yes |  |  | Yes | Yes6 | Yes6 |  | Yes6 | Yes6,4 | Yes6 |
| n50 | 15 | Yes | | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes3 |  |  |
| 60 |  | | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes3 |  |  |
| n51 | 15 | Yes | |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n53 | 15 | Yes | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | | Yes |  |  |  |  |  |  |  |  |  |  |  |
| n65 | 15 | Yes | | Yes | Yes | Yes |  |  |  | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  | Yes |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes |  |  |  | Yes |  |  |  |  |  |
| n66 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n70 | 15 | Yes | | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| n71 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n74 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n75 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n76 | 15 | Yes | |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n77 | 15 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes4 | Yes |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes4 | Yes |
| n78 | 15 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes | Yes |
| 60 |  | | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes | Yes |
| n79 | 15 |  | |  |  |  |  |  | Yes | Yes |  |  |  |  |  |
| 30 |  | |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
| 60 |  | |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
| n80 | 15 | Yes | | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| n81 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n82 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n83 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n84 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n86 | 15 | Yes | | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 60 |  | | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| n89 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n90 | 15 |  | | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| 60 |  | | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| n91 | 15 | Yes | | Yes8 |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n92 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | 15 | Yes | | Yes8 |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n94 | 15 | Yes | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | |  |  |  |  |  |  |  |  |  |  |  |  |
| n95 | 15 | Yes | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: Void.  NOTE 2: Void.  NOTE 3: This UE channel bandwidth is applicable only to downlink.  NOTE 4: This UE channel bandwidth is optional in this release of the specification.  NOTE 5: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.  NOTE 6: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an downlink SCell part of CA configuration.  NOTE 7: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz. For the 30MHz bandwidth, the minimum requirements are specified for NR UL transmission bandwidth configuration confined to either 703-733 or 718-748 MHz.  NOTE 8: This UE channel bandwidth is applicable only to uplink. | | | | | | | | | | | | | | | |

*<End of the change>*

*<Start of the change>*

### 6.2.3 UE additional maximum output power reduction

#### 6.2.3.1 General

Additional emission requirements can be signalled by the network. Each additional emission requirement is associated with a unique network signalling (NS) value indicated in RRC signalling by an NR frequency band number of the applicable operating band and an associated value in the field *additionalSpectrumEmission.* Throughout this specification, the notion of indication or signalling of an NS value refers to the corresponding indication of an NR frequency band number of the applicable operating band, the IE field *freqBandIndicatorNR* and an associated value of *additionalSpectrumEmission* in the relevant RRC information elements [7]*.*

To meet the additional requirements, additional maximum power reduction (A-MPR) is allowed for the maximum output power as specified in Table 6.2.1-1. Unless stated otherwise, the total reduction to UE maximum output power is max(MPR, A-MPR) where MPR is defined in clause 6.2.2. Outer and inner allocation notation used in clause 6.2.3 is defined in clause 6.2.2 In absense of modulation and waveform types the A-MPR applies to all modulation and waveform types.

Table 6.2.3.1-1 specifies the additional requirements with their associated network signalling values and the allowed A-MPR and applicable operating band(s) for each NS value. In case of a power class 3 UE, when IE *powerBoostPi2BPSK* is set to 1, power class 2 A-MPR values apply. The mapping of NR frequency band numbers and values of the *additionalSpectrumEmission* to network signalling labels is specified in Table 6.2.3.1-1A.

For almost contiguous allocations in CP-OFDM waveforms in power class 3, the allowed A-MPR defined in clause 6.2.3 is increased by CEIL{ 10 log10(1 + NRB\_gap / NRB\_alloc), 0.5 } dB, where NRB\_gap is the total number of unallocated RBs between allocated RBs and NRB\_alloc is the total number of allocated RBs, and the parameter LCRB is replaced by NRB\_alloc + NRB\_gap in specifying the RB allocation regions.

Table 6.2.3.1-1: Additional maximum power reduction (A-MPR)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Network signalling label | Requirements (clause) | NR Band | Channel bandwidth (MHz) | Resources blocks (*N*RB) | A-MPR (dB) |
| NS\_01 |  | Table 5.2-1 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | Table 5.3.2-1 | N/A |
| NS\_03 | 6.5.2.3.3 | n2, n25, n66,  n70, n86 |  |  | Clause 6.2.3.7 |
| NS\_03U | 6.5.2.3.3, 6.5.2.4.2 | n2, n25, n66, n86 |  |  | Clause 6.2.3.7 |
| NS\_04 | 6.5.2.3.2, 6.5.3.3.1 | n41 | 10, 15, 20, 30, 40, 50, 60 80, 90, 100 |  | Clause 6.2.3.2 |
| NS\_05 | 6.5.3.3.4 | n1, n65, n84 | 5, 10, 15, 20(NOTE 2) |  | Clause 6.2.3.4 |
| NS\_05U | 6.5.3.3.4, 6.5.2.4.2 | n1, n65, n84 | 5, 10, 15, 20 |  | Clause 6.2.3.4 |
| NS\_06 | 6.5.2.3.4 | n12 | 5, 10, 15 |  | N/A |
| n14 | 5,10 |
| NS\_10 |  | n20 | 15, 20 | Table 6.2.3.3-1 | Table  6.2.3.3-1 |
| NS\_12 | 6.5.3.3.17 | n26 |  |  |  |
| NS\_13 | 6.5.3.3.18 | n26 |  |  |  |
| NS\_14 | 6.5.3.3.19 | n26 |  |  |  |
| NS\_15 | 6.5.3.3.20 | n26 |  |  |  |
| NS\_17 | 6.5.3.3.2 | n28, n83 | 5,10 | Table 5.3.2-1 | N/A |
| NS\_18 | 6.5.3.3.3 | n28, n83 | 5 |  | Table 6.2.3.13-1, A1 |
| 10, 15, 20 |  | Table 6.2.3.13-1, A2 |
| 30 |  | Table 6.2.3.13-1, A3, A4, A5 |
| NS\_21 | 6.5.3.3.12 | n30 | 5, 10 |  | Clause 6.2.3.14 |
| NS\_24 | 6.5.3.3.13 | n65 (NOTE 4) | 5, 10, 15, 20 | Table 6.2.3.15-1 | Clause 6.2.3.15 |
| NS\_27 | 6.5.2.3.8  6.5.3.3.14 | n48 | 5, 10, 15, 20, 40 | Table 6.2.3.16-1 | Table 6.2.3.16-2 |
| NS\_35 | 6.5.2.3.1 | n71 | 5, 10, 15, 20 | Table 5.3.2-1 | N/A |
| NS\_37 | 6.5.3.3.6 | n74  (NOTE 3) | 10, 15 | Table 6.2.3.8-1 | Table  6.2.3.8-1 |
| NS\_38 | 6.5.3.3.7 | n74 | 5, 10, 15, 20 | Table 6.2.3.9-1 | Table  6.2.3.9-1 |
| NS\_39 | 6.5.3.3.8 | n74 | 10, 15, 20 | Table 6.2.3.10-1 | Table 6.2.3.10-1 |
| NS\_40 | 6.5.3.3.9 | n51 | 5 |  | Table  6.2.3.5-1 |
| NS\_41 | 6.5.3.3.10 | n50 | 5, 10, 15, 20, 30, 40, 50, 60 |  | Table 6.2.3.11-1 |
| NS\_42 | 6.5.3.3.11 | n50 | 5, 10, 15, 20, 30, 40, 50, 60 |  | Table 6.2.3.12-1 |
| NS\_43 | 6.5.3.3.5 | n8, n81 | 5, 10, 15 |  | Clause 6.2.3.6 |
| NS\_43U | 6.5.3.3.5, 6.5.2.4.2 | n8, n81 | 5, 10, 15 |  | Clause 6.2.3.6 |
| NS\_44 | 6.5.3.3.24 | n38 | 25, 30, 40 | Table 6.2.3.20-1 | Table 6.2.3.20-1 |
| NS\_45 | 6.5.3.3.21 | n53 | 5, 10 |  | Clause 6.2.3.25 |
| NS\_46 | 6.5.3.2 | n7 | 25, 30, 40, 50 | Table 6.2.3.17-1 | Table 6.2.3.17-2 |
| NS\_47 | 6.5.3.3.15 | n41 (Note 5) | 30 | Table 6.2.3.18-1 | Table 6.2.3.18-2 |
| NS\_48 | 6.5.3.3.18 | n1 | 25, 30, 40 | Table 6.2.3.26-1 | Table 6.2.3.21-1 |
| NS\_49 | 6.5.3.3.19 | n1 | 25, 30, 40 | Table 6.2.3.27-1 | Table 6.2.3.22-1 |
| NS\_50 | 6.5.3.3.16 | n39 | 25, 30, 40 |  | Clause 6.2.3.19 |
| NS\_51 | 6.5.3.3.22 | n65 | 50 | Table 6.2.3.28-1 | Table 6.2.3.28-2 |
| NS\_100 | 6.5.2.4.2 | n1, n2, n3, n5, n8, n18, n25, n26, n65, n66, n80, n81, n84, n86, n89  (NOTE 1) |  |  | Table  6.2.3.1-2 |
| NOTE 1: This NS can be signalled for NR bands that have UTRA services deployed  NOTE 2: No A-MPR is applied for 5 MHz CBW where the lower channel edge is ≥ 1930 MHz,10 MHz CBW where the lower channel edge is ≥ 1950 MHz and 15 MHz CBW where the lower channel edge is ≥ 1955 MHz.  NOTE 3: Applicable when the NR carrier is within 1447.9 – 1462.9 MHz  NOTE 4: Applicable when the upper edge of the channel bandwidth frequency is greater than 1980 MHz.  NOTE 5: Applicable when the NR carrier is within 2545 – 2575 MHz | | | | | |

[The NS\_01 label with the field *additionalPmax* [7] absent is default for all NR bands.]

Table 6.2.3.1-1A: Mapping of network signaling label

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR band | Value of additionalSpectrumEmission | | | | | | | |
| **0** | **1** | **2** | **3** | **4** | **5** | **6** | **7** |
| n1 | NS\_01 | NS\_100 | NS\_05 | NS\_05U | NS\_48 | NS\_49 |  |  |
| n2 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n3 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n5 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n7 | NS\_01 | NS\_46 |  |  |  |  |  |  |
| n8 | NS\_01 | NS\_100 | NS\_43 | NS\_43U |  |  |  |  |
| n12 | NS\_01 | NS\_06 |  |  |  |  |  |  |
| n14 | NS\_01 | NS\_06 |  |  |  |  |  |  |
| n18 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n20 | NS\_01 | Void | NS\_10 |  |  |  |  |  |
| n25 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n26 | NS\_01 | NS\_100 | NS\_12 | NS\_13 | NS\_14 | NS\_15 |  |  |
| n28 | NS\_01 | NS\_17 | NS\_18 |  |  |  |  |  |
| n30 | NS\_01 | NS\_21 |  |  |  |  |  |  |
| n34 | NS\_01 |  |  |  |  |  |  |  |
| n38 | NS\_01 | NS\_44 |  |  |  |  |  |  |
| n39 | NS\_01 | NS\_50 |  |  |  |  |  |  |
| n40 | NS\_01 |  |  |  |  |  |  |  |
| n41 | NS\_01 | NS\_04 | NS\_47 |  |  |  |  |  |
| n48 | NS\_01 | NS\_27 |  |  |  |  |  |  |
| n50 | NS\_01 | NS\_41 | NS\_42 |  |  |  |  |  |
| n51 | NS\_01 | NS\_40 |  |  |  |  |  |  |
| n53 | NS\_01 | NS\_45 |  |  |  |  |  |  |
| n65 | NS\_01 | NS\_24 | NS\_100 | NS\_05 | NS\_05U | NS\_51 |  |  |
| n66 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n70 | NS\_01 | NS\_03 |  |  |  |  |  |  |
| n71 | NS\_01 | NS\_35 |  |  |  |  |  |  |
| n74 | NS\_01 | NS\_37 | NS\_38 | NS\_39 |  |  |  |  |
| n77 | NS\_01 |  |  |  |  |  |  |  |
| n78 | NS\_01 |  |  |  |  |  |  |  |
| n79 | NS\_01 |  |  |  |  |  |  |  |
| n80 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n81 | NS\_01 | NS\_100 | NS\_43 | NS\_43U |  |  |  |  |
| n82 | NS\_01 | Void |  |  |  |  |  |  |
| n83 | NS\_01 | NS\_17 | NS\_18 |  |  |  |  |  |
| n84 | NS\_01 | NS\_100 | NS\_05 | NS\_05U |  |  |  |  |
| n86 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n89 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n95 | NS\_01 |  |  |  |  |  |  |  |
| NOTE: *additionalSpectrumEmission* corresponds to an information element of the same name defined in clause 6.3.2 of TS 38.331 [7]. | | | | | | | | |

*<End of the change>*

*<Start of the change>*

#### 6.2.3.28 A-MPR for NS\_51

Table 6.2.3.28-1: A-MPR regions for NS\_51

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Channel Bandwidth, MHz | Carrier Center Frequency, Fc, MHz | Regions | | A-MPR |
| RBend\*12\*SCS  MHz | LCRB\*12\*SCS  MHz |
| 50 MHz | Fc ≤ 1945 | ≤ 4.5 | > 0 | A7 |
| >4.5, < 32.4 | ≥ max(0, 12\*SCS\*RBend - 14.4) | A4 |
| < 32.4 | < max(0, 12\*SCS\*RBend - 14.4) | A5 |
| ≥ 32.4 | > 0 | A6 |
| 50 MHz | 1945 < Fc ≤ 1980 | < 27 | ≥ max(0, 12\*SCS\*RBend - 14.4) | A1 |
| < 27 | < max(0, 12\*SCS\*RBend - 14.4) | A2 |
| ≥ 27 | > 0 | A3 |

Table 6.2.3.28-2: A-MPR for NS\_51

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Modulation/Waveform | | A1 | A2 | A3 | A4 | A5 | A5 | A7 |
| Outer/Inner | Outer/Inner | Outer/Inner | Outer/Inner | Outer/Inner | Outer/Inner | Outer/Inner |
| DFT-s-OFDM | PI/2 BPSK | 15 | 12.5 | 22 | 7 | 4.5 | 16 | 14 |
| QPSK | 15 | 12.5 | 22 | 7 | 4.5 | 16 | 14 |
| 16 QAM | 15 | 12.5 | 22 | 7 | 4.5 | 16 | 14 |
| 64 QAM | 15 | 12.5 | 22 | 7 | 4.5 | 16 | 14 |
| 256 QAM | 15 | 12.5 | 22 | 7 | 4.5 | 16 | 14 |
| CP-OFDM | QPSK | 15 | 12.5 | 22 | 8.5 | 4.5 | 17 | 14 |
| 16 QAM | 15 | 12.5 | 22 | 8.5 | 4.5 | 17 | 14 |
| 64 QAM | 15 | 12.5 | 22 | 8.5 | 4.5 | 17 | 14 |
| 256 QAM | 15 | 12.5 | 22 | 8.5 | 4.5 | 17 | 14 |

*<End of the change>*

*<Start of the change>*

##### 6.5.3.3.22 Requirement for network signalled values "NS\_48" and “NS\_51”

When "NS\_48" or “NS\_51” is indicated in the cell, the power of any UE emission shall not exceed the levels specified in Table 6.5.3.3.22-1. This requirement also applies for the frequency ranges that are less than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth.

Table 6.5.3.3.22-1: Additional requirements for “NS\_48”

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Protected band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| E-UTRA band 34 –  NR band n34 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1900 | - | 1915 | -15.5 | 5 | 1 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 1 |
| NOTE 1: For these adjacent bands, the emission limit could imply risk of harmful interference to UE(s) operating in the protected operating band. | | | | | | |

##### 6.5.3.3.23 Requirement for network signalled value "NS\_49"

When "NS\_49" is indicated in the cell, the power of any UE emission shall not exceed the levels specified in Table 6.5.3.3.23-1. This requirement also applies for the frequency ranges that are less than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth.

Table 6.5.3.3.23-1: Additional requirements for “NS\_49”

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Protected band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| E-UTRA band 34 -  NR band n34 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 |  |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 1 |
| Frequency range | 1915 | - | 1920 | 1.6 | 5 | 1 |
| NOTE 1: For these adjacent bands, the emission limit could imply risk of harmful interference to UE(s) operating in the protected operating band. | | | | | | |

*<End of the change>*

*<Start of the change>*

### 7.3.2 Reference sensitivity power level

The throughput shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in Annexes A.2.2.2, A.2.3.2, A3.2 and A.3.3 (with one sided dynamic OCNG Pattern OP.1 FDD/TDD for the DL-signal as described in Annex A.5.1.1/A.5.2.1) with parameters specified in Table 7.3.2-1 and Table 7.3.2-2.

Table 7.3.2-1: Two antenna port reference sensitivity QPSK PREFSENS

|  | Operating band / SCS / Channel bandwidth / Duplex-mode | | | | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | | SCS kHz | 5  MHz (dBm) | 10  MHz (dBm) | 15  MHz (dBm) | 20  MHz (dBm) | 25  MHz (dBm) | 30 MHz (dBm) | 40  MHz (dBm) | 50  MHz (dBm) | 60  MHz (dBm) | 70  MHz (dBm) | 80  MHz (dBm) | 90  MHz (dBm) | 100 MHz (dBm) | Duplex Mode | |
| n1 | | 15 | -100.0 | -96.8 | -95.0 | -93.8 | -92.7 | -91.9 | -90.6 |  |  |  |  |  |  | FDD | |
| 30 |  | -97.1 | -95.1 | -94.0 | -92.8 | -92.0 | -90.7 |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 | -93.0 | -92.1 | -90.9 |  |  |  |  |  |  |
| n2 | | 15 | -98.0 | -94.8 | -93.0 | -91.8 |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -95.1 | -93.1 | -92.0 |  |  |  |  |  |  |  |  |  |
| 60 |  | -95.5 | -93.4 | -92.2 |  |  |  |  |  |  |  |  |  |
| n3 | | 15 | -97.0 | -93.8 | -92.0 | -90.8 | -89.7 | -88.9 |  |  |  |  |  |  |  | FDD | |
| 30 |  | -94.1 | -92.1 | -91.0 | -89.8 | -89.0 |  |  |  |  |  |  |  |
| 60 |  | -94.5 | -92.4 | -91.2 | -90.0 | -89.1 |  |  |  |  |  |  |  |
| n5 | | 15 | -98.0 | -94.8 | -93.0 | -86.8 |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -95.1 | -93.1 | -88.6 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n71 | | 15 | -98.0 | -94.8 | -93.0 | -91.8 | -90.7 | -89.9 | -88.6 | -81.5 |  |  |  |  |  | FDD | |
| 30 |  | -95.1 | -93.1 | -92.0 | -90.8 | -90.0 | -88.7 | -81.5 |  |  |  |  |  |
| 60 |  | -95.5 | -93.4 | -92.2 | -91.0 | -90.1 | -88.9 | -81.5 |  |  |  |  |  |
| n8 | | 15 | -97.0 | -93.8 | -91.4 | -85.8 |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -94.1 | -91.7 | -87.2 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | | 15 | -97.0 | -93.8 | -84.0 |  |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -94.1 | -84.1 |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | | 15 | -97.0 | -93.8 |  |  |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -94.1 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | | 15 | -100.0 | -96.8 | -95.0 |  |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -97.1 | -95.1 |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n20 | | 15 | -97.0 | -93.8 | -91.0 | -89.8 |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -94.1 | -91.1 | -90.0 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n25 | | 15 | -96.5 | -93.3 | -91.5 | -90.3 | -89.3 | -82.2 | -79.5 |  |  |  |  |  |  | FDD | |
| 30 |  | -93.6 | -91.6 | -90.5 | -89.4 | -82.3 | -79.6 |  |  |  |  |  |  |
| 60 |  | -94.0 | -91.9 | -90.7 | -89.6 | -82.4 | -79.7 |  |  |  |  |  |  |
| n26 | | 15 | -97.56 | -94.56 | -92.76 | -87.6 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -94.86 | -92.76 | -87.7 |  |  |  |  |  |  |  |  |  |
|  | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n28 | | 15 | -98.5 | -95.5 | -93.5 | -90.8 |  | [-78.5] |  |  |  |  |  |  |  | FDD | |
| 30 |  | -95.6 | -93.6 | -91.0 |  | [-78.6] |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | | 15 | -99.0 | -95.8 |  |  |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -96.1 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | | 15 | -100.0 | -96.8 | -95.0 |  |  |  |  |  |  |  |  |  |  | TDD | |
| 30 |  | -97.1 | -95.1 |  |  |  |  |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 |  |  |  |  |  |  |  |  |  |  |
| n381 | | 15 | -100.0 | -96.8 | -95.0 | -93.8 | -92.7 | -91.9 | -90.6 |  |  |  |  |  |  | TDD | |
| 30 |  | -97.1 | -95.1 | -94.0 | -92.8 | -92.0 | -90.7 |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 | -93.0 | -92.1 | -90.9 |  |  |  |  |  |  |
| n39 | | 15 | -100.0 | -96.8 | -95.0 | -93.8 | -92.7 | -91.9 | -90.6 |  |  |  |  |  |  | TDD | |
| 30 |  | -97.1 | -95.1 | -94.0 | -92.8 | -92.0 | -90.7 |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 | -93.0 | -92.1 | -90.9 |  |  |  |  |  |  |
| n40 | | 15 | -100.0 | -96.8 | -95.0 | -93.8 | -92.7 | -91.9 | -90.6 | -89.6 |  |  |  |  |  | TDD | |
| 30 |  | -97.1 | -95.1 | -94.0 | -92.8 | -92.0 | -90.7 | -89.7 | -88.9 |  | -87.6 |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 | -93.0 | -92.1 | -90.9 | -89.8 | -89.1 |  | -87.6 |  |  |
| n411 | | 15 |  | -94.8 | -93.0 | -91.8 |  | -89.9 | -88.6 | -87.6 |  |  |  |  |  | TDD | |
| 30 |  | -95.1 | -93.1 | -92.0 |  | -90.0 | -88.7 | -87.7 | -86.9 |  | -85.6 | -85.1 | -84.7 |
| 60 |  | -95.5 | -93.4 | -92.2 |  | -90.1 | -88.9 | -87.8 | -87.1 |  | -85.6 | -85.1 | -84.7 |
| n481 | | 15 | -99 | -95.8 | -94.0 | -92.7 |  |  | -89.6 | -88.65 |  |  |  |  |  | TDD | |
| 30 |  | -96.1 | -94.1 | -92.9 |  |  | -89.7 | -88.75 | -87.95 |  | -86.65 | -86.15 | -85.65 |
| 60 |  | -96.5 | -94.4 | -93.1 |  |  | -89.9 | -88.85 | -88.05 |  | -86.75 | -86.25 | -85.75 |
| n50 | | 15 | -100.0 | -96.8 | -95.0 | -93.8 |  | -91.9 | -90.6 | -89.6 |  |  |  |  |  | TDD | |
| 30 |  | -97.1 | -95.1 | -94.0 |  | -92.0 | -90.7 | -89.7 | -88.9 |  | -87.6 |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 |  | -92.1 | -90.9 | -89.8 | -89.1 |  | -87.6 |  |  |
| n51 | | 15 | -100.0 |  |  |  |  |  |  |  |  |  |  |  |  | TDD | |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n53 | | 15 | -100.0 | -96.8 |  |  |  |  |  |  |  |  |  |  |  | TDD | |
| 30 |  | -97.1 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | -97.5 |  |  |  |  |  |  |  |  |  |  |  |
| n65 | | 15 | -99.5 | -96.3 | -94.5 | -93.3 |  |  |  | -89.2 |  |  |  |  |  | FDD | |
| 30 |  | -96.6 | -94.6 | -93.5 |  |  |  | -89.3 |  |  |  |  |  |
| 60 |  | -97.0 | -94.9 | -93.7 |  |  |  | -89.4 |  |  |  |  |  |
| n66 | | 15 | -99.5 | -96.3 | -94.5 | -93.3 | -92.2 | -91.4 | -90.1 |  |  |  |  |  |  | FDD | |
| 30 |  | -96.6 | -94.6 | -93.5 | -92.3 | -91.5 | -90.2 |  |  |  |  |  |  |
| 60 |  | -97.0 | -94.9 | -93.7 | -92.5 | -91.6 | -90.4 |  |  |  |  |  |  |
| n70 | | 15 | -100.0 | -96.8 | -95.0 | -93.8 | -92.7 |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -97.1 | -95.1 | -94.0 | -92.8 |  |  |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 | -93.0 |  |  |  |  |  |  |  |  |
| n71 | | 15 | -97.2 | -94.0 | -91.6 | -86.0 |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -94.3 | -91.9 | -87.4 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n74 | | 15 | -99.53 | -96.33 | -94.53 | -89.33 |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -96.63 | -94.63 | -89.53 |  |  |  |  |  |  |  |  |  |
| 60 |  | -97.03 | -94.93 | -89.63 |  |  |  |  |  |  |  |  |  |
| n771,4 | | 15 |  | -95.3 | -93.5 | -92.2 | -91.2 | -90.4 | -89.1 | -88.1 |  |  |  |  |  | TDD | |
| 30 |  | -95.6 | -93.6 | -92.4 | -91.3 | -90.5 | -89.2 | -88.2 | -87.4 | -86.7 | -86.1 | -85.6 | -85.1 |
| 60 |  | -96.0 | -93.9 | -92.6 | -91.5 | -90.6 | -89.4 | -88.3 | -87.5 | -86.8 | -86.2 | -85.7 | -85.2 |
| n781 | | 15 |  | -95.8 | -94.0 | -92.7 | -91.7 | -90.9 | -89.6 | -88.6 |  |  |  |  |  | TDD | |
| 30 |  | -96.1 | -94.1 | -92.9 | -91.8 | -91 | -89.7 | -88.7 | -87.9 | -87.2 | -86.6 | -86.1 | -85.6 |
| 60 |  | -96.5 | -94.4 | -93.1 | -92 | -91.1 | -89.9 | -88.8 | -88.0 | -87.3 | -86.7 | -86.2 | -85.7 |
| n791 | | 15 |  |  |  |  |  |  | -89.6 | -88.6 |  |  |  |  |  | TDD | |
| 30 |  |  |  |  |  |  | -89.7 | -88.7 | -87.9 |  | -86.6 |  | -85.6 |
| 60 |  |  |  |  |  |  | -89.9 | -88.8 | -88.0 |  | -86.7 |  | -85.7 |
| n91 | | 15 | -100 |  |  |  |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n92 | | 15 | -100 | -96.8 | -95.0 | -93.8 |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -97.1 | -95.1 | -94.0 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | | 15 | -100 |  |  |  |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n94 | | 15 | -100 | -96.8 | -95.0 | -93.8 |  |  |  |  |  |  |  |  |  | FDD | |
| 30 |  | -97.1 | -95.1 | -94.0 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: Four Rx antenna ports shall be the baseline for this operating band except for two Rx vehicular UE.  NOTE 2: The transmitter shall be set to PUMAX as defined in clause 6.2.4  NOTE 3: The requirement is modified by -0.5 dB when the assigned NR channel bandwidth is confined within 1475.9 - 1510.9 MHz.  NOTE 4: The requirement is modified by -0.5 dB when the assigned UE channel bandwidth is confined within 3300 - 3800 MHz.  NOTE 5: For these bandwidths, the minimum requirements are restricted to operation when carrier is configured as a downlink carrier part of CA configuration.  NOTE 6: Values are modified by -0.5dB when carrier channel BW is between 865MHz and 894MHz. | | | | | | | | | | | | | | | | | |

For UE(s) equipped with 4 Rx antenna ports, reference sensitivity for 2Rx antenna ports in Table 7.3.2-1 shall be modified by the amount given in ΔRIB,4R in Table 7.3.2-2 for the applicable operating bands.

Table 7.3.2-2: Four antenna port reference sensitivity allowance ΔRIB,4R

|  |  |
| --- | --- |
| Operating band | ΔRIB,4R (dB) |
| n28, n71 | -2.71 |
| n1, n2, n3, n40, n7, n34, n38, n39, n41, n66, n70 | -2.7 |
| n48, n77, n78, n79 | -2.2 |
| NOTE 1: 4 Rx operation is targeted for FWA form factor | |

The reference receive sensitivity (REFSENS) requirement specified in Table 7.3.2-1 and Table 7.3.2-2 shall be met with uplink transmission bandwidth less than or equal to that specified in Table 7.3.2-3.

Table 7.3.2-3: Uplink configuration for reference sensitivity

|  | Operating band / SCS / Channel bandwidth / Duplex mode | | | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | | SCS kHz | 5  MHz | 10  MHz | 15  MHz | 20  MHz | 25 MHz | 30 MHz | 40  MHz | 50  MHz | 60  MHz | 70  MHz | 80  MHz | 90  MHz | 100 MHz | Duplex Mode |
| n1 | | 15 | 25 | 501 | 751 | 1001 | 1281 | 1281 | 1281 |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | 501 | 641 | 641 | 641 |  |  |  |  |  |  |
| 60 |  | 101 | 18 | 24 | 301 | 301 | 301 |  |  |  |  |  |  |
| n2 | | 15 | 25 | 501 | 501 | 501 |  |  |  |  |  |  |  |  |  | FDD |
| 30 | 101 | 24 | 241 | 241 |  |  |  |  |  |  |  |  |  |
| 60 |  | 101 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| n3 | | 15 | 25 | 501 | 501 | 501 | 501 | 501 |  |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 241 | 241 | 241 | 241 |  |  |  |  |  |  |  |
| 60 |  | 101 | 101 | 101 | 101 | 101 |  |  |  |  |  |  |  |
| n5 | | 15 | 25 | 251 | 201 | 201 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n7 | | 15 | 25 | 501 | 751 | 751 | 721 | 641 | 451 | 451 |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | 361 | 361 | 321 | 201 | 201 |  |  |  |  |  |
| 60 |  | 101 | 18 | 181 | 181 | 161 | 101 | 101 |  |  |  |  |  |
| n8 | | 15 | 25 | 251 | 201 | 201 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | | 15 | 201 | 201 | 201 |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | | 15 | 201 | 201 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | | 15 | 25 | 251 | 251 |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n20 | | 15 | 25 | 201 | 202 | 202 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 102 | 102 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n25 | | 15 | 25 | 501 | 501 | 501 | 501 | 481 | 401 |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 241 | 241 | 241 | 241 | 201 |  |  |  |  |  |  |
| 60 |  | 101 | 101 | 101 | 101 | 101 | 101 |  |  |  |  |  |  |
| n26 | | 15 | 25 | 251 | 251 | 251 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | 121 | 121 |  |  |  |  |  |  |  |  |  |
| n28 | | 15 | 25 | 251 | 251 | 251 |  | 251 |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 | 101 |  | 101 |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | | 15 | 201 | 201 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | | 15 | 25 | 50 | 75 |  |  |  |  |  |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 |  |  |  |  |  |  |  |  |  |  |
| 60 |  | 10 | 18 |  |  |  |  |  |  |  |  |  |  |
| n38 | | 15 | 25 | 50 | 75 | 100 | 128 | 160 | 216 |  |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 |  |  |  |  |  |  |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 |  |  |  |  |  |  |
| n39 | | 15 | 25 | 50 | 75 | 100 | 128 | 160 | 216 |  |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 |  |  |  |  |  |  |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 |  |  |  |  |  |  |
| n40 | | 15 | 25 | 50 | 75 | 100 | 128 | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 | 128 | 162 |  | 216 |  |  |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 | 64 | 75 |  | 100 |  |  |
| n41 | | 15 |  | 50 | 75 | 100 |  | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 |  | 75 | 100 | 128 | 162 |  | 216 | 243 | 270 |
| 60 |  | 10 | 18 | 24 |  | 36 | 50 | 64 | 75 |  | 100 | 120 | 135 |
| n48 | | 15 | 25 | 50 | 75 | 100 |  |  | 216 |  |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 |  |  | 100 |  |  |  |  |  |  |
| 60 |  | 10 | 18 | 24 |  |  | 50 |  |  |  |  |  |  |
| n50 | | 15 | 25 | 50 | 75 | 100 |  | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 |  | 75 | 100 | 128 | 162 |  | NOTE 3 |  |  |
| 60 |  | 10 | 18 | 24 |  | 36 | 50 | 64 | 75 |  | NOTE 3 |  |  |
| n51 | | 15 | 25 |  |  |  |  |  |  |  |  |  |  |  |  | TDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n53 | | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |  |  | TDD |
| 30 |  | 24 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | 10 |  |  |  |  |  |  |  |  |  |  |  |
| n65 | | 15 | 25 | 501 | 751 | 1001 |  |  |  | 1281 |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | 501 |  |  |  | 641 |  |  |  |  |  |
| 60 |  | 101 | 18 | 24 |  |  |  | 301 |  |  |  |  |  |
| n66 | | 15 | 25 | 501 | 751 | 1001 | 1281 | 160 | 216 |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | 501 | 641 | 751 | 1001 |  |  |  |  |  |  |
| 60 |  | 101 | 18 | 24 | 301 | 361 | 501 |  |  |  |  |  |  |
| n70 | | 15 | 25 | 501 | 751 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  |
| 60 |  | 101 | 18 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  |
| n71 | | 15 | 25 | 251 | 201 | 201 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n74 | | 15 | 25 | 251 | 251 | 251 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  | 51 | 51 | 51 |  |  |  |  |  |  |  |  |  |
| n77 | | 15 |  | 50 | 75 | 100 | 128 | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 | 128 | 162 | 180 | 216 | 243 | 270 |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 | 64 | 75 | 90 | 100 | 120 | 135 |
| n78 | | 15 |  | 50 | 75 | 100 | 128 | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 | 128 | 162 | 180 | 216 | 243 | 270 |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 | 64 | 75 | 90 | 100 | 120 | 135 |
| n79 | | 15 |  |  |  |  |  |  | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  |  |  |  |  |  | 100 | 128 | 162 |  | 216 |  | 270 |
| 60 |  |  |  |  |  |  | 50 | 64 | 75 |  | 100 |  | 135 |
| n91 | | 15 | 254 | 201,4 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n92 | | 15 | 25 | 201 | 201 | 201 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | | 15 | 254 | 251,4 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n94 | | 15 | 25 | 251 | 201 | 201 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission bandwidth configuration for the channel bandwidth (Table 5.3.2-1).  NOTE 2: For Band 20; for 15 kHz SCS, in the case of 15 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 11 and in the case of 20 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 16; for 30 kHz SCS, in the case of 15 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 6 and in the case of 20 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 8; for 60 kHz SCS, in the case of 15 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 3 and in the case of 20 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 4;  NOTE 3: For DL channel bandwidths that do not have symmetric UL channel bandwidth, highest valid UL configuration with lowest TX-RX separation (Table 5.4.4-1) shall be used.  NOTE 4: For band n91 and n93, largest supported UL bandwidth configuration shall be used. | | | | | | | | | | | | | | | | |

*<end of the change>*