**3GPP TSG-RAN WG4 Meeting # 95-e R4-2008923**

Electronic Meeting, 25 May – 5 June, 2020

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.104** | **CR** |  | **rev** | **-** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR for TS 38.104: introduction of NR band n13 |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_n13-Core |  | ***Date:*** | 2020-06-01 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Introduction of NR band n13 in TS 38.104 |
|  |  |
| ***Summary of change:*** |  The requirements for n13 are added in relevant clauses. |
|  |  |
| ***Consequences if not approved:*** |  NR band n13 would not be supported. |
|  |  |
| ***Clauses affected:*** | 5.2, 5.3.5, 5.4.2.3, 5.4.3.3, 6.6.4.2.1, 6.6.5.2.3, 6.6.5.2.4, |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.141-1, TS 38.141-2 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

###### *------------------------------ Modified section ------------------------------*

## 5.2 *Operating bands*

NR is designed to operate in the *operating bands* defined in table 5.2-1 and 5.2-2.

NB-IoT is designed to operate in the NR operating bands n1, n2, n3, n5, n7, n8, n12, n13, n14, n18, n20, n25, n28, n41, n65, n66, n70, n71, n74, n90 which are defined in Table 5.2-1.

Table 5.2-1: NR *operating bands* in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | Uplink (UL) *operating band*BS receive / UE transmitFUL,low – FUL,high | Downlink (DL) *operating band*BS transmit / UE receiveFDL,low – FDL,high | Duplex mode |
| n1 | 1920 MHz – 1980 MHz | 2110 MHz – 2170 MHz | FDD |
| n2 | 1850 MHz – 1910 MHz | 1930 MHz – 1990 MHz | FDD |
| n3 | 1710 MHz – 1785 MHz | 1805 MHz – 1880 MHz | FDD |
| n5 | 824 MHz – 849 MHz | 869 MHz – 894 MHz | FDD |
| n7 | 2500 MHz – 2570 MHz | 2620 MHz – 2690 MHz | FDD |
| n8 | 880 MHz – 915 MHz | 925 MHz – 960 MHz | FDD |
| n12 | 699 MHz – 716 MHz | 729 MHz – 746 MHz | FDD |
| n13 | 777 MHz – 787 MHz | 746 MHz – 756 MHz | FDD |
| n14 | 788 MHz – 798 MHz | 758 MHz – 768 MHz | FDD |
| n18 | 815 MHz – 830 MHz | 860 MHz – 875 MHz | FDD |
| n20 | 832 MHz – 862 MHz | 791 MHz – 821 MHz | FDD |
| n25 | 1850 MHz – 1915 MHz | 1930 MHz – 1995 MHz | FDD |
| n26 | 814 MHz – 849 MHz | 859 MHz – 894 MHz | FDD |
| n28 | 703 MHz – 748 MHz | 758 MHz – 803 MHz | FDD |
| n29 | N/A | 717 MHz – 728 MHz | SDL |
| n30 | 2305 MHz – 2315 MHz | 2350 MHz – 2360 MHz | FDD |
| n34 | 2010 MHz – 2025 MHz | 2010 MHz – 2025 MHz | TDD |
| n38 | 2570 MHz – 2620 MHz | 2570 MHz – 2620 MHz | TDD |
| n39 | 1880 MHz – 1920 MHz | 1880 MHz – 1920 MHz | TDD |
| n40 | 2300 MHz – 2400 MHz | 2300 MHz – 2400 MHz | TDD |
| n41 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n48 | 3550 MHz – 3700 MHz | 3550 MHz – 3700 MHz | TDD |
| n50 | 1432 MHz – 1517 MHz | 1432 MHz – 1517 MHz | TDD |
| n51 | 1427 MHz – 1432 MHz | 1427 MHz – 1432 MHz | TDD |
| n53 | 2483.5 MHz – 2495 MHz | 2483.5 MHz – 2495 MHz | TDD |
| n65 | 1920 MHz – 2010 MHz | 2110 MHz – 2200 MHz | FDD |
| n66 | 1710 MHz – 1780 MHz | 2110 MHz – 2200 MHz | FDD |
| n70 | 1695 MHz – 1710 MHz | 1995 MHz – 2020 MHz | FDD |
| n71 | 663 MHz – 698 MHz | 617 MHz – 652 MHz | FDD |
| n74 | 1427 MHz – 1470 MHz | 1475 MHz – 1518 MHz | FDD |
| n75 | N/A | 1432 MHz – 1517 MHz | SDL |
| n76 | N/A | 1427 MHz – 1432 MHz | SDL |
| n77 | 3300 MHz – 4200 MHz | 3300 MHz – 4200 MHz | TDD |
| n78 | 3300 MHz – 3800 MHz | 3300 MHz – 3800 MHz | TDD |
| n79 | 4400 MHz – 5000 MHz | 4400 MHz – 5000 MHz | TDD |
| n80 | 1710 MHz – 1785 MHz | N/A | SUL  |
| n81 | 880 MHz – 915 MHz | N/A | SUL  |
| n82 | 832 MHz – 862 MHz | N/A | SUL  |
| n83 | 703 MHz – 748 MHz | N/A | SUL |
| n84 | 1920 MHz – 1980 MHz | N/A | SUL |
| n86 | 1710 MHz – 1780 MHz | N/A | SUL |
| n89 | 824 MHz – 849 MHz | N/A | SUL |
| n90 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n91 | 832 MHz – 862 MHz | 1427 MHz – 1432 MHz | FDD2 |
| n92 | 832 MHz – 862 MHz | 1432 MHz – 1517 MHz | FDD2 |
| n93 | 880 MHz – 915 MHz | 1427 MHz – 1432 MHz | FDD2 |
| n94 | 880 MHz – 915 MHz | 1432 MHz – 1517 MHz | FDD2 |
| n951 | 2010 MHz – 2025 MHz | N/A | SUL  |
| NOTE 1: This band is applicable in China only.NOTE 2: Variable duplex operation does not enable dynamic variable duplex configuration by the network, and is used such that DL and UL frequency ranges are supported independently in any valid frequency range for the band. |

Table 5.2-2: NR *operating bands* in FR2

|  |  |  |
| --- | --- | --- |
| NR *operating band* | Uplink (UL) and Downlink (DL) *operating band*BS transmit/receiveUE transmit/receiveFUL,low – FUL,highFDL,low – FDL,high | Duplex mode |
| n257 | 26500 MHz – 29500 MHz | TDD |
| n258 | 24250 MHz – 27500 MHz | TDD |
| n260 | 37000 MHz – 40000 MHz | TDD |
| n261 | 27500 MHz – 28350 MHz | TDD |

###### *------------------------------ Modified section ------------------------------*

### 5.3.5 *BS channel bandwidth* per *operating band*

The requirements in this specification apply to the combination of *BS channel bandwidths*, SCS and *operating bands* shown in table 5.3.5-1 for FR1 and in table 5.3.5-2 for FR2. The *transmission bandwidth configuration* in table 5.3.2-1 and table 5.3.2-2 shall be supported for each of the *BS channel bandwidths* within the BS capability. The *BS channel bandwidths* are specified for both the Tx and Rx path.

Table 5.3.5-1: *BS channel bandwidths* and SCS per *operating band* in FR1

|  |
| --- |
| NR band / SCS / *BS channel bandwidth* |
| NR Band | SCSkHz | 5 MHz | 10 MHz | 15 MHz | 20 MHz | 25 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 70 MHz | 80 MHz | 90 MHz | 100 MHz |
| n1 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n2 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n3 | 15 | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| n5 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n7 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n8 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n13 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n20 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n25 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n26 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n28 | 15 | Yes | Yes | Yes | Yes |  | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n29 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| n38 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n39 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n40 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  | Yes |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  | Yes |
| n41 | 15 |  | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
| n48 | 15 | Yes2 | Yes | Yes | Yes |  |  | Yes | Yes1 |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  | Yes | Yes1 | Yes1 |  | Yes1 | Yes1 | Yes1 |
| 60 |  | Yes | Yes | Yes |  |  | Yes | Yes1 | Yes1 |  | Yes1 | Yes1 | Yes1 |
| n50 | 15 | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes |  |  |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes |  |  |
| n51 | 15 | Yes |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n53 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| n65 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n66 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n70 | 15 | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |
| n71 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n74 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n75 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n76 | 15 | Yes |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n77 | 15 |  | Yes | Yes  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
| n78 | 15 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
| n79 | 15 |  |  |  |  |  |  | Yes | Yes |  |  |  |  |  |
| 30 |  |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
| 60 |  |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
| n80 | 15 | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| n81 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n82 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n83 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n84 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n86 | 15 | Yes | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| n89 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n90 | 15 |  | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
| n91 | 15 | Yes | Yes3 |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n92 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | 15 | Yes | Yes3 |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n94 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n95 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an downlink SCell part of CA configurationNOTE 2: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configurationNOTE 3: For this bandwidth, it only applies for UL transmission.NOTE 4: Void. |

###### *------------------------------ Modified section ------------------------------*

#### 5.4.2.3 Channel raster entries for each *operating band*

The RF channel positions on the channel raster in each NR *operating band* are given through the applicable NR-ARFCN in table 5.4.2.3-1 for FR1 and table 5.4.2.3-2 for FR2, using the channel raster to resource element mapping in clause 5.4.2.2.

- For NR *operating bands* with 100 kHz channel raster, ΔFRaster = 20 × ΔFGlobal. In this case, every 20th NR-ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 is given as <20>.

- For NR *operating bands* with 15 kHz channel raster below 3 GHz, ΔFRaster = *I* × ΔFGlobal, where *I* ϵ {3,6}. In this case, every *Ith* NR‑ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 is given as <*I*>.

- For NR *operating bands* with 15 kHz and 60 kHz channel raster above 3 GHz, ΔFRaster = *I* ×ΔFGlobal, where *I* ϵ {1, 2}. In this case, every *Ith* NR‑ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 and table 5.4.2.3-2 is given as <*I*>.

- For frequency bands with two ΔFRaster in FR1, the higher ΔFRaster applies to channels using only the SCS that is equal to or larger than the higher ΔFRaster and SSB SCS is equal to the higher ΔFRaster.

- For frequency bands with two ΔFRaster in FR2, the higher ΔFRaster applies to channels using only the SCS that is equal to the higher ΔFRaster and the SSB SCS that is equal to or larger than the higher ΔFRaster.

Table 5.4.2.3-1: Applicable NR-ARFCN per *operating band* in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | ΔFRaster(kHz)  | Uplinkrange of NREF(First – <Step size> – Last) | Downlinkrange of NREF(First – <Step size> – Last) |
| n1 | 100 | 384000 – <20> – 396000 | 422000 – <20> – 434000 |
| n2 | 100 | 370000 – <20> – 382000 | 386000 – <20> – 398000 |
| n3 | 100 | 342000 – <20> – 357000 | 361000 – <20> – 376000 |
| n5 | 100 | 164800 – <20> – 169800 | 173800 – <20> – 178800 |
| n7 | 100 | 500000 – <20> – 514000 | 524000 – <20> – 538000 |
| n8 | 100 | 176000 – <20> – 183000 | 185000 – <20> – 192000 |
| n12 | 100 | 139800 – <20> – 143200 | 145800 – <20> – 149200 |
| n13 | 100 | 155400 – <20> – 157400 | 149200 – <20> – 151200 |
| n14 | 100 | 157600 – <20> –159600 | 151600 – <20> – 153600 |
| n18 | 100 | 163000 – <20> – 166000 | 172000 – <20> – 175000 |
| n20 | 100 | 166400 – <20> – 172400 | 158200 – <20> – 164200 |
| n25 | 100 | 370000 – <20> – 383000 | 386000 – <20> – 399000 |
| n26 | 100 | 162800 – <20> – 169800 | 171800 – <20> – 178800 |
| n28 | 100 | 140600 – <20> – 149600 | 151600 – <20> – 160600 |
| n29 | 100 | N/A | 143400 – <20> – 145600 |
| n30 | 100 | 461000 – <20> – 463000 | 470000 – <20> – 472000 |
| n34 | 100 | 402000 – <20> – 405000 | 402000 – <20> – 405000 |
| n38 | 100 | 514000 – <20> – 524000 | 514000 – <20> – 524000 |
| n39 | 100 | 376000 – <20> – 384000 | 376000 – <20> – 384000 |
| n40 | 100 | 460000 – <20> – 480000 | 460000 – <20> – 480000 |
| n41 | 15 | 499200 – <3> – 537999 | 499200 – <3> – 537999 |
| 30 | 499200 – <6> – 537996 | 499200 – <6> – 537996 |
| n48 | 15 | 636667 – <1> – 646666 | 636667 – <1> – 646666 |
| 30 | 636668 – <2> – 646666 | 636668 – <2> – 646666 |
| n50 | 100 | 286400 – <20> – 303400 | 286400 – <20> – 303400 |
| n51 | 100 | 285400 – <20> – 286400 | 285400 – <20> – 286400 |
| n53 | 100 | 496700 – <20> – 499000 | 496700 – <20> – 499000 |
| n65 | 100 | 384000 – <20> – 402000 | 422000 – <20> – 440000 |
| n66 | 100 | 342000 – <20> – 356000 | 422000 – <20> – 440000 |
| n70 | 100 | 339000 – <20> – 342000 | 399000 – <20> – 404000 |
| n71 | 100 | 132600 – <20> – 139600 | 123400 – <20> – 130400 |
| n74 | 100 | 285400 – <20> – 294000 | 295000 – <20> – 303600 |
| n75 | 100 | N/A | 286400 – <20> – 303400 |
| n76 | 100 | N/A | 285400 – <20> – 286400 |
| n77 | 15 | 620000 – <1> – 680000 | 620000 – <1> – 680000 |
| 30 | 620000 – <2> – 680000 | 620000 – <2> – 680000 |
| n78 | 15 | 620000 – <1> – 653333 | 620000 – <1> – 653333 |
| 30 | 620000 – <2> – 653332 | 620000 – <2> – 653332 |
| n79 | 15 | 693334 – <1> – 733333 | 693334 – <1> – 733333 |
| 30 | 693334 – <2> – 733332 | 693334 – <2> – 733332 |
| n80 | 100 | 342000 – <20> – 357000 | N/A |
| n81 | 100 | 176000 – <20> – 183000 | N/A |
| n82 | 100 | 166400 – <20> – 172400  | N/A |
| n83 | 100 | 140600 – <20> –149600 | N/A |
| n84 | 100 | 384000 – <20> – 396000 | N/A |
| n86 | 100 | 342000 – <20> – 356000 | N/A |
| n89 | 100 | 164800 – <20> – 169800 | N/A |
| n90 | 15 | 499200 – <3> – 537999 | 499200 – <3> – 537999 |
| 30 | 499200 – <6> – 537996 | 499200 – <6> – 537996 |
| 100 | 499200 – <20> – 538000 | 499200 – <20> – 538000 |
| n91 | 100 | 166400 – <20> – 172400 | 285400 – <20> – 286400 |
| n92 | 100 | 166400 – <20> – 172400 | 286400 – <20> – 303400 |
| n93 | 100 | 176000 – <20> – 183000 | 285400 – <20> – 286400 |
| n94 | 100 | 176000 – <20> – 183000 | 286400 – <20> – 303400 |
| n95 | 100 | 402000 – <20> – 405000 | N/A |

Table 5.4.2.3-2: Applicable NR-ARFCN per *operating band* in FR2

|  |  |  |
| --- | --- | --- |
| NR *operating band* | ΔFRaster(kHz)  | Uplink and Downlinkrange of NREF(First – <Step size> – Last) |
| n257 | 60 | 2054166 – <1> – 2104165 |
| 120 | 2054167 – <2> – 2104165 |
| n258 | 60 | 2016667 – <1> – 2070832 |
| 120 | 2016667 – <2> – 2070831 |
| n260 | 60 | 2229166 – <1> – 2279165 |
| 120 | 2229167 – <2> – 2279165 |
| n261 | 60 | 2070833 – <1> – 2084999 |
| 120 | 2070833 – <2> – 2084999 |

###### *------------------------------ Modified section ------------------------------*

#### 5.4.3.3 Synchronization raster entries for each operating band

The synchronization raster for each band is give in table 5.4.3.3-1. The distance between applicable GSCN entries is given by the <Step size> indicated in table 5.4.3.3-1 for FR1 and table 5.4.3.3-2 for FR2.

Table 5.4.3.3-1: Applicable SS raster entries per *operating band* (FR1)

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | SS Block SCS | SS Block pattern(note) | Range of GSCN(First – <Step size> – Last) |
| n1 | 15 kHz | Case A | 5279 – <1> – 5419 |
| n2 | 15 kHz | Case A | 4829 – <1> – 4969 |
| n3 | 15 kHz | Case A | 4517 – <1> – 4693 |
| n5 | 15 kHz | Case A | 2177 – <1> – 2230 |
| 30 kHz | Case B | 2183 – <1> – 2224 |
| n7 | 15 kHz | Case A | 6554 – <1> – 6718 |
| n8 | 15 kHz | Case A | 2318 – <1> – 2395 |
| n12 | 15 kHz | Case A | 1828 – <1> – 1858 |
| n13 | 15 kHz | Case A | 1871 – <1> – 1885 |
| n14 | 15 kHz | Case A | 1901 – <1> – 1915 |
| n18 | 15kHz | CaseA | 2156 – <1> – 2182 |
| n20 | 15 kHz | Case A | 1982 – <1> – 2047 |
| n25 | 15 kHz | Case A | 4829 – <1> – 4981 |
| n26 | 15 kHz | Case A | 2153 – <1> – 2230 |
| n28 | 15 kHz | Case A | 1901 – <1> – 2002 |
| n29 | 15 kHz | Case A | 1798 – <1> – 1813 |
| n30 | 15 kHz | Case A | 5879 – <1> – 5893 |
| n34 | 15 kHz | Case A | 5030 – <1> – 5056 |
| n38 | 15 kHz | Case A | 6431 – <1> – 6544 |
| n39 | 15 kHz | Case A | 4706 – <1> – 4795 |
| n40 | 15 kHz | Case A | 5756 – <1> – 5995 |
| n41 | 15 kHz | Case A | 6246 – <3> – 6717 |
| 30 kHz | Case C | 6252 – <3> – 6714 |
| n48 | 30 kHz | Case C | 7884 – <1> – 7982 |
| n50 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n51 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n53 | 15 kHz | Case A | 6215 – <1> – 6232 |
| n65 | 15 kHz | Case A | 5279 – <1> – 5494 |
| n66 | 15 kHz | Case A | 5279 – <1> – 5494 |
| 30 kHz | Case B | 5285 – <1> – 5488 |
| n70 | 15 kHz | Case A | 4993 – <1> – 5044 |
| n71 | 15 kHz | Case A | 1547 – <1> – 1624 |
| n74 | 15 kHz | Case A | 3692 – <1> – 3790 |
| n75 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n76 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n77 | 30 kHz | Case C | 7711 – <1> – 8329 |
| n78 | 30 kHz | Case C | 7711 – <1> – 8051 |
| n79 | 30 kHz | Case C | 8480 – <16> – 8880 |
| n90 | 15 kHz | Case A | 6246 – <1> – 6717 |
| 30 kHz | Case C | 6252 – <1> – 6714 |
| n91 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n92 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n93 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n94 | 15 kHz | Case A | 3584 – <1> – 3787 |
| NOTE: SS Block pattern is defined in clause 4.1 in TS 38.213 [10]. |

Table 5.4.3.3-2: Applicable SS raster entries per *operating band* (FR2)

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | SS Block SCS | SS Block pattern(note) | Range of GSCN(First – <Step size> – Last) |
| n257  | 120 kHz | Case D | 22388 – <1> – 22558 |
| 240 kHz | Case E | 22390 – <2> – 22556 |
| n258 | 120 kHz | Case D | 22257 – <1> – 22443 |
| 240 kHz | Case E | 22258 – <2> – 22442 |
| n260  | 120 kHz | Case D | 22995 – <1> – 23166 |
| 240 kHz | Case E | 22996 – <2> – 23164 |
| n261 | 120 kHz | Case D | 22446 – <1> – 22492 |
| 240 kHz | Case E | 22446 – <2> – 22490 |
| NOTE: SS Block pattern is defined in clause 4.1 in TS 38.213 [10]. |

###### *------------------------------ Modified section ------------------------------*

#### 6.6.4.2 *Basic limits*

##### 6.6.4.2.1 *Basic limits* for Wide Area BS (Category A)

For BS operating in Bands n5, n8, n12, n13, n14, n18, n26, n28, n29, n71, *basic limits* are specified in table 6.6.4.2.1‑1.

Table 6.6.4.2.1-1: Wide Area BS operating band unwanted emission limits
(NR bands below 1 GHz) for Category A

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limits* (Note 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.05 MHz ≤ f\_offset < f\_offsetmax  | -13 dBm (Note 3) | 100 kHz  |
| NOTE 1: For a BS supporting *non-contiguous spectrum* operation within any *operating band*, the emission limits within *sub-block gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *sub-block gap*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *sub-block gap*, where the emission limits within *sub-block gaps* shall be -13 dBm/100 kHz.NOTE 2: For a *multi-band connector* with *Inter RF Bandwidth gap* < 2\*ΔfOBUE the emission limits within the *Inter RF Bandwidth gap*s is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or RF Bandwidth on each side of the *Inter RF Bandwidth gap*.NOTE 3: The requirement is not applicable when Δfmax < 10 MHz. |

For BS operating in Bands n1, n2, n3, n7, n25, n30, n34, n38, n39, n40, n41, n48, n50, n65, n66, n70, n74, n75, n77, n78, n79, n90, n92, n94, *basic limits* are specified in table 6.6.4.2.1-2:

Table 6.6.4.2.1-2: Wide Area BS *operating band* unwanted emission limits
(NR bands above 1 GHz) for Category A

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limits* (Note 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.5 MHz ≤ f\_offset < f\_offsetmax  | -13 dBm (Note 3) | 1MHz  |
| NOTE 1: For a BS supporting *non-contiguous spectrum* operation within any *operating band*, the emission limits within *sub-block gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *sub-block gap*, where the contribution from the far-end *sub-block* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *sub-block gap*, where the emission limits within *sub-block gaps* shall be ‑13 dBm/1 MHz.NOTE 2: For a *multi-band connector* with *Inter RF Bandwidth gap* < 2\*ΔfOBUE the emission limits within the *Inter RF Bandwidth gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or RF Bandwidth on each side of the *Inter RF Bandwidth gap*, where the contribution from the far-end *sub-block* or RF Bandwidth shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or RF Bandwidth.NOTE 3: The requirement is not applicable when Δfmax < 10 MHz. |

##### 6.6.4.2.2 Basic limits for Wide Area BS (Category B)

For Category B Operating band unwanted emissions, there are two options for the *basic limits* that may be applied regionally. Either the *basic limits* in clause 6.6.4.2.2.1 or clause 6.6.4.2.2.2 shall be applied.

###### 6.6.4.2.2.1 Category B requirements (Option 1)

For BS operating in Bands n5, n8, n12, n20, n26, n28, n29, n71, the *basic limits* are specified in table 6.6.4.2.2.1-1:

Table 6.6.4.2.2.1-1: Wide Area BS operating band unwanted emission limits
(NR bands below 1 GHz) for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limits* (Note 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.05 MHz ≤ f\_offset < f\_offsetmax  | -16 dBm (Note 3) | 100 kHz  |
| NOTE 1: For a BS supporting *non-contiguous spectrum* operation within any *operating band*, the emission limits within *sub-block gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *sub-block gap*, where the contribution from the far-end *sub-block* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *sub-block gap*, where the emission limits within *sub-block gaps* shall be ‑16 dBm/100 kHz.NOTE 2: For a *multi-band connector* with *Inter RF Bandwidth gap* < 2\*ΔfOBUE the emission limits within the *Inter RF Bandwidth gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or RF Bandwidth on each side of the *Inter RF Bandwidth gap*, where the contribution from the far-end *sub-block* or RF Bandwidth shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or RF Bandwidth.NOTE 3: The requirement is not applicable when Δfmax < 10 MHz. |

For BS operating in Bands n1, n2, n3, n7, n25, n34, n38, n39, n40, n41, n48, n50, n65, n66, n70, n75, n77, n78, n79, n90, n92, n94, *basic limits* are specified in tables 6.6.4.2.2.1-2:

Table 6.6.4.2.2.1-2: Wide Area BS operating band unwanted emission limits
(NR bands above 1 GHz) for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limits* (Note 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.5 MHz ≤ f\_offset < f\_offsetmax  | -15 dBm (Note 3) | 1MHz  |
| NOTE 1: For a BS supporting *non-contiguous spectrum* operation within any *operating band*, the emission limits within *sub-block gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *sub-block gap*, where the contribution from the far-end *sub-block* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *sub-block gap*, where the emission limits within *sub-block gaps* shall be ‑15 dBm/1 MHz.NOTE 2: For a *multi-band connector* with *Inter RF Bandwidth gap* < 2\*ΔfOBUE the emission limits within the *Inter RF Bandwidth gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or RF Bandwidth on each side of the *Inter RF Bandwidth gap*, where the contribution from the far-end *sub-block* or RF Bandwidth shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or RF Bandwidth.NOTE 3: The requirement is not applicable when Δfmax < 10 MHz. |

###### *------------------------------ Modified section ------------------------------*

##### 6.6.5.2.3 Additional spurious emissions requirements

These requirements may be applied for the protection of system operating in frequency ranges other than the BS downlink *operating band*. The limits may apply as an optional protection of such systems that are deployed in the same geographical area as the BS, or they may be set by local or regional regulation as a mandatory requirement for an NR *operating band*. It is in some cases not stated in the present document whether a requirement is mandatory or under what exact circumstances that a limit applies, since this is set by local or regional regulation. An overview of regional requirements in the present document is given in clause 4.5.

Some requirements may apply for the protection of specific equipment (UE, MS and/or BS) or equipment operating in specific systems (GSM, CDMA, UTRA, E-UTRA, NR, etc.) as listed below.

The spurious emission *basic limits* are provided in table 6.6.5.2.3 -1 for a BS where requirements for co-existence with the system listed in the first column apply. For a *multi-band connector*, the exclusions and conditions in the Note column of table 6.6.5.2.3 -1 apply for each supported *operating band*.

Table 6.6.5.2.3-1: BS spurious emissions *basic* *limits* for BS for co-existence with systems operating in other frequency bands

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| System type for NR to co-exist with | Frequency range for co-existence requirement | *Basic limits* | *Measurement bandwidth* | Note |
| GSM900 | 921 – 960 MHz | -57 dBm | 100 kHz | This requirement does not apply to BS operating in band n8 |
| 876 – 915 MHz | -61 dBm | 100 kHz | For the frequency range 880-915 MHz, this requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
| DCS1800 | 1805 – 1880 MHz | -47 dBm | 100 kHz | This requirement does not apply to BS operating in band n3.  |
| 1710 – 1785 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
| PCS1900 | 1930 – 1990 MHz | -47 dBm | 100 kHz | This requirement does not apply to BS operating in band n2, n25 or band n70.  |
| 1850 – 1910 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n2 or n25 since it is already covered by the requirement in clause 6.6.5.2.2.  |
| GSM850 or CDMA850 | 869 – 894 MHz | -57 dBm | 100 kHz | This requirement does not apply to BS operating in band n5 or n26.  |
| 824 – 849 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n5 or n26, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band I orE-UTRA Band 1 or NR Band n1 | 2110 – 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65 |
| 1920 – 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band II orE-UTRA Band 2 or NR Band n2 | 1930 – 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2 or n70.  |
| 1850 – 1910 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band III orE-UTRA Band 3 or NR Band n3 | 1805 – 1880 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n3. |
| 1710 – 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2.  |
| UTRA FDD Band IV orE-UTRA Band 4 | 2110 – 2155 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66 |
| 1710 – 1755 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band V orE-UTRA Band 5 or NR Band n5 | 869 – 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26.  |
| 824 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band VI, XIX orE-UTRA Band 6, 18, 19 or NR Band n18 | 860 – 890 MHz  | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n18. |
| 815 – 830 MHz  | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n18, since it is already covered by the requirement in clause 6.6.5.2.2. |
| 830 – 845 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD Band VII orE-UTRA Band 7 or NR Band n7 | 2620 – 2690 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n7. |
| 2500 – 2570 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n7, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band VIII orE-UTRA Band 8 or NR Band n8 | 925 – 960 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n8. |
| 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band IX orE-UTRA Band 9 | 1844.9 – 1879.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n3. |
| 1749.9 – 1784.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band X orE-UTRA Band 10 | 2110 – 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66 |
| 1710 – 1770 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XI or XXI orE-UTRA Band 11 or 21 | 1475.9 – 1510.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92 or n94. |
| 1427.9 – 1447.9 MHz  | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| 1447.9 – 1462.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92 or n94. |
| UTRA FDD Band XII orE-UTRA Band 12 or NR Band n12 | 729 – 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n12. |
| 699 – 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n12, since it is already covered by the requirement in clause 6.6.5.2.2.For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XIII orE-UTRA Band 13 or NR band n13 | 746 – 756 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n13. |
| 777 – 787 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n13, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XIV orE-UTRA Band 14 or NR band n14 | 758 – 768 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n14. |
| 788 – 798 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n14, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  E-UTRA Band 17 | 734 – 746 MHz | -52 dBm | 1 MHz |  |
| 704 – 716 MHz | -49 dBm | 1 MHz | For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XX or E-UTRA Band 20 or NR Band n20 | 791 – 821 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n20 or n28. |
| 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XXII or E-UTRA Band 22 | 3510 – 3590 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n48, n77 or n78. |
| 3410 – 3490 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n77 or n78. |
| E-UTRA Band 24 | 1525 – 1559 MHz | -52 dBm | 1 MHz |  |
| 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD Band XXV orE-UTRA Band 25 or NR band n25 | 1930 – 1995 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, n25 or n70. |
| 1850 – 1915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n25 since it is already covered by the requirement in clause 6.6.5.2.2. For BS operating in Band n2, it applies for 1910 MHz to 1915 MHz, while the rest is covered in clause 6.6.5.2.2. |
| UTRA FDD Band XXVI orE-UTRA Band 26 or NR Band n26 | 859 – 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26.  |
| 814 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n26 since it is already covered by the requirement in clause 6.6.5.2.2. For BS operating in Band n5, it applies for 814 MHz to 824 MHz, while the rest is covered in clause 6.6.5.2.2. |
| E-UTRA Band 27 | 852 – 869 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n5. |
| 807 – 824 MHz | -49 dBm | 1 MHz | This requirement also applies to BS operating in Band n28, starting 4 MHz above the Band n28 downlink *operating band* (Note 5). |
| E-UTRA Band 28 or NR Band n28 | 758 – 803 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n20 or n28. |
| 703 – 748 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n28, since it is already covered by the requirement in clause 6.6.5.2.2.  |
| E-UTRA Band 29 or NR Band n29 | 717 – 728 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n29. |
| E-UTRA Band 30 or NR Band n30 | 2350 – 2360 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n30 |
| 2305 – 2315 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n30, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 31 | 462.5 – 467.5 MHz | -52 dBm | 1 MHz |  |
| 452.5 – 457.5 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD band XXXII or E-UTRA band 32 | 1452 – 1496 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92 or n94. |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n34. |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n2 or n25. |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n38.  |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n39. |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n41, n53 or [n90]. |
| E-UTRA Band 42 | 3400 – 3600 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 44 | 703 – 803 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n28. |
| E-UTRA Band 45 | 1447 – 1467 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 46 | 5150 – 5925 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 47 | 5855 – 5925 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 50 or NR band n50  | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 53 or NR Band n53 | 2483.5 - 2495 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n41, n53 or n90. |
| E-UTRA Band 65 or NR Band n65 | 2110 – 2200 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65.  |
| 1920 – 2010 MHz | -49 dBm | 1 MHz | For BS operating in Band n1, it applies for 1980 MHz to 2010 MHz, while the rest is covered in clause 6.6.5.2.2. This requirement does not apply to BS operating in band n65, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 66 or NR Band n66 | 2110 – 2200 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66. |
| 1710 – 1780 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 67 | 738 – 758 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n28. |
| E-UTRA Band 68 | 753 -783 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n28. |
| 698-728 MHz | -49 dBm | 1 MHz | For BS operating in Band n28, this requirement applies between 698 MHz and 703 MHz, while the rest is covered in clause 6.6.5.2.2. |
| E-UTRA Band 69 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n38. |
| E-UTRA Band 70 or NR Band n70 | 1995 – 2020 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, n25 or n70 |
| 1695 – 1710 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n70, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 71 or NR Band n71 | 617 – 652 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n71 |
| 663 – 698 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n71, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 72 | 461 – 466 MHz | -52 dBm | 1 MHz |  |
| 451 – 456 MHz | -49 dBm | 1 MHz |  |
| E-UTRA Band 74 or NR Band n74 | 1475 – 1518 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92 or n94. |
| 1427 – 1470 MHz | -49 dBm | 1MHz | This requirement does not apply to BS operating in band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 75 or NR Band n75 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 76 or NR Band n76 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75, n76, n91, n92, n93 or n94. |
| NR Band n77 | 3.3 – 4.2 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n79 |
| NR Band n80 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n81 | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n82 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n83 | 703 – 748 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n28, since it is already covered by the requirement in clause 6.6.5.2.2.  |
| NR Band n84 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n1, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 85 | 728 – 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n12.For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| 698 – 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n12, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n86 | 1710 – 1780 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n89 | 824 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n5, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n91 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75 or n76. |
| 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.6.5.5.1.2. |
| NR Band n92 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75 or n76. |
| 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.6.5.5.1.2. |
| NR Band n93 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75 or n76. |
| 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.5.1.2. |
| NR Band n94 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75 or n76. |
| 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.6.5.5.1.2. |
| NR Band n95 | 2010 – 2025 MHz | -52 dBm | 1 MHz |  |

NOTE 1: As defined in the scope for spurious emissions in this clause, except for the cases where the noted requirements apply to a BS operating in Band n28, the co-existence requirements in table 6.6.5.2.3 -1 do not apply for the ΔfOBUE frequency range immediately outside the downlink *operating band* (see table 5.2-1). Emission limits for this excluded frequency range may be covered by local or regional requirements.

NOTE 2: Table 6.6.5.2.3 -1 assumes that two *operating bands*, where the frequency ranges in table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 3: TDD base stations deployed in the same geographical area, that are synchronized and use the same or adjacent *operating bands* can transmit without additional co-existence requirements. For unsynchronized base stations, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 4: For NR Band n28 BS, specific solutions may be required to fulfil the spurious emissions limits for BS for co-existence with E-UTRA Band 27 UL *operating band*.

NOTE 5: For NR Band n29 BS, specific solutions may be required to fulfil the spurious emissions limits for NR BS for co-existence with UTRA Band XII, E-UTRA Band 12 or NR Band n12 UL operating band, E-UTRA Band 17 UL operating band or E-UTRA Band 85 UL operating band.

The following requirement may be applied for the protection of PHS. This requirement is also applicable at specified frequencies falling between ΔfOBUE below the lowest BS transmitter frequency of the downlink *operating band* and ΔfOBUE above the highest BS transmitter frequency of the downlink *operating band*. ΔfOBUE is defined in clause 6.6.1.

The spurious emission *basic limit* for this requirement is:

Table 6.6.5.2.3-2: BS spurious emissions *basic limits* for BS for co-existence with PHS

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | *Basic limit* | *Measurement Bandwidth* | Note |
| 1884.5 – 1915.7 MHz | -41 dBm | 300 kHz | Applicable when co-existence with PHS system operating in 1884.5 – 1915.7 MHz  |

Table 6.6.5.2.3-3: Void

In certain regions, the following requirement may apply to NR BS operating in Band n50 and n75 within the 1432 – 1452 MHz, and in Band n51 and Band n76. The *basic limit is* specified in Table 6.6.5.2.3-4. This requirement is also applicable at the frequency range from ΔfOBUE below the lowest frequency of the BS downlink *operating band* up to ΔfOBUE above the highest frequency of the BS downlink *operating band*.

Table 6.6.5.2.3-4: Additional operating band unwanted emission *basic limit* for NR BS operating in Band n50 and n75 within 1432 – 1452 MHz, and in Band n51 and n76

|  |  |  |
| --- | --- | --- |
| Filter centre frequency, Ffilter | *Basic limit* | *Measurement Bandwidth* |
| Ffilter = 1413.5 MHz | -42 dBm | 27 MHz |

In certain regions, the following requirement may apply to BS operating in NR Band n50 and n75 within 1492-1517 MHz and in Band n74 within 1492-1518 MHz. The maximum level of emissions, measured on centre frequencies Ffilter with filter bandwidth according to Table 6.6.5.2.3-5, shall be defined according to the *basic limits* PEM,n50/n75,a nor PEM,n50/n75,b declared by the manufacturer.

Table 6.6.5.2.3-5: *Operating band* n50, n74 and n75 declared emission above 1518 MHz

|  |  |  |
| --- | --- | --- |
| Filter centre frequency, Ffilter | Declared *basic limits* (dBm) | *Measurement bandwidth* |
| 1518.5 MHz ≤ Ffilter ≤ 1519.5 MHz | PEM, n50/n75,a | 1 MHz |
| 1520.5 MHz ≤ Ffilter ≤ 1558.5 MHz | PEM,n50/n75,b | 1 MHz |

In certain regions, the following requirement shall be applied to BS operating in Band n13 and n14 to ensure that appropriate interference protection is provided to 700 MHz public safety operations. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the BS downlink operating band up to 10 MHz above the highest frequency of the BS downlink operating band.

The power of any spurious emission shall not exceed:

Table 6.6.5.2.3-6: BS Spurious emissions limits for protection of 700 MHz public safety operations

|  |  |  |  |
| --- | --- | --- | --- |
| Operating Band | Frequency range | Maximum Level | *Measurement Bandwidth* |
| n13 | 763 - 775 MHz | -46 dBm | 6.25 kHz |
| n13 | 793 - 805 MHz | -46 dBm | 6.25 kHz |
| n14 | 769 - 775 MHz | -46 dBm | 6.25 kHz |
| n14 | 799 - 805 MHz | -46 dBm | 6.25 kHz |

In certain regions, the following requirement may apply to NR BS operating in Band n30. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the BS downlink operating band up to 10 MHz above the highest frequency of the BS downlink operating band.

The power of any spurious emission shall not exceed:

Table 6.6.5.2.3-7: Additional NR BS Spurious emissions limits for Band n30

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | *Basic limit* | *Measurement Bandwidth* | Note |
| 2200 – 2345 MHz | -45 dBm | 1 MHz |  |
| 2362.5 – 2365 MHz | -25 dBm | 1 MHz |  |
| 2365 – 2367.5 MHz | -40 dBm | 1 MHz |  |
| 2367.5 – 2370 MHz | -42 dBm | 1 MHz |  |
| 2370 – 2395 MHz | -45 dBm | 1 MHz |  |

The following requirement may apply to BS operating in Band n48 in certain regions. The power of any spurious emission shall not exceed:

Table 6.6.5.2.3-8: Additional BS Spurious emissions limits for Band n48

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | Maximum Level | *Measurement Bandwidth* (NOTE) | Note |
| 3530 MHz – 3720 MHz | -25 dBm | 1 MHz | Applicable 10 MHz from the assigned *channel edge*  |
| 3100 MHz – 3530 MHz3720 MHz – 4200 MHz | -40 dBm | 1 MHz |  |

NOTE: The resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. However, to improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth may be smaller than the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.

NOTE: The regional requirement, included in [12], is defined in terms of EIRP, which is dependent on both the BS emissions at the *antenna connector* and the deployment (including antenna gain and feeder loss). The requirement defined above provides the characteristics of the base station needed to verify compliance with the regional requirement. The assessment of the EIRP level is described in Annex F.

The following requirement shall be applied to BS operating in Band n26 to ensure that appropriate interference protection is provided to 800 MHz public safety operations. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the BS downlink operating band up to 10 MHz above the highest frequency of the BS downlink operating band.

The power of any spurious emission shall not exceed:

Table 6.6.5.2.3-9: BS Spurious emissions limits for protection of 800 MHz public safety operations

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Frequency range | Maximum Level | Measurement Bandwidth | Note |
| n26 | 851 - 859 MHz | -13 dBm | 100 kHz | Applicable for offsets > 37.5kHz from the channel edge |

###### *------------------------------ Modified section ------------------------------*

##### 6.6.5.2.4 Co-location with other base stations

These requirements may be applied for the protection of other BS receivers when GSM900, DCS1800, PCS1900, GSM850, CDMA850, UTRA FDD, UTRA TDD, E-UTRA and/or NR BS are co-located with a BS.

The requirements assume a 30 dB coupling loss between transmitter and receiver and are based on co-location with base stations of the same class.

The *basic limits* are in table 6.6.5.2.4-1 for a BS where requirements for co-location with a BS type listed in the first column apply, depending on the declared Base Station class. For a *multi-band connector*, the exclusions and conditions in the Note column of table 6.6.5.2.4-1 shall apply for each supported *operating band*.

Table 6.6.5.2.4-1: BS spurious emissions *basic* limits for BS co-located with another BS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Type of co-located BS | Frequency range for co-location requirement | *Basic limits* | Measurement bandwidth | Note |
| WA BS | MR BS | LA BS |
|  GSM900 | 876 – 915 MHz | -98 dBm | -91 dBm | -70 dBm | 100 kHz |  |
|  DCS1800 | 1710 – 1785 MHz | -98 dBm | -91 dBm | -80 dBm | 100 kHz |  |
|  PCS1900 | 1850 – 1910 MHz | -98 dBm | -91 dBm | -80 dBm | 100 kHz |  |
|  GSM850 or CDMA850 | 824 – 849 MHz | -98 dBm | -91 dBm | -70 dBm | 100 kHz |  |
| UTRA FDD Band I or E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band II or E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band III or E-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band IV or E-UTRA Band 4 | 1710 – 1755 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band V or E-UTRA Band 5 or NR Band n5 | 824 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VI, XIX or E-UTRA Band 6, 19 | 830 – 845 MHz  | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VII or E-UTRA Band 7 or NR Band n7 | 2500 – 2570 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VIII or E-UTRA Band 8 or NR Band n8 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band IX or E-UTRA Band 9 | 1749.9 – 1784.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band X or E-UTRA Band 10 | 1710 – 1770 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XI or E-UTRA Band 11 | 1427.9 –1447.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n75, n91, n92, n93 or n94 |
| UTRA FDD Band XII orE-UTRA Band 12 or NR Band n12 | 699 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XIII orE-UTRA Band 13 or NR Band n13 | 777 – 787 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XIV orE-UTRA Band 14 or NR Band n14 | 788 – 798 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 17 | 704 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 18 or NR Band n18 | 815 – 830 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XX or E-UTRA Band 20 or NR Band n20 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXI or E-UTRA Band 21 | 1447.9 – 1462.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n75, n92 or n94 |
| UTRA FDD Band XXII or E-UTRA Band 22 | 3410 – 3490 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 23 | 2000 – 2020 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 24 | 1626.5 – 1660.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXV orE-UTRA Band 25 or NR Band n25 | 1850 – 1915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXVI orE-UTRA Band 26 or NR Band n26 | 814 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 27 | 807 – 824 MHz  | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 28 or NR Band n28 | 703 – 748 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 30 or NR Band n30 | 2305 – 2315 MHz  | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 31 | 452.5 – 457.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n34 |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n2 or band n25 |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n38.  |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n39 |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n41, n53 or [n90] |
| E-UTRA Band 42 | 3400 – 3600 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 43 | 3600 – 3800 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 44 | 703 – 803 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n28 |
| E-UTRA Band 45 | 1447 – 1467 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 46 | 5150 – 5925 MHz | N/A | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 50 or NR Band n50  | 1432 – 1517 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n51, n74, n75, n91, n92, n93 or n94 |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | N/A | N/A | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n74, n75, n76, n91, n92, n93 or n94 |
| E-UTRA Band 53 or NR Band n53 | 2483.5 – 2495 MHz | N/A | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n41, n53 or n90 |
| E-UTRA Band 65 or NR Band n65 | 1920 – 2010 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 66 or NR Band n66 | 1710 – 1780 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 68 | 698 – 728 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 70 or NR Band n70 | 1695 – 1710 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 71 or NR Band n71 | 663 – 698 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 72 | 451 – 456 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 74 or NR Band n74  | 1427 – 1470 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n51, n91, n92, n93 or n94 |
| NR Band n77 | 3.3 – 4.2 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n80 | 1710 – 1785 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n81 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n82 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n83 | 703 – 748 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n84 | 1920 – 1980 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 85 | 698 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n86 | 1710 – 1780 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n89 | 824 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n91 | 832 – 862 MHz | N/A | N/A | -88 dBm | 100 kHz |  |
| NR Band n92 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n93 | 880 – 915 MHz | N/A | N/A | -88 dBm | 100 kHz |  |
| NR Band n94 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n95 | 2010 – 2025 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |

NOTE 1: As defined in the scope for spurious emissions in this clause, the co-location requirements in table 6.6.5.2.4-1 do not apply for the frequency range extending ΔfOBUE immediately outside the BS transmit frequency range of a downlink *operating band* (see table 5.2-1). The current state-of-the-art technology does not allow a single generic solution for co-location with other system on adjacent frequencies for 30dB BS-BS minimum coupling loss. However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [4].

NOTE 2: Table 6.6.5.2.4-1 assumes that two *operating bands*, where the corresponding BS transmit and receive frequency ranges in table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-location requirements may apply that are not covered by the 3GPP specifications.

NOTE 3: Co-located TDD base stations that are synchronized and using the same or adjacent *operating band* can transmit without special co-locations requirements. For unsynchronized base stations, special co-location requirements may apply that are not covered by the 3GPP specifications.

###### *------------------------------ End of modified section ------------------------------*