**3GPP TSG-RAN WG4 Meeting #95-e *R4-2008643***

**Electronic Meeting, 25 May– 05 June 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.133** | **CR** | **6894** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | RSS based RSRP measurement to IDLE mode for eMTC in normal coverage |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | LTE\_eMTC5-Core |  | ***Date:*** | 2020-05-25 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Support for RSS based RSRP measurement is introduced in release 16  |
|  |  |
| ***Summary of change:*** | Change #1: conditions for RSS based RSRP measurement in IDLE mode  |
|  |  |
| ***Consequences if not approved:*** | Not clear under what conditions the RSS measurements can be perfromed |
|  |  |
| ***Clauses affected:*** |  4.7.2.1.1, 4.7.2.1.2, 4.7.2.1.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

----------------------------------------------------- Beginning of Change 1 ------------------------------------------------------------

##### 4.7.2.1.1 Measurement and evaluation of serving cell for UE category M1 in normal coverage

The requirements in this subclause apply if UE is in the normal coverage area of the serving cell. The UE is considered to be in normal coverage area of serving cell according to RSRP, RSRP Ês/Iot, SCH\_RP and SCH Ês/Iot of the serving cell defined in Annex B.1.3 for a corresponding Band.

The requirements defined in section 4.2.2.1 apply for this section.

The UE is allowed to perform RSRP measurements based on RSS signals provided UE is configured with *rss-ConfigCarrierInfo* [2] and following conditions are met:

* At least two subframes containing RSS are available within the MPDCCH bandwidth for Nserv successive DRX cycles and the last subframe of the RSS occasion is in the window [n-5, n-1] where n is the first subframe of paging MPDCCH,
* RSS power offset (PRSS)with respect to CRS as defined in *RSS-Config* [2], where PRSS ≥ 0 dB
* RSS-based measurement period (Tmeasure,EUTRAN\_Intra\_NC andTevaluate, E-UTRAN\_Intra\_NC) is not longer than CRS-based measurement period.
* RSS periodicity (TRSS) as defined in *RSS-Config* [2]

If UE performs RSRP measurement based on RSS for serving cell, it is not expected to perform RSRP measurement based on CRS on that serving cell.

------------------------------------------------------------- End of change 1 ------------------------------------------------------------

------------------------------------------------------------- Beginning of change 2 ------------------------------------------------------

##### 4.7.2.1.2 Measurements of intra-frequency cells for UE category M1 in normal coverage

The requirements in this subclause apply if UE is in the normal coverage area of the serving cell. The UE is considered to be in normal coverage area of serving cell according to RSRP, RSRP Ês/Iot, SCH\_RP and SCH Ês/Iot of the serving cell defined in Annex B.1.3 for a corresponding Band.

The UE shall be able to identify new intra-frequency cells and perform RSRP and RSRQ measurements of identified intra-frequency cells without an explicit intra-frequency neighbour list containing physical layer cell identities.

The UE is allowed to perform RSRP measurements based on RSS signals provided UE is configured with *rss-ConfigCarrierInfo* [2] and following conditions are met:

* At least two subframes containing RSS of the measured cell are available within the MPDCCH bandwidth for 3 successive DRX cycles in the window of [n-5, n-1] and the last subframe of the RSS occasion is in the window [n-5, n-1] where n is the first subframe of paging MPDCCH
* RSS-based measurement period (Tmeasure,EUTRAN\_Intra\_NC andTevaluate, E-UTRAN\_Intra\_NC) is not longer than CRS-based measurement period.
* RSS power offset (PRSS)with respect to CRS as defined in *RSS-Config* [2], where PRSS ≥ 0 dB
* RSS periodicity (TRSS) as defined in *RSS-Config* [2]

If UE performs RSRP measurement based on RSS on detected intra-frequency cell, it is not expected to perform RSRP measurement based on CRS on that measured cell.

The UE shall be able to evaluate whether a newly detectable intra-frequency cell meets the reselection criteria defined in TS36.304 within Tdetect,EUTRAN\_Intra\_NCwhen that Treselection= 0. An intra frequency cell is considered to be detectable according to RSRP, RSRP Ês/Iot, SCH\_RP and SCH Ês/Iot defined in Annex B.1.3 for a corresponding Band.

The UE shall measure RSRP and RSRQ at least every Tmeasure,EUTRAN\_Intra\_NC for intra-frequency cells that are identified and measured according to the measurement rules.

The UE shall filter RSRP and RSRQ measurements of each measured intra-frequency cell using at least 2 measurements. Within the set of measurements used for the filtering, at least two measurements shall be spaced by at least Tmeasure,EUTRAN\_Intra\_NC/2.

The UE shall not consider a E-UTRA neighbour cell in cell reselection, if it is indicated as not allowed in the measurement control system information of the serving cell.

For an intra-frequency cell that has been already detected, but that has not been reselected to, the filtering shall be such that the UE shall be capable of evaluating that the intra-frequency cell has met reselection criterion defined [1] within Tevaluate,E-UTRAN\_Intra\_NC when Treselection = 0, provided that the cell is at least 4dB better ranked for Cat-M1 UE.

If Treselection timer has a non zero value and the intra-frequency cell is better ranked than the serving cell, the UE shall evaluate this intra-frequency cell for the Treselection time. If this cell remains better ranked within this duration, then the UE shall reselect that cell.

For UE not configured with eDRX\_IDLE cycle, Tdetect,EUTRAN\_Intra\_NC, Tmeasure,EUTRAN\_Intra\_NC and Tevaluate, E-UTRAN\_Intra\_NC are specified in Table 4.7.2.1.2-1. For UE configured with eDRX\_IDLE cycle, Tdetect,EUTRAN\_Intra\_NC, Tmeasure,EUTRAN\_Intra\_NC and Tevaluate, E-UTRAN\_Intra\_NC are specified in Table 4.7.2.1.2-2, where the requirements apply provided that the serving cell is configured with eDRX\_IDLE and is the same in all PTWs during any of Tdetect,EUTRAN\_Intra\_NC, Tmeasure,EUTRAN\_Intra\_NC and Tevaluate, E-UTRAN\_Intra\_NC when multiple PTWs are used.

Table 4.7.2.1.2-1 : Tdetect,EUTRAN\_Intra\_NC, Tmeasure,EUTRAN\_Intra\_NC and Tevaluate, E-UTRAN\_Intra\_NC

|  |  |  |  |
| --- | --- | --- | --- |
| DRX cycle length [s] | Tdetect,EUTRAN\_Intra\_NC [s] (number of DRX cycles) | Tmeasure,EUTRAN\_Intra\_NC [s] (number of DRX cycles) | Tevaluate,E-UTRAN\_intra\_NC[s] (number of DRX cycles) |
| 0.32 | 11.52 (36) | 1.28 x N1 (4 x N1) | 5.12 x N1 (16 x N1) |
| 0.64 | 17.92 (28) | 1.28 x N1 (2 x N1) | 5.12 x N1 (8 x N1) |
| 1.28 | 32(25) | 1.28 x N1 (1 x N1) | 6.4 x N1 (5 x N1) |
| 2.56 | 58.88 (23) | 2.56 x N1 (1 x N1) | 7.68 x N1 (3 x N1) |
| Note 1: N1 = 3 x TRSS if RSRP is measured on RSS signals defined in *RSS-Config* [2].; otherwise N1=1. |

Table 4.7.2.1.2-2: Tdetect,EUTRAN\_Intra\_NC, Tmeasure,EUTRAN\_Intra\_NC and Tevaluate,E-UTRAN\_Intra\_NC for UE configured with eDRX\_IDLE cycle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| eDRX\_IDLE cycle length [s] | DRX cycle length [s] | PTW length [s] (number of 1.28s periods) | Tdetect,EUTRAN\_Intra\_NC [s] (number of DRX cycles) | Tmeasure,EUTRAN\_Intra\_NC [s] (number of DRX cycles) | Tevaluate,E-UTRAN\_intra\_NC[s] (number of DRX cycles) |
| 5.12 ≤ eDRX\_IDLE cycle length ≤ 2621.44 | 0.32 | ≥1.28 (1) |  (23) | 0.32 x N1 (1 x N1) | 0.64 x N1 (2 x N1) |
| 0.64 | ≥1.28 (1) | 0.64 x N1 (1 x N1) | 1.28 x N1 (2 x N1) |
| 1.28 | ≥2.56 (2) | 1.28 x N1 (1 x N1) | 2.56 x N1 (2 x N1) |
| 2.56 | ≥5.12 (4) | 2.56 x N1 (1 x N1) | 5.12 x N1 (2 x N1) |
| NOTE 1: The number of DRX cycles in this table is given for the DRX cycles within PTWs.NOTE 2: The eDRX\_IDLE cycle lengths are as specified in Section 10.5.5.32 of TS 24.008 [34].Note 3: 3 x TRSS if RSRP is measured on RSS signals defined in *RSS-Config* [2].; otherwise N1=1. |

For any requirement in this section, when the UE transitions between any two states when being configured with eDRX\_IDLE, being configured with eDRX\_IDLE cycle, changing eDRX\_IDLE cycle length, or changing PTW configuration, the UE shall meet the transition requirement, which is the less stringent requirement of the two requirements corresponding to the first state and the second state, during the transition time interval which is the time corresponding to the transition requirement. After the transition time interval, the UE has to meet the requirement corresponding to the second state.

If all the relaxed monitoring criteria defined in clause 5.2.4.12 of TS 36.304 [1] are fulfilled then the UE's intra-frequency measurement is not required to meet Tdetect,EUTRAN\_Intra\_NC, Tmeasure,EUTRAN\_Intra\_NC and Tevaluate,E-UTRAN\_intra\_NC as defined in Table 4.7.2.1.2-1 and Table 4.7.2.1.2-2.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |

##### 4

------------------------------------------------------------- End of change 2 ------------------------------------------------------------