**3GPP TSG-RAN4 Meeting #96-e *Draft R4-201xxxx***

**Online, 17th Aug - 28th Aug 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-4** | **CR** | **0058** | **rev** | **1** | **Current version:** | **15.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to ZP-CSI-RS configuration |
|  |  |
| ***Source to WG:*** | Anritsu Limited |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Perf |  | ***Date:*** | 2020-08-25 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | With the current test configuration, Aperiodic ZP-CSI-RS cannot be scheduled hence test cannot be carried out properly. Details :1. Aperiodic ZP-CSI-RS is scheduled with DCI Format 1-1(DL grant, i.e. with PDSCH)(Ref. 38.212 / 7.3.1.2.2) on slot#1 according to test parameter.
2. Aperiodic NZP-CSI-RS is sent on slot#1 according to test parameter.
3. Annex A.4 Note 2 says, PDSCH is not scheduled on slots containing CSI-RS.

*Annex A.4**Note 2: PDSCH is not scheduled on slots containing CSI-RS or slots which are not full DL*According to 2), slot#1 includes NZP-CSI-RS, then PDSCH cannot be scheuled according to 3). Hence, Aperiodic ZP-CSI-RS scheduling 1), which requires DCI 1-1 (DL Grant, with PDSCH), cannot be carried on slot#1.ZP CSI RS trigger for ZP CSI-RS configuration is not necessary any more since it is associated with “aperiodic” ZP CSI-RS and now we configure “periodic” ZP CSI-RS. |
|  |  |
| ***Summary of change:*** | Resource type of ZP CSI-RS is changed from “Aperiodic” to “Periodic” so that no DCI 1-1 (DL grant, i.e. with PDSCH) transmission is required on slot#1.Periodicity of Periodic ZP CSI-RS is set to X slot with offset 1 so that it is sent on the same timing as Aperiodic NZP-CSI-RS X: Depends on test conditions.ZP CSI-RS trigger at ZP CSI-RS configuration is removed. |
|  |  |
| ***Consequences if not approved:*** | ZP CSI-RS cannot be scheduled then test in 38.521-4 cannot be carried out with the proper condition. |
|  |  |
| ***Clauses affected:*** | 6.3.2.1.1, 6.3.2.1.2, 6.3.2.2.1, 6.3.2.2.2, 6.3.3.1.1, 6.3.6.1.2, 6.3.3.2.1, 6.3.3.2.2, 8.2.2.2.2.1, 8.3.2.2.1, 8.4.2.2**Isolated impact analysis:**No change to UE requirements, changes test parameters only. |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.521-4 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Other Test cases having the same issue : These Test cases will be corrected in the next meeting if the way to solve the issue is agreed at RAN4#96-e.  |
|  |  |
| ***This CR's revision history:*** | R1 : Added the relevant test cases. |

<<Start of change>>

### 6.3.2 2RX requirements

#### 6.3.2.1 FDD

##### 6.3.2.1.1 Single PMI with 4TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.2.1.1-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.2.1.1-2.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |

Table 6.3.2.1.1-1: Test parameters (single layer)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 10 |
| Subcarrier spacing | kHz | 15 |
| Duplex Mode |  | FDD |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 4 x 2(N1,N2) = (2,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 5/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 4, (0,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) |
| CSI-RSinterval and offset |  | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Patten 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| CSI-IM configuration | CSI-IM RE pattern |  | Patten 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | 5/1 |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 4 |
| CSI request |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 6 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.1-6.1 FDD |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (1 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-3), this reported PMI cannot be applied at the gNB downlink before slot#(n+3).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.2.1.1-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.3 |

##### 6.3.2.1.2 Single PMI with 8TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.2.1.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.2.1.2-2.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |

Table 6.3.2.1.2-1: Test parameters (dual-layer)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 10 |
| Subcarrier spacing | kHz | 15 |
| Duplex Mode |  | FDD |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 8 x 2(N1,N2) = (4,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 5/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 8 |
| CDM Type |  | CDM4 (FD2, TD2) |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 8, (4,6) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (5,-) |
| CSI-RSinterval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 5 |
| CSI request |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (4,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 0x FFFF |
| RI Restriction |  | 00000010 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 8 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.1-6.2  |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (1 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.2.1.2-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.5 |

#### 6.3.2.2 TDD

##### 6.3.2.2.1 Single PMI with 4TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.2.2.1-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.2.2.1-2.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |

Table 6.3.2.2.1-1: Test parameters (single layer)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 40 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD DL-UL configuration |  | FR1.30-1 as specified in Annex A |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 4 x 2(N1,N2) = (2,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 4, (0,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) |
| CSI-RSinterval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 16 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 8 |
| CSI request |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 5.5 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.2-8.1 TDD |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot #n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.2.2.1-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.3 |

##### 6.3.2.2.2 Single PMI with 8TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.2.2.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.2.2.2-2.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |

Table 6.3.2.2.2-1: Test parameters (dual-layer)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 40 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD DL-UL configurations |  | FR1.30-1 as specified in Annex A |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 8 x 2(N1,N2) = (4,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 8 |
| CDM Type |  | CDM4 (FD2, TD2) |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 8, (4,6) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (5,-) |
| CSI-RSinterval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForIChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 16 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 8 |
| CSI request |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (4,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 0x FFFF |
| RI Restriction |  | 00000010 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 6.5 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.2-8.2 TDD |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-6), this reported PMI cannot be applied at the gNB downlink before slot#(n+6).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.2.2.2-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.5 |

### 6.3.3 4RX requirements

#### 6.3.3.1 FDD

##### 6.3.3.1.1 Single PMI with 4TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.3.1.1-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.3.1.1-2.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |

Table 6.3.3.1.1-1: Test parameters (single layer)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 10 |
| Subcarrier spacing | kHz | 15 |
| Duplex Mode |  | FDD |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 4 x 4(N1,N2) = (2,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 5/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 4, (0,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) |
| CSI-RSinterval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 4 |
| CSI request |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 6 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.1-6.1 FDD |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (1 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-3), this reported PMI cannot be applied at the gNB downlink before slot#(n+3).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.3.1.1-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.3 |

##### 6.3.3.1.2 Single PMI with 8TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.3.1.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.3.1.2-2.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |

Table 6.3.3.1.2-1: Test parameters (dual-layer)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 10 |
| Subcarrier spacing | kHz | 15 |
| Duplex Mode |  | FDD |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 8 x 4(N1,N2) = (4,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 5/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 8 |
| CDM Type |  | CDM4 (FD2, TD2) |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 8, (4,6) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (5,-) |
| CSI-RSinterval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 5 |
| CSI request |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (4,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 0x FFFF |
| RI Restriction |  | 00000010 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 8 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.1-6.2 FDD |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (1 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.3.1.2-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.5 |

#### 6.3.3.2 TDD

##### 6.3.3.2.1 Single PMI with 4TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.3.2.1-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.3.2.1-2.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |

Table 6.3.3.2.1-1: Test parameters (single layer)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 40 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD DL-UL configuration |  | FR1.30-1 as specified in Annex A |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 4 x 4(N1,N2) = (2,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 4, (0,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) |
| CSI-RSinterval and offset |  | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 16 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 8 |
| CSI request |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 5.5 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.2-8.1 TDD |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.3.2.1-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.3 |

##### 6.3.3.2.2 Single PMI with 8TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.3.2.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.3.2.2-2.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |

Table 6.3.3.2.2-1: Test parameters (dual-layer)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 40 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD DL-UL configurations |  | FR1.30-1 as specified in Annex A |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 8 x 4(N1,N2) = (4,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 8 |
| CDM Type |  | CDM4 (FD2, TD2) |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 8, (4,6) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (5,-) |
| CSI-RSinterval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannnelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 16 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 8 |
| CSI request |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (4,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 0x FFFF |
| RI Restriction |  | 00000010 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 6.5 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.2-8.2 TDD |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-6), this reported PMI cannot be applied at the gNB downlink before slot#(n+6).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.3.2.2-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.5 |

<< Unchaged sections skipped >>

##### 8.2.2.2.2 CQI reporting under fading conditions

8.2.2.2.2.1 Minimum requirement for wideband CQI reporting

The purpose of the requirements is to verify that the UE is tracking the channel variations and selecting the largest transport format possible according to the prevailing channel state for the frequency non-selective scheduling.

The reporting accuracy of CQI under frequency non-selective fading conditions is determined by the reporting variance, the relative increase of the throughput obtained when the transport format is indicated by the reported CQI compared to the throughput obtained when a fixed transport format is configured according to the reported median CQI, and a minimum BLER using the transport formats indicated by the reported CQI. To account for sensitivity of the input SNR the CQI reporting under frequency non-selective fading conditions is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 8.2.2.2.2.1-1 and using the downlink physical channels specified in Annex C.5.1, the minimum requirements are specified by the following:

a) a CQI index not in the set {median CQI -1, median CQI, median CQI +1} shall be reported at least α % of the time, where α% is specified in Table 8.2.2.2.2.1-2;

b) the ratio of the throughput obtained when transmitting the transport format indicated by each reported wideband CQI index and that obtained when transmitting a fixed transport format configured according to the wideband CQI median shall be ≥ γ, where γ is specified in Table 8.2.2.2.2.1-2;

c) when transmitting the transport format indicated by each reported wideband CQI index, the average BLER for the indicated transport formats shall be greater or equal to 0.01.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Table 8.2.2.2.2.1-1 Test parameters

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** | **Test 2** |
| Bandwidth | MHz | 100 |
| Subcarrier spacing | kHz | 120 |
| Duplex Mode |  | TDD |
| TDD Slot Configuration  |  | FR2.120-2 Annex A.1.3 |
|  SNRBB |  dB | 6 | 7 | 12 | 13 |
| Propagation channel |  | TDLA30-35 |
| Antenna configuration |  | 2×2ULA High |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | *Periodic* |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | *FD-CDM2* |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | 8 |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | 13 |
| CSI-RSinterval and offset | slot | 8/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | *Aperiodic* |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | *fd-CDM2* |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | 6 |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | 13 |
| NZP CSI-RS-timeConfiginterval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | 1 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (8, 13) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | *Aperiodic* |
| CQI-table |  | Table 1 |
| reportQuantity |  | *cri-RI-PMI-CQI* |
| timeRestrictionForChannelMeasurements |  | *Not configured* |
| timeRestrictionForInterferenceMeasurements |  | *Not configured* |
| cqi-FormatIndicator |  | *Wideband* |
| pmi-FormatIndicator |  | *Wideband* |
| Sub-band Size | RB | 8 |
| csi-ReportingBand |  | 111111111 |
| CSI-Report periodicity and offset | slot | Not configured  |
| Aperiodic Report Slot Offset |  | 6 |
| CSI request |  | 1 in slots i, where mod(i, 8) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | *typeI-SinglePanel* |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | *Not configured* |
| CodebookSubsetRestriction |  | 000001 |
| RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 1.375 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-1, TBS.1-1 |

<< Unchaged sections skipped >>

##### 8.3.2.2.1 Single PMI with 2TX TypeI-SinglePanel Codebook

For the parameters specified in Table 8.3.2.2.1-1, and using the downlink physical channels specified in Annex C.5.1, the minimum requirements are specified in Table 8.3.2.2.1-2.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |

Table 8.3.2.2.1-1: Test parameters (single layer)

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** | **Test 2** |
| Bandwidth | MHz | 100 | 100 |
| Subcarrier spacing | kHz | 120 | 120 |
| TDD DL-UL configuration |  | FR2.120-2 as specified in Annex A.1.3 | FR2.120-1 as specified in Annex A.1.3 |
| Propagation channel |  | TDLA30-35 | TDLA30-35 |
| Antenna configuration |  | 2 x 2 ULA Low | 2 x 2 ULA Low |
| Beamforming Model |  | As specified in Annex B.4.1 | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 | 4 |
| CDM Type |  | FD-CDM2 | FD-CDM2 |
| Density (ρ) |  | 1 | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 4, (8,-) | Row 4, (8,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) | (13,-) |
| CSI-RSinterval and offset | slot | 8/1 | 5/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 2 | 2 |
| CDM Type |  | FD-CDM2 | FD-CDM2 |
| Density (ρ) |  | 1 | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 3, (6,-) | Row 3, (6,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) | (13,-) |
| CSI-RSinterval and offset | slot | Not configured | Not configured |
| aperiodicTriggeringOffset |  | 0 | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic | Aperiodic |
| CSI-IM RE pattern |  | Pattern 1 | Pattern 1 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (8,13) | (8,13) |
| CSI-IM timeConfiginterval and offset | slot | Not configured | Not configured |
| ReportConfigType |  | Aperiodic | Aperiodic |
| CQI-table |  | Table 1 | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured | Not configured |
| cqi-FormatIndicator |  | Wideband | Wideband |
| pmi-FormatIndicator |  | Wideband | Wideband |
| Sub-band Size | RB | 8 | 8 |
| csi-ReportingBand |  | 111111111 | 111111111 |
| CSI-Report interval and offset | slot | Not configured | Not configured |
| Aperiodic Report Slot Offset |  | 7 | 9 |
| CSI request |  | 1 in slots i, where mod(i, 8) = 1, otherwise it is equal to 0 | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel | typeI-SinglePanel |
| Codebook Mode |  | 1 | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | N/A | N/A |
| CodebookSubsetRestriction |  | 001111 | 001111 |
| RI Restriction |  | N/A | N/A |
| Physical channel for CSI report |  | PUSCH | PUSCH |
| CQI/RI/PMI delay  | ms | 1.375 | 1.75 |
| Maximum number of HARQ transmission |  | 4 | 4 |
| Measurement channel |  | R.PDSCH.5-8.1 TDD | R.PDSCH.5-7.1 TDD |
| Note 1: For random precoder selection, the precoder shall be updated in each slot (0.125 ms granularity).Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-4)], this reported PMI cannot be applied at the gNB downlink before slot#(n+4)].Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

<< Unchaged sections skipped >>

#### 8.4.2.2 TDD

The minimum performance requirement in Table 8.4.2.2-2 is defined as

a) The ratio of the throughput obtained when transmitting based on UE reported RI and that obtained when transmitting with fixed rank 1 shall be ≥ ;

b) The ratio of the throughput obtained when transmitting based on UE reported RI and that obtained when transmitting with fixed rank 2 shall be ≥ ;

For the parameters specified in Table 8.4.2.2-1, and using the downlink physical channels specified in Annex C.5.1, the minimum requirements are specified in Table 8.4.2.2-2.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Table 8.4.2.2-1: RI Test (TDD)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** | **Test 2** | **Test 3** |
| Bandwidth | MHz | 100 | 100 | 100 |
| Subcarrier spacing | kHz | 120 | 120 | 120 |
| Duplex Mode |  | TDD | TDD | TDD |
| TDD Slot Configuration |  | FR1.120-2 | FR1.120-2 | FR1.120-2 |
| SNR  |  dB | 0 | 16 | 16 |
| Propagation channel |  | TDLA30-35 | TDLA30-35 | TDLA30-35 |
| Antenna configuration |  | ULA Low 2x2 | ULA Low 2x2 | XP High 2x2 |
| Beamforming Model |  | As defined in Annex B.4.1 | As defined in Annex B.4.1 | As defined in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic | Periodic | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 | 4 | 4 |
| CDM Type |  | FD-CDM2 | FD-CDM2 | FD-CDM2 |
| Density (ρ) |  | 1 | 1 | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 4, (8,-) | Row 4, (8,-) | Row 4, (8,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) | (13,-) | (13,-) |
| CSI-RSinterval and offset | slot | 8/1 | 8/1 | 8/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic | Aperiodic | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 2 | 2 | 2 |
| CDM Type |  | FD-CDM2 | FD-CDM2 | FD-CDM2 |
| Density (ρ) |  | 1 | 1 | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 3 (6,-) | Row 3 (6,-) | Row 3 (6,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) | (13,-) | (13,-) |
| NZP CSI-RS-timeConfiginterval and offset | slot | Not configured | Not configured | Not configured |
| aperiodicTriggeringOffset |  | 0 | 0 | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic | Periodic | Periodic |
| CSI-IM RE pattern |  | Pattern 1 | Pattern 1 | Pattern 1 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (8,13) | (8,13) | (8,13) |
| CSI-IM timeConfiginterval and offset | slot | Not configured | Not configured | Not configured |
| ReportConfigType |  | Aperiodic  | Aperiodic | Aperiodic |
| CQI-table |  | Table 1 | Table 1 | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI | cri-RI-PMI-CQI | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | not configured | not configured | not configured |
| timeRestrictionForInterferenceMeasurements |  | not configured | not configured | not configured |
| cqi-FormatIndicator |  | Wideband | Wideband | Wideband |
| pmi-FormatIndicator |  | Wideband | Wideband | Wideband |
| Sub-band Size | RB | 8 | 8 | 8 |
| csi-ReportingBand |  | 111111111 | 111111111] | 111111111 |
| CSI-Report interval and offset | slot | Not configured | Not configured | Not configured |
| Aperiodic Report Slot Offset |  | 7 | 7 | 7 |
| CSI request |  | 1 in slots i, where mod(i, 8) = 1, otherwise it is equal to 0 | 1 in slots i, where mod(i, 8) = 1, otherwise it is equal to 0 | 1 in slots i, where mod(i, 8) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 | 1 | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel | typeI-SinglePanel | typeI-SinglePanel |
| Codebook Mode |  | 1 | 1 | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | N/A | N/A | N/A |
| CodebookSubsetRestriction |  | 010000 for fixed rank 2,010011 for following rank | 000011 for fixed rank 1,010011 for following rank | 000011 for fixed rank 1,010011 for following rank |
| RI Restriction |  | N/A | N/A | N/A |
| Physical channel for CSI report |  | PUSCH | PUSCH | PUSCH |
| CQI/RI/PMI delay  | ms | 1.375 | 1.375 | 1.375 |
| Maximum number of HARQ transmission |  | 1 | 1 | 1 |
| RI Configuration |  | Fixed RI = 2 and follow RI | Fixed RI = 1 and follow RI | Fixed RI = 1 and follow RI |

<<End of change>>