**3GPP TSG-RAN4 Meeting #99-e *R4-2108304***

**Electronic meeting, May 19 – 27, 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.133** | **CR** | **draft** | **rev** | **1** | **Current version:** | **16.7.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draftCR on PRS-RSRP accuracy requirements | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | CATT | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_pos-Perf | | | | |  | ***Date:*** | | | 2021-04-30 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The performance requirements for PRS-RSRP measurement need to be specified. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Introduce the performance requirements for PRS-RSRP measurement. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The performance requirements for PRS-RSRP measurement are missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 10.1.24.2.1, 10.1.24.2.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This draft CR is the revision of R4-2109096. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

<Start of Change 1>

#### 10.1.24.2 Measurement Accuracy Requirements

##### 10.1.24.2.1 Absolute PRS RSRP accuracy

The absolute accuracy requirements for PRS-RSRP measurement for FR1 defined in Table 10.1.24.2.1-1 are valid under the following conditions:

* Conditions defined in 38.101-1 Clause 7.3 for reference sensitivity are fulfilled.
* PRP 1,2|dBm according to Annex B.2.x for a corresponding Band

The absolute accuracy requirements for PRS-RSRP measurement for FR2 defined in Table 10.1.24.2.1-2 are valid under the following conditions:

* Conditions defined in 38.101-2 Clause 7.3 for reference sensitivity are fulfilled.
* PRP 1,2|dBm according to Annex B.2.x for a corresponding Band

Table 10.1.24.2.1-1: PRS-RSRP absolute accuracy for FR1

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | | | |
| Normal condition | Extreme condition | PRS Ês/Iot | PRS BW | Repetition factor  ( | Io Note 7 range | | | | |
| NR operating band groups Note 8 | Minimum Io Note 1  dBm / SCSPRS | | | Maximum Io |
| dB | dB | dB | PRB | - |  | dBm / SCSPRS | | | dBm/BWChannel |
| dBm/15kHz Note 6 | dBm/30kHz Note 6 | dBm/60kHz Note 6 |
| [±3.5] | [TBD] | ≥-3dB | ≥24 | All | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A | -127 | -124 | -121 | -50 |
| NR\_FDD\_FR1\_B | -126.5 | -123.5 | -120.5 | -50 |
| NR\_TDD\_FR1\_C | -126 | -123 | -120 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -125.5 | -122.5 | -119.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -125 | -122 | -119 | -50 |
| NR\_FDD\_FR1\_F | -124.5 | -121.5 | -118.5 | -50 |
| NR\_FDD\_FR1\_G | -124 | -121 | -118 | -50 |
| NR\_FDD\_FR1\_H | -123.5 | -120.5 | -117.5 | -50 |
| Note 4 | | | | |
| Note 4 | | | | |
| [±7.5] | [TBD] | ≥-13dB | 24 ≤ BW ≤ 52 | All | Note 4 | | | | |
| [±5.5] | 52< BW≤ 104 | All | Note 4 | | | | |
| [±5] | BW >104 | All | Note 4 | | | | |
| NOTE 1: This minimum Io condition is expressed as the average Io per RE over all REs in an OFDM symbol.  NOTE 2: Void.  NOTE 3: PRS bandwidth is as indicated in *prs-Bandwidth* in the OTDOA or DL-AoD assistance data defined in [34].  NOTE 4: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth ≥ [24] RB.  NOTE 5: The serving cell, the reference cell, and the measured neighbour cell i are on the same carrier frequency.  NOTE 6: The condition level is increased by ∆>0, when applicable, as described in Sections B.3.2 and B.3.3.  NOTE 7: The Io is defined in PRS positioning subframes. The same Io range applies to PRS and non-PRS symbols. Io levels are different in PRS and non-PRS symbols within the same subframe.  NOTE 8: NR operating band groups are as defined in Section 3.5.2. | | | | | | | | | |

Table 10.1.24.2.1-2: PRS-RSRP absolute accuracy for FR2

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | |
| Normal condition | Extreme condition | PRS Ês/Iot | PRS BW | Repetition factor  ( | Io Note 7 range | | |
| Minimum Io Note 1  dBm / SCSPRS | | Maximum Io |
| dB | dB | dB | PRB | - | dBm / SCSPRS | | dBm/BWChannel |
| dBm/120kHz Note 6 | dBm/60kHz Note 6 |
| [±5.5] | [TBD] | ≥-3dB | ≥24 | All | Same value as PRP in Table B.2.x-2, according to UE Power class, operating band and angle of arrival | | -50 |
| Note 4 | | |
| Note 4 | | |
| [±9] | [TBD] | ≥-13dB | 24 ≤ BW ≤ 64 | All | Note 4 | | |
| [±6.5] | BW >64 | All | Note 4 | | |
| NOTE 1: This minimum Io condition is expressed as the average Io per RE over all REs in an OFDM symbol.  NOTE 2: Void.  NOTE 3: PRS bandwidth is as indicated in *prs-Bandwidth* in the OTDOA or DL-AoD assistance data defined in [34].  NOTE 4: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth ≥ [24] RB.  NOTE 5: The serving cell, the reference cell, and the measured neighbour cell i are on the same carrier frequency.  NOTE 6: The condition level is increased by ∆>0, when applicable, as described in Sections B.3.2 and B.3.3.  NOTE 7: The Io is defined in PRS positioning subframes. The same Io range applies to PRS and non-PRS symbols. Io levels are different in PRS and non-PRS symbols within the same subframe.  NOTE 8: NR operating band groups are as defined in Section 3.5.2. | | | | | | | |

##### 10.1.24.2.2 Relative PRS RSRP accuracy

The relative accuracy of PRS-RSRP is defined as the PRS-RSRP measured from one cell compared to the PRS-RSRP measured from another cell on the same frequency, or between any two PRS-RSRP levels measured on the same cell.

The accuracy requirements for PRS-RSRP measurement for FR1 defined in Table 10.1.24.2.2-1 are valid under the following conditions:

* Conditions defined in 38.101-1 Clause 7.3 for reference sensitivity are fulfilled.
* PRP 1,2|dBm according to Annex B.2.x for a corresponding Band

The accuracy requirements for PRS-RSRP measurement for FR2 defined in Table 10.1.24.2.2-2 are valid under the following conditions:

* Conditions defined in 38.101-2 Clause 7.3 for reference sensitivity are fulfilled.
* PRP 1,2|dBm according to Annex B.2.x for a corresponding Band

Table 10.1.24.2.2-1: PRS-RSRP relative accuracy for FR1

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | | | |
| Normal condition | Extreme condition | PRS Ês/Iot | PRS BW | Repetition factor  ( | Io Note 7 range | | | | |
| NR operating band groups Note 8 | Minimum Io Note 1  dBm / SCSPRS | | | Maximum Io |
| dB | dB | dB | PRB | - |  | dBm / SCSPRS | | | dBm/BWChannel |
| dBm/15kHz Note 6 | dBm/30kHz Note 6 | dBm/60kHz Note 6 |
| [±(1.2+margin)] | [TBD] | ≥-3dB | ≥[24] | All | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A | -127 | -124 | -121 | -50 |
| NR\_FDD\_FR1\_B | -126.5 | -123.5 | -120.5 | -50 |
| NR\_TDD\_FR1\_C | -126 | -123 | -120 | -50 |
| NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -125.5 | -122.5 | -119.5 | -50 |
| NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -125 | -122 | -119 | -50 |
| NR\_FDD\_FR1\_F | -124.5 | -121.5 | -118.5 | -50 |
| NR\_FDD\_FR1\_G | -124 | -121 | -118 | -50 |
| NR\_FDD\_FR1\_H | -123.5 | -120.5 | -117.5 | -50 |
| Note 4 | | | | |
| Note 4 | | | | |
| [±(5.5+margin)] | [TBD] | ≥-13dB | 24 ≤ BW ≤ 52 | All | Note 4 | | | | |
| [±(4.6+margin)] | 52< BW≤ 104 | All | Note 4 | | | | |
| [±(3.5+margin)] | BW >104 | All | Note 4 | | | | |
| NOTE 1: This minimum Io condition is expressed as the average Io per RE over all REs in an OFDM symbol.  NOTE 2: Void.  NOTE 3: PRS bandwidth is as indicated in *prs-Bandwidth* in the OTDOA or DL-AoD assistance data defined in [34].  NOTE 4: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth ≥ [24] RB.  NOTE 5: The serving cell, the reference cell, and the measured neighbour cell i are on the same carrier frequency.  NOTE 6: The condition level is increased by ∆>0, when applicable, as described in Sections B.3.2 and B.3.3.  NOTE 7: The Io is defined in PRS positioning subframes. The same Io range applies to PRS and non-PRS symbols. Io levels are different in PRS and non-PRS symbols within the same subframe.  NOTE 8: NR operating band groups are as defined in Section 3.5.2. | | | | | | | | | |

Table 10.1.24.2.2-2: PRS-RSRP relative accuracy for FR2

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | |
| Normal condition | Extreme condition | PRS Ês/Iot | PRS BW | Repetition factor  ( | Io Note 7 range | | |
| Minimum Io Note 1  dBm / SCSPRS | | Maximum Io |
| dB | dB | dB | PRB | - | dBm / SCSPRS | | dBm/BWChannel |
| dBm/120kHz Note 6 | dBm/60kHz Note 6 |
| [±(1.3+margin)] | [TBD] | ≥-3dB | ≥[24] | All | Same value as PRP in Table B.2.x-2, according to UE Power class, operating band and angle of arrival | | -50 |
| Note 4 | | |
| Note 4 | | |
| [±(5.3+margin)] | [TBD] | ≥-13dB | 24 ≤ BW ≤ 64 | All | Note 4 | | |
| [±(2.8+margin)] | BW >64 | All | Note 4 | | |
| NOTE 1: This minimum Io condition is expressed as the average Io per RE over all REs in an OFDM symbol.  NOTE 2: Void.  NOTE 3: PRS bandwidth is as indicated in *prs-Bandwidth* in the OTDOA or DL-AoD assistance data defined in [34].  NOTE 4: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding requirement with the PRS bandwidth ≥ [24] RB.  NOTE 5: The serving cell, the reference cell, and the measured neighbour cell i are on the same carrier frequency.  NOTE 6: The condition level is increased by ∆>0, when applicable, as described in Sections B.3.2 and B.3.3.  NOTE 7: The Io is defined in PRS positioning subframes. The same Io range applies to PRS and non-PRS symbols. Io levels are different in PRS and non-PRS symbols within the same subframe.  NOTE 8: NR operating band groups are as defined in Section 3.5.2. | | | | | | | |

<End of Change 1>