**3GPP TSG-RAN4 Meeting #99-e *R4-2110889***

**Electronic Meeting, May 19–27, 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **Draft** | **rev** | **-** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | draftCR to introduce TC for PRS-RSRP measurement requirements for FR1 in SA |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_pos-Perf |  | ***Date:*** | 2021-04-30 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | This draftCR is based on Big draftCR R4-2017373 endorsed at RAN4#97. According to the work split in R4-2017158, this CR introduces TC for PRS-RSRP measurement requirements for FR1 in SA. |
|  |  |
| ***Summary of change:*** | Introduces TC for PRS-RSRP measurement requirements for FR1 in SA. |
|  |  |
| ***Consequences if not approved:*** | PRS-RSRP measurement requirements for FR1 in SA is not verified. |
|  |  |
| ***Clauses affected:*** | A.6.6.8 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.533 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change 1>

### A.6.6.8 PRS-RSRP measurements

#### A.6.6.8.1 PRS-RSRP reporting delay test case for single positioning frequency layer

##### A.6.6.8.1.1 Test purpose and Environment

The purpose of the test is to verify that the PRS-RSRP measurement meets the delay requirements specified in clause 9.9.3.5 in an environment with AWGN propagation conditions.

The supported test configurations are specified in Table A.6.6.8.1.1-1.

Table A.6.6.8.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. |

In the test there are two synchronous cells: Cell 1 and Cell 2. Cell 1 is the reference as well as the PCell. Cell 2 is a neighbour cell. Both cells are on the same NR RF channel in FR1. The test consists of two consecutive time intervals, with duration of T1 and T2. Both cells transmit PRS during T2.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance aligned with the PRS resources closest in time after after both the *NR-DL-AoD-RequestLocationInformation* message and *NR-DL-AoD-ProvideAssistanceData* message from LMF via LPP [34] are delivered to UE PHY layer, where ΔT = 150 ms is the maximum processing time of the OTDOA assistance data. The DL-AoD assistance data shall be provided to the UE over the air interface during T1. The last TTI containing the DL-AoD assistance data shall be provided to the UE ΔT ms before the start of T2.

The general test parameters are listed in Table A.6.6.8.1.1-2, and cell specific test parameters are listed in Table A.6.6.8.1.1-3.

Table A.6.6.8.1.1-2: General test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Active cell |  | 1, 2, 3 | Cell 1 | Cell 1 is the PCell and the DL-AoD reference cell in the positioning assistance data. |
| Neighbour cell |  | 1, 2, 3 | Cell 2 | Cell 2 is a neighbour cell in the positioning assistance data. |
| RF Channel Number |  | 1, 2, 3 | 1: Cell 1 and Cell 2 |  |
| BWchannel | MHz | 1 | 10: NRB,c = 52 |  |
| 2 | 10: NRB,c = 52 |  |
| 3 | 40: NRB,c = 106 |  |
| SSB configuration |  | 1 | SSB.1 FR1 |  |
|  |  | 2 | SSB.1 FR1 |  |
|  |  | 3 | SSB.2 FR1 |  |
| SMTC configuration |  | 1 | SMTC.2 |  |
|  |  | 2 | SMTC.1 |  |
|  |  | 3 | SMTC.1 |  |
| Measurement gap |  | 1, 2, 3 | GP#24 or GP#0 Note 1 |  |
| CP length |  | 1, 2, 3 | Normal |  |
| DRX |  | 1, 2, 3 |  | OFF |
| Time offset between serving and neighbour cells | μs | 1, 2, 3 | 2 | Synchronous cells |
| Expected RSTD | μs | 1, 2, 3 | 3 |  |
| Expected RSTD uncertainty | μs | 1, 2, 3 | 5 |  |
| T1 | s | 1, 2, 3 | 2 |  |
| T2 | s | 1, 2, 3 | 5 |  |
| NOTE 1: GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured. |

Table A.6.6.8.1.1-3: Cell specific test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | Cell 2 |
|  |  |  | T1 | T2 | T1 | T2 |
| TDD configuration |  | 1 | N/A | N/A |
|  |  | 2 | TDDConf.1.1 | TDDConf.1.1 |
|  |  | 3 | TDDConf.2.1 | TDDConf.2.1 |
| PDSCH RMC configuration |  | 1 | SR.1.1 FDD | N/A |
|  |  | 2 | SR.1.1 TDD |  |
|  |  | 3 | SR.2.1 TDD |  |
| RMSI CORESET RMC configuration |  | 1 | CR.1.1 FDD | N/A |
|  |  | 2 | CR.1.1 TDD |
|  |  | 3 | CR.2.1 TDD |
| Dedicated CORESET RMC configuration |  | 1 | CCR.1.1 FDD | N/A |
|  |  | 2 | CCR.1.1 TDD |
|  |  | 3 | CCR.2.1 TDD |
| OCNG Patterns |  | 1, 2, 3 | OP.1 | OP.1 |
| TRS Configuration |  | 1 | TRS.1.1 FDD | N/A |
|  |  | 2 | TRS.1.1 TDD |
|  |  | 3 | TRS.1.2 TDD |
| Initial BWP configuration |  | 1, 2, 3 | DLBWP.0.1 ULBWP.0.1 | N/A |
| Active DL BWP configuration |  | 1, 2, 3 | DLBWP.1.1 | N/A |
| Active UL BWP configuration |  | 1, 2, 3 | ULBWP.1.1 | N/A |
| PRS configuration |  | 1 | PRS.1.2 FR1 | PRS.1.2 FR1 |
|  | 2 | PRS.1.2 FR1 | PRS.1.2 FR1 |
|  | 3 | PRS.2.2 FR1 | PRS.2.2 FR1 |
|  Note 2 | dBm/SCS | 1 | -98 |
|  |  | 2 | -98 |
|  |  | 3 | -95 |
|  Note 2 | dBm/15 kHz | 1 | -98 |
|  |  | 2 |  |
|  |  | 3 |  |
| PRS  | dB | 1 | -Infinity | -3 | -Infinity | -10 |
|  |  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS  | dB | 1 | -Infinity | -3 | -Infinity | -10 |
|  |  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS-RSRP Note 3 | dBm/SCS kHz | 1 | -Infinity | -101 | -Infinity | -108 |
|  |  | 2 | -Infinity | -101 | -Infinity | -108 |
|  |  | 3 | -Infinity | -98 | -Infinity | -105 |
| Io | dBm/9.36 MHz | 1 | N/A | -62.25 | N/A | -62.25 |
|  | dBm/9.36 MHz | 2 | -62.25 | -62.25 |
|  | dBm/38.16 MHz | 3 | -56.16 | -56.16 |
| Propagation Condition |  | 1, 2, 3 | AWGN |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.Note 3: SS-RSRP levels have been derived from other parameters for information purposes. They are not settable parameters themselves. |

##### A.6.6.8.1.2 Test Requirements

The UE shall perform and report the PRS-RSRP measurements for Cell 1 and Cell 2, within the time limit specified in clause 9.9.3.5, starting from the beginning of time interval T2.

The rate of correct events observed during repeated tests shall be at least 90%.

#### A.6.6.8.2 PRS-RSRP reporting delay test case for dual positioning frequency layer

##### A.6.6.8.2.1 Test purpose and Environment

The purpose of the test is to verify that the PRS-RSRP measurement meets the delay requirements specified in clause 9.9.3.5 in an environment with AWGN propagation conditions.

The supported test configurations are specified in Table A.6.6.8.2.1-1.

Table A.6.6.8.2.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. |

In the test there are two synchronous cells: Cell 1 and Cell 2. Cell 1 is the reference as well as the PCell on NR RF channel #1 in FR1. Cell 2 is a neighbour cell on a different NR RF channel #2 in FR1. The test consists of two consecutive time intervals, with duration of T1 and T2. Both cells transmit PRS during T2.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance aligned with the PRS resources closest in time after after both the *NR-DL-AoD-RequestLocationInformation* message and *NR-DL-AoD-ProvideAssistanceData* message from LMF via LPP [34] are delivered to UE PHY layer, where ΔT = 150 ms is the maximum processing time of the OTDOA assistance data. The DL-AoD assistance data shall be provided to the UE over the air interface during T1. The last TTI containing the DL-AoD assistance data shall be provided to the UE ΔT ms before the start of T2.

The general test parameters are listed in Table A.6.6.8.2.1-2, and cell specific test parameters are listed in Table A.6.6.8.2.1-3.

Table A.6.6.8.2.1-2: General test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Active cell |  | 1, 2, 3 | Cell 1 | Cell 1 is the PCell and the DL-AoD reference cell in the positioning assistance data. |
| Neighbour cell |  | 1, 2, 3 | Cell 2 | Cell 2 is a neighbour cell in the positioning assistance data. |
| RF Channel Number |  | 1, 2, 3 | 1: Cell 1 and Cell 2 |  |
| BWchannel | MHz | 1 | 10: NRB,c = 52 |  |
| 2 | 10: NRB,c = 52 |  |
| 3 | 40: NRB,c = 106 |  |
| SSB configuration |  | 1 | SSB.1 FR1 |  |
|  |  | 2 | SSB.1 FR1 |  |
|  |  | 3 | SSB.2 FR1 |  |
| SMTC configuration |  | 1 | SMTC.2 |  |
|  |  | 2 | SMTC.1 |  |
|  |  | 3 | SMTC.1 |  |
| Measurement gap |  | 1, 2, 3 | GP#24 or GP#0 Note 1 |  |
| CP length |  | 1, 2, 3 | Normal |  |
| DRX |  | 1, 2, 3 |  | OFF |
| Time offset between serving and neighbour cells | μs | 1, 2, 3 | 2 | Synchronous cells |
| Expected RSTD | μs | 1, 2, 3 | 3 |  |
| Expected RSTD uncertainty | μs | 1, 2, 3 | 5 |  |
| T1 | s | 1, 2, 3 | 2 |  |
| T2 | s | 1, 2, 3 | 10 |  |
| NOTE 1: GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured. |

Table A.6.6.8.2.1-3: Cell specific test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | Cell 2 |
|  |  |  | T1 | T2 | T1 | T2 |
| TDD configuration |  | 1 | N/A | N/A |
|  |  | 2 | TDDConf.1.1 | TDDConf.1.1 |
|  |  | 3 | TDDConf.2.1 | TDDConf.2.1 |
| PDSCH RMC configuration |  | 1 | SR.1.1 FDD | N/A |
|  |  | 2 | SR.1.1 TDD |  |
|  |  | 3 | SR.2.1 TDD |  |
| RMSI CORESET RMC configuration |  | 1 | CR.1.1 FDD | N/A |
|  |  | 2 | CR.1.1 TDD |
|  |  | 3 | CR.2.1 TDD |
| Dedicated CORESET RMC configuration |  | 1 | CCR.1.1 FDD | N/A |
|  |  | 2 | CCR.1.1 TDD |
|  |  | 3 | CCR.2.1 TDD |
| OCNG Patterns |  | 1, 2, 3 | OP.1 | OP.1 |
| TRS Configuration |  | 1 | TRS.1.1 FDD | N/A |
|  |  | 2 | TRS.1.1 TDD |
|  |  | 3 | TRS.1.2 TDD |
| Initial BWP configuration |  | 1, 2, 3 | DLBWP.0.1 ULBWP.0.1 | N/A |
| Active DL BWP configuration |  | 1, 2, 3 | DLBWP.1.1 | N/A |
| Active UL BWP configuration |  | 1, 2, 3 | ULBWP.1.1 | N/A |
| PRS configuration |  | 1 | PRS.1.2 FR1 | PRS.1.2 FR1 |
|  | 2 | PRS.1.2 FR1 | PRS.1.2 FR1 |
|  | 3 | PRS.2.2 FR1 | PRS.2.2 FR1 |
|  Note 2 | dBm/SCS | 1 | -98 |
|  |  | 2 | -98 |
|  |  | 3 | -95 |
|  Note 2 | dBm/15 kHz | 1 | -98 |
|  |  | 2 |  |
|  |  | 3 |  |
| PRS  | dB | 1 | -Infinity | -3 | -Infinity | -10 |
|  |  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS  | dB | 1 | -Infinity | -3 | -Infinity | -10 |
|  |  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| PRS-RSRP Note 3 | dBm/SCS kHz | 1 | -Infinity | -101 | -Infinity | -108 |
|  |  | 2 | -Infinity | -101 | -Infinity | -108 |
|  |  | 3 | -Infinity | -98 | -Infinity | -105 |
| Io | dBm/9.36 MHz | 1 | N/A | -62.25 | N/A | -62.25 |
|  | dBm/9.36 MHz | 2 | -62.25 | -62.25 |
|  | dBm/38.16 MHz | 3 | -56.16 | -56.16 |
| Propagation Condition |  | 1, 2, 3 | AWGN |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.Note 3: SS-RSRP levels have been derived from other parameters for information purposes. They are not settable parameters themselves. |

##### A.6.6.8.2.2 Test Requirements

The UE shall perform and report the PRS-RSRP measurements for Cell 1 and Cell 2, within the time limit specified in clause 9.9.3.5, starting from the beginning of time interval T2.

The rate of correct events observed during repeated tests shall be at least 90%.

<End of Change 1>