**3GPP TSG-RAN WG4 Meeting #99-e *Draft R4-2108741***

Electronic meeting, May19th – 27th, 2021

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.104** | **CR** |  | **rev** | 1 | **Current version:** | **17.1.0**  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to TS 38.104 – Introduction of band n262 (47GHz) |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_47GHz\_band-Core |  | ***Date:*** | 2021-05-24 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Add band n262 |
|  |  |
| ***Summary of change:*** | Specify RF requirements for band n262 |
|  |  |
| ***Consequences if not approved:*** | The band will not be specified and no operation could be done in this band. |
|  |  |
| ***Clauses affected:*** | 5.2, 5.3.5, 5.4.2.3, 5.4.3.3, 10.7.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS  |
| ***affected:*** |  | **X** |  Test specifications | TS  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | The corresponding draft CR R4-2016882 was endorsed in RAN4#97-e. |

|  |  |
| --- | --- |
| ***This CR's revision history:*** |  |

*<Start of the change>*

## 5.2 *Operating bands*

NR is designed to operate in the *operating bands* defined in table 5.2-1 and 5.2-2.

NB-IoT is designed to operate in the NR operating bands n1, n2, n3, n5, n7, n8, n12, n13, n14, n18, n20, n25, n26, n28, n41, n65, n66, n70, n71, n74, n90 which are defined in Table 5.2-1.

Table 5.2-1: NR *operating bands* in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | Uplink (UL) *operating band*BS receive / UE transmitFUL,low – FUL,high | Downlink (DL) *operating band*BS transmit / UE receiveFDL,low – FDL,high | Duplex mode |
| n1 | 1920 MHz – 1980 MHz | 2110 MHz – 2170 MHz | FDD |
| n2 | 1850 MHz – 1910 MHz | 1930 MHz – 1990 MHz | FDD |
| n3 | 1710 MHz – 1785 MHz | 1805 MHz – 1880 MHz | FDD |
| n5 | 824 MHz – 849 MHz | 869 MHz – 894 MHz | FDD |
| n7 | 2500 MHz – 2570 MHz | 2620 MHz – 2690 MHz | FDD |
| n8 | 880 MHz – 915 MHz | 925 MHz – 960 MHz | FDD |
| n12 | 699 MHz – 716 MHz | 729 MHz – 746 MHz | FDD |
| n13 | 777 MHz – 787 MHz | 746 MHz – 756 MHz | FDD |
| n14 | 788 MHz – 798 MHz | 758 MHz – 768 MHz | FDD |
| n18 | 815 MHz – 830 MHz | 860 MHz – 875 MHz | FDD |
| n20 | 832 MHz – 862 MHz | 791 MHz – 821 MHz | FDD |
| n247 | 1626.5 MHz – 1660.5 MHz | 1525 MHz – 1559 MHz | FDD |
| n25 | 1850 MHz – 1915 MHz | 1930 MHz – 1995 MHz | FDD |
| n26 | 814 MHz – 849 MHz | 859 MHz – 894 MHz | FDD |
| n28 | 703 MHz – 748 MHz | 758 MHz – 803 MHz | FDD |
| n29 | N/A | 717 MHz – 728 MHz | SDL |
| n30 | 2305 MHz – 2315 MHz | 2350 MHz – 2360 MHz | FDD |
| n34 | 2010 MHz – 2025 MHz | 2010 MHz – 2025 MHz | TDD |
| n38 | 2570 MHz – 2620 MHz | 2570 MHz – 2620 MHz | TDD |
| n39 | 1880 MHz – 1920 MHz | 1880 MHz – 1920 MHz | TDD |
| n40 | 2300 MHz – 2400 MHz | 2300 MHz – 2400 MHz | TDD |
| n41 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n46 | 5150 MHz – 5925 MHz  | 5150 MHz – 5925 MHz | TDD3 |
| n48 | 3550 MHz – 3700 MHz | 3550 MHz – 3700 MHz | TDD |
| n50 | 1432 MHz – 1517 MHz | 1432 MHz – 1517 MHz | TDD |
| n51 | 1427 MHz – 1432 MHz | 1427 MHz – 1432 MHz | TDD |
| n53 | 2483.5 MHz – 2495 MHz | 2483.5 MHz – 2495 MHz | TDD |
| n65 | 1920 MHz – 2010 MHz | 2110 MHz – 2200 MHz | FDD |
| n66 | 1710 MHz – 1780 MHz | 2110 MHz – 2200 MHz | FDD |
| n70 | 1695 MHz – 1710 MHz | 1995 MHz – 2020 MHz | FDD |
| n71 | 663 MHz – 698 MHz | 617 MHz – 652 MHz | FDD |
| n74 | 1427 MHz – 1470 MHz | 1475 MHz – 1518 MHz | FDD |
| n75 | N/A | 1432 MHz – 1517 MHz | SDL |
| n76 | N/A | 1427 MHz – 1432 MHz | SDL |
| n77 | 3300 MHz – 4200 MHz | 3300 MHz – 4200 MHz | TDD |
| n78 | 3300 MHz – 3800 MHz | 3300 MHz – 3800 MHz | TDD |
| n79 | 4400 MHz – 5000 MHz | 4400 MHz – 5000 MHz | TDD |
| n80 | 1710 MHz – 1785 MHz | N/A | SUL  |
| n81 | 880 MHz – 915 MHz | N/A | SUL  |
| n82 | 832 MHz – 862 MHz | N/A | SUL  |
| n83 | 703 MHz – 748 MHz | N/A | SUL |
| n84 | 1920 MHz – 1980 MHz | N/A | SUL |
| n86 | 1710 MHz – 1780 MHz | N/A | SUL |
| n89 | 824 MHz – 849 MHz | N/A | SUL |
| n90 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n91 | 832 MHz – 862 MHz | 1427 MHz – 1432 MHz | FDD2 |
| n92 | 832 MHz – 862 MHz | 1432 MHz – 1517 MHz | FDD2 |
| n93 | 880 MHz – 915 MHz | 1427 MHz – 1432 MHz | FDD2 |
| n94 | 880 MHz – 915 MHz | 1432 MHz – 1517 MHz | FDD2 |
| n951 | 2010 MHz – 2025 MHz | N/A | SUL  |
| n964 | 5925 MHz – 7125 MHz | 5925 MHz – 7125 MHz | TDD3 |
| n975 | 2300 MHz – 2400 MHz | N/A | SUL  |
| n985 | 1880 MHz – 1920 MHz | N/A | SUL  |
| n996 | 1626.5 MHz -1660.5 MHz | N/A | SUL |
| NOTE 1: This band is applicable in China only.NOTE 2: Variable duplex operation does not enable dynamic variable duplex configuration by the network, and is used such that DL and UL frequency ranges are supported independently in any valid frequency range for the band.NOTE 3: This band is restricted to operation with shared spectrum channel access as defined in [20].NOTE 4: This band is applicable in the USA only subject to FCC Report and Order [FCC 20-51].NOTE 5: The requirements for this band are applicable only where no other NR or E-UTRA TDD operating band(s) are used within the frequency range of this band in the same geographical area. For scenarios where other NR or E-UTRA TDD operating band(s) are used within the frequency range of this band in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. NOTE 6: UL operation is restricted to 1627.5 – 1637.5 MHz and 1646.5 – 1656.5 MHz per FCC Order DA 20-48. NOTE 7: DL operation is restricted to 1526-1536 MHz frequency range. UL operation is restricted to 1627.5 – 1637.5 MHz and 1646.5 – 1656.5 MHz per FCC Order DA 20-48. |

Table 5.2-2: NR *operating bands* in FR2

|  |  |  |
| --- | --- | --- |
| NR *operating band* | Uplink (UL) and Downlink (DL) *operating band*BS transmit/receiveUE transmit/receiveFUL,low – FUL,highFDL,low – FDL,high | Duplex mode |
| n257 | 26500 MHz – 29500 MHz | TDD |
| n258 | 24250 MHz – 27500 MHz | TDD |
| n259 | 39500 MHz – 43500 MHz | TDD |
| n260 | 37000 MHz – 40000 MHz | TDD |
| n261 | 27500 MHz – 28350 MHz | TDD |
| n262 | 47200 MHz – 48200 MHz | TDD |

*<End of the change>*

*<Start of the change>*

### 5.3.5 *BS channel bandwidth* per *operating band*

The requirements in this specification apply to the combination of *BS channel bandwidths*, SCS and *operating bands* shown in table 5.3.5-1 for FR1 and in table 5.3.5-2 for FR2. The *transmission bandwidth configuration* in table 5.3.2-1 and table 5.3.2-2 shall be supported for each of the *BS channel bandwidths* within the BS capability. The *BS channel bandwidths* are specified for both the Tx and Rx path.

Table 5.3.5-1: *BS channel bandwidths* and SCS per *operating band* in FR1

| NR band / SCS / *BS channel bandwidth* |
| --- |
| NR Band | SCSkHz | 5 MHz | 10 MHz | 15 MHz | 20 MHz | 25 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 70 MHz | 80 MHz | 90 MHz | 100 MHz |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n1 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n2 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n3 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n5 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n7 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n8 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| n12 | 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| N13 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| n14 | 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| n18 | 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n20 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n24 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
|  | 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| n25 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n26 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  | Yes | Yes |  |  |  |  |  |  |
| n28 | 30 |  | Yes | Yes | Yes |  | Yes | Yes |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| n29 | 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| n30 | 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| n34 | 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n38 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n39 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 15 | Yes4 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n40 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  | Yes |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  | Yes |
|  | 15 |  | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| n41 | 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
|  | 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
|  | 15 |  | Yes6 |  | Yes |  |  | Yes |  |  |  |  |  |  |
| n46 | 30 |  | Yes6 |  | Yes |  |  | Yes |  | Yes |  | Yes |  |  |
|  | 60 |  | Yes6 |  | Yes |  |  | Yes |  | Yes |  | Yes |  |  |
|  | 15 | Yes2 | Yes | Yes | Yes |  | Yes | Yes | Yes1 |  |  |  |  |  |
| n48 | 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes1 | Yes1 | Yes1 | Yes1 | Yes1 | Yes1 |
|  | 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes1 | Yes1 | Yes1 | Yes1 | Yes1 | Yes1 |
|  | 15 | Yes2 | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| n50 | 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes |  |  |
|  | 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes |  |  |
|  | 15 | Yes |  |  |  |  |  |  |  |  |  |  |  |  |
| n51 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| n53 | 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  | Yes |  |  |  |  |  |
| n65 | 30 |  | Yes | Yes | Yes |  |  |  | Yes |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes |  |  |  | Yes |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n66 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |
| n70 | 30 |  | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n71 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n74 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n75 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
|  | 15 | Yes |  |  |  |  |  |  |  |  |  |  |  |  |
| n76 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 |  | Yes | Yes  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n77 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
|  | 15 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n78 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
|  | 15 |  |  |  |  |  |  | Yes | Yes |  |  |  |  |  |
| n79 | 30 |  |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
|  | 60 |  |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n80 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n81 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n82 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  | Yes | Yes |  |  |  |  |  |  |
| n83 | 30 |  | Yes | Yes | Yes |  | Yes | Yes |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n84 | 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| n86 | 30 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n89 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 |  | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| n90 | 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
|  | 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
|  | 15 | Yes | Yes3 |  |  |  |  |  |  |  |  |  |  |  |
| n91 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n92 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes3 |  |  |  |  |  |  |  |  |  |  |  |
| n93 | 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n94 | 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
|  | 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| n95 | 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
|  | 60 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
|  | 15 |  |  |  | Yes |  |  | Yes |  |  |  |  |  |  |
| n96 | 30 |  |  |  | Yes |  |  | Yes |  | Yes |  | Yes |  |  |
|  | 60 |  |  |  | Yes |  |  | Yes |  | Yes |  | Yes |  |  |
| N97 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  | Yes |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  | Yes |
| N98 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n99 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an downlink SCell part of CA configuration.NOTE 2: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.NOTE 3: For this bandwidth, it only applies for UL transmission.NOTE 4: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.NOTE 5: Void.NOTE 6: This bandwidth can only be applied in certain regions where the absence of non 3GPP technologies can be guaranteed on a long term basis in this version of specification. |

Table 5.3.5-2: *BS channel bandwidths* and SCS per *operating band* in FR2

|  |
| --- |
| NR band / SCS / *BS channel bandwidth* |
| NR Band | SCSkHz | 50 MHz | 100 MHz | 200MHz | 400 MHz |
| n257 | 60 | Yes | Yes | Yes |  |
|  | 120 | Yes | Yes | Yes | Yes |
| n258 | 60 | Yes | Yes | Yes |  |
|  | 120 | Yes | Yes | Yes | Yes |
| n259 | 60 | Yes | Yes | Yes |  |
|  | 120 | Yes | Yes | Yes | Yes |
| n260 | 60 | Yes | Yes | Yes |  |
|  | 120 | Yes | Yes | Yes | Yes |
| n261 | 60 | Yes | Yes | Yes |  |
|  | 120 | Yes | Yes | Yes | Yes |
| n262 | 60 | Yes | Yes | Yes |  |
|  | 120 | Yes | Yes | Yes | Yes |

*<End of the change>*

*<Start of the change>*

#### 5.4.2.3 Channel raster entries for each *operating band*

The RF channel positions on the channel raster in each NR *operating band* are given through the applicable NR-ARFCN in table 5.4.2.3-1 for FR1 and table 5.4.2.3-2 for FR2, using the channel raster to resource element mapping in clause 5.4.2.2.

- For NR *operating bands* with 100 kHz channel raster, ΔFRaster = 20 × ΔFGlobal. In this case, every 20th NR-ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 is given as <20>.

- For NR *operating bands* with 15 kHz channel raster below 3 GHz, ΔFRaster = *I* × ΔFGlobal, where *I* ϵ {3,6}. In this case, every *Ith* NR‑ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 is given as <*I*>.

- For NR *operating bands* with 15 kHz and 60 kHz channel raster above 3 GHz, ΔFRaster = *I* ×ΔFGlobal, where *I* ϵ {1, 2}. In this case, every *Ith* NR‑ARFCN within the *operating band* are applicable for the channel raster within the *operating band* and the step size for the channel raster in table 5.4.2.3-1 and table 5.4.2.3-2 is given as <*I*>.

- For frequency bands with two ΔFRaster in FR1, the higher ΔFRaster applies to channels using only the SCS that is equal to or larger than the higher ΔFRaster and SSB SCS is equal to the higher ΔFRaster.

- For frequency bands with two ΔFRaster in FR2, the higher ΔFRaster applies to channels using only the SCS that is equal to the higher ΔFRaster and the SSB SCS that is equal to or larger than the higher ΔFRaster.

Table 5.4.2.3-1: Applicable NR-ARFCN per *operating band* in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | ΔFRaster(kHz)  | Uplinkrange of NREF(First – <Step size> – Last) | Downlinkrange of NREF(First – <Step size> – Last) |
| n1 | 100 | 384000 – <20> – 396000 | 422000 – <20> – 434000 |
| n2 | 100 | 370000 – <20> – 382000 | 386000 – <20> – 398000 |
| n3 | 100 | 342000 – <20> – 357000 | 361000 – <20> – 376000 |
| n5 | 100 | 164800 – <20> – 169800 | 173800 – <20> – 178800 |
| n7 | 100 | 500000 – <20> – 514000 | 524000 – <20> – 538000 |
| n8 | 100 | 176000 – <20> – 183000 | 185000 – <20> – 192000 |
| n12 | 100 | 139800 – <20> – 143200 | 145800 – <20> – 149200 |
| n13 | 100 | 155400 – <20> – 157400 | 149200 – <20> – 151200 |
| n14 | 100 | 157600 – <20> –159600 | 151600 – <20> – 153600 |
| n18 | 100 | 163000 – <20> – 166000 | 172000 – <20> – 175000 |
| n20 | 100 | 166400 – <20> – 172400 | 158200 – <20> – 164200 |
| n25 | 100 | 370000 – <20> – 383000 | 386000 – <20> – 399000 |
| n24 | 100 | 325300 – <20> – 332100 | 305000 – <20> – 311800 |
| n26 | 100 | 162800 – <20> – 169800 | 171800 – <20> – 178800 |
| n28 | 100 | 140600 – <20> – 149600 | 151600 – <20> – 160600 |
| n29 | 100 | N/A | 143400 – <20> – 145600 |
| n30 | 100 | 461000 – <20> – 463000 | 470000 – <20> – 472000 |
| n34 | 100 | 402000 – <20> – 405000 | 402000 – <20> – 405000 |
| n38 | 100 | 514000 – <20> – 524000 | 514000 – <20> – 524000 |
| n39 | 100 | 376000 – <20> – 384000 | 376000 – <20> – 384000 |
| n40 | 100 | 460000 – <20> – 480000 | 460000 – <20> – 480000 |
| n41 | 15 | 499200 – <3> – 537999 | 499200 – <3> – 537999 |
|  | 30 | 499200 – <6> – 537996 | 499200 – <6> – 537996 |
| n461 | 15 | 744000 – <1> – 794333 | 744000 – <1> – 794333 |
| n48 | 15 | 636667 – <1> – 646666 | 636667 – <1> – 646666 |
|  | 30 | 636668 – <2> – 646666 | 636668 – <2> – 646666 |
| n50 | 100 | 286400 – <20> – 303400 | 286400 – <20> – 303400 |
| n51 | 100 | 285400 – <20> – 286400 | 285400 – <20> – 286400 |
| n53 | 100 | 496700 – <20> – 499000 | 496700 – <20> – 499000 |
| n65 | 100 | 384000 – <20> – 402000 | 422000 – <20> – 440000 |
| n66 | 100 | 342000 – <20> – 356000 | 422000 – <20> – 440000 |
| n70 | 100 | 339000 – <20> – 342000 | 399000 – <20> – 404000 |
| n71 | 100 | 132600 – <20> – 139600 | 123400 – <20> – 130400 |
| n74 | 100 | 285400 – <20> – 294000 | 295000 – <20> – 303600 |
| n75 | 100 | N/A | 286400 – <20> – 303400 |
| n76 | 100 | N/A | 285400 – <20> – 286400 |
| n77 | 15 | 620000 – <1> – 680000 | 620000 – <1> – 680000 |
|  | 30 | 620000 – <2> – 680000 | 620000 – <2> – 680000 |
| n78 | 15 | 620000 – <1> – 653333 | 620000 – <1> – 653333 |
|  | 30 | 620000 – <2> – 653332 | 620000 – <2> – 653332 |
| n79 | 15 | 693334 – <1> – 733333 | 693334 – <1> – 733333 |
|  | 30 | 693334 – <2> – 733332 | 693334 – <2> – 733332 |
| n80 | 100 | 342000 – <20> – 357000 | N/A |
| n81 | 100 | 176000 – <20> – 183000 | N/A |
| n82 | 100 | 166400 – <20> – 172400  | N/A |
| n83 | 100 | 140600 – <20> –149600 | N/A |
| n84 | 100 | 384000 – <20> – 396000 | N/A |
| n86 | 100 | 342000 – <20> – 356000 | N/A |
| n89 | 100 | 164800 – <20> – 169800 | N/A |
|  | 15 | 499200 – <3> – 537999 | 499200 – <3> – 537999 |
| n90 | 30 | 499200 – <6> – 537996 | 499200 – <6> – 537996 |
|  | 100 | 499200 – <20> – 538000 | 499200 – <20> – 538000 |
| n91 | 100 | 166400 – <20> – 172400 | 285400 – <20> – 286400 |
| n92 | 100 | 166400 – <20> – 172400 | 286400 – <20> – 303400 |
| n93 | 100 | 176000 – <20> – 183000 | 285400 – <20> – 286400 |
| n94 | 100 | 176000 – <20> – 183000 | 286400 – <20> – 303400 |
| n95 | 100 | 402000 – <20> – 405000 | N/A |
| n962 | 15 | 795000 – <1> – 875000 | 795000 – <1> – 875000 |
| n97 | 100 | 460000 – <20> – 480000 | N/A |
| n98 | 100 | 376000 – <20> – 384000 | N/A |
| n99 | 100 | 325300 -- <20> – 332100 | N/A |
| NOTE 1: Applicable NR-ARFCN for band n46 for 10 MHz channel bandwidth, NREF = {782000, 788668} for 20 MHz channel bandwidth, NREF = {744000, 745332, 746668, 748000, 749332, 750668, 752000, 753332, 754668, 756000, 765332, 766668, 768000, 769332, 770668, 772000, 773332, 774668, 776000, 777332, 778668, 780000, 781332, 783000, 784332, 785668, 787000, 788332, 789668, 791000, 792332, 793668}; for 40 MHz channel bandwidth, NREF = {744668, 746000, 748668, 751332, 754000, 755332, 766000, 767332, 770000, 772668, 775332, 778000, 780668, 783668, 786332, 787668, 790332, 793000}; for 60 MHz channel bandwidth, NREF = {745332, 746668, 748000, 752000, 753332, 754668, 766668, 768000, 769332, 773332, 774668, 778668, 780000, 784332, 785668, 787000, 791000, 792332}; for 80 MHz channel bandwidth, NREF = {746000, 747332, 752668, 754000, 767332, 768668, 774000, 779332, 785000, 786332, 791668}NOTE 2: Applicable NR-ARFCN for band n96 for 20 MHz channel bandwidth, NREF = {797000, 798332, 799668, 801000, 802332, 803668, 805000, 806332, 807668, 809000, 810332, 811668, 813000, 814332, 815668, 817000, 818332, 819668, 821000, 822332, 823668, 825000, 826332, 827668, 829000, 830332, 831668, 833000, 834332, 835668, 837000, 838332, 839668, 841000, 842332, 843668, 845000, 846332, 847668, 849000, 850332, 851668, 853000, 854332, 855668, 857000, 858332, 859668, 861000, 862332, 863668, 865000, 866332, 867668, 869000, 870332, 871668, 873000, 874332} for 40 MHz channel bandwidth, NREF = {797668, 800332, 803000, 805668, 808332, 811000, 813668, 816332, 819000, 821668, 824332, 827000, 829668, 832332, 835000, 837668, 840332, 843000, 845668, 848332, 851000, 853668, 856332, 859000, 861668, 864332, 867000, 869668, 872332} for 60 MHz channel bandwidth, NREF = {798332, 799668, 803668, 805000, 809000, 810332, 814332, 815668, 819668, 821000, 825000, 826332, 830332, 831668, 835668, 837000, 841000, 842332, 846332, 847668, 851668, 853000, 857000, 858332, 862332, 863668, 867668, 869000, 873000} for 80 MHz channel bandwidth, NREF = {799000, 804332, 809668, 815000, 820332, 825668, 831000, 836332, 841668, 847000, 852332, 857668, 863000, 868332} |

Table 5.4.2.3-2: Applicable NR-ARFCN per *operating band* in FR2

|  |  |  |
| --- | --- | --- |
| NR *operating band* | ΔFRaster(kHz)  | Uplink and Downlinkrange of NREF(First – <Step size> – Last) |
| n257 | 60 | 2054166 – <1> – 2104165 |
|  | 120 | 2054167 – <2> – 2104165 |
| n258 | 60 | 2016667 – <1> – 2070832 |
|  | 120 | 2016667 – <2> – 2070831 |
| n259 | 60 | 2270832 – <1> – 2337499 |
|  | 120 | 2270832– <2> – 2337499 |
| n260 | 60 | 2229166 – <1> – 2279165 |
|  | 120 | 2229167 – <2> – 2279165 |
| n261 | 60 | 2070833 – <1> – 2084999 |
|  | 120 | 2070833 – <2> – 2084999 |
| n262 | 60 | 2399166 – <1> – 2415832 |
|  | 120 | 2399167 – <2> – 2415831 |

*<End of the change>*

*<Start of the change>*

#### 5.4.3.3 Synchronization raster entries for each operating band

The synchronization raster for each band is give in table 5.4.3.3-1. The distance between applicable GSCN entries is given by the <Step size> indicated in table 5.4.3.3-1 for FR1 and table 5.4.3.3-2 for FR2.

Table 5.4.3.3-1: Applicable SS raster entries per *operating band* (FR1)

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | SS Block SCS | SS Block pattern(NOTE 1) | Range of GSCN(First – <Step size> – Last) |
| n1 | 15 kHz | Case A | 5279 – <1> – 5419 |
| n2 | 15 kHz | Case A | 4829 – <1> – 4969 |
| n3 | 15 kHz | Case A | 4517 – <1> – 4693 |
| n5 | 15 kHz | Case A | 2177 – <1> – 2230 |
|  | 30 kHz | Case B | 2183 – <1> – 2224 |
| n7 | 15 kHz | Case A | 6554 – <1> – 6718 |
| n8 | 15 kHz | Case A | 2318 – <1> – 2395 |
| n12 | 15 kHz | Case A | 1828 – <1> – 1858 |
| n13 | 15 kHz | Case A | 1871 – <1> – 1885 |
| n14 | 15 kHz | Case A | 1901 – <1> – 1915 |
| n18 | 15kHz | CaseA | 2156 – <1> – 2182 |
| n20 | 15 kHz | Case A | 1982 – <1> – 2047 |
| n24 | 15 kHz | Case A | 3818 – <1> – 3892 |
| 30 kHz | Case B | 3824 – <1> – 3886 |
| n25 | 15 kHz | Case A | 4829 – <1> – 4981 |
| n26 | 15 kHz | Case A | 2153 – <1> – 2230 |
| n28 | 15 kHz | Case A | 1901 – <1> – 2002 |
| n29 | 15 kHz | Case A | 1798 – <1> – 1813 |
| n30 | 15 kHz | Case A | 5879 – <1> – 5893 |
| n34 | 15 kHz | Case A | NOTE 3 |
|  | 30 kHz | Case C | 5036 – <1> – 5050 |
| n38 | 15 kHz | Case A | NOTE 2 |
|  | 30 kHz | Case C | 6437 – <1> – 6538 |
| n39 | 15 kHz | Case A | NOTE 4 |
|  | 30 kHz | Case C | 4712 – <1> – 4789 |
| n40 | 30 kHz | Case C | 5762 – <1> – 5989 |
| n41 | 15 kHz | Case A | 6246 – <3> – 6717 |
|  | 30 kHz | Case C | 6252 – <3> – 6714 |
| n465 | 30 kHz | Case C | 8993 – <1> – 9530 |
| n48 | 30 kHz | Case C | 7884 – <1> – 7982 |
| n50 | 30 kHz | Case C | 3590 – <1> – 3781 |
| n51 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n53 | 15 kHz | Case A | 6215 – <1> – 6232 |
| n65 | 15 kHz | Case A | 5279 – <1> – 5494 |
| n66 | 15 kHz | Case A | 5279 – <1> – 5494 |
|  | 30 kHz | Case B | 5285 – <1> – 5488 |
| n70 | 15 kHz | Case A | 4993 – <1> – 5044 |
| n71 | 15 kHz | Case A | 1547 – <1> – 1624 |
| n74 | 15 kHz | Case A | 3692 – <1> – 3790 |
| n75 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n76 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n77 | 30 kHz | Case C | 7711 – <1> – 8329 |
| n78 | 30 kHz | Case C | 7711 – <1> – 8051 |
| n79 | 30 kHz | Case C | 8480 – <16> – 8880 |
| n90 | 15 kHz | Case A | 6246 – <1> – 6717 |
|  | 30 kHz | Case C | 6252 – <1> – 6714 |
| n91 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n92 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n93 | 15 kHz | Case A | 3572 – <1> – 3574 |
| n94 | 15 kHz | Case A | 3584 – <1> – 3787 |
| n96**6** | 30 kHz | Case C | 9531 – <1> – 10363 |
| NOTE 1: SS Block pattern is defined in clause 4.1 in TS 38.213 [10].NOTE 2: The applicable SS raster entries are GSCN = {6432, 6443, 6457, 6468, 6479, 6493, 6507, 6518, 6532, 6543}NOTE 3: The applicable SS raster entries are GSCN = {5032, 5043, 5054}NOTE 4: The applicable SS raster entries are GSCN = {4707, 4715, 4718, 4729, 4732, 4743, 4747, 4754, 4761, 4768, 4772, 4782, 4786, 4793}NOTE 5: The following GSCN are allowed for operation in band n46: GSCN = {8996, 9010, 9024, 9038, 9051, 9065, 9079, 9093, 9107, 9121, 9218, 9232, 9246, 9260, 9274, 9288, 9301, 9315, 9329, 9343, 9357, 9371, 9385, 9402, 9416, 9430, 9444, 9458, 9472, 9485, 9499, 9513}.NOTE 6: The following GSCN are allowed for operation in band n96: GSCN = { 9548, 9562, 9576, 9590, 9603, 9617, 9631, 9645, 9659, 9673, 9687, 9701, 9714, 9728, 9742, 9756, 9770, 9784, 9798, 9812, 9826, 9840, 9853, 9867, 9881, 9895, 9909, 9923, 9937, 9951, 9964, 9978, 9992, 10006, 10020, 10034, 10048, 10062, 10076, 10090, 10103, 10117, 10131, 10145, 10159, 10173, 10187, 10201, 10214, 10228, 10242, 10256, 10270, 10284, 10298, 10312, 10325, 10339, 10353}. |

Table 5.4.3.3-2: Applicable SS raster entries per *operating band* (FR2)

|  |  |  |  |
| --- | --- | --- | --- |
| NR *operating band* | SS Block SCS | SS Block pattern(note) | Range of GSCN(First – <Step size> – Last) |
| n257  | 120 kHz | Case D | 22388 – <1> – 22558 |
|  | 240 kHz | Case E | 22390 – <2> – 22556 |
| n258 | 120 kHz | Case D | 22257 – <1> – 22443 |
|  | 240 kHz | Case E | 22258 – <2> – 22442 |
| n259 | 120 kHz | Case D | 23140 – <1> – 23369 |
|  | 240 kHz | Case E | 23142 – <2> – 23368 |
| n260  | 120 kHz | Case D | 22995 – <1> – 23166 |
|  | 240 kHz | Case E | 22996 – <2> – 23164 |
| n261 | 120 kHz | Case D | 22446 – <1> – 22492 |
|  | 240 kHz | Case E | 22446 – <2> – 22490 |
| n262 | 120 kHz | Case D | 23586 – <1> – 23641 |
|  | 240 kHz | Case E | 23588 – <2> – 23640 |
| NOTE: SS Block pattern is defined in section 4.1 in TS 38.213 [10]. |

*<End of the change>*

*<Start of the change>*

### 10.7.3 Minimum requirement for *BS type 2-O*

The OTA RX spurious emissions requirement shall apply during the *transmitter OFF period* only.

For the *BS type 2-O*, the power of any RX spurious emission shall not exceed the limits in table 10.7.3-1.

10.7.3-1: Radiated Rx spurious emission limits for *BS type 2-O*

|  |  |  |  |
| --- | --- | --- | --- |
| Spurious frequency range (Note 4) | Limit(Note 5) | Measurement Bandwidth | Note |
| 30 MHz ↔ 1 GHz | -36 dBm | 100 kHz | Note 1 |
| 1 GHz ↔ 18 GHz | -30 dBm | 1 MHz | Note 1 |
| 18 GHz ↔ Fstep,1 | -20 dBm | 10 MHz | Note 2 |
| Fstep,1  ↔ Fstep,2 | -15 dBm | 10 MHz | Note 2 |
| Fstep,2 ↔ Fstep,3  | -10 dBm | 10 MHz | Note 2 |
| Fstep,4  ↔ Fstep,5 | -10 dBm | 10 MHz | Note 2 |
| Fstep,5  ↔ Fstep,6 | -15 dBm | 10 MHz | Note 2 |
| Fstep,6 ↔ 2nd harmonic of the upper frequency edge of the UL *operating band* | -20 dBm | 10 MHz | Note 2, Note 3 |
| NOTE 1: Bandwidth as in ITU-R SM.329 [2], s4.1.NOTE 2: Limit and bandwidth as in ERC Recommendation 74-01 [19], Annex 2.NOTE 3: Upper frequency as in ITU-R SM.329 [2], s2.5 table 1.NOTE 4: The step frequencies Fstep,X are defined in table 10.7.3-2.NOTE 5: Additional limits may apply regionally. |

Table 10.7.3-2: Step frequencies for defining the radiated Rx spurious emission limits for *BS type 2-O*

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Operating band | Fstep,1(GHz) | Fstep,2(GHz) | Fstep,3(GHz) | Fstep,4(GHz) | Fstep,5(GHz) | Fstep,6(GHz) |
| n257 | 18 | 23.5 | 25 | 31 | 32.5 | 41.5 |
| n258 | 18 | 21 | 22.75 | 29 | 30.75 | 40.5 |
| n259 | 23.5 | 35.5 | 38 | 45 | 47.5 | 59.5 |
| n260 | 25 | 34 | 35.5 | 41.5 | 43 | 52 |
| n261 | 18 | 25.5 | 26.0 | 29.85 | 30.35 | 38.35 |
| n262 | 37.2 | 45.2 | 45.7 | 49.7 | 50.2 | 58.2 |

In addition to the requirements in Table 10.7.3-1, the requirement for protection of EESS for BS operating in frequency range 24.25 - 27.5 GHz in clause 9.7.5.3.3 may be applied.

*<End of the change>*