{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Cover","Parameters","FR1 PUSCH high reliability","FR1 PUSCH low latency","FR2 PUSCH high reliability","FR2 PUSCH low latency"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"FR1 PUSCH high reliability","index":2,"n_rows":18,"n_cols":27,"rows_kept":18,"cut":false,"hidden":false,"merged":[[10,6,13,6],[10,7,13,7],[10,9,11,9],[12,9,13,9],[6,9,7,9],[8,9,9,9],[2,9,3,9],[4,9,5,9],[2,8,9,8],[2,6,5,6],[0,7,1,7],[2,7,5,7],[6,6,9,6],[6,7,9,7],[6,2,9,2],[6,3,9,3],[6,4,9,4],[6,5,9,5],[2,0,9,0],[2,1,5,1],[6,1,9,1],[2,2,5,2],[2,3,5,3],[2,5,5,5],[2,4,5,4],[0,0,1,0],[0,5,1,5],[0,2,1,2],[0,1,1,1],[0,12,1,12],[0,8,1,8],[0,9,1,9],[0,13,0,14],[0,11,1,11],[0,10,1,10],[0,3,1,3],[0,6,1,6],[0,4,1,4],[0,25,0,26],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[10,0,17,0],[14,5,17,5],[14,6,17,6],[14,7,17,7],[14,9,15,9],[16,9,17,9],[10,8,17,8],[14,1,17,1],[14,2,17,2],[14,3,17,3],[14,4,17,4],[10,2,13,2],[10,3,13,3],[10,4,13,4],[10,5,13,5],[10,1,13,1]]}
[" Test","Duplex mode","Aggregation factor "," waveform","MCS level","Tx/Rx","Propagation condition","DMRS","SCS","BW","PUSCH mapping type","38.104 req","38.141 req","Samsung",null,"Intel",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Test 1.1","FDD","n2","CP-OFDM","Table 3, MCS5","1T2R","TDLB100-400","DMRS 1+1","15kHz","5MHz","type A",{"$f":"DerivingPerfReq(N3:W3)","v":-8.4},{"$f":"IF(L3>-100,L3+0.6,L3)","v":-7.8000000000000007},-11.3,-9.3000000000000007,-12.1,-10.6,-10,-7.5,-10.3,-8.3000000000000007,-13.7,-11.7,{"$f":"MAX(N3,P3,R3,T3,V3)-MIN(N3,P3,R3,T3,V3)","v":3.6999999999999993},{"$f":"MAX(O3,Q3,S3,U3,W3)-MIN(O3,Q3,S3,U3,W3)","v":4.1999999999999993},{"$f":"AVERAGE(N3,P3,R3,T3,V3)","v":-11.48},{"$f":"AVERAGE(O3,Q3,S3,U3,W3)","v":-9.48}]
[null,null,null,null,null,null,null,null,null,null,"type B",-8.1999999999999993,-7.6,-11,-9,-12.1,-10.6,-9.8000000000000007,-7.3,-10.3,-8.3000000000000007,-13.6,-11.6,{"$f":"MAX(N4,P4,R4,T4,V4)-MIN(N4,P4,R4,T4,V4)","v":3.7999999999999989},{"$f":"MAX(O4,Q4,S4,U4,W4)-MIN(O4,Q4,S4,U4,W4)","v":4.3},{"$f":"AVERAGE(N4,P4,R4,T4,V4)","v":-11.360000000000001},{"$f":"AVERAGE(O4,Q4,S4,U4,W4)","v":-9.3600000000000012}]
[null,null,null,null,null,null,null,null,null,"10MHz","type A",-10.199999999999999,-9.6,-11.9,-9.9,-12.7,-11.2,-10.199999999999999,-7.7,-11.5,-9.5,-14.4,-12.4,4.2000000000000011,4.7,-12.139999999999999,-10.139999999999999]
[null,null,null,null,null,null,null,null,null,null,"type B",-10.1,-9.5,-11.8,-9.8000000000000007,-12.6,-11.1,-9.9,-7.4,-11.5,-9.5,-14.1,-12.1,4.1999999999999993,4.6999999999999993,-11.98,-9.98]
[null,"TDD","n8","CP-OFDM","Table 3, MCS5","1T2R","TDLB100-400","DMRS 1+1",null,"5MHz","type A",-11,-10.4,-11.2,-9.1999999999999993,-12.3,-10.8,-12.9,-10.4,-10.199999999999999,-8.4,-13.9,-11.9,3.7000000000000011,3.5,-12.099999999999998,-10.139999999999999]
[null,null,null,null,null,null,null,null,null,null,"type B",-10,-9.4,-10.9,-8.9,-12.3,-10.8,-12.7,-10.199999999999999,-10.199999999999999,-8.4,-13.9,-11.9,3.7000000000000011,3.5,-12.000000000000002,-10.040000000000001]
[null,null,null,null,null,null,null,null,null,"10MHz","type A",-10.7,-10.1,-11.8,-9.8000000000000007,-13,-11.5,-13.4,-10.9,-11.2,-9.1999999999999993,-14.4,-12.4,3.2000000000000011,3.2000000000000011,-12.760000000000002,-10.760000000000002]
[null,null,null,null,null,null,null,null,null,null,"type B",-10.3,-9.7000000000000011,-11.7,-9.6999999999999993,-13,-11.5,-13.2,-10.7,-11.2,-9.1999999999999993,-14.4,-12.4,3.2000000000000011,3.2000000000000011,-12.7,-10.7]
["Test 1.2","FDD","n2","CP-OFDM","Table 3, MCS5","1T2R","TDLB100-400","DMRS 1+1","30kHz","10MHz","type A",-10.8,{"$f":"IF(L11>-100,L11+0.6,L11)","v":-10.200000000000001},-12.2,-10.199999999999999,-12.9,-11.4,-12.9,-10.4,-10.7,-8.6999999999999993,-13.4,-11.4,2.7000000000000011,2.7000000000000011,-12.42,-10.42]
[null,null,null,null,null,null,null,null,null,null,"type B",-10.8,-10.200000000000001,-12.1,-10.1,-12.8,-11.3,-12.9,-10.4,-10.7,-8.6999999999999993,-13.4,-11.4,2.7000000000000011,2.7000000000000011,-12.379999999999999,-10.379999999999999]
[null,null,null,null,null,null,null,null,null,"40MHz","type A",-11.5,-10.9,-13,-11,-13.6,-12.1,-13,-10.5,-11.5,-9.5,-14.3,-12.3,2.8000000000000007,2.8000000000000007,-13.080000000000002,-11.080000000000002]
[null,null,null,null,null,null,null,null,null,null,"type B",-11.4,-10.8,-12.9,-10.9,-13.6,-12.1,-12.8,-10.3,-11.5,-9.5,-14.3,-12.3,2.8000000000000007,2.8000000000000007,-13.02,-11.02]
[null,"TDD","n2","CP-OFDM","Table 3, MCS5","1T2R","TDLB100-400","DMRS 1+1",null,"10MHz","type A",-10.8,-10.200000000000001,-12.1,-10.1,-13.1,-11.6,-12.8,-10.3,-10.9,-8.9,-13.4,-11.4,2.5,2.6999999999999993,-12.459999999999999,-10.459999999999999]
[null,null,null,null,null,null,null,null,null,null,"type B",-10.9,-10.3,-12,-10,-13.1,-11.6,-13,-10.5,-10.7,-8.6999999999999993,-13.4,-11.4,2.7000000000000011,2.9000000000000004,-12.44,-10.44]
[null,null,null,null,null,null,null,null,null,"40MHz","type A",-11.5,{"$f":"IF(L17>-100,L17+0.6,L17)","v":-10.9},-12.9,-10.9,-13.8,-12.3,-12.9,-10.4,-11.9,-9.9,-14.3,-12.3,2.4000000000000004,2.4000000000000004,-13.16,-11.16]
[null,null,null,null,null,null,null,null,null,null,"type B",-11.4,-10.8,-12.8,-10.8,-13.8,-12.3,-12.9,-10.4,-11.8,-9.8000000000000007,-14.3,-12.3,2.5,2.5,-13.12,-11.12]

{"sheet":"FR1 PUSCH low latency","index":3,"n_rows":6,"n_cols":26,"rows_kept":6,"cut":false,"hidden":false,"merged":[[4,3,5,3],[4,2,5,2],[4,1,5,1],[4,0,5,0],[4,8,5,8],[4,7,5,7],[4,6,5,6],[4,5,5,5],[4,4,5,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[0,8,1,8],[2,8,3,8],[2,1,3,1],[2,0,3,0],[2,2,3,2],[2,3,3,3],[2,4,3,4],[0,24,0,25],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,12,0,13],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,9,1,9],[0,10,1,10],[0,11,1,11],[0,5,1,5],[0,6,1,6],[0,7,1,7]]}
[" Test","Symbol length"," waveform","Tx/Rx","PUSCH mapping type","MCS level","Propagation condition","DMRS","SCS","BW","38.104 req","38.141 req","Samsung",null,"Intel",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Test 2.1","2os","CP-OFDM","1T2R","type B","Table 3, MCS10","TDLC300-100","DMRS 1+0","15kHz","5MHz",{"$f":"DerivingPerfReq(M3:V3)","v":0.5},{"$f":"IF(K3>-100,K3+0.6,K3)","v":1.1000000000000001},-1.26,0.74,-1.5,0,-1.7,0.8,-1.5,0.5,-1.6,0.4,{"$f":"MAX(M3,O3,Q3,S3,U3)-MIN(M3,O3,Q3,S3,U3)","v":0.43999999999999995},{"$f":"MAX(N3,P3,R3,T3,V3)-MIN(N3,P3,R3,T3,V3)","v":0.8},{"$f":"AVERAGE(M3,O3,Q3,S3,U3)","v":-1.512},{"$f":"AVERAGE(N3,P3,R3,T3,V3)","v":0.48799999999999999}]
[null,null,null,null,null,null,null,null,null,"10MHz",{"$f":"DerivingPerfReq(M4:V4)","v":0.3},{"$f":"IF(K4>-100,K4+0.6,K4)","v":0.89999999999999991},-1.71,0.28999999999999998,-2,0.5,-2.2999999999999998,0.2,-1.9,0.1,-1.7,0.3,{"$f":"MAX(M4,O4,Q4,S4,U4)-MIN(M4,O4,Q4,S4,U4)","v":0.59999999999999987},{"$f":"MAX(N4,P4,R4,T4,V4)-MIN(N4,P4,R4,T4,V4)","v":0.4},{"$f":"AVERAGE(M4,O4,Q4,S4,U4)","v":-1.9219999999999999},{"$f":"AVERAGE(N4,P4,R4,T4,V4)","v":0.27800000000000002}]
["Test 2.2","2os","CP-OFDM","1T2R"," type B","Table 3, MCS10","TDLC300-100","DMRS 1+0","30kHz","10MHz",{"$f":"DerivingPerfReq(M5:V5)","v":0.3},{"$f":"IF(K5>-100,K5+0.6,K5)","v":0.89999999999999991},-1.27,0.73,-1.7,0.2,-1.8,0.7,-2,0,-1.9,0.1,0.73,0.73,-1.734,0.34599999999999997]
[null,null,null,null,null,null,null,null,null,"40MHz",{"$f":"DerivingPerfReq(M6:V6)","v":0},{"$f":"IF(K6>-100,K6+0.6,K6)","v":0.6},-1.68,0.32,-2,0.5,-2.5,0,-2.8,-0.8,-2,0,1.1199999999999999,1.3,-2.1960000000000002,4.0000000000000036E-3]

{"sheet":"FR2 PUSCH high reliability","index":4,"n_rows":6,"n_cols":27,"rows_kept":6,"cut":false,"hidden":false,"merged":[[2,7,3,7],[4,7,5,7],[0,10,1,10],[0,11,1,11],[0,12,1,12],[0,13,0,14],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,25,0,26],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24]]}
[" Test","Duplex mode","Aggregation factor "," waveform","MCS level","Tx/Rx","PUSCH mapping type","SCS","BW","DMRS","Propagation condition","38.104 req","38.141 req","Samsung",null,"Intel",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Test 3.1","TDD","n8","CP-OFDM","Table 3,MCS5","1T2R","Type B","60 kHz","50 MHz","DMRS 1+1","TDLA30-300",{"$f":"DerivingPerfReq(N3:W3)","v":-11.9},{"$f":"IF(L3>-100,L3+0.6,L3)","v":-11.3},-13.3,-11.3,-13.4,-11.9,-11.6,-9.1,-14.1,-12.1,-14.3,-12.3,{"$f":"MAX(N3,P3,R3,T3,V3)-MIN(N3,P3,R3,T3,V3)","v":2.7000000000000011},{"$f":"MAX(O3,Q3,S3,U3,W3)-MIN(O3,Q3,S3,U3,W3)","v":3.2000000000000011},{"$f":"AVERAGE(N3,P3,R3,T3,V3)","v":-13.34},{"$f":"AVERAGE(O3,Q3,S3,U3,W3)","v":-11.34}]
["Test 3.2","TDD","n8","CP-OFDM","Table 3,MCS5","1T2R","Type B",null,"100 MHz","DMRS 1+1","TDLA30-300",{"$f":"DerivingPerfReq(N4:W4)","v":-12.2},-11.6,-14.2,-12.2,-13.9,-12.4,-12.9,-10.4,-14.2,-13.3,-14.9,-12.9,{"$f":"MAX(N4,P4,R4,T4,V4)-MIN(N4,P4,R4,T4,V4)","v":2},{"$f":"MAX(O4,Q4,S4,U4,W4)-MIN(O4,Q4,S4,U4,W4)","v":2.9000000000000004},{"$f":"AVERAGE(N4,P4,R4,T4,V4)","v":-14.020000000000001},{"$f":"AVERAGE(O4,Q4,S4,U4,W4)","v":-12.239999999999998}]
["Test 3.3","TDD","n8","CP-OFDM","Table 3,MCS5","1T2R","Type B","120 kHz","50 MHz","DMRS 1+1","TDLA30-300",{"$f":"DerivingPerfReq(N5:W5)","v":-11.2},-10.6,-12.4,-10.4,-12.8,-11.3,-10.199999999999999,-7.7,-13.8,-11.8,-13.1,-11.1,3.6000000000000014,4.1000000000000005,-12.46,-10.46]
["Test 3.4","TDD","n8","CP-OFDM","Table 3,MCS5","1T2R","Type B",null,"100 MHz","DMRS 1+1","TDLA30-300",{"$f":"DerivingPerfReq(N6:W6)","v":-11.7},-11.1,-13.3,-11.3,-13.4,-11.9,-11.9,-9.4,-13.6,-11.6,-14,-12,2.0999999999999996,2.5999999999999996,-13.24,-11.24]

{"sheet":"FR2 PUSCH low latency","index":5,"n_rows":6,"n_cols":26,"rows_kept":6,"cut":false,"hidden":false,"merged":[[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[2,1,5,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,9,1,9],[0,10,1,10],[0,11,1,11],[0,12,0,13],[2,6,5,6],[2,7,5,7],[0,24,0,25],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23]]}
[" Test"," waveform","Tx/Rx","PUSCH mapping type","MCS level","Propagation condition","Symbol length","DMRS","SCS","BW","38.104 req","38.141 req","Samsung",null,"Intel",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Test 4.1","CP-OFDM","1T2R","Type B","Table 3, MCS5","TDLA30-300","4os","DMRS 1+0","60 kHz","50 MHz",{"$f":"DerivingPerfReq(M3:V3)","v":-4.4000000000000004},{"$f":"IF(K3>-100,K3+0.6,K3)","v":-3.8000000000000003},-6.4,-4.4000000000000004,-6.5,-5,-6.6,-4.0999999999999996,-5.9,-3.9,-6.6,-4.5999999999999996,{"$f":"MAX(M3,O3,Q3,S3,U3)-MIN(M3,O3,Q3,S3,U3)","v":0.69999999999999929},{"$f":"MAX(N3,P3,R3,T3,V3)-MIN(N3,P3,R3,T3,V3)","v":1.1000000000000001},{"$f":"AVERAGE(M3,O3,Q3,S3,U3)","v":-6.4},{"$f":"AVERAGE(N3,P3,R3,T3,V3)","v":-4.4000000000000004}]
["Test 4.2",null,null,null,null,null,null,null,null,"100 MHz",{"$f":"DerivingPerfReq(M4:V4)","v":-5},{"$f":"IF(K4>-100,K4+0.6,K4)","v":-4.4000000000000004},-6.7,-4.7,-6.9,-5.4,-7,-4.5,-7.6,-5.6,-6.8,-4.8,{"$f":"MAX(M4,O4,Q4,S4,U4)-MIN(M4,O4,Q4,S4,U4)","v":0.89999999999999947},{"$f":"MAX(N4,P4,R4,T4,V4)-MIN(N4,P4,R4,T4,V4)","v":1.0999999999999996},{"$f":"AVERAGE(M4,O4,Q4,S4,U4)","v":-7},{"$f":"AVERAGE(N4,P4,R4,T4,V4)","v":-5.0000000000000009}]
["Test 4.3",null,null,null,null,null,null,null,"120 kHz","50 MHz",{"$f":"DerivingPerfReq(M5:V5)","v":-4.0999999999999996},-3.4999999999999996,-6,-4,-6.2,-4.7,-6.3,-3.8,-6.8,-4.8,-5.4,-3.4,1.3999999999999995,1.4,-6.1400000000000006,-4.1399999999999997]
["Test 4.4",null,null,null,null,null,null,null,null,"100 MHz",{"$f":"DerivingPerfReq(M6:V6)","v":-5.0999999999999996},-4.5,-6.8,-4.8,-7,-5.5,-7.1,-4.5999999999999996,-7.6,-5.6,-6.9,-4.9000000000000004,0.79999999999999982,1,-7.08,-5.08]