|  |  |  |
| --- | --- | --- |
| PR | Company name | Justification for change/comments |
| 7.0-1 | Futurewei | Rewording to use service requirement style.  |
| 7.0-2 | Futurewei | This not only related to authorization, but also how one PIN element can comnicati with other PIN elements in different PINs. ( maybe fore release 18, only for single PIN case).  |
| 7.0-3 | Futurewei | if this multicast, suggest change to “ transmit with same content ” to avoid confusion, also rephase to “ 5g system shall ….” |
| 7.0-4 | Futurewei | This requirement is too general, nothing new. may be better to use KPI requirement. |
| 7.0-5 | Futurewei | not clear what faults need to be considered. need to rephase to specific the fault issue, is management faults? or connection fault? Or implementation fault management. 3GPP system already have many mechanisms for different fault handling, so maybe it can be considered this already covered. Maybe packet error rate KPI? |
| 7.1-1 | Futurewei | Rewording to use service requirement style. |
| 7.1-2 | Futurewei  | is this general for all 5G connectivity? Is this already be covered? Also, how to define loss of connectivity? E.g.no data during certain period time?Suggest considered this has already been covered.  |
| 7.1-3 | Futurewei  | Is this the same about optimization of discovery to avoid congestion, can be merged. Also, current wording restricts to certain service discovery solution, such as using service discovery message. Suggest to make the requirement more general. |
| 7.2-1 | Futurewei  | Rewording to use service requirement style.Add 5.11.6-2 which is covered by this.  |
| 7.4-1 | Futurewei | Merge 5.11.6-4, which allow different secure communication within a PIN.  |
| 7.4-2 | Futurewei | Rewording to use service requirement style. |
| 7.4-4 | Futurewei | Rewording to use service requirement style. |
| 7.5-2 | Futurewei  | Rewording to use service requirement style. |
| 7.5-4 | Futurewei  | Rewording to use service requirement style. |
| 7.6-1 | Futurewei  | It’s default that there is QoS management association with the 3GPP link? This seems already be covered. |
| 7.7-1 | Futurewei | Rewording to use service requirement style. |
| 7.7-2 | Futurewei | Merge 5.11.6-1 into this.  |
| 7.7-4 | Convida Wireless | Added CPR 7.7-4; it was previously commented that this was mobility or load sharing and covered by existing reqt. Clarify that this is not mobility or load sharing and the PR tries to capture a PEMC assisting a PE with re-establishing 5G connectivity after the PE has discovered it has lost connectivity; the PEMC in this case is not a UE |
| Futurewei  | Rewording to use service requirement style. |
| 7.7-5 | Futurewei  | This is from PR-5.11.6-5, and it is different than 5.1.5-1 and not be covered. prefer to be alone.  |