**3GPP TSG-SA3 Meeting #101e *S3-203103***

**e-meeting, 9 – 20 November 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **33.501** | **CR** | **1006** | **rev** | **-** | **Current version:** | **16.4.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Authorization between NFs and SCP | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | S3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_eSBA | | | | |  | ***Date:*** | | | 2020-11-20 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In TS33.501 in clause 13.3.6 there is a Ed Note stating authorization between NFs and SCP is ffs | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Addition of authorization mechanism between NFs and SCP | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | There will be no authorization mechanism defined between NFs and SCP and Ed Note will be unresolved. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 13.3.6, 13.4.1.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Start of Change 1 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### 

### 13.3.6 Authentication and authorization between SCP and network functions

The SCP and network functions shall use one of the following methods described in clause 13.1 to mutually authenticate each other before service layer messages can be exchanged on that interface:

- If the PLMN uses protection at the transport layer, authentication provided by the transport layer protection solution shall be used for mutual authentication of the SCP and the network functions.

- If the PLMN does not use protection at the transport layer, mutual authentication of the SCP and network functions may be implicit by NDS/IP or physical security.

Authentication between the SCP and the Network Function may be implicit by co-location.

In the present document, authorization between the SCP and the NFs is based on static authorization as described in clause 13.3.0. No dynamic mechanism for establishing authorization between the SCP and NFs is defined.

NFc

SCP

NRF

1. Service Request (optionally includes enhanced CCA')

\* CCA' additionally includes Authorized SCP ID

2. Nnrf\_AccessToken\_Get\_Request (includes CCA' and CCA,

CCA contains the SCP Instance ID in the subject parameter)

3. NRF analyzes the request, and authorizes the SCP

4. Nnrf\_AccessToken\_Get Response

(access token)

##### 13.4.1.3.2 Authorization for indirect communication with delegated discovery procedure

This clause covers the scenario where the NF Service Consumer use the SCP to discover and select the NF Service Producer instance that can process the service request.



Figure 13.4.1.3.2-1: Authorization and service invocation procedure, for indirect communication with delegated discovery

1. The NF Service Consumer sends a service request to the SCP. The service request may include the NF Service Consumer CCA as defined in clause 13.3.8.

2. The SCP may perform a service discovery with the NRF.

3. The SCP sends an access token request (Nnrf\_AccessToken\_Get Request) to the NRF. The access token request includes parameters as defined in clause 13.4.1.1. The access token request may include the NF Service Consumer CCA if received in Step 1.

4. The NRF authenticates the NF Service Consumer using one of the methods described in clause 13.3.1.2. If cNF authentication is successful and the NF Service Consumer is authorized based on the NRF policy, the NRF issues an access token as described in clause 13.4.1.1. The NRF uses the NF Service Consumer instance ID as the subject of the access token.

5. The NRF sends the access token to the SCP in an access token response (Nnrf\_AccessToken\_Get Response).

6. The SCP sends the service request to the NF Service Producer. The service request includes the access token received in Step 5, and may include the NF Service Consumer CCA if received in Step 1.

7. The NF Service Producer authenticates the NF Service Consumer by one of the methods described in clause 13.3.2.2 and if successful, it validates the access token as described in clause 13.4.1.1.

8. If the validation of the access token is successful, the NF Service Producer sends the service response to the SCP.

9. The SCP forwards the service response to the NF Service Consumer.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Change 1 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*