**3GPP TSG-SA WG3 Meeting #102e *S3-210052***

**e-Meeting, 18-29 January 2021** *revision of S3-21wxyz*

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **33.180** | **CR** | **0154** | **Rev** | **-** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | [33.180] R17 Group regroup and user regroup security | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Motorola Solutions, Ericsson, FirstNet, NIST, UK Home Office, NCSC, AT&T, Airbus | | | | | | | | | |
| ***Source to TSG:*** | S3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | MCXSec2 | | | | |  | ***Date:*** | | | 18-Jan-2021 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Key management for group regroup with preconfigured group and user regroup with preconfigured group is needed. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add new clauses for group regroup with preconfigured group security and user regroup with preconfigured group security. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Group regroup with preconfigured group and user regroup with preconfigured group cannot be secured. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.2, X (new), X.1 (new), X.2 (new), F.1.Y (new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* START of change 1 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

CMS Configuration Management Server

CS Crypto Session

CSB-ID Crypto Session Bundle Identifier

CSC Common Services Core

CSK Client-Server Key

CSK-ID Client-Server Key Identifier

DPCK MCData Payload Cipher Key

DPPK MCData Payload Protection Key

DPPK-ID MCData Payload Protection Key Identifier

GBA Generic Bootstrapping Architecture

GMK Group Master Key

GMK-ID Group Master Key Identifier

GMS Group Management Server

GUK-ID Group User Key Identifier

IdM Identity Management

IdMS Identity Management Server

InK Integrity Key

InK-ID Integrity Key Identifier

InterKMRec Interworking Key Management Record

InterKMRec-ID Interworking Key Management Record Identifier

InterSD Interworking Security Data

IWF InterWorking Function

JSON JavaScript Object Notation

JWS JSON Web Signature

JWT JSON Web Token

KDF Key Derivation Function

KFC Key for Floor Control

KFC-ID Key for Floor Control Identifier

KMS Key Management Server

MBCP Media Burst Control Protocol

MCData Mission Critical Data

MCPTT Mission Critical Push to Talk

MCVideo Mission Critical Video

MCX Mission Critical Services

MKFC Multicast Key for Floor Control

MSCCK MBMS subchannel control key

MSRP Message Session Relay Protocol

MuSiK Multicast Signalling Key

MKI Master Key Identifier

NGMI Next Generation Mobile Intelligence

NTP Network Time Protocol

NTP-UTC Network Time Protocol – Coordinated Universal Time

OIDC OpenID Connect

PCK Private Call Key

PCK-ID Private Call Key Identifier

PKCE Proof Key for Code Exchange

PSK Pre-Shared Key

RGK Regroup Key

RGK-SEED Regroup Key Seed

SEG Security Gateway

SeGy Security Gateway

SPK Signalling Protection Key

SRTCP Secure Real-Time Transport Control Protocol

SRTP Secure Real-Time Transport Protocol

SSRC Synchronization Source

TBCP Talk Burst Control Protocol

TGK Traffic Generating Key

TrK KMS Transport Key

TrK-ID KMS Transport Key Identifier

UID User Identifier for MIKEY-SAKKE (referred to as the 'Identifier' in RFC 6509 [11])

XPK XML Protection Key

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* END of change 1 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* START of change 2 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## X Group regroup and user regroup securityX.1 Group regroup with preconfigured group

Group regroup with preconfigured group is defined in TS 23.379 [2] and TS 23.280 [36]. The following applies to MCPTT, MCVideo and MCData.

The basis of this feature is to allow an authorized MC user to dynamically create a temporary group consisting of a set of predefined groups (i.e. all the members of the predefined groups become members of this new regroup group).

Security for group regroup with predefined group is based on a GMK obtained through a predefined group configuration. The group configuration to be used (i.e. the GMK) is identified in the initial preconfigured regroup request message. All users that participate in a secure group regroup call must have the predefined group configuration and GMK.

While some users may not be invited into the group regroup call, they may still have access to the group configuration containing the GMK and therefore key diversity for the group regroup is imperative. In order to create key diversity, a randomly generated 128-bit Regroup Key Seed (RGK-SEED) shall be included in the preconfigured regroup request message. The combination of the preconfigured GMK and RGK-SEED shall create the Regroup Key (RGK) for the group regroup session as defined in F.1.Y.

The RGK-SEED is distributed by the MC service server to those users invited to the regroup group call using unicast on the downlink. To protect the RGK-SEED during transit, the preconfigured regroup request message from the initiating MC client to the MC service server carries the RGK-SEED encrypted on the initiating client’s CSK. The MC service server decrypts the RGK-SEED from the initiating client’s CSK and in turn, delivers the preconfigured regroup request message to each participating MC client. For unicast downlink, the MC service server protects the RGK-SEED with each target client’s individual CSK.

The MC service server shall store the RGK-SEED for the duration of the group regrouping so that late-entry of users to the group regroup may receive the seed. The MC service server shall securely manage the RGK-SEED as described in clause 5.11.1.

Figure X.1-1 provides an example distribution of the RGK-SEED for a preconfigured group regroup call.



Figure X.1-1: Key establishment for group regroup with preconfigured group

1. The authorized user of MC client 1 initiates the group regroup procedure, inviting MC client 2, MC client 3, and MC client 4.

2. MC client 1 sends the preconfigured regroup request message to the MC service server. The preconfigured regroup request message contains the set of group regroup information listed in TS 23.379 [2] together with a randomly generated RGK-SEED protected on the initiating client’s CSK.

3. The MC service server performs the group regroup validation steps described in TS 23.379 [2]. In addition, the MC service server decrypts the RGK-SEED from the initiating client’s CSK and securely stores it.

4a. The MC service server sends a unicast preconfigured regroup request message to MC client 2. The preconfigured regroup request message includes the RGK-SEED encrypted on MC client 2’s CSK.

4b. The MC service server sends a unicast preconfigured regroup request message to MC client 3. The preconfigured regroup request message includes the RGK-SEED encrypted on MC client 3’s CSK.

4c. The MC service server sends a unicast preconfigured regroup request message to MC client 4. The preconfigured regroup request message includes the RGK-SEED encrypted on MC client 4’s CSK.

5. MC client 2, MC client 3, and MC client 4 notify their users of the regrouping

.

6a. MC client 2 may optionally send a preconfigured regroup response to the MC service server to acknowledge the regrouping action.

6b. MC client 3 may optionally send a preconfigured regroup response to the MC service server to acknowledge the regrouping action.

6c. MC client 4 may optionally send a preconfigured regroup response to the MC service server to acknowledge the regrouping action.

7. The MC service server affiliates the regrouped MC clients to the regroup group.

8. The MC service server sends a preconfigured regroup response to MC client 1.

9a. MC client 1 calculates the RGK to be used for the regroup group session. This step may happen any time after step 1.

9b. MC client 2 calculates the RGK to be used for the regroup group session. This step may happen any time after step 5.

9c. MC clients 3 and 4 calculate the RGK to be used for the regroup group session. This step may happen any time after step 5.

## X.2 User regroup with preconfigured group

User regroup with preconfigured group is defined in TS 23.379 [2] and TS 23.280 [36]. The following applies to MCPTT, MCVideo and MCData.

The basis of this feature is to allow the MC operator to dynamically create a temporary group consisting of a specified set of users (i.e. all the users identified in the user regroup become members of this new temporary group).

Security for user regroup with predefined group is based on a GMK obtained through a predefined group configuration. The group configuration to be used (i.e. the GMK) is identified in the initial preconfigured regroup request message. All users that participate in a secure user regroup call must have the predefined group configuration and GMK.

While some users may not be invited into the user regroup call, they still may have access to the group configuration containing the GMK and therefore key diversity for the user regroup is imperative. In order to create key diversity, a randomly generated 128-bit Regroup Key Seed (RGK-SEED) shall be included in the preconfigured regroup request message. The combination of the preconfigured GMK and RGK-SEED shall create the Regroup Key (RGK) for the user regroup session as described in F.1.Y.

The RGK-SEED is provided to those users invited to the user regroup call using unicast on the downlink. Multicast is not used on the downlink for user regroup. To protect the RGK-SEED during transit, the preconfigured regroup request message from the initiating MC client to the MC service server carries the RGK-SEED encrypted on the initiating client’s CSK. The MC service server decrypts the RGK-SEED from the initiating client’s CSK and in turn, delivers the preconfigured regroup request message unicast to each participating MC client with the RGK-SEED encrypted on each target client’s individual CSK.

The MC service server temporarily stores the RGK-SEED for the duration of the user regrouping so that late-entry users may receive the seed. The MC service server shall securely manage the RGK-SEED as described in clause 5.11.1.

Figure X.2-1 provides an example showing the distribution of the RGK-SEED for a preconfigured user regroup call.



Figure X.2-1: Key establishment for user regroup with preconfigured group

1. The authorized user of MC client 1 initiates the user regroup procedure.

2. MC client 1 sends the preconfigured regroup request message to the MC service server. The preconfigured regroup request message contains the set of user regroup information listed in TS 23.379 [2] together with a randomly generated RGK-SEED protected on the initiating client’s CSK.

3. The MC service server performs the validation steps described in TS 23.379 [2]. In addition, the MC service server decrypts the RGK-SEED from the initiating client’s CSK and securely stores it.

4a. The MC service server sends a unicast preconfigured regroup request message to MC client 2. The preconfigured regroup request message includes the RGK-SEED encrypted on client 2’s CSK.

4b. The MC service server sends a unicast preconfigured regroup request message to MC client 3. The preconfigured regroup request message includes the RGK-SEED encrypted on client 3’s CSK.

5a. MC client 2 notifies the user of the regrouping.

5b. MC client 3 notifies the user of the regrouping.

6a. MC client 2 may send a preconfigured regroup response to the MC service server to acknowledge the regrouping action.

6b. MC client 3 may send a preconfigured regroup response to the MC service server to acknowledge the regrouping action.

7. The MC service server affiliates the regrouped MC clients to the user regroup group.

8. The MC service server sends a preconfigured regroup response to MC client 1.

9a. MC client 1 calculates the RGK to be used for the user regroup session. This step may happen any time after step 1.

9b. MC client 2 calculates the RGK to be used for the user regroup session. This step may happen any time after step 5a.

9c. MC client 3 calculates the RGK to be used for the user regroup session. This step may happen any time after step 5b.\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* END of change 2 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* START of change 3 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### F.1.Y Calculation of regroup key (RGK) for preconfigured groups

To generate the regroup key (RGK) for preconfigured groups defined in clause X, the following parameters shall be used to form the input S to the KDF specified in annex B of 3GPP TS 33.220 [27]:

- FC = 0x54, (for preconfigured group regroup or preconfigured user regroup media confidentiality),

- P0 = GMK,

- L0 = length of P0, expressed in number of bytes (e.g. 0x00 0x17),

- P1 = RGK-SEED,

- L1 = length of P1, expressed in number of bytes (e.g. 0x00 0x17),

- P2 = GMK-ID,

- L2 = length of P2, expressed in number of bytes (e.g. 0x00 0x17),

- P3 = MC Group ID,

- L3 = length of P3, expressed in number of bytes (e.g. 0x00 0x17),

The GMK (P0) shall be the GMK associated with the preconfigured group, the RGK-SEED (P1) shall be the distributed regroup key seed (as defined in clause X), the GMK-ID (P2) shall be the GMK-ID of the GMK associated with the preconfigured group, and the MC Group ID (P3) shall be the MCPTT group ID of the regroup group provided in the preconfigured regroup request message. The GMK, RGK-SEED, GMK-ID and MC Group ID shall follow the encodings specified in annex B of 3GPP TS 33.220 [17].

The 128 least significant bits of the 256 bits of the KDF output shall be used as the RGK.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* END of change 3 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*