**3GPP TSG-SA3 Meeting #104-e *S3-21xxxx***

e-meeting, 16 - 27 August 2021

**Title: LS on full registration request message to be rerouted via RAN**

**Response to:**

**Release: Rel-17**

**Work Item: FS\_AMFREAL\_SEC**

**Source: SA3**

**To: SA2, RAN3, CT1**

**Cc:**

**Contact person: Juan Deng**

**dengjuan5@huawei.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:**

# 1 Overall description

In step 7(B), clause 4.2.2.2.3 of TS 23.502, it is specified that

*“The Reroute NAS message includes the information about the target AMF, and the full Registration Request message. If the initial AMF has obtained the information as described at step 4b, that information is included. The (R)AN sends the Initial UE message to the target AMF (step 7b) indicating reroute due to slicing including the information from step 4b that the NSSF provided.”*

It is not clear what is a full Registration Request (RR) message. Also the term “Initial UE message”, different from the term “full Registration Request message”, rises different understanding in SA3.

1 that is sent from the (R)AN to the target AMF the same as

Q2 to SA2: Is the full Registration Request message the entire REGISTRATION REQUEST message that contains both clear text IEs and non-clear text IEs, as defined in clause 4.4.6. in TS 24.501?

# 2 Actions

**To SA2**

**ACTION:**

SA2 is kindly requested to clarify the above questions.

RAN3 is kindly requested to align with SA2 terminology regarding the registration request message to be rerouted via RAN to avoid confusion.

# 3 Dates of next TSG SA WG 3 meetings

SA3#105-e 8 - 12 November 2021 Electronic meeting

SA3#106 7-11 February TBD