**3GPP TSG-SA3 Meeting #106-e S3-220089-r1**

**e-meeting, 14 – 25 February 2022** Revision of S3-21XXXX

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **33.535** | **CR** | 117 | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Clarification on the NF consumer in 6.6.1 |
|  |  |
| ***Source to WG:*** | ZTE |
| ***Source to TSG:*** | S3 |
|  |  |
| ***Work item code:*** | AKMA |  | ***Date:*** | 2022-02-06 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Some clarification on NF consumers which can initiate this AKMA context removal procedure is needed. The NF consumer should know whether to trigger this procedure, some example is added. |
|  |  |
| ***Summary of change:*** | This CR proposes to add some clarification on NF consumer. |
|  |  |
| ***Consequences if not approved:*** | May cause some misunderstanding. |
|  |  |
| ***Clauses affected:*** | 6.6.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Start changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### 6.6.1 General

This procedure is used to remove the AKMA context in the AAnF. NF consumers (e.g. O&M system, UDM) may initiate this procedure due to local policy.



Figure 6.6.1-1: AAnF AKMA context removal procedure

1. NF initiates an AAnF AKMA context removal procedure to delete the AKMA context in AAnF.

2. NF discovers the AAnF of the UE, as specified in clause 6.7 and sends a Naanf\_AKMA\_Context\_Remove request to AAnF to remove AKMA context for the UE.

3. AAnF shall delete AKMA Context (e.g. SUPI, A-KID and KAKMA) from its local database.

4. AAnF sends a Naanf\_AKMA\_Context\_Remove response to NF.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*