**3GPP TSG-SA3 Meeting #110Ad-Hoc-e *S3-231892r1***

**Electronic meeting, Online, 17 - 21 April 2023**

**Source:**  **Huawei, HiSilicon**

**Title:** **conclusions to KI#3**

**Document for: Approval**

**Agenda Item: 5.12**

# 1 Decision/action requested

***It is proposed to approve the change described in this document.***

# 2 References

[1]

# 3 Rationale

This contribution proposes conclusions to KI#2.

# 4 Detailed proposal

pCR

\*\*\* BEGINNING OF CHANGES \*\*\*

## 6.2 Conclusions to Key Issue #3

For protection of the NSAC procedure in a multiple NSACF scenario, normative work is recommended based on the following principle:

* When performing the NSAC procedure in a multiple NSACF scenario, the primary NSACF needs to validate the number of UEs and the number of PDU sessions for an S-NSSAI received from a local NSACF~~, based on information stored in UDM.~~

 \*\*\* END OF CHANGES \*\*\*