**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The LI solution for EPC in TS 33.107 and TS 33.108 does not provide any way to handle EPS/5GS interworking scenarios. |
|  |  |
| ***Summary of change:*** | This CR updates TS 33.128 clauses on LI at the MME and aligns the messages with the equivalent messages in 5GS. The current version of TS 33.128 has two options for LI at the MME. This CR provides a third option that will provide LI in the case of EPS/5GS interworking. |
|  |  |
| ***Consequences if not approved:*** | LI in EPS/5GS interworking cases will not be possible. |
|  |  |
| ***Clauses affected:*** | 2, 6.3.1, 6.3.2.2, 6.3.2.3, Annex A |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 33.128 17.0.0 CR 0165, TS 33.127 17.0.0 CR 0123  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | TS 33.128 17.0.0 CR 0165 contains additional ASN.1 referenced by this CR. TS 33.127 17.0.0 CR 0123 contains the stage 2 for this CR. |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* Start of First Change \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System".

[3] 3GPP TS 33.126: "Lawful Interception Requirements".

[4] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[5] 3GPP TS 33.127: "Lawful Interception (LI) Architecture and Functions".

[6] ETSI TS 103 120: " Lawful Interception (LI); Interface for warrant information".

[7] ETSI TS 103 221-1: "Lawful Interception (LI); Internal Network Interfaces; Part 1: X1".

[8] ETSI TS 103 221-2: "Lawful Interception (LI); Internal Network Interfaces; Part 2: X2/X3".

 [9] ETSI TS 102 232-1: "Lawful Interception (LI); Handover Interface and Service-Specific Details (SSD) for IP delivery; Part 1: Handover specification for IP delivery".

[10] ETSI TS 102 232-7: "Lawful Interception (LI); Handover Interface and Service-Specific Details (SSD) for IP delivery; Part 7: Service-specific details for Mobile Services".

[11] 3GPP TS 33.501: "Security Architecture and Procedures for the 5G System".

[12] 3GPP TS 33.108: "3G security; Handover interface for Lawful Interception (LI)".

[13] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS)".

[14] 3GPP TS 24.007: "Mobile radio interface signalling layer 3; General Aspects".

[15] 3GPP TS 29.244: "Interface between the Control Plane and the User Plane nodes".

[16] 3GPP TS 29.502: "5G System; Session Management Services; Stage 3".

[17] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[18] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)".

[19] 3GPP TS 23.003: "Numbering, addressing and identification ".

[20] OMA-TS-MLP-V3\_5-20181211-C: "Open Mobile Alliance; Mobile Location Protocol, Candidate Version 3.5", <https://www.openmobilealliance.org/release/MLS/V1_4-20181211-C/OMA-TS-MLP-V3_5-20181211-C.pdf>.

[21] 3GPP TS 29.540: "5G System; SMS Services; Stage 3".

[22] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[23] 3GPP TS 38.413: "NG Application Protocol (NGAP)".

[24] 3GPP TS 29.572: "Location Management Services; Stage 3".

[25] 3GPP TS 29.503: "5G System; Unified Data Management Services".

[26] IETF RFC 815: "IP datagram reassembly algorithms".

[27] IETF RFC 2460: "Internet Protocol, Version 6 (IPv6) Specification".

[28] IETF RFC 793: "Transmission Control Protocol".

[29] IETF RFC 768: "User Datagram Protocol".

[30] IETF RFC 4340: "Datagram Congestion Control Protocol (DCCP)".

[31] IETF RFC 4960: "Stream Control Transmission Protocol".

[32] IANA (www.iana.org): Assigned Internet Protocol Numbers, "Protocol Numbers".

[33] IETF RFC 6437: "IPv6 Flow Label Specification".

[34] IETF RFC 791: "Internet Protocol".

[35] Open Geospatial Consortium OGC 05-010: "URNs of definitions in ogc namespace".

[36] 3GPP TS 33.107: "3G security; Lawful interception architecture and functions".

[37] 3GPP TS 37.340: "Evolved Universal Radio Access (E-UTRA) and NR-Multi-connectivity; Stage 2".

[38] 3GPP TS 36.413: "S1 Application Protocol (S1AP)".

[39] OMA-TS-MMS\_ENC-V1\_3-20110913-A: "Multimedia Messaging Service Encapsulation Protocol".

[40] 3GPP TS 23.140: "Multimedia Messaging Protocol. Functional Description. Stage 2".

[41] 3GPP TS 38.415: "NG-RAN; PDU Session User Plane Protocol".

[42] 3GPP TS 23.273: "5G System (5GS) Location Services (LCS); Stage 2".

[43] IETF RFC 4566: "SDP: Session Description Protocol".

[44] 3GPP TS 24.193: "Stage 3: Access Traffic Steering, Switching and Splitting (ATSSS)".

[45] 3GPP TS 29.509: "5G System; Authentication Server Services; Stage 3".

[46] 3GPP TS 24.011: "Point-to-Point (PP) Short Message Service (SMS) support on mobile radio interface".

[47] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[48] 3GPP TS 29.504: "5G System; Unified Data Repository Services; Stage 3".

[49] 3GPP TS 29.505: "5G System; Usage of the Unified Data Repository services for Subscription Data; Stage 3".

[Re1] 3GPP TS 23.401 "General Packet Radio Service (GPRS) enhancements for Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access".

[Re2] 3GPP TS 24.301 "Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS), Stage 3".

[Re3] 3GPP TS 23.271 "Functional stage 2 description of Location Services (LCS)".

[Re4] 3GPP TS 36.413 "S1 Application Protocol (S1AP)".

[Re5] 3GPP TS 29.172 "Evolved Packet Core (EPC) LCS Protocol (ELP) between the Gateway Mobile Location Centre (GMLC) and the Mobile Management Entity (MME); SLg interface".

[Re6] 3GPP TS 29.171 "LCS Application Protocol (LCS-AP) between the Mobile Management Entity (MME) and Evolved Serving Mobile Location Centre (E-SMLC); SLs interface".

\*\*\* Start of Change 2 of 4 \*\*\*

### 6.3.1 General

The present document allows three options for EPC LI stage 3 interfaces for 4G / LTE:

- Option A: Use LI\_X1, LI\_X2 and LI\_X3 interfaces specified below in in clause 6.3.2 and 6.3.3.

- Option B: Use LI\_X1, LI\_X2 and LI\_X3 interfaces as specified in clause 6.3.2 and 6.3.3.

- Option C: Use TS 33.107 [36] clause 12 natively as defined in that document.

For implementations that include EPS/5GS interworking, option A shall be used.

In all cases, the present document specifies the stage 3 for the LI\_HI1, LI\_HI2 and LI\_HI3 interfaces.

\*\*\* Start of Change 3 of 4 \*\*\*

#### 6.3.2.2 Generation of xIRI over LI\_X2

6.3.2.2.1 GeneralIf the MME receives one or more cell IDs in an S1 message (as specified in TS 36.413 [38]), the POI associated with the MME shall report all of them.

The IRI-POI in the MME shall only generate xIRI containing the MMEIdentifierAssociation record in the following scenarios;

- IdentifierAssociation: MMEIdentifierAssociation and Tracking Area/EPS Location Update (see TS 33.107 [36] clause 12.2.1.2) records shall be generated. No other record types shall be generated for that target.

- All: All AMF record types shall be generated.

When Option A specified in clause 6.3.1 is used:

- The IRI-POI present in the MME shall send the xIRIs over LI\_X2 for each of the events listed in TS 33.127 [5] clause 6.3.2.3, the details of which are described in the following sub-clauses.

- In addition to the xIRI events listed in TS 33.127 [5] clause 6.3.2.3, the MME shall support xIRI generation in case of SMS over NAS as specified in clause 18.2.4 of TS 33.107 [36]. For records related to SMS over NAS in EPS:

- The IRI-POI present in the MME shall set the payload format to EpsHI2Operations.EpsIRIContent (value 14), see clause 5.3 and ETSI TS 103 221-2 [8] clause 5.4. The payload field shall contain an EpsHI2Operations.EpsIRIContent structure encoded according to TS 33.108 [12] clauses 10.5, 15.2 and B.9.

- As the LIID may be not available at the MME but is mandatory in EpsHI2Operations.EpsIRIContent according to Annex B.9 of TS 33.108 [12], its value in the lawfulInterceptionIdentifier field of the encoded PDU shall be set to the fixed string "LIIDNotPresent".

When Option B specified in clause 6.3.1 is used:

- The IRI-POI present in the MME shall send the xIRIs over LI\_X2 for each of the events listed in TS 33.107 [36] clause 12.2.1.1, the details of which are specified in clause 12.2.3 of the same TS, and in case of SMS over NAS as specified in clause 18.2.4 of TS 33.107 [36].- For all records except MMEIdentifierAssociation (see clause 6.3.2.2.2), the IRI-POI present in the MME shall set the payload format to EpsHI2Operations.EpsIRIContent (value 14), see clause 5.3 and ETSI TS 103 221-2 [8] clause 5.4. The payload field shall contain an EpsHI2Operations.EpsIRIContent structure encoded according to TS 33.108 [12] clauses 10.5, 15.2 and B.9.

- As the LIID may be not available at the MME but is mandatory in EpsHI2Operations.EpsIRIContent according to Annex B.9 of TS 33.108 [12], its value in the lawfulInterceptionIdentifier field of the encoded PDU shall be set to the fixed string "LIIDNotPresent".

- In addition to the xIRI events listed in TS 33.107 [36], the MME shall support xIRI containing the MMEIdentiferAssociation record in clause 6.3.2.2.2.

##### 6.3.2.2.2 MME identifier association

The IRI-POI present in the MME shall generate an xIRI containing an MMEIdentifierAssociation record when the IRI-POI present in the MME detects a new identifier association for a UE matching one of the target identifiers provided via LI\_X1. Generation of this record is subject to this record type being enabled for a specific target (see clause 6.3.2.2.1).

Table 6.3.2-1: Payload for MMEIdentifierAssociation record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| iMSI | IMSI associated with the procedure. (see NOTE 1). | M |
| iMEI | IMEI used in the procedure, if available (see NOTE 1). | C |
| mSISDN | MSISDN used in the procedure, if available (see NOTE 1). | C |
| gUTI | LTE GUTI used in the procedure. | M |
| location | Location information available when identifier association occurs.Encoded as a *userLocation* parameter (*location>locationInfo> userLocation*) and, when Dual Connectivity is activated, as an *additionalCellIDs* parameter (*location>locationInfo>additionalCellIDs*), see Annex A. | M |
| tAIList | List of tracking areas associated with the registration area within which the UE is current registered. (See NOTE 2). | C |
| NOTE 1: IMSI shall always be provided, in addition to the warrant target identifier if different to IMSI. Other identifiers shall be provided if available.NOTE 2: List shall be included each time there is a change to the registration area. |

When transmitting the xIRI, the IRI-POI present in the MME shall set the payload format to 2, and provide the payload as a BER-encoded TS33128Payloads.XIRIPayloads structure.

##### 6.3.2.2.C1 Attach

The IRI-POI in the MME shall generate an xIRI containing an MMEAttach record when the IRI-POI present in the MME detects that a UE matching one of the target identifiers provided via LI\_X1 has successfully attached to EPS. Accordingly, the IRI-POI in the MME generates the xIRI when the following event is detected:

- MME sends an S1: ATTACH ACCEPT message to the target UE and the UE EPS Mobility Management (EMM) state within the MME is changed to EMM-REGISTERED.

Table 6.3.2-Ta1: Payload for MMEAttach record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| attachType | Specifies the type of EPS Attach, see TS 24.301 [Re2] clause 9.9.3.11. This is derived from the information received from the UE in the Attach Request message. | M |
| attachResult | Specifies the result of the attach procedure, see TS 24.301 [Re2] clause 9.9.3.10. | M |
| iMSI | IMSI associated with the registration. | M |
| iMEI | IMEI associated with the registration, if available. | C |
| mSISDN | mSISDN associated with the registration, if available. | C |
| gUTI | GUTI provided as outcome of initial attach or used in other cases, see TS 24.301 [Re2] clause 5.5.1.2.4. | M |
| location | Location information determined by the network during the registration, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*) and, when Dual Connectivity is activated, as an *additionalCellIDs* parameter (*location>locationInfo>additionalCellIDs*), see Annex A. | C |
| ePSTAIList | List of tracking areas associated with the registration area within which the UE is currently registered, see TS 24.301 [Re2], clause 9.9.3.33. (see NOTE) | C |
| sMSServiceStatus | Indicates the availability of SMS Services. Shall be provided if present in the ATTACH ACCEPT. | C |
| oldGUTI | Old GUTI used in the registration, if available. | C |
| eMM5GRegStatus | UE Status, if provided in the REGISTRATION REQUEST message, see TS 24.501 [13] clause 9.11.3.56. | C |
| NOTE: List shall be included each time there is a change to the registration area. |

##### 6.3.2.2.C2 Detach

The IRI-POI in the MME shall generate an xIRI containing an MMEDetach record when the IRI-POI present in the MME detects that a UE matching one of the target identifiers provided via LI\_X1 has deregistered from the EPS. Accordingly, the IRI-POI in the MME generates the xIRI when any of the following events is detected:

- For network initiated de-registration, when the MME receives the S1: DETACH ACCEPT message from the target UE, when the MME receives an S3: DETACH NOTIFICATION about the target UE from the SGSN or when implicit deregistration timer expires; and in all cases the UE EMM state within the MME is changed to EMM-DEREGISTERED.

- For UE initiated de-registration, when the MME sends the S1: DETACH ACCEPT message to the target UE or when the MME receives the S1: DETACH REQUEST message from the target UE with deregistration type value of “switch off”; and in both cases the UE EMM state within the MME is changed to EMM-DEREGISTERED.

Table 6.3.2-Ta2: Payload for MMEDetach record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| deregistrationDirection | Indicates whether the deregistration was initiated by the network or by the UE. | M |
| detachType | Indicates the type of detach as determined by the direction of the detach request and the value of the DetachType information element, see Table 6.3.2-Ta3. | M |
| iMSI | IMSI associated with the detach. | M |
| iMEI | IMEI associated with the detach, if available. | C |
| mSISDN | mSISDN associated with the detach, if available. | C |
| gUTI | GUTI associated with the detach, if available. | C |
| cause | Indicates the EMM cause value for network-initiated detach, see TS 24.301 [Re2], clause 9.9.3.9. | C |
| location | Location information determined by the network during the deregistration, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| switchOffIndicator | If Bit 4 of the Detach type information element sent in the Detach Request is set to 0, this parameter shall be set to “normalDetach”. If Bit 4 of the Detach type information element sent in the Detach Request is set to 1, this parameter shall be set to “switchOff”. See TS 24.301 [Re2], clause 9.9.3.7. This parameter is conditional only for backwards compatibility. | C |

Table 6.3.2-Ta3: detachType values

|  |  |  |
| --- | --- | --- |
| Type of detach value | Direction | detachType value |
| 001 | UE🡪network | ePSDetach |
| 010 | UE🡪network | iMSIDetach |
| 011 | UE🡪network | combinedEPSIMSIDetach |
| 110 | UE🡪network | reserved |
| 111 | UE🡪network | reserved |
| Any Other | UE🡪network | combinedEPSIMSIDetach |
| 001 | network🡪UE | reAttachRequired |
| 010 | network🡪UE | reAttachNotRequired |
| 011 | network🡪UE | iMSIDetach |
| 110 | network🡪UE | reserved |
| 111 | network🡪UE | reserved |
| Any Other | network🡪UE | reAttachNotRequired |

The IRI-POI in the MME shall populate the ePSDetachType field with the values listed in table 6.3.2-Ta3 based on the Detach Type sent in the Detach Request message (see TS 24.301 [Re2] clause 9.9.3.7) and the direction of the Detach Request associated to the event that triggered the generation of the xIRI.

If the Detach Request message associated to the event that triggered the generation of the xIRI has the EMM Cause field populated, the IRI-POI in the MME shall set the value of the cause field of the MMEDetach record to the integer value of the EMM Cause, see TS 24.301 [Re2], clause 9.9.3.9.

##### 6.3.2.2.C3 Tracking Area/EPS Location update

When the reporting of location information is authorised, the IRI-POI in the MME shall generate an xIRI containing an MMELocationUpdate record each time the IRI-POI present in an MME detects that the target’s UE location is updated due to target’s UE mobility or as a part of an MME service procedure. The generation of such separate xIRI is not required if the updated UE location information is obtained as a part of a procedure producing some other xIRIs (e.g. mobility registration). In that case the location information is included into the respective xIRI.

The UE mobility events resulting in generation of an MMELocationUpdate xIRI include the *S1 Path Switch Request* (*intra E-UTRAN handover* *X2 based handover* procedure described in 3GPP TS 23.401 [Re1], clause 5.5.1.1) and the *S1 Handover Notify* (*Intra E-UTRAN S1 based handover* procedure described in 3GPP TS 23.401 [Re1], clause 5.5.1.2).

The MMELocationUpdate xIRI is also generated when the MME receives an E-UTRAN S1AP *ERAB Modification Indication* message as a result of Dual Connectivity activation/release for the target's UE, as described in 3GPP TS 37.340 [37], clause 10.

Based on regulatory requirements and operator policy, the location information obtained by the MME from E-UTRAN or the LCS in the course of some service operations may result in the generation of the MMELocationUpdate xIRI record. Additionally, the IRI-POI in the MME shall capture the location information in the scenarios described in TS 23.271 [Re3], clause 4.4.2. Also, in the case of Mobile Originated LCS service invoked by the target, the location information may be derived from the Location Service Response sent to the UE via the MME (see TS 23.271 [Re3], clause 9.2.6).

Optionally, based on regulatory and operator policy, other MME messages that do not generate separate xIRI but carry location information such as emergency services or LCS may trigger the generation of an MMELocationUpdate xIRI record.

Table 6.3.2-Ta4: Payload for MMELocationUpdate record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| iMSI | iMSI associated with the location update. | M |
| iMEI | iMEI associated with the location update, if available. | C |
| mSISDN | mSISDN associated with the location update, if available as part of the subscription profile. | C |
| gUTI | GUTI assigned during the location update, if available, see TS 24.301 [Re1]. | C |
| location | Updated location information determined by the network. Depending on the service or message type from which the location information is extracted, it may be encoded in several forms (Annex A). | M |
| oldGUTI | GUTI used to initiate the location update, if available, see TS 24.301 [Re1]. | C |
| sMSServiceStatus | Indicates the availability of SMS Services. Shall be provided if present in the TRACKING AREA UPDATE ACCEPT. |  |

##### 6.3.2.2.C4 Start of interception with EPS attached UE

The IRI-POI in the MME shall generate an xIRI containing an MMEStartOfInterceptionWithEPSAttachedUE record when the IRI-POI present in the MME detects that interception is activated on a UE that has already attached to the EPS. A UE is considered already attached to the EPS when the EMM state for for that UE is EMM-REGISTERED. Therefore, the IRI-POI present in the MME shall generate the xIRI MMEStartOfInterceptionWithEPSAttachedUE record when it detects that a new interception for a UE is activated (i.e. provisioned by the LIPF) and the EPS mobility management state within the MME for that UE is EMM-REGISTERED.

Table 6.3.2-Ta5: Payload for MMEStartOfInterceptionWithEPSAttachedUE record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| attachType | Specifies the type of EPS Attach, see TS 24.301 [Re2] clause 9.9.3.11. This is derived from the information received from the UE in the Attach Request message. | M |
| attachResult | Specifies the result of the attach procedure, see TS 24.301 [Re2] clause 9.9.3.10. | M |
| iMSI | IMSI associated with the registration. | M |
| iMEI | IMEI associated with the registration, if available. | C |
| mSISDN | mSISDN associated with the registration, if available. | C |
| gUTI | GUTI provided as outcome of initial attach or used in other cases, see TS 24.301 [Re2] clause 5.5.1.2.4. | M |
| location | Location information determined by the network during the registration, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*) and, when Dual Connectivity is activated, as an *additionalCellIDs* parameter (*location>locationInfo>additionalCellIDs*), see Annex A. | C |
| timeOfRegistration | Time at which the last registration occurred, if available. This is the time stamp when the ATTACH ACCEPT message is sent to the UE or (when applicable) when the ATTACH COMPLETE is received from the UE.Shall be given qualified with time zone information (i.e. as UTC or offset from UTC, not as local time). | C |
| ePSTAIList | List of tracking areas associated with the registration area within which the UE is currently registered, see TS 24.301 [Re2], clause 9.9.3.33. (see NOTE) | C |
| sMSServiceStatus | Indicates the availability of SMS Services. Shall be provided if present in the ATTACH ACCEPT. | C |
| oldGUTI | Old GUTI used in the registration, if available. | C |
| eMM5GRegStatus | UE Status, if provided in the REGISTRATION REQUEST message, see TS 24.501 [13] clause 9.11.3.56. | C |
| NOTE: List shall be included each time there is a change to the registration area. |

##### The IRI-POI present in the MME generating an xIRI containing an MMEStartOfInterceptionWithEPSAttachedUE record shall set the Payload Direction field in the PDU header to *not applicable* (see ETSI TS 103 221-2 [8] clause 5.2.6).6.3.2.2.C5 MME unsuccessful procedure

The IRI-POI in the MME shall generate an xIRI containing an MMEUnsuccessfulProcedure record when the IRI-POI present in the MME detects an unsuccessful procedure for a UE matching one of the target identifiers provided via LI\_X1.

Accordingly, the IRI-POI in the MME generates the xIRI when any of the following events is detected:

- MME sends a reject to any EMM request message to the target UE and the UE EPS Mobility Management (EMM) within the MME is changed to EMM-DEREGISTERED.

- MME aborts a registration procedure before the UE EPS Mobility Management (EMM) state within the MME is changed to EMM-REGISTERED.

- MME sends a reject to any ESM request message to the target UE.

Unsuccessful attach attempts shall be reported only if the target UE has been successfully authenticated.

Table 6.3.2-Ta6: Payload for MMEUnsuccessfulProcedure record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| failedprocedureType | Specifies the procedure which failed at the MME. | M |
| failureCause | Provides the value of the ESM or EMM cause, see TS 24.301 [Re2], clauses 9.9.3.9 and 9.9.4.4. | M |
| iMSI | IMSI associated with the procedure, if available (see NOTE). | C |
| iMEI | IMEI associated with the procedure, if available. | C |
| mSISDN | mSISDN associated with the procedure, if available. | C |
| gUTI | GUTI provided used in the procedure, if available. | C |
| location | Location information determined by the network during the procedure, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| NOTE: At least one identity shall be provided, the others shall be provided if available. |

#### 6.3.2.3 Generation of IRI over LI\_HI2

When Option A or Option B specified in clause 6.3.1 are used and an xIRI is received over LI\_X2 from the IRI-POI in the MME, the MDF2 shall generate the corresponding IRI message and deliver it over LI\_HI2 without undue delay. The IRI message shall contain a copy of the relevant record received in the xIRI over LI\_X2.

When Option C specified in clause 6.3.1 is used and an The MDF2 shall generate IRI messages based on the proprietary information received from the MME and provide it over LI\_HI2 without undue delay.

The IRI record may be enriched with any additional information available at the MDF (e.g. additional location information).

When Option A specified in clause 6.3.1 is used, LI\_HI2 shall be realised as described in clause 6.3.2.3.C1a.

When Option B or Option C specified in clause 6.3.1 used, LI\_HI2 shall be realised as described in clause 6.3.2.3.C1b.

When Option C specified in clause 6.3.1 is used, LI\_HI2 shall be realised as described in clause 6.3.2.3.C1c.

##### 6.3.2.3.C1a Option A

The IRI message the MDF2 generates shall contain a copy of the relevant record received in the xIRI over LI\_X2 and provide it over LI\_HI2 without undue delay.

The timestamp field of the psHeader structure shall be set to the time at which the MME event was observed (i.e. the timestamp field of the X2 PDU).

Table 6.3.2-Ta7 shows the IRI type (see ETSI TS 102 232-1 [9] clause 5.2.10) to be used for each IRI message.

Table 6.3.2-Ta7: IRI type for IRI messages

|  |  |
| --- | --- |
| IRI message | IRI type |
| MMEAttach | REPORT |
| MMEDetach | REPORT |
| MMELocationUpdate | REPORT |
| MMEStartOfInterceptionWithEPSAttachedUE | REPORT |
| MMEUnsuccessfulProcedure | REPORT |
| MMEIdentifierAssociation | REPORT |

These IRI messages shall omit the CIN (see ETSI TS 102 232-1 [9] clause 5.2.4).

The threeGPP33128DefinedIRI field in ETSI TS 102 232-7 [10] clause 15 shall be populated with the BER-encoded IRIPayload.

When an additional warrant is activated on a target UE and the LIPF uses the same XID for the additional warrant, the MDF2 shall be able to generate and deliver the IRI message containing the MMEStartOfInterceptionWithEPSAttachedUE record to the LEMF associated with the additional warrant without receiving a corresponding xIRI. The payload of the MMEStartOfInterceptionWithEPSAttachedUE record is specified in table 6.3.2-Ta5.

For records related to SMS over NAS in EPS, the process detailed in clause 6.3.2.3.C1b shall be used.

##### 6.3.2.3.C1b Option B and Option C

For all messages except MMEIdentifierAssociation, the IRI messages shall include an IRI payload encoded according to Annex B.9 of TS 33.108 [12].

The MDF2 shall encode the correct value of LIID in the IRI message, replacing the value "LIIDNotPresent" given in the xIRI (see clause 6.3.2.2).

For MMEIdentifierAssociation messages, the IRI message shall be encoded as an IRIEvent structure according to Annex B, and used to populate the threeGPP33128DefinedIRI field in ETSI TS 102 232-7 [10] clause 15.

##### 6.3.2.3.C1c Option C

For all messages except MMEIdentifierAssociation, the IRI messages shall include an IRI payload encoded according to Annex B.9 of TS 33.108 [12].

The MDF2 shall encode the correct value of LIID in the IRI message, replacing the value "LIIDNotPresent" given in the xIRI (see clause 6.3.2.2).

For MMEIdentifierAssociation messages, the IRI message shall be encoded as an IRIEvent structure according to Annex B, and used to populate the threeGPP33128DefinedIRI field in ETSI TS 102 232-7 [10] clause 15.

\*\*\* Start of Change 4 of 4 \*\*\*

Annex A (normative):
Structure of both the Internal and External Interfaces

TS33128Payloads

{itu-t(0) identified-organization(4) etsi(0) securityDomain(2) lawfulIntercept(2) threeGPP(4) ts33128(19) r17(17) version0(0)}

DEFINITIONS IMPLICIT TAGS EXTENSIBILITY IMPLIED ::=

BEGIN

-- =============

-- Relative OIDs

-- =============

tS33128PayloadsOID RELATIVE-OID ::= {threeGPP(4) ts33128(19) r17(17) version0(0)}

xIRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xIRI(1)}

xCCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xCC(2)}

iRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID iRI(3)}

cCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID cC(4)}

lINotificationPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID lINotification(5)}

-- ===============

-- X2 xIRI payload

-- ===============

XIRIPayload ::= SEQUENCE

{

 xIRIPayloadOID [1] RELATIVE-OID,

 event [2] XIRIEvent

}

XIRIEvent ::= CHOICE

{

 -- Access and mobility related events, see clause 6.2.2

 registration [1] AMFRegistration,

 deregistration [2] AMFDeregistration,

 locationUpdate [3] AMFLocationUpdate,

 startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

 unsuccessfulAMProcedure [5] AMFUnsuccessfulProcedure,

 -- PDU session-related events, see clause 6.2.3

 pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

 pDUSessionModification [7] SMFPDUSessionModification,

 pDUSessionRelease [8] SMFPDUSessionRelease,

 startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

 unsuccessfulSMProcedure [10] SMFUnsuccessfulProcedure,

 -- Subscriber-management related events, see clause 7.2.2

 servingSystemMessage [11] UDMServingSystemMessage,

 -- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

 sMSMessage [12] SMSMessage,

 -- LALS-related events, see clause 7.3.3

 lALSReport [13] LALSReport,

 -- PDHR/PDSR-related events, see clause 6.2.3.4.1

 pDHeaderReport [14] PDHeaderReport,

 pDSummaryReport [15] PDSummaryReport,

 -- tag 16 is reserved because there is no equivalent mDFCellSiteReport in XIRIEvent

 -- MMS-related events, see clause 7.4.2

 mMSSend [17] MMSSend,

 mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

 mMSNotification [19] MMSNotification,

 mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

 mMSNotificationResponse [21] MMSNotificationResponse,

 mMSRetrieval [22] MMSRetrieval,

 mMSDeliveryAck [23] MMSDeliveryAck,

 mMSForward [24] MMSForward,

 mMSDeleteFromRelay [25] MMSDeleteFromRelay,

 mMSDeliveryReport [26] MMSDeliveryReport,

 mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

 mMSReadReport [28] MMSReadReport,

 mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

 mMSCancel [30] MMSCancel,

 mMSMBoxStore [31] MMSMBoxStore,

 mMSMBoxUpload [32] MMSMBoxUpload,

 mMSMBoxDelete [33] MMSMBoxDelete,

 mMSMBoxViewRequest [34] MMSMBoxViewRequest,

 mMSMBoxViewResponse [35] MMSMBoxViewResponse,

 -- PTC-related events, see clause 7.5.2

 pTCRegistration [36] PTCRegistration,

 pTCSessionInitiation [37] PTCSessionInitiation,

 pTCSessionAbandon [38] PTCSessionAbandon,

 pTCSessionStart [39] PTCSessionStart,

 pTCSessionEnd [40] PTCSessionEnd,

 pTCStartOfInterception [41] PTCStartOfInterception,

 pTCPreEstablishedSession [42] PTCPreEstablishedSession,

 pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

 pTCPartyJoin [44] PTCPartyJoin,

 pTCPartyDrop [45] PTCPartyDrop,

 pTCPartyHold [46] PTCPartyHold,

 pTCMediaModification [47] PTCMediaModification,

 pTCGroupAdvertisement [48] PTCGroupAdvertisement,

 pTCFloorControl [49] PTCFloorControl,

 pTCTargetPresence [50] PTCTargetPresence,

 pTCParticipantPresence [51] PTCParticipantPresence,

 pTCListManagement [52] PTCListManagement,

 pTCAccessPolicy [53] PTCAccessPolicy,

 -- More Subscriber-management related events, see clause 7.2.2

 subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

 cancelLocationMessage [55] UDMCancelLocationMessage,

 -- SMS-related events continued from choice 12

 sMSReport [56] SMSReport,

 -- MA PDU session-related events, see clause 6.2.3.2.7

 sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

 sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

 sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

 startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

 unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

 -- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

 aMFIdentifierAssocation [62] AMFIdentifierAssocation,

 mMEIdentifierAssocation [63] MMEIdentifierAssocation,

 -- PDU to MA PDU session-related events, see clause 6.2.3.2.8

sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

 --EPS Events, see clause 6.3

 --MME Events, see clause 6.3.2.2

 mMEAttach [2531] MMEAttach,

 mMEDetach [2532] MMEDetach,

 mMELocationUpdate [2533] MMELocationUpdate,

 mMEStartOfInterceptionWithEPSAttachedUE [2534] MMEStartOfInterceptionWithEPSAttachedUE,

 mMEUnsuccessfulProcedure [2535] MMEUnsuccessfulProcedure

}

-- ==============

-- X3 xCC payload

-- ==============

-- No additional xCC payload definitions required in the present document.

-- ===============

-- HI2 IRI payload

-- ===============

IRIPayload ::= SEQUENCE

{

 iRIPayloadOID [1] RELATIVE-OID,

 event [2] IRIEvent,

 targetIdentifiers [3] SEQUENCE OF IRITargetIdentifier OPTIONAL

}

IRIEvent ::= CHOICE

{

 -- Registration-related events, see clause 6.2.2

 registration [1] AMFRegistration,

 deregistration [2] AMFDeregistration,

 locationUpdate [3] AMFLocationUpdate,

 startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

 unsuccessfulRegistrationProcedure [5] AMFUnsuccessfulProcedure,

 -- PDU session-related events, see clause 6.2.3

 pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

 pDUSessionModification [7] SMFPDUSessionModification,

 pDUSessionRelease [8] SMFPDUSessionRelease,

 startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

 unsuccessfulSessionProcedure [10] SMFUnsuccessfulProcedure,

 -- Subscriber-management related events, see clause 7.2.2

 servingSystemMessage [11] UDMServingSystemMessage,

 -- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

 sMSMessage [12] SMSMessage,

 -- LALS-related events, see clause 7.3.3

 lALSReport [13] LALSReport,

 -- PDHR/PDSR-related events, see clause 6.2.3.4.1

 pDHeaderReport [14] PDHeaderReport,

 pDSummaryReport [15] PDSummaryReport,

 -- MDF-related events, see clause 7.3.4

 mDFCellSiteReport [16] MDFCellSiteReport,

 -- MMS-related events, see clause 7.4.2

 mMSSend [17] MMSSend,

 mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

 mMSNotification [19] MMSNotification,

 mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

 mMSNotificationResponse [21] MMSNotificationResponse,

 mMSRetrieval [22] MMSRetrieval,

 mMSDeliveryAck [23] MMSDeliveryAck,

 mMSForward [24] MMSForward,

 mMSDeleteFromRelay [25] MMSDeleteFromRelay,

 mMSDeliveryReport [26] MMSDeliveryReport,

 mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

 mMSReadReport [28] MMSReadReport,

 mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

 mMSCancel [30] MMSCancel,

 mMSMBoxStore [31] MMSMBoxStore,

 mMSMBoxUpload [32] MMSMBoxUpload,

 mMSMBoxDelete [33] MMSMBoxDelete,

 mMSMBoxViewRequest [34] MMSMBoxViewRequest,

 mMSMBoxViewResponse [35] MMSMBoxViewResponse,

 -- PTC-related events, see clause 7.5.2

 pTCRegistration [36] PTCRegistration,

 pTCSessionInitiation [37] PTCSessionInitiation,

 pTCSessionAbandon [38] PTCSessionAbandon,

 pTCSessionStart [39] PTCSessionStart,

 pTCSessionEnd [40] PTCSessionEnd,

 pTCStartOfInterception [41] PTCStartOfInterception,

 pTCPreEstablishedSession [42] PTCPreEstablishedSession,

 pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

 pTCPartyJoin [44] PTCPartyJoin,

 pTCPartyDrop [45] PTCPartyDrop,

 pTCPartyHold [46] PTCPartyHold,

 pTCMediaModification [47] PTCMediaModification,

 pTCGroupAdvertisement [48] PTCGroupAdvertisement,

 pTCFloorControl [49] PTCFloorControl,

 pTCTargetPresence [50] PTCTargetPresence,

 pTCParticipantPresence [51] PTCParticipantPresence,

 pTCListManagement [52] PTCListManagement,

 pTCAccessPolicy [53] PTCAccessPolicy,

 -- More Subscriber-management related events, see clause 7.2.2

 subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

 cancelLocationMessage [55] UDMCancelLocationMessage,

 -- SMS-related events, continued from choice 12

 sMSReport [56] SMSReport,

 -- MA PDU session-related events, see clause 6.2.3.2.7

 sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

 sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

 sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

 startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

 unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

 -- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

 aMFIdentifierAssocation [62] AMFIdentifierAssocation,

 mMEIdentifierAssocation [63] MMEIdentifierAssocation,

 -- PDU to MA PDU session-related events, see clause 6.2.3.2.8

 sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

 --EPS Events, see clause 6.3

 --MME Events, see clause 6.3.2.2

 mMEAttach [2531] MMEAttach,

 mMEDetach [2532] MMEDetach,

 mMELocationUpdate [2533] MMELocationUpdate,

 mMEStartOfInterceptionWithEPSAttachedUE [2534] MMEStartOfInterceptionWithEPSAttachedUE,

 mMEUnsuccessfulProcedure [2535] MMEUnsuccessfulProcedure

}

IRITargetIdentifier ::= SEQUENCE

{

 identifier [1] TargetIdentifier,

 provenance [2] TargetIdentifierProvenance OPTIONAL

}

-- ==============

-- HI3 CC payload

-- ==============

CCPayload ::= SEQUENCE

{

 cCPayloadOID [1] RELATIVE-OID,

 pDU [2] CCPDU

}

CCPDU ::= CHOICE

{

 uPFCCPDU [1] UPFCCPDU,

 extendedUPFCCPDU [2] ExtendedUPFCCPDU,

 mMSCCPDU [3] MMSCCPDU

}

-- ===========================

-- HI4 LI notification payload

-- ===========================

LINotificationPayload ::= SEQUENCE

{

 lINotificationPayloadOID [1] RELATIVE-OID,

 notification [2] LINotificationMessage

}

LINotificationMessage ::= CHOICE

{

 lINotification [1] LINotification

}

-- ==================

-- 5G AMF definitions

-- ==================

-- See clause 6.2.2.2.2 for details of this structure

AMFRegistration ::= SEQUENCE

{

 registrationType [1] AMFRegistrationType,

 registrationResult [2] AMFRegistrationResult,

 slice [3] Slice OPTIONAL,

 sUPI [4] SUPI,

 sUCI [5] SUCI OPTIONAL,

 pEI [6] PEI OPTIONAL,

 gPSI [7] GPSI OPTIONAL,

 gUTI [8] FiveGGUTI,

 location [9] Location OPTIONAL,

 non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

 fiveGSTAIList [11] TAIList OPTIONAL

}

-- See clause 6.2.2.2.3 for details of this structure

AMFDeregistration ::= SEQUENCE

{

 deregistrationDirection [1] AMFDirection,

 accessType [2] AccessType,

 sUPI [3] SUPI OPTIONAL,

 sUCI [4] SUCI OPTIONAL,

 pEI [5] PEI OPTIONAL,

 gPSI [6] GPSI OPTIONAL,

 gUTI [7] FiveGGUTI OPTIONAL,

 cause [8] FiveGMMCause OPTIONAL,

 location [9] Location OPTIONAL

}

-- See clause 6.2.2.2.4 for details of this structure

AMFLocationUpdate ::= SEQUENCE

{

 sUPI [1] SUPI,

 sUCI [2] SUCI OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 gUTI [5] FiveGGUTI OPTIONAL,

 location [6] Location

}

-- See clause 6.2.2.2.5 for details of this structure

AMFStartOfInterceptionWithRegisteredUE ::= SEQUENCE

{

 registrationResult [1] AMFRegistrationResult,

 registrationType [2] AMFRegistrationType OPTIONAL,

 slice [3] Slice OPTIONAL,

 sUPI [4] SUPI,

 sUCI [5] SUCI OPTIONAL,

 pEI [6] PEI OPTIONAL,

 gPSI [7] GPSI OPTIONAL,

 gUTI [8] FiveGGUTI,

 location [9] Location OPTIONAL,

 non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

 timeOfRegistration [11] Timestamp OPTIONAL,

 fiveGSTAIList [12] TAIList OPTIONAL

}

-- See clause 6.2.2.2.6 for details of this structure

AMFUnsuccessfulProcedure ::= SEQUENCE

{

 failedProcedureType [1] AMFFailedProcedureType,

 failureCause [2] AMFFailureCause,

 requestedSlice [3] NSSAI OPTIONAL,

 sUPI [4] SUPI OPTIONAL,

 sUCI [5] SUCI OPTIONAL,

 pEI [6] PEI OPTIONAL,

 gPSI [7] GPSI OPTIONAL,

 gUTI [8] FiveGGUTI OPTIONAL,

 location [9] Location OPTIONAL

}

-- =================

-- 5G AMF parameters

-- =================

AMFID ::= SEQUENCE

{

 aMFRegionID [1] AMFRegionID,

 aMFSetID [2] AMFSetID,

 aMFPointer [3] AMFPointer

}

AMFDirection ::= ENUMERATED

{

 networkInitiated(1),

 uEInitiated(2)

}

AMFFailedProcedureType ::= ENUMERATED

{

 registration(1),

 sMS(2),

 pDUSessionEstablishment(3)

}

AMFFailureCause ::= CHOICE

{

 fiveGMMCause [1] FiveGMMCause,

 fiveGSMCause [2] FiveGSMCause

}

AMFPointer ::= INTEGER (0..63)

AMFRegistrationResult ::= ENUMERATED

{

 threeGPPAccess(1),

 nonThreeGPPAccess(2),

 threeGPPAndNonThreeGPPAccess(3)

}

AMFRegionID ::= INTEGER (0..255)

AMFRegistrationType ::= ENUMERATED

{

 initial(1),

 mobility(2),

 periodic(3),

 emergency(4)

}

AMFSetID ::= INTEGER (0..1023)

-- ==================

-- 5G SMF definitions

-- ==================

-- See clause 6.2.3.2.2 for details of this structure

SMFPDUSessionEstablishment ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 gTPTunnelID [6] FTEID,

 pDUSessionType [7] PDUSessionType,

 sNSSAI [8] SNSSAI OPTIONAL,

 uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

 non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

 location [11] Location OPTIONAL,

 dNN [12] DNN,

 aMFID [13] AMFID OPTIONAL,

 hSMFURI [14] HSMFURI OPTIONAL,

 requestType [15] FiveGSMRequestType,

 accessType [16] AccessType OPTIONAL,

 rATType [17] RATType OPTIONAL,

 sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

 uEEPSPDNConnection [19] UEEPSPDNConnection OPTIONAL

}

-- See clause 6.2.3.2.3 for details of this structure

SMFPDUSessionModification ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 sNSSAI [5] SNSSAI OPTIONAL,

 non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

 location [7] Location OPTIONAL,

 requestType [8] FiveGSMRequestType,

 accessType [9] AccessType OPTIONAL,

 rATType [10] RATType OPTIONAL,

 pDUSessionID [11] PDUSessionID OPTIONAL

}

-- See clause 6.2.3.2.4 for details of this structure

SMFPDUSessionRelease ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 pDUSessionID [4] PDUSessionID,

 timeOfFirstPacket [5] Timestamp OPTIONAL,

 timeOfLastPacket [6] Timestamp OPTIONAL,

 uplinkVolume [7] INTEGER OPTIONAL,

 downlinkVolume [8] INTEGER OPTIONAL,

 location [9] Location OPTIONAL,

 cause [10] SMFErrorCodes OPTIONAL

}

-- See clause 6.2.3.2.5 for details of this structure

SMFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 gTPTunnelID [6] FTEID,

 pDUSessionType [7] PDUSessionType,

 sNSSAI [8] SNSSAI OPTIONAL,

 uEEndpoint [9] SEQUENCE OF UEEndpointAddress,

 non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

 location [11] Location OPTIONAL,

 dNN [12] DNN,

 aMFID [13] AMFID OPTIONAL,

 hSMFURI [14] HSMFURI OPTIONAL,

 requestType [15] FiveGSMRequestType,

 accessType [16] AccessType OPTIONAL,

 rATType [17] RATType OPTIONAL,

 sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

 timeOfSessionEstablishment [19] Timestamp OPTIONAL

}

-- See clause 6.2.3.2.6 for details of this structure

SMFUnsuccessfulProcedure ::= SEQUENCE

{

 failedProcedureType [1] SMFFailedProcedureType,

 failureCause [2] FiveGSMCause,

 initiator [3] Initiator,

 requestedSlice [4] NSSAI OPTIONAL,

 sUPI [5] SUPI OPTIONAL,

 sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [7] PEI OPTIONAL,

 gPSI [8] GPSI OPTIONAL,

 pDUSessionID [9] PDUSessionID OPTIONAL,

 uEEndpoint [10] SEQUENCE OF UEEndpointAddress OPTIONAL,

 non3GPPAccessEndpoint [11] UEEndpointAddress OPTIONAL,

 dNN [12] DNN OPTIONAL,

 aMFID [13] AMFID OPTIONAL,

 hSMFURI [14] HSMFURI OPTIONAL,

 requestType [15] FiveGSMRequestType OPTIONAL,

 accessType [16] AccessType OPTIONAL,

 rATType [17] RATType OPTIONAL,

 sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

 location [19] Location OPTIONAL

}

-- See clause 6.2.3.2.8 for details of this structure

SMFPDUtoMAPDUSessionModification ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 sNSSAI [5] SNSSAI OPTIONAL,

 non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

 location [7] Location OPTIONAL,

 requestType [8] FiveGSMRequestType,

 accessType [9] AccessType OPTIONAL,

 rATType [10] RATType OPTIONAL,

 pDUSessionID [11] PDUSessionID,

 requestIndication [12] RequestIndication,

 aTSSSContainer [13] ATSSSContainer

}

-- See clause 6.2.3.2.7.1 for details of this structure

SMFMAPDUSessionEstablishment ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 pDUSessionType [6] PDUSessionType,

 accessInfo [7] SEQUENCE OF AccessInfo,

 sNSSAI [8] SNSSAI OPTIONAL,

 uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

 location [10] Location OPTIONAL,

 dNN [11] DNN,

 aMFID [12] AMFID OPTIONAL,

 hSMFURI [13] HSMFURI OPTIONAL,

 requestType [14] FiveGSMRequestType,

 sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

 servingNetwork [16] SMFServingNetwork,

 oldPDUSessionID [17] PDUSessionID OPTIONAL,

 mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

 ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

 mAAcceptedIndication [20] SMFMAAcceptedIndication,

 aTSSSContainer [21] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.2 for details of this structure

SMFMAPDUSessionModification ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 accessInfo [6] SEQUENCE OF AccessInfo OPTIONAL,

 sNSSAI [7] SNSSAI OPTIONAL,

 location [8] Location OPTIONAL,

 requestType [9] FiveGSMRequestType OPTIONAL,

 servingNetwork [10] SMFServingNetwork,

 oldPDUSessionID [11] PDUSessionID OPTIONAL,

 mAUpgradeIndication [12] SMFMAUpgradeIndication OPTIONAL,

 ePSPDNCnxInfo [13] SMFEPSPDNCnxInfo OPTIONAL,

 mAAcceptedIndication [14] SMFMAAcceptedIndication,

 aTSSSContainer [15] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.3 for details of this structure

SMFMAPDUSessionRelease ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 pDUSessionID [4] PDUSessionID,

 timeOfFirstPacket [5] Timestamp OPTIONAL,

 timeOfLastPacket [6] Timestamp OPTIONAL,

 uplinkVolume [7] INTEGER OPTIONAL,

 downlinkVolume [8] INTEGER OPTIONAL,

 location [9] Location OPTIONAL,

 cause [10] SMFErrorCodes OPTIONAL

}

-- See clause 6.2.3.2.7.4 for details of this structure

SMFStartOfInterceptionWithEstablishedMAPDUSession ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 pDUSessionType [6] PDUSessionType,

 accessInfo [7] SEQUENCE OF AccessInfo,

 sNSSAI [8] SNSSAI OPTIONAL,

 uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

 location [10] Location OPTIONAL,

 dNN [11] DNN,

 aMFID [12] AMFID OPTIONAL,

 hSMFURI [13] HSMFURI OPTIONAL,

 requestType [14] FiveGSMRequestType OPTIONAL,

 sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

 servingNetwork [16] SMFServingNetwork,

 oldPDUSessionID [17] PDUSessionID OPTIONAL,

 mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

 ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

 mAAcceptedIndication [20] SMFMAAcceptedIndication,

 aTSSSContainer [21] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.5 for details of this structure

SMFMAUnsuccessfulProcedure ::= SEQUENCE

{

 failedProcedureType [1] SMFFailedProcedureType,

 failureCause [2] FiveGSMCause,

 requestedSlice [3] NSSAI OPTIONAL,

 initiator [4] Initiator,

 sUPI [5] SUPI OPTIONAL,

 sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [7] PEI OPTIONAL,

 gPSI [8] GPSI OPTIONAL,

 pDUSessionID [9] PDUSessionID OPTIONAL,

 accessInfo [10] SEQUENCE OF AccessInfo,

 uEEndpoint [11] SEQUENCE OF UEEndpointAddress OPTIONAL,

 location [12] Location OPTIONAL,

 dNN [13] DNN OPTIONAL,

 aMFID [14] AMFID OPTIONAL,

 hSMFURI [15] HSMFURI OPTIONAL,

 requestType [16] FiveGSMRequestType OPTIONAL,

 sMPDUDNRequest [17] SMPDUDNRequest OPTIONAL

}

-- =================

-- 5G SMF parameters

-- =================

SMFFailedProcedureType ::= ENUMERATED

{

 pDUSessionEstablishment(1),

 pDUSessionModification(2),

 pDUSessionRelease(3)

}

SMFServingNetwork ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 nID [2] NID OPTIONAL

}

AccessInfo ::= SEQUENCE

{

 accessType [1] AccessType,

 rATType [2] RATType OPTIONAL,

 gTPTunnelID [3] FTEID,

 non3GPPAccessEndpoint [4] UEEndpointAddress OPTIONAL,

 establishmentStatus [5] EstablishmentStatus,

 aNTypeToReactivate [6] AccessType OPTIONAL

}

-- see Clause 6.1.2 of TS 24.193[44] for the details of the ATSSS container contents.

ATSSSContainer ::= OCTET STRING

EstablishmentStatus ::= ENUMERATED

{

 established(0),

 released(1)

}

SMFMAUpgradeIndication ::= BOOLEAN

-- Given in YAML encoding as defined in clause 6.1.6.2.31 of TS 29.502[16]

SMFEPSPDNCnxInfo ::= UTF8String

SMFMAAcceptedIndication ::= BOOLEAN

-- see Clause 6.1.6.3.8 of TS 29.502[16] for the details of this structure.

SMFErrorCodes ::= UTF8String

-- see Clause 6.1.6.3.2 of TS 29.502[16] for details of this structure.

UEEPSPDNConnection ::= OCTET STRING

-- see Clause 6.1.6.3.6 of TS 29.502[16] for the details of this structure.

RequestIndication ::= ENUMERATED

{

 uEREQPDUSESMOD(0),

 uEREQPDUSESREL(1),

 pDUSESMOB(2),

 nWREQPDUSESAUTH(3),

 nWREQPDUSESMOD(4),

 nWREQPDUSESREL(5),

 eBIASSIGNMENTREQ(6),

 rELDUETO5GANREQUEST(7)

}

-- ==================

-- 5G UPF definitions

-- ==================

UPFCCPDU ::= OCTET STRING

-- See clause 6.2.3.8 for the details of this structure

ExtendedUPFCCPDU ::= SEQUENCE

{

 payload [1] UPFCCPDUPayload,

 qFI [2] QFI OPTIONAL

}

-- =================

-- 5G UPF parameters

-- =================

UPFCCPDUPayload ::= CHOICE

{

 uPFIPCC [1] OCTET STRING,

 uPFEthernetCC [2] OCTET STRING,

 uPFUnstructuredCC [3] OCTET STRING

}

QFI ::= INTEGER (0..63)

-- ==================

-- 5G UDM definitions

-- ==================

UDMServingSystemMessage ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 gUAMI [4] GUAMI OPTIONAL,

 gUMMEI [5] GUMMEI OPTIONAL,

 pLMNID [6] PLMNID OPTIONAL,

 servingSystemMethod [7] UDMServingSystemMethod,

 serviceID [8] ServiceID OPTIONAL

}

UDMSubscriberRecordChangeMessage ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 oldPEI [4] PEI OPTIONAL,

 oldSUPI [5] SUPI OPTIONAL,

 oldGPSI [6] GPSI OPTIONAL,

 oldserviceID [7] ServiceID OPTIONAL,

 subscriberRecordChangeMethod [8] UDMSubscriberRecordChangeMethod,

 serviceID [9] ServiceID OPTIONAL

}

UDMCancelLocationMessage ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 gUAMI [4] GUAMI OPTIONAL,

 pLMNID [5] PLMNID OPTIONAL,

 cancelLocationMethod [6] UDMCancelLocationMethod

}

-- =================

-- 5G UDM parameters

-- =================

UDMServingSystemMethod ::= ENUMERATED

{

 amf3GPPAccessRegistration(0),

 amfNon3GPPAccessRegistration(1),

 unknown(2)

}

UDMSubscriberRecordChangeMethod ::= ENUMERATED

{

 pEIChange(1),

 sUPIChange(2),

 gPSIChange(3),

 uEDeprovisioning(4),

 unknown(5),

 serviceIDChange(6)

}

UDMCancelLocationMethod ::= ENUMERATED

{

 aMF3GPPAccessDeregistration(1),

 aMFNon3GPPAccessDeregistration(2),

 uDMDeregistration(3),

 unknown(4)

}

ServiceID ::= SEQUENCE

{

 nSSAI [1] NSSAI OPTIONAL,

 cAGID [2] SEQUENCE OF CAGID OPTIONAL

}

CAGID ::= UTF8String

-- ===================

-- 5G SMSF definitions

-- ===================

-- See clause 6.2.5.3 for details of this structure

SMSMessage ::= SEQUENCE

{

 originatingSMSParty [1] SMSParty,

 terminatingSMSParty [2] SMSParty,

 direction [3] Direction,

 linkTransferStatus [4] SMSTransferStatus,

 otherMessage [5] SMSOtherMessageIndication OPTIONAL,

 location [6] Location OPTIONAL,

 peerNFAddress [7] SMSNFAddress OPTIONAL,

 peerNFType [8] SMSNFType OPTIONAL,

 sMSTPDUData [9] SMSTPDUData OPTIONAL,

 messageType [10] SMSMessageType OPTIONAL,

 rPMessageReference [11] SMSRPMessageReference OPTIONAL

}

SMSReport ::= SEQUENCE

{

 location [1] Location OPTIONAL,

 sMSTPDUData [2] SMSTPDUData,

 messageType [3] SMSMessageType,

 rPMessageReference [4] SMSRPMessageReference

}

-- ==================

-- 5G SMSF parameters

-- ==================

SMSAddress ::= OCTET STRING(SIZE(2..12))

SMSMessageType ::= ENUMERATED

{

 deliver(1),

 deliverReportAck(2),

 deliverReportError(3),

 statusReport(4),

 command(5),

 submit(6),

 submitReportAck(7),

 submitReportError(8),

 reserved(9)

}

SMSParty ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 sMSAddress [4] SMSAddress OPTIONAL

}

SMSTransferStatus ::= ENUMERATED

{

 transferSucceeded(1),

 transferFailed(2),

 undefined(3)

}

SMSOtherMessageIndication ::= BOOLEAN

SMSNFAddress ::= CHOICE

{

 iPAddress [1] IPAddress,

 e164Number [2] E164Number

}

SMSNFType ::= ENUMERATED

{

 sMSGMSC(1),

 iWMSC(2),

 sMSRouter(3)

}

SMSRPMessageReference ::= INTEGER (0..255)

SMSTPDUData ::= CHOICE

{

 sMSTPDU [1] SMSTPDU,

 truncatedSMSTPDU [2] TruncatedSMSTPDU

}

SMSTPDU ::= OCTET STRING (SIZE(1..270))

TruncatedSMSTPDU ::= OCTET STRING (SIZE(1..130))

-- ===============

-- MMS definitions

-- ===============

MMSSend ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 dateTime [3] Timestamp,

 originatingMMSParty [4] MMSParty,

 terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

 cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

 bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

 direction [8] MMSDirection,

 subject [9] MMSSubject OPTIONAL,

 messageClass [10] MMSMessageClass OPTIONAL,

 expiry [11] MMSExpiry,

 desiredDeliveryTime [12] Timestamp OPTIONAL,

 priority [13] MMSPriority OPTIONAL,

 senderVisibility [14] BOOLEAN OPTIONAL,

 deliveryReport [15] BOOLEAN OPTIONAL,

 readReport [16] BOOLEAN OPTIONAL,

 store [17] BOOLEAN OPTIONAL,

 state [18] MMState OPTIONAL,

 flags [19] MMFlags OPTIONAL,

 replyCharging [20] MMSReplyCharging OPTIONAL,

 applicID [21] UTF8String OPTIONAL,

 replyApplicID [22] UTF8String OPTIONAL,

 auxApplicInfo [23] UTF8String OPTIONAL,

 contentClass [24] MMSContentClass OPTIONAL,

 dRMContent [25] BOOLEAN OPTIONAL,

 adaptationAllowed [26] MMSAdaptation OPTIONAL,

 contentType [27] MMSContentType,

 responseStatus [28] MMSResponseStatus,

 responseStatusText [29] UTF8String OPTIONAL,

 messageID [30] UTF8String

}

MMSSendByNonLocalTarget ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 messageID [3] UTF8String,

 terminatingMMSParty [4] SEQUENCE OF MMSParty,

 originatingMMSParty [5] MMSParty,

 direction [6] MMSDirection,

 contentType [7] MMSContentType,

 messageClass [8] MMSMessageClass OPTIONAL,

 dateTime [9] Timestamp,

 expiry [10] MMSExpiry OPTIONAL,

 deliveryReport [11] BOOLEAN OPTIONAL,

 priority [12] MMSPriority OPTIONAL,

 senderVisibility [13] BOOLEAN OPTIONAL,

 readReport [14] BOOLEAN OPTIONAL,

 subject [15] MMSSubject OPTIONAL,

 forwardCount [16] INTEGER OPTIONAL,

 previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

 prevSentByDateTime [18] Timestamp OPTIONAL,

 applicID [19] UTF8String OPTIONAL,

 replyApplicID [20] UTF8String OPTIONAL,

 auxApplicInfo [21] UTF8String OPTIONAL,

 contentClass [22] MMSContentClass OPTIONAL,

 dRMContent [23] BOOLEAN OPTIONAL,

 adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotification ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 originatingMMSParty [3] MMSParty OPTIONAL,

 direction [4] MMSDirection,

 subject [5] MMSSubject OPTIONAL,

 deliveryReportRequested [6] BOOLEAN OPTIONAL,

 stored [7] BOOLEAN OPTIONAL,

 messageClass [8] MMSMessageClass,

 priority [9] MMSPriority OPTIONAL,

 messageSize [10] INTEGER,

 expiry [11] MMSExpiry,

 replyCharging [12] MMSReplyCharging OPTIONAL

}

MMSSendToNonLocalTarget ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 messageID [3] UTF8String,

 terminatingMMSParty [4] SEQUENCE OF MMSParty,

 originatingMMSParty [5] MMSParty,

 direction [6] MMSDirection,

 contentType [7] MMSContentType,

 messageClass [8] MMSMessageClass OPTIONAL,

 dateTime [9] Timestamp,

 expiry [10] MMSExpiry OPTIONAL,

 deliveryReport [11] BOOLEAN OPTIONAL,

 priority [12] MMSPriority OPTIONAL,

 senderVisibility [13] BOOLEAN OPTIONAL,

 readReport [14] BOOLEAN OPTIONAL,

 subject [15] MMSSubject OPTIONAL,

 forwardCount [16] INTEGER OPTIONAL,

 previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

 prevSentByDateTime [18] Timestamp OPTIONAL,

 applicID [19] UTF8String OPTIONAL,

 replyApplicID [20] UTF8String OPTIONAL,

 auxApplicInfo [21] UTF8String OPTIONAL,

 contentClass [22] MMSContentClass OPTIONAL,

 dRMContent [23] BOOLEAN OPTIONAL,

 adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotificationResponse ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 status [4] MMStatus,

 reportAllowed [5] BOOLEAN OPTIONAL

}

MMSRetrieval ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 messageID [3] UTF8String,

 dateTime [4] Timestamp,

 originatingMMSParty [5] MMSParty OPTIONAL,

 previouslySentBy [6] MMSPreviouslySentBy OPTIONAL,

 prevSentByDateTime [7] Timestamp OPTIONAL,

 terminatingMMSParty [8] SEQUENCE OF MMSParty OPTIONAL,

 cCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

 direction [10] MMSDirection,

 subject [11] MMSSubject OPTIONAL,

 state [12] MMState OPTIONAL,

 flags [13] MMFlags OPTIONAL,

 messageClass [14] MMSMessageClass OPTIONAL,

 priority [15] MMSPriority,

 deliveryReport [16] BOOLEAN OPTIONAL,

 readReport [17] BOOLEAN OPTIONAL,

 replyCharging [18] MMSReplyCharging OPTIONAL,

 retrieveStatus [19] MMSRetrieveStatus OPTIONAL,

 retrieveStatusText [20] UTF8String OPTIONAL,

 applicID [21] UTF8String OPTIONAL,

 replyApplicID [22] UTF8String OPTIONAL,

 auxApplicInfo [23] UTF8String OPTIONAL,

 contentClass [24] MMSContentClass OPTIONAL,

 dRMContent [25] BOOLEAN OPTIONAL,

 replaceID [26] UTF8String OPTIONAL,

 contentType [27] UTF8String OPTIONAL

}

MMSDeliveryAck ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 reportAllowed [3] BOOLEAN OPTIONAL,

 status [4] MMStatus,

 direction [5] MMSDirection

}

MMSForward ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 dateTime [3] Timestamp OPTIONAL,

 originatingMMSParty [4] MMSParty,

 terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

 cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

 bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

 direction [8] MMSDirection,

 expiry [9] MMSExpiry OPTIONAL,

 desiredDeliveryTime [10] Timestamp OPTIONAL,

 deliveryReportAllowed [11] BOOLEAN OPTIONAL,

 deliveryReport [12] BOOLEAN OPTIONAL,

 store [13] BOOLEAN OPTIONAL,

 state [14] MMState OPTIONAL,

 flags [15] MMFlags OPTIONAL,

 contentLocationReq [16] UTF8String,

 replyCharging [17] MMSReplyCharging OPTIONAL,

 responseStatus [18] MMSResponseStatus,

 responseStatusText [19] UTF8String OPTIONAL,

 messageID [20] UTF8String OPTIONAL,

 contentLocationConf [21] UTF8String OPTIONAL,

 storeStatus [22] MMSStoreStatus OPTIONAL,

 storeStatusText [23] UTF8String OPTIONAL

}

MMSDeleteFromRelay ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 contentLocationReq [4] SEQUENCE OF UTF8String,

 contentLocationConf [5] SEQUENCE OF UTF8String,

 deleteResponseStatus [6] MMSDeleteResponseStatus,

 deleteResponseText [7] SEQUENCE OF UTF8String

}

MMSMBoxStore ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 contentLocationReq [4] UTF8String,

 state [5] MMState OPTIONAL,

 flags [6] MMFlags OPTIONAL,

 contentLocationConf [7] UTF8String OPTIONAL,

 storeStatus [8] MMSStoreStatus,

 storeStatusText [9] UTF8String OPTIONAL

}

MMSMBoxUpload ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 state [4] MMState OPTIONAL,

 flags [5] MMFlags OPTIONAL,

 contentType [6] UTF8String,

 contentLocation [7] UTF8String OPTIONAL,

 storeStatus [8] MMSStoreStatus,

 storeStatusText [9] UTF8String OPTIONAL,

 mMessages [10] SEQUENCE OF MMBoxDescription

}

MMSMBoxDelete ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 contentLocationReq [4] SEQUENCE OF UTF8String,

 contentLocationConf [5] SEQUENCE OF UTF8String OPTIONAL,

 responseStatus [6] MMSDeleteResponseStatus,

 responseStatusText [7] UTF8String OPTIONAL

}

MMSDeliveryReport ::= SEQUENCE

{

 version [1] MMSVersion,

 messageID [2] UTF8String,

 terminatingMMSParty [3] SEQUENCE OF MMSParty,

 mMSDateTime [4] Timestamp,

 responseStatus [5] MMSResponseStatus,

 responseStatusText [6] UTF8String OPTIONAL,

 applicID [7] UTF8String OPTIONAL,

 replyApplicID [8] UTF8String OPTIONAL,

 auxApplicInfo [9] UTF8String OPTIONAL

}

MMSDeliveryReportNonLocalTarget ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 messageID [3] UTF8String,

 terminatingMMSParty [4] SEQUENCE OF MMSParty,

 originatingMMSParty [5] MMSParty,

 direction [6] MMSDirection,

 mMSDateTime [7] Timestamp,

 forwardToOriginator [8] BOOLEAN OPTIONAL,

 status [9] MMStatus,

 statusExtension [10] MMStatusExtension,

 statusText [11] MMStatusText,

 applicID [12] UTF8String OPTIONAL,

 replyApplicID [13] UTF8String OPTIONAL,

 auxApplicInfo [14] UTF8String OPTIONAL

}

MMSReadReport ::= SEQUENCE

{

 version [1] MMSVersion,

 messageID [2] UTF8String,

 terminatingMMSParty [3] SEQUENCE OF MMSParty,

 originatingMMSParty [4] SEQUENCE OF MMSParty,

 direction [5] MMSDirection,

 mMSDateTime [6] Timestamp,

 readStatus [7] MMSReadStatus,

 applicID [8] UTF8String OPTIONAL,

 replyApplicID [9] UTF8String OPTIONAL,

 auxApplicInfo [10] UTF8String OPTIONAL

}

MMSReadReportNonLocalTarget ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 terminatingMMSParty [3] SEQUENCE OF MMSParty,

 originatingMMSParty [4] SEQUENCE OF MMSParty,

 direction [5] MMSDirection,

 messageID [6] UTF8String,

 mMSDateTime [7] Timestamp,

 readStatus [8] MMSReadStatus,

 readStatusText [9] MMSReadStatusText OPTIONAL,

 applicID [10] UTF8String OPTIONAL,

 replyApplicID [11] UTF8String OPTIONAL,

 auxApplicInfo [12] UTF8String OPTIONAL

}

MMSCancel ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 cancelID [3] UTF8String,

 direction [4] MMSDirection

}

MMSMBoxViewRequest ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 contentLocation [3] UTF8String OPTIONAL,

 state [4] SEQUENCE OF MMState OPTIONAL,

 flags [5] SEQUENCE OF MMFlags OPTIONAL,

 start [6] INTEGER OPTIONAL,

 limit [7] INTEGER OPTIONAL,

 attributes [8] SEQUENCE OF UTF8String OPTIONAL,

 totals [9] INTEGER OPTIONAL,

 quotas [10] MMSQuota OPTIONAL

}

MMSMBoxViewResponse ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 contentLocation [3] UTF8String OPTIONAL,

 state [4] SEQUENCE OF MMState OPTIONAL,

 flags [5] SEQUENCE OF MMFlags OPTIONAL,

 start [6] INTEGER OPTIONAL,

 limit [7] INTEGER OPTIONAL,

 attributes [8] SEQUENCE OF UTF8String OPTIONAL,

 mMSTotals [9] BOOLEAN OPTIONAL,

 mMSQuotas [10] BOOLEAN OPTIONAL,

 mMessages [11] SEQUENCE OF MMBoxDescription

}

MMBoxDescription ::= SEQUENCE

{

 contentLocation [1] UTF8String OPTIONAL,

 messageID [2] UTF8String OPTIONAL,

 state [3] MMState OPTIONAL,

 flags [4] SEQUENCE OF MMFlags OPTIONAL,

 dateTime [5] Timestamp OPTIONAL,

 originatingMMSParty [6] MMSParty OPTIONAL,

 terminatingMMSParty [7] SEQUENCE OF MMSParty OPTIONAL,

 cCRecipients [8] SEQUENCE OF MMSParty OPTIONAL,

 bCCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

 messageClass [10] MMSMessageClass OPTIONAL,

 subject [11] MMSSubject OPTIONAL,

 priority [12] MMSPriority OPTIONAL,

 deliveryTime [13] Timestamp OPTIONAL,

 readReport [14] BOOLEAN OPTIONAL,

 messageSize [15] INTEGER OPTIONAL,

 replyCharging [16] MMSReplyCharging OPTIONAL,

 previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

 previouslySentByDateTime [18] Timestamp OPTIONAL,

 contentType [19] UTF8String OPTIONAL

}

-- =========

-- MMS CCPDU

-- =========

MMSCCPDU ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 mMSContent [3] OCTET STRING

}

-- ==============

-- MMS parameters

-- ==============

MMSAdaptation ::= SEQUENCE

{

 allowed [1] BOOLEAN,

 overriden [2] BOOLEAN

}

MMSCancelStatus ::= ENUMERATED

{

 cancelRequestSuccessfullyReceived(1),

 cancelRequestCorrupted(2)

}

MMSContentClass ::= ENUMERATED

{

 text(1),

 imageBasic(2),

 imageRich(3),

 videoBasic(4),

 videoRich(5),

 megaPixel(6),

 contentBasic(7),

 contentRich(8)

}

MMSContentType ::= UTF8String

MMSDeleteResponseStatus ::= ENUMERATED

{

 ok(1),

 errorUnspecified(2),

 errorServiceDenied(3),

 errorMessageFormatCorrupt(4),

 errorSendingAddressUnresolved(5),

 errorMessageNotFound(6),

 errorNetworkProblem(7),

 errorContentNotAccepted(8),

 errorUnsupportedMessage(9),

 errorTransientFailure(10),

 errorTransientSendingAddressUnresolved(11),

 errorTransientMessageNotFound(12),

 errorTransientNetworkProblem(13),

 errorTransientPartialSuccess(14),

 errorPermanentFailure(15),

 errorPermanentServiceDenied(16),

 errorPermanentMessageFormatCorrupt(17),

 errorPermanentSendingAddressUnresolved(18),

 errorPermanentMessageNotFound(19),

 errorPermanentContentNotAccepted(20),

 errorPermanentReplyChargingLimitationsNotMet(21),

 errorPermanentReplyChargingRequestNotAccepted(22),

 errorPermanentReplyChargingForwardingDenied(23),

 errorPermanentReplyChargingNotSupported(24),

 errorPermanentAddressHidingNotSupported(25),

 errorPermanentLackOfPrepaid(26)

}

MMSDirection ::= ENUMERATED

{

 fromTarget(0),

 toTarget(1)

}

MMSElementDescriptor ::= SEQUENCE

{

 reference [1] UTF8String,

 parameter [2] UTF8String OPTIONAL,

 value [3] UTF8String OPTIONAL

}

MMSExpiry ::= SEQUENCE

{

 expiryPeriod [1] INTEGER,

 periodFormat [2] MMSPeriodFormat

}

MMFlags ::= SEQUENCE

{

 length [1] INTEGER,

 flag [2] MMStateFlag,

 flagString [3] UTF8String

}

MMSMessageClass ::= ENUMERATED

{

 personal(1),

 advertisement(2),

 informational(3),

 auto(4)

}

MMSParty ::= SEQUENCE

{

 mMSPartyIDs [1] SEQUENCE OF MMSPartyID,

 nonLocalID [2] NonLocalID

}

MMSPartyID ::= CHOICE

{

 e164Number [1] E164Number,

 emailAddress [2] EmailAddress,

 iMSI [3] IMSI,

 iMPU [4] IMPU,

 iMPI [5] IMPI,

 sUPI [6] SUPI,

 gPSI [7] GPSI

}

MMSPeriodFormat ::= ENUMERATED

{

 absolute(1),

 relative(2)

}

MMSPreviouslySent ::= SEQUENCE

{

 previouslySentByParty [1] MMSParty,

 sequenceNumber [2] INTEGER,

 previousSendDateTime [3] Timestamp

}

MMSPreviouslySentBy ::= SEQUENCE OF MMSPreviouslySent

MMSPriority ::= ENUMERATED

{

 low(1),

 normal(2),

 high(3)

}

MMSQuota ::= SEQUENCE

{

 quota [1] INTEGER,

 quotaUnit [2] MMSQuotaUnit

}

MMSQuotaUnit ::= ENUMERATED

{

 numMessages(1),

 bytes(2)

}

MMSReadStatus ::= ENUMERATED

{

 read(1),

 deletedWithoutBeingRead(2)

}

MMSReadStatusText ::= UTF8String

MMSReplyCharging ::= ENUMERATED

{

 requested(0),

 requestedTextOnly(1),

 accepted(2),

 acceptedTextOnly(3)

}

MMSResponseStatus ::= ENUMERATED

{

 ok(1),

 errorUnspecified(2),

 errorServiceDenied(3),

 errorMessageFormatCorrupt(4),

 errorSendingAddressUnresolved(5),

 errorMessageNotFound(6),

 errorNetworkProblem(7),

 errorContentNotAccepted(8),

 errorUnsupportedMessage(9),

 errorTransientFailure(10),

 errorTransientSendingAddressUnresolved(11),

 errorTransientMessageNotFound(12),

 errorTransientNetworkProblem(13),

 errorTransientPartialSuccess(14),

 errorPermanentFailure(15),

 errorPermanentServiceDenied(16),

 errorPermanentMessageFormatCorrupt(17),

 errorPermanentSendingAddressUnresolved(18),

 errorPermanentMessageNotFound(19),

 errorPermanentContentNotAccepted(20),

 errorPermanentReplyChargingLimitationsNotMet(21),

 errorPermanentReplyChargingRequestNotAccepted(22),

 errorPermanentReplyChargingForwardingDenied(23),

 errorPermanentReplyChargingNotSupported(24),

 errorPermanentAddressHidingNotSupported(25),

 errorPermanentLackOfPrepaid(26)

}

MMSRetrieveStatus ::= ENUMERATED

{

 success(1),

 errorTransientFailure(2),

 errorTransientMessageNotFound(3),

 errorTransientNetworkProblem(4),

 errorPermanentFailure(5),

 errorPermanentServiceDenied(6),

 errorPermanentMessageNotFound(7),

 errorPermanentContentUnsupported(8)

}

MMSStoreStatus ::= ENUMERATED

{

 success(1),

 errorTransientFailure(2),

 errorTransientNetworkProblem(3),

 errorPermanentFailure(4),

 errorPermanentServiceDenied(5),

 errorPermanentMessageFormatCorrupt(6),

 errorPermanentMessageNotFound(7),

 errorMMBoxFull(8)

}

MMState ::= ENUMERATED

{

 draft(1),

 sent(2),

 new(3),

 retrieved(4),

 forwarded(5)

}

MMStateFlag ::= ENUMERATED

{

 add(1),

 remove(2),

 filter(3)

}

MMStatus ::= ENUMERATED

{

 expired(1),

 retrieved(2),

 rejected(3),

 deferred(4),

 unrecognized(5),

 indeterminate(6),

 forwarded(7),

 unreachable(8)

}

MMStatusExtension ::= ENUMERATED

{

 rejectionByMMSRecipient(0),

 rejectionByOtherRS(1)

}

MMStatusText ::= UTF8String

MMSSubject ::= UTF8String

MMSVersion ::= SEQUENCE

{

 majorVersion [1] INTEGER,

 minorVersion [2] INTEGER

}

-- ==================

-- 5G PTC definitions

-- ==================

PTCRegistration ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCServerURI [2] UTF8String,

 pTCRegistrationRequest [3] PTCRegistrationRequest,

 pTCRegistrationOutcome [4] PTCRegistrationOutcome

}

PTCSessionInitiation ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCServerURI [3] UTF8String,

 pTCSessionInfo [4] PTCSessionInfo,

 pTCOriginatingID [5] PTCTargetInformation,

 pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

 location [8] Location OPTIONAL,

 pTCBearerCapability [9] UTF8String OPTIONAL,

 pTCHost [10] PTCTargetInformation OPTIONAL

}

PTCSessionAbandon ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 location [4] Location OPTIONAL,

 pTCAbandonCause [5] INTEGER

}

PTCSessionStart ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCServerURI [3] UTF8String,

 pTCSessionInfo [4] PTCSessionInfo,

 pTCOriginatingID [5] PTCTargetInformation,

 pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

 location [8] Location OPTIONAL,

 pTCHost [9] PTCTargetInformation OPTIONAL,

 pTCBearerCapability [10] UTF8String OPTIONAL

}

PTCSessionEnd ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCServerURI [3] UTF8String,

 pTCSessionInfo [4] PTCSessionInfo,

 pTCParticipants [5] SEQUENCE OF PTCTargetInformation OPTIONAL,

 location [6] Location OPTIONAL,

 pTCSessionEndCause [7] PTCSessionEndCause

}

PTCStartOfInterception ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 preEstSessionID [3] PTCSessionInfo OPTIONAL,

 pTCOriginatingID [4] PTCTargetInformation,

 pTCSessionInfo [5] PTCSessionInfo OPTIONAL,

 pTCHost [6] PTCTargetInformation OPTIONAL,

 pTCParticipants [7] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCMediaStreamAvail [8] BOOLEAN OPTIONAL,

 pTCBearerCapability [9] UTF8String OPTIONAL

}

PTCPreEstablishedSession ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCServerURI [2] UTF8String,

 rTPSetting [3] RTPSetting,

 pTCMediaCapability [4] UTF8String,

 pTCPreEstSessionID [5] PTCSessionInfo,

 pTCPreEstStatus [6] PTCPreEstStatus,

 pTCMediaStreamAvail [7] BOOLEAN OPTIONAL,

 location [8] Location OPTIONAL,

 pTCFailureCode [9] PTCFailureCode OPTIONAL

}

PTCInstantPersonalAlert ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCIPAPartyID [2] PTCTargetInformation,

 pTCIPADirection [3] Direction

}

PTCPartyJoin ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCParticipantPresenceStatus [5] MultipleParticipantPresenceStatus OPTIONAL,

 pTCMediaStreamAvail [6] BOOLEAN OPTIONAL,

 pTCBearerCapability [7] UTF8String OPTIONAL

}

PTCPartyDrop ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 pTCPartyDrop [4] PTCTargetInformation,

 pTCParticipantPresenceStatus [5] PTCParticipantPresenceStatus OPTIONAL

}

PTCPartyHold ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCHoldID [5] SEQUENCE OF PTCTargetInformation,

 pTCHoldRetrieveInd [6] BOOLEAN

}

PTCMediaModification ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 pTCMediaStreamAvail [4] BOOLEAN OPTIONAL,

 pTCBearerCapability [5] UTF8String

}

PTCGroupAdvertisement ::=SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCIDList [3] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCGroupAuthRule [4] PTCGroupAuthRule OPTIONAL,

 pTCGroupAdSender [5] PTCTargetInformation,

 pTCGroupNickname [6] UTF8String OPTIONAL

}

PTCFloorControl ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessioninfo [3] PTCSessionInfo,

 pTCFloorActivity [4] SEQUENCE OF PTCFloorActivity,

 pTCFloorSpeakerID [5] PTCTargetInformation OPTIONAL,

 pTCMaxTBTime [6] INTEGER OPTIONAL,

 pTCQueuedFloorControl [7] BOOLEAN OPTIONAL,

 pTCQueuedPosition [8] INTEGER OPTIONAL,

 pTCTalkBurstPriority [9] PTCTBPriorityLevel OPTIONAL,

 pTCTalkBurstReason [10] PTCTBReasonCode OPTIONAL

}

PTCTargetPresence ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCTargetPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCParticipantPresence ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCParticipantPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCListManagement ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCListManagementType [3] PTCListManagementType OPTIONAL,

 pTCListManagementAction [4] PTCListManagementAction OPTIONAL,

 pTCListManagementFailure [5] PTCListManagementFailure OPTIONAL,

 pTCContactID [6] PTCTargetInformation OPTIONAL,

 pTCIDList [7] SEQUENCE OF PTCIDList OPTIONAL,

 pTCHost [8] PTCTargetInformation OPTIONAL

}

PTCAccessPolicy ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCAccessPolicyType [3] PTCAccessPolicyType OPTIONAL,

 pTCUserAccessPolicy [4] PTCUserAccessPolicy OPTIONAL,

 pTCGroupAuthRule [5] PTCGroupAuthRule OPTIONAL,

 pTCContactID [6] PTCTargetInformation OPTIONAL,

 pTCAccessPolicyFailure [7] PTCAccessPolicyFailure OPTIONAL

}

-- =================

-- 5G PTC parameters

-- =================

PTCRegistrationRequest ::= ENUMERATED

{

 register(1),

 reRegister(2),

 deRegister(3)

}

PTCRegistrationOutcome ::= ENUMERATED

{

 success(1),

 failure(2)

}

PTCSessionEndCause ::= ENUMERATED

{

 initiaterLeavesSession(1),

 definedParticipantLeaves(2),

 numberOfParticipants(3),

 sessionTimerExpired(4),

 pTCSpeechInactive(5),

 allMediaTypesInactive(6)

}

PTCTargetInformation ::= SEQUENCE

{

 identifiers [1] SEQUENCE SIZE(1..MAX) OF PTCIdentifiers

}

PTCIdentifiers ::= CHOICE

{

 mCPTTID [1] UTF8String,

 instanceIdentifierURN [2] UTF8String,

 pTCChatGroupID [3] PTCChatGroupID,

 iMPU [4] IMPU,

 iMPI [5] IMPI

}

PTCSessionInfo ::= SEQUENCE

{

 pTCSessionURI [1] UTF8String,

 pTCSessionType [2] PTCSessionType

}

PTCSessionType ::= ENUMERATED

{

 ondemand(1),

 preEstablished(2),

 adhoc(3),

 prearranged(4),

 groupSession(5)

}

MultipleParticipantPresenceStatus ::= SEQUENCE OF PTCParticipantPresenceStatus

PTCParticipantPresenceStatus ::= SEQUENCE

{

 presenceID [1] PTCTargetInformation,

 presenceType [2] PTCPresenceType,

 presenceStatus [3] BOOLEAN

}

PTCPresenceType ::= ENUMERATED

{

 pTCClient(1),

 pTCGroup(2)

}

PTCPreEstStatus ::= ENUMERATED

{

 established(1),

 modified(2),

 released(3)

}

RTPSetting ::= SEQUENCE

{

 iPAddress [1] IPAddress,

 portNumber [2] PortNumber

}

PTCIDList ::= SEQUENCE

{

 pTCPartyID [1] PTCTargetInformation,

 pTCChatGroupID [2] PTCChatGroupID

}

PTCChatGroupID ::= SEQUENCE

{

 groupIdentity [1] UTF8String

}

PTCFloorActivity ::= ENUMERATED

{

 tBCPRequest(1),

 tBCPGranted(2),

 tBCPDeny(3),

 tBCPIdle(4),

 tBCPTaken(5),

 tBCPRevoke(6),

 tBCPQueued(7),

 tBCPRelease(8)

}

PTCTBPriorityLevel ::= ENUMERATED

{

 preEmptive(1),

 highPriority(2),

 normalPriority(3),

 listenOnly(4)

}

PTCTBReasonCode ::= ENUMERATED

{

 noQueuingAllowed(1),

 oneParticipantSession(2),

 listenOnly(3),

 exceededMaxDuration(4),

 tBPrevented(5)

}

PTCListManagementType ::= ENUMERATED

{

 contactListManagementAttempt(1),

 groupListManagementAttempt(2),

 contactListManagementResult(3),

 groupListManagementResult(4),

 requestUnsuccessful(5)

}

PTCListManagementAction ::= ENUMERATED

{

 create(1),

 modify(2),

 retrieve(3),

 delete(4),

 notify(5)

}

PTCAccessPolicyType ::= ENUMERATED

{

 pTCUserAccessPolicyAttempt(1),

 groupAuthorizationRulesAttempt(2),

 pTCUserAccessPolicyQuery(3),

 groupAuthorizationRulesQuery(4),

 pTCUserAccessPolicyResult(5),

 groupAuthorizationRulesResult(6),

 requestUnsuccessful(7)

}

PTCUserAccessPolicy ::= ENUMERATED

{

 allowIncomingPTCSessionRequest(1),

 blockIncomingPTCSessionRequest(2),

 allowAutoAnswerMode(3),

 allowOverrideManualAnswerMode(4)

}

PTCGroupAuthRule ::= ENUMERATED

{

 allowInitiatingPTCSession(1),

 blockInitiatingPTCSession(2),

 allowJoiningPTCSession(3),

 blockJoiningPTCSession(4),

 allowAddParticipants(5),

 blockAddParticipants(6),

 allowSubscriptionPTCSessionState(7),

 blockSubscriptionPTCSessionState(8),

 allowAnonymity(9),

 forbidAnonymity(10)

}

PTCFailureCode ::= ENUMERATED

{

 sessionCannotBeEstablished(1),

 sessionCannotBeModified(2)

}

PTCListManagementFailure ::= ENUMERATED

{

 requestUnsuccessful(1),

 requestUnknown(2)

}

PTCAccessPolicyFailure ::= ENUMERATED

{

 requestUnsuccessful(1),

 requestUnknown(2)

}

-- ===================

-- 5G LALS definitions

-- ===================

LALSReport ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 location [4] Location OPTIONAL

}

-- =====================

-- PDHR/PDSR definitions

-- =====================

PDHeaderReport ::= SEQUENCE

{

 pDUSessionID [1] PDUSessionID,

 sourceIPAddress [2] IPAddress,

 sourcePort [3] PortNumber OPTIONAL,

 destinationIPAddress [4] IPAddress,

 destinationPort [5] PortNumber OPTIONAL,

 nextLayerProtocol [6] NextLayerProtocol,

 iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

 direction [8] Direction,

 packetSize [9] INTEGER

}

PDSummaryReport ::= SEQUENCE

{

 pDUSessionID [1] PDUSessionID,

 sourceIPAddress [2] IPAddress,

 sourcePort [3] PortNumber OPTIONAL,

 destinationIPAddress [4] IPAddress,

 destinationPort [5] PortNumber OPTIONAL,

 nextLayerProtocol [6] NextLayerProtocol,

 iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

 direction [8] Direction,

 pDSRSummaryTrigger [9] PDSRSummaryTrigger,

 firstPacketTimestamp [10] Timestamp,

 lastPacketTimestamp [11] Timestamp,

 packetCount [12] INTEGER,

 byteCount [13] INTEGER

}

-- ====================

-- PDHR/PDSR parameters

-- ====================

PDSRSummaryTrigger ::= ENUMERATED

{

 timerExpiry(1),

 packetCount(2),

 byteCount(3),

 startOfFlow(4),

 endOfFlow(5)

}

-- ==================================

-- Identifier Association definitions

-- ==================================

AMFIdentifierAssocation ::= SEQUENCE

{

 sUPI [1] SUPI,

 sUCI [2] SUCI OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 gUTI [5] FiveGGUTI,

 location [6] Location,

 fiveGSTAIList [7] TAIList OPTIONAL

}

MMEIdentifierAssocation ::= SEQUENCE

{

 iMSI [1] IMSI,

 iMEI [2] IMEI OPTIONAL,

 mSISDN [3] MSISDN OPTIONAL,

 gUTI [4] GUTI,

 location [5] Location,

 tAIList [6] TAIList OPTIONAL

}

-- =================================

-- Identifier Association parameters

-- =================================

GUTI ::= SEQUENCE

{

 mCC [1] MCC,

 mNC [2] MNC,

 mMEGroupID [3] MMEGroupID,

 mMECode [4] MMECode,

 mTMSI [5] TMSI

}

MMEGroupID ::= OCTET STRING (SIZE(2))

MMECode ::= OCTET STRING (SIZE(1))

TMSI ::= OCTET STRING (SIZE(4))

-- ===================

-- EPS MME definitions

-- ===================

MMEAttach ::= SEQUENCE

{

 attachType [1] EPSAttachType,

 attachResult [2] EPSAttachResult,

 iMSI [3] IMSI,

 iMEI [4] IMEI OPTIONAL,

 mSISDN [5] MSISDN OPTIONAL,

 gUTI [6] GUTI OPTIONAL,

 location [7] Location OPTIONAL,

 ePSTAIList [8] TAIList OPTIONAL,

 sMSServiceStatus [9] EPSSMSServiceStatus OPTIONAL,

 oldGUTI [10] GUTI OPTIONAL,

 eMM5GRegStatus [11] EMM5GMMStatus OPTIONAL

}

MMEDetach ::= SEQUENCE

{

 detachDirection [1] MMEDirection,

 detachType [2] EPSDetachType,

 iMSI [3] IMSI,

 iMEI [4] IMEI OPTIONAL,

 mSISDN [5] MSISDN OPTIONAL,

 gUTI [6] GUTI OPTIONAL,

 cause [7] EMMCause OPTIONAL,

 location [8] Location OPTIONAL,

 switchOffIndicator [9] SwitchOffIndicator OPTIONAL

}

MMELocationUpdate ::= SEQUENCE

{

 iMSI [1] IMSI,

 iMEI [2] IMEI OPTIONAL,

 mSISDN [3] MSISDN OPTIONAL,

 gUTI [4] GUTI OPTIONAL,

 location [5] Location OPTIONAL,

 oldGUTI [6] GUTI OPTIONAL,

 sMSServiceStatus [7] EPSSMSServiceStatus OPTIONAL

}

MMEStartOfInterceptionWithEPSAttachedUE ::= SEQUENCE

{

 attachType [1] EPSAttachType,

 attachResult [2] EPSAttachResult,

 iMSI [3] IMSI,

 iMEI [4] IMEI OPTIONAL,

 mSISDN [5] MSISDN OPTIONAL,

 gUTI [6] GUTI OPTIONAL,

 location [7] Location OPTIONAL,

 timeOfRegistration [8] Timestamp OPTIONAL,

 ePSTAIList [9] TAIList OPTIONAL,

 sMSServiceStatus [10] EPSSMSServiceStatus OPTIONAL,

 oldGUTI [11] GUTI OPTIONAL,

 eMM5GRegStatus [12] EMM5GMMStatus OPTIONAL

}

MMEUnsuccessfulProcedure ::= SEQUENCE

{

 failedProcedureType [1] MMEFailedProcedureType,

 failureCause [2] MMEFailureCause,

 iMSI [3] IMSI OPTIONAL,

 iMEI [4] IMEI OPTIONAL,

 mSISDN [5] MSISDN OPTIONAL,

 gUTI [6] GUTI OPTIONAL,

 location [7] Location OPTIONAL

}

-- ==================

-- EPS MME parameters

-- ==================

EMMCause ::= INTEGER (0..255)

ESMCause ::= INTEGER (0..255)

EPSAttachType ::= ENUMERATED

{

 ePSAttach(1),

 combinedEPSIMSIAttach(2),

 ePSRLOSAttach(3),

 ePSEmergencyAttach(4),

 reserved(5)

}

EPSAttachResult ::= ENUMERATED

{

 ePSOnly(1),

 combinedEPSIMSI(2)

}

EPSDetachType ::= ENUMERATED

{

 ePSDetach(1),

 iMSIDetach(2),

 combinedEPSIMSIDetach(3),

 reAttachRequired(4),

 reAttachNotRequired(5),

 reserved(6)

}

EPSSMSServiceStatus ::= ENUMERATED

{

 sMSServicesNotAvailable(1),

 sMSServicesNotAvailableInThisPLMN(2),

 networkFailure(3),

 congestion(4)

}

MMEDirection ::= ENUMERATED

{

 networkInitiated(1),

 uEInitiated(2)

}

MMEFailedProcedureType ::= ENUMERATED

{

 attachReject(1),

 authenticationReject(2),

 securityModeReject(3),

 serviceReject(4),

 trackingAreaUpdateReject(5),

 activateDedicatedEPSBearerContextReject(6),

 activateDefaultEPSBearerContextReject(7),

 bearerResourceAllocationReject(8),

 bearerResourceModificationReject(9),

 modifyEPSBearerContectReject(10),

 pDNConnectivityReject(11),

 pDNDisconnectReject(12)

}

MMEFailureCause ::= CHOICE

{

 eMMCause [1] EMMCause,

 eSMCause [2] ESMCause

}

-- ===========================

-- LI Notification definitions

-- ===========================

LINotification ::= SEQUENCE

{

 notificationType [1] LINotificationType,

 appliedTargetID [2] TargetIdentifier OPTIONAL,

 appliedDeliveryInformation [3] SEQUENCE OF LIAppliedDeliveryInformation OPTIONAL,

 appliedStartTime [4] Timestamp OPTIONAL,

 appliedEndTime [5] Timestamp OPTIONAL

}

-- ==========================

-- LI Notification parameters

-- ==========================

LINotificationType ::= ENUMERATED

{

 activation(1),

 deactivation(2),

 modification(3)

}

LIAppliedDeliveryInformation ::= SEQUENCE

{

 hI2DeliveryIPAddress [1] IPAddress OPTIONAL,

 hI2DeliveryPortNumber [2] PortNumber OPTIONAL,

 hI3DeliveryIPAddress [3] IPAddress OPTIONAL,

 hI3DeliveryPortNumber [4] PortNumber OPTIONAL

}

-- ===============

-- MDF definitions

-- ===============

MDFCellSiteReport ::= SEQUENCE OF CellInformation

-- =================

-- Common Parameters

-- =================

AccessType ::= ENUMERATED

{

 threeGPPAccess(1),

 nonThreeGPPAccess(2),

 threeGPPandNonThreeGPPAccess(3)

}

Direction ::= ENUMERATED

{

 fromTarget(1),

 toTarget(2)

}

DNN ::= UTF8String

E164Number ::= NumericString (SIZE(1..15))

EmailAddress ::= UTF8String

FiveGGUTI ::= SEQUENCE

{

 mCC [1] MCC,

 mNC [2] MNC,

 aMFRegionID [3] AMFRegionID,

 aMFSetID [4] AMFSetID,

 aMFPointer [5] AMFPointer,

 fiveGTMSI [6] FiveGTMSI

}

FiveGMMCause ::= INTEGER (0..255)

FiveGSMRequestType ::= ENUMERATED

{

 initialRequest(1),

 existingPDUSession(2),

 initialEmergencyRequest(3),

 existingEmergencyPDUSession(4),

 modificationRequest(5),

 reserved(6),

 mAPDURequest(7)

}

FiveGSMCause ::= INTEGER (0..255)

FiveGTMSI ::= INTEGER (0..4294967295)

FTEID ::= SEQUENCE

{

 tEID [1] INTEGER (0.. 4294967295),

 iPv4Address [2] IPv4Address OPTIONAL,

 iPv6Address [3] IPv6Address OPTIONAL

}

GPSI ::= CHOICE

{

 mSISDN [1] MSISDN,

 nAI [2] NAI

}

GUAMI ::= SEQUENCE

{

 aMFID [1] AMFID,

 pLMNID [2] PLMNID

}

GUMMEI ::= SEQUENCE

{

 mMEID [1] MMEID,

 mCC [2] MCC,

 mNC [3] MNC

}

HomeNetworkPublicKeyID ::= OCTET STRING

HSMFURI ::= UTF8String

IMEI ::= NumericString (SIZE(14))

IMEISV ::= NumericString (SIZE(16))

IMPI ::= NAI

IMPU ::= CHOICE

{

 sIPURI [1] SIPURI,

 tELURI [2] TELURI

}

IMSI ::= NumericString (SIZE(6..15))

Initiator ::= ENUMERATED

{

 uE(1),

 network(2),

 unknown(3)

}

IPAddress ::= CHOICE

{

 iPv4Address [1] IPv4Address,

 iPv6Address [2] IPv6Address

}

IPv4Address ::= OCTET STRING (SIZE(4))

IPv6Address ::= OCTET STRING (SIZE(16))

IPv6FlowLabel ::= INTEGER(0..1048575)

MACAddress ::= OCTET STRING (SIZE(6))

MCC ::= NumericString (SIZE(3))

MNC ::= NumericString (SIZE(2..3))

MMEID ::= SEQUENCE

{

 mMEGI [1] MMEGI,

 mMEC [2] MMEC

}

MMEC ::= NumericString

MMEGI ::= NumericString

MSISDN ::= NumericString (SIZE(1..15))

NAI ::= UTF8String

NextLayerProtocol ::= INTEGER(0..255)

NonLocalID ::= ENUMERATED

{

 local(1),

 nonLocal(2)

}

NSSAI ::= SEQUENCE OF SNSSAI

PLMNID ::= SEQUENCE

{

 mCC [1] MCC,

 mNC [2] MNC

}

PDUSessionID ::= INTEGER (0..255)

PDUSessionType ::= ENUMERATED

{

 iPv4(1),

 iPv6(2),

 iPv4v6(3),

 unstructured(4),

 ethernet(5)

}

PEI ::= CHOICE

{

 iMEI [1] IMEI,

 iMEISV [2] IMEISV

}

PortNumber ::= INTEGER(0..65535)

ProtectionSchemeID ::= INTEGER (0..15)

RATType ::= ENUMERATED

{

 nR(1),

 eUTRA(2),

 wLAN(3),

 virtual(4),

 nBIOT(5),

 wireline(6),

 wirelineCable(7),

 wirelineBBF(8),

 lTEM(9),

 nRU(10),

 eUTRAU(11),

 trustedN3GA(12),

 trustedWLAN(13),

 uTRA(14),

 gERA(15)

}

RejectedNSSAI ::= SEQUENCE OF RejectedSNSSAI

RejectedSNSSAI ::= SEQUENCE

{

 causeValue [1] RejectedSliceCauseValue,

 sNSSAI [2] SNSSAI

}

RejectedSliceCauseValue ::= INTEGER (0..255)

RoutingIndicator ::= INTEGER (0..9999)

SchemeOutput ::= OCTET STRING

SIPURI ::= UTF8String

Slice ::= SEQUENCE

{

 allowedNSSAI [1] NSSAI OPTIONAL,

 configuredNSSAI [2] NSSAI OPTIONAL,

 rejectedNSSAI [3] RejectedNSSAI OPTIONAL

}

SMPDUDNRequest ::= OCTET STRING

SNSSAI ::= SEQUENCE

{

 sliceServiceType [1] INTEGER (0..255),

 sliceDifferentiator [2] OCTET STRING (SIZE(3)) OPTIONAL

}

SUCI ::= SEQUENCE

{

 mCC [1] MCC,

 mNC [2] MNC,

 routingIndicator [3] RoutingIndicator,

 protectionSchemeID [4] ProtectionSchemeID,

 homeNetworkPublicKeyID [5] HomeNetworkPublicKeyID,

 schemeOutput [6] SchemeOutput

}

SUPI ::= CHOICE

{

 iMSI [1] IMSI,

 nAI [2] NAI

}

SUPIUnauthenticatedIndication ::= BOOLEAN

TargetIdentifier ::= CHOICE

{

 sUPI [1] SUPI,

 iMSI [2] IMSI,

 pEI [3] PEI,

 iMEI [4] IMEI,

 gPSI [5] GPSI,

 mSISDN [6] MSISDN,

 nAI [7] NAI,

 iPv4Address [8] IPv4Address,

 iPv6Address [9] IPv6Address,

 ethernetAddress [10] MACAddress

}

TargetIdentifierProvenance ::= ENUMERATED

{

 lEAProvided(1),

 observed(2),

 matchedOn(3),

 other(4)

}

TELURI ::= UTF8String

Timestamp ::= GeneralizedTime

UEEndpointAddress ::= CHOICE

{

 iPv4Address [1] IPv4Address,

 iPv6Address [2] IPv6Address,

 ethernetAddress [3] MACAddress

}

-- ===================

-- Location parameters

-- ===================

Location ::= SEQUENCE

{

 locationInfo [1] LocationInfo OPTIONAL,

 positioningInfo [2] PositioningInfo OPTIONAL,

 locationPresenceReport [3] LocationPresenceReport OPTIONAL,

 ePSLocationInfo [4] EPSLocationInfo OPTIONAL

}

CellSiteInformation ::= SEQUENCE

{

 geographicalCoordinates [1] GeographicalCoordinates,

 azimuth [2] INTEGER (0..359) OPTIONAL,

 operatorSpecificInformation [3] UTF8String OPTIONAL

}

-- TS 29.518 [22], clause 6.4.6.2.6

LocationInfo ::= SEQUENCE

{

 userLocation [1] UserLocation OPTIONAL,

 currentLoc [2] BOOLEAN OPTIONAL,

 geoInfo [3] GeographicArea OPTIONAL,

 rATType [4] RATType OPTIONAL,

 timeZone [5] TimeZone OPTIONAL,

 additionalCellIDs [6] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.7

UserLocation ::= SEQUENCE

{

 eUTRALocation [1] EUTRALocation OPTIONAL,

 nRLocation [2] NRLocation OPTIONAL,

 n3GALocation [3] N3GALocation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.8

EUTRALocation ::= SEQUENCE

{

 tAI [1] TAI,

 eCGI [2] ECGI,

 ageOfLocatonInfo [3] INTEGER OPTIONAL,

 uELocationTimestamp [4] Timestamp OPTIONAL,

 geographicalInformation [5] UTF8String OPTIONAL,

 geodeticInformation [6] UTF8String OPTIONAL,

 globalNGENbID [7] GlobalRANNodeID OPTIONAL,

 cellSiteInformation [8] CellSiteInformation OPTIONAL,

 globalENbID [9] GlobalRANNodeID OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.9

NRLocation ::= SEQUENCE

{

 tAI [1] TAI,

 nCGI [2] NCGI,

 ageOfLocatonInfo [3] INTEGER OPTIONAL,

 uELocationTimestamp [4] Timestamp OPTIONAL,

 geographicalInformation [5] UTF8String OPTIONAL,

 geodeticInformation [6] UTF8String OPTIONAL,

 globalGNbID [7] GlobalRANNodeID OPTIONAL,

 cellSiteInformation [8] CellSiteInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.10

N3GALocation ::= SEQUENCE

{

 tAI [1] TAI OPTIONAL,

 n3IWFID [2] N3IWFIDNGAP OPTIONAL,

 uEIPAddr [3] IPAddr OPTIONAL,

 portNumber [4] INTEGER OPTIONAL

}

-- TS 38.413 [23], clause 9.3.2.4

IPAddr ::= SEQUENCE

{

 iPv4Addr [1] IPv4Address OPTIONAL,

 iPv6Addr [2] IPv6Address OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.28

GlobalRANNodeID ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 aNNodeID [2] ANNodeID,

 nID [3] NID OPTIONAL

}

ANNodeID ::= CHOICE

{

 n3IWFID [1] N3IWFIDSBI,

 gNbID [2] GNbID,

 nGENbID [3] NGENbID,

 eNbID [4] ENbID

}

-- TS 38.413 [23], clause 9.3.1.6

GNbID ::= BIT STRING(SIZE(22..32))

-- TS 29.571 [17], clause 5.4.4.4

TAI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 tAC [2] TAC,

 nID [3] NID OPTIONAL

}

CGI ::= SEQUENCE

{

 lAI [1] LAI,

 cellID [2] CellID

}

LAI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 lAC [2] LAC

}

LAC ::= OCTET STRING (SIZE(2))

CellID ::= OCTET STRING (SIZE(2))

SAI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 lAC [2] LAC,

 sAC [3] SAC

}

SAC ::= OCTET STRING (SIZE(2))

-- TS 29.571 [17], clause 5.4.4.5

ECGI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 eUTRACellID [2] EUTRACellID,

 nID [3] NID OPTIONAL

}

TAIList ::= SEQUENCE OF TAI

-- TS 29.571 [17], clause 5.4.4.6

NCGI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 nRCellID [2] NRCellID,

 nID [3] NID OPTIONAL

}

RANCGI ::= CHOICE

{

 eCGI [1] ECGI,

 nCGI [2] NCGI

}

CellInformation ::= SEQUENCE

{

 rANCGI [1] RANCGI,

 cellSiteinformation [2] CellSiteInformation OPTIONAL,

 timeOfLocation [3] Timestamp OPTIONAL

}

-- TS 38.413 [23], clause 9.3.1.57

N3IWFIDNGAP ::= BIT STRING (SIZE(16))

-- TS 29.571 [17], clause 5.4.4.28

N3IWFIDSBI ::= UTF8String

-- TS 29.571 [17], table 5.4.2-1

TAC ::= OCTET STRING (SIZE(2..3))

-- TS 38.413 [23], clause 9.3.1.9

EUTRACellID ::= BIT STRING (SIZE(28))

-- TS 38.413 [23], clause 9.3.1.7

NRCellID ::= BIT STRING (SIZE(36))

-- TS 38.413 [23], clause 9.3.1.8

NGENbID ::= CHOICE

{

 macroNGENbID [1] BIT STRING (SIZE(20)),

 shortMacroNGENbID [2] BIT STRING (SIZE(18)),

 longMacroNGENbID [3] BIT STRING (SIZE(21))

}

-- TS 23.003 [19], clause 12.7.1 encoded as per TS 29.571 [17], clause 5.4.2

NID ::= UTF8String (SIZE(11))

-- TS 36.413 [38], clause 9.2.1.37

ENbID ::= CHOICE

{

 macroENbID [1] BIT STRING (SIZE(20)),

 homeENbID [2] BIT STRING (SIZE(28)),

 shortMacroENbID [3] BIT STRING (SIZE(18)),

 longMacroENbID [4] BIT STRING (SIZE(21))

}

-- TS 29.518 [22], clause 6.4.6.2.3

PositioningInfo ::= SEQUENCE

{

 positionInfo [1] LocationData OPTIONAL,

 rawMLPResponse [2] RawMLPResponse OPTIONAL

}

RawMLPResponse ::= CHOICE

{

 -- The following parameter contains a copy of unparsed XML code of the

 -- MLP response message, i.e. the entire XML document containing

 -- a <slia> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.2) or

 -- a <slirep> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.3) MLP message.

 mLPPositionData [1] UTF8String,

 -- OMA MLP result id, defined in OMA-TS-MLP-V3\_5-20181211-C [20], Clause 5.4

 mLPErrorCode [2] INTEGER (1..699)

}

-- TS 29.572 [24], clause 6.1.6.2.3

LocationData ::= SEQUENCE

{

 locationEstimate [1] GeographicArea,

 accuracyFulfilmentIndicator [2] AccuracyFulfilmentIndicator OPTIONAL,

 ageOfLocationEstimate [3] AgeOfLocationEstimate OPTIONAL,

 velocityEstimate [4] VelocityEstimate OPTIONAL,

 civicAddress [5] CivicAddress OPTIONAL,

 positioningDataList [6] SET OF PositioningMethodAndUsage OPTIONAL,

 gNSSPositioningDataList [7] SET OF GNSSPositioningMethodAndUsage OPTIONAL,

 eCGI [8] ECGI OPTIONAL,

 nCGI [9] NCGI OPTIONAL,

 altitude [10] Altitude OPTIONAL,

 barometricPressure [11] BarometricPressure OPTIONAL

}

-- TS 29.172 [Re5], table 6.2.2-2

EPSLocationInfo ::= SEQUENCE

{

 locationData [1] LocationData,

 cGI [2] CGI OPTIONAL,

 sAI [3] SAI OPTIONAL,

 eSMLCCellInfo [4] ESMLCCellInfo OPTIONAL

}

-- TS 29.172 [Re5], clause 7.4.57

ESMLCCellInfo ::= SEQUENCE

{

 eCGI [1] ECGI,

 cellPortionID [2] CellPortionID

}

-- TS 29.171 [Re6], clause 7.4.31

CellPortionID ::= INTEGER (0..4095)

-- TS 29.518 [22], clause 6.2.6.2.5

LocationPresenceReport ::= SEQUENCE

{

 type [1] AMFEventType,

 timestamp [2] Timestamp,

 areaList [3] SET OF AMFEventArea OPTIONAL,

 timeZone [4] TimeZone OPTIONAL,

 accessTypes [5] SET OF AccessType OPTIONAL,

 rMInfoList [6] SET OF RMInfo OPTIONAL,

 cMInfoList [7] SET OF CMInfo OPTIONAL,

 reachability [8] UEReachability OPTIONAL,

 location [9] UserLocation OPTIONAL,

 additionalCellIDs [10] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.3.3

AMFEventType ::= ENUMERATED

{

 locationReport(1),

 presenceInAOIReport(2)

}

-- TS 29.518 [22], clause 6.2.6.2.16

AMFEventArea ::= SEQUENCE

{

 presenceInfo [1] PresenceInfo OPTIONAL,

 lADNInfo [2] LADNInfo OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.27

PresenceInfo ::= SEQUENCE

{

 presenceState [1] PresenceState OPTIONAL,

 trackingAreaList [2] SET OF TAI OPTIONAL,

 eCGIList [3] SET OF ECGI OPTIONAL,

 nCGIList [4] SET OF NCGI OPTIONAL,

 globalRANNodeIDList [5] SET OF GlobalRANNodeID OPTIONAL,

 globalENbIDList [6] SET OF GlobalRANNodeID OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.2.17

LADNInfo ::= SEQUENCE

{

 lADN [1] UTF8String,

 presence [2] PresenceState OPTIONAL

}

-- TS 29.571 [17], clause 5.4.3.20

PresenceState ::= ENUMERATED

{

 inArea(1),

 outOfArea(2),

 unknown(3),

 inactive(4)

}

-- TS 29.518 [22], clause 6.2.6.2.8

RMInfo ::= SEQUENCE

{

 rMState [1] RMState,

 accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.2.9

CMInfo ::= SEQUENCE

{

 cMState [1] CMState,

 accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.3.7

UEReachability ::= ENUMERATED

{

 unreachable(1),

 reachable(2),

 regulatoryOnly(3)

}

-- TS 29.518 [22], clause 6.2.6.3.9

RMState ::= ENUMERATED

{

 registered(1),

 deregistered(2)

}

-- TS 29.518 [22], clause 6.2.6.3.10

CMState ::= ENUMERATED

{

 idle(1),

 connected(2)

}

-- TS 29.572 [24], clause 6.1.6.2.5

GeographicArea ::= CHOICE

{

 point [1] Point,

 pointUncertaintyCircle [2] PointUncertaintyCircle,

 pointUncertaintyEllipse [3] PointUncertaintyEllipse,

 polygon [4] Polygon,

 pointAltitude [5] PointAltitude,

 pointAltitudeUncertainty [6] PointAltitudeUncertainty,

 ellipsoidArc [7] EllipsoidArc

}

-- TS 29.572 [24], clause 6.1.6.3.12

AccuracyFulfilmentIndicator ::= ENUMERATED

{

 requestedAccuracyFulfilled(1),

 requestedAccuracyNotFulfilled(2)

}

-- TS 29.572 [24], clause 6.1.6.2.17

VelocityEstimate ::= CHOICE

{

 horVelocity [1] HorizontalVelocity,

 horWithVertVelocity [2] HorizontalWithVerticalVelocity,

 horVelocityWithUncertainty [3] HorizontalVelocityWithUncertainty,

 horWithVertVelocityAndUncertainty [4] HorizontalWithVerticalVelocityAndUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.14

CivicAddress ::= SEQUENCE

{

 country [1] UTF8String,

 a1 [2] UTF8String OPTIONAL,

 a2 [3] UTF8String OPTIONAL,

 a3 [4] UTF8String OPTIONAL,

 a4 [5] UTF8String OPTIONAL,

 a5 [6] UTF8String OPTIONAL,

 a6 [7] UTF8String OPTIONAL,

 prd [8] UTF8String OPTIONAL,

 pod [9] UTF8String OPTIONAL,

 sts [10] UTF8String OPTIONAL,

 hno [11] UTF8String OPTIONAL,

 hns [12] UTF8String OPTIONAL,

 lmk [13] UTF8String OPTIONAL,

 loc [14] UTF8String OPTIONAL,

 nam [15] UTF8String OPTIONAL,

 pc [16] UTF8String OPTIONAL,

 bld [17] UTF8String OPTIONAL,

 unit [18] UTF8String OPTIONAL,

 flr [19] UTF8String OPTIONAL,

 room [20] UTF8String OPTIONAL,

 plc [21] UTF8String OPTIONAL,

 pcn [22] UTF8String OPTIONAL,

 pobox [23] UTF8String OPTIONAL,

 addcode [24] UTF8String OPTIONAL,

 seat [25] UTF8String OPTIONAL,

 rd [26] UTF8String OPTIONAL,

 rdsec [27] UTF8String OPTIONAL,

 rdbr [28] UTF8String OPTIONAL,

 rdsubbr [29] UTF8String OPTIONAL,

 prm [30] UTF8String OPTIONAL,

 pom [31] UTF8String OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.15

PositioningMethodAndUsage ::= SEQUENCE

{

 method [1] PositioningMethod,

 mode [2] PositioningMode,

 usage [3] Usage,

 methodCode [4] MethodCode OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.16

GNSSPositioningMethodAndUsage ::= SEQUENCE

{

 mode [1] PositioningMode,

 gNSS [2] GNSSID,

 usage [3] Usage

}

-- TS 29.572 [24], clause 6.1.6.2.6

Point ::= SEQUENCE

{

 geographicalCoordinates [1] GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.7

PointUncertaintyCircle ::= SEQUENCE

{

 geographicalCoordinates [1] GeographicalCoordinates,

 uncertainty [2] Uncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.8

PointUncertaintyEllipse ::= SEQUENCE

{

 geographicalCoordinates [1] GeographicalCoordinates,

 uncertainty [2] UncertaintyEllipse,

 confidence [3] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.9

Polygon ::= SEQUENCE

{

 pointList [1] SET SIZE (3..15) OF GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.10

PointAltitude ::= SEQUENCE

{

 point [1] GeographicalCoordinates,

 altitude [2] Altitude

}

-- TS 29.572 [24], clause 6.1.6.2.11

PointAltitudeUncertainty ::= SEQUENCE

{

 point [1] GeographicalCoordinates,

 altitude [2] Altitude,

 uncertaintyEllipse [3] UncertaintyEllipse,

 uncertaintyAltitude [4] Uncertainty,

 confidence [5] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.12

EllipsoidArc ::= SEQUENCE

{

 point [1] GeographicalCoordinates,

 innerRadius [2] InnerRadius,

 uncertaintyRadius [3] Uncertainty,

 offsetAngle [4] Angle,

 includedAngle [5] Angle,

 confidence [6] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.4

GeographicalCoordinates ::= SEQUENCE

{

 latitude [1] UTF8String,

 longitude [2] UTF8String,

 mapDatumInformation [3] OGCURN OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.22

UncertaintyEllipse ::= SEQUENCE

{

 semiMajor [1] Uncertainty,

 semiMinor [2] Uncertainty,

 orientationMajor [3] Orientation

}

-- TS 29.572 [24], clause 6.1.6.2.18

HorizontalVelocity ::= SEQUENCE

{

 hSpeed [1] HorizontalSpeed,

 bearing [2] Angle

}

-- TS 29.572 [24], clause 6.1.6.2.19

HorizontalWithVerticalVelocity ::= SEQUENCE

{

 hSpeed [1] HorizontalSpeed,

 bearing [2] Angle,

 vSpeed [3] VerticalSpeed,

 vDirection [4] VerticalDirection

}

-- TS 29.572 [24], clause 6.1.6.2.20

HorizontalVelocityWithUncertainty ::= SEQUENCE

{

 hSpeed [1] HorizontalSpeed,

 bearing [2] Angle,

 uncertainty [3] SpeedUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.21

HorizontalWithVerticalVelocityAndUncertainty ::= SEQUENCE

{

 hspeed [1] HorizontalSpeed,

 bearing [2] Angle,

 vSpeed [3] VerticalSpeed,

 vDirection [4] VerticalDirection,

 hUncertainty [5] SpeedUncertainty,

 vUncertainty [6] SpeedUncertainty

}

-- The following types are described in TS 29.572 [24], table 6.1.6.3.2-1

Altitude ::= UTF8String

Angle ::= INTEGER (0..360)

Uncertainty ::= INTEGER (0..127)

Orientation ::= INTEGER (0..180)

Confidence ::= INTEGER (0..100)

InnerRadius ::= INTEGER (0..65535)

AgeOfLocationEstimate ::= INTEGER (0..32767)

HorizontalSpeed ::= UTF8String

VerticalSpeed ::= UTF8String

SpeedUncertainty ::= UTF8String

BarometricPressure ::= INTEGER (30000..155000)

-- TS 29.572 [24], clause 6.1.6.3.13

VerticalDirection ::= ENUMERATED

{

 upward(1),

 downward(2)

}

-- TS 29.572 [24], clause 6.1.6.3.6

PositioningMethod ::= ENUMERATED

{

 cellID(1),

 eCID(2),

 oTDOA(3),

 barometricPressure(4),

 wLAN(5),

 bluetooth(6),

 mBS(7),

 motionSensor(8),

 dLTDOA(9),

 dLAOD(10),

 multiRTT(11),

 nRECID(12),

 uLTDOA(13),

 uLAOA(14),

 networkSpecific(15)

}

-- TS 29.572 [24], clause 6.1.6.3.7

PositioningMode ::= ENUMERATED

{

 uEBased(1),

 uEAssisted(2),

 conventional(3)

}

-- TS 29.572 [24], clause 6.1.6.3.8

GNSSID ::= ENUMERATED

{

 gPS(1),

 galileo(2),

 sBAS(3),

 modernizedGPS(4),

 qZSS(5),

 gLONASS(6),

 bDS(7),

 nAVIC(8)

}

-- TS 29.572 [24], clause 6.1.6.3.9

Usage ::= ENUMERATED

{

 unsuccess(1),

 successResultsNotUsed(2),

 successResultsUsedToVerifyLocation(3),

 successResultsUsedToGenerateLocation(4),

 successMethodNotDetermined(5)

}

-- TS 29.571 [17], table 5.2.2-1

TimeZone ::= UTF8String

-- Open Geospatial Consortium URN [35]

OGCURN ::= UTF8String

-- TS 29.572 [24], clause 6.1.6.2.15

MethodCode ::= INTEGER (16..31)

END

\*\*\* End of All Changes \*\*\*