**3GPP TSG-SA3 Meeting #83-LI-e-b *s3i210804r1***

**Online, , 1st Nov 2021 - 5th Nov 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **33.128** | **CR** | **0262** | **rev** | **1** | **Current version:** | **16.8.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarification to default behaviour for ServiceScoping at the MDF | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | SA3-LI(OTD, NTAC, Ministère Economie et Finances, Nokia, Nokia Shanghai Bell) | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | LI16 | | | | |  | ***Date:*** | | | 2021-11-02 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | There is no default behaviour defined for the MDF when ServiceScoping is not sent or when ServiceScoping is sent, but there are no ServiceTypes defined. This CR adds a default behaviour. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Specifies default behaviour when MDF is not provisioned with ServiceScoping details. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The default behaviour of the MDF will remain ambiguous. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.4.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR … CR … | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | S3i210805 is the Release 17 mirror of this CR. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | S3i210804 | | | | | | | | |

### 4.4.2 CSP service type

srequirements of the warrant with the following :

- Voice.

- Data.

- Messaging (e.g. SMS/MMS).

- Push-to-Talk (including MCPTT).

- LALS (the Target Positioning service, per TS 33.127 [5], clause 7.3.3.2).

When multiple service types are applicable to a target due to multiple warrants, the MDF2/MDF3 shall be able to deliver interception product to each LEMF based on the CSP service type(s) of the respective warrant.

When no service type is provisioned, the MDF2/MDF3 shall deliver all interception product it receives from the POIs.