**3GPP TSG-SA3 Meeting #83-LI-e-b *s3i210819***

**Online, , 1st Nov 2021 - 5th Nov 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **33.128** | **CR** | **0273** | **rev** | **1** | **Current version:** | **17.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | SA3-LI (OTD) | | | | | | | | | |
| ***Source to TSG:*** | SA3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | LI17 | | | | |  | ***Date:*** | | | 2021-11-04 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Currently, TS 33.127 has a defined separated location reporting capability that has not yet been defined in TS 33.128. This CR aligns stage 2 and stage 3 while providing a capaiblity to report location independly from other message types from the IRI-POIs. This CR also adds the missing age of location information and locationtimestamp to N3GALocation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | This contrtibution modifies clause 6.2.3.2.1 to add trigger for SeparatedLocationReporting at the SMF, modifies clause 7.7.2.1.1 to add trigger for SeparatedLocationReporting at the NEF, adds a new clause, 7.3.X for Separated Location Reporting, adds a table in 7.3.X.1, and modifes the ASN.1 for the new message and additional reporting capabilties for N3GALocation information. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Stage 2 and Stage 3 alignment. CSPs may not be able to fully meet LI obligations. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.3.X, Annex A ASN.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | s3i210819 | | | | | | | | |

\*\*\*START OF CHANGES\*\*\*

\*\*\*START OF FIRST CHANGE\*\*\*

#### 6.2.3.2 Generation of xIRI at IRI-POI in SMF over LI\_X2

##### 6.2.3.2.1 General

The IRI-POI present in the SMF shall send the xIRIs over LI\_X2 for each of the events listed in TS 33.127 [5] clause 6.2.3.3, the details of which are described in the following clauses. The IRI-POI present in the SMF shall also send a SeparatedLocationReporting xIRI (as described in clause 7.3.X.1 of the present document) when the IRI-POI provisioned in the H-SMF detects that the V-SMF has sent location data via the HsmfUpdateData service operation to the H-SMF that does not otherwise trigger an existing SMF record type.

\*\*\*END OF FIRST CHANGE\*\*\*

\*\*\*START OF SECOND CHANGE\*\*\*

### 7.7.2 LI for NIDD using NEF

#### 7.7.2.1 Generation of xIRI at IRI-POI in NEF over LI\_X2

##### 7.7.2.1.1 General

The IRI-POI present in the NEF shall send the xIRIs over LI\_X2 for each of the events listed in TS 33.127 [5] clause 7.7.2.3, the details of which are described in the following clauses. Each event will be based on PDU session between NEF and target UE, except for Unsuccessful Procedure event. The IRI-POI in the NEF shall also send a SeparatedLocationReporting xIRI (as described in clause 7.3.X.1 of the present document) when the IRI-POI provisioned in the NEF receives updated UE location information via the Nnef\_Location\_LocationUpdateNotify service operation destined for an external AF.

\*\*\*END OF SECOND CHANGE\*\*\*

\*\*\*START OF THIRD CHANGE\*\*\*

### 7.3.X Separated location reporting

#### 7.3.X.1 General description

When location information cannot be reported via an existing message generation at the IRI-POI, a separate xIRI may be generated from any provisioned IRI-POI that has access to location information and included in the SeparatedLocationReporting record.

The following information needs to be transferred from the IRI-POI to the MDF2 in order to enable a MDF2 to perform its functionality:

- Target identity.

- Event date/time.

- Target location(s).

- Date/time of UE location(s).

- Nature and identity of the POI.

- Location source(s).

Details of how the IRI-POI in the SMF generates this record can be found in clause 6.2.3.2.1 of the present document.

Details of how the IRI-POI in the NEF generates this record can be found in clause 7.7.2.1.1 of the present document.

Table 7.3.X-1: Payload for SeparatedLocationReporting record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI associated with the registration (see clause 6.2.2.4). | M |
| sUCI | SUCI used in the registration, if available. | C |
| pEI | PEI provided by the UE during the registration, if available. | C |
| gPSI | GPSI obtained in the registration, if available as part of the subscription profile. | C |
| gUTI | 5G-GUTI provided as outcome of initial registration or used in other cases, see TS 24.501 [13] clause 5.5.1.2.2. | C |
| location | Location information determined by the network at the time of message generation. | M |
| non3GPPAccessEndpoint | For Non-3GPP access, UE's local IP address used to reach the N3IWF, TNGF or TWIF. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). | C |
| fiveGSTAIList | List of tracking areas associated with the location update registration area within which the UE is currently registered, see TS 24.501 [13], clause 9.11.3.9. List shall be included each time there is a change to the registration area. | C |
| rATType | RAT Type associated with the data for which location information is provided, see TS 23.502 [4] clause 4.3.2. Values given as per TS 29.571 [17] clause 5.4.3.2. | C |

\*\*\*END OF THIRD CHANGE\*\*\*

\*\*\*START OF FOURTH CHANGE\*\*\*

Annex A (normative):  
ASN.1 Schema for the Internal and External Interfaces

TS33128Payloads

{itu-t(0) identified-organization(4) etsi(0) securityDomain(2) lawfulIntercept(2) threeGPP(4) ts33128(19) r17(17) version1(1)}

DEFINITIONS IMPLICIT TAGS EXTENSIBILITY IMPLIED ::=

BEGIN

-- =============

-- Relative OIDs

-- =============

tS33128PayloadsOID RELATIVE-OID ::= {threeGPP(4) ts33128(19) r17(17) version1(1)}

xIRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xIRI(1)}

xCCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xCC(2)}

iRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID iRI(3)}

cCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID cC(4)}

lINotificationPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID lINotification(5)}

-- ===============

-- X2 xIRI payload

-- ===============

XIRIPayload ::= SEQUENCE

{

xIRIPayloadOID [1] RELATIVE-OID,

event [2] XIRIEvent

}

XIRIEvent ::= CHOICE

{

-- Access and mobility related events, see clause 6.2.2

registration [1] AMFRegistration,

deregistration [2] AMFDeregistration,

locationUpdate [3] AMFLocationUpdate,

startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

unsuccessfulAMProcedure [5] AMFUnsuccessfulProcedure,

-- PDU session-related events, see clause 6.2.3

pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

pDUSessionModification [7] SMFPDUSessionModification,

pDUSessionRelease [8] SMFPDUSessionRelease,

startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

unsuccessfulSMProcedure [10] SMFUnsuccessfulProcedure,

-- Subscriber-management related events, see clause 7.2.2

servingSystemMessage [11] UDMServingSystemMessage,

-- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

sMSMessage [12] SMSMessage,

-- LALS-related events, see clause 7.3.3

lALSReport [13] LALSReport,

-- PDHR/PDSR-related events, see clause 6.2.3.4.1

pDHeaderReport [14] PDHeaderReport,

pDSummaryReport [15] PDSummaryReport,

-- tag 16 is reserved because there is no equivalent mDFCellSiteReport in XIRIEvent

-- MMS-related events, see clause 7.4.2

mMSSend [17] MMSSend,

mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

mMSNotification [19] MMSNotification,

mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

mMSNotificationResponse [21] MMSNotificationResponse,

mMSRetrieval [22] MMSRetrieval,

mMSDeliveryAck [23] MMSDeliveryAck,

mMSForward [24] MMSForward,

mMSDeleteFromRelay [25] MMSDeleteFromRelay,

mMSDeliveryReport [26] MMSDeliveryReport,

mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

mMSReadReport [28] MMSReadReport,

mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

mMSCancel [30] MMSCancel,

mMSMBoxStore [31] MMSMBoxStore,

mMSMBoxUpload [32] MMSMBoxUpload,

mMSMBoxDelete [33] MMSMBoxDelete,

mMSMBoxViewRequest [34] MMSMBoxViewRequest,

mMSMBoxViewResponse [35] MMSMBoxViewResponse,

-- PTC-related events, see clause 7.5.2

pTCRegistration [36] PTCRegistration,

pTCSessionInitiation [37] PTCSessionInitiation,

pTCSessionAbandon [38] PTCSessionAbandon,

pTCSessionStart [39] PTCSessionStart,

pTCSessionEnd [40] PTCSessionEnd,

pTCStartOfInterception [41] PTCStartOfInterception,

pTCPreEstablishedSession [42] PTCPreEstablishedSession,

pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

pTCPartyJoin [44] PTCPartyJoin,

pTCPartyDrop [45] PTCPartyDrop,

pTCPartyHold [46] PTCPartyHold,

pTCMediaModification [47] PTCMediaModification,

pTCGroupAdvertisement [48] PTCGroupAdvertisement,

pTCFloorControl [49] PTCFloorControl,

pTCTargetPresence [50] PTCTargetPresence,

pTCParticipantPresence [51] PTCParticipantPresence,

pTCListManagement [52] PTCListManagement,

pTCAccessPolicy [53] PTCAccessPolicy,

-- More Subscriber-management related events, see clause 7.2.2

subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

cancelLocationMessage [55] UDMCancelLocationMessage,

-- SMS-related events continued from choice 12

sMSReport [56] SMSReport,

-- MA PDU session-related events, see clause 6.2.3.2.7

sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

-- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

aMFIdentifierAssociation [62] AMFIdentifierAssociation,

mMEIdentifierAssociation [63] MMEIdentifierAssociation,

-- PDU to MA PDU session-related events, see clause 6.2.3.2.8

sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

-- NEF services related events, see clause 7.7.2

nEFPDUSessionEstablishment [65] NEFPDUSessionEstablishment,

nEFPDUSessionModification [66] NEFPDUSessionModification,

nEFPDUSessionRelease [67] NEFPDUSessionRelease,

nEFUnsuccessfulProcedure [68] NEFUnsuccessfulProcedure,

nEFStartOfInterceptionWithEstablishedPDUSession [69] NEFStartOfInterceptionWithEstablishedPDUSession,

nEFdeviceTrigger [70] NEFDeviceTrigger,

nEFdeviceTriggerReplace [71] NEFDeviceTriggerReplace,

nEFdeviceTriggerCancellation [72] NEFDeviceTriggerCancellation,

nEFdeviceTriggerReportNotify [73] NEFDeviceTriggerReportNotify,

nEFMSISDNLessMOSMS [74] NEFMSISDNLessMOSMS,

nEFExpectedUEBehaviourUpdate [75] NEFExpectedUEBehaviourUpdate,

-- SCEF services related events, see clause 7.8.2

sCEFPDNConnectionEstablishment [76] SCEFPDNConnectionEstablishment,

sCEFPDNConnectionUpdate [77] SCEFPDNConnectionUpdate,

sCEFPDNConnectionRelease [78] SCEFPDNConnectionRelease,

sCEFUnsuccessfulProcedure [79] SCEFUnsuccessfulProcedure,

sCEFStartOfInterceptionWithEstablishedPDNConnection [80] SCEFStartOfInterceptionWithEstablishedPDNConnection,

sCEFdeviceTrigger [81] SCEFDeviceTrigger,

sCEFdeviceTriggerReplace [82] SCEFDeviceTriggerReplace,

sCEFdeviceTriggerCancellation [83] SCEFDeviceTriggerCancellation,

sCEFdeviceTriggerReportNotify [84] SCEFDeviceTriggerReportNotify,

sCEFMSISDNLessMOSMS [85] SCEFMSISDNLessMOSMS,

sCEFCommunicationPatternUpdate [86] SCEFCommunicationPatternUpdate,

-- EPS Events, see clause 6.3

-- MME Events, see clause 6.3.2.2

mMEAttach [87] MMEAttach,

mMEDetach [88] MMEDetach,

mMELocationUpdate [89] MMELocationUpdate,

mMEStartOfInterceptionWithEPSAttachedUE [90] MMEStartOfInterceptionWithEPSAttachedUE,

mMEUnsuccessfulProcedure [91] MMEUnsuccessfulProcedure,

-- AKMA key management events, see clause 7.9.1

aAnFAnchorKeyRegister [92] AAnFAnchorKeyRegister,

aAnFKAKMAApplicationKeyGet [93] AAnFKAKMAApplicationKeyGet,

aAnFStartOfInterceptWithEstablishedAKMAKeyMaterial [94] AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial,

aAnFAKMAContextRemovalRecord [95] AAnFAKMAContextRemovalRecord,

aFAKMAApplicationKeyRefresh [96] AFAKMAApplicationKeyRefresh,

aFStartOfInterceptWithEstablishedAKMAApplicationKey [97] AFStartOfInterceptWithEstablishedAKMAApplicationKey,

aFAuxiliarySecurityParameterEstablishment [98] AFAuxiliarySecurityParameterEstablishment,

aFApplicationKeyRemoval [99] AFApplicationKeyRemoval,

-- HR LI Events, see clause 7.10.3.3

n9HRPDUSessionInfo [100] N9HRPDUSessionInfo,

s8HRBearerInfo [101] S8HRBearerInfo,

-- Separated Location Reporting, see clause 7.3.X

separatedLocationReporting [2731] SeparatedLocationReporting

}

-- ==============

-- X3 xCC payload

-- ==============

-- No additional xCC payload definitions required in the present document.

-- ===============

-- HI2 IRI payload

-- ===============

IRIPayload ::= SEQUENCE

{

iRIPayloadOID [1] RELATIVE-OID,

event [2] IRIEvent,

targetIdentifiers [3] SEQUENCE OF IRITargetIdentifier OPTIONAL

}

IRIEvent ::= CHOICE

{

-- Registration-related events, see clause 6.2.2

registration [1] AMFRegistration,

deregistration [2] AMFDeregistration,

locationUpdate [3] AMFLocationUpdate,

startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

unsuccessfulRegistrationProcedure [5] AMFUnsuccessfulProcedure,

-- PDU session-related events, see clause 6.2.3

pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

pDUSessionModification [7] SMFPDUSessionModification,

pDUSessionRelease [8] SMFPDUSessionRelease,

startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

unsuccessfulSessionProcedure [10] SMFUnsuccessfulProcedure,

-- Subscriber-management related events, see clause 7.2.2

servingSystemMessage [11] UDMServingSystemMessage,

-- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

sMSMessage [12] SMSMessage,

-- LALS-related events, see clause 7.3.3

lALSReport [13] LALSReport,

-- PDHR/PDSR-related events, see clause 6.2.3.4.1

pDHeaderReport [14] PDHeaderReport,

pDSummaryReport [15] PDSummaryReport,

-- MDF-related events, see clause 7.3.4

mDFCellSiteReport [16] MDFCellSiteReport,

-- MMS-related events, see clause 7.4.2

mMSSend [17] MMSSend,

mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

mMSNotification [19] MMSNotification,

mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

mMSNotificationResponse [21] MMSNotificationResponse,

mMSRetrieval [22] MMSRetrieval,

mMSDeliveryAck [23] MMSDeliveryAck,

mMSForward [24] MMSForward,

mMSDeleteFromRelay [25] MMSDeleteFromRelay,

mMSDeliveryReport [26] MMSDeliveryReport,

mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

mMSReadReport [28] MMSReadReport,

mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

mMSCancel [30] MMSCancel,

mMSMBoxStore [31] MMSMBoxStore,

mMSMBoxUpload [32] MMSMBoxUpload,

mMSMBoxDelete [33] MMSMBoxDelete,

mMSMBoxViewRequest [34] MMSMBoxViewRequest,

mMSMBoxViewResponse [35] MMSMBoxViewResponse,

-- PTC-related events, see clause 7.5.2

pTCRegistration [36] PTCRegistration,

pTCSessionInitiation [37] PTCSessionInitiation,

pTCSessionAbandon [38] PTCSessionAbandon,

pTCSessionStart [39] PTCSessionStart,

pTCSessionEnd [40] PTCSessionEnd,

pTCStartOfInterception [41] PTCStartOfInterception,

pTCPreEstablishedSession [42] PTCPreEstablishedSession,

pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

pTCPartyJoin [44] PTCPartyJoin,

pTCPartyDrop [45] PTCPartyDrop,

pTCPartyHold [46] PTCPartyHold,

pTCMediaModification [47] PTCMediaModification,

pTCGroupAdvertisement [48] PTCGroupAdvertisement,

pTCFloorControl [49] PTCFloorControl,

pTCTargetPresence [50] PTCTargetPresence,

pTCParticipantPresence [51] PTCParticipantPresence,

pTCListManagement [52] PTCListManagement,

pTCAccessPolicy [53] PTCAccessPolicy,

-- More Subscriber-management related events, see clause 7.2.2

subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

cancelLocationMessage [55] UDMCancelLocationMessage,

-- SMS-related events, continued from choice 12

sMSReport [56] SMSReport,

-- MA PDU session-related events, see clause 6.2.3.2.7

sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

-- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

aMFIdentifierAssociation [62] AMFIdentifierAssociation,

mMEIdentifierAssociation [63] MMEIdentifierAssociation,

-- PDU to MA PDU session-related events, see clause 6.2.3.2.8

sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

-- NEF services related events, see clause 7.7.2,

nEFPDUSessionEstablishment [65] NEFPDUSessionEstablishment,

nEFPDUSessionModification [66] NEFPDUSessionModification,

nEFPDUSessionRelease [67] NEFPDUSessionRelease,

nEFUnsuccessfulProcedure [68] NEFUnsuccessfulProcedure,

nEFStartOfInterceptionWithEstablishedPDUSession [69] NEFStartOfInterceptionWithEstablishedPDUSession,

nEFdeviceTrigger [70] NEFDeviceTrigger,

nEFdeviceTriggerReplace [71] NEFDeviceTriggerReplace,

nEFdeviceTriggerCancellation [72] NEFDeviceTriggerCancellation,

nEFdeviceTriggerReportNotify [73] NEFDeviceTriggerReportNotify,

nEFMSISDNLessMOSMS [74] NEFMSISDNLessMOSMS,

nEFExpectedUEBehaviourUpdate [75] NEFExpectedUEBehaviourUpdate,

-- SCEF services related events, see clause 7.8.2

sCEFPDNConnectionEstablishment [76] SCEFPDNConnectionEstablishment,

sCEFPDNConnectionUpdate [77] SCEFPDNConnectionUpdate,

sCEFPDNConnectionRelease [78] SCEFPDNConnectionRelease,

sCEFUnsuccessfulProcedure [79] SCEFUnsuccessfulProcedure,

sCEFStartOfInterceptionWithEstablishedPDNConnection [80] SCEFStartOfInterceptionWithEstablishedPDNConnection,

sCEFdeviceTrigger [81] SCEFDeviceTrigger,

sCEFdeviceTriggerReplace [82] SCEFDeviceTriggerReplace,

sCEFdeviceTriggerCancellation [83] SCEFDeviceTriggerCancellation,

sCEFdeviceTriggerReportNotify [84] SCEFDeviceTriggerReportNotify,

sCEFMSISDNLessMOSMS [85] SCEFMSISDNLessMOSMS,

sCEFCommunicationPatternUpdate [86] SCEFCommunicationPatternUpdate,

-- EPS Events, see clause 6.3

-- MME Events, see clause 6.3.2.2

mMEAttach [87] MMEAttach,

mMEDetach [88] MMEDetach,

mMELocationUpdate [89] MMELocationUpdate,

mMEStartOfInterceptionWithEPSAttachedUE [90] MMEStartOfInterceptionWithEPSAttachedUE,

mMEUnsuccessfulProcedure [91] MMEUnsuccessfulProcedure,

-- AKMA key management events, see clause 7.9.1

aAnFAnchorKeyRegister [92] AAnFAnchorKeyRegister,

aAnFKAKMAApplicationKeyGet [93] AAnFKAKMAApplicationKeyGet,

aAnFStartOfInterceptWithEstablishedAKMAKeyMaterial [94] AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial,

aAnFAKMAContextRemovalRecord [95] AAnFAKMAContextRemovalRecord,

aFAKMAApplicationKeyRefresh [96] AFAKMAApplicationKeyRefresh,

aFStartOfInterceptWithEstablishedAKMAApplicationKey [97] AFStartOfInterceptWithEstablishedAKMAApplicationKey,

aFAuxiliarySecurityParameterEstablishment [98] AFAuxiliarySecurityParameterEstablishment,

aFApplicationKeyRemoval [99] AFApplicationKeyRemoval,

-- tag 100 is reserved because there is no equivalent n9HRPDUSessionInfo in IRIEvent.

-- tag 101 is reserved because there is no equivalent S8HRBearerInfo in IRIEvent.

-- Separated Location Reporting, see clause 7.3.X

separatedLocationReporting [2731] SeparatedLocationReporting

}

IRITargetIdentifier ::= SEQUENCE

{

identifier [1] TargetIdentifier,

provenance [2] TargetIdentifierProvenance OPTIONAL

}

-- ==============

-- HI3 CC payload

-- ==============

CCPayload ::= SEQUENCE

{

cCPayloadOID [1] RELATIVE-OID,

pDU [2] CCPDU

}

CCPDU ::= CHOICE

{

uPFCCPDU [1] UPFCCPDU,

extendedUPFCCPDU [2] ExtendedUPFCCPDU,

mMSCCPDU [3] MMSCCPDU,

nIDDCCPDU [4] NIDDCCPDU,

pTCCCPDU [5] PTCCCPDU

}

-- ===========================

-- HI4 LI notification payload

-- ===========================

LINotificationPayload ::= SEQUENCE

{

lINotificationPayloadOID [1] RELATIVE-OID,

notification [2] LINotificationMessage

}

LINotificationMessage ::= CHOICE

{

lINotification [1] LINotification

}

-- =================

-- HR LI definitions

-- =================

N9HRPDUSessionInfo ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

pDUSessionID [3] PDUSessionID,

location [4] Location OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

dNN [6] DNN OPTIONAL,

messageCause [7] N9HRMessageCause

}

S8HRBearerInfo ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

bearerID [3] EPSBearerID,

linkedBearerID [4] EPSBearerID OPTIONAL,

location [5] Location OPTIONAL,

aPN [6] APN OPTIONAL,

sGWIPAddress [7] IPAddress OPTIONAL,

messageCause [8] S8HRMessageCause

}

-- ================

-- HR LI parameters

-- ================

N9HRMessageCause ::= ENUMERATED

{

pDUSessionEstablished(1),

pDUSessionModified(2),

pDUSessionReleased(3),

updatedLocationAvailable(4),

sMFChanged(5),

other(6)

}

S8HRMessageCause ::= ENUMERATED

{

bearerActivated(1),

bearerModified(2),

bearerDeleted(3),

pDNDisconnected(4),

updatedLocationAvailable(5),

sGWChanged(6),

other(7)

}

-- ==================

-- 5G NEF definitions

-- ==================

-- See clause 7.7.2.1.2 for details of this structure

NEFPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

sNSSAI [4] SNSSAI,

nEFID [5] NEFID,

dNN [6] DNN,

rDSSupport [7] RDSSupport,

sMFID [8] SMFID,

aFID [9] AFID

}

-- See clause 7.7.2.1.3 for details of this structure

NEFPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

sNSSAI [3] SNSSAI,

initiator [4] Initiator,

rDSSourcePortNumber [5] RDSPortNumber OPTIONAL,

rDSDestinationPortNumber [6] RDSPortNumber OPTIONAL,

applicationID [7] ApplicationID OPTIONAL,

aFID [8] AFID OPTIONAL,

rDSAction [9] RDSAction OPTIONAL,

serializationFormat [10] SerializationFormat OPTIONAL

}

-- See clause 7.7.2.1.4 for details of this structure

NEFPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

timeOfFirstPacket [4] Timestamp OPTIONAL,

timeOfLastPacket [5] Timestamp OPTIONAL,

uplinkVolume [6] INTEGER OPTIONAL,

downlinkVolume [7] INTEGER OPTIONAL,

releaseCause [8] NEFReleaseCause

}

-- See clause 7.7.2.1.5 for details of this structure

NEFUnsuccessfulProcedure ::= SEQUENCE

{

failureCause [1] NEFFailureCause,

sUPI [2] SUPI,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

dNN [5] DNN OPTIONAL,

sNSSAI [6] SNSSAI OPTIONAL,

rDSDestinationPortNumber [7] RDSPortNumber,

applicationID [8] ApplicationID,

aFID [9] AFID

}

-- See clause 7.7.2.1.6 for details of this structure

NEFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

dNN [4] DNN,

sNSSAI [5] SNSSAI,

nEFID [6] NEFID,

rDSSupport [7] RDSSupport,

sMFID [8] SMFID,

aFID [9] AFID

}

-- See clause 7.7.3.1.1 for details of this structure

NEFDeviceTrigger ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

aFID [4] AFID,

triggerPayload [5] TriggerPayload OPTIONAL,

validityPeriod [6] INTEGER OPTIONAL,

priorityDT [7] PriorityDT OPTIONAL,

sourcePortId [8] PortNumber OPTIONAL,

destinationPortId [9] PortNumber OPTIONAL

}

-- See clause 7.7.3.1.2 for details of this structure

NEFDeviceTriggerReplace ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

aFID [4] AFID,

triggerPayload [5] TriggerPayload OPTIONAL,

validityPeriod [6] INTEGER OPTIONAL,

priorityDT [7] PriorityDT OPTIONAL,

sourcePortId [8] PortNumber OPTIONAL,

destinationPortId [9] PortNumber OPTIONAL

}

-- See clause 7.7.3.1.3 for details of this structure

NEFDeviceTriggerCancellation ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID

}

-- See clause 7.7.3.1.4 for details of this structure

NEFDeviceTriggerReportNotify ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

deviceTriggerDeliveryResult [4] DeviceTriggerDeliveryResult

}

-- See clause 7.7.4.1.1 for details of this structure

NEFMSISDNLessMOSMS ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

terminatingSMSParty [3] AFID,

sMS [4] SMSTPDUData OPTIONAL,

sourcePort [5] PortNumber OPTIONAL,

destinationPort [6] PortNumber OPTIONAL

}

-- See clause 7.7.5.1.1 for details of this structure

NEFExpectedUEBehaviourUpdate ::= SEQUENCE

{

gPSI [1] GPSI,

expectedUEMovingTrajectory [2] SEQUENCE OF UMTLocationArea5G OPTIONAL,

stationaryIndication [3] StationaryIndication OPTIONAL,

communicationDurationTime [4] INTEGER OPTIONAL,

periodicTime [5] INTEGER OPTIONAL,

scheduledCommunicationTime [6] ScheduledCommunicationTime OPTIONAL,

scheduledCommunicationType [7] ScheduledCommunicationType OPTIONAL,

batteryIndication [8] BatteryIndication OPTIONAL,

trafficProfile [9] TrafficProfile OPTIONAL,

expectedTimeAndDayOfWeekInTrajectory [10] SEQUENCE OF UMTLocationArea5G OPTIONAL,

aFID [11] AFID,

validityTime [12] Timestamp OPTIONAL

}

-- ==========================

-- Common SCEF/NEF parameters

-- ==========================

RDSSupport ::= BOOLEAN

RDSPortNumber ::= INTEGER (0..15)

RDSAction ::= ENUMERATED

{

reservePort(1),

releasePort(2)

}

SerializationFormat ::= ENUMERATED

{

xml(1),

json(2),

cbor(3)

}

ApplicationID ::= OCTET STRING

NIDDCCPDU ::= OCTET STRING

TriggerID ::= UTF8String

PriorityDT ::= ENUMERATED

{

noPriority(1),

priority(2)

}

TriggerPayload ::= OCTET STRING

DeviceTriggerDeliveryResult ::= ENUMERATED

{

success(1),

unknown(2),

failure(3),

triggered(4),

expired(5),

unconfirmed(6),

replaced(7),

terminate(8)

}

StationaryIndication ::= ENUMERATED

{

stationary(1),

mobile(2)

}

BatteryIndication ::= ENUMERATED

{

batteryRecharge(1),

batteryReplace(2),

batteryNoRecharge(3),

batteryNoReplace(4),

noBattery(5)

}

ScheduledCommunicationTime ::= SEQUENCE

{

days [1] SEQUENCE OF Daytime

}

UMTLocationArea5G ::= SEQUENCE

{

timeOfDay [1] Daytime,

durationSec [2] INTEGER,

location [3] NRLocation

}

Daytime ::= SEQUENCE

{

daysOfWeek [1] Day OPTIONAL,

timeOfDayStart [2] Timestamp OPTIONAL,

timeOfDayEnd [3] Timestamp OPTIONAL

}

Day ::= ENUMERATED

{

monday(1),

tuesday(2),

wednesday(3),

thursday(4),

friday(5),

saturday(6),

sunday(7)

}

TrafficProfile ::= ENUMERATED

{

singleTransUL(1),

singleTransDL(2),

dualTransULFirst(3),

dualTransDLFirst(4),

multiTrans(5)

}

ScheduledCommunicationType ::= ENUMERATED

{

downlinkOnly(1),

uplinkOnly(2),

bidirectional(3)

}

-- =================

-- 5G NEF parameters

-- =================

NEFFailureCause ::= ENUMERATED

{

userUnknown(1),

niddConfigurationNotAvailable(2),

contextNotFound(3),

portNotFree(4),

portNotAssociatedWithSpecifiedApplication(5)

}

NEFReleaseCause ::= ENUMERATED

{

sMFRelease(1),

dNRelease(2),

uDMRelease(3),

cHFRelease(4),

localConfigurationPolicy(5),

unknownCause(6)

}

AFID ::= UTF8String

NEFID ::= UTF8String

-- ==================

-- SCEF definitions

-- ==================

-- See clause 7.8.2.1.2 for details of this structure

SCEFPDNConnectionEstablishment ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

ePSBearerID [5] EPSBearerID,

sCEFID [6] SCEFID,

aPN [7] APN,

rDSSupport [8] RDSSupport,

sCSASID [9] SCSASID

}

-- See clause 7.8.2.1.3 for details of this structure

SCEFPDNConnectionUpdate ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

initiator [4] Initiator,

rDSSourcePortNumber [5] RDSPortNumber OPTIONAL,

rDSDestinationPortNumber [6] RDSPortNumber OPTIONAL,

applicationID [7] ApplicationID OPTIONAL,

sCSASID [8] SCSASID OPTIONAL,

rDSAction [9] RDSAction OPTIONAL,

serializationFormat [10] SerializationFormat OPTIONAL

}

-- See clause 7.8.2.1.4 for details of this structure

SCEFPDNConnectionRelease ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

ePSBearerID [4] EPSBearerID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

releaseCause [9] SCEFReleaseCause

}

-- See clause 7.8.2.1.5 for details of this structure

SCEFUnsuccessfulProcedure ::= SEQUENCE

{

failureCause [1] SCEFFailureCause,

iMSI [2] IMSI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

externalIdentifier [4] NAI OPTIONAL,

ePSBearerID [5] EPSBearerID,

aPN [6] APN,

rDSDestinationPortNumber [7] RDSPortNumber OPTIONAL,

applicationID [8] ApplicationID OPTIONAL,

sCSASID [9] SCSASID

}

-- See clause 7.8.2.1.6 for details of this structure

SCEFStartOfInterceptionWithEstablishedPDNConnection ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

ePSBearerID [5] EPSBearerID,

sCEFID [6] SCEFID,

aPN [7] APN,

rDSSupport [8] RDSSupport,

sCSASID [9] SCSASID

}

-- See clause 7.8.3.1.1 for details of this structure

SCEFDeviceTrigger ::= SEQUENCE

{

iMSI [1] IMSI,

mSISDN [2] MSISDN,

externalIdentifier [3] NAI,

triggerId [4] TriggerID,

sCSASID [5] SCSASID OPTIONAL,

triggerPayload [6] TriggerPayload OPTIONAL,

validityPeriod [7] INTEGER OPTIONAL,

priorityDT [8] PriorityDT OPTIONAL,

sourcePortId [9] PortNumber OPTIONAL,

destinationPortId [10] PortNumber OPTIONAL

}

-- See clause 7.8.3.1.2 for details of this structure

SCEFDeviceTriggerReplace ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID,

sCSASID [5] SCSASID OPTIONAL,

triggerPayload [6] TriggerPayload OPTIONAL,

validityPeriod [7] INTEGER OPTIONAL,

priorityDT [8] PriorityDT OPTIONAL,

sourcePortId [9] PortNumber OPTIONAL,

destinationPortId [10] PortNumber OPTIONAL

}

-- See clause 7.8.3.1.3 for details of this structure

SCEFDeviceTriggerCancellation ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID

}

-- See clause 7.8.3.1.4 for details of this structure

SCEFDeviceTriggerReportNotify ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID,

deviceTriggerDeliveryResult [5] DeviceTriggerDeliveryResult

}

-- See clause 7.8.4.1.1 for details of this structure

SCEFMSISDNLessMOSMS ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifie [3] NAI OPTIONAL,

terminatingSMSParty [4] SCSASID,

sMS [5] SMSTPDUData OPTIONAL,

sourcePort [6] PortNumber OPTIONAL,

destinationPort [7] PortNumber OPTIONAL

}

-- See clause 7.8.5.1.1 for details of this structure

SCEFCommunicationPatternUpdate ::= SEQUENCE

{

mSISDN [1] MSISDN OPTIONAL,

externalIdentifier [2] NAI OPTIONAL,

periodicCommunicationIndicator [3] PeriodicCommunicationIndicator OPTIONAL,

communicationDurationTime [4] INTEGER OPTIONAL,

periodicTime [5] INTEGER OPTIONAL,

scheduledCommunicationTime [6] ScheduledCommunicationTime OPTIONAL,

scheduledCommunicationType [7] ScheduledCommunicationType OPTIONAL,

stationaryIndication [8] StationaryIndication OPTIONAL,

batteryIndication [9] BatteryIndication OPTIONAL,

trafficProfile [10] TrafficProfile OPTIONAL,

expectedUEMovingTrajectory [11] SEQUENCE OF UMTLocationArea5G OPTIONAL,

sCSASID [13] SCSASID,

validityTime [14] Timestamp OPTIONAL

}

-- =================

-- SCEF parameters

-- =================

SCEFFailureCause ::= ENUMERATED

{

userUnknown(1),

niddConfigurationNotAvailable(2),

invalidEPSBearer(3),

operationNotAllowed(4),

portNotFree(5),

portNotAssociatedWithSpecifiedApplication(6)

}

SCEFReleaseCause ::= ENUMERATED

{

mMERelease(1),

dNRelease(2),

hSSRelease(3),

localConfigurationPolicy(4),

unknownCause(5)

}

SCSASID ::= UTF8String

SCEFID ::= UTF8String

PeriodicCommunicationIndicator ::= ENUMERATED

{

periodic(1),

nonPeriodic(2)

}

EPSBearerID ::= INTEGER (0..255)

APN ::= UTF8String

-- =======================

-- AKMA AAnF definitions

-- =======================

AAnFAnchorKeyRegister ::= SEQUENCE

{

aKID [1] NAI,

sUPI [2] SUPI,

kAKMA [3] KAKMA OPTIONAL

}

AAnFKAKMAApplicationKeyGet ::= SEQUENCE

{

type [1] KeyGetType,

aKID [2] NAI,

keyInfo [3] AFKeyInfo

}

AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial ::= SEQUENCE

{

aKID [1] NAI,

kAKMA [2] KAKMA OPTIONAL,

aFKeyList [3] SEQUENCE OF AFKeyInfo OPTIONAL

}

AAnFAKMAContextRemovalRecord ::= SEQUENCE

{

aKID [1] NAI,

nFID [2] NFID

}

-- ======================

-- AKMA common parameters

-- ======================

FQDN ::= UTF8String

NFID ::= UTF8String

UAProtocolID ::= OCTET STRING (SIZE(5))

AKMAAFID ::= SEQUENCE

{

aFFQDN [1] FQDN,

uaProtocolID [2] UAProtocolID

}

UAStarParams ::= CHOICE

{

tls12 [1] TLS12UAStarParams,

generic [2] GenericUAStarParams

}

GenericUAStarParams ::= SEQUENCE

{

genericClientParams [1] OCTET STRING,

genericServerParams [2] OCTET STRING

}

-- ===========================================

-- Specific UaStarParmas for TLS 1.2 (RFC5246)

-- ===========================================

TLSCipherType ::= ENUMERATED

{

stream(1),

block(2),

aead(3)

}

TLSCompressionAlgorithm ::= ENUMERATED

{

null(1),

deflate(2)

}

TLSPRFAlgorithm ::= ENUMERATED

{

rfc5246(1)

}

TLSCipherSuite ::= SEQUENCE (SIZE(2)) OF INTEGER (0..255)

TLS12UAStarParams ::= SEQUENCE

{

preMasterSecret [1] OCTET STRING (SIZE(6)) OPTIONAL,

masterSecret [2] OCTET STRING (SIZE(6)),

pRFAlgorithm [3] TLSPRFAlgorithm,

cipherSuite [4] TLSCipherSuite,

cipherType [5] TLSCipherType,

encKeyLength [6] INTEGER (0..255),

blockLength [7] INTEGER (0..255),

fixedIVLength [8] INTEGER (0..255),

recordIVLength [9] INTEGER (0..255),

macLength [10] INTEGER (0..255),

macKeyLength [11] INTEGER (0..255),

compressionAlgorithm [12] TLSCompressionAlgorithm,

clientRandom [13] OCTET STRING (SIZE(4)),

serverRandom [14] OCTET STRING (SIZE(4)),

clientSequenceNumber [15] INTEGER,

serverSequenceNumber [16] INTEGER,

sessionID [17] OCTET STRING (SIZE(0..32)),

tLSExtensions [18] OCTET STRING (SIZE(0..65535))

}

KAF ::= OCTET STRING

KAKMA ::= OCTET STRING

-- ====================

-- AKMA AAnF parameters

-- ====================

KeyGetType ::= ENUMERATED

{

internal(1),

external(2)

}

AFKeyInfo ::= SEQUENCE

{

aFID [1] AKMAAFID,

kAF [2] KAF,

kAFExpTime [3] KAFExpiryTime

}

-- =======================

-- AKMA AF definitions

-- =======================

AFAKMAApplicationKeyRefresh ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

kAF [3] KAF,

uaStarParams [4] UAStarParams OPTIONAL

}

AFStartOfInterceptWithEstablishedAKMAApplicationKey ::= SEQUENCE

{

aFID [1] FQDN,

aKID [2] NAI,

kAFParamList [3] SEQUENCE OF AFSecurityParams

}

AFAuxiliarySecurityParameterEstablishment ::= SEQUENCE

{

aFSecurityParams [1] AFSecurityParams

}

AFSecurityParams ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

kAF [3] KAF,

uaStarParams [4] UAStarParams

}

AFApplicationKeyRemoval ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

removalCause [3] AFKeyRemovalCause

}

-- ===================

-- AKMA AF parameters

-- ===================

KAFParams ::= SEQUENCE

{

aKID [1] NAI,

kAF [2] KAF,

kAFExpTime [3] KAFExpiryTime,

uaStarParams [4] UAStarParams

}

KAFExpiryTime ::= GeneralizedTime

AFKeyRemovalCause ::= ENUMERATED

{

unknown(1),

keyExpiry(2),

applicationSpecific(3)

}

-- ==================

-- 5G AMF definitions

-- ==================

-- See clause 6.2.2.2.2 for details of this structure

AMFRegistration ::= SEQUENCE

{

registrationType [1] AMFRegistrationType,

registrationResult [2] AMFRegistrationResult,

slice [3] Slice OPTIONAL,

sUPI [4] SUPI,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI,

location [9] Location OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

fiveGSTAIList [11] TAIList OPTIONAL,

sMSOverNasIndicator [12] SMSOverNASIndicator OPTIONAL,

oldGUTI [13] EPS5GGUTI OPTIONAL,

eMM5GRegStatus [14] EMM5GMMStatus OPTIONAL,

nonIMEISVPEI [15] NonIMEISVPEI OPTIONAL,

mACRestIndicator [16] MACRestrictionIndicator OPTIONAL

}

-- See clause 6.2.2.2.3 for details of this structure

AMFDeregistration ::= SEQUENCE

{

deregistrationDirection [1] AMFDirection,

accessType [2] AccessType,

sUPI [3] SUPI OPTIONAL,

sUCI [4] SUCI OPTIONAL,

pEI [5] PEI OPTIONAL,

gPSI [6] GPSI OPTIONAL,

gUTI [7] FiveGGUTI OPTIONAL,

cause [8] FiveGMMCause OPTIONAL,

location [9] Location OPTIONAL,

switchOffIndicator [10] SwitchOffIndicator OPTIONAL,

reRegRequiredIndicator [11] ReRegRequiredIndicator OPTIONAL

}

-- See clause 6.2.2.2.4 for details of this structure

AMFLocationUpdate ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI OPTIONAL,

location [6] Location,

sMSOverNASIndicator [7] SMSOverNASIndicator OPTIONAL,

oldGUTI [8] EPS5GGUTI OPTIONAL

}

-- See clause 6.2.2.2.5 for details of this structure

AMFStartOfInterceptionWithRegisteredUE ::= SEQUENCE

{

registrationResult [1] AMFRegistrationResult,

registrationType [2] AMFRegistrationType OPTIONAL,

slice [3] Slice OPTIONAL,

sUPI [4] SUPI,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI,

location [9] Location OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

timeOfRegistration [11] Timestamp OPTIONAL,

fiveGSTAIList [12] TAIList OPTIONAL,

sMSOverNASIndicator [13] SMSOverNASIndicator OPTIONAL,

oldGUTI [14] EPS5GGUTI OPTIONAL,

eMM5GRegStatus [15] EMM5GMMStatus OPTIONAL

}

-- See clause 6.2.2.2.6 for details of this structure

AMFUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] AMFFailedProcedureType,

failureCause [2] AMFFailureCause,

requestedSlice [3] NSSAI OPTIONAL,

sUPI [4] SUPI OPTIONAL,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI OPTIONAL,

location [9] Location OPTIONAL

}

-- =================

-- 5G AMF parameters

-- =================

AMFID ::= SEQUENCE

{

aMFRegionID [1] AMFRegionID,

aMFSetID [2] AMFSetID,

aMFPointer [3] AMFPointer

}

AMFDirection ::= ENUMERATED

{

networkInitiated(1),

uEInitiated(2)

}

AMFFailedProcedureType ::= ENUMERATED

{

registration(1),

sMS(2),

pDUSessionEstablishment(3)

}

AMFFailureCause ::= CHOICE

{

fiveGMMCause [1] FiveGMMCause,

fiveGSMCause [2] FiveGSMCause

}

AMFPointer ::= INTEGER (0..63)

AMFRegistrationResult ::= ENUMERATED

{

threeGPPAccess(1),

nonThreeGPPAccess(2),

threeGPPAndNonThreeGPPAccess(3)

}

AMFRegionID ::= INTEGER (0..255)

AMFRegistrationType ::= ENUMERATED

{

initial(1),

mobility(2),

periodic(3),

emergency(4)

}

AMFSetID ::= INTEGER (0..1023)

-- ==================

-- 5G SMF definitions

-- ==================

-- See clause 6.2.3.2.2 for details of this structure

SMFPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

gTPTunnelID [6] FTEID,

pDUSessionType [7] PDUSessionType,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

location [11] Location OPTIONAL,

dNN [12] DNN,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

uEEPSPDNConnection [19] UEEPSPDNConnection OPTIONAL

}

-- See clause 6.2.3.2.3 for details of this structure

SMFPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

location [7] Location OPTIONAL,

requestType [8] FiveGSMRequestType,

accessType [9] AccessType OPTIONAL,

rATType [10] RATType OPTIONAL,

pDUSessionID [11] PDUSessionID OPTIONAL

}

-- See clause 6.2.3.2.4 for details of this structure

SMFPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

location [9] Location OPTIONAL,

cause [10] SMFErrorCodes OPTIONAL

}

-- See clause 6.2.3.2.5 for details of this structure

SMFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

gTPTunnelID [6] FTEID,

pDUSessionType [7] PDUSessionType,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

location [11] Location OPTIONAL,

dNN [12] DNN,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

timeOfSessionEstablishment [19] Timestamp OPTIONAL

}

-- See clause 6.2.3.2.6 for details of this structure

SMFUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] SMFFailedProcedureType,

failureCause [2] FiveGSMCause,

initiator [3] Initiator,

requestedSlice [4] NSSAI OPTIONAL,

sUPI [5] SUPI OPTIONAL,

sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

pEI [7] PEI OPTIONAL,

gPSI [8] GPSI OPTIONAL,

pDUSessionID [9] PDUSessionID OPTIONAL,

uEEndpoint [10] SEQUENCE OF UEEndpointAddress OPTIONAL,

non3GPPAccessEndpoint [11] UEEndpointAddress OPTIONAL,

dNN [12] DNN OPTIONAL,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType OPTIONAL,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

location [19] Location OPTIONAL

}

-- See clause 6.2.3.2.8 for details of this structure

SMFPDUtoMAPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

location [7] Location OPTIONAL,

requestType [8] FiveGSMRequestType,

accessType [9] AccessType OPTIONAL,

rATType [10] RATType OPTIONAL,

pDUSessionID [11] PDUSessionID,

requestIndication [12] RequestIndication,

aTSSSContainer [13] ATSSSContainer

}

-- See clause 6.2.3.2.7.1 for details of this structure

SMFMAPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

pDUSessionType [6] PDUSessionType,

accessInfo [7] SEQUENCE OF AccessInfo,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [10] Location OPTIONAL,

dNN [11] DNN,

aMFID [12] AMFID OPTIONAL,

hSMFURI [13] HSMFURI OPTIONAL,

requestType [14] FiveGSMRequestType,

sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

servingNetwork [16] SMFServingNetwork,

oldPDUSessionID [17] PDUSessionID OPTIONAL,

mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [20] SMFMAAcceptedIndication,

aTSSSContainer [21] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.2 for details of this structure

SMFMAPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

accessInfo [6] SEQUENCE OF AccessInfo OPTIONAL,

sNSSAI [7] SNSSAI OPTIONAL,

location [8] Location OPTIONAL,

requestType [9] FiveGSMRequestType OPTIONAL,

servingNetwork [10] SMFServingNetwork,

oldPDUSessionID [11] PDUSessionID OPTIONAL,

mAUpgradeIndication [12] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [13] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [14] SMFMAAcceptedIndication,

aTSSSContainer [15] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.3 for details of this structure

SMFMAPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

location [9] Location OPTIONAL,

cause [10] SMFErrorCodes OPTIONAL

}

-- See clause 6.2.3.2.7.4 for details of this structure

SMFStartOfInterceptionWithEstablishedMAPDUSession ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

pDUSessionType [6] PDUSessionType,

accessInfo [7] SEQUENCE OF AccessInfo,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [10] Location OPTIONAL,

dNN [11] DNN,

aMFID [12] AMFID OPTIONAL,

hSMFURI [13] HSMFURI OPTIONAL,

requestType [14] FiveGSMRequestType OPTIONAL,

sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

servingNetwork [16] SMFServingNetwork,

oldPDUSessionID [17] PDUSessionID OPTIONAL,

mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [20] SMFMAAcceptedIndication,

aTSSSContainer [21] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.5 for details of this structure

SMFMAUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] SMFFailedProcedureType,

failureCause [2] FiveGSMCause,

requestedSlice [3] NSSAI OPTIONAL,

initiator [4] Initiator,

sUPI [5] SUPI OPTIONAL,

sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

pEI [7] PEI OPTIONAL,

gPSI [8] GPSI OPTIONAL,

pDUSessionID [9] PDUSessionID OPTIONAL,

accessInfo [10] SEQUENCE OF AccessInfo,

uEEndpoint [11] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [12] Location OPTIONAL,

dNN [13] DNN OPTIONAL,

aMFID [14] AMFID OPTIONAL,

hSMFURI [15] HSMFURI OPTIONAL,

requestType [16] FiveGSMRequestType OPTIONAL,

sMPDUDNRequest [17] SMPDUDNRequest OPTIONAL

}

-- =================

-- 5G SMF parameters

-- =================

SMFID ::= UTF8String

SMFFailedProcedureType ::= ENUMERATED

{

pDUSessionEstablishment(1),

pDUSessionModification(2),

pDUSessionRelease(3)

}

SMFServingNetwork ::= SEQUENCE

{

pLMNID [1] PLMNID,

nID [2] NID OPTIONAL

}

AccessInfo ::= SEQUENCE

{

accessType [1] AccessType,

rATType [2] RATType OPTIONAL,

gTPTunnelID [3] FTEID,

non3GPPAccessEndpoint [4] UEEndpointAddress OPTIONAL,

establishmentStatus [5] EstablishmentStatus,

aNTypeToReactivate [6] AccessType OPTIONAL

}

-- see Clause 6.1.2 of TS 24.193[44] for the details of the ATSSS container contents.

ATSSSContainer ::= OCTET STRING

EstablishmentStatus ::= ENUMERATED

{

established(0),

released(1)

}

SMFMAUpgradeIndication ::= BOOLEAN

-- Given in YAML encoding as defined in clause 6.1.6.2.31 of TS 29.502[16]

SMFEPSPDNCnxInfo ::= UTF8String

SMFMAAcceptedIndication ::= BOOLEAN

-- see Clause 6.1.6.3.8 of TS 29.502[16] for the details of this structure.

SMFErrorCodes ::= UTF8String

-- see Clause 6.1.6.3.2 of TS 29.502[16] for details of this structure.

UEEPSPDNConnection ::= OCTET STRING

-- see Clause 6.1.6.3.6 of TS 29.502[16] for the details of this structure.

RequestIndication ::= ENUMERATED

{

uEREQPDUSESMOD(0),

uEREQPDUSESREL(1),

pDUSESMOB(2),

nWREQPDUSESAUTH(3),

nWREQPDUSESMOD(4),

nWREQPDUSESREL(5),

eBIASSIGNMENTREQ(6),

rELDUETO5GANREQUEST(7)

}

-- ==================

-- 5G UPF definitions

-- ==================

UPFCCPDU ::= OCTET STRING

-- See clause 6.2.3.8 for the details of this structure

ExtendedUPFCCPDU ::= SEQUENCE

{

payload [1] UPFCCPDUPayload,

qFI [2] QFI OPTIONAL

}

-- =================

-- 5G UPF parameters

-- =================

UPFCCPDUPayload ::= CHOICE

{

uPFIPCC [1] OCTET STRING,

uPFEthernetCC [2] OCTET STRING,

uPFUnstructuredCC [3] OCTET STRING

}

QFI ::= INTEGER (0..63)

-- ==================

-- 5G UDM definitions

-- ==================

UDMServingSystemMessage ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

gUAMI [4] GUAMI OPTIONAL,

gUMMEI [5] GUMMEI OPTIONAL,

pLMNID [6] PLMNID OPTIONAL,

servingSystemMethod [7] UDMServingSystemMethod,

serviceID [8] ServiceID OPTIONAL

}

UDMSubscriberRecordChangeMessage ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

oldPEI [4] PEI OPTIONAL,

oldSUPI [5] SUPI OPTIONAL,

oldGPSI [6] GPSI OPTIONAL,

oldserviceID [7] ServiceID OPTIONAL,

subscriberRecordChangeMethod [8] UDMSubscriberRecordChangeMethod,

serviceID [9] ServiceID OPTIONAL

}

UDMCancelLocationMessage ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

gUAMI [4] GUAMI OPTIONAL,

pLMNID [5] PLMNID OPTIONAL,

cancelLocationMethod [6] UDMCancelLocationMethod

}

-- =================

-- 5G UDM parameters

-- =================

UDMServingSystemMethod ::= ENUMERATED

{

amf3GPPAccessRegistration(0),

amfNon3GPPAccessRegistration(1),

unknown(2)

}

UDMSubscriberRecordChangeMethod ::= ENUMERATED

{

pEIChange(1),

sUPIChange(2),

gPSIChange(3),

uEDeprovisioning(4),

unknown(5),

serviceIDChange(6)

}

UDMCancelLocationMethod ::= ENUMERATED

{

aMF3GPPAccessDeregistration(1),

aMFNon3GPPAccessDeregistration(2),

uDMDeregistration(3),

unknown(4)

}

ServiceID ::= SEQUENCE

{

nSSAI [1] NSSAI OPTIONAL,

cAGID [2] SEQUENCE OF CAGID OPTIONAL

}

CAGID ::= UTF8String

-- ===================

-- 5G SMSF definitions

-- ===================

-- See clause 6.2.5.3 for details of this structure

SMSMessage ::= SEQUENCE

{

originatingSMSParty [1] SMSParty,

terminatingSMSParty [2] SMSParty,

direction [3] Direction,

linkTransferStatus [4] SMSTransferStatus,

otherMessage [5] SMSOtherMessageIndication OPTIONAL,

location [6] Location OPTIONAL,

peerNFAddress [7] SMSNFAddress OPTIONAL,

peerNFType [8] SMSNFType OPTIONAL,

sMSTPDUData [9] SMSTPDUData OPTIONAL,

messageType [10] SMSMessageType OPTIONAL,

rPMessageReference [11] SMSRPMessageReference OPTIONAL

}

SMSReport ::= SEQUENCE

{

location [1] Location OPTIONAL,

sMSTPDUData [2] SMSTPDUData,

messageType [3] SMSMessageType,

rPMessageReference [4] SMSRPMessageReference

}

-- ==================

-- 5G SMSF parameters

-- ==================

SMSAddress ::= OCTET STRING(SIZE(2..12))

SMSMessageType ::= ENUMERATED

{

deliver(1),

deliverReportAck(2),

deliverReportError(3),

statusReport(4),

command(5),

submit(6),

submitReportAck(7),

submitReportError(8),

reserved(9)

}

SMSParty ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

sMSAddress [4] SMSAddress OPTIONAL

}

SMSTransferStatus ::= ENUMERATED

{

transferSucceeded(1),

transferFailed(2),

undefined(3)

}

SMSOtherMessageIndication ::= BOOLEAN

SMSNFAddress ::= CHOICE

{

iPAddress [1] IPAddress,

e164Number [2] E164Number

}

SMSNFType ::= ENUMERATED

{

sMSGMSC(1),

iWMSC(2),

sMSRouter(3)

}

SMSRPMessageReference ::= INTEGER (0..255)

SMSTPDUData ::= CHOICE

{

sMSTPDU [1] SMSTPDU,

truncatedSMSTPDU [2] TruncatedSMSTPDU

}

SMSTPDU ::= OCTET STRING (SIZE(1..270))

TruncatedSMSTPDU ::= OCTET STRING (SIZE(1..130))

-- ===============

-- MMS definitions

-- ===============

MMSSend ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

dateTime [3] Timestamp,

originatingMMSParty [4] MMSParty,

terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

direction [8] MMSDirection,

subject [9] MMSSubject OPTIONAL,

messageClass [10] MMSMessageClass OPTIONAL,

expiry [11] MMSExpiry,

desiredDeliveryTime [12] Timestamp OPTIONAL,

priority [13] MMSPriority OPTIONAL,

senderVisibility [14] BOOLEAN OPTIONAL,

deliveryReport [15] BOOLEAN OPTIONAL,

readReport [16] BOOLEAN OPTIONAL,

store [17] BOOLEAN OPTIONAL,

state [18] MMState OPTIONAL,

flags [19] MMFlags OPTIONAL,

replyCharging [20] MMSReplyCharging OPTIONAL,

applicID [21] UTF8String OPTIONAL,

replyApplicID [22] UTF8String OPTIONAL,

auxApplicInfo [23] UTF8String OPTIONAL,

contentClass [24] MMSContentClass OPTIONAL,

dRMContent [25] BOOLEAN OPTIONAL,

adaptationAllowed [26] MMSAdaptation OPTIONAL,

contentType [27] MMSContentType,

responseStatus [28] MMSResponseStatus,

responseStatusText [29] UTF8String OPTIONAL,

messageID [30] UTF8String

}

MMSSendByNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

contentType [7] MMSContentType,

messageClass [8] MMSMessageClass OPTIONAL,

dateTime [9] Timestamp,

expiry [10] MMSExpiry OPTIONAL,

deliveryReport [11] BOOLEAN OPTIONAL,

priority [12] MMSPriority OPTIONAL,

senderVisibility [13] BOOLEAN OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

subject [15] MMSSubject OPTIONAL,

forwardCount [16] INTEGER OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [18] Timestamp OPTIONAL,

applicID [19] UTF8String OPTIONAL,

replyApplicID [20] UTF8String OPTIONAL,

auxApplicInfo [21] UTF8String OPTIONAL,

contentClass [22] MMSContentClass OPTIONAL,

dRMContent [23] BOOLEAN OPTIONAL,

adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotification ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

originatingMMSParty [3] MMSParty OPTIONAL,

direction [4] MMSDirection,

subject [5] MMSSubject OPTIONAL,

deliveryReportRequested [6] BOOLEAN OPTIONAL,

stored [7] BOOLEAN OPTIONAL,

messageClass [8] MMSMessageClass,

priority [9] MMSPriority OPTIONAL,

messageSize [10] INTEGER,

expiry [11] MMSExpiry,

replyCharging [12] MMSReplyCharging OPTIONAL

}

MMSSendToNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

contentType [7] MMSContentType,

messageClass [8] MMSMessageClass OPTIONAL,

dateTime [9] Timestamp,

expiry [10] MMSExpiry OPTIONAL,

deliveryReport [11] BOOLEAN OPTIONAL,

priority [12] MMSPriority OPTIONAL,

senderVisibility [13] BOOLEAN OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

subject [15] MMSSubject OPTIONAL,

forwardCount [16] INTEGER OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [18] Timestamp OPTIONAL,

applicID [19] UTF8String OPTIONAL,

replyApplicID [20] UTF8String OPTIONAL,

auxApplicInfo [21] UTF8String OPTIONAL,

contentClass [22] MMSContentClass OPTIONAL,

dRMContent [23] BOOLEAN OPTIONAL,

adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotificationResponse ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

status [4] MMStatus,

reportAllowed [5] BOOLEAN OPTIONAL

}

MMSRetrieval ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

messageID [3] UTF8String,

dateTime [4] Timestamp,

originatingMMSParty [5] MMSParty OPTIONAL,

previouslySentBy [6] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [7] Timestamp OPTIONAL,

terminatingMMSParty [8] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

direction [10] MMSDirection,

subject [11] MMSSubject OPTIONAL,

state [12] MMState OPTIONAL,

flags [13] MMFlags OPTIONAL,

messageClass [14] MMSMessageClass OPTIONAL,

priority [15] MMSPriority,

deliveryReport [16] BOOLEAN OPTIONAL,

readReport [17] BOOLEAN OPTIONAL,

replyCharging [18] MMSReplyCharging OPTIONAL,

retrieveStatus [19] MMSRetrieveStatus OPTIONAL,

retrieveStatusText [20] UTF8String OPTIONAL,

applicID [21] UTF8String OPTIONAL,

replyApplicID [22] UTF8String OPTIONAL,

auxApplicInfo [23] UTF8String OPTIONAL,

contentClass [24] MMSContentClass OPTIONAL,

dRMContent [25] BOOLEAN OPTIONAL,

replaceID [26] UTF8String OPTIONAL,

contentType [27] UTF8String OPTIONAL

}

MMSDeliveryAck ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

reportAllowed [3] BOOLEAN OPTIONAL,

status [4] MMStatus,

direction [5] MMSDirection

}

MMSForward ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

dateTime [3] Timestamp OPTIONAL,

originatingMMSParty [4] MMSParty,

terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

direction [8] MMSDirection,

expiry [9] MMSExpiry OPTIONAL,

desiredDeliveryTime [10] Timestamp OPTIONAL,

deliveryReportAllowed [11] BOOLEAN OPTIONAL,

deliveryReport [12] BOOLEAN OPTIONAL,

store [13] BOOLEAN OPTIONAL,

state [14] MMState OPTIONAL,

flags [15] MMFlags OPTIONAL,

contentLocationReq [16] UTF8String,

replyCharging [17] MMSReplyCharging OPTIONAL,

responseStatus [18] MMSResponseStatus,

responseStatusText [19] UTF8String OPTIONAL,

messageID [20] UTF8String OPTIONAL,

contentLocationConf [21] UTF8String OPTIONAL,

storeStatus [22] MMSStoreStatus OPTIONAL,

storeStatusText [23] UTF8String OPTIONAL

}

MMSDeleteFromRelay ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] SEQUENCE OF UTF8String,

contentLocationConf [5] SEQUENCE OF UTF8String,

deleteResponseStatus [6] MMSDeleteResponseStatus,

deleteResponseText [7] SEQUENCE OF UTF8String

}

MMSMBoxStore ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] UTF8String,

state [5] MMState OPTIONAL,

flags [6] MMFlags OPTIONAL,

contentLocationConf [7] UTF8String OPTIONAL,

storeStatus [8] MMSStoreStatus,

storeStatusText [9] UTF8String OPTIONAL

}

MMSMBoxUpload ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

state [4] MMState OPTIONAL,

flags [5] MMFlags OPTIONAL,

contentType [6] UTF8String,

contentLocation [7] UTF8String OPTIONAL,

storeStatus [8] MMSStoreStatus,

storeStatusText [9] UTF8String OPTIONAL,

mMessages [10] SEQUENCE OF MMBoxDescription

}

MMSMBoxDelete ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] SEQUENCE OF UTF8String,

contentLocationConf [5] SEQUENCE OF UTF8String OPTIONAL,

responseStatus [6] MMSDeleteResponseStatus,

responseStatusText [7] UTF8String OPTIONAL

}

MMSDeliveryReport ::= SEQUENCE

{

version [1] MMSVersion,

messageID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

mMSDateTime [4] Timestamp,

responseStatus [5] MMSResponseStatus,

responseStatusText [6] UTF8String OPTIONAL,

applicID [7] UTF8String OPTIONAL,

replyApplicID [8] UTF8String OPTIONAL,

auxApplicInfo [9] UTF8String OPTIONAL

}

MMSDeliveryReportNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

mMSDateTime [7] Timestamp,

forwardToOriginator [8] BOOLEAN OPTIONAL,

status [9] MMStatus,

statusExtension [10] MMStatusExtension,

statusText [11] MMStatusText,

applicID [12] UTF8String OPTIONAL,

replyApplicID [13] UTF8String OPTIONAL,

auxApplicInfo [14] UTF8String OPTIONAL

}

MMSReadReport ::= SEQUENCE

{

version [1] MMSVersion,

messageID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

originatingMMSParty [4] SEQUENCE OF MMSParty,

direction [5] MMSDirection,

mMSDateTime [6] Timestamp,

readStatus [7] MMSReadStatus,

applicID [8] UTF8String OPTIONAL,

replyApplicID [9] UTF8String OPTIONAL,

auxApplicInfo [10] UTF8String OPTIONAL

}

MMSReadReportNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

originatingMMSParty [4] SEQUENCE OF MMSParty,

direction [5] MMSDirection,

messageID [6] UTF8String,

mMSDateTime [7] Timestamp,

readStatus [8] MMSReadStatus,

readStatusText [9] MMSReadStatusText OPTIONAL,

applicID [10] UTF8String OPTIONAL,

replyApplicID [11] UTF8String OPTIONAL,

auxApplicInfo [12] UTF8String OPTIONAL

}

MMSCancel ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

cancelID [3] UTF8String,

direction [4] MMSDirection

}

MMSMBoxViewRequest ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

contentLocation [3] UTF8String OPTIONAL,

state [4] SEQUENCE OF MMState OPTIONAL,

flags [5] SEQUENCE OF MMFlags OPTIONAL,

start [6] INTEGER OPTIONAL,

limit [7] INTEGER OPTIONAL,

attributes [8] SEQUENCE OF UTF8String OPTIONAL,

totals [9] INTEGER OPTIONAL,

quotas [10] MMSQuota OPTIONAL

}

MMSMBoxViewResponse ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

contentLocation [3] UTF8String OPTIONAL,

state [4] SEQUENCE OF MMState OPTIONAL,

flags [5] SEQUENCE OF MMFlags OPTIONAL,

start [6] INTEGER OPTIONAL,

limit [7] INTEGER OPTIONAL,

attributes [8] SEQUENCE OF UTF8String OPTIONAL,

mMSTotals [9] BOOLEAN OPTIONAL,

mMSQuotas [10] BOOLEAN OPTIONAL,

mMessages [11] SEQUENCE OF MMBoxDescription

}

MMBoxDescription ::= SEQUENCE

{

contentLocation [1] UTF8String OPTIONAL,

messageID [2] UTF8String OPTIONAL,

state [3] MMState OPTIONAL,

flags [4] SEQUENCE OF MMFlags OPTIONAL,

dateTime [5] Timestamp OPTIONAL,

originatingMMSParty [6] MMSParty OPTIONAL,

terminatingMMSParty [7] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [8] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

messageClass [10] MMSMessageClass OPTIONAL,

subject [11] MMSSubject OPTIONAL,

priority [12] MMSPriority OPTIONAL,

deliveryTime [13] Timestamp OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

messageSize [15] INTEGER OPTIONAL,

replyCharging [16] MMSReplyCharging OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

previouslySentByDateTime [18] Timestamp OPTIONAL,

contentType [19] UTF8String OPTIONAL

}

-- =========

-- MMS CCPDU

-- =========

MMSCCPDU ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

mMSContent [3] OCTET STRING

}

-- ==============

-- MMS parameters

-- ==============

MMSAdaptation ::= SEQUENCE

{

allowed [1] BOOLEAN,

overriden [2] BOOLEAN

}

MMSCancelStatus ::= ENUMERATED

{

cancelRequestSuccessfullyReceived(1),

cancelRequestCorrupted(2)

}

MMSContentClass ::= ENUMERATED

{

text(1),

imageBasic(2),

imageRich(3),

videoBasic(4),

videoRich(5),

megaPixel(6),

contentBasic(7),

contentRich(8)

}

MMSContentType ::= UTF8String

MMSDeleteResponseStatus ::= ENUMERATED

{

ok(1),

errorUnspecified(2),

errorServiceDenied(3),

errorMessageFormatCorrupt(4),

errorSendingAddressUnresolved(5),

errorMessageNotFound(6),

errorNetworkProblem(7),

errorContentNotAccepted(8),

errorUnsupportedMessage(9),

errorTransientFailure(10),

errorTransientSendingAddressUnresolved(11),

errorTransientMessageNotFound(12),

errorTransientNetworkProblem(13),

errorTransientPartialSuccess(14),

errorPermanentFailure(15),

errorPermanentServiceDenied(16),

errorPermanentMessageFormatCorrupt(17),

errorPermanentSendingAddressUnresolved(18),

errorPermanentMessageNotFound(19),

errorPermanentContentNotAccepted(20),

errorPermanentReplyChargingLimitationsNotMet(21),

errorPermanentReplyChargingRequestNotAccepted(22),

errorPermanentReplyChargingForwardingDenied(23),

errorPermanentReplyChargingNotSupported(24),

errorPermanentAddressHidingNotSupported(25),

errorPermanentLackOfPrepaid(26)

}

MMSDirection ::= ENUMERATED

{

fromTarget(0),

toTarget(1)

}

MMSElementDescriptor ::= SEQUENCE

{

reference [1] UTF8String,

parameter [2] UTF8String OPTIONAL,

value [3] UTF8String OPTIONAL

}

MMSExpiry ::= SEQUENCE

{

expiryPeriod [1] INTEGER,

periodFormat [2] MMSPeriodFormat

}

MMFlags ::= SEQUENCE

{

length [1] INTEGER,

flag [2] MMStateFlag,

flagString [3] UTF8String

}

MMSMessageClass ::= ENUMERATED

{

personal(1),

advertisement(2),

informational(3),

auto(4)

}

MMSParty ::= SEQUENCE

{

mMSPartyIDs [1] SEQUENCE OF MMSPartyID,

nonLocalID [2] NonLocalID

}

MMSPartyID ::= CHOICE

{

e164Number [1] E164Number,

emailAddress [2] EmailAddress,

iMSI [3] IMSI,

iMPU [4] IMPU,

iMPI [5] IMPI,

sUPI [6] SUPI,

gPSI [7] GPSI

}

MMSPeriodFormat ::= ENUMERATED

{

absolute(1),

relative(2)

}

MMSPreviouslySent ::= SEQUENCE

{

previouslySentByParty [1] MMSParty,

sequenceNumber [2] INTEGER,

previousSendDateTime [3] Timestamp

}

MMSPreviouslySentBy ::= SEQUENCE OF MMSPreviouslySent

MMSPriority ::= ENUMERATED

{

low(1),

normal(2),

high(3)

}

MMSQuota ::= SEQUENCE

{

quota [1] INTEGER,

quotaUnit [2] MMSQuotaUnit

}

MMSQuotaUnit ::= ENUMERATED

{

numMessages(1),

bytes(2)

}

MMSReadStatus ::= ENUMERATED

{

read(1),

deletedWithoutBeingRead(2)

}

MMSReadStatusText ::= UTF8String

MMSReplyCharging ::= ENUMERATED

{

requested(0),

requestedTextOnly(1),

accepted(2),

acceptedTextOnly(3)

}

MMSResponseStatus ::= ENUMERATED

{

ok(1),

errorUnspecified(2),

errorServiceDenied(3),

errorMessageFormatCorrupt(4),

errorSendingAddressUnresolved(5),

errorMessageNotFound(6),

errorNetworkProblem(7),

errorContentNotAccepted(8),

errorUnsupportedMessage(9),

errorTransientFailure(10),

errorTransientSendingAddressUnresolved(11),

errorTransientMessageNotFound(12),

errorTransientNetworkProblem(13),

errorTransientPartialSuccess(14),

errorPermanentFailure(15),

errorPermanentServiceDenied(16),

errorPermanentMessageFormatCorrupt(17),

errorPermanentSendingAddressUnresolved(18),

errorPermanentMessageNotFound(19),

errorPermanentContentNotAccepted(20),

errorPermanentReplyChargingLimitationsNotMet(21),

errorPermanentReplyChargingRequestNotAccepted(22),

errorPermanentReplyChargingForwardingDenied(23),

errorPermanentReplyChargingNotSupported(24),

errorPermanentAddressHidingNotSupported(25),

errorPermanentLackOfPrepaid(26)

}

MMSRetrieveStatus ::= ENUMERATED

{

success(1),

errorTransientFailure(2),

errorTransientMessageNotFound(3),

errorTransientNetworkProblem(4),

errorPermanentFailure(5),

errorPermanentServiceDenied(6),

errorPermanentMessageNotFound(7),

errorPermanentContentUnsupported(8)

}

MMSStoreStatus ::= ENUMERATED

{

success(1),

errorTransientFailure(2),

errorTransientNetworkProblem(3),

errorPermanentFailure(4),

errorPermanentServiceDenied(5),

errorPermanentMessageFormatCorrupt(6),

errorPermanentMessageNotFound(7),

errorMMBoxFull(8)

}

MMState ::= ENUMERATED

{

draft(1),

sent(2),

new(3),

retrieved(4),

forwarded(5)

}

MMStateFlag ::= ENUMERATED

{

add(1),

remove(2),

filter(3)

}

MMStatus ::= ENUMERATED

{

expired(1),

retrieved(2),

rejected(3),

deferred(4),

unrecognized(5),

indeterminate(6),

forwarded(7),

unreachable(8)

}

MMStatusExtension ::= ENUMERATED

{

rejectionByMMSRecipient(0),

rejectionByOtherRS(1)

}

MMStatusText ::= UTF8String

MMSSubject ::= UTF8String

MMSVersion ::= SEQUENCE

{

majorVersion [1] INTEGER,

minorVersion [2] INTEGER

}

-- ==================

-- 5G PTC definitions

-- ==================

PTCRegistration ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCServerURI [2] UTF8String,

pTCRegistrationRequest [3] PTCRegistrationRequest,

pTCRegistrationOutcome [4] PTCRegistrationOutcome

}

PTCSessionInitiation ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCOriginatingID [5] PTCTargetInformation,

pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

location [8] Location OPTIONAL,

pTCBearerCapability [9] UTF8String OPTIONAL,

pTCHost [10] PTCTargetInformation OPTIONAL

}

PTCSessionAbandon ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

location [4] Location OPTIONAL,

pTCAbandonCause [5] INTEGER

}

PTCSessionStart ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCOriginatingID [5] PTCTargetInformation,

pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

location [8] Location OPTIONAL,

pTCHost [9] PTCTargetInformation OPTIONAL,

pTCBearerCapability [10] UTF8String OPTIONAL

}

PTCSessionEnd ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCParticipants [5] SEQUENCE OF PTCTargetInformation OPTIONAL,

location [6] Location OPTIONAL,

pTCSessionEndCause [7] PTCSessionEndCause

}

PTCStartOfInterception ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

preEstSessionID [3] PTCSessionInfo OPTIONAL,

pTCOriginatingID [4] PTCTargetInformation,

pTCSessionInfo [5] PTCSessionInfo OPTIONAL,

pTCHost [6] PTCTargetInformation OPTIONAL,

pTCParticipants [7] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCMediaStreamAvail [8] BOOLEAN OPTIONAL,

pTCBearerCapability [9] UTF8String OPTIONAL

}

PTCPreEstablishedSession ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCServerURI [2] UTF8String,

rTPSetting [3] RTPSetting,

pTCMediaCapability [4] UTF8String,

pTCPreEstSessionID [5] PTCSessionInfo,

pTCPreEstStatus [6] PTCPreEstStatus,

pTCMediaStreamAvail [7] BOOLEAN OPTIONAL,

location [8] Location OPTIONAL,

pTCFailureCode [9] PTCFailureCode OPTIONAL

}

PTCInstantPersonalAlert ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCIPAPartyID [2] PTCTargetInformation,

pTCIPADirection [3] Direction

}

PTCPartyJoin ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [5] MultipleParticipantPresenceStatus OPTIONAL,

pTCMediaStreamAvail [6] BOOLEAN OPTIONAL,

pTCBearerCapability [7] UTF8String OPTIONAL

}

PTCPartyDrop ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCPartyDrop [4] PTCTargetInformation,

pTCParticipantPresenceStatus [5] PTCParticipantPresenceStatus OPTIONAL

}

PTCPartyHold ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCHoldID [5] SEQUENCE OF PTCTargetInformation,

pTCHoldRetrieveInd [6] BOOLEAN

}

PTCMediaModification ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCMediaStreamAvail [4] BOOLEAN OPTIONAL,

pTCBearerCapability [5] UTF8String

}

PTCGroupAdvertisement ::=SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCIDList [3] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCGroupAuthRule [4] PTCGroupAuthRule OPTIONAL,

pTCGroupAdSender [5] PTCTargetInformation,

pTCGroupNickname [6] UTF8String OPTIONAL

}

PTCFloorControl ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessioninfo [3] PTCSessionInfo,

pTCFloorActivity [4] SEQUENCE OF PTCFloorActivity,

pTCFloorSpeakerID [5] PTCTargetInformation OPTIONAL,

pTCMaxTBTime [6] INTEGER OPTIONAL,

pTCQueuedFloorControl [7] BOOLEAN OPTIONAL,

pTCQueuedPosition [8] INTEGER OPTIONAL,

pTCTalkBurstPriority [9] PTCTBPriorityLevel OPTIONAL,

pTCTalkBurstReason [10] PTCTBReasonCode OPTIONAL

}

PTCTargetPresence ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCTargetPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCParticipantPresence ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCParticipantPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCListManagement ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCListManagementType [3] PTCListManagementType OPTIONAL,

pTCListManagementAction [4] PTCListManagementAction OPTIONAL,

pTCListManagementFailure [5] PTCListManagementFailure OPTIONAL,

pTCContactID [6] PTCTargetInformation OPTIONAL,

pTCIDList [7] SEQUENCE OF PTCIDList OPTIONAL,

pTCHost [8] PTCTargetInformation OPTIONAL

}

PTCAccessPolicy ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCAccessPolicyType [3] PTCAccessPolicyType OPTIONAL,

pTCUserAccessPolicy [4] PTCUserAccessPolicy OPTIONAL,

pTCGroupAuthRule [5] PTCGroupAuthRule OPTIONAL,

pTCContactID [6] PTCTargetInformation OPTIONAL,

pTCAccessPolicyFailure [7] PTCAccessPolicyFailure OPTIONAL

}

-- =========

-- PTC CCPDU

-- =========

PTCCCPDU ::= OCTET STRING

-- =================

-- 5G PTC parameters

-- =================

PTCRegistrationRequest ::= ENUMERATED

{

register(1),

reRegister(2),

deRegister(3)

}

PTCRegistrationOutcome ::= ENUMERATED

{

success(1),

failure(2)

}

PTCSessionEndCause ::= ENUMERATED

{

initiaterLeavesSession(1),

definedParticipantLeaves(2),

numberOfParticipants(3),

sessionTimerExpired(4),

pTCSpeechInactive(5),

allMediaTypesInactive(6)

}

PTCTargetInformation ::= SEQUENCE

{

identifiers [1] SEQUENCE SIZE(1..MAX) OF PTCIdentifiers

}

PTCIdentifiers ::= CHOICE

{

mCPTTID [1] UTF8String,

instanceIdentifierURN [2] UTF8String,

pTCChatGroupID [3] PTCChatGroupID,

iMPU [4] IMPU,

iMPI [5] IMPI

}

PTCSessionInfo ::= SEQUENCE

{

pTCSessionURI [1] UTF8String,

pTCSessionType [2] PTCSessionType

}

PTCSessionType ::= ENUMERATED

{

ondemand(1),

preEstablished(2),

adhoc(3),

prearranged(4),

groupSession(5)

}

MultipleParticipantPresenceStatus ::= SEQUENCE OF PTCParticipantPresenceStatus

PTCParticipantPresenceStatus ::= SEQUENCE

{

presenceID [1] PTCTargetInformation,

presenceType [2] PTCPresenceType,

presenceStatus [3] BOOLEAN

}

PTCPresenceType ::= ENUMERATED

{

pTCClient(1),

pTCGroup(2)

}

PTCPreEstStatus ::= ENUMERATED

{

established(1),

modified(2),

released(3)

}

RTPSetting ::= SEQUENCE

{

iPAddress [1] IPAddress,

portNumber [2] PortNumber

}

PTCIDList ::= SEQUENCE

{

pTCPartyID [1] PTCTargetInformation,

pTCChatGroupID [2] PTCChatGroupID

}

PTCChatGroupID ::= SEQUENCE

{

groupIdentity [1] UTF8String

}

PTCFloorActivity ::= ENUMERATED

{

tBCPRequest(1),

tBCPGranted(2),

tBCPDeny(3),

tBCPIdle(4),

tBCPTaken(5),

tBCPRevoke(6),

tBCPQueued(7),

tBCPRelease(8)

}

PTCTBPriorityLevel ::= ENUMERATED

{

preEmptive(1),

highPriority(2),

normalPriority(3),

listenOnly(4)

}

PTCTBReasonCode ::= ENUMERATED

{

noQueuingAllowed(1),

oneParticipantSession(2),

listenOnly(3),

exceededMaxDuration(4),

tBPrevented(5)

}

PTCListManagementType ::= ENUMERATED

{

contactListManagementAttempt(1),

groupListManagementAttempt(2),

contactListManagementResult(3),

groupListManagementResult(4),

requestUnsuccessful(5)

}

PTCListManagementAction ::= ENUMERATED

{

create(1),

modify(2),

retrieve(3),

delete(4),

notify(5)

}

PTCAccessPolicyType ::= ENUMERATED

{

pTCUserAccessPolicyAttempt(1),

groupAuthorizationRulesAttempt(2),

pTCUserAccessPolicyQuery(3),

groupAuthorizationRulesQuery(4),

pTCUserAccessPolicyResult(5),

groupAuthorizationRulesResult(6),

requestUnsuccessful(7)

}

PTCUserAccessPolicy ::= ENUMERATED

{

allowIncomingPTCSessionRequest(1),

blockIncomingPTCSessionRequest(2),

allowAutoAnswerMode(3),

allowOverrideManualAnswerMode(4)

}

PTCGroupAuthRule ::= ENUMERATED

{

allowInitiatingPTCSession(1),

blockInitiatingPTCSession(2),

allowJoiningPTCSession(3),

blockJoiningPTCSession(4),

allowAddParticipants(5),

blockAddParticipants(6),

allowSubscriptionPTCSessionState(7),

blockSubscriptionPTCSessionState(8),

allowAnonymity(9),

forbidAnonymity(10)

}

PTCFailureCode ::= ENUMERATED

{

sessionCannotBeEstablished(1),

sessionCannotBeModified(2)

}

PTCListManagementFailure ::= ENUMERATED

{

requestUnsuccessful(1),

requestUnknown(2)

}

PTCAccessPolicyFailure ::= ENUMERATED

{

requestUnsuccessful(1),

requestUnknown(2)

}

-- ===================

-- 5G LALS definitions

-- ===================

LALSReport ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

-- pEI [2] PEI OPTIONAL, deprecated in Release-16, do not re-use this tag number

gPSI [3] GPSI OPTIONAL,

location [4] Location OPTIONAL,

iMPU [5] IMPU OPTIONAL,

iMSI [7] IMSI OPTIONAL,

mSISDN [8] MSISDN OPTIONAL

}

-- =====================

-- PDHR/PDSR definitions

-- =====================

PDHeaderReport ::= SEQUENCE

{

pDUSessionID [1] PDUSessionID,

sourceIPAddress [2] IPAddress,

sourcePort [3] PortNumber OPTIONAL,

destinationIPAddress [4] IPAddress,

destinationPort [5] PortNumber OPTIONAL,

nextLayerProtocol [6] NextLayerProtocol,

iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

direction [8] Direction,

packetSize [9] INTEGER

}

PDSummaryReport ::= SEQUENCE

{

pDUSessionID [1] PDUSessionID,

sourceIPAddress [2] IPAddress,

sourcePort [3] PortNumber OPTIONAL,

destinationIPAddress [4] IPAddress,

destinationPort [5] PortNumber OPTIONAL,

nextLayerProtocol [6] NextLayerProtocol,

iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

direction [8] Direction,

pDSRSummaryTrigger [9] PDSRSummaryTrigger,

firstPacketTimestamp [10] Timestamp,

lastPacketTimestamp [11] Timestamp,

packetCount [12] INTEGER,

byteCount [13] INTEGER

}

-- ====================

-- PDHR/PDSR parameters

-- ====================

PDSRSummaryTrigger ::= ENUMERATED

{

timerExpiry(1),

packetCount(2),

byteCount(3),

startOfFlow(4),

endOfFlow(5)

}

-- ==================================

-- Identifier Association definitions

-- ==================================

AMFIdentifierAssociation ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI,

location [6] Location,

fiveGSTAIList [7] TAIList OPTIONAL

}

MMEIdentifierAssociation ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

gUTI [4] GUTI,

location [5] Location,

tAIList [6] TAIList OPTIONAL

}

-- =================================

-- Identifier Association parameters

-- =================================

MMEGroupID ::= OCTET STRING (SIZE(2))

MMECode ::= OCTET STRING (SIZE(1))

TMSI ::= OCTET STRING (SIZE(4))

-- ===================

-- EPS MME definitions

-- ===================

MMEAttach ::= SEQUENCE

{

attachType [1] EPSAttachType,

attachResult [2] EPSAttachResult,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL,

ePSTAIList [8] TAIList OPTIONAL,

sMSServiceStatus [9] EPSSMSServiceStatus OPTIONAL,

oldGUTI [10] GUTI OPTIONAL,

eMM5GRegStatus [11] EMM5GMMStatus OPTIONAL

}

MMEDetach ::= SEQUENCE

{

detachDirection [1] MMEDirection,

detachType [2] EPSDetachType,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

cause [7] EMMCause OPTIONAL,

location [8] Location OPTIONAL,

switchOffIndicator [9] SwitchOffIndicator OPTIONAL

}

MMELocationUpdate ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

gUTI [4] GUTI OPTIONAL,

location [5] Location OPTIONAL,

oldGUTI [6] GUTI OPTIONAL,

sMSServiceStatus [7] EPSSMSServiceStatus OPTIONAL

}

MMEStartOfInterceptionWithEPSAttachedUE ::= SEQUENCE

{

attachType [1] EPSAttachType,

attachResult [2] EPSAttachResult,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL,

ePSTAIList [9] TAIList OPTIONAL,

sMSServiceStatus [10] EPSSMSServiceStatus OPTIONAL,

eMM5GRegStatus [12] EMM5GMMStatus OPTIONAL

}

MMEUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] MMEFailedProcedureType,

failureCause [2] MMEFailureCause,

iMSI [3] IMSI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL

}

-- ==================

-- EPS MME parameters

-- ==================

EMMCause ::= INTEGER (0..255)

ESMCause ::= INTEGER (0..255)

EPSAttachType ::= ENUMERATED

{

ePSAttach(1),

combinedEPSIMSIAttach(2),

ePSRLOSAttach(3),

ePSEmergencyAttach(4),

reserved(5)

}

EPSAttachResult ::= ENUMERATED

{

ePSOnly(1),

combinedEPSIMSI(2)

}

EPSDetachType ::= ENUMERATED

{

ePSDetach(1),

iMSIDetach(2),

combinedEPSIMSIDetach(3),

reAttachRequired(4),

reAttachNotRequired(5),

reserved(6)

}

EPSSMSServiceStatus ::= ENUMERATED

{

sMSServicesNotAvailable(1),

sMSServicesNotAvailableInThisPLMN(2),

networkFailure(3),

congestion(4)

}

MMEDirection ::= ENUMERATED

{

networkInitiated(1),

uEInitiated(2)

}

MMEFailedProcedureType ::= ENUMERATED

{

attachReject(1),

authenticationReject(2),

securityModeReject(3),

serviceReject(4),

trackingAreaUpdateReject(5),

activateDedicatedEPSBearerContextReject(6),

activateDefaultEPSBearerContextReject(7),

bearerResourceAllocationReject(8),

bearerResourceModificationReject(9),

modifyEPSBearerContectReject(10),

pDNConnectivityReject(11),

pDNDisconnectReject(12)

}

MMEFailureCause ::= CHOICE

{

eMMCause [1] EMMCause,

eSMCause [2] ESMCause

}

-- ===========================

-- LI Notification definitions

-- ===========================

LINotification ::= SEQUENCE

{

notificationType [1] LINotificationType,

appliedTargetID [2] TargetIdentifier OPTIONAL,

appliedDeliveryInformation [3] SEQUENCE OF LIAppliedDeliveryInformation OPTIONAL,

appliedStartTime [4] Timestamp OPTIONAL,

appliedEndTime [5] Timestamp OPTIONAL

}

-- ==========================

-- LI Notification parameters

-- ==========================

LINotificationType ::= ENUMERATED

{

activation(1),

deactivation(2),

modification(3)

}

LIAppliedDeliveryInformation ::= SEQUENCE

{

hI2DeliveryIPAddress [1] IPAddress OPTIONAL,

hI2DeliveryPortNumber [2] PortNumber OPTIONAL,

hI3DeliveryIPAddress [3] IPAddress OPTIONAL,

hI3DeliveryPortNumber [4] PortNumber OPTIONAL

}

-- ===============

-- MDF definitions

-- ===============

MDFCellSiteReport ::= SEQUENCE OF CellInformation

-- ==============================

-- 5G EPS Interworking Parameters

-- ==============================

EMM5GMMStatus ::= SEQUENCE

{

eMMRegStatus [1] EMMRegStatus OPTIONAL,

fiveGMMStatus [2] FiveGMMStatus OPTIONAL

}

EPS5GGUTI ::= CHOICE

{

gUTI [1] GUTI,

fiveGGUTI [2] FiveGGUTI

}

EMMRegStatus ::= ENUMERATED

{

uEEMMRegistered(1),

uENotEMMRegistered(2)

}

FiveGMMStatus ::= ENUMERATED

{

uE5GMMRegistered(1),

uENot5GMMRegistered(2)

}

-- ========================================

-- Separated Location Reporting definitions

-- ========================================

SeparatedLocationReporting ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI OPTIONAL,

location [6] Location,

non3GPPAccessEndpoint [7] UEEndpointAddress OPTIONAL,

fiveGSTAIList [8] TAIList OPTIONAL,

rATType [9] RATType OPTIONAL

}

-- =================

-- Common Parameters

-- =================

AccessType ::= ENUMERATED

{

threeGPPAccess(1),

nonThreeGPPAccess(2),

threeGPPandNonThreeGPPAccess(3)

}

Direction ::= ENUMERATED

{

fromTarget(1),

toTarget(2)

}

DNN ::= UTF8String

E164Number ::= NumericString (SIZE(1..15))

EmailAddress ::= UTF8String

FiveGGUTI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

aMFRegionID [3] AMFRegionID,

aMFSetID [4] AMFSetID,

aMFPointer [5] AMFPointer,

fiveGTMSI [6] FiveGTMSI

}

FiveGMMCause ::= INTEGER (0..255)

FiveGSMRequestType ::= ENUMERATED

{

initialRequest(1),

existingPDUSession(2),

initialEmergencyRequest(3),

existingEmergencyPDUSession(4),

modificationRequest(5),

reserved(6),

mAPDURequest(7)

}

FiveGSMCause ::= INTEGER (0..255)

FiveGTMSI ::= INTEGER (0..4294967295)

FTEID ::= SEQUENCE

{

tEID [1] INTEGER (0.. 4294967295),

iPv4Address [2] IPv4Address OPTIONAL,

iPv6Address [3] IPv6Address OPTIONAL

}

GPSI ::= CHOICE

{

mSISDN [1] MSISDN,

nAI [2] NAI

}

GUAMI ::= SEQUENCE

{

aMFID [1] AMFID,

pLMNID [2] PLMNID

}

GUMMEI ::= SEQUENCE

{

mMEID [1] MMEID,

mCC [2] MCC,

mNC [3] MNC

}

GUTI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

mMEGroupID [3] MMEGroupID,

mMECode [4] MMECode,

mTMSI [5] TMSI

}

HomeNetworkPublicKeyID ::= OCTET STRING

HSMFURI ::= UTF8String

IMEI ::= NumericString (SIZE(14))

IMEISV ::= NumericString (SIZE(16))

IMPI ::= NAI

IMPU ::= CHOICE

{

sIPURI [1] SIPURI,

tELURI [2] TELURI

}

IMSI ::= NumericString (SIZE(6..15))

Initiator ::= ENUMERATED

{

uE(1),

network(2),

unknown(3)

}

IPAddress ::= CHOICE

{

iPv4Address [1] IPv4Address,

iPv6Address [2] IPv6Address

}

IPv4Address ::= OCTET STRING (SIZE(4))

IPv6Address ::= OCTET STRING (SIZE(16))

IPv6FlowLabel ::= INTEGER(0..1048575)

MACAddress ::= OCTET STRING (SIZE(6))

MACRestrictionIndicator ::= ENUMERATED

{

noResrictions(1),

mACAddressNotUseableAsEquipmentIdentifier(2),

unknown(3)

}

MCC ::= NumericString (SIZE(3))

MNC ::= NumericString (SIZE(2..3))

MMEID ::= SEQUENCE

{

mMEGI [1] MMEGI,

mMEC [2] MMEC

}

MMEC ::= NumericString

MMEGI ::= NumericString

MSISDN ::= NumericString (SIZE(1..15))

NAI ::= UTF8String

NextLayerProtocol ::= INTEGER(0..255)

NonLocalID ::= ENUMERATED

{

local(1),

nonLocal(2)

}

NonIMEISVPEI ::= CHOICE

{

mACAddress [1] MACAddress

}

NSSAI ::= SEQUENCE OF SNSSAI

PLMNID ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC

}

PDUSessionID ::= INTEGER (0..255)

PDUSessionType ::= ENUMERATED

{

iPv4(1),

iPv6(2),

iPv4v6(3),

unstructured(4),

ethernet(5)

}

PEI ::= CHOICE

{

iMEI [1] IMEI,

iMEISV [2] IMEISV

}

PortNumber ::= INTEGER(0..65535)

ProtectionSchemeID ::= INTEGER (0..15)

RATType ::= ENUMERATED

{

nR(1),

eUTRA(2),

wLAN(3),

virtual(4),

nBIOT(5),

wireline(6),

wirelineCable(7),

wirelineBBF(8),

lTEM(9),

nRU(10),

eUTRAU(11),

trustedN3GA(12),

trustedWLAN(13),

uTRA(14),

gERA(15)

}

RejectedNSSAI ::= SEQUENCE OF RejectedSNSSAI

RejectedSNSSAI ::= SEQUENCE

{

causeValue [1] RejectedSliceCauseValue,

sNSSAI [2] SNSSAI

}

RejectedSliceCauseValue ::= INTEGER (0..255)

ReRegRequiredIndicator ::= ENUMERATED

{

reRegistrationRequired(1),

reRegistrationNotRequired(2)

}

RoutingIndicator ::= INTEGER (0..9999)

SchemeOutput ::= OCTET STRING

SIPURI ::= UTF8String

Slice ::= SEQUENCE

{

allowedNSSAI [1] NSSAI OPTIONAL,

configuredNSSAI [2] NSSAI OPTIONAL,

rejectedNSSAI [3] RejectedNSSAI OPTIONAL

}

SMPDUDNRequest ::= OCTET STRING

-- TS 24.501 [13], clause 9.11.3.6.1

SMSOverNASIndicator ::= ENUMERATED

{

sMSOverNASNotAllowed(1),

sMSOverNASAllowed(2)

}

SNSSAI ::= SEQUENCE

{

sliceServiceType [1] INTEGER (0..255),

sliceDifferentiator [2] OCTET STRING (SIZE(3)) OPTIONAL

}

SUCI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

routingIndicator [3] RoutingIndicator,

protectionSchemeID [4] ProtectionSchemeID,

homeNetworkPublicKeyID [5] HomeNetworkPublicKeyID,

schemeOutput [6] SchemeOutput

}

SUPI ::= CHOICE

{

iMSI [1] IMSI,

nAI [2] NAI

}

SUPIUnauthenticatedIndication ::= BOOLEAN

SwitchOffIndicator ::= ENUMERATED

{

normalDetach(1),

switchOff(2)

}

TargetIdentifier ::= CHOICE

{

sUPI [1] SUPI,

iMSI [2] IMSI,

pEI [3] PEI,

iMEI [4] IMEI,

gPSI [5] GPSI,

mSISDN [6] MSISDN,

nAI [7] NAI,

iPv4Address [8] IPv4Address,

iPv6Address [9] IPv6Address,

ethernetAddress [10] MACAddress

}

TargetIdentifierProvenance ::= ENUMERATED

{

lEAProvided(1),

observed(2),

matchedOn(3),

other(4)

}

TELURI ::= UTF8String

Timestamp ::= GeneralizedTime

UEEndpointAddress ::= CHOICE

{

iPv4Address [1] IPv4Address,

iPv6Address [2] IPv6Address,

ethernetAddress [3] MACAddress

}

-- ===================

-- Location parameters

-- ===================

Location ::= SEQUENCE

{

locationInfo [1] LocationInfo OPTIONAL,

positioningInfo [2] PositioningInfo OPTIONAL,

locationPresenceReport [3] LocationPresenceReport OPTIONAL,

ePSLocationInfo [4] EPSLocationInfo OPTIONAL

}

CellSiteInformation ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

azimuth [2] INTEGER (0..359) OPTIONAL,

operatorSpecificInformation [3] UTF8String OPTIONAL

}

-- TS 29.518 [22], clause 6.4.6.2.6

LocationInfo ::= SEQUENCE

{

userLocation [1] UserLocation OPTIONAL,

currentLoc [2] BOOLEAN OPTIONAL,

geoInfo [3] GeographicArea OPTIONAL,

rATType [4] RATType OPTIONAL,

timeZone [5] TimeZone OPTIONAL,

additionalCellIDs [6] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.7

UserLocation ::= SEQUENCE

{

eUTRALocation [1] EUTRALocation OPTIONAL,

nRLocation [2] NRLocation OPTIONAL,

n3GALocation [3] N3GALocation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.8

EUTRALocation ::= SEQUENCE

{

tAI [1] TAI,

eCGI [2] ECGI,

ageOfLocationInfo [3] INTEGER OPTIONAL,

uELocationTimestamp [4] Timestamp OPTIONAL,

geographicalInformation [5] UTF8String OPTIONAL,

geodeticInformation [6] UTF8String OPTIONAL,

globalNGENbID [7] GlobalRANNodeID OPTIONAL,

cellSiteInformation [8] CellSiteInformation OPTIONAL,

globalENbID [9] GlobalRANNodeID OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.9

NRLocation ::= SEQUENCE

{

tAI [1] TAI,

nCGI [2] NCGI,

ageOfLocationInfo [3] INTEGER OPTIONAL,

uELocationTimestamp [4] Timestamp OPTIONAL,

geographicalInformation [5] UTF8String OPTIONAL,

geodeticInformation [6] UTF8String OPTIONAL,

globalGNbID [7] GlobalRANNodeID OPTIONAL,

cellSiteInformation [8] CellSiteInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.10

N3GALocation ::= SEQUENCE

{

tAI [1] TAI OPTIONAL,

n3IWFID [2] N3IWFIDNGAP OPTIONAL,

uEIPAddr [3] IPAddr OPTIONAL,

portNumber [4] INTEGER OPTIONAL,

tNAPID [5] TNAPID OPTIONAL,

tWAPID [6] TWAPID OPTIONAL,

hFCNodeID [7] HFCNodeID OPTIONAL,

gLI [8] GLI OPTIONAL,

w5GBANLineType [9] W5GBANLineType OPTIONAL,

gCI [10] GCI OPTIONAL,

ageOfLocationInfo [11] INTEGER OPTIONAL,

uELocationTimestamp [12] Timestamp OPTIONAL

}

-- TS 38.413 [23], clause 9.3.2.4

IPAddr ::= SEQUENCE

{

iPv4Addr [1] IPv4Address OPTIONAL,

iPv6Addr [2] IPv6Address OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.28

GlobalRANNodeID ::= SEQUENCE

{

pLMNID [1] PLMNID,

aNNodeID [2] ANNodeID,

nID [3] NID OPTIONAL

}

ANNodeID ::= CHOICE

{

n3IWFID [1] N3IWFIDSBI,

gNbID [2] GNbID,

nGENbID [3] NGENbID,

eNbID [4] ENbID,

wAGFID [5] WAGFID,

tNGFID [6] TNGFID

}

-- TS 38.413 [23], clause 9.3.1.6

GNbID ::= BIT STRING(SIZE(22..32))

-- TS 29.571 [17], clause 5.4.4.4

TAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

tAC [2] TAC,

nID [3] NID OPTIONAL

}

CGI ::= SEQUENCE

{

lAI [1] LAI,

cellID [2] CellID

}

LAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

lAC [2] LAC

}

LAC ::= OCTET STRING (SIZE(2))

CellID ::= OCTET STRING (SIZE(2))

SAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

lAC [2] LAC,

sAC [3] SAC

}

SAC ::= OCTET STRING (SIZE(2))

-- TS 29.571 [17], clause 5.4.4.5

ECGI ::= SEQUENCE

{

pLMNID [1] PLMNID,

eUTRACellID [2] EUTRACellID,

nID [3] NID OPTIONAL

}

TAIList ::= SEQUENCE OF TAI

-- TS 29.571 [17], clause 5.4.4.6

NCGI ::= SEQUENCE

{

pLMNID [1] PLMNID,

nRCellID [2] NRCellID,

nID [3] NID OPTIONAL

}

RANCGI ::= CHOICE

{

eCGI [1] ECGI,

nCGI [2] NCGI

}

CellInformation ::= SEQUENCE

{

rANCGI [1] RANCGI,

cellSiteinformation [2] CellSiteInformation OPTIONAL,

timeOfLocation [3] Timestamp OPTIONAL

}

-- TS 38.413 [23], clause 9.3.1.57

N3IWFIDNGAP ::= BIT STRING (SIZE(16))

-- TS 29.571 [17], clause 5.4.4.28

N3IWFIDSBI ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.28 and table 5.4.2-1

TNGFID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.28 and table 5.4.2-1

WAGFID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.62

TNAPID ::= SEQUENCE

{

sSID [1] SSID OPTIONAL,

bSSID [2] BSSID OPTIONAL,

civicAddress [3] CivicAddressBytes OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.64

TWAPID ::= SEQUENCE

{

sSID [1] SSID OPTIONAL,

bSSID [2] BSSID OPTIONAL,

civicAddress [3] CivicAddressBytes OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.62 and clause 5.4.4.64

SSID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.62 and clause 5.4.4.64

BSSID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.36 and table 5.4.2-1

HFCNodeID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.2-1

-- Contains the original binary data i.e. value of the YAML field after base64 encoding is removed

GLI ::= OCTET STRING (SIZE(0..150))

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.2-1

GCI ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.10 and clause 5.4.3.33

W5GBANLineType ::= ENUMERATED

{

dSL(1),

pON(2)

}

-- TS 29.571 [17], table 5.4.2-1

TAC ::= OCTET STRING (SIZE(2..3))

-- TS 38.413 [23], clause 9.3.1.9

EUTRACellID ::= BIT STRING (SIZE(28))

-- TS 38.413 [23], clause 9.3.1.7

NRCellID ::= BIT STRING (SIZE(36))

-- TS 38.413 [23], clause 9.3.1.8

NGENbID ::= CHOICE

{

macroNGENbID [1] BIT STRING (SIZE(20)),

shortMacroNGENbID [2] BIT STRING (SIZE(18)),

longMacroNGENbID [3] BIT STRING (SIZE(21))

}

-- TS 23.003 [19], clause 12.7.1 encoded as per TS 29.571 [17], clause 5.4.2

NID ::= UTF8String (SIZE(11))

-- TS 36.413 [38], clause 9.2.1.37

ENbID ::= CHOICE

{

macroENbID [1] BIT STRING (SIZE(20)),

homeENbID [2] BIT STRING (SIZE(28)),

shortMacroENbID [3] BIT STRING (SIZE(18)),

longMacroENbID [4] BIT STRING (SIZE(21))

}

-- TS 29.518 [22], clause 6.4.6.2.3

PositioningInfo ::= SEQUENCE

{

positionInfo [1] LocationData OPTIONAL,

rawMLPResponse [2] RawMLPResponse OPTIONAL

}

RawMLPResponse ::= CHOICE

{

-- The following parameter contains a copy of unparsed XML code of the

-- MLP response message, i.e. the entire XML document containing

-- a <slia> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.2) or

-- a <slirep> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.3) MLP message.

mLPPositionData [1] UTF8String,

-- OMA MLP result id, defined in OMA-TS-MLP-V3\_5-20181211-C [20], Clause 5.4

mLPErrorCode [2] INTEGER (1..699)

}

-- TS 29.572 [24], clause 6.1.6.2.3

LocationData ::= SEQUENCE

{

locationEstimate [1] GeographicArea,

accuracyFulfilmentIndicator [2] AccuracyFulfilmentIndicator OPTIONAL,

ageOfLocationEstimate [3] AgeOfLocationEstimate OPTIONAL,

velocityEstimate [4] VelocityEstimate OPTIONAL,

civicAddress [5] CivicAddress OPTIONAL,

positioningDataList [6] SET OF PositioningMethodAndUsage OPTIONAL,

gNSSPositioningDataList [7] SET OF GNSSPositioningMethodAndUsage OPTIONAL,

eCGI [8] ECGI OPTIONAL,

nCGI [9] NCGI OPTIONAL,

altitude [10] Altitude OPTIONAL,

barometricPressure [11] BarometricPressure OPTIONAL

}

-- TS 29.172 [53], table 6.2.2-2

EPSLocationInfo ::= SEQUENCE

{

locationData [1] LocationData,

cGI [2] CGI OPTIONAL,

sAI [3] SAI OPTIONAL,

eSMLCCellInfo [4] ESMLCCellInfo OPTIONAL

}

-- TS 29.172 [53], clause 7.4.57

ESMLCCellInfo ::= SEQUENCE

{

eCGI [1] ECGI,

cellPortionID [2] CellPortionID

}

-- TS 29.171 [54], clause 7.4.31

CellPortionID ::= INTEGER (0..4095)

-- TS 29.518 [22], clause 6.2.6.2.5

LocationPresenceReport ::= SEQUENCE

{

type [1] AMFEventType,

timestamp [2] Timestamp,

areaList [3] SET OF AMFEventArea OPTIONAL,

timeZone [4] TimeZone OPTIONAL,

accessTypes [5] SET OF AccessType OPTIONAL,

rMInfoList [6] SET OF RMInfo OPTIONAL,

cMInfoList [7] SET OF CMInfo OPTIONAL,

reachability [8] UEReachability OPTIONAL,

location [9] UserLocation OPTIONAL,

additionalCellIDs [10] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.3.3

AMFEventType ::= ENUMERATED

{

locationReport(1),

presenceInAOIReport(2)

}

-- TS 29.518 [22], clause 6.2.6.2.16

AMFEventArea ::= SEQUENCE

{

presenceInfo [1] PresenceInfo OPTIONAL,

lADNInfo [2] LADNInfo OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.27

PresenceInfo ::= SEQUENCE

{

presenceState [1] PresenceState OPTIONAL,

trackingAreaList [2] SET OF TAI OPTIONAL,

eCGIList [3] SET OF ECGI OPTIONAL,

nCGIList [4] SET OF NCGI OPTIONAL,

globalRANNodeIDList [5] SET OF GlobalRANNodeID OPTIONAL,

globalENbIDList [6] SET OF GlobalRANNodeID OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.2.17

LADNInfo ::= SEQUENCE

{

lADN [1] UTF8String,

presence [2] PresenceState OPTIONAL

}

-- TS 29.571 [17], clause 5.4.3.20

PresenceState ::= ENUMERATED

{

inArea(1),

outOfArea(2),

unknown(3),

inactive(4)

}

-- TS 29.518 [22], clause 6.2.6.2.8

RMInfo ::= SEQUENCE

{

rMState [1] RMState,

accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.2.9

CMInfo ::= SEQUENCE

{

cMState [1] CMState,

accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.3.7

UEReachability ::= ENUMERATED

{

unreachable(1),

reachable(2),

regulatoryOnly(3)

}

-- TS 29.518 [22], clause 6.2.6.3.9

RMState ::= ENUMERATED

{

registered(1),

deregistered(2)

}

-- TS 29.518 [22], clause 6.2.6.3.10

CMState ::= ENUMERATED

{

idle(1),

connected(2)

}

-- TS 29.572 [24], clause 6.1.6.2.5

GeographicArea ::= CHOICE

{

point [1] Point,

pointUncertaintyCircle [2] PointUncertaintyCircle,

pointUncertaintyEllipse [3] PointUncertaintyEllipse,

polygon [4] Polygon,

pointAltitude [5] PointAltitude,

pointAltitudeUncertainty [6] PointAltitudeUncertainty,

ellipsoidArc [7] EllipsoidArc

}

-- TS 29.572 [24], clause 6.1.6.3.12

AccuracyFulfilmentIndicator ::= ENUMERATED

{

requestedAccuracyFulfilled(1),

requestedAccuracyNotFulfilled(2)

}

-- TS 29.572 [24], clause 6.1.6.2.17

VelocityEstimate ::= CHOICE

{

horVelocity [1] HorizontalVelocity,

horWithVertVelocity [2] HorizontalWithVerticalVelocity,

horVelocityWithUncertainty [3] HorizontalVelocityWithUncertainty,

horWithVertVelocityAndUncertainty [4] HorizontalWithVerticalVelocityAndUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.14

CivicAddress ::= SEQUENCE

{

country [1] UTF8String,

a1 [2] UTF8String OPTIONAL,

a2 [3] UTF8String OPTIONAL,

a3 [4] UTF8String OPTIONAL,

a4 [5] UTF8String OPTIONAL,

a5 [6] UTF8String OPTIONAL,

a6 [7] UTF8String OPTIONAL,

prd [8] UTF8String OPTIONAL,

pod [9] UTF8String OPTIONAL,

sts [10] UTF8String OPTIONAL,

hno [11] UTF8String OPTIONAL,

hns [12] UTF8String OPTIONAL,

lmk [13] UTF8String OPTIONAL,

loc [14] UTF8String OPTIONAL,

nam [15] UTF8String OPTIONAL,

pc [16] UTF8String OPTIONAL,

bld [17] UTF8String OPTIONAL,

unit [18] UTF8String OPTIONAL,

flr [19] UTF8String OPTIONAL,

room [20] UTF8String OPTIONAL,

plc [21] UTF8String OPTIONAL,

pcn [22] UTF8String OPTIONAL,

pobox [23] UTF8String OPTIONAL,

addcode [24] UTF8String OPTIONAL,

seat [25] UTF8String OPTIONAL,

rd [26] UTF8String OPTIONAL,

rdsec [27] UTF8String OPTIONAL,

rdbr [28] UTF8String OPTIONAL,

rdsubbr [29] UTF8String OPTIONAL,

prm [30] UTF8String OPTIONAL,

pom [31] UTF8String OPTIONAL

}

-- TS 29.571 [17], clauses 5.4.4.62 and 5.4.4.64

-- Contains the original binary data i.e. value of the YAML field after base64 encoding is removed

CivicAddressBytes ::= OCTET STRING

-- TS 29.572 [24], clause 6.1.6.2.15

PositioningMethodAndUsage ::= SEQUENCE

{

method [1] PositioningMethod,

mode [2] PositioningMode,

usage [3] Usage,

methodCode [4] MethodCode OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.16

GNSSPositioningMethodAndUsage ::= SEQUENCE

{

mode [1] PositioningMode,

gNSS [2] GNSSID,

usage [3] Usage

}

-- TS 29.572 [24], clause 6.1.6.2.6

Point ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.7

PointUncertaintyCircle ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

uncertainty [2] Uncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.8

PointUncertaintyEllipse ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

uncertainty [2] UncertaintyEllipse,

confidence [3] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.9

Polygon ::= SEQUENCE

{

pointList [1] SET SIZE (3..15) OF GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.10

PointAltitude ::= SEQUENCE

{

point [1] GeographicalCoordinates,

altitude [2] Altitude

}

-- TS 29.572 [24], clause 6.1.6.2.11

PointAltitudeUncertainty ::= SEQUENCE

{

point [1] GeographicalCoordinates,

altitude [2] Altitude,

uncertaintyEllipse [3] UncertaintyEllipse,

uncertaintyAltitude [4] Uncertainty,

confidence [5] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.12

EllipsoidArc ::= SEQUENCE

{

point [1] GeographicalCoordinates,

innerRadius [2] InnerRadius,

uncertaintyRadius [3] Uncertainty,

offsetAngle [4] Angle,

includedAngle [5] Angle,

confidence [6] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.4

GeographicalCoordinates ::= SEQUENCE

{

latitude [1] UTF8String,

longitude [2] UTF8String,

mapDatumInformation [3] OGCURN OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.22

UncertaintyEllipse ::= SEQUENCE

{

semiMajor [1] Uncertainty,

semiMinor [2] Uncertainty,

orientationMajor [3] Orientation

}

-- TS 29.572 [24], clause 6.1.6.2.18

HorizontalVelocity ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle

}

-- TS 29.572 [24], clause 6.1.6.2.19

HorizontalWithVerticalVelocity ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

vSpeed [3] VerticalSpeed,

vDirection [4] VerticalDirection

}

-- TS 29.572 [24], clause 6.1.6.2.20

HorizontalVelocityWithUncertainty ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

uncertainty [3] SpeedUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.21

HorizontalWithVerticalVelocityAndUncertainty ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

vSpeed [3] VerticalSpeed,

vDirection [4] VerticalDirection,

hUncertainty [5] SpeedUncertainty,

vUncertainty [6] SpeedUncertainty

}

-- The following types are described in TS 29.572 [24], table 6.1.6.3.2-1

Altitude ::= UTF8String

Angle ::= INTEGER (0..360)

Uncertainty ::= INTEGER (0..127)

Orientation ::= INTEGER (0..180)

Confidence ::= INTEGER (0..100)

InnerRadius ::= INTEGER (0..65535)

AgeOfLocationEstimate ::= INTEGER (0..32767)

HorizontalSpeed ::= UTF8String

VerticalSpeed ::= UTF8String

SpeedUncertainty ::= UTF8String

BarometricPressure ::= INTEGER (30000..155000)

-- TS 29.572 [24], clause 6.1.6.3.13

VerticalDirection ::= ENUMERATED

{

upward(1),

downward(2)

}

-- TS 29.572 [24], clause 6.1.6.3.6

PositioningMethod ::= ENUMERATED

{

cellID(1),

eCID(2),

oTDOA(3),

barometricPressure(4),

wLAN(5),

bluetooth(6),

mBS(7),

motionSensor(8),

dLTDOA(9),

dLAOD(10),

multiRTT(11),

nRECID(12),

uLTDOA(13),

uLAOA(14),

networkSpecific(15)

}

-- TS 29.572 [24], clause 6.1.6.3.7

PositioningMode ::= ENUMERATED

{

uEBased(1),

uEAssisted(2),

conventional(3)

}

-- TS 29.572 [24], clause 6.1.6.3.8

GNSSID ::= ENUMERATED

{

gPS(1),

galileo(2),

sBAS(3),

modernizedGPS(4),

qZSS(5),

gLONASS(6),

bDS(7),

nAVIC(8)

}

-- TS 29.572 [24], clause 6.1.6.3.9

Usage ::= ENUMERATED

{

unsuccess(1),

successResultsNotUsed(2),

successResultsUsedToVerifyLocation(3),

successResultsUsedToGenerateLocation(4),

successMethodNotDetermined(5)

}

-- TS 29.571 [17], table 5.2.2-1

TimeZone ::= UTF8String

-- Open Geospatial Consortium URN [35]

OGCURN ::= UTF8String

-- TS 29.572 [24], clause 6.1.6.2.15

MethodCode ::= INTEGER (16..31)

END

\*\*\*END OF FOURTH CHANGE\*\*\*

\*\*\*END OF ALL CHANGES\*\*\*